@N|Running in 32-bit mode
@N: CG364 :"C:\Microsemi\Libero_v10.0\Synopsys\synplify_F201109M\lib\proasic\smartfusion.v":1868:7:1868:9|Synthesizing module VCC
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":67:7:67:15|Synthesizing module BIBUF_MSS
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":51:7:51:17|Synthesizing module TRIBUFF_MSS
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":23:7:23:15|Synthesizing module INBUF_MSS
@N: CG364 :"C:\Microsemi\Libero_v10.0\Synopsys\synplify_F201109M\lib\proasic\smartfusion.v":1141:7:1141:9|Synthesizing module GND
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\work\SPI_Flash_Read_Write\mss_tshell.v":1:7:1:13|Synthesizing module MSS_APB
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":37:7:37:16|Synthesizing module OUTBUF_MSS
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":151:7:151:13|Synthesizing module MSS_CCC
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":1:7:1:16|Synthesizing module MSS_XTLOSC
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\work\SPI_Flash_Read_Write\MSS_CCC_0\SPI_Flash_Read_Write_tmp_MSS_CCC_0_MSS_CCC.v":5:7:5:48|Synthesizing module SPI_Flash_Read_Write_tmp_MSS_CCC_0_MSS_CCC
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\work\SPI_Flash_Read_Write\SPI_Flash_Read_Write.v":5:7:5:26|Synthesizing module SPI_Flash_Read_Write
@N: CG364 :"C:\A2F_AC343_DF\A2F500\component\work\SPI_TOP\SPI_TOP.v":5:7:5:13|Synthesizing module SPI_TOP

