@W: CG775 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":30:7:30:14|Found Component CoreAPB3 in library COREAPB3_LIB
@W: CL118 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\hdl\spi_master.v":217:8:217:11|Latch generated from always block for signal next_state[3:0]; possible missing assignment in an if or case statement.
@W: CS263 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\hdl\spi_sfr.v":381:16:381:26|Port-width mismatch for port tx_data_reg. Formal has width 8, Actual 32
@W: CL246 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\hdl\spi.v":38:16:38:20|Input port bits 23 to 4 of PADDR[23:0] are unused
@W: CL246 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\hdl\spi.v":38:16:38:20|Input port bits 1 to 0 of PADDR[23:0] are unused
@W: CL157 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":62:7:62:18|*Output RCOSC_CLKOUT has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":63:7:63:20|*Output MAINXIN_CLKOUT has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":64:7:64:18|*Output LPXIN_CLKOUT has undriven bits -- simulation mismatch possible.
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":36:7:36:10|Input CLKA is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":37:7:37:14|Input CLKA_PAD is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":38:7:38:15|Input CLKA_PADP is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":39:7:39:15|Input CLKA_PADN is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":40:7:40:10|Input CLKB is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":41:7:41:14|Input CLKB_PAD is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":42:7:42:15|Input CLKB_PADP is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":43:7:43:15|Input CLKB_PADN is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":44:7:44:10|Input CLKC is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":45:7:45:14|Input CLKC_PAD is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":46:7:46:15|Input CLKC_PADP is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":47:7:47:15|Input CLKC_PADN is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":49:7:49:11|Input LPXIN is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\work\mss_top\MSS_CCC_0\mss_top_tmp_MSS_CCC_0_MSS_CCC.v":50:7:50:13|Input MAC_CLK is unused
@W: CL246 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":54:18:54:22|Input port bits 23 to 12 of PADDR[23:0] are unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":52:13:52:19|Input PRESETN is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":53:13:53:16|Input PCLK is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":84:18:84:25|Input PRDATAS1 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":85:18:85:25|Input PRDATAS2 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":86:18:86:25|Input PRDATAS3 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":87:18:87:25|Input PRDATAS4 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":88:18:88:25|Input PRDATAS5 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":89:18:89:25|Input PRDATAS6 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":90:18:90:25|Input PRDATAS7 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":91:18:91:25|Input PRDATAS8 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":92:18:92:25|Input PRDATAS9 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":93:18:93:26|Input PRDATAS10 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":94:18:94:26|Input PRDATAS11 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":95:18:95:26|Input PRDATAS12 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":96:18:96:26|Input PRDATAS13 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":97:18:97:26|Input PRDATAS14 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":98:18:98:26|Input PRDATAS15 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":100:13:100:20|Input PREADYS1 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":101:13:101:20|Input PREADYS2 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":102:13:102:20|Input PREADYS3 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":103:13:103:20|Input PREADYS4 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":104:13:104:20|Input PREADYS5 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":105:13:105:20|Input PREADYS6 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":106:13:106:20|Input PREADYS7 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":107:13:107:20|Input PREADYS8 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":108:13:108:20|Input PREADYS9 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":109:13:109:21|Input PREADYS10 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":110:13:110:21|Input PREADYS11 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":111:13:111:21|Input PREADYS12 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":112:13:112:21|Input PREADYS13 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":113:13:113:21|Input PREADYS14 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":114:13:114:21|Input PREADYS15 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":116:13:116:21|Input PSLVERRS1 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":117:13:117:21|Input PSLVERRS2 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":118:13:118:21|Input PSLVERRS3 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":119:13:119:21|Input PSLVERRS4 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":120:13:120:21|Input PSLVERRS5 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":121:13:121:21|Input PSLVERRS6 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":122:13:122:21|Input PSLVERRS7 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":123:13:123:21|Input PSLVERRS8 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":124:13:124:21|Input PSLVERRS9 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":125:13:125:22|Input PSLVERRS10 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":126:13:126:22|Input PSLVERRS11 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":127:13:127:22|Input PSLVERRS12 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":128:13:128:22|Input PSLVERRS13 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":129:13:129:22|Input PSLVERRS14 is unused
@W: CL159 :"C:\A2F_AC356_DF\A2F500\FTDI\FTDI_SPI\component\Actel\DirectCore\CoreAPB3\3.0.103\rtl\vlog\core\coreapb3.v":130:13:130:22|Input PSLVERRS15 is unused

