Debug File version: Ver 1.0
Creator: Designer
Creator version: v11.3
Creator build: 11.3.0.112
External die name: M2GL010T
Package: 484 FBGA
Design Name: IGLOO2_Oversampling_top
Probe A IO: available for probe A
Probe B IO: not available for probing
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[5]:Transmitter_0/prbs7_10_0/LFSR[6]:Q Type=0 ADDR=0x12021F (WADDR=0x12 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[14]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[14]:Q Type=0 ADDR=0x10010E (WADDR=0x10 BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[2]:Q Type=0 ADDR=0x278018 (WADDR=0x27 BADDR=0x2 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[12]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[12]:Q Type=0 ADDR=0x2B8318 (WADDR=0x2B BADDR=0x2 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[4]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[4]:Q Type=0 ADDR=0x70213 (WADDR=0x7 BADDR=0x0 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[4]:IGLOO2_Oversampling_0/ConfigMaster_0/state[4]:Q Type=0 ADDR=0x11830F (WADDR=0x11 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[17]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[17]:Q Type=0 ADDR=0x138210 (WADDR=0x13 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/envm_soft_reset[0]:IGLOO2_Oversampling_0/ConfigMaster_0/envm_soft_reset[0]:Q Type=0 ADDR=0xF8313 (WADDR=0xF BADDR=0x2 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[22]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[22]:Q Type=0 ADDR=0x8020F (WADDR=0x8 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[6]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[6]:Q Type=0 ADDR=0xF020D (WADDR=0xF BADDR=0x0 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[27]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[27]:Q Type=0 ADDR=0x88010 (WADDR=0x8 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0_uart_data_out[4]:UART_INTERFACE_0/FabUART_0/uart_data_out_t[4]:Q Type=0 ADDR=0x1B031A (WADDR=0x1B BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_state[0]:UART_INTERFACE_0/COREUART_0/make_RX/rx_state[0]:Q Type=0 ADDR=0x15801D (WADDR=0x15 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1D)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[12]:UART_INTERFACE_0/FabUART_0/state[12]:Q Type=0 ADDR=0x19001A (WADDR=0x19 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[30]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[30]:Q Type=0 ADDR=0x12000F (WADDR=0x12 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[17]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[17]:Q Type=0 ADDR=0x158111 (WADDR=0x15 BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[26]:Transmitter_0/FIFO_PRBS_0/data[24]:Q Type=0 ADDR=0x130220 (WADDR=0x13 BADDR=0x0 PRBR=0x2 CLOFFSET=0x20)
ProbePoint: Name=Transmitter_0/prbs7_10_0/tx_count[1]:Transmitter_0/prbs7_10_0/tx_count[1]:Q Type=0 ADDR=0x12031E (WADDR=0x12 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1E)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/mux_sel[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/mux_sel[0]:Q Type=0 ADDR=0x260219 (WADDR=0x26 BADDR=0x0 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[2]:Q Type=0 ADDR=0x288317 (WADDR=0x28 BADDR=0x2 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[8]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[8]:Q Type=0 ADDR=0x78212 (WADDR=0x7 BADDR=0x2 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[12]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[12]:Q Type=0 ADDR=0xB8012 (WADDR=0xB BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[16]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[16]:Q Type=0 ADDR=0x70212 (WADDR=0x7 BADDR=0x0 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0_clear:UART_INTERFACE_0/FabUART_0/clear_t:Q Type=0 ADDR=0x1A001C (WADDR=0x1A BADDR=0x0 PRBR=0x0 CLOFFSET=0x1C)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_bit_sel[2]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_bit_sel[2]:Q Type=0 ADDR=0x178219 (WADDR=0x17 BADDR=0x2 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PSLVERR:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PSLVERR:Q Type=0 ADDR=0x2030F (WADDR=0x2 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[17]:IGLOO2_Oversampling_0/ConfigMaster_0/state[17]:Q Type=0 ADDR=0xD830F (WADDR=0xD BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/samples[0]:UART_INTERFACE_0/COREUART_0/make_RX/samples[0]:Q Type=0 ADDR=0x15031D (WADDR=0x15 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[29]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[29]:Q Type=0 ADDR=0x80010 (WADDR=0x8 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[9]:Q Type=0 ADDR=0x27831B (WADDR=0x27 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[29]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[29]:Q Type=0 ADDR=0x8820F (WADDR=0x8 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[2]:Receiver_0/Downsampler_0/reg_check[2]:Q Type=0 ADDR=0x290319 (WADDR=0x29 BADDR=0x0 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[4]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[4]:Q Type=0 ADDR=0x110312 (WADDR=0x11 BADDR=0x0 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[21]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[21]:Q Type=0 ADDR=0x280218 (WADDR=0x28 BADDR=0x0 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[16]:IGLOO2_Oversampling_0/ConfigMaster_0/state[16]:Q Type=0 ADDR=0xE8010 (WADDR=0xE BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[12]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[12]:Q Type=0 ADDR=0xD8311 (WADDR=0xD BADDR=0x2 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[29]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[29]:Q Type=0 ADDR=0x2A811B (WADDR=0x2A BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[13]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[13]:Q Type=0 ADDR=0x13020E (WADDR=0x13 BADDR=0x0 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[9]:Receiver_0/Downsampler_0/reg_check[9]:Q Type=0 ADDR=0x268018 (WADDR=0x26 BADDR=0x2 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[3]:Q Type=0 ADDR=0x270017 (WADDR=0x27 BADDR=0x0 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[5]:Receiver_0/Downsampler_0/reg_check[5]:Q Type=0 ADDR=0x25031A (WADDR=0x25 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[5]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[5]:Q Type=0 ADDR=0x10000D (WADDR=0x10 BADDR=0x0 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[10]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[10]:Q Type=0 ADDR=0xE810D (WADDR=0xE BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[5]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[5]:Q Type=0 ADDR=0xD8011 (WADDR=0xD BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[0]:UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[0]:Q Type=0 ADDR=0x188319 (WADDR=0x18 BADDR=0x2 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[4]:UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[4]:Q Type=0 ADDR=0x180319 (WADDR=0x18 BADDR=0x0 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[4]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[4]:Q Type=0 ADDR=0x58212 (WADDR=0x5 BADDR=0x2 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/reg_data_out[3]:Transmitter_0/FIFO_PRBS_0/reg_data_out[3]:Q Type=0 ADDR=0x138320 (WADDR=0x13 BADDR=0x2 PRBR=0x3 CLOFFSET=0x20)
ProbePoint: Name=Transmitter_0/prbs7_10_0/tx_count[0]:Transmitter_0/prbs7_10_0/tx_count[0]:Q Type=0 ADDR=0x11801E (WADDR=0x11 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1E)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[9]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[9]:Q Type=0 ADDR=0x80211 (WADDR=0x8 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[23]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[23]:Q Type=0 ADDR=0x100110 (WADDR=0x10 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[4]:Receiver_0/Downsampler_0/reg_data_out[4]:Q Type=0 ADDR=0x24011B (WADDR=0x24 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[9]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[9]:Q Type=0 ADDR=0xC0012 (WADDR=0xC BADDR=0x0 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[7]:Receiver_0/Downsampler_0/reg_check[7]:Q Type=0 ADDR=0x25011A (WADDR=0x25 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[16]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[16]:Q Type=0 ADDR=0x50111 (WADDR=0x5 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[5]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[5]:Q Type=0 ADDR=0x78012 (WADDR=0x7 BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[0]:Receiver_0/Downsampler_0/temp_data[0]:Q Type=0 ADDR=0x24801A (WADDR=0x24 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/state[0]:IGLOO2_Oversampling_0/CORECONFIGP_0/state[0]:Q Type=0 ADDR=0x30110 (WADDR=0x3 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[4]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[4]:Q Type=0 ADDR=0xA8010 (WADDR=0xA BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[17]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[17]:Q Type=0 ADDR=0x50211 (WADDR=0x5 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHWRITE:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHWRITE:Q Type=0 ADDR=0xA8211 (WADDR=0xA BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[11]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[11]:Q Type=0 ADDR=0x9800E (WADDR=0x9 BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[23]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[23]:Q Type=0 ADDR=0x8830D (WADDR=0x8 BADDR=0x2 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[4]:Q Type=0 ADDR=0x26801A (WADDR=0x26 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[27]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[27]:Q Type=0 ADDR=0x8020E (WADDR=0x8 BADDR=0x0 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[18]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[18]:Q Type=0 ADDR=0x28011C (WADDR=0x28 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[30]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[30]:Q Type=0 ADDR=0x128011 (WADDR=0x12 BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[2]:IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[2]:Q Type=0 ADDR=0xE8113 (WADDR=0xE BADDR=0x2 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[12]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[12]:Q Type=0 ADDR=0xC020D (WADDR=0xC BADDR=0x0 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHTRANS:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHTRANS:Q Type=0 ADDR=0xE0012 (WADDR=0xE BADDR=0x0 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/receive_full:UART_INTERFACE_0/COREUART_0/make_RX/receive_full_int:Q Type=0 ADDR=0x16821D (WADDR=0x16 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[21]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[21]:Q Type=0 ADDR=0x90010 (WADDR=0x9 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[15]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[15]:Q Type=0 ADDR=0x11830E (WADDR=0x11 BADDR=0x2 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[24]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[24]:Q Type=0 ADDR=0x1810F (WADDR=0x1 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[24]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[24]:Q Type=0 ADDR=0x2A011A (WADDR=0x2A BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[16]:UART_INTERFACE_0/FabUART_0/state[16]:Q Type=0 ADDR=0x19021A (WADDR=0x19 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[13]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[13]:Q Type=0 ADDR=0xA010F (WADDR=0xA BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[11]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[11]:Q Type=0 ADDR=0x2B0319 (WADDR=0x2B BADDR=0x0 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[12]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[12]:Q Type=0 ADDR=0x2800F (WADDR=0x2 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_val_debug:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_val_debug:Q Type=0 ADDR=0x298319 (WADDR=0x29 BADDR=0x2 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[27]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[27]:Q Type=0 ADDR=0x29821B (WADDR=0x29 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[28]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[28]:Q Type=0 ADDR=0x13000F (WADDR=0x13 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[22]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[22]:Q Type=0 ADDR=0xB0311 (WADDR=0xB BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[17]:UART_INTERFACE_0/FabUART_0/state[17]:Q Type=0 ADDR=0x1B021A (WADDR=0x1B BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[20]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[20]:Q Type=0 ADDR=0x29021A (WADDR=0x29 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/receive_count[2]:UART_INTERFACE_0/COREUART_0/make_RX/receive_count[2]:Q Type=0 ADDR=0x15011D (WADDR=0x15 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[18]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[18]:Q Type=0 ADDR=0x48211 (WADDR=0x4 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[29]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[29]:Q Type=0 ADDR=0x9010F (WADDR=0x9 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[9]:Q Type=0 ADDR=0x298318 (WADDR=0x29 BADDR=0x2 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[0]:Q Type=0 ADDR=0x260117 (WADDR=0x26 BADDR=0x0 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[4]:Q Type=0 ADDR=0x27021A (WADDR=0x27 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_bit_cnt[2]:UART_INTERFACE_0/COREUART_0/make_RX/rx_bit_cnt[2]:Q Type=0 ADDR=0x17021D (WADDR=0x17 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1D)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[7]:Q Type=0 ADDR=0x280117 (WADDR=0x28 BADDR=0x0 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[23]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[23]:Q Type=0 ADDR=0x100010 (WADDR=0x10 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[19]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[19]:Q Type=0 ADDR=0x28811A (WADDR=0x28 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[0]:Q Type=0 ADDR=0x298218 (WADDR=0x29 BADDR=0x2 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[28]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[28]:Q Type=0 ADDR=0x5830E (WADDR=0x5 BADDR=0x2 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[0]:Q Type=0 ADDR=0x270218 (WADDR=0x27 BADDR=0x0 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[4]:UART_INTERFACE_0/FabUART_0/state[4]:Q Type=0 ADDR=0x1B821A (WADDR=0x1B BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[10]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[10]:Q Type=0 ADDR=0x13811B (WADDR=0x13 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[2]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[2]:Q Type=0 ADDR=0xA810E (WADDR=0xA BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[21]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[21]:Q Type=0 ADDR=0x130210 (WADDR=0x13 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[6]:Q Type=0 ADDR=0x288119 (WADDR=0x28 BADDR=0x2 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[6]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[6]:Q Type=0 ADDR=0x110112 (WADDR=0x11 BADDR=0x0 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[17]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[17]:Q Type=0 ADDR=0x148010 (WADDR=0x14 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[10]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[10]:Q Type=0 ADDR=0xA830E (WADDR=0xA BADDR=0x2 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[0]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[0]:Q Type=0 ADDR=0xB000E (WADDR=0xB BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHSIZE[1]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHSIZE[1]:Q Type=0 ADDR=0xA8311 (WADDR=0xA BADDR=0x2 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/INIT_DONE_q1:IGLOO2_Oversampling_0/CORECONFIGP_0/INIT_DONE_q1:Q Type=0 ADDR=0x60312 (WADDR=0x6 BADDR=0x0 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[13]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[13]:Q Type=0 ADDR=0x13010E (WADDR=0x13 BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/Downsampler_0_error:Receiver_0/Downsampler_0/reg_error:Q Type=0 ADDR=0x27021B (WADDR=0x27 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/RESET_N_M2F_clk_base:IGLOO2_Oversampling_0/CORERESETP_0/RESET_N_M2F_clk_base:Q Type=0 ADDR=0x60111 (WADDR=0x6 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0_error_count[3]:Receiver_0/prbs7_10_0/reg_error[3]:Q Type=0 ADDR=0x1B001B (WADDR=0x1B BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[8]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[8]:Q Type=0 ADDR=0xA830F (WADDR=0xA BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[2]:UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[2]:Q Type=0 ADDR=0x180219 (WADDR=0x18 BADDR=0x0 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/DA_FSM_STATE[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/DA_FSM_STATE[0]:Q Type=0 ADDR=0x250019 (WADDR=0x25 BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[14]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[14]:Q Type=0 ADDR=0xC820D (WADDR=0xC BADDR=0x2 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[7]:Transmitter_0/prbs7_10_0/LFSR[8]:Q Type=0 ADDR=0x12811F (WADDR=0x12 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1F)
ProbePoint: Name=RX_c:RX_ibuf/U0/U_IOIN:Y:qr<1> Type=1 ADDR=0x110300 (WADDR=0x11 BADDR=0x0 PRBR=0x3 CLOFFSET=0x0)
ProbePoint: Name=RX_c:RX_ibuf/U0/U_IOIN:Y:qf<1> Type=1 ADDR=0x110700 (WADDR=0x11 BADDR=0x0 PRBR=0x7 CLOFFSET=0x0)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[19]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[19]:Q Type=0 ADDR=0x2B821A (WADDR=0x2B BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[12]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[12]:Q Type=0 ADDR=0x6030E (WADDR=0x6 BADDR=0x0 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[20]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[20]:Q Type=0 ADDR=0x108311 (WADDR=0x10 BADDR=0x2 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/prbs7_10_0/lock_count[1]:Receiver_0/prbs7_10_0/lock_count[1]:Q Type=0 ADDR=0x22011B (WADDR=0x22 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[5]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[5]:Q Type=0 ADDR=0x11000D (WADDR=0x11 BADDR=0x0 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[27]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[27]:Q Type=0 ADDR=0x12030F (WADDR=0x12 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0_error_count[2]:Receiver_0/prbs7_10_0/reg_error[2]:Q Type=0 ADDR=0x1B831B (WADDR=0x1B BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[1]:Transmitter_0/Replicator_0/X[0]:Q Type=0 ADDR=0x13811F (WADDR=0x13 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[3]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[3]:Q Type=0 ADDR=0xE030D (WADDR=0xE BADDR=0x0 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[28]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[28]:Q Type=0 ADDR=0x29811B (WADDR=0x29 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/state[1]:IGLOO2_Oversampling_0/CORECONFIGP_0/state[1]:Q Type=0 ADDR=0x38010 (WADDR=0x3 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[9]:Q Type=0 ADDR=0x288117 (WADDR=0x28 BADDR=0x2 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[21]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[21]:Q Type=0 ADDR=0x120011 (WADDR=0x12 BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[25]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[25]:Q Type=0 ADDR=0x108010 (WADDR=0x10 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[15]:IGLOO2_Oversampling_0/ConfigMaster_0/state[15]:Q Type=0 ADDR=0xE000F (WADDR=0xE BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[8]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[8]:Q Type=0 ADDR=0x11830D (WADDR=0x11 BADDR=0x2 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[22]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[22]:Q Type=0 ADDR=0x270018 (WADDR=0x27 BADDR=0x0 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[18]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[18]:Q Type=0 ADDR=0x138310 (WADDR=0x13 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[7]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[7]:Q Type=0 ADDR=0x80212 (WADDR=0x8 BADDR=0x0 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_state[1]:UART_INTERFACE_0/COREUART_0/make_RX/rx_state[1]:Q Type=0 ADDR=0x15811D (WADDR=0x15 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[19]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[19]:Q Type=0 ADDR=0x8830F (WADDR=0x8 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[3]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[3]:Q Type=0 ADDR=0x178119 (WADDR=0x17 BADDR=0x2 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[12]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[12]:Q Type=0 ADDR=0x58210 (WADDR=0x5 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[5]:Q Type=0 ADDR=0x298317 (WADDR=0x29 BADDR=0x2 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/busy:IGLOO2_Oversampling_0/ConfigMaster_0/busy:Q Type=0 ADDR=0xF8212 (WADDR=0xF BADDR=0x2 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[23]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[23]:Q Type=0 ADDR=0x70312 (WADDR=0x7 BADDR=0x0 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[18]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[18]:Q Type=0 ADDR=0x158211 (WADDR=0x15 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[3]:Transmitter_0/prbs7_10_0/LFSR[4]:Q Type=0 ADDR=0x12801F (WADDR=0x12 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[8]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[8]:Q Type=0 ADDR=0x68213 (WADDR=0x6 BADDR=0x2 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/prbs7_10_0/lock_count[0]:Receiver_0/prbs7_10_0/lock_count[0]:Q Type=0 ADDR=0x22811B (WADDR=0x22 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[2]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[2]:Q Type=0 ADDR=0xE8112 (WADDR=0xE BADDR=0x2 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[3]:Q Type=0 ADDR=0x280118 (WADDR=0x28 BADDR=0x0 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[17]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[17]:Q Type=0 ADDR=0x150110 (WADDR=0x15 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[10]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[10]:Q Type=0 ADDR=0xA000E (WADDR=0xA BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[6]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[6]:Q Type=0 ADDR=0x15020F (WADDR=0x15 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/masterDataInProg[0]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/masterDataInProg[0]:Q Type=0 ADDR=0xC8311 (WADDR=0xC BADDR=0x2 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[9]:Q Type=0 ADDR=0x290219 (WADDR=0x29 BADDR=0x0 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[3]:Q Type=0 ADDR=0x29021C (WADDR=0x29 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[5]:Q Type=0 ADDR=0x278017 (WADDR=0x27 BADDR=0x2 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[15]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[15]:Q Type=0 ADDR=0xC830D (WADDR=0xC BADDR=0x2 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[16]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[16]:Q Type=0 ADDR=0x26031A (WADDR=0x26 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[2]:Q Type=0 ADDR=0x2B0318 (WADDR=0x2B BADDR=0x0 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[11]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[11]:Q Type=0 ADDR=0xA8210 (WADDR=0xA BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[10]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[10]:Q Type=0 ADDR=0x288219 (WADDR=0x28 BADDR=0x2 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[7]:Q Type=0 ADDR=0x290117 (WADDR=0x29 BADDR=0x0 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[2]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[2]:Q Type=0 ADDR=0x4000F (WADDR=0x4 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[9]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[9]:Q Type=0 ADDR=0x3010F (WADDR=0x3 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[8]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[8]:Q Type=0 ADDR=0x10800E (WADDR=0x10 BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[24]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[24]:Q Type=0 ADDR=0x7820E (WADDR=0x7 BADDR=0x2 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[7]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[7]:Q Type=0 ADDR=0x4800F (WADDR=0x4 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[1]:UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[1]:Q Type=0 ADDR=0x18011D (WADDR=0x18 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1D)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[1]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[1]:Q Type=0 ADDR=0x14801B (WADDR=0x14 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[4]:Q Type=0 ADDR=0x288318 (WADDR=0x28 BADDR=0x2 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[31]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[31]:Q Type=0 ADDR=0xC010F (WADDR=0xC BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[16]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[16]:Q Type=0 ADDR=0x26831A (WADDR=0x26 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[15]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[15]:Q Type=0 ADDR=0x7820D (WADDR=0x7 BADDR=0x2 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[26]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[26]:Q Type=0 ADDR=0x7000F (WADDR=0x7 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[19]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[19]:Q Type=0 ADDR=0x9800F (WADDR=0x9 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=connect_o_obuf/U0/DOUT1:connect_o_obuf/U0/U_IOTRI:DOUT:do_qf<2> Type=4 ADDR=0x31830B (WADDR=0x31 BADDR=0x2 PRBR=0x3 CLOFFSET=0xB)
ProbePoint: Name=connect_o_obuf/U0/DOUT1:connect_o_obuf/U0/U_IOTRI:DOUT:do_qsdr<2> Type=4 ADDR=0x31820B (WADDR=0x31 BADDR=0x2 PRBR=0x2 CLOFFSET=0xB)
ProbePoint: Name=connect_o_obuf/U0/EOUT1:connect_o_obuf/U0/U_IOTRI:EOUT:oe_qf<2> Type=4 ADDR=0x31010B (WADDR=0x31 BADDR=0x0 PRBR=0x1 CLOFFSET=0xB)
ProbePoint: Name=connect_o_obuf/U0/EOUT1:connect_o_obuf/U0/U_IOTRI:EOUT:oe_qsdr<2> Type=4 ADDR=0x31000B (WADDR=0x31 BADDR=0x0 PRBR=0x0 CLOFFSET=0xB)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[6]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[6]:Q Type=0 ADDR=0x78011 (WADDR=0x7 BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[12]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[12]:Q Type=0 ADDR=0x11010E (WADDR=0x11 BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_DATA_OUT[1]:UART_INTERFACE_0/COREUART_0/make_RX/rx_byte[1]:Q Type=0 ADDR=0x18011C (WADDR=0x18 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[2]:Q Type=0 ADDR=0x268117 (WADDR=0x26 BADDR=0x2 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[13]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[13]:Q Type=0 ADDR=0xD0011 (WADDR=0xD BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/receive_control_0/RX_VALIN_reg:Receiver_0/receive_buffer_top_0/receive_control_0/RX_VALIN_reg:Q Type=0 ADDR=0x2A0219 (WADDR=0x2A BADDR=0x0 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[14]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[14]:Q Type=0 ADDR=0x4830F (WADDR=0x4 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[0]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[0]:Q Type=0 ADDR=0xA010E (WADDR=0xA BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[31]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[31]:Q Type=0 ADDR=0x7800D (WADDR=0x7 BADDR=0x2 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[0]:IGLOO2_Oversampling_0/ConfigMaster_0/state[0]:Q Type=0 ADDR=0xD8010 (WADDR=0xD BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[13]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[13]:Q Type=0 ADDR=0xB830D (WADDR=0xB BADDR=0x2 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[4]:Q Type=0 ADDR=0x2A8019 (WADDR=0x2A BADDR=0x2 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[15]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[15]:Q Type=0 ADDR=0x2B8219 (WADDR=0x2B BADDR=0x2 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/envm_busy[0]:IGLOO2_Oversampling_0/ConfigMaster_0/envm_busy[0]:Q Type=0 ADDR=0xF8213 (WADDR=0xF BADDR=0x2 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[1]:Receiver_0/Downsampler_0/reg_data_out[1]:Q Type=0 ADDR=0x24831B (WADDR=0x24 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[4]:Transmitter_0/Replicator_0/X[3]:Q Type=0 ADDR=0x13001F (WADDR=0x13 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[3]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[3]:Q Type=0 ADDR=0xF0012 (WADDR=0xF BADDR=0x0 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[4]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[4]:Q Type=0 ADDR=0x80111 (WADDR=0x8 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/receive_count[1]:UART_INTERFACE_0/COREUART_0/make_RX/receive_count[1]:Q Type=0 ADDR=0x14811D (WADDR=0x14 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/mss_reset_state:IGLOO2_Oversampling_0/CORERESETP_0/mss_reset_state:Q Type=0 ADDR=0x60011 (WADDR=0x6 BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[8]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[8]:Q Type=0 ADDR=0x5820E (WADDR=0x5 BADDR=0x2 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0_uart_oen:UART_INTERFACE_0/FabUART_0/uart_oen_t:Q Type=0 ADDR=0x17831C (WADDR=0x17 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[3]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[3]:Q Type=0 ADDR=0x15830F (WADDR=0x15 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/mss_reset_select:IGLOO2_Oversampling_0/CORERESETP_0/mss_reset_select:Q Type=0 ADDR=0x68211 (WADDR=0x6 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[14]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[14]:Q Type=0 ADDR=0x4820F (WADDR=0x4 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0_EPCS_TX_DATA[2]:Transmitter_0/FIFO_PRBS_0/reg_data_out[2]:Q Type=0 ADDR=0x140120 (WADDR=0x14 BADDR=0x0 PRBR=0x1 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[5]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[5]:Q Type=0 ADDR=0xD810D (WADDR=0xD BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[2]:Q Type=0 ADDR=0x258217 (WADDR=0x25 BADDR=0x2 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/data_flag:UART_INTERFACE_0/FabUART_0/data_flag:Q Type=0 ADDR=0x19811B (WADDR=0x19 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[1]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[1]:Q Type=0 ADDR=0x14020F (WADDR=0x14 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[14]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[14]:Q Type=0 ADDR=0x2A811A (WADDR=0x2A BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[7]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[7]:Q Type=0 ADDR=0x4810F (WADDR=0x4 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[9]:Q Type=0 ADDR=0x28031B (WADDR=0x28 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[5]:UART_INTERFACE_0/FabUART_0/state[5]:Q Type=0 ADDR=0x1B831A (WADDR=0x1B BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[6]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[6]:Q Type=0 ADDR=0x9810E (WADDR=0x9 BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[9]:Q Type=0 ADDR=0x290317 (WADDR=0x29 BADDR=0x0 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[31]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[31]:Q Type=0 ADDR=0x12030D (WADDR=0x12 BADDR=0x0 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[26]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[26]:Q Type=0 ADDR=0x7010F (WADDR=0x7 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[30]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[30]:Q Type=0 ADDR=0x128111 (WADDR=0x12 BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[2]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[2]:Q Type=0 ADDR=0x70013 (WADDR=0x7 BADDR=0x0 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PREADY:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PREADY:Q Type=0 ADDR=0x30010 (WADDR=0x3 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[24]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[24]:Q Type=0 ADDR=0x11810F (WADDR=0x11 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[9]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[9]:Q Type=0 ADDR=0x7800C (WADDR=0x7 BADDR=0x2 PRBR=0x0 CLOFFSET=0xC)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[4]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[4]:Q Type=0 ADDR=0xD800D (WADDR=0xD BADDR=0x2 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[27]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[27]:Q Type=0 ADDR=0x2B801A (WADDR=0x2B BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[1]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[1]:Q Type=0 ADDR=0xB0110 (WADDR=0xB BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0_genrate_err:UART_INTERFACE_0/FabUART_0/genrate_err_t:Q Type=0 ADDR=0x1A011C (WADDR=0x1A BADDR=0x0 PRBR=0x1 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[1]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[1]:Q Type=0 ADDR=0x9030C (WADDR=0x9 BADDR=0x0 PRBR=0x3 CLOFFSET=0xC)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[4]:Q Type=0 ADDR=0x2A8219 (WADDR=0x2A BADDR=0x2 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[29]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[29]:Q Type=0 ADDR=0x2B031B (WADDR=0x2B BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[10]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[10]:Q Type=0 ADDR=0x258119 (WADDR=0x25 BADDR=0x2 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[18]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[18]:Q Type=0 ADDR=0x90210 (WADDR=0x9 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[20]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[20]:Q Type=0 ADDR=0x29001A (WADDR=0x29 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[27]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[27]:Q Type=0 ADDR=0x2B8119 (WADDR=0x2B BADDR=0x2 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[2]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[2]:Q Type=0 ADDR=0x14811B (WADDR=0x14 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_bit_cnt[1]:UART_INTERFACE_0/COREUART_0/make_RX/rx_bit_cnt[1]:Q Type=0 ADDR=0x16001D (WADDR=0x16 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[3]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[3]:Q Type=0 ADDR=0x6010F (WADDR=0x6 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_DATA_OUT[5]:UART_INTERFACE_0/COREUART_0/make_RX/rx_byte[5]:Q Type=0 ADDR=0x18821C (WADDR=0x18 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[26]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[26]:Q Type=0 ADDR=0x2B021B (WADDR=0x2B BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/release_sdif0_core:IGLOO2_Oversampling_0/CORERESETP_0/release_sdif0_core:Q Type=0 ADDR=0x80113 (WADDR=0x8 BADDR=0x0 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[7]:Q Type=0 ADDR=0x268017 (WADDR=0x26 BADDR=0x2 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[7]:Q Type=0 ADDR=0x28801A (WADDR=0x28 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[37]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[37]:Q Type=0 ADDR=0x2C0119 (WADDR=0x2C BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[28]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[28]:Q Type=0 ADDR=0x13010F (WADDR=0x13 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[6]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[6]:Q Type=0 ADDR=0x14011B (WADDR=0x14 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[6]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[6]:Q Type=0 ADDR=0xA0310 (WADDR=0xA BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[24]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[24]:Q Type=0 ADDR=0x7000E (WADDR=0x7 BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[14]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[14]:Q Type=0 ADDR=0xA020F (WADDR=0xA BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[23]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[23]:Q Type=0 ADDR=0x1800F (WADDR=0x1 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[20]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[20]:Q Type=0 ADDR=0x100111 (WADDR=0x10 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[14]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[14]:Q Type=0 ADDR=0x10010F (WADDR=0x10 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[7]:Receiver_0/Downsampler_0/reg_data_out[7]:Q Type=0 ADDR=0x24011A (WADDR=0x24 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[19]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[19]:Q Type=0 ADDR=0x158311 (WADDR=0x15 BADDR=0x2 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[3]:IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[3]:Q Type=0 ADDR=0xE8013 (WADDR=0xE BADDR=0x2 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[28]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[28]:Q Type=0 ADDR=0x12810F (WADDR=0x12 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[9]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[9]:Q Type=0 ADDR=0xD010D (WADDR=0xD BADDR=0x0 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[6]:Q Type=0 ADDR=0x29031A (WADDR=0x29 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[23]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[23]:Q Type=0 ADDR=0x28011A (WADDR=0x28 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[13]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[13]:Q Type=0 ADDR=0x260218 (WADDR=0x26 BADDR=0x0 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[14]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[14]:Q Type=0 ADDR=0x25831A (WADDR=0x25 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[16]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[16]:Q Type=0 ADDR=0x6010D (WADDR=0x6 BADDR=0x0 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[3]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[3]:Q Type=0 ADDR=0x8820E (WADDR=0x8 BADDR=0x2 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[8]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[8]:Q Type=0 ADDR=0x7020F (WADDR=0x7 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[8]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[8]:Q Type=0 ADDR=0xD000D (WADDR=0xD BADDR=0x0 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[0]:UART_INTERFACE_0/FabUART_0/state[0]:Q Type=0 ADDR=0x1A021C (WADDR=0x1A BADDR=0x0 PRBR=0x2 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[18]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[18]:Q Type=0 ADDR=0x108011 (WADDR=0x10 BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[11]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[11]:Q Type=0 ADDR=0x60113 (WADDR=0x6 BADDR=0x0 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[25]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[25]:Q Type=0 ADDR=0x12010F (WADDR=0x12 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[17]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[17]:Q Type=0 ADDR=0x80310 (WADDR=0x8 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[7]:Receiver_0/Downsampler_0/temp_data[7]:Q Type=0 ADDR=0x248219 (WADDR=0x24 BADDR=0x2 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=CLK0_c:CLK0_ibuf/U0/U_IOIN:Y:qr<0> Type=4 ADDR=0x320213 (WADDR=0x32 BADDR=0x0 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=CLK0_c:CLK0_ibuf/U0/U_IOIN:Y:qf<0> Type=4 ADDR=0x320313 (WADDR=0x32 BADDR=0x0 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[15]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[15]:Q Type=0 ADDR=0x26021A (WADDR=0x26 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[0]:Q Type=0 ADDR=0x250217 (WADDR=0x25 BADDR=0x0 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0_enable_rcosc:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0_enable_rcosc:Q Type=0 ADDR=0x60313 (WADDR=0x6 BADDR=0x0 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/baud_clock:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_clock_int:Q Type=0 ADDR=0x15011B (WADDR=0x15 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[1]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[1]:Q Type=0 ADDR=0xF810D (WADDR=0xF BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[8]:UART_INTERFACE_0/FabUART_0/state[8]:Q Type=0 ADDR=0x1A011A (WADDR=0x1A BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[21]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[21]:Q Type=0 ADDR=0x28001A (WADDR=0x28 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[5]:Transmitter_0/FIFO_PRBS_0/data[3]:Q Type=0 ADDR=0x130020 (WADDR=0x13 BADDR=0x0 PRBR=0x0 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[4]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[4]:Q Type=0 ADDR=0xB0310 (WADDR=0xB BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[28]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[28]:Q Type=0 ADDR=0x2B8019 (WADDR=0x2B BADDR=0x2 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[6]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[6]:Q Type=0 ADDR=0x14000F (WADDR=0x14 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=TX_obuf/U0/DOUT1:TX_obuf/U0/U_IOTRI:DOUT:do_qf<3> Type=1 ADDR=0x100600 (WADDR=0x10 BADDR=0x0 PRBR=0x6 CLOFFSET=0x0)
ProbePoint: Name=TX_obuf/U0/DOUT1:TX_obuf/U0/U_IOTRI:DOUT:do_qsdr<3> Type=1 ADDR=0x100200 (WADDR=0x10 BADDR=0x0 PRBR=0x2 CLOFFSET=0x0)
ProbePoint: Name=TX_obuf/U0/EOUT1:TX_obuf/U0/U_IOTRI:EOUT:oe_qf<3> Type=1 ADDR=0x100700 (WADDR=0x10 BADDR=0x0 PRBR=0x7 CLOFFSET=0x0)
ProbePoint: Name=TX_obuf/U0/EOUT1:TX_obuf/U0/U_IOTRI:EOUT:oe_qsdr<3> Type=1 ADDR=0x100300 (WADDR=0x10 BADDR=0x0 PRBR=0x3 CLOFFSET=0x0)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[18]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[18]:Q Type=0 ADDR=0x108111 (WADDR=0x10 BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[31]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[31]:Q Type=0 ADDR=0x120211 (WADDR=0x12 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[27]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[27]:Q Type=0 ADDR=0x270318 (WADDR=0x27 BADDR=0x0 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[3]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[3]:Q Type=0 ADDR=0x14821B (WADDR=0x14 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[18]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[18]:Q Type=0 ADDR=0x110311 (WADDR=0x11 BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[17]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[17]:Q Type=0 ADDR=0x27011A (WADDR=0x27 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[5]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[5]:Q Type=0 ADDR=0x14001B (WADDR=0x14 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[8]:Q Type=0 ADDR=0x28021B (WADDR=0x28 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[19]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[19]:Q Type=0 ADDR=0xA8111 (WADDR=0xA BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[10]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[10]:Q Type=0 ADDR=0x58310 (WADDR=0x5 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[25]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[25]:Q Type=0 ADDR=0x9830F (WADDR=0x9 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[19]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[19]:Q Type=0 ADDR=0x90310 (WADDR=0x9 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[0]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[0]:Q Type=0 ADDR=0x148110 (WADDR=0x14 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[1]:Q Type=0 ADDR=0x290118 (WADDR=0x29 BADDR=0x0 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_DATA_OUT[3]:UART_INTERFACE_0/COREUART_0/make_RX/rx_byte[3]:Q Type=0 ADDR=0x18031C (WADDR=0x18 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[15]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[15]:Q Type=0 ADDR=0x2A821A (WADDR=0x2A BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/samples[1]:UART_INTERFACE_0/COREUART_0/make_RX/samples[1]:Q Type=0 ADDR=0x14801D (WADDR=0x14 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1D)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[10]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[10]:Q Type=0 ADDR=0x250318 (WADDR=0x25 BADDR=0x0 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[4]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[4]:Q Type=0 ADDR=0x12810D (WADDR=0x12 BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/receive_control_0/RX_VALIN_reg_d:Receiver_0/receive_buffer_top_0/receive_control_0/RX_VALIN_reg_d:Q Type=0 ADDR=0x2A0119 (WADDR=0x2A BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[24]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[24]:Q Type=0 ADDR=0x7810E (WADDR=0x7 BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[0]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[0]:Q Type=0 ADDR=0x6020D (WADDR=0x6 BADDR=0x0 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[15]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[15]:Q Type=0 ADDR=0x68012 (WADDR=0x6 BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[15]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[15]:Q Type=0 ADDR=0x11820D (WADDR=0x11 BADDR=0x2 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=TX_c:UART_INTERFACE_0/COREUART_0/make_TX/tx:Q Type=0 ADDR=0x17831A (WADDR=0x17 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/release_sdif0_core_clk_base:IGLOO2_Oversampling_0/CORERESETP_0/release_sdif0_core_clk_base:Q Type=0 ADDR=0x48313 (WADDR=0x4 BADDR=0x2 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[22]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[22]:Q Type=0 ADDR=0x28001C (WADDR=0x28 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[6]:Q Type=0 ADDR=0x258018 (WADDR=0x25 BADDR=0x2 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[11]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[11]:Q Type=0 ADDR=0x7800E (WADDR=0x7 BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/prbs7_10_0/LFSR[7]:Receiver_0/prbs7_10_0/LFSR[7]:Q Type=0 ADDR=0x23801A (WADDR=0x23 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[22]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[22]:Q Type=0 ADDR=0x8010F (WADDR=0x8 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[9]:Transmitter_0/Replicator_0/X[9]:Q Type=0 ADDR=0x13021F (WADDR=0x13 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[5]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[5]:Q Type=0 ADDR=0xA8110 (WADDR=0xA BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/CORECONFIGP_0_SOFT_RESET_F2M:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[1]:Q Type=0 ADDR=0x2830F (WADDR=0x2 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[9]:Receiver_0/Downsampler_0/reg_data_out[9]:Q Type=0 ADDR=0x24021A (WADDR=0x24 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[9]:Q Type=0 ADDR=0x250017 (WADDR=0x25 BADDR=0x0 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[5]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[5]:Q Type=0 ADDR=0x2810F (WADDR=0x2 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[7]:Q Type=0 ADDR=0x288019 (WADDR=0x28 BADDR=0x2 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[14]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[14]:Q Type=0 ADDR=0x100312 (WADDR=0x10 BADDR=0x0 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[24]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[24]:Q Type=0 ADDR=0x6000E (WADDR=0x6 BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/trans_detect_bit3:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/trans_detect_bit3:Q Type=0 ADDR=0x2A0018 (WADDR=0x2A BADDR=0x0 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[17]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[17]:Q Type=0 ADDR=0x26821B (WADDR=0x26 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[16]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[16]:Q Type=0 ADDR=0x6820E (WADDR=0x6 BADDR=0x2 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[18]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[18]:Q Type=0 ADDR=0x108211 (WADDR=0x10 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[3]:Q Type=0 ADDR=0x29021B (WADDR=0x29 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[1]:Q Type=0 ADDR=0x280217 (WADDR=0x28 BADDR=0x0 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[21]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[21]:Q Type=0 ADDR=0x70112 (WADDR=0x7 BADDR=0x0 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[6]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[6]:Q Type=0 ADDR=0x60010 (WADDR=0x6 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[22]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[22]:Q Type=0 ADDR=0x13020F (WADDR=0x13 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[10]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[10]:Q Type=0 ADDR=0x250018 (WADDR=0x25 BADDR=0x0 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[10]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[10]:Q Type=0 ADDR=0x10830D (WADDR=0x10 BADDR=0x2 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[19]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[19]:Q Type=0 ADDR=0x8800E (WADDR=0x8 BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[0]:Q Type=0 ADDR=0x268318 (WADDR=0x26 BADDR=0x2 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/sdif0_state[1]:IGLOO2_Oversampling_0/CORERESETP_0/sdif0_state[1]:Q Type=0 ADDR=0x50113 (WADDR=0x5 BADDR=0x0 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[3]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[3]:Q Type=0 ADDR=0xD0211 (WADDR=0xD BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterRegAddrSel:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/masterRegAddrSel:Q Type=0 ADDR=0xE0212 (WADDR=0xE BADDR=0x0 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0_uart_data_out[3]:UART_INTERFACE_0/FabUART_0/uart_data_out_t[3]:Q Type=0 ADDR=0x1B011A (WADDR=0x1B BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[1]:UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[1]:Q Type=0 ADDR=0x180019 (WADDR=0x18 BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[7]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[7]:Q Type=0 ADDR=0x6820F (WADDR=0x6 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[1]:UART_INTERFACE_0/FabUART_0/state[1]:Q Type=0 ADDR=0x19831B (WADDR=0x19 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0_CONFIG_DONE:IGLOO2_Oversampling_0/CORECONFIGP_0/control_reg_1:Q Type=0 ADDR=0x30211 (WADDR=0x3 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[5]:Receiver_0/Downsampler_0/temp_data[5]:Q Type=0 ADDR=0x24801B (WADDR=0x24 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[23]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[23]:Q Type=0 ADDR=0x80110 (WADDR=0x8 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[12]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[12]:Q Type=0 ADDR=0x11020E (WADDR=0x11 BADDR=0x0 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[11]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[11]:Q Type=0 ADDR=0x14810F (WADDR=0x14 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[15]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[15]:Q Type=0 ADDR=0x11800D (WADDR=0x11 BADDR=0x2 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[3]:Q Type=0 ADDR=0x258117 (WADDR=0x25 BADDR=0x2 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[25]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[25]:Q Type=0 ADDR=0x48011 (WADDR=0x4 BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[18]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[18]:Q Type=0 ADDR=0x2A831A (WADDR=0x2A BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[2]:Receiver_0/Downsampler_0/temp_data[2]:Q Type=0 ADDR=0x29831A (WADDR=0x29 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[16]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[16]:Q Type=0 ADDR=0x138110 (WADDR=0x13 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/prbs7_10_0/LFSR[5]:Receiver_0/prbs7_10_0/LFSR[5]:Q Type=0 ADDR=0x23831B (WADDR=0x23 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[9]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[9]:Q Type=0 ADDR=0xB020E (WADDR=0xB BADDR=0x0 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[7]:Q Type=0 ADDR=0x28031A (WADDR=0x28 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0_error_count[5]:Receiver_0/prbs7_10_0/reg_error[5]:Q Type=0 ADDR=0x1B021B (WADDR=0x1B BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_val:Receiver_0/Downsampler_0/temp_val:Q Type=0 ADDR=0x24831A (WADDR=0x24 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[12]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[12]:Q Type=0 ADDR=0xC800D (WADDR=0xC BADDR=0x2 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[29]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[29]:Q Type=0 ADDR=0x118111 (WADDR=0x11 BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[30]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[30]:Q Type=0 ADDR=0x128211 (WADDR=0x12 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[29]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[29]:Q Type=0 ADDR=0xE0312 (WADDR=0xE BADDR=0x0 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_bit_cnt[0]:UART_INTERFACE_0/COREUART_0/make_RX/rx_bit_cnt[0]:Q Type=0 ADDR=0x16011D (WADDR=0x16 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[7]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[7]:Q Type=0 ADDR=0x10800D (WADDR=0x10 BADDR=0x2 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[18]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[18]:Q Type=0 ADDR=0x280219 (WADDR=0x28 BADDR=0x0 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[1]:Receiver_0/Downsampler_0/temp_data[1]:Q Type=0 ADDR=0x24811B (WADDR=0x24 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[6]:Q Type=0 ADDR=0x2A0017 (WADDR=0x2A BADDR=0x0 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[8]:Q Type=0 ADDR=0x250317 (WADDR=0x25 BADDR=0x0 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[20]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[20]:Q Type=0 ADDR=0x5820D (WADDR=0x5 BADDR=0x2 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[3]:Q Type=0 ADDR=0x258317 (WADDR=0x25 BADDR=0x2 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[31]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[31]:Q Type=0 ADDR=0x98310 (WADDR=0x9 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=Transmitter_0_EPCS_TX_DATA[6]:Transmitter_0/FIFO_PRBS_0/reg_data_out[6]:Q Type=0 ADDR=0x140020 (WADDR=0x14 BADDR=0x0 PRBR=0x0 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[29]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[29]:Q Type=0 ADDR=0x12800F (WADDR=0x12 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[20]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[20]:Q Type=0 ADDR=0x9810F (WADDR=0x9 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[28]:Transmitter_0/Replicator_0/X[27]:Q Type=0 ADDR=0x118120 (WADDR=0x11 BADDR=0x2 PRBR=0x1 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[26]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[26]:Q Type=0 ADDR=0x60110 (WADDR=0x6 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[14]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[14]:Q Type=0 ADDR=0x68310 (WADDR=0x6 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/sdif0_state[0]:IGLOO2_Oversampling_0/CORERESETP_0/sdif0_state[0]:Q Type=0 ADDR=0x50313 (WADDR=0x5 BADDR=0x0 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[9]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[9]:Q Type=0 ADDR=0x12030E (WADDR=0x12 BADDR=0x0 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[15]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[15]:Q Type=0 ADDR=0x6000F (WADDR=0x6 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_CLEAR_ERRCNTR_o:Receiver_0/receive_buffer_top_0/receive_control_0/clear_errcnt_reg:Q Type=0 ADDR=0x1B801B (WADDR=0x1B BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[4]:UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[4]:Q Type=0 ADDR=0x18821D (WADDR=0x18 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[9]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[9]:Q Type=0 ADDR=0x10810D (WADDR=0x10 BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/cntr_2bit_en:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/cntr_2bit_en:Q Type=0 ADDR=0x258319 (WADDR=0x25 BADDR=0x2 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[14]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[14]:Q Type=0 ADDR=0x26821A (WADDR=0x26 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/envm_soft_reset[1]:IGLOO2_Oversampling_0/ConfigMaster_0/envm_soft_reset[1]:Q Type=0 ADDR=0xF0013 (WADDR=0xF BADDR=0x0 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[24]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[24]:Q Type=0 ADDR=0xB0211 (WADDR=0xB BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[29]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[29]:Q Type=0 ADDR=0x120210 (WADDR=0x12 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[18]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[18]:Q Type=0 ADDR=0x258218 (WADDR=0x25 BADDR=0x2 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/receive_control_0/RC_FSM_state[0]:Receiver_0/receive_buffer_top_0/receive_control_0/RC_FSM_state[0]:Q Type=0 ADDR=0x298019 (WADDR=0x29 BADDR=0x2 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[31]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[31]:Q Type=0 ADDR=0x88210 (WADDR=0x8 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[3]:UART_INTERFACE_0/FabUART_0/state[3]:Q Type=0 ADDR=0x19821A (WADDR=0x19 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[6]:Receiver_0/Downsampler_0/reg_data_out[6]:Q Type=0 ADDR=0x240119 (WADDR=0x24 BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[2]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[2]:Q Type=0 ADDR=0x58312 (WADDR=0x5 BADDR=0x2 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[3]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[3]:Q Type=0 ADDR=0x2820F (WADDR=0x2 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[2]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[2]:Q Type=0 ADDR=0x4010F (WADDR=0x4 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[13]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[13]:Q Type=0 ADDR=0x5020F (WADDR=0x5 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[13]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[13]:Q Type=0 ADDR=0x25001A (WADDR=0x25 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/enable_lock:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/enable_lock:Q Type=0 ADDR=0x2A0019 (WADDR=0x2A BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[26]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[26]:Q Type=0 ADDR=0x2A831B (WADDR=0x2A BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[9]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[9]:Q Type=0 ADDR=0x13801B (WADDR=0x13 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[3]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[3]:Q Type=0 ADDR=0x2010F (WADDR=0x2 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/FAB_RESET_N_int:IGLOO2_Oversampling_0/CORERESETP_0/FAB_RESET_N_int:Q Type=0 ADDR=0x68111 (WADDR=0x6 BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[19]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[19]:Q Type=0 ADDR=0x110211 (WADDR=0x11 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[17]:Transmitter_0/FIFO_PRBS_0/data[15]:Q Type=0 ADDR=0x130120 (WADDR=0x13 BADDR=0x0 PRBR=0x1 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[29]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[29]:Q Type=0 ADDR=0x48311 (WADDR=0x4 BADDR=0x2 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[1]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[1]:Q Type=0 ADDR=0x58010 (WADDR=0x5 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_cntr[0]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_cntr[0]:Q Type=0 ADDR=0x18031B (WADDR=0x18 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[9]:Transmitter_0/prbs7_10_0/LFSR[10]:Q Type=0 ADDR=0x11821F (WADDR=0x11 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[12]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[12]:Q Type=0 ADDR=0x5810E (WADDR=0x5 BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[2]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[2]:Q Type=0 ADDR=0x17821A (WADDR=0x17 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[7]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[7]:Q Type=0 ADDR=0xD830D (WADDR=0xD BADDR=0x2 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[14]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[14]:Q Type=0 ADDR=0xA0210 (WADDR=0xA BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[9]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[9]:Q Type=0 ADDR=0x3000F (WADDR=0x3 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[23]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[23]:Q Type=0 ADDR=0x2B011A (WADDR=0x2B BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[2]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[2]:Q Type=0 ADDR=0x100311 (WADDR=0x10 BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[21]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[21]:Q Type=0 ADDR=0x118011 (WADDR=0x11 BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[3]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[3]:Q Type=0 ADDR=0x58012 (WADDR=0x5 BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/enable_lock_dly:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/enable_lock_dly:Q Type=0 ADDR=0x250119 (WADDR=0x25 BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[1]:Receiver_0/Downsampler_0/reg_check[1]:Q Type=0 ADDR=0x29031B (WADDR=0x29 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[18]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[18]:Q Type=0 ADDR=0x80112 (WADDR=0x8 BADDR=0x0 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[3]:Q Type=0 ADDR=0x270317 (WADDR=0x27 BADDR=0x0 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[3]:UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[3]:Q Type=0 ADDR=0x18001D (WADDR=0x18 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[13]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[13]:Q Type=0 ADDR=0xC810D (WADDR=0xC BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[2]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[2]:Q Type=0 ADDR=0x12000D (WADDR=0x12 BADDR=0x0 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[8]:Q Type=0 ADDR=0x29801B (WADDR=0x29 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[23]:Transmitter_0/FIFO_PRBS_0/data[21]:Q Type=0 ADDR=0x138220 (WADDR=0x13 BADDR=0x2 PRBR=0x2 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[21]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[21]:Q Type=0 ADDR=0x50011 (WADDR=0x5 BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[27]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[27]:Q Type=0 ADDR=0x28011B (WADDR=0x28 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[4]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[4]:Q Type=0 ADDR=0x12820D (WADDR=0x12 BADDR=0x2 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[21]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[21]:Q Type=0 ADDR=0x27811B (WADDR=0x27 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[5]:Q Type=0 ADDR=0x27821A (WADDR=0x27 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/Error_Inject_i_delay2:Transmitter_0/FIFO_PRBS_0/Error_Inject_i_delay2:Q Type=0 ADDR=0x19011C (WADDR=0x19 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[20]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[20]:Q Type=0 ADDR=0x2A021A (WADDR=0x2A BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[11]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[11]:Q Type=0 ADDR=0x3820F (WADDR=0x3 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/tx_hold_reg[2]:UART_INTERFACE_0/COREUART_0/tx_hold_reg[2]:Q Type=0 ADDR=0x18001A (WADDR=0x18 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[31]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[31]:Q Type=0 ADDR=0x68212 (WADDR=0x6 BADDR=0x2 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[3]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[3]:Q Type=0 ADDR=0x80312 (WADDR=0x8 BADDR=0x0 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[15]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[15]:Q Type=0 ADDR=0x108212 (WADDR=0x10 BADDR=0x2 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[5]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[5]:Q Type=0 ADDR=0xA810F (WADDR=0xA BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/HADDR_fast[0]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR_fast[0]:Q Type=0 ADDR=0x158210 (WADDR=0x15 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[19]:IGLOO2_Oversampling_0/ConfigMaster_0/state[19]:Q Type=0 ADDR=0xF8012 (WADDR=0xF BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[0]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[0]:Q Type=0 ADDR=0x15031B (WADDR=0x15 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[16]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[16]:Q Type=0 ADDR=0x6800E (WADDR=0x6 BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[9]:Q Type=0 ADDR=0x260018 (WADDR=0x26 BADDR=0x0 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[4]:Receiver_0/Downsampler_0/temp_data[4]:Q Type=0 ADDR=0x24811A (WADDR=0x24 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[2]:Q Type=0 ADDR=0x278117 (WADDR=0x27 BADDR=0x2 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[6]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[6]:Q Type=0 ADDR=0x14830F (WADDR=0x14 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[22]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[22]:Q Type=0 ADDR=0x2B031A (WADDR=0x2B BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[13]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[13]:Q Type=0 ADDR=0x110012 (WADDR=0x11 BADDR=0x0 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[25]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[25]:Q Type=0 ADDR=0x108110 (WADDR=0x10 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[11]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[11]:Q Type=0 ADDR=0x11810E (WADDR=0x11 BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[16]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[16]:Q Type=0 ADDR=0x2B001A (WADDR=0x2B BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[19]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[19]:Q Type=0 ADDR=0x250118 (WADDR=0x25 BADDR=0x0 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[22]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[22]:Q Type=0 ADDR=0x8000F (WADDR=0x8 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[2]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[2]:Q Type=0 ADDR=0xB010F (WADDR=0xB BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[4]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[4]:Q Type=0 ADDR=0x12800D (WADDR=0x12 BADDR=0x2 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[10]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[10]:Q Type=0 ADDR=0xA800E (WADDR=0xA BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/stop_strobe:UART_INTERFACE_0/COREUART_0/make_RX/stop_strobe:Q Type=0 ADDR=0x15821D (WADDR=0x15 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[9]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[9]:Q Type=0 ADDR=0xA030E (WADDR=0xA BADDR=0x0 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/sm0_areset_n_rcosc:IGLOO2_Oversampling_0/CORERESETP_0/sm0_areset_n_rcosc:Q Type=0 ADDR=0x58213 (WADDR=0x5 BADDR=0x2 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[4]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[4]:Q Type=0 ADDR=0x5810D (WADDR=0x5 BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[25]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[25]:Q Type=0 ADDR=0x80210 (WADDR=0x8 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/i[1]:Transmitter_0/FIFO_PRBS_0/i[1]:Q Type=0 ADDR=0x128220 (WADDR=0x12 BADDR=0x2 PRBR=0x2 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/sm0_areset_n_q1:IGLOO2_Oversampling_0/CORERESETP_0/sdif0_areset_n_q1:Q Type=0 ADDR=0x50112 (WADDR=0x5 BADDR=0x0 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[1]:Q Type=0 ADDR=0x28811B (WADDR=0x28 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[13]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[13]:Q Type=0 ADDR=0x26811A (WADDR=0x26 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[22]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[22]:Q Type=0 ADDR=0xC020F (WADDR=0xC BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[26]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[26]:Q Type=0 ADDR=0x100310 (WADDR=0x10 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[15]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[15]:Q Type=0 ADDR=0x11810D (WADDR=0x11 BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[8]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[8]:Q Type=0 ADDR=0x11030E (WADDR=0x11 BADDR=0x0 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[5]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[5]:Q Type=0 ADDR=0x11010D (WADDR=0x11 BADDR=0x0 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/mux_sel[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/mux_sel[2]:Q Type=0 ADDR=0x260119 (WADDR=0x26 BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[22]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[22]:Q Type=0 ADDR=0x13030F (WADDR=0x13 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[23]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[23]:Q Type=0 ADDR=0x9820F (WADDR=0x9 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[8]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[8]:Q Type=0 ADDR=0x60112 (WADDR=0x6 BADDR=0x0 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/sdif3_spll_lock_q1:IGLOO2_Oversampling_0/CORERESETP_0/sdif0_spll_lock_q1:Q Type=0 ADDR=0x48013 (WADDR=0x4 BADDR=0x2 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/prbs7_10_0/LFSR[3]:Receiver_0/prbs7_10_0/LFSR[3]:Q Type=0 ADDR=0x23821B (WADDR=0x23 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[16]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[16]:Q Type=0 ADDR=0x25821A (WADDR=0x25 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[19]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[19]:Q Type=0 ADDR=0x29811A (WADDR=0x29 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[13]:UART_INTERFACE_0/FabUART_0/state[13]:Q Type=0 ADDR=0x19031A (WADDR=0x19 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[28]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[28]:Q Type=0 ADDR=0x2A821B (WADDR=0x2A BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/count[0]:IGLOO2_Oversampling_0/ConfigMaster_0/count[0]:Q Type=0 ADDR=0xB8010 (WADDR=0xB BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[5]:Q Type=0 ADDR=0x27011B (WADDR=0x27 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[4]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[4]:Q Type=0 ADDR=0x14831B (WADDR=0x14 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[10]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[10]:Q Type=0 ADDR=0x60013 (WADDR=0x6 BADDR=0x0 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[30]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[30]:Q Type=0 ADDR=0x8000E (WADDR=0x8 BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[15]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[15]:Q Type=0 ADDR=0x1820F (WADDR=0x1 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[7]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[7]:Q Type=0 ADDR=0x68113 (WADDR=0x6 BADDR=0x2 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/defSlaveSMCurrentState:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/default_slave_sm/defSlaveSMCurrentState:Q Type=0 ADDR=0xC0211 (WADDR=0xC BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[16]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[16]:Q Type=0 ADDR=0xC8012 (WADDR=0xC BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[11]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[11]:Q Type=0 ADDR=0xC0212 (WADDR=0xC BADDR=0x0 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[1]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[1]:Q Type=0 ADDR=0x1C00F (WADDR=0x1 BADDR=0x3 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[0]:Receiver_0/Downsampler_0/reg_data_out[0]:Q Type=0 ADDR=0x23821A (WADDR=0x23 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/tx_hold_reg[3]:UART_INTERFACE_0/COREUART_0/tx_hold_reg[3]:Q Type=0 ADDR=0x18811A (WADDR=0x18 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[7]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[7]:Q Type=0 ADDR=0x12010E (WADDR=0x12 BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[11]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[11]:Q Type=0 ADDR=0x280317 (WADDR=0x28 BADDR=0x0 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[7]:UART_INTERFACE_0/FabUART_0/state[7]:Q Type=0 ADDR=0x1A001A (WADDR=0x1A BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[5]:Q Type=0 ADDR=0x27811A (WADDR=0x27 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[13]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[13]:Q Type=0 ADDR=0x26001A (WADDR=0x26 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[3]:Q Type=0 ADDR=0x258118 (WADDR=0x25 BADDR=0x2 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[5]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[5]:Q Type=0 ADDR=0x178019 (WADDR=0x17 BADDR=0x2 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[14]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[14]:Q Type=0 ADDR=0xE0211 (WADDR=0xE BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[12]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[12]:Q Type=0 ADDR=0x11020F (WADDR=0x11 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[22]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[22]:Q Type=0 ADDR=0x2B811A (WADDR=0x2B BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/prbs7_10_0_lock_again:Receiver_0/prbs7_10_0/reg_lock_again:Q Type=0 ADDR=0x298219 (WADDR=0x29 BADDR=0x2 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[22]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[22]:Q Type=0 ADDR=0x78112 (WADDR=0x7 BADDR=0x2 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[10]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[10]:Q Type=0 ADDR=0xE0011 (WADDR=0xE BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[5]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[5]:Q Type=0 ADDR=0xD810E (WADDR=0xD BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[1]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[1]:Q Type=0 ADDR=0x14030F (WADDR=0x14 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHSIZE[0]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHSIZE[0]:Q Type=0 ADDR=0xA0111 (WADDR=0xA BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/xmit_clock:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_clock:Q Type=0 ADDR=0x18011B (WADDR=0x18 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/sm0_areset_n_clk_base:IGLOO2_Oversampling_0/CORERESETP_0/sm0_areset_n_clk_base:Q Type=0 ADDR=0x50012 (WADDR=0x5 BADDR=0x0 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[12]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[12]:Q Type=0 ADDR=0x13831B (WADDR=0x13 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[32]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[32]:Q Type=0 ADDR=0x2B801B (WADDR=0x2B BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[12]:IGLOO2_Oversampling_0/ConfigMaster_0/state[12]:Q Type=0 ADDR=0xD0210 (WADDR=0xD BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[12]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[12]:Q Type=0 ADDR=0x28031C (WADDR=0x28 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[9]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[9]:Q Type=0 ADDR=0xE830D (WADDR=0xE BADDR=0x2 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[7]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[7]:Q Type=0 ADDR=0xC8112 (WADDR=0xC BADDR=0x2 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[14]:IGLOO2_Oversampling_0/ConfigMaster_0/state[14]:Q Type=0 ADDR=0xF8112 (WADDR=0xF BADDR=0x2 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_bit_sel[1]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_bit_sel[1]:Q Type=0 ADDR=0x188119 (WADDR=0x18 BADDR=0x2 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[25]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[25]:Q Type=0 ADDR=0xA8011 (WADDR=0xA BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[0]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[0]:Q Type=0 ADDR=0x17801A (WADDR=0x17 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[11]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[11]:Q Type=0 ADDR=0x268217 (WADDR=0x26 BADDR=0x2 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[1]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[1]:Q Type=0 ADDR=0xC8312 (WADDR=0xC BADDR=0x2 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[6]:Receiver_0/Downsampler_0/temp_data[6]:Q Type=0 ADDR=0x248119 (WADDR=0x24 BADDR=0x2 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[7]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[7]:Q Type=0 ADDR=0xE0111 (WADDR=0xE BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[14]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[14]:Q Type=0 ADDR=0xA820E (WADDR=0xA BADDR=0x2 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[23]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[23]:Q Type=0 ADDR=0xB0011 (WADDR=0xB BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[3]:Q Type=0 ADDR=0x280018 (WADDR=0x28 BADDR=0x0 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0_enable_q1:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0_enable_q1:Q Type=0 ADDR=0x58013 (WADDR=0x5 BADDR=0x2 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[27]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[27]:Q Type=0 ADDR=0xA0010 (WADDR=0xA BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[11]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[11]:Q Type=0 ADDR=0x280119 (WADDR=0x28 BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[13]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[13]:Q Type=0 ADDR=0x7010C (WADDR=0x7 BADDR=0x0 PRBR=0x1 CLOFFSET=0xC)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[6]:Q Type=0 ADDR=0x28831A (WADDR=0x28 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[17]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[17]:Q Type=0 ADDR=0x110212 (WADDR=0x11 BADDR=0x0 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/prbs7_10_0/LFSR[4]:Receiver_0/prbs7_10_0/LFSR[4]:Q Type=0 ADDR=0x23811A (WADDR=0x23 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[2]:Q Type=0 ADDR=0x28821B (WADDR=0x28 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[5]:Q Type=0 ADDR=0x2C031B (WADDR=0x2C BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[17]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[17]:Q Type=0 ADDR=0x8800C (WADDR=0x8 BADDR=0x2 PRBR=0x0 CLOFFSET=0xC)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[0]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[0]:Q Type=0 ADDR=0x40211 (WADDR=0x4 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[9]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[9]:Q Type=0 ADDR=0xB030E (WADDR=0xB BADDR=0x0 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[12]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[12]:Q Type=0 ADDR=0x2B0219 (WADDR=0x2B BADDR=0x0 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/sm0_areset_n_rcosc_q1:IGLOO2_Oversampling_0/CORERESETP_0/sdif0_areset_n_rcosc_q1:Q Type=0 ADDR=0x58113 (WADDR=0x5 BADDR=0x2 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/tx_hold_reg[5]:UART_INTERFACE_0/COREUART_0/tx_hold_reg[5]:Q Type=0 ADDR=0x18821A (WADDR=0x18 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[18]:IGLOO2_Oversampling_0/ConfigMaster_0/state[18]:Q Type=0 ADDR=0xF0112 (WADDR=0xF BADDR=0x0 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/INIT_DONE:IGLOO2_Oversampling_0/CORERESETP_0/init_done_clk_base:Q Type=0 ADDR=0x50213 (WADDR=0x5 BADDR=0x0 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[23]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[23]:Q Type=0 ADDR=0xC810F (WADDR=0xC BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/Error_Inject_i_delay1:Transmitter_0/FIFO_PRBS_0/Error_Inject_i_delay1:Q Type=0 ADDR=0x1A031C (WADDR=0x1A BADDR=0x0 PRBR=0x3 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[6]:Q Type=0 ADDR=0x27801B (WADDR=0x27 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[8]:Receiver_0/Downsampler_0/reg_data_out[8]:Q Type=0 ADDR=0x24021B (WADDR=0x24 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[19]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[19]:Q Type=0 ADDR=0x28811C (WADDR=0x28 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[19]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[19]:Q Type=0 ADDR=0x1C30F (WADDR=0x1 BADDR=0x3 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[16]:Transmitter_0/Replicator_0/X[15]:Q Type=0 ADDR=0x13031F (WADDR=0x13 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1F)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[10]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[10]:Q Type=0 ADDR=0x2A0218 (WADDR=0x2A BADDR=0x0 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[5]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[5]:Q Type=0 ADDR=0x70313 (WADDR=0x7 BADDR=0x0 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[12]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[12]:Q Type=0 ADDR=0x6020E (WADDR=0x6 BADDR=0x0 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[5]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[5]:Q Type=0 ADDR=0x98210 (WADDR=0x9 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[20]:Transmitter_0/FIFO_PRBS_0/data[18]:Q Type=0 ADDR=0x13821F (WADDR=0x13 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[26]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[26]:Q Type=0 ADDR=0xA0011 (WADDR=0xA BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[30]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[30]:Q Type=0 ADDR=0x130111 (WADDR=0x13 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[21]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[21]:Q Type=0 ADDR=0xA0211 (WADDR=0xA BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_bit_cnt[3]:UART_INTERFACE_0/COREUART_0/make_RX/rx_bit_cnt[3]:Q Type=0 ADDR=0x17031D (WADDR=0x17 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[9]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[9]:Q Type=0 ADDR=0x78312 (WADDR=0x7 BADDR=0x2 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[19]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[19]:Q Type=0 ADDR=0x110011 (WADDR=0x11 BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[18]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[18]:Q Type=0 ADDR=0x9010D (WADDR=0x9 BADDR=0x0 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[7]:IGLOO2_Oversampling_0/ConfigMaster_0/state[7]:Q Type=0 ADDR=0xC820F (WADDR=0xC BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[13]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[13]:Q Type=0 ADDR=0xB020F (WADDR=0xB BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[13]:Transmitter_0/Replicator_0/X[12]:Q Type=0 ADDR=0x118020 (WADDR=0x11 BADDR=0x2 PRBR=0x0 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[5]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[5]:Q Type=0 ADDR=0x2000F (WADDR=0x2 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0_uart_wen:UART_INTERFACE_0/FabUART_0/uart_wen_t:Q Type=0 ADDR=0x19031B (WADDR=0x19 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[28]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[28]:Q Type=0 ADDR=0x29031C (WADDR=0x29 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/release_sdif0_core_q1:IGLOO2_Oversampling_0/CORERESETP_0/release_sdif0_core_q1:Q Type=0 ADDR=0x48213 (WADDR=0x4 BADDR=0x2 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[13]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[13]:Q Type=0 ADDR=0x13000E (WADDR=0x13 BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[4]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[4]:Q Type=0 ADDR=0xF010D (WADDR=0xF BADDR=0x0 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[3]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[3]:Q Type=0 ADDR=0x15010F (WADDR=0x15 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWRITE:IGLOO2_Oversampling_0/ConfigMaster_0/HWRITE:Q Type=0 ADDR=0xB800F (WADDR=0xB BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[31]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[31]:Q Type=0 ADDR=0x130211 (WADDR=0x13 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[3]:IGLOO2_Oversampling_0/ConfigMaster_0/state[3]:Q Type=0 ADDR=0x11000F (WADDR=0x11 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[11]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[11]:Q Type=0 ADDR=0x3830F (WADDR=0x3 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[12]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[12]:Q Type=0 ADDR=0x6010E (WADDR=0x6 BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[21]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[21]:Q Type=0 ADDR=0x2B0119 (WADDR=0x2B BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/m0s16DataSel:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[16]:Q Type=0 ADDR=0xC0312 (WADDR=0xC BADDR=0x0 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[0]:Q Type=0 ADDR=0x28001B (WADDR=0x28 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[24]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[24]:Q Type=0 ADDR=0x128110 (WADDR=0x12 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[14]:UART_INTERFACE_0/FabUART_0/state[14]:Q Type=0 ADDR=0x18811B (WADDR=0x18 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[38]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[38]:Q Type=0 ADDR=0x2B811B (WADDR=0x2B BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[1]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[1]:Q Type=0 ADDR=0x78313 (WADDR=0x7 BADDR=0x2 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/receive_count[3]:UART_INTERFACE_0/COREUART_0/make_RX/receive_count[3]:Q Type=0 ADDR=0x15001D (WADDR=0x15 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[0]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[0]:Q Type=0 ADDR=0x100112 (WADDR=0x10 BADDR=0x0 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[11]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[11]:Q Type=0 ADDR=0xD0111 (WADDR=0xD BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[1]:Q Type=0 ADDR=0x2C0219 (WADDR=0x2C BADDR=0x0 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/tx_hold_reg[0]:UART_INTERFACE_0/COREUART_0/tx_hold_reg[0]:Q Type=0 ADDR=0x18831A (WADDR=0x18 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[31]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[31]:Q Type=0 ADDR=0x2C0319 (WADDR=0x2C BADDR=0x0 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=start_c:UART_INTERFACE_0/FabUART_0/start_t:Q Type=0 ADDR=0x19831C (WADDR=0x19 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[9]:Q Type=0 ADDR=0x29831B (WADDR=0x29 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[1]:Q Type=0 ADDR=0x260217 (WADDR=0x26 BADDR=0x0 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[26]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[26]:Q Type=0 ADDR=0x28801B (WADDR=0x28 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[27]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[27]:Q Type=0 ADDR=0xB0111 (WADDR=0xB BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[9]:UART_INTERFACE_0/FabUART_0/state[9]:Q Type=0 ADDR=0x1A011B (WADDR=0x1A BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[8]:Q Type=0 ADDR=0x280017 (WADDR=0x28 BADDR=0x0 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[28]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[28]:Q Type=0 ADDR=0x8030F (WADDR=0x8 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[7]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[7]:Q Type=0 ADDR=0x14021B (WADDR=0x14 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/Replicator_0_tx_val_out:Transmitter_0/Replicator_0/reg_tx_val_out:Q Type=0 ADDR=0x128120 (WADDR=0x12 BADDR=0x2 PRBR=0x1 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[0]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[0]:Q Type=0 ADDR=0x78213 (WADDR=0x7 BADDR=0x2 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[3]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[3]:Q Type=0 ADDR=0x100012 (WADDR=0x10 BADDR=0x0 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[13]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[13]:Q Type=0 ADDR=0xA020E (WADDR=0xA BADDR=0x0 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[17]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[17]:Q Type=0 ADDR=0x30210 (WADDR=0x3 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[11]:UART_INTERFACE_0/FabUART_0/state[11]:Q Type=0 ADDR=0x1A811A (WADDR=0x1A BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[8]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[8]:Q Type=0 ADDR=0x14031B (WADDR=0x14 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[0]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[0]:Q Type=0 ADDR=0xB010E (WADDR=0xB BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[1]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[1]:Q Type=0 ADDR=0x13810F (WADDR=0x13 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HTRANS[1]:IGLOO2_Oversampling_0/ConfigMaster_0/HTRANS_1[1]:Q Type=0 ADDR=0xE020F (WADDR=0xE BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[23]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[23]:Q Type=0 ADDR=0x29011A (WADDR=0x29 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[13]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[13]:Q Type=0 ADDR=0x5030F (WADDR=0x5 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[17]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[17]:Q Type=0 ADDR=0xA030F (WADDR=0xA BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0_EPCS_TX_DATA[4]:Transmitter_0/FIFO_PRBS_0/reg_data_out[4]:Q Type=0 ADDR=0x140220 (WADDR=0x14 BADDR=0x0 PRBR=0x2 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[0]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[0]:Q Type=0 ADDR=0x158310 (WADDR=0x15 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[6]:Q Type=0 ADDR=0x278218 (WADDR=0x27 BADDR=0x2 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[4]:IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[4]:Q Type=0 ADDR=0xF0313 (WADDR=0xF BADDR=0x0 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0_error_count[1]:Receiver_0/prbs7_10_0/reg_error[1]:Q Type=0 ADDR=0x1B821B (WADDR=0x1B BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_RXRDY:UART_INTERFACE_0/COREUART_0/genblk1_RXRDY:Q Type=0 ADDR=0x16811D (WADDR=0x16 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[0]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[0]:Q Type=0 ADDR=0x150010 (WADDR=0x15 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[6]:IGLOO2_Oversampling_0/ConfigMaster_0/state[6]:Q Type=0 ADDR=0xB820F (WADDR=0xB BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[7]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[7]:Q Type=0 ADDR=0x5830D (WADDR=0x5 BADDR=0x2 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[19]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[19]:Q Type=0 ADDR=0x68210 (WADDR=0x6 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[25]:Transmitter_0/Replicator_0/X[24]:Q Type=0 ADDR=0x120320 (WADDR=0x12 BADDR=0x0 PRBR=0x3 CLOFFSET=0x20)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[8]:Q Type=0 ADDR=0x2C021B (WADDR=0x2C BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[9]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[9]:Q Type=0 ADDR=0x10820D (WADDR=0x10 BADDR=0x2 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[7]:Q Type=0 ADDR=0x260118 (WADDR=0x26 BADDR=0x0 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[20]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[20]:Q Type=0 ADDR=0x130110 (WADDR=0x13 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[12]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[12]:Q Type=0 ADDR=0x25801A (WADDR=0x25 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[5]:Receiver_0/Downsampler_0/reg_data_out[5]:Q Type=0 ADDR=0x24001B (WADDR=0x24 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[5]:Q Type=0 ADDR=0x288218 (WADDR=0x28 BADDR=0x2 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[10]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[10]:Q Type=0 ADDR=0xD020D (WADDR=0xD BADDR=0x0 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[20]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[20]:Q Type=0 ADDR=0x40311 (WADDR=0x4 BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[21]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[21]:Q Type=0 ADDR=0x2A001A (WADDR=0x2A BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[3]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[3]:Q Type=0 ADDR=0x12810E (WADDR=0x12 BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[15]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[15]:Q Type=0 ADDR=0xB810D (WADDR=0xB BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[25]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[25]:Q Type=0 ADDR=0x2A801B (WADDR=0x2A BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[7]:Transmitter_0/Replicator_0/X[6]:Q Type=0 ADDR=0x120020 (WADDR=0x12 BADDR=0x0 PRBR=0x0 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[27]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[27]:Q Type=0 ADDR=0x10000F (WADDR=0x10 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[2]:UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[2]:Q Type=0 ADDR=0x18031D (WADDR=0x18 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1D)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[2]:Q Type=0 ADDR=0x2C011B (WADDR=0x2C BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[6]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[6]:Q Type=0 ADDR=0x9010E (WADDR=0x9 BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[19]:Transmitter_0/Replicator_0/X[18]:Q Type=0 ADDR=0x13831F (WADDR=0x13 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[15]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[15]:Q Type=0 ADDR=0x28010 (WADDR=0x2 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[0]:UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[0]:Q Type=0 ADDR=0x17801D (WADDR=0x17 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1D)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[0]:Receiver_0/Downsampler_0/reg_check[0]:Q Type=0 ADDR=0x28831B (WADDR=0x28 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[6]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[6]:Q Type=0 ADDR=0xA820F (WADDR=0xA BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[1]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[1]:Q Type=0 ADDR=0xB030F (WADDR=0xB BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/POWER_ON_RESET_N_q1:IGLOO2_Oversampling_0/CORERESETP_0/POWER_ON_RESET_N_q1:Q Type=0 ADDR=0x70210 (WADDR=0x7 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[0]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[0]:Q Type=0 ADDR=0xF800E (WADDR=0xF BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[27]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[27]:Q Type=0 ADDR=0x120010 (WADDR=0x12 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[7]:Q Type=0 ADDR=0x2C0019 (WADDR=0x2C BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[8]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[8]:Q Type=0 ADDR=0xB000F (WADDR=0xB BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[22]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[22]:Q Type=0 ADDR=0x290119 (WADDR=0x29 BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[20]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[20]:Q Type=0 ADDR=0x68010 (WADDR=0x6 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0_lock:Receiver_0/prbs7_10_0/reg_lock:Q Type=0 ADDR=0x22831B (WADDR=0x22 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[23]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[23]:Q Type=0 ADDR=0x110310 (WADDR=0x11 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[30]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[30]:Q Type=0 ADDR=0xE0112 (WADDR=0xE BADDR=0x0 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[7]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[7]:Q Type=0 ADDR=0x6810F (WADDR=0x6 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[2]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[2]:Q Type=0 ADDR=0x9000D (WADDR=0x9 BADDR=0x0 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[28]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[28]:Q Type=0 ADDR=0x7800F (WADDR=0x7 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[2]:Transmitter_0/FIFO_PRBS_0/data[0]:Q Type=0 ADDR=0x14031F (WADDR=0x14 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[25]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[25]:Q Type=0 ADDR=0x60212 (WADDR=0x6 BADDR=0x0 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[0]:Q Type=0 ADDR=0x258017 (WADDR=0x25 BADDR=0x2 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[26]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[26]:Q Type=0 ADDR=0x288118 (WADDR=0x28 BADDR=0x2 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[8]:Transmitter_0/prbs7_10_0/LFSR[9]:Q Type=0 ADDR=0x11801F (WADDR=0x11 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1F)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[20]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[20]:Q Type=0 ADDR=0x258318 (WADDR=0x25 BADDR=0x2 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[6]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[6]:Q Type=0 ADDR=0xD820D (WADDR=0xD BADDR=0x2 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_DATA_OUT[4]:UART_INTERFACE_0/COREUART_0/make_RX/rx_byte[4]:Q Type=0 ADDR=0x18811C (WADDR=0x18 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0_error_count[0]:Receiver_0/prbs7_10_0/reg_error[0]:Q Type=0 ADDR=0x1B811B (WADDR=0x1B BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[1]:Transmitter_0/prbs7_10_0/LFSR[2]:Q Type=0 ADDR=0x12831F (WADDR=0x12 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[9]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[9]:Q Type=0 ADDR=0x10030D (WADDR=0x10 BADDR=0x0 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[5]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[5]:Q Type=0 ADDR=0x108012 (WADDR=0x10 BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/tx_hold_reg[1]:UART_INTERFACE_0/COREUART_0/tx_hold_reg[1]:Q Type=0 ADDR=0x18801A (WADDR=0x18 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[2]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[2]:Q Type=0 ADDR=0x13030E (WADDR=0x13 BADDR=0x0 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[30]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[30]:Q Type=0 ADDR=0x7820F (WADDR=0x7 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[26]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[26]:Q Type=0 ADDR=0x2B831A (WADDR=0x2B BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[8]:Q Type=0 ADDR=0x278317 (WADDR=0x27 BADDR=0x2 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/ddr_ready_clk_base:IGLOO2_Oversampling_0/CORERESETP_0/ddr_ready_clk_base:Q Type=0 ADDR=0x40013 (WADDR=0x4 BADDR=0x0 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[7]:UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[7]:Q Type=0 ADDR=0x17821D (WADDR=0x17 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1D)
ProbePoint: Name=Receiver_0/prbs7_10_0/LFSR[2]:Receiver_0/prbs7_10_0/LFSR[2]:Q Type=0 ADDR=0x24031B (WADDR=0x24 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0_uart_data_out[5]:UART_INTERFACE_0/FabUART_0/uart_data_out_t[5]:Q Type=0 ADDR=0x1A821A (WADDR=0x1A BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0_error_out:Receiver_0/prbs7_10_0/reg_error_out:Q Type=0 ADDR=0x1B031B (WADDR=0x1B BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/mux_sel[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/mux_sel[1]:Q Type=0 ADDR=0x260319 (WADDR=0x26 BADDR=0x0 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[23]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[23]:Q Type=0 ADDR=0x128010 (WADDR=0x12 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[12]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[12]:Q Type=0 ADDR=0x60213 (WADDR=0x6 BADDR=0x0 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[4]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[4]:Q Type=0 ADDR=0x5000F (WADDR=0x5 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[20]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[20]:Q Type=0 ADDR=0x100011 (WADDR=0x10 BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[0]:Q Type=0 ADDR=0x28821C (WADDR=0x28 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[7]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[7]:Q Type=0 ADDR=0x11020D (WADDR=0x11 BADDR=0x0 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[36]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[36]:Q Type=0 ADDR=0x2C021A (WADDR=0x2C BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[7]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[7]:Q Type=0 ADDR=0x6800F (WADDR=0x6 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[3]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[3]:Q Type=0 ADDR=0x6020F (WADDR=0x6 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/count[1]:IGLOO2_Oversampling_0/ConfigMaster_0/count[1]:Q Type=0 ADDR=0xC0310 (WADDR=0xC BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[2]:IGLOO2_Oversampling_0/ConfigMaster_0/state[2]:Q Type=0 ADDR=0x10020F (WADDR=0x10 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[0]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[0]:Q Type=0 ADDR=0x58112 (WADDR=0x5 BADDR=0x2 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/baud_cntr[11]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/genblk1_baud_cntr[11]:Q Type=0 ADDR=0x13821B (WADDR=0x13 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/RB_LOCK_o:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/lock_gen:Q Type=0 ADDR=0x260019 (WADDR=0x26 BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0_uart_data_out[0]:UART_INTERFACE_0/FabUART_0/uart_data_out_t[0]:Q Type=0 ADDR=0x1B001A (WADDR=0x1B BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[8]:Receiver_0/Downsampler_0/reg_check[8]:Q Type=0 ADDR=0x288018 (WADDR=0x28 BADDR=0x2 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[2]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[2]:Q Type=0 ADDR=0x58110 (WADDR=0x5 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0_uart_data_out[2]:UART_INTERFACE_0/FabUART_0/uart_data_out_t[2]:Q Type=0 ADDR=0x1A021A (WADDR=0x1A BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/receive_control_0/RC_FSM_state[1]:Receiver_0/receive_buffer_top_0/receive_control_0/RC_FSM_state[1]:Q Type=0 ADDR=0x2A0319 (WADDR=0x2A BADDR=0x0 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWRITE:IGLOO2_Oversampling_0/CORECONFIGP_0/pwrite:Q Type=0 ADDR=0x30310 (WADDR=0x3 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[25]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[25]:Q Type=0 ADDR=0x2B011B (WADDR=0x2B BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/RESET_N_M2F_q1:IGLOO2_Oversampling_0/CORERESETP_0/RESET_N_M2F_q1:Q Type=0 ADDR=0x60211 (WADDR=0x6 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[10]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[10]:Q Type=0 ADDR=0x10010D (WADDR=0x10 BADDR=0x0 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[27]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[27]:Q Type=0 ADDR=0x9000F (WADDR=0x9 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0_uart_data_out[1]:UART_INTERFACE_0/FabUART_0/uart_data_out_t[1]:Q Type=0 ADDR=0x1A031A (WADDR=0x1A BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[25]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[25]:Q Type=0 ADDR=0x7810C (WADDR=0x7 BADDR=0x2 PRBR=0x1 CLOFFSET=0xC)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/cntr_2bit_zero:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/cntr_2bit_zero:Q Type=0 ADDR=0x230019 (WADDR=0x23 BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[1]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[1]:Q Type=0 ADDR=0xE8312 (WADDR=0xE BADDR=0x2 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[26]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[26]:Q Type=0 ADDR=0x110110 (WADDR=0x11 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[18]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[18]:Q Type=0 ADDR=0xB0210 (WADDR=0xB BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[35]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[35]:Q Type=0 ADDR=0x2B001B (WADDR=0x2B BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[6]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[6]:Q Type=0 ADDR=0x3020F (WADDR=0x3 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[8]:Q Type=0 ADDR=0x2A8317 (WADDR=0x2A BADDR=0x2 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[25]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[25]:Q Type=0 ADDR=0x128210 (WADDR=0x12 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[6]:UART_INTERFACE_0/FabUART_0/state[6]:Q Type=0 ADDR=0x19001B (WADDR=0x19 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[6]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[6]:Q Type=0 ADDR=0x68013 (WADDR=0x6 BADDR=0x2 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[4]:Q Type=0 ADDR=0x29011B (WADDR=0x29 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_cntr[1]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_cntr[1]:Q Type=0 ADDR=0x18821B (WADDR=0x18 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[9]:Transmitter_0/FIFO_PRBS_0/data[9]:Q Type=0 ADDR=0x13011F (WADDR=0x13 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[31]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[31]:Q Type=0 ADDR=0x48111 (WADDR=0x4 BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[24]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[24]:Q Type=0 ADDR=0x29011C (WADDR=0x29 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1C)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[24]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[24]:Q Type=0 ADDR=0x2A801A (WADDR=0x2A BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[30]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[30]:Q Type=0 ADDR=0x7830E (WADDR=0x7 BADDR=0x2 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[5]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[5]:Q Type=0 ADDR=0x12830E (WADDR=0x12 BADDR=0x2 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/sdif3_spll_lock_q2:IGLOO2_Oversampling_0/CORERESETP_0/sdif0_spll_lock_q2:Q Type=0 ADDR=0x48113 (WADDR=0x4 BADDR=0x2 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[34]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[34]:Q Type=0 ADDR=0x2B831B (WADDR=0x2B BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[7]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[7]:Q Type=0 ADDR=0x60012 (WADDR=0x6 BADDR=0x0 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[15]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[15]:Q Type=0 ADDR=0x6830F (WADDR=0x6 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[17]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[17]:Q Type=0 ADDR=0x2B8319 (WADDR=0x2B BADDR=0x2 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[20]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[20]:Q Type=0 ADDR=0x27821B (WADDR=0x27 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[12]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[12]:Q Type=0 ADDR=0x70211 (WADDR=0x7 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[24]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[24]:Q Type=0 ADDR=0x110210 (WADDR=0x11 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/i[0]:Transmitter_0/FIFO_PRBS_0/i[0]:Q Type=0 ADDR=0x130320 (WADDR=0x13 BADDR=0x0 PRBR=0x3 CLOFFSET=0x20)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[7]:Q Type=0 ADDR=0x28021A (WADDR=0x28 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[24]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[24]:Q Type=0 ADDR=0x80311 (WADDR=0x8 BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[0]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[0]:Q Type=0 ADDR=0x138010 (WADDR=0x13 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[19]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[19]:Q Type=0 ADDR=0x130010 (WADDR=0x13 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[24]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[24]:Q Type=0 ADDR=0x110010 (WADDR=0x11 BADDR=0x0 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[17]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[17]:Q Type=0 ADDR=0x27001A (WADDR=0x27 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[11]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[11]:Q Type=0 ADDR=0x2A0118 (WADDR=0x2A BADDR=0x0 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/expected[18]:IGLOO2_Oversampling_0/ConfigMaster_0/expected[18]:Q Type=0 ADDR=0x98010 (WADDR=0x9 BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[7]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[7]:Q Type=0 ADDR=0x11030D (WADDR=0x11 BADDR=0x0 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[21]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[21]:Q Type=0 ADDR=0x120111 (WADDR=0x12 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[20]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[20]:Q Type=0 ADDR=0xC000F (WADDR=0xC BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HSIZE[1]:IGLOO2_Oversampling_0/ConfigMaster_0/HSIZE[1]:Q Type=0 ADDR=0xD030E (WADDR=0xD BADDR=0x0 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[2]:Receiver_0/Downsampler_0/reg_data_out[2]:Q Type=0 ADDR=0x29821A (WADDR=0x29 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[2]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[2]:Q Type=0 ADDR=0xF000D (WADDR=0xF BADDR=0x0 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[10]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[10]:Q Type=0 ADDR=0x250117 (WADDR=0x25 BADDR=0x0 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[2]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[2]:Q Type=0 ADDR=0x12010D (WADDR=0x12 BADDR=0x0 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[10]:UART_INTERFACE_0/FabUART_0/state[10]:Q Type=0 ADDR=0x1A001B (WADDR=0x1A BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[30]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[30]:Q Type=0 ADDR=0x28831C (WADDR=0x28 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[7]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[7]:Q Type=0 ADDR=0xD000E (WADDR=0xD BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/FIC_2_APB_M_PRESET_N_clk_base:IGLOO2_Oversampling_0/CORERESETP_0/FIC_2_APB_M_PRESET_N_clk_base:Q Type=0 ADDR=0x70311 (WADDR=0x7 BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=start_obuf/U0/DOUT1:start_obuf/U0/U_IOTRI:DOUT:do_qf<0> Type=4 ADDR=0x32410A (WADDR=0x32 BADDR=0x1 PRBR=0x1 CLOFFSET=0xA)
ProbePoint: Name=start_obuf/U0/DOUT1:start_obuf/U0/U_IOTRI:DOUT:do_qsdr<0> Type=4 ADDR=0x32400A (WADDR=0x32 BADDR=0x1 PRBR=0x0 CLOFFSET=0xA)
ProbePoint: Name=start_obuf/U0/EOUT1:start_obuf/U0/U_IOTRI:EOUT:oe_qf<0> Type=4 ADDR=0x32010A (WADDR=0x32 BADDR=0x0 PRBR=0x1 CLOFFSET=0xA)
ProbePoint: Name=start_obuf/U0/EOUT1:start_obuf/U0/U_IOTRI:EOUT:oe_qsdr<0> Type=4 ADDR=0x32000A (WADDR=0x32 BADDR=0x0 PRBR=0x0 CLOFFSET=0xA)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[0]:Q Type=0 ADDR=0x2A8118 (WADDR=0x2A BADDR=0x2 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[8]:Q Type=0 ADDR=0x2A021B (WADDR=0x2A BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[11]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[11]:Q Type=0 ADDR=0x15030F (WADDR=0x15 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[5]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[5]:Q Type=0 ADDR=0x78211 (WADDR=0x7 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[9]:Receiver_0/Downsampler_0/temp_data[9]:Q Type=0 ADDR=0x24821A (WADDR=0x24 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[29]:Transmitter_0/FIFO_PRBS_0/data[27]:Q Type=0 ADDR=0x120220 (WADDR=0x12 BADDR=0x0 PRBR=0x2 CLOFFSET=0x20)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[23]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[23]:Q Type=0 ADDR=0x2A031A (WADDR=0x2A BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[8]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[8]:Q Type=0 ADDR=0xE800D (WADDR=0xE BADDR=0x2 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/envm_busy[1]:IGLOO2_Oversampling_0/ConfigMaster_0/envm_busy[1]:Q Type=0 ADDR=0xF8113 (WADDR=0xF BADDR=0x2 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/Downsampler_0_data_out[3]:Receiver_0/Downsampler_0/reg_data_out[3]:Q Type=0 ADDR=0x24031A (WADDR=0x24 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[24]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[24]:Q Type=0 ADDR=0x290218 (WADDR=0x29 BADDR=0x0 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[3]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[3]:Q Type=0 ADDR=0x70113 (WADDR=0x7 BADDR=0x0 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[10]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[10]:Q Type=0 ADDR=0x10020D (WADDR=0x10 BADDR=0x0 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[28]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[28]:Q Type=0 ADDR=0x13830F (WADDR=0x13 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[14]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[14]:Q Type=0 ADDR=0x38210 (WADDR=0x3 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[5]:IGLOO2_Oversampling_0/ConfigMaster_0/state[5]:Q Type=0 ADDR=0xD8310 (WADDR=0xD BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[6]:Receiver_0/Downsampler_0/reg_check[6]:Q Type=0 ADDR=0x250218 (WADDR=0x25 BADDR=0x0 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[10]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[10]:Q Type=0 ADDR=0x4030F (WADDR=0x4 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[30]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[30]:Q Type=0 ADDR=0x68312 (WADDR=0x6 BADDR=0x2 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[33]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[33]:Q Type=0 ADDR=0x29001C (WADDR=0x29 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[10]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[10]:Q Type=0 ADDR=0x108312 (WADDR=0x10 BADDR=0x2 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[10]:IGLOO2_Oversampling_0/ConfigMaster_0/state[10]:Q Type=0 ADDR=0xD000F (WADDR=0xD BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[0]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[0]:Q Type=0 ADDR=0xE000D (WADDR=0xE BADDR=0x0 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[14]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[14]:Q Type=0 ADDR=0x7020E (WADDR=0x7 BADDR=0x0 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/CLR_INIT_DONE_q1:IGLOO2_Oversampling_0/CORERESETP_0/CLR_INIT_DONE_q1:Q Type=0 ADDR=0x40312 (WADDR=0x4 BADDR=0x0 PRBR=0x3 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[17]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[17]:Q Type=0 ADDR=0x26011A (WADDR=0x26 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/prbs7_10_0/rx_count[0]:Receiver_0/prbs7_10_0/rx_count[0]:Q Type=0 ADDR=0x23021B (WADDR=0x23 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[28]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[28]:Q Type=0 ADDR=0x78111 (WADDR=0x7 BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[25]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[25]:Q Type=0 ADDR=0x290318 (WADDR=0x29 BADDR=0x0 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[25]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[25]:Q Type=0 ADDR=0x108210 (WADDR=0x10 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[28]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[28]:Q Type=0 ADDR=0x120110 (WADDR=0x12 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[25]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[25]:Q Type=0 ADDR=0x2A011B (WADDR=0x2A BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[11]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[11]:Q Type=0 ADDR=0x68110 (WADDR=0x6 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[13]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[13]:Q Type=0 ADDR=0x70012 (WADDR=0x7 BADDR=0x0 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/Downsampler_0_rx_val_out:Receiver_0/Downsampler_0/reg_rx_val_out:Q Type=0 ADDR=0x24001A (WADDR=0x24 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[6]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[6]:Q Type=0 ADDR=0x3030F (WADDR=0x3 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[21]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[21]:Q Type=0 ADDR=0x90110 (WADDR=0x9 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[18]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[18]:Q Type=0 ADDR=0x28821A (WADDR=0x28 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[11]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[11]:Q Type=0 ADDR=0xD030D (WADDR=0xD BADDR=0x0 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[2]:Transmitter_0/prbs7_10_0/LFSR[3]:Q Type=0 ADDR=0x12031F (WADDR=0x12 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1F)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[3]:UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[3]:Q Type=0 ADDR=0x188219 (WADDR=0x18 BADDR=0x2 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[26]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[26]:Q Type=0 ADDR=0x9810D (WADDR=0x9 BADDR=0x2 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[8]:Transmitter_0/FIFO_PRBS_0/data[6]:Q Type=0 ADDR=0x128320 (WADDR=0x12 BADDR=0x2 PRBR=0x3 CLOFFSET=0x20)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[1]:Q Type=0 ADDR=0x2A0318 (WADDR=0x2A BADDR=0x0 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[6]:Q Type=0 ADDR=0x2C011A (WADDR=0x2C BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[0]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[0]:Q Type=0 ADDR=0x30111 (WADDR=0x3 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD2[1]:Q Type=0 ADDR=0x260317 (WADDR=0x26 BADDR=0x0 PRBR=0x3 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[11]:IGLOO2_Oversampling_0/ConfigMaster_0/state[11]:Q Type=0 ADDR=0xD8110 (WADDR=0xD BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD1[4]:Q Type=0 ADDR=0x26831B (WADDR=0x26 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0_SOFT_FAB_RESET:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[4]:Q Type=0 ADDR=0x5010F (WADDR=0x5 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[22]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[22]:Q Type=0 ADDR=0x1830F (WADDR=0x1 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/FIC_2_APB_M_PRESET_N_q1:IGLOO2_Oversampling_0/CORERESETP_0/FIC_2_APB_M_PRESET_N_q1:Q Type=0 ADDR=0x70011 (WADDR=0x7 BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/DA_FSM_STATE[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/DA_FSM_STATE[1]:Q Type=0 ADDR=0x250319 (WADDR=0x25 BADDR=0x0 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[6]:UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[6]:Q Type=0 ADDR=0x18021D (WADDR=0x18 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/CLR_INIT_DONE_clk_base:IGLOO2_Oversampling_0/CORERESETP_0/CLR_INIT_DONE_clk_base:Q Type=0 ADDR=0x48112 (WADDR=0x4 BADDR=0x2 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/prbs7_10_0/LFSR[6]:Receiver_0/prbs7_10_0/LFSR[6]:Q Type=0 ADDR=0x23801B (WADDR=0x23 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[17]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[17]:Q Type=0 ADDR=0xA8310 (WADDR=0xA BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[26]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[26]:Q Type=0 ADDR=0x118110 (WADDR=0x11 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[8]:Q Type=0 ADDR=0x290019 (WADDR=0x29 BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/CONFIG_DONE_clk_base:IGLOO2_Oversampling_0/CORERESETP_0/CONFIG_DONE_clk_base:Q Type=0 ADDR=0x40213 (WADDR=0x4 BADDR=0x0 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/POWER_ON_RESET_N_clk_base:IGLOO2_Oversampling_0/CORERESETP_0/POWER_ON_RESET_N_clk_base:Q Type=0 ADDR=0x70310 (WADDR=0x7 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[10]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[10]:Q Type=0 ADDR=0x70111 (WADDR=0x7 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[26]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[26]:Q Type=0 ADDR=0x7030F (WADDR=0x7 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[12]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[12]:Q Type=0 ADDR=0x11000E (WADDR=0x11 BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/CONFIG_DONE_q1:IGLOO2_Oversampling_0/CORERESETP_0/CONFIG_DONE_q1:Q Type=0 ADDR=0x40313 (WADDR=0x4 BADDR=0x0 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_DATA_OUT[0]:UART_INTERFACE_0/COREUART_0/make_RX/rx_byte[0]:Q Type=0 ADDR=0x17821C (WADDR=0x17 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[8]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[8]:Q Type=0 ADDR=0x108112 (WADDR=0x10 BADDR=0x2 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[31]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[31]:Q Type=0 ADDR=0x120311 (WADDR=0x12 BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[10]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[10]:Q Type=0 ADDR=0x9820D (WADDR=0x9 BADDR=0x2 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[21]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[21]:Q Type=0 ADDR=0x9830C (WADDR=0x9 BADDR=0x2 PRBR=0x3 CLOFFSET=0xC)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[5]:Q Type=0 ADDR=0x290017 (WADDR=0x29 BADDR=0x0 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[16]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[16]:Q Type=0 ADDR=0x148210 (WADDR=0x14 BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_cntr[3]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_cntr[3]:Q Type=0 ADDR=0x18001B (WADDR=0x18 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[15]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[15]:Q Type=0 ADDR=0x27831A (WADDR=0x27 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[4]:Transmitter_0/prbs7_10_0/LFSR[5]:Q Type=0 ADDR=0x12821F (WADDR=0x12 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/regHADDR[20]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/regHADDR[20]:Q Type=0 ADDR=0x100211 (WADDR=0x10 BADDR=0x0 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[16]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[16]:Q Type=0 ADDR=0x158011 (WADDR=0x15 BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[4]:Q Type=0 ADDR=0x2B821B (WADDR=0x2B BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_cntr[2]:UART_INTERFACE_0/COREUART_0/make_CLOCK_GEN/xmit_cntr[2]:Q Type=0 ADDR=0x18831B (WADDR=0x18 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[0]:Transmitter_0/prbs7_10_0/LFSR[1]:Q Type=0 ADDR=0x12011F (WADDR=0x12 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[8]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[8]:Q Type=0 ADDR=0x10810E (WADDR=0x10 BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_DATA_OUT[2]:UART_INTERFACE_0/COREUART_0/make_RX/rx_byte[2]:Q Type=0 ADDR=0x18001C (WADDR=0x18 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[31]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[31]:Q Type=0 ADDR=0x9020F (WADDR=0x9 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[13]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[13]:Q Type=0 ADDR=0x14010E (WADDR=0x14 BADDR=0x0 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[5]:Q Type=0 ADDR=0x29001B (WADDR=0x29 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[29]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[29]:Q Type=0 ADDR=0x7000C (WADDR=0x7 BADDR=0x0 PRBR=0x0 CLOFFSET=0xC)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[9]:IGLOO2_Oversampling_0/ConfigMaster_0/state[9]:Q Type=0 ADDR=0x11820F (WADDR=0x11 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/prbs7_10_0/rx_count[1]:Receiver_0/prbs7_10_0/rx_count[1]:Q Type=0 ADDR=0x23031B (WADDR=0x23 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[4]:Q Type=0 ADDR=0x290217 (WADDR=0x29 BADDR=0x0 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[15]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[15]:Q Type=0 ADDR=0x25811A (WADDR=0x25 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/data[14]:Transmitter_0/FIFO_PRBS_0/data[12]:Q Type=0 ADDR=0x120120 (WADDR=0x12 BADDR=0x0 PRBR=0x1 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[4]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[4]:Q Type=0 ADDR=0x88310 (WADDR=0x8 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[21]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[21]:Q Type=0 ADDR=0xA0110 (WADDR=0xA BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[2]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[2]:Q Type=0 ADDR=0xE020D (WADDR=0xE BADDR=0x0 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[14]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[14]:Q Type=0 ADDR=0xB800D (WADDR=0xB BADDR=0x2 PRBR=0x0 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[24]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[24]:Q Type=0 ADDR=0x2A031B (WADDR=0x2A BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[25]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[25]:Q Type=0 ADDR=0x9030F (WADDR=0x9 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/prbs7_10_0_tx_val:Transmitter_0/prbs7_10_0/reg_tx_val:Q Type=0 ADDR=0x11811F (WADDR=0x11 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/INIT_DONE_q2:IGLOO2_Oversampling_0/CORECONFIGP_0/INIT_DONE_q2:Q Type=0 ADDR=0x38111 (WADDR=0x3 BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/reg_data_out[7]:Transmitter_0/FIFO_PRBS_0/reg_data_out[7]:Q Type=0 ADDR=0x138120 (WADDR=0x13 BADDR=0x2 PRBR=0x1 CLOFFSET=0x20)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[3]:Receiver_0/Downsampler_0/reg_check[3]:Q Type=0 ADDR=0x280019 (WADDR=0x28 BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[20]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[20]:Q Type=0 ADDR=0x88110 (WADDR=0x8 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[11]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[11]:Q Type=0 ADDR=0xF030D (WADDR=0xF BADDR=0x0 PRBR=0x3 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/cntr_2bit[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/cntr_2bit[1]:Q Type=0 ADDR=0x230119 (WADDR=0x23 BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[29]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[29]:Q Type=0 ADDR=0x118311 (WADDR=0x11 BADDR=0x2 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[13]:IGLOO2_Oversampling_0/ConfigMaster_0/state[13]:Q Type=0 ADDR=0xE0310 (WADDR=0xE BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[29]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[29]:Q Type=0 ADDR=0x2A001B (WADDR=0x2A BADDR=0x0 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Transmitter_0/prbs7_10_0_data_out[6]:Transmitter_0/prbs7_10_0/LFSR[7]:Q Type=0 ADDR=0x12001F (WADDR=0x12 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PENABLE:IGLOO2_Oversampling_0/CORECONFIGP_0/SDIF0_PENABLE:Q Type=0 ADDR=0x40110 (WADDR=0x4 BADDR=0x0 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[5]:UART_INTERFACE_0/COREUART_0/make_TX/tx_byte[5]:Q Type=0 ADDR=0x180119 (WADDR=0x18 BADDR=0x0 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_DATA_OUT[7]:UART_INTERFACE_0/COREUART_0/make_RX/rx_byte[7]:Q Type=0 ADDR=0x18021C (WADDR=0x18 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[29]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[29]:Q Type=0 ADDR=0x118211 (WADDR=0x11 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[28]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[28]:Q Type=0 ADDR=0x268118 (WADDR=0x26 BADDR=0x2 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/reg_data_out[9]:Transmitter_0/FIFO_PRBS_0/reg_data_out[9]:Q Type=0 ADDR=0x14011F (WADDR=0x14 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1F)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/scan_t:UART_INTERFACE_0/FabUART_0/scan_t:Q Type=0 ADDR=0x19011A (WADDR=0x19 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[27]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[27]:Q Type=0 ADDR=0x12830F (WADDR=0x12 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[3]:Receiver_0/Downsampler_0/temp_data[3]:Q Type=0 ADDR=0x248319 (WADDR=0x24 BADDR=0x2 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/tx_hold_reg[4]:UART_INTERFACE_0/COREUART_0/tx_hold_reg[4]:Q Type=0 ADDR=0x18011A (WADDR=0x18 BADDR=0x0 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PADDR[13]:IGLOO2_Oversampling_0/CORECONFIGP_0/paddr[13]:Q Type=0 ADDR=0x28110 (WADDR=0x2 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[9]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[9]:Q Type=0 ADDR=0xD8111 (WADDR=0xD BADDR=0x2 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D0[1]:Q Type=0 ADDR=0x2A8018 (WADDR=0x2A BADDR=0x2 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HSIZE[0]:IGLOO2_Oversampling_0/ConfigMaster_0/HSIZE[0]:Q Type=0 ADDR=0xD800E (WADDR=0xD BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/samples[2]:UART_INTERFACE_0/COREUART_0/make_RX/samples[2]:Q Type=0 ADDR=0x14831D (WADDR=0x14 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1D)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[6]:Q Type=0 ADDR=0x288217 (WADDR=0x28 BADDR=0x2 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/prbs7_10_0/LFSR[1]:Receiver_0/prbs7_10_0/LFSR[1]:Q Type=0 ADDR=0x23831A (WADDR=0x23 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[27]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[27]:Q Type=0 ADDR=0x138211 (WADDR=0x13 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/reg_data_out[5]:Transmitter_0/FIFO_PRBS_0/reg_data_out[5]:Q Type=0 ADDR=0x140320 (WADDR=0x14 BADDR=0x0 PRBR=0x3 CLOFFSET=0x20)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[8]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[8]:Q Type=0 ADDR=0x280318 (WADDR=0x28 BADDR=0x0 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[23]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[23]:Q Type=0 ADDR=0x270118 (WADDR=0x27 BADDR=0x0 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[21]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[21]:Q Type=0 ADDR=0xB810F (WADDR=0xB BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[1]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[1]:Q Type=0 ADDR=0x98110 (WADDR=0x9 BADDR=0x2 PRBR=0x1 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[16]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[16]:Q Type=0 ADDR=0x27801A (WADDR=0x27 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[26]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[26]:Q Type=0 ADDR=0x40011 (WADDR=0x4 BADDR=0x0 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[8]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[8]:Q Type=0 ADDR=0xD8211 (WADDR=0xD BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[19]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[19]:Q Type=0 ADDR=0x110111 (WADDR=0x11 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Transmitter_0/Replicator_0_data_out[22]:Transmitter_0/Replicator_0/X[21]:Q Type=0 ADDR=0x13801F (WADDR=0x13 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[17]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[17]:Q Type=0 ADDR=0x150310 (WADDR=0x15 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[4]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[4]:Q Type=0 ADDR=0x12820E (WADDR=0x12 BADDR=0x2 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[27]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[27]:Q Type=0 ADDR=0x40111 (WADDR=0x4 BADDR=0x0 PRBR=0x1 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/trans_detect_bit9:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/trans_detect_bit9:Q Type=0 ADDR=0x298118 (WADDR=0x29 BADDR=0x2 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[16]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[16]:Q Type=0 ADDR=0x148310 (WADDR=0x14 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[15]:UART_INTERFACE_0/FabUART_0/state[15]:Q Type=0 ADDR=0x18801B (WADDR=0x18 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[7]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[7]:Q Type=0 ADDR=0x278118 (WADDR=0x27 BADDR=0x2 PRBR=0x1 CLOFFSET=0x18)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[5]:UART_INTERFACE_0/COREUART_0/make_RX/rx_shift[5]:Q Type=0 ADDR=0x18831D (WADDR=0x18 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1D)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[3]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[3]:Q Type=0 ADDR=0x290018 (WADDR=0x29 BADDR=0x0 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=Receiver_0_error_count[4]:Receiver_0/prbs7_10_0/reg_error[4]:Q Type=0 ADDR=0x1B011B (WADDR=0x1B BADDR=0x0 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[2]:Q Type=0 ADDR=0x260017 (WADDR=0x26 BADDR=0x0 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[13]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[13]:Q Type=0 ADDR=0xE8012 (WADDR=0xE BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[13]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[13]:Q Type=0 ADDR=0x2B021A (WADDR=0x2B BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[30]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[30]:Q Type=0 ADDR=0x1C10F (WADDR=0x1 BADDR=0x3 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[8]:IGLOO2_Oversampling_0/ConfigMaster_0/state[8]:Q Type=0 ADDR=0xD800F (WADDR=0xD BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[0]:IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[0]:Q Type=0 ADDR=0xE8213 (WADDR=0xE BADDR=0x2 PRBR=0x2 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/ddr_ready:IGLOO2_Oversampling_0/CORERESETP_0/ddr_ready:Q Type=0 ADDR=0x58313 (WADDR=0x5 BADDR=0x2 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/Downsampler_0/reg_check[4]:Receiver_0/Downsampler_0/reg_check[4]:Q Type=0 ADDR=0x25021A (WADDR=0x25 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_VALOUT_o:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_VALOUT_reg:Q Type=0 ADDR=0x280319 (WADDR=0x28 BADDR=0x0 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[6]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[6]:Q Type=0 ADDR=0x15810F (WADDR=0x15 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[2]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[2]:Q Type=0 ADDR=0x2B0018 (WADDR=0x2B BADDR=0x0 PRBR=0x0 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0_CLR_INIT_DONE:IGLOO2_Oversampling_0/CORECONFIGP_0/control_reg_2:Q Type=0 ADDR=0x38011 (WADDR=0x3 BADDR=0x2 PRBR=0x0 CLOFFSET=0x11)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[20]:IGLOO2_Oversampling_0/ConfigMaster_0/state[20]:Q Type=0 ADDR=0xF8013 (WADDR=0xF BADDR=0x2 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[14]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[14]:Q Type=0 ADDR=0x26811B (WADDR=0x26 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/psel:IGLOO2_Oversampling_0/CORECONFIGP_0/psel:Q Type=0 ADDR=0x40310 (WADDR=0x4 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[14]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[14]:Q Type=0 ADDR=0x10820E (WADDR=0x10 BADDR=0x2 PRBR=0x2 CLOFFSET=0xE)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_bit_sel[0]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_bit_sel[0]:Q Type=0 ADDR=0x188019 (WADDR=0x18 BADDR=0x2 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[11]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[11]:Q Type=0 ADDR=0x14820F (WADDR=0x14 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_RX/receive_count[0]:UART_INTERFACE_0/COREUART_0/make_RX/receive_count[0]:Q Type=0 ADDR=0x14821D (WADDR=0x14 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1D)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[10]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[10]:Q Type=0 ADDR=0x4020F (WADDR=0x4 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=UART_INTERFACE_0/FabUART_0/state[2]:UART_INTERFACE_0/FabUART_0/state[2]:Q Type=0 ADDR=0x19811A (WADDR=0x19 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[1]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[1]:Q Type=0 ADDR=0xE010D (WADDR=0xE BADDR=0x0 PRBR=0x1 CLOFFSET=0xD)
ProbePoint: Name=Receiver_0/Downsampler_0/temp_data[8]:Receiver_0/Downsampler_0/temp_data[8]:Q Type=0 ADDR=0x24821B (WADDR=0x24 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[1]:IGLOO2_Oversampling_0/ConfigMaster_0/pause_count[1]:Q Type=0 ADDR=0xE8313 (WADDR=0xE BADDR=0x2 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[1]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_state[1]:Q Type=0 ADDR=0x17811A (WADDR=0x17 BADDR=0x2 PRBR=0x1 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/trans_detect_bit6:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/trans_detect_bit6:Q Type=0 ADDR=0x2A8119 (WADDR=0x2A BADDR=0x2 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[14]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[14]:Q Type=0 ADDR=0x10000E (WADDR=0x10 BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[16]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[16]:Q Type=0 ADDR=0x6810E (WADDR=0x6 BADDR=0x2 PRBR=0x1 CLOFFSET=0xE)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[22]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[22]:Q Type=0 ADDR=0x9000E (WADDR=0x9 BADDR=0x0 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[11]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[11]:Q Type=0 ADDR=0x258219 (WADDR=0x25 BADDR=0x2 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[28]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[28]:Q Type=0 ADDR=0x50311 (WADDR=0x5 BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[4]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[4]:Q Type=0 ADDR=0x270117 (WADDR=0x27 BADDR=0x0 PRBR=0x1 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/cntr_2bit[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/cntr_2bit[0]:Q Type=0 ADDR=0x230219 (WADDR=0x23 BADDR=0x0 PRBR=0x2 CLOFFSET=0x19)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_TXRDY:UART_INTERFACE_0/COREUART_0/make_TX/txrdy_int:Q Type=0 ADDR=0x18031A (WADDR=0x18 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[0]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[0]:Q Type=0 ADDR=0x270217 (WADDR=0x27 BADDR=0x0 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[3]:IGLOO2_Oversampling_0/ConfigMaster_0/bytecount[3]:Q Type=0 ADDR=0xE030E (WADDR=0xE BADDR=0x0 PRBR=0x3 CLOFFSET=0xE)
ProbePoint: Name=Transmitter_0_EPCS_TX_DATA[0]:Transmitter_0/FIFO_PRBS_0/reg_data_out[0]:Q Type=0 ADDR=0x14021F (WADDR=0x14 BADDR=0x0 PRBR=0x2 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[1]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[1]:Q Type=0 ADDR=0xD8012 (WADDR=0xD BADDR=0x2 PRBR=0x0 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[14]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[14]:Q Type=0 ADDR=0x2B0019 (WADDR=0x2B BADDR=0x0 PRBR=0x0 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[11]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[11]:Q Type=0 ADDR=0x60310 (WADDR=0x6 BADDR=0x0 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[12]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[12]:Q Type=0 ADDR=0x2020F (WADDR=0x2 BADDR=0x0 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[6]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D2[6]:Q Type=0 ADDR=0x278318 (WADDR=0x27 BADDR=0x2 PRBR=0x3 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[23]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[23]:Q Type=0 ADDR=0x8810F (WADDR=0x8 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/receive_control_0_START_LOCK_o:Receiver_0/receive_buffer_top_0/receive_control_0/start_lock_reg:Q Type=0 ADDR=0x298119 (WADDR=0x29 BADDR=0x2 PRBR=0x1 CLOFFSET=0x19)
ProbePoint: Name=connect_o_c:UART_INTERFACE_0/FabUART_0/connect_t:Q Type=0 ADDR=0x19821B (WADDR=0x19 BADDR=0x2 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins1[26]:IGLOO2_Oversampling_0/ConfigMaster_0/ins1[26]:Q Type=0 ADDR=0xF8010 (WADDR=0xF BADDR=0x2 PRBR=0x0 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[12]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D3[12]:Q Type=0 ADDR=0x27031A (WADDR=0x27 BADDR=0x0 PRBR=0x3 CLOFFSET=0x1A)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HWDATA[5]:IGLOO2_Oversampling_0/ConfigMaster_0/HWDATA[5]:Q Type=0 ADDR=0x9000C (WADDR=0x9 BADDR=0x0 PRBR=0x0 CLOFFSET=0xC)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0/make_TX/xmit_bit_sel[3]:UART_INTERFACE_0/COREUART_0/make_TX/xmit_bit_sel[3]:Q Type=0 ADDR=0x178319 (WADDR=0x17 BADDR=0x2 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/ddr_ready_q1:IGLOO2_Oversampling_0/CORERESETP_0/ddr_ready_q1:Q Type=0 ADDR=0x40113 (WADDR=0x4 BADDR=0x0 PRBR=0x1 CLOFFSET=0x13)
ProbePoint: Name=Receiver_0/receive_buffer_top_0_RX_DATAOUT_o[29]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/RX_DATAOUT_reg[29]:Q Type=0 ADDR=0x268218 (WADDR=0x26 BADDR=0x2 PRBR=0x2 CLOFFSET=0x18)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[2]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[2]:Q Type=0 ADDR=0xA800F (WADDR=0xA BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/reg_data_out[1]:Transmitter_0/FIFO_PRBS_0/reg_data_out[1]:Q Type=0 ADDR=0x14001F (WADDR=0x14 BADDR=0x0 PRBR=0x0 CLOFFSET=0x1F)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[27]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[27]:Q Type=0 ADDR=0x68112 (WADDR=0x6 BADDR=0x2 PRBR=0x1 CLOFFSET=0x12)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[9]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/rx_data_debug[9]:Q Type=0 ADDR=0x2D021B (WADDR=0x2D BADDR=0x0 PRBR=0x2 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/rdata[28]:IGLOO2_Oversampling_0/ConfigMaster_0/rdata[28]:Q Type=0 ADDR=0x7810F (WADDR=0x7 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[1]:Q Type=0 ADDR=0x2A8319 (WADDR=0x2A BADDR=0x2 PRBR=0x3 CLOFFSET=0x19)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[3]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[3]:Q Type=0 ADDR=0x6030F (WADDR=0x6 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[0]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/slavestage_16/slave_arbiter/arbRegSMCurrentState[0]:Q Type=0 ADDR=0xF0212 (WADDR=0xF BADDR=0x0 PRBR=0x2 CLOFFSET=0x12)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[30]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[30]:Q Type=0 ADDR=0x7830F (WADDR=0x7 BADDR=0x2 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[22]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_write[22]:Q Type=0 ADDR=0x13820F (WADDR=0x13 BADDR=0x2 PRBR=0x2 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[9]:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0[9]:Q Type=0 ADDR=0x68313 (WADDR=0x6 BADDR=0x2 PRBR=0x3 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/IGLOO2_Oversampling_HPMS_0_FIC_2_APB_MASTER_PRDATA[8]:IGLOO2_Oversampling_0/CORECONFIGP_0/FIC_2_APB_M_PRDATA[8]:Q Type=0 ADDR=0x3800F (WADDR=0x3 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0_M_HADDR[24]:IGLOO2_Oversampling_0/ConfigMaster_0/HADDR[24]:Q Type=0 ADDR=0x118310 (WADDR=0x11 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/INIT_DONE_q3:IGLOO2_Oversampling_0/CORECONFIGP_0/INIT_DONE_q3:Q Type=0 ADDR=0x38211 (WADDR=0x3 BADDR=0x2 PRBR=0x2 CLOFFSET=0x11)
ProbePoint: Name=UART_INTERFACE_0/COREUART_0_DATA_OUT[6]:UART_INTERFACE_0/COREUART_0/make_RX/rx_byte[6]:Q Type=0 ADDR=0x18831C (WADDR=0x18 BADDR=0x2 PRBR=0x3 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[3]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[3]:Q Type=0 ADDR=0x15000F (WADDR=0x15 BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[8]:IGLOO2_Oversampling_0/CORECONFIGP_0/soft_reset_reg[8]:Q Type=0 ADDR=0x3810F (WADDR=0x3 BADDR=0x2 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[2]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[2]:Q Type=0 ADDR=0x12020D (WADDR=0x12 BADDR=0x0 PRBR=0x2 CLOFFSET=0xD)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[22]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[22]:Q Type=0 ADDR=0x10030F (WADDR=0x10 BADDR=0x0 PRBR=0x3 CLOFFSET=0xF)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[1]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/checkD3[1]:Q Type=0 ADDR=0x278217 (WADDR=0x27 BADDR=0x2 PRBR=0x2 CLOFFSET=0x17)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[29]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[29]:Q Type=0 ADDR=0x2C831B (WADDR=0x2C BADDR=0x2 PRBR=0x3 CLOFFSET=0x1B)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[10]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[10]:Q Type=0 ADDR=0x11800E (WADDR=0x11 BADDR=0x2 PRBR=0x0 CLOFFSET=0xE)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[25]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/D1[25]:Q Type=0 ADDR=0x28801C (WADDR=0x28 BADDR=0x2 PRBR=0x0 CLOFFSET=0x1C)
ProbePoint: Name=IGLOO2_Oversampling_0_SDIF0_INIT_APB_PWDATA[29]:IGLOO2_Oversampling_0/CORECONFIGP_0/pwdata[29]:Q Type=0 ADDR=0x60210 (WADDR=0x6 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[1]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[1]:Q Type=0 ADDR=0x14010F (WADDR=0x14 BADDR=0x0 PRBR=0x1 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[11]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[11]:Q Type=0 ADDR=0xA000F (WADDR=0xA BADDR=0x0 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0/FIFO_PRBS_0/flag:Transmitter_0/FIFO_PRBS_0/flag:Q Type=0 ADDR=0x128020 (WADDR=0x12 BADDR=0x2 PRBR=0x0 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[15]:IGLOO2_Oversampling_0/CoreAHBLite_0/matrix4x16/masterstage_0/SDATASELInt[15]:Q Type=0 ADDR=0xE0311 (WADDR=0xE BADDR=0x0 PRBR=0x3 CLOFFSET=0x11)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[5]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[5]:Q Type=0 ADDR=0x288017 (WADDR=0x28 BADDR=0x2 PRBR=0x0 CLOFFSET=0x17)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/ins2[16]:IGLOO2_Oversampling_0/ConfigMaster_0/ins2[16]:Q Type=0 ADDR=0x150210 (WADDR=0x15 BADDR=0x0 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[26]:IGLOO2_Oversampling_0/ConfigMaster_0/haddr_fetch[26]:Q Type=0 ADDR=0x128310 (WADDR=0x12 BADDR=0x2 PRBR=0x3 CLOFFSET=0x10)
ProbePoint: Name=IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0_enable:IGLOO2_Oversampling_0/CORERESETP_0/count_sdif0_enable:Q Type=0 ADDR=0x50013 (WADDR=0x5 BADDR=0x0 PRBR=0x0 CLOFFSET=0x13)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[15]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[15]:Q Type=0 ADDR=0x5800F (WADDR=0x5 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=Transmitter_0_EPCS_TX_DATA[8]:Transmitter_0/FIFO_PRBS_0/reg_data_out[8]:Q Type=0 ADDR=0x138020 (WADDR=0x13 BADDR=0x2 PRBR=0x0 CLOFFSET=0x20)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/mask[20]:IGLOO2_Oversampling_0/ConfigMaster_0/mask[20]:Q Type=0 ADDR=0x8800F (WADDR=0x8 BADDR=0x2 PRBR=0x0 CLOFFSET=0xF)
ProbePoint: Name=IGLOO2_Oversampling_0/ConfigMaster_0/state[1]:IGLOO2_Oversampling_0/ConfigMaster_0/state[1]:Q Type=0 ADDR=0xE8210 (WADDR=0xE BADDR=0x2 PRBR=0x2 CLOFFSET=0x10)
ProbePoint: Name=Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[39]:Receiver_0/receive_buffer_top_0/rx_data_aligner_0/buf_data[39]:Q Type=0 ADDR=0x2D031B (WADDR=0x2D BADDR=0x0 PRBR=0x3 CLOFFSET=0x1B)
