#Build: Synplify Pro I-2013.09M-SP1 , Build 034R, Jan 17 2014
#install: C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1
#OS: Windows 7 6.1
#Hostname: W764-UPPALAPATI

#Implementation: synthesis

$ Start of Compile
#Fri Apr 18 09:30:48 2014

Synopsys Verilog Compiler, version comp201309rcp1, Build 078R, built Jan 14 2014
@N|Running in 64-bit mode
Copyright (C) 1994-2013 Synopsys, Inc. This software and the associated documentation are proprietary to Synopsys, Inc. This software may only be used in accordance with the terms and conditions of a written license agreement with Synopsys, Inc.  All other use or distribution of the software is strictly prohibited.

@I::"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\generic\igloo2.v"
@I::"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\vlog\umr_capim.v"
@I::"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\vlog\scemi_objects.v"
@I::"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\vlog\scemi_pipes.svh"
@I::"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\vlog\hypermods.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_top\FCCC_0\IGLOO2_Oversampling_top_FCCC_0_FCCC.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\CCC_0\IGLOO2_Oversampling_CCC_0_FCCC.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigMaster\2.0.101\rtl\vlog\core\coreconfigmaster.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigP\5.0.101\rtl\vlog\core\coreconfigp.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\SgCore\OSC\1.0.100\osc_comps.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_HPMS\IGLOO2_Oversampling_HPMS_syn.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_HPMS\IGLOO2_Oversampling_HPMS.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_addrdec.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_defaultslavesm.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\IGLOO2_Oversampling.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\hdl\Downsampler_Rx.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\hdl\PRBS_GenCheck.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\hdl\rx_data_aligner.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\hdl\receive_control.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\hdl\receive_buffer_top.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\Receiver\Receiver.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_top\SERDES_IF_0\IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF_syn.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_top\SERDES_IF_0\IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\hdl\FIFO_PRBS.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\hdl\Replicator_Tx.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\Transmitter\Transmitter.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Clock_gen.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Rx_async.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\fifo_256x8_smartfusion2.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\UART_INTERFACE.v"
@I::"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_top\IGLOO2_Oversampling_top.v"
@W: CG775 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":32:7:32:17|Found Component CoreAHBLite in library COREAHBLITE_LIB
Verilog syntax check successful!
Selecting top level module IGLOO2_Oversampling_top
@N: CG364 :"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\generic\igloo2.v":362:7:362:12|Synthesizing module CLKINT

@N: CG364 :"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\generic\igloo2.v":371:7:371:9|Synthesizing module VCC

@N: CG364 :"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\generic\igloo2.v":367:7:367:9|Synthesizing module GND

@N: CG364 :"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\generic\igloo2.v":722:7:722:9|Synthesizing module CCC

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_top\FCCC_0\IGLOO2_Oversampling_top_FCCC_0_FCCC.v":5:7:5:41|Synthesizing module IGLOO2_Oversampling_top_FCCC_0_FCCC

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\CCC_0\IGLOO2_Oversampling_CCC_0_FCCC.v":5:7:5:36|Synthesizing module IGLOO2_Oversampling_CCC_0_FCCC

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigMaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":24:7:24:22|Synthesizing module CoreConfigMaster

	DATA_LOCATION=32'b00000000000000111110100000000000
	ADDR_SYSREG_SOFT_RESET=32'b01000000000000111000000001001000
	ADDR_SYSREG_ENVM_BUSY=32'b01000000000000111000000101011000
	S0=32'b00000000000000000000000000000000
	S1=32'b00000000000000000000000000000001
	S2=32'b00000000000000000000000000000010
	S3=32'b00000000000000000000000000000011
	S4=32'b00000000000000000000000000000100
	S5=32'b00000000000000000000000000000101
	S6=32'b00000000000000000000000000000110
	S7=32'b00000000000000000000000000000111
	S8=32'b00000000000000000000000000001000
	S9=32'b00000000000000000000000000001001
	S10=32'b00000000000000000000000000001010
	S11=32'b00000000000000000000000000001011
	S12=32'b00000000000000000000000000001100
	S13=32'b00000000000000000000000000001101
	S14=32'b00000000000000000000000000001110
	P0=32'b00000000000000000000000000001111
	P1=32'b00000000000000000000000000010000
	P2=32'b00000000000000000000000000010001
	P3=32'b00000000000000000000000000010010
	P4=32'b00000000000000000000000000010011
	P5=32'b00000000000000000000000000010100
	P6=32'b00000000000000000000000000010101
	OP_COPY=7'b0000000
   Generated name = CoreConfigMaster_Z1

@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigMaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Optimizing register bit HTRANS[0] to a constant 0
@W: CL260 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigMaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Pruning register bit 0 of HTRANS[1:0] 

@W: CG775 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":32:7:32:17|Found Component CoreAHBLite in library COREAHBLITE_LIB
@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_addrdec.v":29:7:29:25|Synthesizing module COREAHBLITE_ADDRDEC

	MEMSPACE=3'b001
	HADDR_SHG_CFG=1'b1
	SC=16'b0000000001010101
	M_AHBSLOTENABLE=17'b10000000000000000
	MSB_ADDR=32'b00000000000000000000000000011111
	SLAVE_0=16'b0000000000000001
	SLAVE_1=16'b0000000000000010
	SLAVE_2=16'b0000000000000100
	SLAVE_3=16'b0000000000001000
	SLAVE_4=16'b0000000000010000
	SLAVE_5=16'b0000000000100000
	SLAVE_6=16'b0000000001000000
	SLAVE_7=16'b0000000010000000
	SLAVE_8=16'b0000000100000000
	SLAVE_9=16'b0000001000000000
	SLAVE_10=16'b0000010000000000
	SLAVE_11=16'b0000100000000000
	SLAVE_12=16'b0001000000000000
	SLAVE_13=16'b0010000000000000
	SLAVE_14=16'b0100000000000000
	SLAVE_15=16'b1000000000000000
	NONE=16'b0000000000000000
   Generated name = COREAHBLITE_ADDRDEC_Z2

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_defaultslavesm.v":29:7:29:32|Synthesizing module COREAHBLITE_DEFAULTSLAVESM

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":31:7:31:29|Synthesizing module COREAHBLITE_MASTERSTAGE

	MEMSPACE=3'b001
	HADDR_SHG_CFG=1'b1
	SC=16'b0000000001010101
	M_AHBSLOTENABLE=17'b10000000000000000
	IDLE=1'b0
	REGISTERED=1'b1
	SLAVE_NONE=17'b00000000000000000
   Generated name = COREAHBLITE_MASTERSTAGE_1_1_85_65536_0_1_0

@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":629:0:629:5|Sharing sequential element addrRegSMCurrentState.
@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_addrdec.v":29:7:29:25|Synthesizing module COREAHBLITE_ADDRDEC

	MEMSPACE=3'b001
	HADDR_SHG_CFG=1'b1
	SC=16'b0000000001010101
	M_AHBSLOTENABLE=17'b00000000000000000
	MSB_ADDR=32'b00000000000000000000000000011111
	SLAVE_0=16'b0000000000000001
	SLAVE_1=16'b0000000000000010
	SLAVE_2=16'b0000000000000100
	SLAVE_3=16'b0000000000001000
	SLAVE_4=16'b0000000000010000
	SLAVE_5=16'b0000000000100000
	SLAVE_6=16'b0000000001000000
	SLAVE_7=16'b0000000010000000
	SLAVE_8=16'b0000000100000000
	SLAVE_9=16'b0000001000000000
	SLAVE_10=16'b0000010000000000
	SLAVE_11=16'b0000100000000000
	SLAVE_12=16'b0001000000000000
	SLAVE_13=16'b0010000000000000
	SLAVE_14=16'b0100000000000000
	SLAVE_15=16'b1000000000000000
	NONE=16'b0000000000000000
   Generated name = COREAHBLITE_ADDRDEC_Z3

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":31:7:31:29|Synthesizing module COREAHBLITE_MASTERSTAGE

	MEMSPACE=3'b001
	HADDR_SHG_CFG=1'b1
	SC=16'b0000000001010101
	M_AHBSLOTENABLE=17'b00000000000000000
	IDLE=1'b0
	REGISTERED=1'b1
	SLAVE_NONE=17'b00000000000000000
   Generated name = COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0

@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":629:0:629:5|Sharing sequential element addrRegSMCurrentState.
@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":28:7:28:30|Synthesizing module COREAHBLITE_SLAVEARBITER

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v":30:7:30:28|Synthesizing module COREAHBLITE_SLAVESTAGE

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":31:7:31:28|Synthesizing module COREAHBLITE_MATRIX4X16

	MEMSPACE=3'b001
	HADDR_SHG_CFG=1'b1
	SC=16'b0000000001010101
	M0_AHBSLOTENABLE=17'b10000000000000000
	M1_AHBSLOTENABLE=17'b00000000000000000
	M2_AHBSLOTENABLE=17'b00000000000000000
	M3_AHBSLOTENABLE=17'b00000000000000000
   Generated name = COREAHBLITE_MATRIX4X16_1_1_85_65536_0_0_0

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":32:7:32:17|Synthesizing module CoreAHBLite

	FAMILY=6'b010011
	MEMSPACE=3'b001
	HADDR_SHG_CFG=1'b1
	SC_0=1'b1
	SC_1=1'b0
	SC_2=1'b1
	SC_3=1'b0
	SC_4=1'b1
	SC_5=1'b0
	SC_6=1'b1
	SC_7=1'b0
	SC_8=1'b0
	SC_9=1'b0
	SC_10=1'b0
	SC_11=1'b0
	SC_12=1'b0
	SC_13=1'b0
	SC_14=1'b0
	SC_15=1'b0
	M0_AHBSLOT0ENABLE=1'b0
	M0_AHBSLOT1ENABLE=1'b0
	M0_AHBSLOT2ENABLE=1'b0
	M0_AHBSLOT3ENABLE=1'b0
	M0_AHBSLOT4ENABLE=1'b0
	M0_AHBSLOT5ENABLE=1'b0
	M0_AHBSLOT6ENABLE=1'b0
	M0_AHBSLOT7ENABLE=1'b0
	M0_AHBSLOT8ENABLE=1'b0
	M0_AHBSLOT9ENABLE=1'b0
	M0_AHBSLOT10ENABLE=1'b0
	M0_AHBSLOT11ENABLE=1'b0
	M0_AHBSLOT12ENABLE=1'b0
	M0_AHBSLOT13ENABLE=1'b0
	M0_AHBSLOT14ENABLE=1'b0
	M0_AHBSLOT15ENABLE=1'b0
	M0_AHBSLOT16ENABLE=1'b1
	M1_AHBSLOT0ENABLE=1'b0
	M1_AHBSLOT1ENABLE=1'b0
	M1_AHBSLOT2ENABLE=1'b0
	M1_AHBSLOT3ENABLE=1'b0
	M1_AHBSLOT4ENABLE=1'b0
	M1_AHBSLOT5ENABLE=1'b0
	M1_AHBSLOT6ENABLE=1'b0
	M1_AHBSLOT7ENABLE=1'b0
	M1_AHBSLOT8ENABLE=1'b0
	M1_AHBSLOT9ENABLE=1'b0
	M1_AHBSLOT10ENABLE=1'b0
	M1_AHBSLOT11ENABLE=1'b0
	M1_AHBSLOT12ENABLE=1'b0
	M1_AHBSLOT13ENABLE=1'b0
	M1_AHBSLOT14ENABLE=1'b0
	M1_AHBSLOT15ENABLE=1'b0
	M1_AHBSLOT16ENABLE=1'b0
	M2_AHBSLOT0ENABLE=1'b0
	M2_AHBSLOT1ENABLE=1'b0
	M2_AHBSLOT2ENABLE=1'b0
	M2_AHBSLOT3ENABLE=1'b0
	M2_AHBSLOT4ENABLE=1'b0
	M2_AHBSLOT5ENABLE=1'b0
	M2_AHBSLOT6ENABLE=1'b0
	M2_AHBSLOT7ENABLE=1'b0
	M2_AHBSLOT8ENABLE=1'b0
	M2_AHBSLOT9ENABLE=1'b0
	M2_AHBSLOT10ENABLE=1'b0
	M2_AHBSLOT11ENABLE=1'b0
	M2_AHBSLOT12ENABLE=1'b0
	M2_AHBSLOT13ENABLE=1'b0
	M2_AHBSLOT14ENABLE=1'b0
	M2_AHBSLOT15ENABLE=1'b0
	M2_AHBSLOT16ENABLE=1'b0
	M3_AHBSLOT0ENABLE=1'b0
	M3_AHBSLOT1ENABLE=1'b0
	M3_AHBSLOT2ENABLE=1'b0
	M3_AHBSLOT3ENABLE=1'b0
	M3_AHBSLOT4ENABLE=1'b0
	M3_AHBSLOT5ENABLE=1'b0
	M3_AHBSLOT6ENABLE=1'b0
	M3_AHBSLOT7ENABLE=1'b0
	M3_AHBSLOT8ENABLE=1'b0
	M3_AHBSLOT9ENABLE=1'b0
	M3_AHBSLOT10ENABLE=1'b0
	M3_AHBSLOT11ENABLE=1'b0
	M3_AHBSLOT12ENABLE=1'b0
	M3_AHBSLOT13ENABLE=1'b0
	M3_AHBSLOT14ENABLE=1'b0
	M3_AHBSLOT15ENABLE=1'b0
	M3_AHBSLOT16ENABLE=1'b0
	M0_AHBSLOTENABLE=17'b10000000000000000
	M1_AHBSLOTENABLE=17'b00000000000000000
	M2_AHBSLOTENABLE=17'b00000000000000000
	M3_AHBSLOTENABLE=17'b00000000000000000
	SC=16'b0000000001010101
   Generated name = CoreAHBLite_Z4

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigP\5.0.101\rtl\vlog\core\coreconfigp.v":22:7:22:17|Synthesizing module CoreConfigP

	FAMILY=32'b00000000000000000000000000010011
	MDDR_IN_USE=32'b00000000000000000000000000000000
	FDDR_IN_USE=32'b00000000000000000000000000000000
	SDIF0_IN_USE=32'b00000000000000000000000000000001
	SDIF1_IN_USE=32'b00000000000000000000000000000000
	SDIF2_IN_USE=32'b00000000000000000000000000000000
	SDIF3_IN_USE=32'b00000000000000000000000000000000
	SDIF0_PCIE=32'b00000000000000000000000000000001
	SDIF1_PCIE=32'b00000000000000000000000000000000
	SDIF2_PCIE=32'b00000000000000000000000000000000
	SDIF3_PCIE=32'b00000000000000000000000000000000
	ENABLE_SOFT_RESETS=32'b00000000000000000000000000000001
	DEVICE_090=32'b00000000000000000000000000000000
	S0=2'b00
	S1=2'b01
	S2=2'b10
   Generated name = CoreConfigP_Z5

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":23:7:23:16|Synthesizing module CoreResetP

	FAMILY=32'b00000000000000000000000000010011
	EXT_RESET_CFG=32'b00000000000000000000000000000000
	DEVICE_VOLTAGE=32'b00000000000000000000000000000010
	MDDR_IN_USE=32'b00000000000000000000000000000000
	FDDR_IN_USE=32'b00000000000000000000000000000000
	SDIF0_IN_USE=32'b00000000000000000000000000000001
	SDIF1_IN_USE=32'b00000000000000000000000000000000
	SDIF2_IN_USE=32'b00000000000000000000000000000000
	SDIF3_IN_USE=32'b00000000000000000000000000000000
	SDIF0_PCIE=32'b00000000000000000000000000000001
	SDIF1_PCIE=32'b00000000000000000000000000000000
	SDIF2_PCIE=32'b00000000000000000000000000000000
	SDIF3_PCIE=32'b00000000000000000000000000000000
	SDIF0_PCIE_HOTRESET=32'b00000000000000000000000000000001
	SDIF1_PCIE_HOTRESET=32'b00000000000000000000000000000001
	SDIF2_PCIE_HOTRESET=32'b00000000000000000000000000000001
	SDIF3_PCIE_HOTRESET=32'b00000000000000000000000000000001
	SDIF0_PCIE_L2P2=32'b00000000000000000000000000000001
	SDIF1_PCIE_L2P2=32'b00000000000000000000000000000001
	SDIF2_PCIE_L2P2=32'b00000000000000000000000000000001
	SDIF3_PCIE_L2P2=32'b00000000000000000000000000000001
	ENABLE_SOFT_RESETS=32'b00000000000000000000000000000001
	DDR_WAIT=32'b00000000000000000000000011001000
	RCOSC_MEGAHERTZ=32'b00000000000000000000000000110010
	SDIF_INTERVAL=32'b00000000000000000001100101100100
	DDR_INTERVAL=32'b00000000000000000010011100010000
	COUNT_WIDTH_SDIF=32'b00000000000000000000000000001101
	COUNT_WIDTH_DDR=32'b00000000000000000000000000001110
	S0=32'b00000000000000000000000000000000
	S1=32'b00000000000000000000000000000001
	S2=32'b00000000000000000000000000000010
	S3=32'b00000000000000000000000000000011
	S4=32'b00000000000000000000000000000100
	S5=32'b00000000000000000000000000000101
	S6=32'b00000000000000000000000000000110
   Generated name = CoreResetP_Z6

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":31:7:31:30|Synthesizing module coreresetp_pcie_hotreset

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1562:4:1562:9|Pruning register count_ddr[13:0] 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1530:4:1530:9|Pruning register count_sdif3[12:0] 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1498:4:1498:9|Pruning register count_sdif2[12:0] 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1466:4:1466:9|Pruning register count_sdif1[12:0] 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif1_enable_q1 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif2_enable_q1 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif3_enable_q1 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif1_enable_rcosc 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif2_enable_rcosc 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif3_enable_rcosc 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_ddr_enable_q1 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_ddr_enable_rcosc 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1314:4:1314:9|Pruning register count_sdif3_enable 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1249:4:1249:9|Pruning register count_sdif2_enable 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1184:4:1184:9|Pruning register count_sdif1_enable 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Pruning register count_ddr_enable 

@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1337:4:1337:9|Sharing sequential element M3_RESET_N_int.
@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":936:4:936:9|Sharing sequential element sdif2_spll_lock_q1.
@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":936:4:936:9|Sharing sequential element sdif1_spll_lock_q1.
@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":936:4:936:9|Sharing sequential element fpll_lock_q1.
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1382:4:1382:9|Optimizing register bit EXT_RESET_OUT_int to a constant 0
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Pruning register release_ext_reset 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1382:4:1382:9|Pruning register EXT_RESET_OUT_int 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1382:4:1382:9|Pruning register sm2_state[2:0] 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":756:4:756:9|Pruning register sm2_areset_n_q1 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":756:4:756:9|Pruning register sm2_areset_n_clk_base 

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\SgCore\OSC\1.0.100\osc_comps.v":51:7:51:24|Synthesizing module RCOSC_25_50MHZ_FAB

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\SgCore\OSC\1.0.100\osc_comps.v":11:7:11:20|Synthesizing module RCOSC_25_50MHZ

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":5:7:5:38|Synthesizing module IGLOO2_Oversampling_FABOSC_0_OSC

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_HPMS\IGLOO2_Oversampling_HPMS_syn.v":5:7:5:13|Synthesizing module MSS_010

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_HPMS\IGLOO2_Oversampling_HPMS.v":9:7:9:30|Synthesizing module IGLOO2_Oversampling_HPMS

@N: CG364 :"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\generic\igloo2.v":713:7:713:14|Synthesizing module SYSRESET

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\IGLOO2_Oversampling.v":9:7:9:25|Synthesizing module IGLOO2_Oversampling

@N: CG364 :"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\generic\igloo2.v":156:7:156:10|Synthesizing module AND3

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\hdl\Downsampler_Rx.v":29:7:29:17|Synthesizing module Downsampler

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\hdl\PRBS_GenCheck.v":26:7:26:14|Synthesizing module prbs7_10

@N: CG179 :"C:\Microsemi\IGLOO2_Oversampling\hdl\PRBS_GenCheck.v":193:24:193:36|Removing redundant assignment
@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\hdl\rx_data_aligner.v":29:7:29:21|Synthesizing module rx_data_aligner

@N: CG179 :"C:\Microsemi\IGLOO2_Oversampling\hdl\rx_data_aligner.v":506:22:506:35|Removing redundant assignment
@N: CG179 :"C:\Microsemi\IGLOO2_Oversampling\hdl\rx_data_aligner.v":507:22:507:34|Removing redundant assignment
@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\hdl\receive_control.v":29:7:29:21|Synthesizing module receive_control

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\hdl\receive_buffer_top.v":26:7:26:24|Synthesizing module receive_buffer_top

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\Receiver\Receiver.v":9:7:9:14|Synthesizing module Receiver

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_top\SERDES_IF_0\IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF_syn.v":5:7:5:16|Synthesizing module SERDESIF_0

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_top\SERDES_IF_0\IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF.v":5:7:5:51|Synthesizing module IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF

@N: CG364 :"C:\Microsemi\Libero_v11.3\Synopsys\synplify_I201309MSP1\lib\generic\igloo2.v":126:7:126:10|Synthesizing module AND2

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FIFO_PRBS.v":23:7:23:15|Synthesizing module FIFO_PRBS

@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FIFO_PRBS.v":74:1:74:6|Optimizing register bit reg_tx_val_out to a constant 1
@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\hdl\Replicator_Tx.v":26:7:26:16|Synthesizing module Replicator

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\Transmitter\Transmitter.v":9:7:9:17|Synthesizing module Transmitter

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Clock_gen.v":38:7:38:41|Synthesizing module UART_INTERFACE_COREUART_0_Clock_gen

	BAUD_VAL_FRCTN_EN=32'b00000000000000000000000000000000
   Generated name = UART_INTERFACE_COREUART_0_Clock_gen_0s

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":31:7:31:40|Synthesizing module UART_INTERFACE_COREUART_0_Tx_async

	TX_FIFO=32'b00000000000000000000000000000000
	tx_idle=32'b00000000000000000000000000000000
	tx_load=32'b00000000000000000000000000000001
	start_bit=32'b00000000000000000000000000000010
	tx_data_bits=32'b00000000000000000000000000000011
	parity_bit=32'b00000000000000000000000000000100
	tx_stop_bit=32'b00000000000000000000000000000101
	delay_state=32'b00000000000000000000000000000110
   Generated name = UART_INTERFACE_COREUART_0_Tx_async_0s_0s_1s_2s_3s_4s_5s_6s

@N: CG179 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":349:21:349:29|Removing redundant assignment
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":112:0:112:5|Optimizing register bit fifo_read_en0 to a constant 1
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":112:0:112:5|Pruning register fifo_read_en0 

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Rx_async.v":30:7:30:40|Synthesizing module UART_INTERFACE_COREUART_0_Rx_async

	RX_FIFO=32'b00000000000000000000000000000000
	receive_states_rx_idle=32'b00000000000000000000000000000000
	receive_states_rx_data_bits=32'b00000000000000000000000000000001
	receive_states_rx_stop_bit=32'b00000000000000000000000000000010
   Generated name = UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s

@N: CG179 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Rx_async.v":243:23:243:35|Removing redundant assignment
@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Rx_async.v":459:0:459:5|Sharing sequential element clear_framing_error_en.
@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":31:7:31:40|Synthesizing module UART_INTERFACE_COREUART_0_COREUART

	TX_FIFO=32'b00000000000000000000000000000000
	RX_FIFO=32'b00000000000000000000000000000000
	RX_LEGACY_MODE=32'b00000000000000000000000000000000
	FAMILY=32'b00000000000000000000000000010011
	BAUD_VAL_FRCTN_EN=32'b00000000000000000000000000000000
   Generated name = UART_INTERFACE_COREUART_0_COREUART_0s_0s_0s_19s_0s

@N: CG179 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":374:22:374:33|Removing redundant assignment
@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":111:14:111:24|No assignment to wire tx_dout_reg

@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":112:14:112:20|No assignment to wire rx_dout

@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":118:8:118:20|No assignment to wire fifo_empty_tx

@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":119:8:119:20|No assignment to wire fifo_empty_rx

@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":123:8:123:19|No assignment to wire fifo_full_tx

@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":124:8:124:19|No assignment to wire fifo_full_rx

@W: CG133 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":135:8:135:17|No assignment to data_ready
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":360:0:360:5|Pruning register overflow_reg 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":335:0:335:5|Pruning register rx_dout_reg_empty 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":335:0:335:5|Pruning register rx_dout_reg_empty_q 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":320:0:320:5|Pruning register rx_dout_reg[7:0] 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":287:0:287:5|Pruning register rx_state[1:0] 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":272:0:272:5|Pruning register clear_framing_error_reg 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":272:0:272:5|Pruning register clear_framing_error_reg0 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":257:0:257:5|Pruning register clear_parity_reg 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":257:0:257:5|Pruning register clear_parity_reg0 

@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":154:0:154:5|Pruning register fifo_write_tx 

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v":26:7:26:13|Synthesizing module FabUART

@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v":91:0:91:5|Optimizing register bit uart_data_out_t[6] to a constant 0
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v":91:0:91:5|Optimizing register bit uart_data_out_t[7] to a constant 0
@W: CL279 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v":91:0:91:5|Pruning register bits 7 to 6 of uart_data_out_t[7:0] 

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\UART_INTERFACE.v":9:7:9:20|Synthesizing module UART_INTERFACE

@N: CG364 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_top\IGLOO2_Oversampling_top.v":9:7:9:29|Synthesizing module IGLOO2_Oversampling_top

@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v":91:0:91:5|Trying to extract state machine for register state
Extracted state machine for register state
State machine has 18 reachable states with original encodings of:
   00000
   00001
   00010
   00011
   00100
   00101
   00110
   00111
   01000
   01001
   01010
   01011
   01100
   01101
   01110
   01111
   10000
   10001
@W: CL156 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":111:14:111:24|*Input tx_dout_reg[7:0] to expression [instance] has undriven bits that are tied to 0 -- simulation mismatch possible.
@W: CL156 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":118:8:118:20|*Input fifo_empty_tx to expression [instance] has undriven bits that are tied to 0 -- simulation mismatch possible.
@W: CL156 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":123:8:123:19|*Input fifo_full_tx to expression [instance] has undriven bits that are tied to 0 -- simulation mismatch possible.
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Rx_async.v":255:0:255:5|Trying to extract state machine for register rx_state
Extracted state machine for register rx_state
State machine has 3 reachable states with original encodings of:
   00
   01
   10
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":112:0:112:5|Trying to extract state machine for register xmit_state
Extracted state machine for register xmit_state
State machine has 6 reachable states with original encodings of:
   00000000000000000000000000000000
   00000000000000000000000000000001
   00000000000000000000000000000010
   00000000000000000000000000000011
   00000000000000000000000000000100
   00000000000000000000000000000101
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":43:11:43:21|Input tx_dout_reg is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":44:6:44:15|Input fifo_empty is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":45:6:45:14|Input fifo_full is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Clock_gen.v":50:15:50:31|Input BAUD_VAL_FRACTION is unused
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FIFO_PRBS.v":74:1:74:6|Optimizing register bit reg_tx_val_out to a constant 1
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FIFO_PRBS.v":74:1:74:6|Trying to extract state machine for register i
Extracted state machine for register i
State machine has 3 reachable states with original encodings of:
   00
   01
   10
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\hdl\receive_control.v":82:4:82:9|Trying to extract state machine for register RC_FSM_state
Extracted state machine for register RC_FSM_state
State machine has 3 reachable states with original encodings of:
   00
   01
   10
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\hdl\rx_data_aligner.v":349:4:349:9|Trying to extract state machine for register DA_FSM_STATE
Extracted state machine for register DA_FSM_STATE
State machine has 4 reachable states with original encodings of:
   00
   01
   10
   11
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\hdl\PRBS_GenCheck.v":92:2:92:7|Trying to extract state machine for register tx_count
Extracted state machine for register tx_count
State machine has 3 reachable states with original encodings of:
   00
   01
   10
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\hdl\PRBS_GenCheck.v":92:2:92:7|Trying to extract state machine for register rx_count
Extracted state machine for register rx_count
State machine has 3 reachable states with original encodings of:
   00
   01
   10
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_HPMS\IGLOO2_Oversampling_HPMS.v":51:14:51:31|Input port bit 0 of FIC_0_AHB_S_HTRANS[1:0] is unused

@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":15:7:15:24|*Output RCOSC_25_50MHZ_CCC has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":17:7:17:20|*Output RCOSC_1MHZ_CCC has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":18:7:18:20|*Output RCOSC_1MHZ_O2F has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":19:7:19:16|*Output XTLOSC_CCC has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":20:7:20:16|*Output XTLOSC_O2F has undriven bits -- simulation mismatch possible.
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":14:7:14:9|Input XTL is unused
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":179:4:179:9|Trying to extract state machine for register state
Extracted state machine for register state
State machine has 4 reachable states with original encodings of:
   00
   01
   10
   11
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":36:24:36:29|Input port bit 31 of prdata[31:0] is unused

@W: CL246 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":36:24:36:29|Input port bits 25 to 0 of prdata[31:0] are unused

@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":936:4:936:9|Sharing sequential element sdif1_spll_lock_q2.
@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":936:4:936:9|Sharing sequential element sdif2_spll_lock_q2.
@N: CL177 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":936:4:936:9|Sharing sequential element fpll_lock_q2.
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1314:4:1314:9|Trying to extract state machine for register sdif3_state
Extracted state machine for register sdif3_state
State machine has 4 reachable states with original encodings of:
   000
   001
   010
   011
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1249:4:1249:9|Trying to extract state machine for register sdif2_state
Extracted state machine for register sdif2_state
State machine has 4 reachable states with original encodings of:
   000
   001
   010
   011
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1184:4:1184:9|Trying to extract state machine for register sdif1_state
Extracted state machine for register sdif1_state
State machine has 4 reachable states with original encodings of:
   000
   001
   010
   011
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1119:4:1119:9|Trying to extract state machine for register sdif0_state
Extracted state machine for register sdif0_state
State machine has 4 reachable states with original encodings of:
   000
   001
   010
   011
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Trying to extract state machine for register sm0_state
Extracted state machine for register sm0_state
State machine has 4 reachable states with original encodings of:
   000
   001
   010
   011
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":56:20:56:28|Input FPLL_LOCK is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":63:20:63:34|Input SDIF1_SPLL_LOCK is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":67:20:67:34|Input SDIF2_SPLL_LOCK is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":71:20:71:34|Input SDIF3_SPLL_LOCK is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":88:20:88:29|Input SDIF1_PSEL is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":89:20:89:31|Input SDIF1_PWRITE is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":90:20:90:31|Input SDIF1_PRDATA is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":91:20:91:29|Input SDIF2_PSEL is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":92:20:92:31|Input SDIF2_PWRITE is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":93:20:93:31|Input SDIF2_PRDATA is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":94:20:94:29|Input SDIF3_PSEL is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":95:20:95:31|Input SDIF3_PWRITE is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":96:20:96:31|Input SDIF3_PRDATA is unused
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigP\5.0.101\rtl\vlog\core\coreconfigp.v":433:4:433:9|Trying to extract state machine for register state
Extracted state machine for register state
State machine has 3 reachable states with original encodings of:
   00
   01
   10
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":128:15:128:23|Input port bit 0 of HTRANS_M0[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":139:15:139:23|Input port bit 0 of HTRANS_M1[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":150:15:150:23|Input port bit 0 of HTRANS_M2[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":161:15:161:23|Input port bit 0 of HTRANS_M3[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":171:15:171:22|Input port bit 1 of HRESP_S0[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":184:15:184:22|Input port bit 1 of HRESP_S1[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":197:15:197:22|Input port bit 1 of HRESP_S2[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":210:15:210:22|Input port bit 1 of HRESP_S3[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":223:15:223:22|Input port bit 1 of HRESP_S4[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":236:15:236:22|Input port bit 1 of HRESP_S5[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":249:15:249:22|Input port bit 1 of HRESP_S6[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":262:15:262:22|Input port bit 1 of HRESP_S7[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":275:15:275:22|Input port bit 1 of HRESP_S8[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":288:15:288:22|Input port bit 1 of HRESP_S9[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":301:15:301:23|Input port bit 1 of HRESP_S10[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":314:15:314:23|Input port bit 1 of HRESP_S11[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":327:15:327:23|Input port bit 1 of HRESP_S12[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":340:15:340:23|Input port bit 1 of HRESP_S13[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":353:15:353:23|Input port bit 1 of HRESP_S14[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":366:15:366:23|Input port bit 1 of HRESP_S15[1:0] is unused

@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":379:15:379:23|Input port bit 1 of HRESP_S16[1:0] is unused

@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":131:15:131:23|Input HBURST_M0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":132:15:132:22|Input HPROT_M0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":142:15:142:23|Input HBURST_M1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":143:15:143:22|Input HPROT_M1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":153:15:153:23|Input HBURST_M2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":154:15:154:22|Input HPROT_M2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":164:15:164:23|Input HBURST_M3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":165:15:165:22|Input HPROT_M3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":58:18:58:26|Input HWDATA_M1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":67:18:67:26|Input HWDATA_M2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":76:18:76:26|Input HWDATA_M3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":80:18:80:26|Input HRDATA_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":81:13:81:24|Input HREADYOUT_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":82:13:82:20|Input HRESP_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":91:18:91:26|Input HRDATA_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":92:13:92:24|Input HREADYOUT_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":93:13:93:20|Input HRESP_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":102:18:102:26|Input HRDATA_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":103:13:103:24|Input HREADYOUT_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":104:13:104:20|Input HRESP_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":113:18:113:26|Input HRDATA_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":114:13:114:24|Input HREADYOUT_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":115:13:115:20|Input HRESP_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":124:18:124:26|Input HRDATA_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":125:13:125:24|Input HREADYOUT_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":126:13:126:20|Input HRESP_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":135:18:135:26|Input HRDATA_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":136:13:136:24|Input HREADYOUT_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":137:13:137:20|Input HRESP_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":146:18:146:26|Input HRDATA_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":147:13:147:24|Input HREADYOUT_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":148:13:148:20|Input HRESP_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":157:18:157:26|Input HRDATA_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":158:13:158:24|Input HREADYOUT_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":159:13:159:20|Input HRESP_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":168:18:168:26|Input HRDATA_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":169:13:169:24|Input HREADYOUT_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":170:13:170:20|Input HRESP_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":179:18:179:26|Input HRDATA_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":180:13:180:24|Input HREADYOUT_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":181:13:181:20|Input HRESP_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":190:18:190:27|Input HRDATA_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":191:13:191:25|Input HREADYOUT_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":192:13:192:21|Input HRESP_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":201:18:201:27|Input HRDATA_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":202:13:202:25|Input HREADYOUT_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":203:13:203:21|Input HRESP_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":212:18:212:27|Input HRDATA_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":213:13:213:25|Input HREADYOUT_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":214:13:214:21|Input HRESP_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":223:18:223:27|Input HRDATA_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":224:13:224:25|Input HREADYOUT_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":225:13:225:21|Input HRESP_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":234:18:234:27|Input HRDATA_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":235:13:235:25|Input HREADYOUT_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":236:13:236:21|Input HRESP_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":245:18:245:27|Input HRDATA_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":246:13:246:25|Input HREADYOUT_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":247:13:247:21|Input HRESP_S15 is unused
@W: CL246 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v":46:15:46:33|Input port bits 3 to 2 of MPREVDATASLAVEREADY[3:0] are unused

@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Trying to extract state machine for register arbRegSMCurrentState
Extracted state machine for register arbRegSMCurrentState
State machine has 16 reachable states with original encodings of:
   0000
   0001
   0010
   0011
   0100
   0101
   0110
   0111
   1000
   1001
   1010
   1011
   1100
   1101
   1110
   1111
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":50:16:50:25|Input SDATAREADY is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":51:16:51:21|Input SHRESP is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":60:16:60:24|Input HRDATA_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":61:11:61:22|Input HREADYOUT_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":62:16:62:24|Input HRDATA_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":63:11:63:22|Input HREADYOUT_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":64:16:64:24|Input HRDATA_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":65:11:65:22|Input HREADYOUT_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":66:16:66:24|Input HRDATA_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":67:11:67:22|Input HREADYOUT_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":68:16:68:24|Input HRDATA_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":69:11:69:22|Input HREADYOUT_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":70:16:70:24|Input HRDATA_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":71:11:71:22|Input HREADYOUT_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":72:16:72:24|Input HRDATA_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":73:11:73:22|Input HREADYOUT_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":74:16:74:24|Input HRDATA_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":75:11:75:22|Input HREADYOUT_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":76:16:76:24|Input HRDATA_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":77:11:77:22|Input HREADYOUT_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":78:16:78:24|Input HRDATA_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":79:11:79:22|Input HREADYOUT_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":80:16:80:25|Input HRDATA_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":81:11:81:23|Input HREADYOUT_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":82:16:82:25|Input HRDATA_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":83:11:83:23|Input HREADYOUT_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":84:16:84:25|Input HRDATA_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":85:11:85:23|Input HREADYOUT_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":86:16:86:25|Input HRDATA_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":87:11:87:23|Input HREADYOUT_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":88:16:88:25|Input HRDATA_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":89:11:89:23|Input HREADYOUT_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":90:16:90:25|Input HRDATA_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":91:11:91:23|Input HREADYOUT_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":92:16:92:25|Input HRDATA_S16 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":93:11:93:23|Input HREADYOUT_S16 is unused
@W: CL246 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":50:16:50:25|Input port bits 15 to 0 of SDATAREADY[16:0] are unused

@W: CL246 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":51:16:51:21|Input port bits 15 to 0 of SHRESP[16:0] are unused

@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":60:16:60:24|Input HRDATA_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":61:11:61:22|Input HREADYOUT_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":62:16:62:24|Input HRDATA_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":63:11:63:22|Input HREADYOUT_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":64:16:64:24|Input HRDATA_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":65:11:65:22|Input HREADYOUT_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":66:16:66:24|Input HRDATA_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":67:11:67:22|Input HREADYOUT_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":68:16:68:24|Input HRDATA_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":69:11:69:22|Input HREADYOUT_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":70:16:70:24|Input HRDATA_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":71:11:71:22|Input HREADYOUT_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":72:16:72:24|Input HRDATA_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":73:11:73:22|Input HREADYOUT_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":74:16:74:24|Input HRDATA_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":75:11:75:22|Input HREADYOUT_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":76:16:76:24|Input HRDATA_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":77:11:77:22|Input HREADYOUT_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":78:16:78:24|Input HRDATA_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":79:11:79:22|Input HREADYOUT_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":80:16:80:25|Input HRDATA_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":81:11:81:23|Input HREADYOUT_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":82:16:82:25|Input HRDATA_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":83:11:83:23|Input HREADYOUT_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":84:16:84:25|Input HRDATA_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":85:11:85:23|Input HREADYOUT_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":86:16:86:25|Input HRDATA_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":87:11:87:23|Input HREADYOUT_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":88:16:88:25|Input HRDATA_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":89:11:89:23|Input HREADYOUT_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":90:16:90:25|Input HRDATA_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":91:11:91:23|Input HREADYOUT_S15 is unused
@N: CL201 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigMaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Trying to extract state machine for register state
Extracted state machine for register state
State machine has 21 reachable states with original encodings of:
   00000
   00001
   00010
   00011
   00100
   00101
   00110
   00111
   01001
   01010
   01011
   01100
   01101
   01110
   01111
   10000
   10001
   10010
   10011
   10100
   10101
@END

At c_ver Exit (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 94MB peak: 121MB)

Process took 0h:00m:02s realtime, 0h:00m:02s cputime
# Fri Apr 18 09:30:51 2014

###########################################################]
Pre-mapping Report

Synopsys Generic Technology Pre-mapping, Version mapact, Build 1154R, Built Jan 20 2014 10:24:19
Copyright (C) 1994-2013, Synopsys, Inc. This software and the associated documentation are proprietary to Synopsys, Inc. This software may only be used in accordance with the terms and conditions of a written license agreement with Synopsys, Inc.  All other use or distribution of the software is strictly prohibited.
Product Version I-2013.09M-SP1 

Mapper Startup Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 99MB)

@L: C:\Microsemi\IGLOO2_Oversampling\synthesis\IGLOO2_Oversampling_top_scck.rpt 
Printing clock  summary report in "C:\Microsemi\IGLOO2_Oversampling\synthesis\IGLOO2_Oversampling_top_scck.rpt" file 
@N: MF248 |Running in 64-bit mode.
@N: MF667 |Clock conversion disabled 

Design Input Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 110MB peak: 112MB)


Mapper Initialization Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 110MB peak: 112MB)


Start loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 111MB peak: 112MB)


Finished loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 111MB peak: 113MB)

@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3567:27:3567:39|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_15,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_14
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3522:27:3522:39|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_14,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_13
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3477:27:3477:39|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_13,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_12
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3432:27:3432:39|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_12,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_11
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3387:27:3387:39|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_11,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3297:26:3297:37|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_9,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3252:27:3252:38|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_8,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3207:27:3207:38|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_7,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3162:27:3162:38|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_6,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3117:27:3117:38|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_5,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3072:27:3072:38|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_4,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3027:27:3027:38|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_3,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":2982:27:2982:38|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_2,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":3342:27:3342:39|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_10,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":2937:27:2937:38|Removing user instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_1,  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_0
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.MDDR_DDR_AXI_S_CORE_RESET_N_int,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.FDDR_CORE_RESET_N_int
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigp\5.0.101\rtl\vlog\core\coreconfigp.v":447:4:447:9|Removing sequential instance MDDR_PENABLE of view:PrimLib.dffr(prim) in hierarchy view:work.CoreConfigP_Z5(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigp\5.0.101\rtl\vlog\core\coreconfigp.v":447:4:447:9|Removing sequential instance FDDR_PENABLE of view:PrimLib.dffr(prim) in hierarchy view:work.CoreConfigP_Z5(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigp\5.0.101\rtl\vlog\core\coreconfigp.v":447:4:447:9|Removing sequential instance SDIF1_PENABLE of view:PrimLib.dffr(prim) in hierarchy view:work.CoreConfigP_Z5(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigp\5.0.101\rtl\vlog\core\coreconfigp.v":447:4:447:9|Removing sequential instance SDIF2_PENABLE of view:PrimLib.dffr(prim) in hierarchy view:work.CoreConfigP_Z5(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigp\5.0.101\rtl\vlog\core\coreconfigp.v":447:4:447:9|Removing sequential instance SDIF3_PENABLE of view:PrimLib.dffr(prim) in hierarchy view:work.CoreConfigP_Z5(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":92:2:92:7|Removing sequential instance reg_tx_val of view:PrimLib.dffre(prim) in hierarchy view:work.prbs7_10_prbs7_10_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":183:2:183:7|Removing sequential instance reg_error_out of view:PrimLib.dffse(prim) in hierarchy view:work.prbs7_10_prbs7_10_0_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":158:2:158:7|Removing sequential instance reg_lock of view:PrimLib.dffre(prim) in hierarchy view:work.prbs7_10_prbs7_10_0_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":205:2:205:7|Removing sequential instance reg_lock_again of view:PrimLib.dffr(prim) in hierarchy view:work.prbs7_10_prbs7_10_0_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":459:0:459:5|Removing sequential instance fifo_write of view:PrimLib.dffs(prim) in hierarchy view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":459:0:459:5|Removing sequential instance clear_parity_en_1 of view:PrimLib.dffr(prim) in hierarchy view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\fabuart.v":91:0:91:5|Removing sequential instance timer_switch_t of view:PrimLib.dffse(prim) in hierarchy view:work.FabUART(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHMASTLOCK of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_1(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHSIZE[2:0] of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_1(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHWRITE of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_1(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHMASTLOCK of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_2(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHSIZE[2:0] of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_2(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHWRITE of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_2(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHMASTLOCK of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_3(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHSIZE[2:0] of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_3(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance regHWRITE of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_3(verilog) because there are no references to its outputs 
@N: BN115 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":2708:2:2708:14|Removing instance masterstage_1 of view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_1(verilog) because there are no references to its outputs 
@N: BN115 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":2771:2:2771:14|Removing instance masterstage_2 of view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_2(verilog) because there are no references to its outputs 
@N: BN115 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":2834:2:2834:14|Removing instance masterstage_3 of view:COREAHBLITE_LIB.COREAHBLITE_MASTERSTAGE_1_1_85_0_0_1_0_masterstage_3(verilog) because there are no references to its outputs 
@N: BN115 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":2892:27:2892:38|Removing instance slavestage_0 of view:COREAHBLITE_LIB.COREAHBLITE_SLAVESTAGE_slavestage_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Removing sequential instance USER_FAB_RESET_N_int of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Removing sequential instance FDDR_CORE_RESET_N_int of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1184:4:1184:9|Removing sequential instance SDIF1_PHY_RESET_N_int of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1184:4:1184:9|Removing sequential instance SDIF1_CORE_RESET_N_0 of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1249:4:1249:9|Removing sequential instance SDIF2_PHY_RESET_N_int of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1249:4:1249:9|Removing sequential instance SDIF2_CORE_RESET_N_0 of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1314:4:1314:9|Removing sequential instance SDIF3_PHY_RESET_N_int of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1314:4:1314:9|Removing sequential instance SDIF3_CORE_RESET_N_0 of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":198:0:198:5|Removing sequential instance overflow of view:PrimLib.dffre(prim) in hierarchy view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":405:0:405:5|Removing sequential instance parity_err of view:PrimLib.dffre(prim) in hierarchy view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":223:0:223:5|Removing sequential instance framing_error of view:PrimLib.dffre(prim) in hierarchy view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1119:4:1119:9|Removing sequential instance SDIF0_PHY_RESET_N_int of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN115 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1642:33:1642:41|Removing instance genblk2\.sdif0_phr of view:work.coreresetp_pcie_hotreset(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1184:4:1184:9|Removing sequential instance sdif1_state[3:0] of view:PrimLib.statemachine(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1249:4:1249:9|Removing sequential instance sdif2_state[3:0] of view:PrimLib.statemachine(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1314:4:1314:9|Removing sequential instance sdif3_state[3:0] of view:PrimLib.statemachine(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":257:4:257:9|Removing sequential instance sdif_core_reset_n of view:PrimLib.dffr(prim) in hierarchy view:work.coreresetp_pcie_hotreset(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1119:4:1119:9|Removing sequential instance SDIF0_CORE_RESET_N_0 of view:PrimLib.dffre(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":257:4:257:9|Removing sequential instance sdif_core_reset_n_q1 of view:PrimLib.dffr(prim) in hierarchy view:work.coreresetp_pcie_hotreset(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v":82:4:82:9|Removing sequential instance masterDataInProg[3:0] of view:PrimLib.dffre(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_SLAVESTAGE_slavestage_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":784:4:784:9|Removing sequential instance sdif1_areset_n_clk_base of view:PrimLib.dffr(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":798:4:798:9|Removing sequential instance sdif2_areset_n_clk_base of view:PrimLib.dffr(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":812:4:812:9|Removing sequential instance sdif3_areset_n_clk_base of view:PrimLib.dffr(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN115 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v":90:29:90:41|Removing instance slave_arbiter of view:COREAHBLITE_LIB.COREAHBLITE_SLAVEARBITER_slave_arbiter(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":784:4:784:9|Removing sequential instance sdif1_areset_n_q1 of view:PrimLib.dffr(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":798:4:798:9|Removing sequential instance sdif2_areset_n_q1 of view:PrimLib.dffr(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":812:4:812:9|Removing sequential instance sdif3_areset_n_q1 of view:PrimLib.dffr(prim) in hierarchy view:work.CoreResetP_Z6(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":255:0:255:5|Removing sequential instance overflow_int of view:PrimLib.dffre(prim) in hierarchy view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":255:0:255:5|Removing sequential instance framing_error_int of view:PrimLib.dffre(prim) in hierarchy view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":179:4:179:9|Removing sequential instance hot_reset_n of view:PrimLib.dffse(prim) in hierarchy view:work.coreresetp_pcie_hotreset(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing sequential instance arbRegSMCurrentState[15:0] of view:PrimLib.statemachine(prim) in hierarchy view:COREAHBLITE_LIB.COREAHBLITE_SLAVEARBITER_slave_arbiter(verilog) because there are no references to its outputs 
syn_allowed_resources : blockrams=21  set on top level netlist IGLOO2_Oversampling_top


Clock Summary
**************

Start                                                                          Requested     Requested     Clock        Clock              
Clock                                                                          Frequency     Period        Type         Group              
-------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock                          100.0 MHz     10.000        inferred     Inferred_clkgroup_5
IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock        100.0 MHz     10.000        inferred     Inferred_clkgroup_6
IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock                       100.0 MHz     10.000        inferred     Inferred_clkgroup_3
IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock                     100.0 MHz     10.000        inferred     Inferred_clkgroup_0
IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     100.0 MHz     10.000        inferred     Inferred_clkgroup_4
IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     100.0 MHz     10.000        inferred     Inferred_clkgroup_1
===========================================================================================================================================

@W: MT530 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\clock_gen.v":275:6:275:11|Found inferred clock IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock which controls 116 sequential elements including UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[12:0]. This clock has no specified timing constraint which may adversely impact design performance. 
@W: MT530 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Found inferred clock IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock which controls 103 sequential elements including Transmitter_0.FIFO_PRBS_0.reg_data_out[9:0]. This clock has no specified timing constraint which may adversely impact design performance. 
@W: MT530 :"c:\microsemi\igloo2_oversampling\component\work\igloo2_oversampling_top\serdes_if_0\igloo2_oversampling_top_serdes_if_0_serdes_if.v":127:52:127:64|Found inferred clock IGLOO2_Oversampling_top_FCCC_0_FCCC|GL1_net_inferred_clock which controls 0 sequential elements including SERDES_IF_0.SERDESIF_INST. This clock has no specified timing constraint which may adversely impact design performance. 
@W: MT530 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigp\5.0.101\rtl\vlog\core\coreconfigp.v":433:4:433:9|Found inferred clock IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock which controls 107 sequential elements including IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PREADY. This clock has no specified timing constraint which may adversely impact design performance. 
@W: MT530 :"c:\microsemi\igloo2_oversampling\hdl\downsampler_rx.v":59:2:59:7|Found inferred clock IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock which controls 299 sequential elements including Receiver_0.Downsampler_0.reg_check[9:0]. This clock has no specified timing constraint which may adversely impact design performance. 
@W: MT530 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigmaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Found inferred clock IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock which controls 480 sequential elements including IGLOO2_Oversampling_0.ConfigMaster_0.state[20:0]. This clock has no specified timing constraint which may adversely impact design performance. 
@W: MT530 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1434:4:1434:9|Found inferred clock IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock which controls 30 sequential elements including IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[12:0]. This clock has no specified timing constraint which may adversely impact design performance. 

Finished Pre Mapping Phase.
@N: BN225 |Writing default property annotation file C:\Microsemi\IGLOO2_Oversampling\synthesis\IGLOO2_Oversampling_top.sap.
Pre-mapping successful!

At Mapper Exit (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 77MB peak: 143MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime
# Fri Apr 18 09:30:54 2014

###########################################################]
Map & Optimize Report

Synopsys Generic Technology Mapper, Version mapact, Build 1154R, Built Jan 20 2014 10:24:19
Copyright (C) 1994-2013, Synopsys, Inc. This software and the associated documentation are proprietary to Synopsys, Inc. This software may only be used in accordance with the terms and conditions of a written license agreement with Synopsys, Inc.  All other use or distribution of the software is strictly prohibited.
Product Version I-2013.09M-SP1 

Mapper Startup Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 100MB)

@N: MF248 |Running in 64-bit mode.
@N: MF667 |Clock conversion disabled 

Design Input Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 101MB)


Mapper Initialization Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 101MB)


Start loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 100MB peak: 101MB)


Finished loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 100MB peak: 103MB)



Starting Optimization and Mapping (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 139MB peak: 140MB)

@W: MO111 :"c:\microsemi\igloo2_oversampling\component\work\igloo2_oversampling\fabosc_0\igloo2_oversampling_fabosc_0_osc.v":20:7:20:16|Tristate driver XTLOSC_O2F on net XTLOSC_O2F has its enable tied to GND (module IGLOO2_Oversampling_FABOSC_0_OSC) 
@W: MO111 :"c:\microsemi\igloo2_oversampling\component\work\igloo2_oversampling\fabosc_0\igloo2_oversampling_fabosc_0_osc.v":19:7:19:16|Tristate driver XTLOSC_CCC on net XTLOSC_CCC has its enable tied to GND (module IGLOO2_Oversampling_FABOSC_0_OSC) 
@W: MO111 :"c:\microsemi\igloo2_oversampling\component\work\igloo2_oversampling\fabosc_0\igloo2_oversampling_fabosc_0_osc.v":18:7:18:20|Tristate driver RCOSC_1MHZ_O2F on net RCOSC_1MHZ_O2F has its enable tied to GND (module IGLOO2_Oversampling_FABOSC_0_OSC) 
@W: MO111 :"c:\microsemi\igloo2_oversampling\component\work\igloo2_oversampling\fabosc_0\igloo2_oversampling_fabosc_0_osc.v":17:7:17:20|Tristate driver RCOSC_1MHZ_CCC on net RCOSC_1MHZ_CCC has its enable tied to GND (module IGLOO2_Oversampling_FABOSC_0_OSC) 
@W: MO111 :"c:\microsemi\igloo2_oversampling\component\work\igloo2_oversampling\fabosc_0\igloo2_oversampling_fabosc_0_osc.v":15:7:15:24|Tristate driver RCOSC_25_50MHZ_CCC on net RCOSC_25_50MHZ_CCC has its enable tied to GND (module IGLOO2_Oversampling_FABOSC_0_OSC) 
@W: MO171 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Sequential instance Transmitter_0.FIFO_PRBS_0.reg_tx_val_out reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":668:4:668:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF1_PERST_N_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":687:4:687:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF2_PERST_N_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":706:4:706:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF3_PERST_N_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":668:4:668:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF1_PERST_N_q2 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":687:4:687:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF2_PERST_N_q2 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":706:4:706:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF3_PERST_N_q2 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":649:4:649:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF0_PERST_N_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":668:4:668:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF1_PERST_N_q3 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":687:4:687:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF2_PERST_N_q3 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":706:4:706:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF3_PERST_N_q3 reduced to a combinational gate by constant propagation 
@W: MO171 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":742:4:742:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sm1_areset_n_q1 reduced to a combinational gate by constant propagation 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":92:2:92:7|Removing sequential instance tx_count[2:0] of view:PrimLib.statemachine(prim) in hierarchy view:work.prbs7_10_prbs7_10_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":92:2:92:7|Removing sequential instance rx_count[2:0] of view:PrimLib.statemachine(prim) in hierarchy view:work.prbs7_10_prbs7_10_0_0(verilog) because there are no references to its outputs 
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":936:4:936:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif3_spll_lock_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sdif0_spll_lock_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":936:4:936:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif3_spll_lock_q2,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sdif0_spll_lock_q2
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":742:4:742:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sm1_areset_n_clk_base,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF0_PERST_N_q2
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":871:4:871:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif2_areset_n_rcosc_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sdif1_areset_n_rcosc_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":885:4:885:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif3_areset_n_rcosc_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sdif1_areset_n_rcosc_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":829:4:829:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_rcosc_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sdif1_areset_n_rcosc_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":885:4:885:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif3_areset_n_rcosc,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_rcosc
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":871:4:871:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif2_areset_n_rcosc,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_rcosc
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":857:4:857:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif1_areset_n_rcosc,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_rcosc
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1530:4:1530:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif3_core,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.ddr_ready
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1498:4:1498:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif2_core,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.ddr_ready
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1466:4:1466:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif1_core,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.ddr_ready
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1595:4:1595:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif2_core_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif1_core_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1595:4:1595:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif3_core_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif1_core_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1595:4:1595:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif1_core_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.ddr_ready_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1595:4:1595:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif3_core_clk_base,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif2_core_clk_base
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1595:4:1595:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif2_core_clk_base,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif1_core_clk_base
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1595:4:1595:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.release_sdif1_core_clk_base,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.ddr_ready_clk_base

Available hyper_sources - for debug and ip models
	None Found

@W: MO129 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":649:4:649:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF0_PERST_N_q2 reduced to a combinational gate by constant propagation
@W: MO129 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1337:4:1337:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.RESET_N_F2M_int reduced to a combinational gate by constant propagation
@W: MO129 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":649:4:649:9|Sequential instance IGLOO2_Oversampling_0.CORERESETP_0.SDIF0_PERST_N_q3 reduced to a combinational gate by constant propagation
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":857:4:857:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif1_areset_n_rcosc_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sdif0_areset_n_rcosc_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":728:4:728:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_q1,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sdif0_areset_n_q1
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":843:4:843:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif0_areset_n_rcosc,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_rcosc
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":770:4:770:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sdif0_areset_n_clk_base,  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_clk_base
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":183:2:183:7|Removing sequential instance reg_error[5:0] of view:PrimLib.dffr(prim) in hierarchy view:work.prbs7_10_prbs7_10_0_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":379:0:379:5|Removing sequential instance rx_parity_calc of view:PrimLib.dffre(prim) in hierarchy view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\fabuart.v":91:0:91:5|Removing sequential instance switch_t of view:PrimLib.dffre(prim) in hierarchy view:work.FabUART(verilog) because there are no references to its outputs 
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Removing sequential instance IGLOO2_Oversampling_0.CORERESETP_0.sm0_state[3:0],  because it is equivalent to instance IGLOO2_Oversampling_0.CORERESETP_0.sdif0_state[3:0]

Finished RTL optimizations (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 138MB peak: 141MB)

@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance CoreAHBLite_0.matrix4x16.masterstage_0.regHSIZE[2] in hierarchy view:work.IGLOO2_Oversampling(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v":82:4:82:9|Removing sequential instance CoreAHBLite_0.matrix4x16.slavestage_16.masterDataInProg[3] in hierarchy view:work.IGLOO2_Oversampling(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v":82:4:82:9|Removing sequential instance CoreAHBLite_0.matrix4x16.slavestage_16.masterDataInProg[2] in hierarchy view:work.IGLOO2_Oversampling(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v":82:4:82:9|Removing sequential instance CoreAHBLite_0.matrix4x16.slavestage_16.masterDataInProg[1] in hierarchy view:work.IGLOO2_Oversampling(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":233:0:233:5|Removing sequential instance CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[0] in hierarchy view:work.IGLOO2_Oversampling(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":233:0:233:5|Removing sequential instance CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[2] in hierarchy view:work.IGLOO2_Oversampling(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":233:0:233:5|Removing sequential instance CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[4] in hierarchy view:work.IGLOO2_Oversampling(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":233:0:233:5|Removing sequential instance CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[6] in hierarchy view:work.IGLOO2_Oversampling(verilog) because there are no references to its outputs 
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.regHADDR[31],  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.regHADDR[28]
Encoding state machine state[20:0] (view:work.CoreConfigMaster_Z1(verilog))
original code -> new code
   00000 -> 000000000000000000001
   00001 -> 000000000000000000010
   00010 -> 000000000000000000100
   00011 -> 000000000000000001000
   00100 -> 000000000000000010000
   00101 -> 000000000000000100000
   00110 -> 000000000000001000000
   00111 -> 000000000000010000000
   01001 -> 000000000000100000000
   01010 -> 000000000001000000000
   01011 -> 000000000010000000000
   01100 -> 000000000100000000000
   01101 -> 000000001000000000000
   01110 -> 000000010000000000000
   01111 -> 000000100000000000000
   10000 -> 000001000000000000000
   10001 -> 000010000000000000000
   10010 -> 000100000000000000000
   10011 -> 001000000000000000000
   10100 -> 010000000000000000000
   10101 -> 100000000000000000000
@N:"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigmaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Found counter in view:work.CoreConfigMaster_Z1(verilog) inst pause_count[4:0]
@N: MF179 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigmaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":509:21:509:46|Found 32 bit by 32 bit '==' comparator, 'd_state128'
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigmaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Removing sequential instance HSIZE[2] in hierarchy view:work.CoreConfigMaster_Z1(verilog) because there are no references to its outputs 
@A: BN291 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigmaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Boundary register HSIZE[2] packed into a complex cell. To disable register packing, set syn_keep=1 on net between register and complex cell. 
Encoding state machine arbRegSMCurrentState[15:0] (view:COREAHBLITE_LIB.COREAHBLITE_SLAVEARBITER_slave_arbiter_0(verilog))
original code -> new code
   0000 -> 0000000000000001
   0001 -> 0000000000000010
   0010 -> 0000000000000100
   0011 -> 0000000000001000
   0100 -> 0000000000010000
   0101 -> 0000000000100000
   0110 -> 0000000001000000
   0111 -> 0000000010000000
   1000 -> 0000000100000000
   1001 -> 0000001000000000
   1010 -> 0000010000000000
   1011 -> 0000100000000000
   1100 -> 0001000000000000
   1101 -> 0010000000000000
   1110 -> 0100000000000000
   1111 -> 1000000000000000
@W: MO160 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Register bit arbRegSMCurrentState[12] is always 0, optimizing ...
@W: MO160 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Register bit arbRegSMCurrentState[8] is always 0, optimizing ...
@W: MO160 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Register bit arbRegSMCurrentState[4] is always 0, optimizing ...
Encoding state machine state[2:0] (view:work.CoreConfigP_Z5(verilog))
original code -> new code
   00 -> 00
   01 -> 01
   10 -> 10
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigp\5.0.101\rtl\vlog\core\coreconfigp.v":241:4:241:9|Removing sequential instance paddr[16] in hierarchy view:work.CoreConfigP_Z5(verilog) because there are no references to its outputs 
Encoding state machine sdif0_state[3:0] (view:work.CoreResetP_Z6(verilog))
original code -> new code
   000 -> 00
   001 -> 01
   010 -> 10
   011 -> 11
@N:"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreresetp\5.1.100\rtl\vlog\core\coreresetp.v":1434:4:1434:9|Found counter in view:work.CoreResetP_Z6(verilog) inst count_sdif0[12:0]
Encoding state machine rx_count[2:0] (view:work.prbs7_10_prbs7_10_0(verilog))
original code -> new code
   00 -> 00
   01 -> 01
   10 -> 10
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":92:2:92:7|Removing sequential instance LFSR[8] in hierarchy view:work.prbs7_10_prbs7_10_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":92:2:92:7|Removing sequential instance LFSR[9] in hierarchy view:work.prbs7_10_prbs7_10_0(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":92:2:92:7|Removing sequential instance LFSR[10] in hierarchy view:work.prbs7_10_prbs7_10_0(verilog) because there are no references to its outputs 
@N:"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":183:2:183:7|Found counter in view:work.prbs7_10_prbs7_10_0(verilog) inst reg_error[5:0]
@N: MF179 :"c:\microsemi\igloo2_oversampling\hdl\prbs_gencheck.v":188:118:188:131|Found 10 bit by 10 bit '==' comparator, 'un1_data_in'
Encoding state machine DA_FSM_STATE[3:0] (view:work.rx_data_aligner(verilog))
original code -> new code
   00 -> 00
   01 -> 01
   10 -> 10
   11 -> 11
Encoding state machine RC_FSM_state[2:0] (view:work.receive_control(verilog))
original code -> new code
   00 -> 00
   01 -> 01
   10 -> 10
Encoding state machine i[2:0] (view:work.FIFO_PRBS(verilog))
original code -> new code
   00 -> 00
   01 -> 01
   10 -> 10
Encoding state machine tx_count[2:0] (view:work.prbs7_10_prbs7_10_0_0(verilog))
original code -> new code
   00 -> 00
   01 -> 01
   10 -> 10
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\coreuart.v":154:0:154:5|Removing instance UART_INTERFACE_0.COREUART_0.tx_hold_reg[7],  because it is equivalent to instance UART_INTERFACE_0.COREUART_0.tx_hold_reg[6]
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\coreuart.v":154:0:154:5|Removing sequential instance tx_hold_reg[6] in hierarchy view:work.UART_INTERFACE_COREUART_0_COREUART_0s_0s_0s_19s_0s(verilog) because there are no references to its outputs 
@N:"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\clock_gen.v":275:6:275:11|Found counter in view:work.UART_INTERFACE_COREUART_0_Clock_gen_0s(verilog) inst genblk1\.baud_cntr[12:0]
Encoding state machine xmit_state[5:0] (view:work.UART_INTERFACE_COREUART_0_Tx_async_0s_0s_1s_2s_3s_4s_5s_6s(verilog))
original code -> new code
   00000000000000000000000000000000 -> 000001
   00000000000000000000000000000001 -> 000010
   00000000000000000000000000000010 -> 000100
   00000000000000000000000000000011 -> 001000
   00000000000000000000000000000100 -> 010000
   00000000000000000000000000000101 -> 100000
@W: MO160 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\tx_async.v":112:0:112:5|Register bit xmit_state[4] is always 0, optimizing ...
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\tx_async.v":332:0:332:5|Removing sequential instance tx_parity in hierarchy view:work.UART_INTERFACE_COREUART_0_Tx_async_0s_0s_1s_2s_3s_4s_5s_6s(verilog) because there are no references to its outputs 
Encoding state machine rx_state[2:0] (view:work.UART_INTERFACE_COREUART_0_Rx_async_0s_0s_1s_2s(verilog))
original code -> new code
   00 -> 00
   01 -> 01
   10 -> 10
Encoding state machine state[17:0] (view:work.FabUART(verilog))
original code -> new code
   00000 -> 000000000000000001
   00001 -> 000000000000000010
   00010 -> 000000000000000100
   00011 -> 000000000000001000
   00100 -> 000000000000010000
   00101 -> 000000000000100000
   00110 -> 000000000001000000
   00111 -> 000000000010000000
   01000 -> 000000000100000000
   01001 -> 000000001000000000
   01010 -> 000000010000000000
   01011 -> 000000100000000000
   01100 -> 000001000000000000
   01101 -> 000010000000000000
   01110 -> 000100000000000000
   01111 -> 001000000000000000
   10000 -> 010000000000000000
   10001 -> 100000000000000000
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\tx_async.v":112:0:112:5|Removing instance UART_INTERFACE_0.COREUART_0.make_TX.tx_byte[7],  because it is equivalent to instance UART_INTERFACE_0.COREUART_0.make_TX.tx_byte[6]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[28],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[27]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[29],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[27]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[25],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[24]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[26],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[24]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[22],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[21]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[23],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[21]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[20],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[19]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[19],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[18]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[16],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[15]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[17],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[15]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[13],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[12]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[14],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[12]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[10],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[9]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[11],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[9]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[7],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[6]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[8],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[6]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[4],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[3]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[5],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[3]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[1],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[0]
@W: BN132 :"c:\microsemi\igloo2_oversampling\hdl\fifo_prbs.v":74:1:74:6|Removing instance Transmitter_0.FIFO_PRBS_0.data[2],  because it is equivalent to instance Transmitter_0.FIFO_PRBS_0.data[0]
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":167:0:167:5|Removing sequential instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.regHADDR[28] in hierarchy view:work.IGLOO2_Oversampling_top(verilog) because there are no references to its outputs 
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\tx_async.v":112:0:112:5|Removing sequential instance UART_INTERFACE_0.COREUART_0.make_TX.tx_byte[6] in hierarchy view:work.IGLOO2_Oversampling_top(verilog) because there are no references to its outputs 

Finished factoring (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 154MB peak: 155MB)


Finished gated-clock and generated-clock conversion (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 150MB peak: 156MB)

@N: BN362 :"c:\microsemi\igloo2_oversampling\component\work\uart_interface\coreuart_0\rtl\vlog\core\rx_async.v":335:0:335:5|Removing sequential instance UART_INTERFACE_0.COREUART_0.make_RX.rx_shift[8] in hierarchy view:work.IGLOO2_Oversampling_top(verilog) because there are no references to its outputs 

Finished generic timing optimizations - Pass 1 (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 149MB peak: 156MB)

@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[7],  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[11]
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[15],  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[11]
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[14],  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[6]
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[10],  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[6]
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing sequential instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[11] in hierarchy view:work.IGLOO2_Oversampling_top(verilog) because there are no references to its outputs 
@N: FX404 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigmaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":147:8:147:11|Found addmux in view:work.IGLOO2_Oversampling_top(verilog) inst IGLOO2_Oversampling_0.ConfigMaster_0.d_bytecount_0[15:0] from IGLOO2_Oversampling_0.ConfigMaster_0.un1_bytecount_16[15:0] 

Starting Early Timing Optimization (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:01s; Memory used current: 149MB peak: 156MB)


Finished Early Timing Optimization (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:01s; Memory used current: 149MB peak: 156MB)


Finished generic timing optimizations - Pass 2 (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:01s; Memory used current: 149MB peak: 156MB)

@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing sequential instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[6] in hierarchy view:work.IGLOO2_Oversampling_top(verilog) because there are no references to its outputs 
@W: BN132 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[9],  because it is equivalent to instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[5]
@N: BN362 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreahblite\5.0.100\rtl\vlog\core\coreahblite_slavearbiter.v":452:4:452:9|Removing sequential instance IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.slave_arbiter.arbRegSMCurrentState[5] in hierarchy view:work.IGLOO2_Oversampling_top(verilog) because there are no references to its outputs 

Finished preparing to map (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 150MB peak: 156MB)


Finished technology mapping (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 163MB peak: 165MB)

Pass		 CPU time		Worst Slack		Luts / Registers
------------------------------------------------------------
Pass		 CPU time		Worst Slack		Luts / Registers
------------------------------------------------------------
   1		0h:00m:02s		   -25.38ns		1092 /      1009
   2		0h:00m:02s		   -24.54ns		1092 /      1009
   3		0h:00m:02s		   -24.54ns		1092 /      1009
------------------------------------------------------------

@N: FX271 :"c:\microsemi\igloo2_oversampling\component\actel\directcore\coreconfigmaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Instance "IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[0]" with 5 loads replicated 1 times to improve timing 
Timing driven replication report
Added 1 Registers via timing driven replication
Added 1 LUTs via timing driven replication



Pass		 CPU time		Worst Slack		Luts / Registers
------------------------------------------------------------
   1		0h:00m:02s		   -15.06ns		1104 /      1010
------------------------------------------------------------



Pass		 CPU time		Worst Slack		Luts / Registers
------------------------------------------------------------
   1		0h:00m:02s		   -15.06ns		1104 /      1010
------------------------------------------------------------

@N: FP130 |Promoting Net SERDES_IF_0_EPCS_1_TX_CLK on CLKINT  I_134 
@N: FP130 |Promoting Net IGLOO2_Oversampling_0_INIT_APB_S_PCLK on CLKINT  I_135 
@N: FP130 |Promoting Net IGLOO2_Oversampling_0_INIT_APB_S_PRESET_N on CLKINT  I_136 
@N: FP130 |Promoting Net SERDES_IF_0_EPCS_1_RX_CLK on CLKINT  I_137 
@N: FP130 |Promoting Net IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_rcosc on CLKINT  I_138 
@N: FP130 |Promoting Net IGLOO2_Oversampling_0.CORERESETP_0.sm0_areset_n_clk_base on CLKINT  I_139 
@N: FP130 |Promoting Net Receiver_0.AND3_0_Y on CLKINT  I_140 
@N: FP130 |Promoting Net Transmitter_0.EPCS_TX_RESET_net_0 on CLKINT  I_141 
@N: FP130 |Promoting Net FCCC_0_LOCK on CLKINT  I_142 
@N: FP130 |Promoting Net IGLOO2_Oversampling_0.HPMS_READY_i_0_i on CLKINT  I_143 

Added 0 Buffers
Added 0 Cells via replication
	Added 0 Sequential Cells via replication
	Added 0 Combinational Cells via replication

Finished technology timing optimizations and critical path resynthesis (Real Time elapsed 0h:00m:03s; CPU Time elapsed 0h:00m:03s; Memory used current: 152MB peak: 165MB)


Finished restoring hierarchy (Real Time elapsed 0h:00m:03s; CPU Time elapsed 0h:00m:03s; Memory used current: 152MB peak: 165MB)



#### START OF CLOCK OPTIMIZATION REPORT #####[

Clock optimization not enabled
6 non-gated/non-generated clock tree(s) driving 907 clock pin(s) of sequential element(s)
1 gated/generated clock tree(s) driving 106 clock pin(s) of sequential element(s)
0 instances converted, 106 sequential instances remain driven by gated/generated clocks

===================================================================== Non-Gated/Non-Generated Clocks ======================================================================
Clock Tree ID     Driving Element                                         Drive Element Type     Fanout     Sample Instance                                                
---------------------------------------------------------------------------------------------------------------------------------------------------------------------------
@K:CKID0002       SERDES_IF_0.SERDESIF_INST                               SERDESIF_0             289        Receiver_0.prbs7_10_0.reg_error[5]                             
@K:CKID0003       SERDES_IF_0.SERDESIF_INST                               SERDESIF_0             69         Transmitter_0.Replicator_0.reg_tx_val_out                      
@K:CKID0004       IGLOO2_Oversampling_0.CCC_0.GL0_INST                    CLKINT                 423        IGLOO2_Oversampling_0.IGLOO2_Oversampling_HPMS_0.MSS_ADLIB_INST
@K:CKID0005       FCCC_0.GL0_INST                                         CLKINT                 106        UART_INTERFACE_0.FabUART_0.state[14]                           
@K:CKID0006       IGLOO2_Oversampling_0.FABOSC_0.I_RCOSC_25_50MHZ_FAB     RCOSC_25_50MHZ_FAB     19         IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[12]             
@K:CKID0007       FCCC_0.GL1_INST                                         CLKINT                 1          SERDES_IF_0.SERDESIF_INST                                      
===========================================================================================================================================================================
============================================================================================================== Gated/Generated Clocks ===============================================================================================================
Clock Tree ID     Driving Element                                                     Drive Element Type     Fanout     Sample Instance                                      Explanation                                                             
-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
@K:CKID0001       IGLOO2_Oversampling_0.IGLOO2_Oversampling_HPMS_0.MSS_ADLIB_INST     MSS_010                106        IGLOO2_Oversampling_0.CORECONFIGP_0.INIT_DONE_q3     No generated or derived clock directive on output of sequential instance
=====================================================================================================================================================================================================================================================


##### END OF CLOCK OPTIMIZATION REPORT ######]

Writing Analyst data base C:\Microsemi\IGLOO2_Oversampling\synthesis\IGLOO2_Oversampling_top.srm

Finished Writing Netlist Databases (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:03s; Memory used current: 147MB peak: 165MB)

Writing EDIF Netlist and constraint files
@N: BW103 |Synopsys Constraint File time units using default value of 1ns 
@N: BW107 |Synopsys Constraint File capacitance units using default value of 1pF 
I-2013.09M-SP1 

Finished Writing EDIF Netlist and constraint files (Real Time elapsed 0h:00m:05s; CPU Time elapsed 0h:00m:04s; Memory used current: 148MB peak: 165MB)

@W: MT246 :"c:\microsemi\igloo2_oversampling\component\work\igloo2_oversampling\igloo2_oversampling.v":1003:9:1003:20|Blackbox SYSRESET is missing a user supplied timing model. This may have a negative effect on timing analysis and optimizations (Quality of Results) 
@W: MT246 :"c:\microsemi\igloo2_oversampling\component\work\igloo2_oversampling\ccc_0\igloo2_oversampling_ccc_0_fccc.v":23:36:23:43|Blackbox CCC is missing a user supplied timing model. This may have a negative effect on timing analysis and optimizations (Quality of Results) 
@W: MT420 |Found inferred clock IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock with period 10.00ns. Please declare a user-defined clock on object "n:SERDES_IF_0.EPCS_1_RX_CLK"

@W: MT420 |Found inferred clock IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock with period 10.00ns. Please declare a user-defined clock on object "n:SERDES_IF_0.EPCS_1_TX_CLK"

@W: MT420 |Found inferred clock IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock with period 10.00ns. Please declare a user-defined clock on object "n:IGLOO2_Oversampling_0.IGLOO2_Oversampling_HPMS_0.FIC_2_APB_M_PCLK"

@W: MT420 |Found inferred clock IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock with period 10.00ns. Please declare a user-defined clock on object "n:IGLOO2_Oversampling_0.FABOSC_0.N_RCOSC_25_50MHZ_CLKOUT"

@W: MT420 |Found inferred clock IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock with period 10.00ns. Please declare a user-defined clock on object "n:IGLOO2_Oversampling_0.CCC_0.GL0_net"

@W: MT420 |Found inferred clock IGLOO2_Oversampling_top_FCCC_0_FCCC|GL1_net_inferred_clock with period 10.00ns. Please declare a user-defined clock on object "n:FCCC_0.GL1_net"

@W: MT420 |Found inferred clock IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock with period 10.00ns. Please declare a user-defined clock on object "n:FCCC_0.GL0_net"



##### START OF TIMING REPORT #####[
# Timing Report written on Fri Apr 18 09:31:00 2014
#


Top view:               IGLOO2_Oversampling_top
Requested Frequency:    100.0 MHz
Wire load mode:         top
Paths requested:        5
Constraint File(s):    
@N: MT320 |Timing report estimates place and route data. Please look at the place and route timing report for final timing.

@N: MT322 |Clock constraints cover only FF-to-FF paths associated with the clock.



Performance Summary 
*******************


Worst slack in design: 0.862

                                                                               Requested     Estimated     Requested     Estimated               Clock        Clock              
Starting Clock                                                                 Frequency     Frequency     Period        Period        Slack     Type         Group              
---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock                          100.0 MHz     110.5 MHz     10.000        9.053         0.947     inferred     Inferred_clkgroup_5
IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock        100.0 MHz     408.6 MHz     10.000        2.447         7.553     inferred     Inferred_clkgroup_6
IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock                       100.0 MHz     120.8 MHz     10.000        8.277         0.862     inferred     Inferred_clkgroup_3
IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock                     100.0 MHz     219.4 MHz     10.000        4.557         5.443     inferred     Inferred_clkgroup_0
IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     100.0 MHz     148.4 MHz     10.000        6.738         3.262     inferred     Inferred_clkgroup_4
IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     100.0 MHz     400.7 MHz     10.000        2.496         7.504     inferred     Inferred_clkgroup_1
System                                                                         100.0 MHz     NA            10.000        NA            NA        system       system_clkgroup    
=================================================================================================================================================================================





Clock Relationships
*******************

Clocks                                                                                                                                                  |    rise  to  rise   |    fall  to  fall   |    rise  to  fall   |    fall  to  rise 
----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
Starting                                                                    Ending                                                                      |  constraint  slack  |  constraint  slack  |  constraint  slack  |  constraint  slack
----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock                  IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock                  |  10.000      5.443  |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock                  IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock  |  Diff grp    -      |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock                  IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock  |  Diff grp    -      |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock  IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock  |  10.000      7.504  |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock                    IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock                    |  10.000      2.983  |  No paths    -      |  5.000       2.951  |  5.000       0.862
IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock                    IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock                       |  Diff grp    -      |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock  IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock                  |  Diff grp    -      |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock  IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock  |  10.000      3.262  |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock                       IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock                    |  Diff grp    -      |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock                       IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock                       |  10.000      0.947  |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock                       IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     |  Diff grp    -      |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock                       |  Diff grp    -      |  No paths    -      |  No paths    -      |  No paths    -    
IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     |  10.000      7.553  |  No paths    -      |  No paths    -      |  No paths    -    
==============================================================================================================================================================================================================================================
 Note: 'No paths' indicates there are no paths in the design for that pair of clock edges.
       'Diff grp' indicates that paths exist but the starting clock and ending clock are in different clock groups.



Interface Information 
*********************

No IO constraint found



====================================
Detailed Report for Clock: IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock
====================================



Starting Points with Worst Slack
********************************

                                                                                 Starting                                                                                                                      Arrival          
Instance                                                                         Reference                                                 Type        Pin                Net                                  Time        Slack
                                                                                 Clock                                                                                                                                          
--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_0.IGLOO2_Oversampling_HPMS_0.MSS_ADLIB_INST                  IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     MSS_010     F_FM0_READYOUT     CoreAHBLite_0_AHBmslave16_HREADY     2.910       0.947
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[3]      IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[3]                       0.076       1.941
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[10]     IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[10]                      0.076       2.008
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[8]      IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[8]                       0.076       2.155
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[11]     IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[11]                      0.076       2.223
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[9]      IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[9]                       0.076       2.227
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[13]     IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[13]                      0.076       2.264
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[12]     IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[12]                      0.076       2.294
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[1]      IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[1]                       0.076       2.319
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.SDATASELInt[15]     IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE         Q                  SDATASELInt[15]                      0.076       2.332
================================================================================================================================================================================================================================


Ending Points with Worst Slack
******************************

                                                       Starting                                                                                            Required          
Instance                                               Reference                                                 Type     Pin     Net                      Time         Slack
                                                       Clock                                                                                                                 
-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[4]          IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR[4]               9.778        0.947
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[0]          IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR[0]               9.848        1.179
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR_fast[0]     IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR_fast[0]          9.848        1.179
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[15]         IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR_0_iv_i_0[15]     9.778        1.198
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[16]         IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR_0_iv_i_0[16]     9.778        1.198
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[17]         IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR_0_iv_i_0[17]     9.778        1.198
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[31]         IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR[31]              9.778        1.217
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[1]          IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR[1]               9.848        1.244
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[2]          IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR[2]               9.848        1.244
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[5]          IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock     SLE      D       d_HADDR[5]               9.848        1.244
=============================================================================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      10.000
    - Setup time:                            0.222
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         9.778

    - Propagation time:                      8.831
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 0.947

    Number of logic level(s):                6
    Starting point:                          IGLOO2_Oversampling_0.IGLOO2_Oversampling_HPMS_0.MSS_ADLIB_INST / F_FM0_READYOUT
    Ending point:                            IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[4] / D
    The start point is clocked by            IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock [rising] on pin CLK_BASE
    The end   point is clocked by            IGLOO2_Oversampling_CCC_0_FCCC|GL0_net_inferred_clock [rising] on pin CLK

Instance / Net                                                                                            Pin                Pin               Arrival     No. of    
Name                                                                                          Type        Name               Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_0.IGLOO2_Oversampling_HPMS_0.MSS_ADLIB_INST                               MSS_010     F_FM0_READYOUT     Out     2.910     2.910       -         
CoreAHBLite_0_AHBmslave16_HREADY                                                              Net         -                  -       0.989     -           11        
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.masterDataInProg_RNI7TTB1[0]     CFG4        C                  In      -         3.899       -         
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.slavestage_16.masterDataInProg_RNI7TTB1[0]     CFG4        Y                  Out     0.196     4.095       -         
d_bytecount_3_sqmuxa_1                                                                        Net         -                  -       0.761     -           12        
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.HREADY_M_iv                      CFG2        A                  In      -         4.856       -         
IGLOO2_Oversampling_0.CoreAHBLite_0.matrix4x16.masterstage_0.HREADY_M_iv                      CFG2        Y                  Out     0.076     4.932       -         
HREADY_i_3                                                                                    Net         -                  -       0.914     -           32        
IGLOO2_Oversampling_0.ConfigMaster_0.un1_d_HWRITE_1_sqmuxa                                    CFG4        D                  In      -         5.846       -         
IGLOO2_Oversampling_0.ConfigMaster_0.un1_d_HWRITE_1_sqmuxa                                    CFG4        Y                  Out     0.384     6.230       -         
un1_d_HWRITE_1_sqmuxa                                                                         Net         -                  -       0.914     -           32        
IGLOO2_Oversampling_0.ConfigMaster_0.d_HADDR_0_iv_2_RNO[4]                                    CFG2        A                  In      -         7.144       -         
IGLOO2_Oversampling_0.ConfigMaster_0.d_HADDR_0_iv_2_RNO[4]                                    CFG2        Y                  Out     0.067     7.212       -         
un32_d_HADDR_m[4]                                                                             Net         -                  -       0.483     -           1         
IGLOO2_Oversampling_0.ConfigMaster_0.d_HADDR_0_iv_2[4]                                        CFG4        B                  In      -         7.695       -         
IGLOO2_Oversampling_0.ConfigMaster_0.d_HADDR_0_iv_2[4]                                        CFG4        Y                  Out     0.143     7.838       -         
d_HADDR_0_iv_2[4]                                                                             Net         -                  -       0.483     -           1         
IGLOO2_Oversampling_0.ConfigMaster_0.d_HADDR_0_iv[4]                                          CFG4        D                  In      -         8.321       -         
IGLOO2_Oversampling_0.ConfigMaster_0.d_HADDR_0_iv[4]                                          CFG4        Y                  Out     0.372     8.693       -         
d_HADDR[4]                                                                                    Net         -                  -       0.138     -           1         
IGLOO2_Oversampling_0.ConfigMaster_0.HADDR[4]                                                 SLE         D                  In      -         8.831       -         
=====================================================================================================================================================================
Total path delay (propagation time + setup) of 9.053 is 4.371(48.3%) logic and 4.683(51.7%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value




====================================
Detailed Report for Clock: IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock
====================================



Starting Points with Worst Slack
********************************

                                                      Starting                                                                                                        Arrival          
Instance                                              Reference                                                                   Type     Pin     Net                Time        Slack
                                                      Clock                                                                                                                            
---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[0]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[0]     0.076       7.553
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[1]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[1]     0.094       7.746
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[2]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[2]     0.094       7.760
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[3]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[3]     0.094       7.774
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[4]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[4]     0.094       7.789
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[5]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[5]     0.094       7.803
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[6]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[6]     0.094       7.817
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[7]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[7]     0.094       7.831
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[8]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[8]     0.094       7.845
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[9]     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      Q       count_sdif0[9]     0.094       7.858
=======================================================================================================================================================================================


Ending Points with Worst Slack
******************************

                                                          Starting                                                                                                             Required          
Instance                                                  Reference                                                                   Type     Pin     Net                     Time         Slack
                                                          Clock                                                                                                                                  
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_0.CORERESETP_0.release_sdif0_core     IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      EN      release_sdif0_core4     9.707        7.553
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[12]        IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[12]       9.778        7.681
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[11]        IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[11]       9.778        7.695
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[10]        IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[10]       9.778        7.709
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[9]         IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[9]        9.778        7.723
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[8]         IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[8]        9.778        7.738
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[7]         IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[7]        9.778        7.752
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[6]         IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[6]        9.778        7.766
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[5]         IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[5]        9.778        7.780
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[4]         IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock     SLE      D       count_sdif0_s[4]        9.778        7.795
=================================================================================================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      10.000
    - Setup time:                            0.293
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         9.707

    - Propagation time:                      2.154
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 7.553

    Number of logic level(s):                2
    Starting point:                          IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[0] / Q
    Ending point:                            IGLOO2_Oversampling_0.CORERESETP_0.release_sdif0_core / EN
    The start point is clocked by            IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock [rising] on pin CLK
    The end   point is clocked by            IGLOO2_Oversampling_FABOSC_0_OSC|N_RCOSC_25_50MHZ_CLKOUT_inferred_clock [rising] on pin CLK

Instance / Net                                                        Pin      Pin               Arrival     No. of    
Name                                                         Type     Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_0.CORERESETP_0.count_sdif0[0]            SLE      Q        Out     0.076     0.076       -         
count_sdif0[0]                                               Net      -        -       0.637     -           3         
IGLOO2_Oversampling_0.CORERESETP_0.release_sdif0_core4_8     CFG4     D        In      -         0.714       -         
IGLOO2_Oversampling_0.CORERESETP_0.release_sdif0_core4_8     CFG4     Y        Out     0.411     1.124       -         
release_sdif0_core4_8                                        Net      -        -       0.483     -           1         
IGLOO2_Oversampling_0.CORERESETP_0.release_sdif0_core4       CFG4     D        In      -         1.607       -         
IGLOO2_Oversampling_0.CORERESETP_0.release_sdif0_core4       CFG4     Y        Out     0.408     2.016       -         
release_sdif0_core4                                          Net      -        -       0.138     -           1         
IGLOO2_Oversampling_0.CORERESETP_0.release_sdif0_core        SLE      EN       In      -         2.154       -         
=======================================================================================================================
Total path delay (propagation time + setup) of 2.447 is 1.189(48.6%) logic and 1.259(51.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value




====================================
Detailed Report for Clock: IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock
====================================



Starting Points with Worst Slack
********************************

                                                      Starting                                                                                                                                         Arrival          
Instance                                              Reference                                                    Type           Pin               Net                                                Time        Slack
                                                      Clock                                                                                                                                                             
------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_0.CORECONFIGP_0.psel              IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            Q                 psel                                               0.094       0.862
IGLOO2_Oversampling_0.CORECONFIGP_0.state[1]          IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            Q                 state[1]                                           0.076       2.951
SERDES_IF_0.SERDESIF_INST                             IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SERDESIF_0     APB_PRDATA[7]     IGLOO2_Oversampling_0_SDIF0_INIT_APB_PRDATA[7]     5.543       2.983
SERDES_IF_0.SERDESIF_INST                             IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SERDESIF_0     APB_PRDATA[0]     IGLOO2_Oversampling_0_SDIF0_INIT_APB_PRDATA[0]     5.106       3.381
IGLOO2_Oversampling_0.CORECONFIGP_0.SDIF0_PENABLE     IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            Q                 IGLOO2_Oversampling_0_SDIF0_INIT_APB_PENABLE       0.094       3.382
SERDES_IF_0.SERDESIF_INST                             IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SERDESIF_0     APB_PRDATA[4]     IGLOO2_Oversampling_0_SDIF0_INIT_APB_PRDATA[4]     5.102       3.424
SERDES_IF_0.SERDESIF_INST                             IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SERDESIF_0     APB_PRDATA[2]     IGLOO2_Oversampling_0_SDIF0_INIT_APB_PRDATA[2]     5.047       3.479
SERDES_IF_0.SERDESIF_INST                             IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SERDESIF_0     APB_PRDATA[1]     IGLOO2_Oversampling_0_SDIF0_INIT_APB_PRDATA[1]     5.041       3.485
SERDES_IF_0.SERDESIF_INST                             IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SERDESIF_0     APB_PRDATA[5]     IGLOO2_Oversampling_0_SDIF0_INIT_APB_PRDATA[5]     5.041       3.485
SERDES_IF_0.SERDESIF_INST                             IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SERDESIF_0     APB_PRDATA[6]     IGLOO2_Oversampling_0_SDIF0_INIT_APB_PRDATA[6]     5.035       3.491
========================================================================================================================================================================================================================


Ending Points with Worst Slack
******************************

                                                               Starting                                                                                                                                Required          
Instance                                                       Reference                                                    Type           Pin          Net                                            Time         Slack
                                                               Clock                                                                                                                                                     
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
SERDES_IF_0.SERDESIF_INST                                      IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SERDESIF_0     APB_PSEL     IGLOO2_Oversampling_0_SDIF0_INIT_APB_PSELx     3.430        0.862
IGLOO2_Oversampling_0.CORECONFIGP_0.state[1]                   IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            D            state_ns[1]                                    4.778        1.718
IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PREADY         IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            EN           N_71_i_0                                       4.707        1.822
IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PRDATA[0]      IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            D            prdata[0]                                      4.778        1.947
IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PRDATA[15]     IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            D            prdata[15]                                     4.778        1.947
IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PRDATA[16]     IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            D            prdata[16]                                     4.778        1.947
IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PRDATA[17]     IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            D            prdata[17]                                     4.778        1.947
IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PRDATA[18]     IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            D            prdata[18]                                     4.778        1.947
IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PRDATA[19]     IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            D            prdata[19]                                     4.778        1.947
IGLOO2_Oversampling_0.CORECONFIGP_0.FIC_2_APB_M_PRDATA[20]     IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock     SLE            D            prdata[20]                                     4.778        1.947
=========================================================================================================================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      5.000
    - Setup time:                            1.570
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         3.430

    - Propagation time:                      2.568
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (critical) :                     0.862

    Number of logic level(s):                1
    Starting point:                          IGLOO2_Oversampling_0.CORECONFIGP_0.psel / Q
    Ending point:                            SERDES_IF_0.SERDESIF_INST / APB_PSEL
    The start point is clocked by            IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock [falling] on pin CLK
    The end   point is clocked by            IGLOO2_Oversampling_HPMS|FIC_2_APB_M_PCLK_inferred_clock [rising] on pin APB_CLK

Instance / Net                                                             Pin          Pin               Arrival     No. of    
Name                                                        Type           Name         Dir     Delay     Time        Fan Out(s)
--------------------------------------------------------------------------------------------------------------------------------
IGLOO2_Oversampling_0.CORECONFIGP_0.psel                    SLE            Q            Out     0.094     0.094       -         
psel                                                        Net            -            -       1.294     -           20        
IGLOO2_Oversampling_0.CORECONFIGP_0.R_SDIF0_PSEL_1_0_a2     CFG3           C            In      -         1.388       -         
IGLOO2_Oversampling_0.CORECONFIGP_0.R_SDIF0_PSEL_1_0_a2     CFG3           Y            Out     0.182     1.570       -         
IGLOO2_Oversampling_0_SDIF0_INIT_APB_PSELx                  Net            -            -       0.998     -           36        
SERDES_IF_0.SERDESIF_INST                                   SERDESIF_0     APB_PSEL     In      -         2.568       -         
================================================================================================================================
Total path delay (propagation time + setup) of 4.138 is 1.846(44.6%) logic and 2.292(55.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value




====================================
Detailed Report for Clock: IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock
====================================



Starting Points with Worst Slack
********************************

                                                                      Starting                                                                                          Arrival          
Instance                                                              Reference                                                      Type     Pin     Net               Time        Slack
                                                                      Clock                                                                                                              
-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[8]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[8]      0.076       5.443
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[5]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[5]      0.076       5.513
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[9]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[9]      0.094       5.636
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[0]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[0]      0.076       5.654
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[10]     IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[10]     0.094       5.703
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[6]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[6]      0.076       5.728
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[11]     IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[11]     0.094       5.746
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[7]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[7]      0.076       5.800
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[12]     IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[12]     0.076       5.837
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[1]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      Q       baud_cntr[1]      0.094       5.847
=========================================================================================================================================================================================


Ending Points with Worst Slack
******************************

                                                                      Starting                                                                                            Required          
Instance                                                              Reference                                                      Type     Pin     Net                 Time         Slack
                                                                      Clock                                                                                                                 
--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[12]     IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[12]     9.778        5.443
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[11]     IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[11]     9.778        5.457
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[10]     IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[10]     9.778        5.471
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[9]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[9]      9.778        5.486
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[8]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[8]      9.778        5.500
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[7]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[7]      9.778        5.514
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[6]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[6]      9.778        5.528
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[1]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[1]      9.778        5.535
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[5]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[5]      9.778        5.541
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[4]      IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock     SLE      D       baud_cntr_s[4]      9.778        5.554
============================================================================================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      10.000
    - Setup time:                            0.222
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         9.778

    - Propagation time:                      4.335
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 5.443

    Number of logic level(s):                14
    Starting point:                          UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[8] / Q
    Ending point:                            UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[12] / D
    The start point is clocked by            IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock [rising] on pin CLK
    The end   point is clocked by            IGLOO2_Oversampling_top_FCCC_0_FCCC|GL0_net_inferred_clock [rising] on pin CLK

Instance / Net                                                                                         Pin      Pin               Arrival     No. of    
Name                                                                                          Type     Name     Dir     Delay     Time        Fan Out(s)
--------------------------------------------------------------------------------------------------------------------------------------------------------
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[8]                              SLE      Q        Out     0.076     0.076       -         
baud_cntr[8]                                                                                  Net      -        -       0.587     -           2         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.make_baud_cntr\.baud_cntr8_7              CFG4     D        In      -         0.663       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.make_baud_cntr\.baud_cntr8_7              CFG4     Y        Out     0.411     1.073       -         
baud_cntr8_7                                                                                  Net      -        -       0.548     -           2         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.make_baud_cntr\.baud_cntr8_1_RNI29NL1     ARI1     D        In      -         1.621       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.make_baud_cntr\.baud_cntr8_1_RNI29NL1     ARI1     Y        Out     0.411     2.032       -         
baud_cntr8_1_RNI29NL1_Y                                                                       Net      -        -       0.971     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIJLG04[1]                     ARI1     B        In      -         3.003       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIJLG04[1]                     ARI1     FCO      Out     0.155     3.158       -         
baud_cntr_cry[1]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIG40H4[2]                     ARI1     FCI      In      -         3.158       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIG40H4[2]                     ARI1     FCO      Out     0.014     3.172       -         
baud_cntr_cry[2]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIEKF15[3]                     ARI1     FCI      In      -         3.172       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIEKF15[3]                     ARI1     FCO      Out     0.014     3.187       -         
baud_cntr_cry[3]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNID5VH5[4]                     ARI1     FCI      In      -         3.187       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNID5VH5[4]                     ARI1     FCO      Out     0.014     3.201       -         
baud_cntr_cry[4]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIDNE26[5]                     ARI1     FCI      In      -         3.201       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIDNE26[5]                     ARI1     FCO      Out     0.014     3.215       -         
baud_cntr_cry[5]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIEAUI6[6]                     ARI1     FCI      In      -         3.215       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIEAUI6[6]                     ARI1     FCO      Out     0.014     3.229       -         
baud_cntr_cry[6]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIGUD37[7]                     ARI1     FCI      In      -         3.229       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIGUD37[7]                     ARI1     FCO      Out     0.014     3.243       -         
baud_cntr_cry[7]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIJJTJ7[8]                     ARI1     FCI      In      -         3.243       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIJJTJ7[8]                     ARI1     FCO      Out     0.014     3.258       -         
baud_cntr_cry[8]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIN9D48[9]                     ARI1     FCI      In      -         3.258       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIN9D48[9]                     ARI1     FCO      Out     0.014     3.272       -         
baud_cntr_cry[9]                                                                              Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNI3KTL8[10]                    ARI1     FCI      In      -         3.272       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNI3KTL8[10]                    ARI1     FCO      Out     0.014     3.286       -         
baud_cntr_cry[10]                                                                             Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIGVD79[11]                    ARI1     FCI      In      -         3.286       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNIGVD79[11]                    ARI1     FCO      Out     0.014     3.300       -         
baud_cntr_cry[11]                                                                             Net      -        -       0.000     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNO[12]                         ARI1     FCI      In      -         3.300       -         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr_RNO[12]                         ARI1     S        Out     0.063     3.364       -         
baud_cntr_s[12]                                                                               Net      -        -       0.971     -           1         
UART_INTERFACE_0.COREUART_0.make_CLOCK_GEN.genblk1\.baud_cntr[12]                             SLE      D        In      -         4.335       -         
========================================================================================================================================================
Total path delay (propagation time + setup) of 4.557 is 1.480(32.5%) logic and 3.077(67.5%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value




====================================
Detailed Report for Clock: IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock
====================================



Starting Points with Worst Slack
********************************

                                             Starting                                                                                                                      Arrival          
Instance                                     Reference                                                                      Type     Pin     Net                           Time        Slack
                                             Clock                                                                                                                                          
--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
Receiver_0.Downsampler_0.reg_data_out[2]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       Downsampler_0_data_out[2]     0.094       3.262
Receiver_0.prbs7_10_0.LFSR[7]                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       LFSR[7]                       0.094       3.265
Receiver_0.prbs7_10_0.LFSR[4]                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       LFSR[4]                       0.094       4.049
Receiver_0.prbs7_10_0.LFSR[5]                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       LFSR[5]                       0.094       4.105
Receiver_0.Downsampler_0.reg_data_out[7]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       Downsampler_0_data_out[7]     0.094       4.288
Receiver_0.prbs7_10_0.LFSR[6]                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       LFSR[6]                       0.094       4.680
Receiver_0.prbs7_10_0.LFSR[1]                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       LFSR[1]                       0.094       4.810
Receiver_0.Downsampler_0.reg_data_out[4]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       Downsampler_0_data_out[4]     0.094       5.021
Receiver_0.Downsampler_0.reg_data_out[3]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       Downsampler_0_data_out[3]     0.094       5.038
Receiver_0.prbs7_10_0.LFSR[2]                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      Q       LFSR[2]                       0.094       5.131
============================================================================================================================================================================================


Ending Points with Worst Slack
******************************

                                        Starting                                                                                                                 Required          
Instance                                Reference                                                                      Type     Pin     Net                      Time         Slack
                                        Clock                                                                                                                                      
-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
Receiver_0.prbs7_10_0.lock_count[1]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      D       N_14_i_1                 9.778        3.262
Receiver_0.prbs7_10_0.reg_lock          IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      EN      un1_lock_count13_i_0     9.707        3.931
Receiver_0.prbs7_10_0.reg_error[0]      IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      EN      N_179_i_0                9.707        3.999
Receiver_0.prbs7_10_0.reg_error[1]      IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      EN      N_179_i_0                9.707        3.999
Receiver_0.prbs7_10_0.reg_error[2]      IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      EN      N_179_i_0                9.707        3.999
Receiver_0.prbs7_10_0.reg_error[3]      IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      EN      N_179_i_0                9.707        3.999
Receiver_0.prbs7_10_0.reg_error[4]      IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      EN      N_179_i_0                9.707        3.999
Receiver_0.prbs7_10_0.reg_error[5]      IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      EN      N_179_i_0                9.707        3.999
Receiver_0.prbs7_10_0.reg_error_out     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      EN      N_179_i_0                9.707        3.999
Receiver_0.prbs7_10_0.lock_count[0]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock     SLE      D       N_12_i_0                 9.778        4.002
===================================================================================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      10.000
    - Setup time:                            0.222
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         9.778

    - Propagation time:                      6.516
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 3.262

    Number of logic level(s):                8
    Starting point:                          Receiver_0.Downsampler_0.reg_data_out[2] / Q
    Ending point:                            Receiver_0.prbs7_10_0.lock_count[1] / D
    The start point is clocked by            IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock [rising] on pin CLK
    The end   point is clocked by            IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_RX_CLK_inferred_clock [rising] on pin CLK

Instance / Net                                                 Pin      Pin               Arrival     No. of    
Name                                                  Type     Name     Dir     Delay     Time        Fan Out(s)
----------------------------------------------------------------------------------------------------------------
Receiver_0.Downsampler_0.reg_data_out[2]              SLE      Q        Out     0.094     0.094       -         
Downsampler_0_data_out[2]                             Net      -        -       0.587     -           2         
Receiver_0.prbs7_10_0.un1_data_in_2_0                 CFG2     B        In      -         0.681       -         
Receiver_0.prbs7_10_0.un1_data_in_2_0                 CFG2     Y        Out     0.143     0.824       -         
un1_data_in_2_0                                       Net      -        -       0.483     -           1         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2_0_2       CFG4     D        In      -         1.307       -         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2_0_2       CFG4     Y        Out     0.411     1.718       -         
un1_lock_count13_i_o2_0_2                             Net      -        -       0.483     -           1         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2_0_6_1     CFG4     D        In      -         2.201       -         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2_0_6_1     CFG4     Y        Out     0.384     2.585       -         
un1_lock_count13_i_o2_0_6_1                           Net      -        -       0.483     -           1         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2_0_6       CFG4     C        In      -         3.068       -         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2_0_6       CFG4     Y        Out     0.196     3.265       -         
un1_lock_count13_i_o2_0_6                             Net      -        -       0.483     -           1         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2_0         CFG4     D        In      -         3.748       -         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2_0         CFG4     Y        Out     0.408     4.156       -         
N_164                                                 Net      -        -       0.548     -           2         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2           CFG3     B        In      -         4.704       -         
Receiver_0.prbs7_10_0.un1_lock_count13_i_o2           CFG3     Y        Out     0.143     4.847       -         
N_165                                                 Net      -        -       0.648     -           5         
Receiver_0.prbs7_10_0.lock_count_3_i_x2[1]            CFG3     C        In      -         5.495       -         
Receiver_0.prbs7_10_0.lock_count_3_i_x2[1]            CFG3     Y        Out     0.200     5.695       -         
N_81_i                                                Net      -        -       0.483     -           1         
Receiver_0.prbs7_10_0.lock_count_RNO[1]               CFG4     C        In      -         6.178       -         
Receiver_0.prbs7_10_0.lock_count_RNO[1]               CFG4     Y        Out     0.200     6.378       -         
N_14_i_1                                              Net      -        -       0.138     -           1         
Receiver_0.prbs7_10_0.lock_count[1]                   SLE      D        In      -         6.516       -         
================================================================================================================
Total path delay (propagation time + setup) of 6.738 is 2.402(35.6%) logic and 4.336(64.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value




====================================
Detailed Report for Clock: IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock
====================================



Starting Points with Worst Slack
********************************

                                              Starting                                                                                                                    Arrival          
Instance                                      Reference                                                                      Type     Pin     Net                         Time        Slack
                                              Clock                                                                                                                                        
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
Transmitter_0.Replicator_0.reg_tx_val_out     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       Replicator_0_tx_val_out     0.094       7.504
Transmitter_0.FIFO_PRBS_0.i[0]                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       i[0]                        0.076       7.715
Transmitter_0.FIFO_PRBS_0.i[1]                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       i[1]                        0.094       7.734
Transmitter_0.prbs7_10_0.tx_count[0]          IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       tx_count[0]                 0.076       7.959
Transmitter_0.FIFO_PRBS_0.flag                IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       flag                        0.094       8.049
Transmitter_0.prbs7_10_0.tx_count[1]          IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       tx_count[1]                 0.076       8.099
Transmitter_0.FIFO_PRBS_0.data[21]            IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       data[23]                    0.076       8.104
Transmitter_0.FIFO_PRBS_0.data[24]            IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       data[26]                    0.076       8.104
Transmitter_0.FIFO_PRBS_0.data[27]            IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       data[29]                    0.076       8.104
Transmitter_0.FIFO_PRBS_0.data[18]            IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      Q       data[20]                    0.076       8.157
===========================================================================================================================================================================================


Ending Points with Worst Slack
******************************

                                              Starting                                                                                                        Required          
Instance                                      Reference                                                                      Type     Pin     Net             Time         Slack
                                              Clock                                                                                                                             
--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
Transmitter_0.FIFO_PRBS_0.reg_data_out[0]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[1]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[2]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[3]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[4]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[5]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[6]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[7]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[8]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
Transmitter_0.FIFO_PRBS_0.reg_data_out[9]     IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock     SLE      EN      un1_i17_i_0     9.707        7.504
================================================================================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      10.000
    - Setup time:                            0.293
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         9.707

    - Propagation time:                      2.202
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 7.504

    Number of logic level(s):                1
    Starting point:                          Transmitter_0.Replicator_0.reg_tx_val_out / Q
    Ending point:                            Transmitter_0.FIFO_PRBS_0.reg_data_out[0] / EN
    The start point is clocked by            IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock [rising] on pin CLK
    The end   point is clocked by            IGLOO2_Oversampling_top_SERDES_IF_0_SERDES_IF|EPCS_1_TX_CLK_inferred_clock [rising] on pin CLK

Instance / Net                                         Pin      Pin               Arrival     No. of    
Name                                          Type     Name     Dir     Delay     Time        Fan Out(s)
--------------------------------------------------------------------------------------------------------
Transmitter_0.Replicator_0.reg_tx_val_out     SLE      Q        Out     0.094     0.094       -         
Replicator_0_tx_val_out                       Net      -        -       0.827     -           5         
Transmitter_0.FIFO_PRBS_0.flag_RNIUQIH        CFG4     D        In      -         0.921       -         
Transmitter_0.FIFO_PRBS_0.flag_RNIUQIH        CFG4     Y        Out     0.408     1.329       -         
un1_i17_i_0                                   Net      -        -       0.873     -           10        
Transmitter_0.FIFO_PRBS_0.reg_data_out[0]     SLE      EN       In      -         2.202       -         
========================================================================================================
Total path delay (propagation time + setup) of 2.496 is 0.796(31.9%) logic and 1.700(68.1%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value



##### END OF TIMING REPORT #####]

---------------------------------------
Resource Usage Report for IGLOO2_Oversampling_top 

Mapping to part: m2gl010tfbga484-1
Cell usage:
AND2            1 use
AND3            1 use
CCC             2 uses
CLKINT          13 uses
MSS_010         1 use
RCOSC_25_50MHZ  1 use
RCOSC_25_50MHZ_FAB  1 use
SERDESIF_0      1 use
SYSRESET        1 use
CFG1           9 uses
CFG2           212 uses
CFG3           227 uses
CFG4           513 uses

Carry primitives used for arithmetic functions:
ARI1           138 uses


Sequential Cells: 
SLE            1010 uses

DSP Blocks:    0

I/O ports: 22
I/O primitives: 5
INBUF          2 uses
OUTBUF         3 uses


Global Clock Buffers: 13


Total LUTs:    1099

Mapper successful!

At Mapper Exit (Real Time elapsed 0h:00m:05s; CPU Time elapsed 0h:00m:04s; Memory used current: 54MB peak: 165MB)

Process took 0h:00m:05s realtime, 0h:00m:04s cputime
# Fri Apr 18 09:31:00 2014

###########################################################]
