@W: CG775 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":32:7:32:17|Found Component CoreAHBLite in library COREAHBLITE_LIB
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigMaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Optimizing register bit HTRANS[0] to a constant 0
@W: CL260 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreConfigMaster\2.0.101\rtl\vlog\core\coreconfigmaster.v":541:4:541:9|Pruning register bit 0 of HTRANS[1:0] 
@W: CG775 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":32:7:32:17|Found Component CoreAHBLite in library COREAHBLITE_LIB
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1562:4:1562:9|Pruning register count_ddr[13:0] 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1530:4:1530:9|Pruning register count_sdif3[12:0] 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1498:4:1498:9|Pruning register count_sdif2[12:0] 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1466:4:1466:9|Pruning register count_sdif1[12:0] 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif1_enable_q1 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif2_enable_q1 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif3_enable_q1 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif1_enable_rcosc 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif2_enable_rcosc 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_sdif3_enable_rcosc 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_ddr_enable_q1 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1404:4:1404:9|Pruning register count_ddr_enable_rcosc 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1314:4:1314:9|Pruning register count_sdif3_enable 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1249:4:1249:9|Pruning register count_sdif2_enable 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1184:4:1184:9|Pruning register count_sdif1_enable 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Pruning register count_ddr_enable 
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1382:4:1382:9|Optimizing register bit EXT_RESET_OUT_int to a constant 0
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1031:4:1031:9|Pruning register release_ext_reset 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1382:4:1382:9|Pruning register EXT_RESET_OUT_int 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":1382:4:1382:9|Pruning register sm2_state[2:0] 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":756:4:756:9|Pruning register sm2_areset_n_q1 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":756:4:756:9|Pruning register sm2_areset_n_clk_base 
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FIFO_PRBS.v":74:1:74:6|Optimizing register bit reg_tx_val_out to a constant 1
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":112:0:112:5|Optimizing register bit fifo_read_en0 to a constant 1
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":112:0:112:5|Pruning register fifo_read_en0 
@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":111:14:111:24|No assignment to wire tx_dout_reg
@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":112:14:112:20|No assignment to wire rx_dout
@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":118:8:118:20|No assignment to wire fifo_empty_tx
@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":119:8:119:20|No assignment to wire fifo_empty_rx
@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":123:8:123:19|No assignment to wire fifo_full_tx
@W: CG360 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":124:8:124:19|No assignment to wire fifo_full_rx
@W: CG133 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":135:8:135:17|No assignment to data_ready
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":360:0:360:5|Pruning register overflow_reg 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":335:0:335:5|Pruning register rx_dout_reg_empty 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":335:0:335:5|Pruning register rx_dout_reg_empty_q 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":320:0:320:5|Pruning register rx_dout_reg[7:0] 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":287:0:287:5|Pruning register rx_state[1:0] 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":272:0:272:5|Pruning register clear_framing_error_reg 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":272:0:272:5|Pruning register clear_framing_error_reg0 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":257:0:257:5|Pruning register clear_parity_reg 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":257:0:257:5|Pruning register clear_parity_reg0 
@W: CL169 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":154:0:154:5|Pruning register fifo_write_tx 
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v":91:0:91:5|Optimizing register bit uart_data_out_t[6] to a constant 0
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v":91:0:91:5|Optimizing register bit uart_data_out_t[7] to a constant 0
@W: CL279 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FabUART.v":91:0:91:5|Pruning register bits 7 to 6 of uart_data_out_t[7:0] 
@W: CL156 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":111:14:111:24|*Input tx_dout_reg[7:0] to expression [instance] has undriven bits that are tied to 0 -- simulation mismatch possible.
@W: CL156 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":118:8:118:20|*Input fifo_empty_tx to expression [instance] has undriven bits that are tied to 0 -- simulation mismatch possible.
@W: CL156 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\CoreUART.v":123:8:123:19|*Input fifo_full_tx to expression [instance] has undriven bits that are tied to 0 -- simulation mismatch possible.
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":43:11:43:21|Input tx_dout_reg is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":44:6:44:15|Input fifo_empty is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Tx_async.v":45:6:45:14|Input fifo_full is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\UART_INTERFACE\COREUART_0\rtl\vlog\core\Clock_gen.v":50:15:50:31|Input BAUD_VAL_FRACTION is unused
@W: CL190 :"C:\Microsemi\IGLOO2_Oversampling\hdl\FIFO_PRBS.v":74:1:74:6|Optimizing register bit reg_tx_val_out to a constant 1
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling_HPMS\IGLOO2_Oversampling_HPMS.v":51:14:51:31|Input port bit 0 of FIC_0_AHB_S_HTRANS[1:0] is unused
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":15:7:15:24|*Output RCOSC_25_50MHZ_CCC has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":17:7:17:20|*Output RCOSC_1MHZ_CCC has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":18:7:18:20|*Output RCOSC_1MHZ_O2F has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":19:7:19:16|*Output XTLOSC_CCC has undriven bits -- simulation mismatch possible.
@W: CL157 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":20:7:20:16|*Output XTLOSC_O2F has undriven bits -- simulation mismatch possible.
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\work\IGLOO2_Oversampling\FABOSC_0\IGLOO2_Oversampling_FABOSC_0_OSC.v":14:7:14:9|Input XTL is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":36:24:36:29|Input port bit 31 of prdata[31:0] is unused
@W: CL246 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp_pcie_hotreset.v":36:24:36:29|Input port bits 25 to 0 of prdata[31:0] are unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":56:20:56:28|Input FPLL_LOCK is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":63:20:63:34|Input SDIF1_SPLL_LOCK is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":67:20:67:34|Input SDIF2_SPLL_LOCK is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":71:20:71:34|Input SDIF3_SPLL_LOCK is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":88:20:88:29|Input SDIF1_PSEL is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":89:20:89:31|Input SDIF1_PWRITE is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":90:20:90:31|Input SDIF1_PRDATA is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":91:20:91:29|Input SDIF2_PSEL is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":92:20:92:31|Input SDIF2_PWRITE is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":93:20:93:31|Input SDIF2_PRDATA is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":94:20:94:29|Input SDIF3_PSEL is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":95:20:95:31|Input SDIF3_PWRITE is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreResetP\5.1.100\rtl\vlog\core\coreresetp.v":96:20:96:31|Input SDIF3_PRDATA is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":128:15:128:23|Input port bit 0 of HTRANS_M0[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":139:15:139:23|Input port bit 0 of HTRANS_M1[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":150:15:150:23|Input port bit 0 of HTRANS_M2[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":161:15:161:23|Input port bit 0 of HTRANS_M3[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":171:15:171:22|Input port bit 1 of HRESP_S0[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":184:15:184:22|Input port bit 1 of HRESP_S1[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":197:15:197:22|Input port bit 1 of HRESP_S2[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":210:15:210:22|Input port bit 1 of HRESP_S3[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":223:15:223:22|Input port bit 1 of HRESP_S4[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":236:15:236:22|Input port bit 1 of HRESP_S5[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":249:15:249:22|Input port bit 1 of HRESP_S6[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":262:15:262:22|Input port bit 1 of HRESP_S7[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":275:15:275:22|Input port bit 1 of HRESP_S8[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":288:15:288:22|Input port bit 1 of HRESP_S9[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":301:15:301:23|Input port bit 1 of HRESP_S10[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":314:15:314:23|Input port bit 1 of HRESP_S11[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":327:15:327:23|Input port bit 1 of HRESP_S12[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":340:15:340:23|Input port bit 1 of HRESP_S13[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":353:15:353:23|Input port bit 1 of HRESP_S14[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":366:15:366:23|Input port bit 1 of HRESP_S15[1:0] is unused
@W: CL247 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":379:15:379:23|Input port bit 1 of HRESP_S16[1:0] is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":131:15:131:23|Input HBURST_M0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":132:15:132:22|Input HPROT_M0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":142:15:142:23|Input HBURST_M1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":143:15:143:22|Input HPROT_M1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":153:15:153:23|Input HBURST_M2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":154:15:154:22|Input HPROT_M2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":164:15:164:23|Input HBURST_M3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite.v":165:15:165:22|Input HPROT_M3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":58:18:58:26|Input HWDATA_M1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":67:18:67:26|Input HWDATA_M2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":76:18:76:26|Input HWDATA_M3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":80:18:80:26|Input HRDATA_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":81:13:81:24|Input HREADYOUT_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":82:13:82:20|Input HRESP_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":91:18:91:26|Input HRDATA_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":92:13:92:24|Input HREADYOUT_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":93:13:93:20|Input HRESP_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":102:18:102:26|Input HRDATA_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":103:13:103:24|Input HREADYOUT_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":104:13:104:20|Input HRESP_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":113:18:113:26|Input HRDATA_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":114:13:114:24|Input HREADYOUT_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":115:13:115:20|Input HRESP_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":124:18:124:26|Input HRDATA_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":125:13:125:24|Input HREADYOUT_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":126:13:126:20|Input HRESP_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":135:18:135:26|Input HRDATA_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":136:13:136:24|Input HREADYOUT_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":137:13:137:20|Input HRESP_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":146:18:146:26|Input HRDATA_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":147:13:147:24|Input HREADYOUT_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":148:13:148:20|Input HRESP_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":157:18:157:26|Input HRDATA_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":158:13:158:24|Input HREADYOUT_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":159:13:159:20|Input HRESP_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":168:18:168:26|Input HRDATA_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":169:13:169:24|Input HREADYOUT_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":170:13:170:20|Input HRESP_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":179:18:179:26|Input HRDATA_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":180:13:180:24|Input HREADYOUT_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":181:13:181:20|Input HRESP_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":190:18:190:27|Input HRDATA_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":191:13:191:25|Input HREADYOUT_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":192:13:192:21|Input HRESP_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":201:18:201:27|Input HRDATA_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":202:13:202:25|Input HREADYOUT_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":203:13:203:21|Input HRESP_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":212:18:212:27|Input HRDATA_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":213:13:213:25|Input HREADYOUT_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":214:13:214:21|Input HRESP_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":223:18:223:27|Input HRDATA_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":224:13:224:25|Input HREADYOUT_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":225:13:225:21|Input HRESP_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":234:18:234:27|Input HRDATA_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":235:13:235:25|Input HREADYOUT_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":236:13:236:21|Input HRESP_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":245:18:245:27|Input HRDATA_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":246:13:246:25|Input HREADYOUT_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_matrix4x16.v":247:13:247:21|Input HRESP_S15 is unused
@W: CL246 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_slavestage.v":46:15:46:33|Input port bits 3 to 2 of MPREVDATASLAVEREADY[3:0] are unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":50:16:50:25|Input SDATAREADY is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":51:16:51:21|Input SHRESP is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":60:16:60:24|Input HRDATA_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":61:11:61:22|Input HREADYOUT_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":62:16:62:24|Input HRDATA_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":63:11:63:22|Input HREADYOUT_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":64:16:64:24|Input HRDATA_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":65:11:65:22|Input HREADYOUT_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":66:16:66:24|Input HRDATA_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":67:11:67:22|Input HREADYOUT_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":68:16:68:24|Input HRDATA_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":69:11:69:22|Input HREADYOUT_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":70:16:70:24|Input HRDATA_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":71:11:71:22|Input HREADYOUT_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":72:16:72:24|Input HRDATA_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":73:11:73:22|Input HREADYOUT_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":74:16:74:24|Input HRDATA_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":75:11:75:22|Input HREADYOUT_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":76:16:76:24|Input HRDATA_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":77:11:77:22|Input HREADYOUT_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":78:16:78:24|Input HRDATA_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":79:11:79:22|Input HREADYOUT_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":80:16:80:25|Input HRDATA_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":81:11:81:23|Input HREADYOUT_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":82:16:82:25|Input HRDATA_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":83:11:83:23|Input HREADYOUT_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":84:16:84:25|Input HRDATA_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":85:11:85:23|Input HREADYOUT_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":86:16:86:25|Input HRDATA_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":87:11:87:23|Input HREADYOUT_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":88:16:88:25|Input HRDATA_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":89:11:89:23|Input HREADYOUT_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":90:16:90:25|Input HRDATA_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":91:11:91:23|Input HREADYOUT_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":92:16:92:25|Input HRDATA_S16 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":93:11:93:23|Input HREADYOUT_S16 is unused
@W: CL246 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":50:16:50:25|Input port bits 15 to 0 of SDATAREADY[16:0] are unused
@W: CL246 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":51:16:51:21|Input port bits 15 to 0 of SHRESP[16:0] are unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":60:16:60:24|Input HRDATA_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":61:11:61:22|Input HREADYOUT_S0 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":62:16:62:24|Input HRDATA_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":63:11:63:22|Input HREADYOUT_S1 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":64:16:64:24|Input HRDATA_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":65:11:65:22|Input HREADYOUT_S2 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":66:16:66:24|Input HRDATA_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":67:11:67:22|Input HREADYOUT_S3 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":68:16:68:24|Input HRDATA_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":69:11:69:22|Input HREADYOUT_S4 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":70:16:70:24|Input HRDATA_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":71:11:71:22|Input HREADYOUT_S5 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":72:16:72:24|Input HRDATA_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":73:11:73:22|Input HREADYOUT_S6 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":74:16:74:24|Input HRDATA_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":75:11:75:22|Input HREADYOUT_S7 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":76:16:76:24|Input HRDATA_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":77:11:77:22|Input HREADYOUT_S8 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":78:16:78:24|Input HRDATA_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":79:11:79:22|Input HREADYOUT_S9 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":80:16:80:25|Input HRDATA_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":81:11:81:23|Input HREADYOUT_S10 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":82:16:82:25|Input HRDATA_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":83:11:83:23|Input HREADYOUT_S11 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":84:16:84:25|Input HRDATA_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":85:11:85:23|Input HREADYOUT_S12 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":86:16:86:25|Input HRDATA_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":87:11:87:23|Input HREADYOUT_S13 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":88:16:88:25|Input HRDATA_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":89:11:89:23|Input HREADYOUT_S14 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":90:16:90:25|Input HRDATA_S15 is unused
@W: CL159 :"C:\Microsemi\IGLOO2_Oversampling\component\Actel\DirectCore\CoreAHBLite\5.0.100\rtl\vlog\core\coreahblite_masterstage.v":91:11:91:23|Input HREADYOUT_S15 is unused

