# Microsemi Physical design constraints file

# Version: v11.5 11.5.0.26

# Design Name: MC_System 

# Input Netlist Format: EDIF 

# Family: SmartFusion2 , Die: M2S010 , Package: 484 FBGA , Speed grade: -1 

# Date generated: Tue Mar 10 11:25:41 2015 


#
# I/O constraints
#

set_io AMBA_SLAVE_0_PADDRS\[0\] -DIRECTION OUTPUT -pinname E4 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[1\] -DIRECTION OUTPUT -pinname K6 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[2\] -DIRECTION OUTPUT -pinname A18 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[3\] -DIRECTION OUTPUT -pinname A13 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[4\] -DIRECTION OUTPUT -pinname U19 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[5\] -DIRECTION OUTPUT -pinname N1 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[6\] -DIRECTION OUTPUT -pinname AA13 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[7\] -DIRECTION OUTPUT -pinname AA17 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[8\] -DIRECTION OUTPUT -pinname B1 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[9\] -DIRECTION OUTPUT -pinname D4 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[10\] -DIRECTION OUTPUT -pinname F17 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[11\] -DIRECTION OUTPUT -pinname E13 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[12\] -DIRECTION OUTPUT -pinname J18 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[13\] -DIRECTION OUTPUT -pinname A10 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[14\] -DIRECTION OUTPUT -pinname Y18 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[15\] -DIRECTION OUTPUT -pinname D18 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[16\] -DIRECTION OUTPUT -pinname D13 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[17\] -DIRECTION OUTPUT -pinname C17 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[18\] -DIRECTION OUTPUT -pinname A19 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[19\] -DIRECTION OUTPUT -pinname A11 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[20\] -DIRECTION OUTPUT -pinname G6 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[21\] -DIRECTION OUTPUT -pinname L8 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[22\] -DIRECTION OUTPUT -pinname F14 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[23\] -DIRECTION OUTPUT -pinname H4 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[24\] -DIRECTION OUTPUT -pinname G12 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[25\] -DIRECTION OUTPUT -pinname K16 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[26\] -DIRECTION OUTPUT -pinname W14 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[27\] -DIRECTION OUTPUT -pinname E10 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[28\] -DIRECTION OUTPUT -pinname H6 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[29\] -DIRECTION OUTPUT -pinname H5 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[30\] -DIRECTION OUTPUT -pinname C13 -fixed no
set_io AMBA_SLAVE_0_PADDRS\[31\] -DIRECTION OUTPUT -pinname W11 -fixed no
set_io AMBA_SLAVE_0_PENABLES -DIRECTION OUTPUT -pinname E5 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[0\] -DIRECTION INPUT -pinname N17 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[1\] -DIRECTION INPUT -pinname A15 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[2\] -DIRECTION INPUT -pinname K15 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[3\] -DIRECTION INPUT -pinname AA16 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[4\] -DIRECTION INPUT -pinname AB15 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[5\] -DIRECTION INPUT -pinname M1 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[6\] -DIRECTION INPUT -pinname K4 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[7\] -DIRECTION INPUT -pinname H20 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[8\] -DIRECTION INPUT -pinname N20 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[9\] -DIRECTION INPUT -pinname W9 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[10\] -DIRECTION INPUT -pinname G17 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[11\] -DIRECTION INPUT -pinname A21 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[12\] -DIRECTION INPUT -pinname L20 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[13\] -DIRECTION INPUT -pinname R22 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[14\] -DIRECTION INPUT -pinname G1 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[15\] -DIRECTION INPUT -pinname L2 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[16\] -DIRECTION INPUT -pinname M7 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[17\] -DIRECTION INPUT -pinname D14 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[18\] -DIRECTION INPUT -pinname M6 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[19\] -DIRECTION INPUT -pinname W15 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[20\] -DIRECTION INPUT -pinname J6 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[21\] -DIRECTION INPUT -pinname N16 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[22\] -DIRECTION INPUT -pinname A20 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[23\] -DIRECTION INPUT -pinname U14 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[24\] -DIRECTION INPUT -pinname D21 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[25\] -DIRECTION INPUT -pinname G18 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[26\] -DIRECTION INPUT -pinname C19 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[27\] -DIRECTION INPUT -pinname AB13 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[28\] -DIRECTION INPUT -pinname V16 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[29\] -DIRECTION INPUT -pinname AB19 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[30\] -DIRECTION INPUT -pinname L16 -fixed no
set_io AMBA_SLAVE_0_PRDATAS0\[31\] -DIRECTION INPUT -pinname D2 -fixed no
set_io AMBA_SLAVE_0_PREADYS0 -DIRECTION INPUT -pinname Y19 -fixed no
set_io AMBA_SLAVE_0_PSELS0 -DIRECTION OUTPUT -pinname T13 -fixed no
set_io AMBA_SLAVE_0_PSLVERRS0 -DIRECTION INPUT -pinname Y15 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[0\] -DIRECTION OUTPUT -pinname H7 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[1\] -DIRECTION OUTPUT -pinname D8 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[2\] -DIRECTION OUTPUT -pinname E2 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[3\] -DIRECTION OUTPUT -pinname A16 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[4\] -DIRECTION OUTPUT -pinname A4 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[5\] -DIRECTION OUTPUT -pinname F5 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[6\] -DIRECTION OUTPUT -pinname F3 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[7\] -DIRECTION OUTPUT -pinname K2 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[8\] -DIRECTION OUTPUT -pinname J4 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[9\] -DIRECTION OUTPUT -pinname E8 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[10\] -DIRECTION OUTPUT -pinname A14 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[11\] -DIRECTION OUTPUT -pinname AB14 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[12\] -DIRECTION OUTPUT -pinname D10 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[13\] -DIRECTION OUTPUT -pinname D20 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[14\] -DIRECTION OUTPUT -pinname B9 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[15\] -DIRECTION OUTPUT -pinname AB17 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[16\] -DIRECTION OUTPUT -pinname V14 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[17\] -DIRECTION OUTPUT -pinname N6 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[18\] -DIRECTION OUTPUT -pinname C3 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[19\] -DIRECTION OUTPUT -pinname V11 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[20\] -DIRECTION OUTPUT -pinname A12 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[21\] -DIRECTION OUTPUT -pinname C1 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[22\] -DIRECTION OUTPUT -pinname M22 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[23\] -DIRECTION OUTPUT -pinname J2 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[24\] -DIRECTION OUTPUT -pinname T3 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[25\] -DIRECTION OUTPUT -pinname B21 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[26\] -DIRECTION OUTPUT -pinname G7 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[27\] -DIRECTION OUTPUT -pinname F21 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[28\] -DIRECTION OUTPUT -pinname H19 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[29\] -DIRECTION OUTPUT -pinname N19 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[30\] -DIRECTION OUTPUT -pinname D3 -fixed no
set_io AMBA_SLAVE_0_PWDATAS\[31\] -DIRECTION OUTPUT -pinname C15 -fixed no
set_io AMBA_SLAVE_0_PWRITES -DIRECTION OUTPUT -pinname R16 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[0\] -DIRECTION OUTPUT -pinname B5 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[1\] -DIRECTION OUTPUT -pinname D5 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[2\] -DIRECTION OUTPUT -pinname B3 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[3\] -DIRECTION OUTPUT -pinname B11 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[4\] -DIRECTION OUTPUT -pinname B22 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[5\] -DIRECTION OUTPUT -pinname R3 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[6\] -DIRECTION OUTPUT -pinname L7 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[7\] -DIRECTION OUTPUT -pinname R4 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[8\] -DIRECTION OUTPUT -pinname D9 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[9\] -DIRECTION OUTPUT -pinname E21 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[10\] -DIRECTION OUTPUT -pinname C16 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[11\] -DIRECTION OUTPUT -pinname D12 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[12\] -DIRECTION OUTPUT -pinname Y14 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[13\] -DIRECTION OUTPUT -pinname H1 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[14\] -DIRECTION OUTPUT -pinname N4 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[15\] -DIRECTION OUTPUT -pinname K21 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[16\] -DIRECTION OUTPUT -pinname A6 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[17\] -DIRECTION OUTPUT -pinname E19 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[18\] -DIRECTION OUTPUT -pinname D16 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[19\] -DIRECTION OUTPUT -pinname N8 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[20\] -DIRECTION OUTPUT -pinname L4 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[21\] -DIRECTION OUTPUT -pinname B2 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[22\] -DIRECTION OUTPUT -pinname B15 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[23\] -DIRECTION OUTPUT -pinname F8 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[24\] -DIRECTION OUTPUT -pinname C9 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[25\] -DIRECTION OUTPUT -pinname B19 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[26\] -DIRECTION OUTPUT -pinname V13 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[27\] -DIRECTION OUTPUT -pinname M2 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[28\] -DIRECTION OUTPUT -pinname B7 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[29\] -DIRECTION OUTPUT -pinname A3 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[30\] -DIRECTION OUTPUT -pinname G16 -fixed no
set_io AMBA_SLAVE_1_PADDRS\[31\] -DIRECTION OUTPUT -pinname U13 -fixed no
set_io AMBA_SLAVE_1_PENABLES -DIRECTION OUTPUT -pinname A2 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[0\] -DIRECTION INPUT -pinname K20 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[1\] -DIRECTION INPUT -pinname M8 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[2\] -DIRECTION INPUT -pinname N21 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[3\] -DIRECTION INPUT -pinname D11 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[4\] -DIRECTION INPUT -pinname W16 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[5\] -DIRECTION INPUT -pinname L3 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[6\] -DIRECTION INPUT -pinname AB18 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[7\] -DIRECTION INPUT -pinname A5 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[8\] -DIRECTION INPUT -pinname AA18 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[9\] -DIRECTION INPUT -pinname N5 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[10\] -DIRECTION INPUT -pinname L18 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[11\] -DIRECTION INPUT -pinname M21 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[12\] -DIRECTION INPUT -pinname K8 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[13\] -DIRECTION INPUT -pinname L19 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[14\] -DIRECTION INPUT -pinname E22 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[15\] -DIRECTION INPUT -pinname F19 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[16\] -DIRECTION INPUT -pinname P3 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[17\] -DIRECTION INPUT -pinname E7 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[18\] -DIRECTION INPUT -pinname P2 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[19\] -DIRECTION INPUT -pinname Y13 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[20\] -DIRECTION INPUT -pinname J3 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[21\] -DIRECTION INPUT -pinname F4 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[22\] -DIRECTION INPUT -pinname F10 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[23\] -DIRECTION INPUT -pinname B17 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[24\] -DIRECTION INPUT -pinname M3 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[25\] -DIRECTION INPUT -pinname M5 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[26\] -DIRECTION INPUT -pinname K1 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[27\] -DIRECTION INPUT -pinname K7 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[28\] -DIRECTION INPUT -pinname E1 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[29\] -DIRECTION INPUT -pinname E12 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[30\] -DIRECTION INPUT -pinname L21 -fixed no
set_io AMBA_SLAVE_1_PRDATAS1\[31\] -DIRECTION INPUT -pinname P4 -fixed no
set_io AMBA_SLAVE_1_PREADYS1 -DIRECTION INPUT -pinname E15 -fixed no
set_io AMBA_SLAVE_1_PSELS1 -DIRECTION OUTPUT -pinname W17 -fixed no
set_io AMBA_SLAVE_1_PSLVERRS1 -DIRECTION INPUT -pinname D6 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[0\] -DIRECTION OUTPUT -pinname C22 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[1\] -DIRECTION OUTPUT -pinname B6 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[2\] -DIRECTION OUTPUT -pinname C5 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[3\] -DIRECTION OUTPUT -pinname F6 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[4\] -DIRECTION OUTPUT -pinname F15 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[5\] -DIRECTION OUTPUT -pinname C7 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[6\] -DIRECTION OUTPUT -pinname G13 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[7\] -DIRECTION OUTPUT -pinname A9 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[8\] -DIRECTION OUTPUT -pinname C18 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[9\] -DIRECTION OUTPUT -pinname C4 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[10\] -DIRECTION OUTPUT -pinname G14 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[11\] -DIRECTION OUTPUT -pinname P22 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[12\] -DIRECTION OUTPUT -pinname F12 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[13\] -DIRECTION OUTPUT -pinname E18 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[14\] -DIRECTION OUTPUT -pinname E17 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[15\] -DIRECTION OUTPUT -pinname P16 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[16\] -DIRECTION OUTPUT -pinname U15 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[17\] -DIRECTION OUTPUT -pinname Y9 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[18\] -DIRECTION OUTPUT -pinname C11 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[19\] -DIRECTION OUTPUT -pinname P18 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[20\] -DIRECTION OUTPUT -pinname B13 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[21\] -DIRECTION OUTPUT -pinname C20 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[22\] -DIRECTION OUTPUT -pinname K17 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[23\] -DIRECTION OUTPUT -pinname L5 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[24\] -DIRECTION OUTPUT -pinname P1 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[25\] -DIRECTION OUTPUT -pinname A17 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[26\] -DIRECTION OUTPUT -pinname G5 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[27\] -DIRECTION OUTPUT -pinname N22 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[28\] -DIRECTION OUTPUT -pinname F18 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[29\] -DIRECTION OUTPUT -pinname F20 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[30\] -DIRECTION OUTPUT -pinname J1 -fixed no
set_io AMBA_SLAVE_1_PWDATAS\[31\] -DIRECTION OUTPUT -pinname D1 -fixed no
set_io AMBA_SLAVE_1_PWRITES -DIRECTION OUTPUT -pinname P7 -fixed no
set_io FAB_CCC_GL1 -DIRECTION OUTPUT -pinname AA15 -fixed no
set_io FIC_0_CLK -DIRECTION OUTPUT -pinname K5 -fixed no
set_io GPIO_0_M2F -DIRECTION OUTPUT -pinname A7 -fixed no
set_io GPIO_1_M2F -DIRECTION OUTPUT -pinname N3 -fixed no
set_io GPIO_2_M2F -DIRECTION OUTPUT -pinname G19 -fixed no
set_io USB_ULPI_DATA\[0\] -DIRECTION INOUT -pinname V22 -fixed no
set_io USB_ULPI_DATA\[1\] -DIRECTION INOUT -pinname V21 -fixed no
set_io USB_ULPI_DATA\[2\] -DIRECTION INOUT -pinname U22 -fixed no
set_io USB_ULPI_DATA\[3\] -DIRECTION INOUT -pinname U21 -fixed no
set_io USB_ULPI_DATA\[4\] -DIRECTION INOUT -pinname T20 -fixed no
set_io USB_ULPI_DATA\[5\] -DIRECTION INOUT -pinname T21 -fixed no
set_io USB_ULPI_DATA\[6\] -DIRECTION INOUT -pinname P17 -fixed no
set_io USB_ULPI_DATA\[7\] -DIRECTION INOUT -pinname V19 -fixed no
set_io USB_ULPI_DIR -DIRECTION INPUT -pinname R18 -fixed no
set_io USB_ULPI_NXT -DIRECTION INPUT -pinname T19 -fixed no
set_io USB_ULPI_STP -DIRECTION OUTPUT -pinname T18 -fixed no
set_io USB_ULPI_XCLK -DIRECTION INPUT -pinname R17 -fixed no

#
# Core cell constraints
#

set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[4\] -fixed no 375 36
set_location MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2\[0\] -fixed no 268 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[11\] -fixed no 390 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[21\] -fixed no 395 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[10\] -fixed no 388 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[17\] -fixed no 374 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[20\] -fixed no 393 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[27\] -fixed no 389 39
set_location MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2\[1\] -fixed no 335 33
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[0\] -fixed no 383 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[19\] -fixed no 384 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[29\] -fixed no 387 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[5\] -fixed no 372 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PSLVERR_u_0 -fixed no 387 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[12\] -fixed no 386 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[22\] -fixed no 390 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[15\] -fixed no 378 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[25\] -fixed no 389 36
set_location MC_System_sb_0/CCC_0/GL0_INST -fixed no 225 54
set_location MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1 -fixed no 218 102
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[3\] -fixed no 388 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[7\] -fixed no 384 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[6\] -fixed no 376 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[31\] -fixed no 385 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[30\] -fixed no 393 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[16\] -fixed no 373 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[26\] -fixed no 373 39
set_location MC_System_sb_0/CCC_0/GL1_INST -fixed no 222 54
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[9\] -fixed no 395 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[13\] -fixed no 382 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[23\] -fixed no 391 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[14\] -fixed no 381 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[24\] -fixed no 372 39
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[1\] -fixed no 377 36
set_location MC_System_sb_0/CCC_0/GL1_INST/U0_RGB1 -fixed no 218 0
set_location MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2_0\[0\] -fixed no 386 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[8\] -fixed no 392 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/N_39_i -fixed no 385 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[2\] -fixed no 394 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[18\] -fixed no 374 36
set_location MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1\[28\] -fixed no 379 36
set_location MC_System_sb_0/CCC_0/CCC_INST -fixed no 372 92
