
fsm_encoding {3617411741} sequential

fsm_state_encoding {3617411741} idle {00}

fsm_state_encoding {3617411741} ref_speed_scale {01}

fsm_state_encoding {3617411741} output {10}

fsm_registers {3617411741} {state[1]}  {state[0]} 
