@W: MO160 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Register bit state[0] is always 0, optimizing ...
@W: MO160 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\clarke.vhd":161:8:161:9|Register bit state[0] is always 0, optimizing ...
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":781:8:781:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm1_areset_n_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":781:8:781:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm1_areset_n_clk_base reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1331:8:1331:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.RESET_N_F2M_int reduced to a combinational gate by constant propagation 
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Stepper_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[1],  because it is equivalent to instance Stepper_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[0]
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[1] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[2] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[0] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[2] reduced to a combinational gate by constant propagation
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Removing instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[1],  because it is equivalent to instance Stepper_Axis_0.adc_measurements_0.s_r_sck_max_count[3]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Removing instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[0],  because it is equivalent to instance Stepper_Axis_0.adc_measurements_0.s_r_sck_max_count[3]
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\seq_controller.vhd":289:2:289:3|Sequential instance Stepper_Axis_0.seq_controller_0.state[1] reduced to a combinational gate by constant propagation
