pin,slack
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_18:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_18:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:CLK,1483
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:D,8712
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:Q,1483
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[5]:A,4463
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[5]:B,4379
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[5]:C,4190
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[5]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[5]:Y,4190
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14:A,3897
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14:B,2942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14:CC,2868
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14:S,2868
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14:UB,2942
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/IQ_PI_DONE_PROC_op_eq_un9_clear_buffer_i:A,7896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/IQ_PI_DONE_PROC_op_eq_un9_clear_buffer_i:B,7861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/IQ_PI_DONE_PROC_op_eq_un9_clear_buffer_i:Y,7861
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7:B,2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7:CC,2698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7:P,2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7:S,2698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:D,5114
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI6R56D[10]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI6R56D[10]:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI6R56D[10]:C,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI6R56D[10]:CC,2841
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI6R56D[10]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI6R56D[10]:P,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI6R56D[10]:S,2841
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI6R56D[10]:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_168:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_168:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_168:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_168:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0:An,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0:ENn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0:YNn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_6:B,6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_6:CC,7203
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_6:P,6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_6:S,7203
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:CLK,4212
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:D,8717
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:Q,4212
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[29]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[29]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[29]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILN0I1[33]:A,4779
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILN0I1[33]:B,3723
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILN0I1[33]:C,4852
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILN0I1[33]:Y,3723
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_6:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_6:C,4211
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_6:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_6:IPC,4211
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:D,29
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_13:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_13:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_2:A,3715
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_2:B,3411
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_2:C,3593
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_2:Y,3411
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:D,6502
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:C,6754
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0:B,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0:P,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_3:B,2143
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_3:C,1759
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_3:CC,1188
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_3:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_3:S,1188
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_3:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI2QAV[1]:A,7843
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI2QAV[1]:B,7792
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI2QAV[1]:Y,7792
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[0],6966
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[10],6753
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[11],6692
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[1],6888
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[2],6830
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[3],6920
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[4],6849
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[5],6788
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[6],6917
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[7],6801
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[8],6740
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CC[9],6835
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CI,6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:CO,6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[0],6940
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[1],6877
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[2],7060
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[3],7036
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[6],7048
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[7],7097
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[8],7167
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:P[9],7154
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[10]:A,5044
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[10]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[10]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[10]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[10]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:CLK,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:Q,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:D,6059
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:CLK,1422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:D,8683
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:Q,1422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[22]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[1]:A,4034
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[1]:C,5037
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[1]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[1]:D,4907
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[1]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[1]:Y,4034
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_4_0:A,3445
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_4_0:B,808
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_4_0:C,1220
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_4_0:CC,1332
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_4_0:D,-360
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_4_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_4_0:S,1332
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_4_0:UB,-360
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI11LU[1]:A,6912
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI11LU[1]:B,6549
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI11LU[1]:C,6458
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI11LU[1]:Y,6458
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJP8P1[10]:A,2467
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJP8P1[10]:B,2234
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJP8P1[10]:C,2345
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJP8P1[10]:Y,2234
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:C,6772
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:IPC,6772
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[8]:A,4652
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[8]:B,2116
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[8]:C,2072
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[8]:Y,2072
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:CLK,6875
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:D,7005
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:Q,6875
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITSKU[1]:A,6799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITSKU[1]:B,6410
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITSKU[1]:C,6339
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITSKU[1]:Y,6339
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_13:B,6361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_13:C,4413
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_13:IPB,6361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_13:IPC,4413
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:CLK,4947
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:Q,4947
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[2]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_246:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_246:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_246:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_246:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_246:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:CLK,6755
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:D,6917
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:Q,6755
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[10],2890
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[11],2841
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[1],4368
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[2],4304
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[3],4032
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[4],3964
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[5],3914
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[6],3074
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[7],2950
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[8],2889
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CC[9],2972
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:CO,2765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[0],3764
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[1],3793
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[2],2765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[3],2784
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[6],2796
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[7],2802
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[8],2872
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:P[9],2902
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[0],6195
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[1],6526
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[3]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[3]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[3]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[3]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16:A,3867
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16:B,3325
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16:CC,2844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16:S,2844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16:UB,3325
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_ns_i_0[0]:A,6935
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_ns_i_0[0]:B,6956
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_ns_i_0[0]:Y,6935
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:CLK,6847
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:Q,6847
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[37]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[37]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[37]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_6:B,4597
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_6:C,3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_6:CC,3761
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_6:P,3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_6:S,3761
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_6:UB,4597
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:CLK,7909
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:Q,7909
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[7]:A,4443
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[7]:B,6667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[7]:C,3307
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[7]:D,4120
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[7]:Y,3307
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:CLK,6847
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:Q,6847
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_12:A,6244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_12:B,6037
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_12:P,6198
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_12:UB,6037
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_23:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_23:B,7786
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_23:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_23:CC,6692
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_23:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_23:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_23:S,6692
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_23:UB,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[2]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[2]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[2]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:CLK,2014
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:D,7384
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:Q,2014
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[5]:A,2076
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[5]:B,2948
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[5]:C,5242
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[5]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[5]:D,5085
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[5]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[5]:Y,2076
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[11]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_10:B,6197
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_10:UB,6197
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_2:B,6048
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_2:C,6156
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_2:CC,6251
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_2:P,6048
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_2:S,6251
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_5:A,1840
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_5:B,1717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_5:C,459
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_5:D,1113
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_5:Y,459
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_7:B,1651
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_7:C,1235
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_7:CC,1104
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_7:P,1235
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_7:S,1104
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:CLK,3295
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:Q,3295
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_0:A,3095
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_0:B,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_0:C,4649
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_0:D,3987
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_0:Y,2867
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:C,6833
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPC,6833
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[1]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[1]:B,6926
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[1]:C,7024
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[1]:CC,7386
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[1]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[1]:P,6926
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[1]:S,7386
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:CLK,1898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:D,8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:Q,1898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:CLK,6768
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:D,7066
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:Q,6768
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_14:B,6238
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_14:UB,6238
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[40]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[40]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[40]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[40]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[40]:Y,88
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_11:A,7835
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_11:B,7009
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_11:CC,6879
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_11:S,6879
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_11:UB,7009
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_6:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_6:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_6:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_6:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_6:IPC,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:CLK,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:Q,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[14]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[2]:A,8004
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[2]:B,7916
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[2]:C,7842
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[2]:D,7742
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[2]:Y,7742
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_16:B,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_16:S,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:CLK,383
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:D,6851
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:Q,383
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:CLK,648
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:D,8674
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:Q,648
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:CLK,4469
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:D,4351
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:Q,4469
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_35:B,6446
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_35:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_35:D,6486
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_35:IPB,6446
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_35:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_35:IPD,6486
A0_PWM_VH_O_obuf/U0/U_IOENFF:A,
A0_PWM_VH_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIQVB62[27]:A,4699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIQVB62[27]:B,3717
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIQVB62[27]:C,3673
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIQVB62[27]:Y,3673
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_8_0:A,1563
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_8_0:B,958
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_8_0:C,1370
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_8_0:CC,738
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_8_0:D,-210
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_8_0:P,-137
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_8_0:S,738
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_8_0:UB,-210
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:CC[0],2656
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:CC[1],2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:CC[2],2868
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:CC[3],2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:CC[4],2844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:CC[5],2564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:CI,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[0],2853
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[1],2794
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[2],2942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[3],3197
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[4],3325
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[13]:A,6985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[13]:B,6901
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[13]:C,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[13]:Y,6226
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:C,6747
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:IPC,6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14_0:A,6219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14_0:B,7274
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14_0:C,7084
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14_0:CC,5357
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14_0:S,5357
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14_0:UB,7084
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[5]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[5]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[5]:C,5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[5]:Y,5224
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:CLK,6711
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:D,6888
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:Q,6711
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[10]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[10]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[10]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIALCR7[6]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIALCR7[6]:B,4368
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIALCR7[6]:C,7228
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIALCR7[6]:CC,4196
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIALCR7[6]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIALCR7[6]:P,4368
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIALCR7[6]:S,4196
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIALCR7[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[9]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[9]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[9]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_2:A,3361
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_2:B,4639
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_2:P,3361
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_2:UB,4639
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:CLK,6841
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:Q,6841
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[1]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[2]:A,6966
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[2]:B,6918
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[2]:Y,6918
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[34]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[34]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[34]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[34]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[34]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[13]:A,4507
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[13]:B,4397
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[13]:C,3458
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[13]:D,3378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[13]:Y,3378
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3_RNIOSV81[1]:A,3510
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3_RNIOSV81[1]:B,3194
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3_RNIOSV81[1]:C,2368
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3_RNIOSV81[1]:D,2105
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3_RNIOSV81[1]:Y,2105
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:CLK,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:D,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:Q,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[23]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[23]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[23]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[23]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:CLK,6731
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:Q,6731
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10:A,7808
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10:B,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10:CC,5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10:S,5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10:UB,5114
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[6]:A,1697
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[6]:B,4397
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[6]:C,2876
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[6]:Y,1697
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[11]:A,4213
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[11]:B,1890
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[11]:C,1901
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[11]:Y,1890
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNIR9B31[0]:A,5948
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNIR9B31[0]:B,5858
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNIR9B31[0]:C,5826
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNIR9B31[0]:Y,5826
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:CLK,5115
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:Q,5115
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[12]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[12]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[12]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[12]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:CLK,6731
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:D,6974
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:Q,6731
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[32]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[32]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[32]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[32]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[32]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_16:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_16:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17:B,4364
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17:UB,4364
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[14]:A,1836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[14]:B,2708
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[14]:C,5002
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[14]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[14]:D,4845
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[14]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[14]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[14]:Y,1836
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_8:B,1647
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_8:C,1265
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_8:CC,1290
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_8:P,1265
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_8:S,1290
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2]:B,5723
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2]:C,6001
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2]:CC,5882
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2]:P,5723
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2]:S,5882
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:CLK,4981
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:D,6944
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:Q,4981
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[16]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:CLK,4930
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:Q,4930
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:D,3351
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_8:A,3072
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_8:B,4745
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_8:P,3072
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_8:UB,4745
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI2N4T7[12]:A,6283
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI2N4T7[12]:B,1306
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI2N4T7[12]:C,1376
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI2N4T7[12]:CC,1499
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI2N4T7[12]:D,5882
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI2N4T7[12]:P,1412
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI2N4T7[12]:S,1499
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI2N4T7[12]:UB,1306
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:CLK,4315
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:D,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:EN,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:Q,4315
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_Z:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_0[1]:A,3206
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_0[1]:B,3228
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_0[1]:C,2207
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_0[1]:Y,2207
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_8:A,1270
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_8:B,1510
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_8:P,1270
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_8:UB,1510
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_14:A,5299
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_14:B,4562
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_14:CC,4221
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_14:S,4221
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_14:UB,4562
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_18_0:A,1821
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_18_0:B,1143
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_18_0:C,1218
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_18_0:CC,-331
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_18_0:D,-23
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_18_0:P,86
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_18_0:S,-331
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_18_0:UB,-23
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:C,6791
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:IPC,6791
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO_0:A,5846
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO_0:B,5798
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO_0:C,3911
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO_0:D,3861
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO_0:Y,3861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:CLK,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:D,6935
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:Q,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHUK4H[15]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHUK4H[15]:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHUK4H[15]:C,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHUK4H[15]:CC,2826
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHUK4H[15]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHUK4H[15]:P,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHUK4H[15]:S,2826
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHUK4H[15]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:CLK,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:Q,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[15]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_16:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_16:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_10:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_10:C,4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_10:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_10:IPC,4251
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_28:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_28:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[7]:A,3570
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[7]:B,5804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[7]:C,2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[7]:D,3228
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[7]:Y,2456
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[5]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[5]:B,5130
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[5]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[5]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[5]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:CLK,608
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:D,8673
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:Q,608
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:CLK,2006
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:D,6921
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:Q,2006
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0_RNO:A,3292
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0_RNO:B,6117
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0_RNO:C,5815
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0_RNO:D,4043
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0_RNO:Y,3292
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:CLK,3367
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:Q,3367
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:D,3501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_14_0:A,7398
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_14_0:B,6817
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_14_0:C,3021
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_14_0:CC,2735
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_14_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_14_0:P,3169
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_14_0:S,2735
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_14_0:UB,3021
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_o3[5]:A,3767
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_o3[5]:B,3710
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_o3[5]:Y,3710
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_5:A,5966
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_5:B,5262
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_5:CC,5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_5:S,5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_5:UB,5262
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_9:A,4495
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_9:B,4373
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_9:P,4423
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_9:UB,4373
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:CLK,5159
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:Q,5159
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:CLK,136
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:D,2373
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:Q,136
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[1]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_XCLK_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_XCLK_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:B,7863
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:C,6809
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:D,7849
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPB,7863
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPC,6809
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPD,7849
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_10_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_10_0:B,6815
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_10_0:C,3019
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_10_0:CC,2678
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_10_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_10_0:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_10_0:S,2678
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_10_0:UB,3019
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO_0:A,3182
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO_0:B,2076
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO_0:C,5021
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO_0:D,4832
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO_0:Y,2076
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[4]:A,2764
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[4]:B,4033
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[4]:C,5872
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[4]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[4]:D,5718
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[4]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[4]:Y,2764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:CLK,1530
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:Q,1530
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_7:A,4984
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_7:B,4883
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_7:P,4928
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_7:UB,4883
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:CLK,6841
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:Q,6841
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[1]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:CLK,4699
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:D,8854
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:Q,4699
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18:A,3669
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18:B,1592
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18:P,1676
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18:UB,1592
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_10:A,7848
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_10:B,7084
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_10:CC,6911
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_10:S,6911
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_10:UB,7084
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:B,7882
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:C,6814
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:IPB,7882
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:IPC,6814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[1]:A,3351
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[1]:B,3377
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[1]:Y,3351
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_14:B,2692
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_14:UB,2692
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:CLK,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:D,5754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:Q,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[9]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[9]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[9]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:D,7820
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:EN,8389
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:CLK,4221
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:D,8684
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:Q,4221
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:CLK,4438
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:D,8684
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:Q,4438
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:CLK,232
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:D,6895
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:Q,232
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:C,6833
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPC,6833
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:CLK,6306
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:Q,6306
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:CLK,7060
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:Q,7060
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[4]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:CLK,5825
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:D,6911
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:Q,5825
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_8:B,6895
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_8:C,6983
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_8:CC,6840
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_8:P,6895
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_8:S,6840
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[21]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[21]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[21]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:C,6791
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:IPC,6791
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_14:B,6357
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_14:C,4265
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_14:IPB,6357
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_14:IPC,4265
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[11]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:IPENn,
GPIO_0_M2F_obuf/U0/U_IOENFF:A,
GPIO_0_M2F_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_21:A,7185
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_21:B,6990
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_21:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_21:CC,6962
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_21:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_21:P,7099
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_21:S,6962
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_21:UB,6990
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_32:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_32:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[0]:A,2274
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[0]:B,5982
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[0]:Y,2274
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:CLK,3109
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:Q,3109
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[15]:A,3747
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[15]:B,3666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[15]:C,3441
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[15]:D,2276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[15]:Y,2276
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[15]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[15]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[15]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[32]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[4]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[4]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[4]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_15:A,3645
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_15:B,1100
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_15:P,1219
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_15:UB,1100
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11:B,3651
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11:C,3675
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11:CC,3393
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11:S,3393
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11:UB,3651
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:CLK,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:D,8679
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:Q,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIFLN43[10]:A,2926
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIFLN43[10]:B,2686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIFLN43[10]:C,2798
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIFLN43[10]:Y,2686
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[12]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[12]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[12]:Y,5379
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIRODMF[39]:A,2627
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIRODMF[39]:B,1947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIRODMF[39]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIRODMF[39]:CC,1422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIRODMF[39]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIRODMF[39]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIRODMF[39]:S,1422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIRODMF[39]:UB,1947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0:A,5365
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0:B,6263
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0:C,5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0:D,6558
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0:P,5242
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0:UB,5116
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:CLK,4836
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:D,6830
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:Q,4836
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:CLK,709
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:D,8677
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:Q,709
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIJ7DU1[0]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIJ7DU1[0]:B,4087
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIJ7DU1[0]:C,6924
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIJ7DU1[0]:CC,5677
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIJ7DU1[0]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIJ7DU1[0]:P,4087
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIJ7DU1[0]:S,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIJ7DU1[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[3]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[3]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[3]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:CLK,3559
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:D,8686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:Q,3559
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_7:A,5395
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_7:B,5103
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_7:CC,5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_7:P,5157
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_7:S,5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_7:UB,5103
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:CLK,3691
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:D,6817
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:Q,3691
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[39]:A,829
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[39]:B,686
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[39]:C,212
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[39]:Y,212
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:CLK,2823
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:D,2223
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:Q,2823
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:CLK,6847
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:Q,6847
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[6]:A,6075
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[6]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[6]:Y,6075
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_10:B,1122
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_10:UB,1122
BLDC_Encoder_Axis_0/MSC_i_9/s_count_1_sqmuxa_0_a2:A,6667
BLDC_Encoder_Axis_0/MSC_i_9/s_count_1_sqmuxa_0_a2:B,6638
BLDC_Encoder_Axis_0/MSC_i_9/s_count_1_sqmuxa_0_a2:C,6439
BLDC_Encoder_Axis_0/MSC_i_9/s_count_1_sqmuxa_0_a2:D,4298
BLDC_Encoder_Axis_0/MSC_i_9/s_count_1_sqmuxa_0_a2:Y,4298
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[2]:A,6250
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[2]:B,6166
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[2]:C,5491
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[2]:Y,5491
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_4_217_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_4_217_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_4_217_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_4_217_i_m2:Y,7698
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_35:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_35:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_35:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_35:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:CLK,6745
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:Q,6745
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[42]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[42]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[42]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[42]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[42]:Y,88
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO_0:A,3185
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO_0:B,2121
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO_0:C,5033
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO_0:D,4844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO_0:Y,2121
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:D,8854
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/s_mas_done_dly[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:CLK,4849
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:D,8712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:Q,4849
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:CLK,6818
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:Q,6818
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:CLK,4110
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:Q,4110
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_13:A,3384
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_13:B,5124
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_13:P,3384
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_13:UB,5124
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:CLK,6037
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:D,8673
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:Q,6037
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[4]:A,4383
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[4]:B,1987
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[4]:C,4258
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[4]:Y,1987
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_215:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_215:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_215:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_215:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_215:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:CLK,5844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:D,8670
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:Q,5844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:CC[0],2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:CC[1],2624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:CC[2],2692
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:CC[3],2711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:CC[4],2681
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:CC[5],2937
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:CI,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[0],2899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[9]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[9]:B,4532
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[9]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[9]:Y,91
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:D,8827
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/s_mas_done_dly[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:CLK,7730
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:Q,7730
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:CLK,4268
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:D,5686
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:Q,4268
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_5_0:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_5_0:B,6535
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_5_0:C,5392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_5_0:CC,5340
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_5_0:D,6836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_5_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_5_0:S,5340
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_5_0:UB,5392
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_10:B,6145
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_10:UB,6145
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_11:B,4287
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_11:UB,4287
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:CLK,3250
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:D,7149
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:Q,3250
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:CLK,5132
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:D,8664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:Q,5132
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_0:A,5439
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_0:B,5345
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_0:C,3488
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_0:D,3341
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_0:Y,3341
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[32]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[32]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[32]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_18:A,1059
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_18:B,908
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_18:C,877
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_18:D,738
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_18:Y,738
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[14]:A,6021
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[14]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[14]:Y,6021
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:CC[6],2764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:CI,2764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[0],3066
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[1],2997
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[3],3183
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[0],2917
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[1],3015
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[2],3141
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[3],3063
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[4],3100
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[5],3204
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_1:UB[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_56:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_56:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_56:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_56:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_56:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[35]:A,648
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[35]:B,505
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[35]:C,31
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[35]:Y,31
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_5:A,7100
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_5:B,6959
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_5:C,6517
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_5:CC,6710
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_5:P,6639
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_5:S,6710
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_5:UB,6517
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:D,5390
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[6]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:CLK,4947
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:Q,4947
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0:A,7162
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0:B,6617
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0:C,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0:CC,1945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0:P,1870
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0:S,1945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0:UB,1816
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_129:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_129:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_129:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_129:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_129:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:C,6763
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:IPC,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[35]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[35]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[35]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[35]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_5:A,7835
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_5:B,6875
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_5:CC,7005
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_5:S,7005
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_5:UB,6875
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[10],4269
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[11],4220
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[1],5686
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[2],5503
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[3],5081
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[4],5011
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[5],4950
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[6],4453
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[7],4348
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[8],4287
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CC[9],4351
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:CO,4341
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[0],5159
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[1],4918
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[2],4252
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[3],4239
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[6],4220
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[7],4380
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[8],4461
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:P[9],4459
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[1],4912
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_1:A,6771
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_1:B,6697
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_1:CC,7544
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_1:P,6705
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_1:S,7544
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_1:UB,6697
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[16]:A,2384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[16]:B,2342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[16]:Y,2342
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_3[17]:A,3898
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_3[17]:B,2368
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_3[17]:C,3884
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_3[17]:D,3571
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_3[17]:Y,2368
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[11]:A,6281
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[11]:B,6233
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[11]:C,5529
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[11]:Y,5529
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:B,7863
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:C,6809
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:D,7849
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPB,7863
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPC,6809
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPD,7849
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[21]:A,364
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[21]:B,287
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[21]:C,-253
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[21]:Y,-253
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[24]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[24]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[24]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[24]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[24]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset_RNIJJH41[13]:A,5001
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset_RNIJJH41[13]:B,3526
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset_RNIJJH41[13]:C,4879
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset_RNIJJH41[13]:Y,3526
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:CLK,1963
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:D,6994
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:Q,1963
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[0]:A,5969
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[0]:B,5892
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[0]:C,5513
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[0]:D,4276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[0]:Y,4276
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_26:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_26:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[16]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[16]:B,4745
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[16]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[16]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[16]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:CC[0],6837
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:CC[1],6759
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:CC[2],6701
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:CC[3],6791
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:CC[4],6720
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:CC[5],6659
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:CI,6659
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[0],6922
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[1],6834
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[2],6986
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[3],7237
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[4],7376
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_1[6]:A,3682
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_1[6]:B,4748
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_1[6]:C,3564
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_1[6]:Y,3564
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[16]:A,7591
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[16]:B,5549
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[16]:C,5345
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[16]:CC,4737
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[16]:D,7121
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[16]:P,5437
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[16]:S,4737
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[16]:UB,5345
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:CLK,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:Q,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[0]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[0]:B,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[0]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1:A,1395
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1:B,1316
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1:CC,1688
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1:P,1316
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1:S,1688
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1:UB,1339
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_30:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_30:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[10],6911
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[11],6850
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[1],7524
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[2],7460
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[3],7145
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[4],7078
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[5],7028
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[6],7049
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[7],6958
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[8],6898
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CC[9],6995
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:CO,6793
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[0],6920
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[1],6877
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[2],7051
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[3],7036
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[6],7048
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[7],7088
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[8],7158
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:P[9],7154
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[0],6793
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[10],7084
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[11],7205
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[1],6895
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[2],7019
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[3],6938
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[4],6976
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[5],7068
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[6],6959
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[7],7017
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[8],7125
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_0:UB[9],7066
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:D,5427
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[24]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[24]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[24]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[24]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[24]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[30]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[30]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[30]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__m6_0_o2:A,6856
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__m6_0_o2:B,6808
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__m6_0_o2:Y,6808
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_18:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_18:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:CLK,1992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:D,1884
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:Q,1992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[30]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[30]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[30]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[30]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3:A,7088
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3:B,6944
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3:CC,7151
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3:P,7042
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3:S,7151
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3:UB,6944
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[7]:A,5897
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[7]:B,5468
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[7]:C,5357
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[7]:D,4265
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[7]:Y,4265
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:CLK,4791
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:EN,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:Q,4791
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[24]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[24]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[24]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[24]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[42]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[42]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[42]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[42]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[31]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[31]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[31]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5:B,5139
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5:CC,4504
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5:S,4504
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_31:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_31:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:C,6771
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:IPC,6771
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[12]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[12]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[12]:Y,7440
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un8_s_cs_n:A,6970
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un8_s_cs_n:B,6759
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un8_s_cs_n:C,6902
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un8_s_cs_n:Y,6759
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:CLK,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:Q,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_1:A,7073
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_1:B,7028
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_1:C,6577
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_1:CC,7101
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_1:P,6608
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_1:S,7101
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_1:UB,6577
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[15]:A,6327
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[15]:B,6250
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[15]:C,5868
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[15]:D,4634
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[15]:Y,4634
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry:B,4798
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry:C,6701
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry:CC,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry:D,4608
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry:P,4627
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry:UB,4608
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[14]:A,2147
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[14]:B,3517
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[14]:C,5246
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[14]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[14]:D,5107
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[14]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[14]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[14]:Y,2147
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:CLK,1935
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:Q,1935
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:CO,1273
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[0],3010
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[1],1688
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[2],1787
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[3],1484
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[6],1402
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[7],1322
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[8],1337
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:P[9],1454
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[0],2843
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[10],1293
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[11],1346
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[1],1699
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[2],1748
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[3],1373
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[4],1339
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[5],1378
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[6],1306
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[7],1273
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[8],1303
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_0:UB[9],1359
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_9:A,3595
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_9:B,1152
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_9:P,1261
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_9:UB,1152
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:D,8717
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:CLK,5897
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:D,8706
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:Q,5897
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0:A,3432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0:B,7196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0:C,6720
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0:CC,1893
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0:P,3432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0:S,1893
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0:UB,6720
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:CLK,5320
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:Q,5320
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:D,3501
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:CLK,5821
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:D,6000
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:Q,5821
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[6]:A,4792
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[6]:B,4749
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[6]:C,4290
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[6]:Y,4290
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:CLK,2152
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:D,1893
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:Q,2152
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_2_i_m2_i_m2[17]:A,4662
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_2_i_m2_i_m2[17]:B,2368
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_2_i_m2_i_m2[17]:C,4547
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_2_i_m2_i_m2[17]:Y,2368
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[32]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[32]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[32]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[32]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[32]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[43]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[43]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[43]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[43]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_12:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_12:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:CLK,1931
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:D,8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:Q,1931
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[13]:A,7273
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[13]:B,5225
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[13]:C,4984
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[13]:CC,4740
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[13]:D,6760
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[13]:P,5100
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[13]:S,4740
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[13]:UB,4984
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_9:A,7048
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_9:B,6889
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_9:CC,7020
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_9:P,6982
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_9:S,7020
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_9:UB,6889
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:CLK,7832
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:Q,7832
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[33]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_3[1]:A,5212
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_3[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_3[1]:C,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_3[1]:D,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_3[1]:Y,5212
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:CLK,6890
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:Q,6890
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_26:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_26:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1:B,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1:C,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1:CC,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[43]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[43]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[43]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[43]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10:A,971
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10:B,993
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10:C,840
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10:D,698
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10:Y,698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:CLK,4226
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:Q,4226
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:CC[6],4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:CI,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[0],4273
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[1],4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[3],4332
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[0],4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[1],4130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[2],4221
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[3],4208
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[4],4174
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[5],6370
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[1]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[1]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[1]:C,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[1]:Y,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_2[2]:A,3988
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_2[2]:B,3903
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_2[2]:C,1877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_2[2]:Y,1877
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[13]:A,1275
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[13]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[13]:Y,1275
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[5]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[5]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[5]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[5]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_RNO[2]:A,6926
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_RNO[2]:B,6609
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_RNO[2]:C,6913
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_RNO[2]:D,6785
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_RNO[2]:Y,6609
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:C,6745
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:IPC,6745
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m31_1:A,4665
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m31_1:B,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m31_1:C,4781
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m31_1:Y,1898
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:C,6771
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:IPC,6771
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12_1:A,1674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12_1:B,1547
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12_1:C,1425
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12_1:Y,1425
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9:A,7206
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9:B,5144
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9:CC,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9:P,5232
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9:S,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9:UB,5144
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:CLK,4184
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:D,5877
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:Q,4184
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[1]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_152:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_152:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_152:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_152:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_152:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2BOC9[27]:A,2723
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2BOC9[27]:B,1689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2BOC9[27]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2BOC9[27]:CC,1657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2BOC9[27]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2BOC9[27]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2BOC9[27]:S,1657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2BOC9[27]:UB,1689
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:CLK,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:D,7252
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:Q,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_12:B,6915
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_12:CC,7105
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_12:P,6915
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_12:S,7105
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:CLK,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:Q,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_28:A,7848
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_28:B,7086
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_28:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_28:CC,6803
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_28:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_28:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_28:S,6803
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_28:UB,7086
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:CLK,6389
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:Q,6389
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[2]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[2]:B,6955
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[2]:C,6999
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[2]:CC,7114
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[2]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[2]:P,6955
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[2]:S,7114
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:CLK,5427
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:Q,5427
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_14:B,2152
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_14:UB,2152
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:CLK,4493
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:Q,4493
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:CLK,6062
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:D,8678
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:Q,6062
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1CRPH[43]:A,2505
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1CRPH[43]:B,2502
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1CRPH[43]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1CRPH[43]:CC,1347
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1CRPH[43]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1CRPH[43]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1CRPH[43]:S,1347
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1CRPH[43]:UB,3136
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5UN81[11]:A,3163
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5UN81[11]:B,3086
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5UN81[11]:C,2639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5UN81[11]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[7]:A,5637
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[7]:B,2988
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[7]:C,3355
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[7]:D,3225
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[7]:Y,2988
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:CLK,6745
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:Q,6745
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[17]:A,2720
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[17]:B,4790
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[17]:C,4223
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[17]:Y,2720
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6:A,6142
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6:B,6065
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6:C,3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6:D,4481
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6:Y,3654
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:D,5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o_0_sqmuxa_0_a3:A,5547
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o_0_sqmuxa_0_a3:B,6729
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o_0_sqmuxa_0_a3:Y,5547
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_197:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_197:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_197:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_197:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_197:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIGND62[29]:A,3856
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIGND62[29]:B,4780
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIGND62[29]:C,3802
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIGND62[29]:Y,3802
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:D,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:CLK,4344
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:D,8717
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:Q,4344
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[10]:A,4502
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[10]:B,4418
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[10]:C,4241
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[10]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[10]:Y,4241
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_2[7]:A,6971
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_2[7]:B,6959
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_2[7]:C,3954
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_2[7]:D,5801
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_2[7]:Y,3954
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:CLK,6814
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:Q,6814
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[1]:A,4066
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[1]:C,5212
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[1]:D,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[1]:Y,4066
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_10_0:A,3323
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_10_0:B,943
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_10_0:C,1355
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_10_0:CC,871
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_10_0:D,-225
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_10_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_10_0:S,871
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_10_0:UB,-225
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:CLK,4374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:D,6370
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:Q,4374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:CLK,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:D,6718
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:Q,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[1]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[1]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[1]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_32:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_32:B,5978
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_32:C,5878
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_32:CC,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_32:D,5701
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_32:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_32:S,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_32:UB,5701
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[6]:A,4495
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[6]:B,2099
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[6]:C,4370
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[6]:Y,2099
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/MISO_DATA_REG_PROC_un11_s_sckctr_done:A,7818
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/MISO_DATA_REG_PROC_un11_s_sckctr_done:B,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/MISO_DATA_REG_PROC_un11_s_sckctr_done:Y,7740
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:C,6697
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:IPC,6697
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:C,6742
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:IPC,6742
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[12]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[12]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[12]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_14:A,6016
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_14:B,5578
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_14:CC,4995
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_14:S,4995
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_14:UB,5578
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:CLK,6037
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:Q,6037
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8_RNI5CG62:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8_RNI5CG62:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8_RNI5CG62:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8_RNI5CG62:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8_RNI5CG62:D,5953
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8_RNI5CG62:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8_RNI5CG62:UB,5953
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[34]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[34]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[34]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[34]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[34]:Y,88
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:C,6709
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:IPC,6709
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[0]:A,4890
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[0]:B,4819
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[0]:Y,4819
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[10]:A,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[10]:B,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[10]:C,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[10]:Y,7659
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO_0:A,5617
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO_0:B,5532
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO_0:C,3669
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO_0:D,3582
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO_0:Y,3582
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_1:A,4803
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_1:B,4717
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_1:P,4717
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_1:UB,4752
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_7_0:A,7200
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_7_0:B,6735
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_7_0:C,2930
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_7_0:CC,2726
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_7_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_7_0:P,2971
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_7_0:S,2726
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_7_0:UB,2930
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:CLK,2111
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:Q,2111
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:CLK,5139
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:Q,5139
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_15:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_15:B,7395
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_15:CC,6907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_15:S,6907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_15:UB,7395
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:CLK,3921
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:Q,3921
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:CLK,4706
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:D,6992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:Q,4706
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0:A,6123
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0:B,5879
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0:C,5796
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0:P,5948
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0:UB,5796
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[7]:A,1809
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[7]:B,4509
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[7]:C,2988
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[7]:Y,1809
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_5:B,6169
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_5:UB,6169
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:CLK,5922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:Q,5922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[13]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[13]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[13]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[13]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy:B,6699
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy:C,6457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy:P,6457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[32]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[32]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[32]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[32]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:CLK,4785
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:D,6927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:Q,4785
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:CLK,2610
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:D,8706
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:Q,2610
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:CLK,7946
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:Q,7946
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJUI84[2]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJUI84[2]:B,7049
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJUI84[2]:C,2784
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJUI84[2]:CC,4032
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJUI84[2]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJUI84[2]:P,2784
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJUI84[2]:S,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJUI84[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_26:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_26:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_26:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_26:CC,6645
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_26:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_26:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_26:S,6645
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_26:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_7_0:A,1493
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_7_0:B,868
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_7_0:C,1280
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_7_0:CC,908
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_7_0:D,-300
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_7_0:P,-207
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_7_0:S,908
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_7_0:UB,-300
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIBR4O[5]:A,3127
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIBR4O[5]:B,3050
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIBR4O[5]:C,2603
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIBR4O[5]:Y,2603
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_23:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_23:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:CLK,5016
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:Q,5016
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:CLK,7895
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:Q,7895
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_12:A,7207
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_12:B,7005
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_12:C,6583
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_12:CC,6548
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_12:P,6746
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_12:S,6548
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_12:UB,6583
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:C,6689
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:IPC,6689
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_66:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_66:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_66:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_66:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_66:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[14]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[14]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[14]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_15_96_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_15_96_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_15_96_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_15_96_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:CLK,1672
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:D,6027
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:Q,1672
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[6]:A,2920
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[6]:B,2818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[6]:C,2595
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[6]:Y,2595
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:CLK,5967
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:Q,5967
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:CLK,4252
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:Q,4252
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:CLK,5357
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:Q,5357
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0_a2:A,5182
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0_a2:B,5434
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0_a2:C,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0_a2:D,5110
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0_a2:Y,2990
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:CLK,4982
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:Q,4982
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[4]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_71:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_71:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_71:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_71:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:CLK,829
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:D,8674
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:Q,829
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[10],2167
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[11],2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[1],7061
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[2],2745
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[3],2324
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[4],2254
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[5],2193
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[6],2297
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[7],2223
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[8],2175
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CC[9],2246
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:CO,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[0],6457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[1],2088
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[2],2187
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[3],2153
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[6],2231
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[7],2378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[8],2448
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:P[9],2439
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[10],2179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[11],2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[1],2070
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[2],2122
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[3],2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[4],2047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[5],2248
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[6],2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[7],2282
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[8],2372
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_0:UB[9],2336
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI30N3B[6]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI30N3B[6]:B,4380
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI30N3B[6]:C,7228
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI30N3B[6]:CC,4348
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI30N3B[6]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI30N3B[6]:P,4380
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI30N3B[6]:S,4348
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI30N3B[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_11:B,1346
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_11:UB,1346
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:CLK,7691
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:Q,7691
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[11]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[15]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[15]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[15]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[22]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIV1TT2[1]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIV1TT2[1]:B,4240
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIV1TT2[1]:C,7107
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIV1TT2[1]:CC,5613
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIV1TT2[1]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIV1TT2[1]:P,4240
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIV1TT2[1]:S,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIV1TT2[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[0]:A,2687
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[0]:B,1540
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[0]:C,3689
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[0]:D,2421
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[0]:Y,1540
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_5:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_5:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_5:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_5:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_5:IPC,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:C,6750
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:IPC,6750
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[24]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[24]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[24]:Y,5366
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_188:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_188:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_188:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_188:IPA,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_5:B,6197
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_5:UB,6197
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[8]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[8]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[8]:C,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[8]:Y,5143
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:CLK,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:Q,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[17]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[17]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[17]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[17]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[17]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[17]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[17]:Y,4589
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[1]:A,4034
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[1]:B,4066
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[1]:C,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[1]:D,4823
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[1]:Y,4034
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_10:B,5127
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_10:UB,5127
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_269:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_269:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_269:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_269:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_269:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:CLK,3796
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:D,6784
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:Q,3796
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4:A,6847
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4:B,6770
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4:C,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4:D,5186
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4:Y,4359
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:CLK,7827
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:Q,7827
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_228:A,6051
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_228:B,4561
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_228:C,5927
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_228:Y,4561
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[6]:A,1473
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[6]:B,5190
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[6]:Y,1473
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_1:A,1397
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_1:B,1410
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_1:C,182
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_1:D,836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_1:Y,182
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:CLK,7237
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:D,6695
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:Q,7237
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_27:B,6426
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_27:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_27:IPB,6426
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_27:IPC,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:CLK,6791
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:Q,6791
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_s_17:B,5691
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_s_17:C,5760
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_s_17:CC,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_s_17:S,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[21]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[21]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[21]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[16]:A,2830
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[16]:B,2753
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[16]:C,2044
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[16]:Y,2044
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:CLK,6143
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:D,4368
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:Q,6143
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_25:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_25:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:CLK,6174
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:Q,6174
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[4]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[4]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[4]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:CLK,6022
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:D,7101
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:Q,6022
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[15]:A,6157
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[15]:B,6079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[15]:C,4587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[15]:D,5567
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[15]:Y,4587
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_14:A,5778
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_14:B,5211
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_14:CC,5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_14:S,5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_14:UB,5211
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7:B,4545
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7:CC,4500
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7:P,4545
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7:S,4500
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIQ1F12[6]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIQ1F12[6]:B,7145
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIQ1F12[6]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIQ1F12[6]:CC,7029
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIQ1F12[6]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIQ1F12[6]:P,7145
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIQ1F12[6]:S,7029
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIQ1F12[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_14:B,4866
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_14:C,4711
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_14:P,4711
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_14:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[2]:A,1665
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[2]:B,5382
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[2]:Y,1665
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2:B,2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2:CC,3036
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2:P,2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2:S,3036
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_9:B,6957
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_9:CC,7149
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_9:P,6957
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_9:S,7149
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_9:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n:A,7035
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n:B,6992
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n:C,5824
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n:Y,5824
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:CLK,5127
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:D,3751
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:Q,5127
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:CLK,294
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:D,8679
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:Q,294
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[28]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_12:B,6940
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_12:CC,6966
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_12:P,6940
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_12:S,6966
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[17]:A,5077
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[17]:B,4986
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[17]:C,4790
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[17]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[17]:Y,4790
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_25_0:A,1835
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_25_0:B,1254
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_25_0:C,1327
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_25_0:CC,308
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_25_0:D,86
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_25_0:P,100
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_25_0:S,308
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_25_0:UB,86
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:CLK,2780
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:D,2534
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:Q,2780
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:CLK,4258
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:D,5666
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:Q,4258
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61[2]:A,2323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61[2]:B,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61[2]:C,2318
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61[2]:D,2196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61[2]:Y,2014
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[14]:A,5934
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[14]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[14]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[14]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[14]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:CLK,4418
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:D,6803
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:Q,4418
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:CLK,6772
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:Q,6772
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:CLK,4485
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:D,4650
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:Q,4485
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[14]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[14]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[14]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[14]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[22]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[22]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[22]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[22]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[22]:Y,-45
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[15]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[15]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[15]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_13_0:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_13_0:B,6480
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_13_0:C,5340
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_13_0:CC,5212
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_13_0:D,6781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_13_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_13_0:S,5212
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_13_0:UB,5340
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIE3VA1[17]:A,2722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIE3VA1[17]:B,2444
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIE3VA1[17]:C,3831
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIE3VA1[17]:Y,2444
A0_PWM_WL_O_obuf/U0/U_IOOUTFF:A,2345
A0_PWM_WL_O_obuf/U0/U_IOOUTFF:Y,2345
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:CLK,4996
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:Q,4996
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:D,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:CLK,1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:D,8686
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:Q,1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:CLK,7082
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:D,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:Q,7082
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_4:A,1869
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_4:B,1478
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_4:C,382
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_4:D,1036
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_4:Y,382
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[9]:A,5884
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[9]:B,5472
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[9]:C,5371
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[9]:D,4256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[9]:Y,4256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[7]:A,6093
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[7]:B,6045
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[7]:C,5341
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[7]:Y,5341
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5_RNO:A,5834
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5_RNO:B,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5_RNO:C,5712
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5_RNO:Y,4359
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[16]:A,6907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[16]:B,6604
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[16]:C,5754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[16]:Y,5754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10:S,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[10]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[10]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[10]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_11:B,1588
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_11:C,1206
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_11:CC,1270
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_11:P,1206
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_11:S,1270
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_11:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_15:A,6017
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_15:B,5395
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_15:CC,5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_15:S,5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_15:UB,5395
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[14]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[14]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[14]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_10:A,7749
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_10:B,6921
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_10:CC,6803
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_10:S,6803
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_10:UB,6921
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:C,6828
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPC,6828
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5T1M1[17]:A,2783
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5T1M1[17]:B,4200
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5T1M1[17]:Y,2783
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_276:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_276:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_276:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_276:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_276:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_276:IPC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[1]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[1]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[1]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[1]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_2:A,4424
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_2:B,6080
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_2:P,4424
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_2:UB,6080
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:CLK,4749
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:D,7044
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:Q,4749
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:CLK,2710
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:Q,2710
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_2:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_2:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_2:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_2:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_2:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_2:IPC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:CLK,6833
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:Q,6833
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:CLK,4850
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:D,6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:Q,4850
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_96:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_96:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_96:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_96:IPA,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRR662[16]:A,4590
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRR662[16]:B,3608
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRR662[16]:C,3564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRR662[16]:Y,3564
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4_RNI91OB1:A,6315
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4_RNI91OB1:B,4619
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4_RNI91OB1:C,4504
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4_RNI91OB1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4_RNI91OB1:D,5996
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4_RNI91OB1:P,4504
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4_RNI91OB1:UB,5996
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:CLK,6762
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:D,3483
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:Q,6762
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:D,5509
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[3]:A,2896
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[3]:B,2938
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[3]:Y,2896
A0_RUNNING_LED_obuf/U0/U_IOENFF:A,
A0_RUNNING_LED_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:D,5187
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[4]:A,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[4]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[4]:C,5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[4]:Y,5274
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_49:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_49:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_49:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_49:IPA,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:CLK,5299
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:Q,5299
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:CLK,6690
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:D,7046
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:Q,6690
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[42]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[42]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[42]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[42]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[42]:Y,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o_RNO:A,7398
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o_RNO:B,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o_RNO:Y,7398
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_a2_2_0[1]:A,3131
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_a2_2_0[1]:B,4361
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_a2_2_0[1]:Y,3131
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[27]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[27]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[27]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[27]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[27]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_14_0:A,2896
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_14_0:B,7170
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_14_0:C,6704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_14_0:CC,1716
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_14_0:D,4546
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_14_0:P,2896
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_14_0:S,1716
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_14_0:UB,4546
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[28]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[28]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[28]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[28]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[3]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[3]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[3]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[3]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:CLK,5905
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:D,5916
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:Q,5905
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:CLK,5771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:Q,5771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:CLK,4927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:Q,4927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[8]:A,4231
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[8]:B,1908
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[8]:C,1919
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[8]:Y,1908
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:B,7685
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:C,6697
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:IPB,7685
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:IPC,6697
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[0]:A,2970
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[0]:B,4239
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[0]:C,6071
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[0]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[0]:D,5917
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[0]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[0]:Y,2970
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:CLK,3032
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:D,2879
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:Q,3032
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_2:A,1471
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_2:B,1311
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_2:C,165
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_2:D,782
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_2:Y,165
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:CLK,3314
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:D,6969
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:Q,3314
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_7:B,3551
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_7:CC,3468
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_7:P,3551
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_7:S,3468
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:CLK,6763
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:Q,6763
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[12]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[2]:A,6953
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[2]:B,6879
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[2]:C,5857
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[2]:D,4624
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[2]:Y,4624
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[23]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[23]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[23]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[13]:A,5285
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[13]:B,5194
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[13]:C,4998
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[13]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[13]:Y,4998
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIBJE62[32]:A,4721
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIBJE62[32]:B,3672
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIBJE62[32]:C,3695
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIBJE62[32]:Y,3672
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:D,3263
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[21]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[21]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[21]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[21]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:CLK,5752
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:Q,5752
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[13]:A,5978
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[13]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[13]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[13]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[13]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:CLK,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:Q,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_6_0:A,2548
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_6_0:B,6980
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_6_0:C,6514
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_6_0:CC,1984
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_6_0:D,4356
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_6_0:P,2548
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_6_0:S,1984
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_6_0:UB,4356
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_2:A,1887
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_2:B,1748
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_2:P,1787
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_2:UB,1748
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_2:A,6217
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_2:B,4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_2:P,4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_2:UB,4722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV7MJ1[9]:A,2829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV7MJ1[9]:B,2901
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV7MJ1[9]:Y,2829
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[5]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[5]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[5]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[5]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[14]:A,4450
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[14]:B,3431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[14]:C,5831
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[14]:D,4382
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[14]:Y,3431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_axb_0_i_0:A,3488
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_axb_0_i_0:B,3436
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_axb_0_i_0:Y,3436
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:D,8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:CLK,1422
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:Q,1422
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:CLK,6941
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:Q,6941
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7_0:A,5521
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7_0:B,6576
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7_0:C,6947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7_0:CC,5501
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7_0:P,5521
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7_0:S,5501
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7_0:UB,6947
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:B,7662
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:C,6724
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:IPB,7662
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:IPC,6724
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVVLU[1]:A,6950
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVVLU[1]:B,6580
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVVLU[1]:C,6496
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVVLU[1]:Y,6496
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:C,6724
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:IPC,6724
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:CLK,6705
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:Q,6705
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[16]:A,5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[16]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[16]:C,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[16]:Y,5079
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:D,6203
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:CLK,6070
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:Q,6070
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:CLK,5771
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:D,4627
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:Q,5771
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:C,6747
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:IPC,6747
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m0_2_03_0_0:A,3372
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m0_2_03_0_0:B,3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m0_2_03_0_0:Y,3324
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:CLK,3871
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:D,8717
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:Q,3871
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[2]:A,7938
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[2]:B,1540
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[2]:C,7836
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[2]:Y,1540
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_15:A,6349
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_15:B,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_15:P,6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_15:UB,6183
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_10:B,3169
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_10:UB,3169
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[24]:A,407
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[24]:B,330
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[24]:C,-210
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[24]:Y,-210
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state_ns_0[1]:A,7984
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state_ns_0[1]:B,7896
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state_ns_0[1]:C,7745
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state_ns_0[1]:D,5637
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state_ns_0[1]:Y,5637
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_4:B,1339
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_4:UB,1339
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[2]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[2]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[2]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[2]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[2]:Y,261
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[8]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[8]:B,7209
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[8]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[8]:CC,7112
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[8]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[8]:P,7209
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[8]:S,7112
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO:A,5515
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO:B,5467
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO:C,3543
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO:D,3543
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO:Y,3543
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIP8GM[3]:A,3778
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIP8GM[3]:B,3471
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIP8GM[3]:C,3656
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIP8GM[3]:Y,3471
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:CLK,3621
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:Q,3621
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[9]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[9]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[9]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[9]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_13:A,4089
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_13:B,6112
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_13:P,4089
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_13:UB,6112
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_15:B,2311
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_15:C,1927
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_15:CC,1100
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_15:S,1100
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_15:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:CLK,7090
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:Q,7090
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:CLK,6122
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:Q,6122
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[10]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[10]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[10]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[10]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[10]:Y,261
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61_0[2]:A,5439
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61_0[2]:B,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61_0[2]:C,5589
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61_0[2]:Y,4796
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:CLK,6684
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:D,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:Q,6684
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:CLK,1818
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:D,8674
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:Q,1818
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_26:B,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_26:C,4380
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_26:IPB,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_26:IPC,4380
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_2:A,5320
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_2:B,5235
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_2:CC,5494
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_2:P,5271
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_2:S,5494
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_2:UB,5235
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:CLK,5075
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:Q,5075
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:CLK,6990
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:Q,6990
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[2]:A,4185
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[2]:B,4096
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[2]:C,3900
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[2]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[2]:Y,3900
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[16]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[16]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[16]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[16]:Y,6423
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:CLK,3585
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:D,7000
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:EN,7854
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:Q,3585
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[2]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[2]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[2]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:CLK,5210
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:Q,5210
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_wmux_0:A,3277
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_wmux_0:B,4140
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_wmux_0:C,4316
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_wmux_0:CC,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_wmux_0:D,4192
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_wmux_0:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_wmux_0:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_wmux_0:Y,3277
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:D,6703
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_33:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_33:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:C,6734
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:IPC,6734
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:CLK,4520
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:Q,4520
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:D,3393
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:B,7926
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:C,6738
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:IPB,7926
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:IPC,6738
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_21:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_21:B,7154
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_21:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_21:CC,6835
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_21:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_21:P,7154
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_21:S,6835
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_21:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0[17]:A,2720
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0[17]:B,2677
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0[17]:C,5065
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0[17]:D,3741
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0[17]:Y,2677
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_15:B,6432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_15:C,5454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_15:IPB,6432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_15:IPC,5454
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:CLK,4798
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:D,7061
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:Q,4798
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:CLK,4652
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:D,7958
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:Q,4652
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:CLK,5199
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:Q,5199
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[5]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg_1_sqmuxa_i:A,7864
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg_1_sqmuxa_i:B,7765
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg_1_sqmuxa_i:C,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg_1_sqmuxa_i:Y,7557
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:CLK,6745
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:D,6842
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:Q,6745
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_12:A,7070
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_12:B,6922
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_12:CC,6837
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_12:P,6922
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_12:S,6837
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_7:A,5214
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_7:B,5103
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_7:CC,5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_7:P,5157
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_7:S,5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_7:UB,5103
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:CLK,3169
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:Q,3169
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[10]:A,5597
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[10]:B,2948
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[10]:C,3315
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[10]:D,3185
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[10]:Y,2948
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_31:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_31:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[22]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[22]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[22]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[0]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[0]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[0]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:B,7933
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:C,6738
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:IPB,7933
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:IPC,6738
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0:A,3436
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0:B,4183
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0:P,3436
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0:UB,4183
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_3_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_3_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_3_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_3_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_3_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:D,5357
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:D,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_10:A,6038
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_10:B,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_10:CC,5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_10:S,5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_10:UB,5114
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_11:B,3169
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_11:UB,3169
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_31:B,6401
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_31:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_31:D,6364
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_31:IPB,6401
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_31:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_31:IPD,6364
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:B,7718
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:C,6771
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:IPB,7718
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:IPC,6771
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[3]:A,6241
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[3]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[3]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[3]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[3]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_RNO:A,4181
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_RNO:Y,4181
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:CLK,6220
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:D,8671
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:Q,6220
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[1]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[1]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[1]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[1]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_30:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_30:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:CLK,2883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:D,8671
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:Q,2883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[9]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_falling:A,7804
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_falling:B,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_falling:Y,7733
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[19]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[19]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[19]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[19]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[19]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[17]:A,5531
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[17]:B,5828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[17]:C,4431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[17]:D,5269
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[17]:Y,4431
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_58:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_58:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_58:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_58:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO:A,5622
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO:B,5574
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO:C,3717
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO:D,3637
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO:Y,3637
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_11:B,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_11:CC,7004
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_11:S,7004
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_11:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]_CC_0:UB[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_220:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_220:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_220:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_220:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_220:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[8]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[8]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[8]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:CLK,4170
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:D,8676
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:Q,4170
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_16:A,5796
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_16:B,5442
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_16:CC,5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_16:S,5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_16:UB,5442
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIE76N6[13]:A,6991
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIE76N6[13]:B,1411
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIE76N6[13]:C,1485
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIE76N6[13]:CC,1356
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIE76N6[13]:D,5983
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIE76N6[13]:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIE76N6[13]:S,1356
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIE76N6[13]:UB,1411
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:CLK,1519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:D,8684
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:Q,1519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[37]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[37]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[37]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[37]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[37]:Y,88
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:CLK,7916
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:Q,7916
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/mas_done_o_Z:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[1]:A,4918
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[1]:B,4866
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[1]:C,4775
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[1]:D,4669
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[1]:Y,4669
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:CLK,6129
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:Q,6129
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:CLK,6037
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:D,8673
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:Q,6037
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_0:A,5350
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_0:B,5299
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_0:C,3428
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_0:D,3348
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_0:Y,3348
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_2:A,5694
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_2:B,5292
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_2:CC,6139
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_2:P,5324
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_2:S,6059
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_2:UB,5292
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3PI33[11]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3PI33[11]:B,7473
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3PI33[11]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3PI33[11]:CC,7022
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3PI33[11]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3PI33[11]:P,7473
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3PI33[11]:S,7022
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3PI33[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_10:B,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_10:UB,4242
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:C,6791
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:IPC,6791
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_229:A,6132
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_229:B,4657
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_229:C,6010
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_229:Y,4657
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_8:A,7200
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_8:B,7090
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_8:CC,6914
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_8:P,7158
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_8:S,6914
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_8:UB,7090
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[8]:A,6357
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[8]:B,6273
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[8]:C,5598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[8]:Y,5598
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[8]:A,1712
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[8]:B,4414
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[8]:C,2893
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[8]:Y,1712
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:CLK,7815
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:Q,7815
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_6:B,6829
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_6:C,6889
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_6:CC,6804
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_6:P,6829
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_6:S,6804
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:C,6818
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[0]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[0]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[0]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[0]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:CLK,4823
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:D,7127
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:Q,4823
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:CLK,8854
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:D,6720
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:EN,7874
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:Q,8854
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mas_en:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:CLK,3937
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:Q,3937
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI432L9[26]:A,2044
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI432L9[26]:B,1591
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI432L9[26]:C,207
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI432L9[26]:D,1933
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI432L9[26]:Y,207
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI0SHT[29]:A,4032
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI0SHT[29]:B,3717
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI0SHT[29]:C,3910
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI0SHT[29]:Y,3717
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:CLK,6762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:Q,6762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:C,6709
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:IPC,6709
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_236:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_236:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_236:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_236:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_236:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[2]:A,7808
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[2]:B,5767
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[2]:C,4836
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[2]:CC,4792
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[2]:D,6610
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[2]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[2]:S,4792
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[2]:UB,4836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[9]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[9]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[9]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:C,6733
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:IPC,6733
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_10:A,2759
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_10:B,2741
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_10:C,2583
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_10:D,2421
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_10:Y,2421
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[0],787
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[10],394
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[11],268
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[1],631
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[2],695
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[3],708
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[4],-277
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[5],-393
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[6],-331
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[7],6
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[8],525
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CC[9],518
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CI,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:CO,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[0],-199
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[1],-193
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[2],87
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[3],-7
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[6],86
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[7],111
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[8],193
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:P[9],192
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[0],-323
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[10],106
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[11],212
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[1],-308
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[2],-157
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[3],-177
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[4],-140
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[5],-28
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[6],-23
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[7],31
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[8],121
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_1:UB[9],88
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIHSC6H[5]:A,6390
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIHSC6H[5]:B,1356
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIHSC6H[5]:C,1431
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIHSC6H[5]:CC,1333
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIHSC6H[5]:D,5928
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIHSC6H[5]:P,1519
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIHSC6H[5]:S,1333
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIHSC6H[5]:UB,1356
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:D,8728
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[31]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[31]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[31]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[31]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[31]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:CLK,4354
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:D,6742
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:Q,4354
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_2:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_2:C,4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_2:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_2:IPC,4251
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:CLK,5851
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:Q,5851
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:CLK,7152
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:D,6862
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:Q,7152
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:CLK,6709
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:Q,6709
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[4]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[2]:A,5874
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[2]:B,5813
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[2]:C,4624
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[2]:D,4640
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[2]:Y,4624
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:CLK,4883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:D,7069
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:Q,4883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[41]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[41]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[41]:Y,7555
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[12]:A,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[12]:B,7920
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[12]:C,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[12]:Y,7659
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[1]:A,4394
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[1]:C,4272
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[1]:Y,4272
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIITR81[32]:A,5023
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIITR81[32]:B,4866
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIITR81[32]:C,4634
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIITR81[32]:D,4533
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIITR81[32]:Y,4533
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[33]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[33]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[33]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_14:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_14:B,7143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_14:CC,6817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_14:S,6817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_14:UB,7143
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14:A,2324
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14:B,1651
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14:CC,1328
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14:S,1328
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14:UB,1651
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_12:A,7149
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_12:B,7077
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_12:CC,6953
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_12:P,7077
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_12:S,6953
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:CLK,1680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:D,8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:Q,1680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_6:A,7110
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_6:B,7013
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_6:C,6575
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_6:CC,6618
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_6:P,6645
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_6:S,6618
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_6:UB,6575
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:B,7939
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:C,6763
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:IPB,7939
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:IPC,6763
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_5:A,5182
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_5:B,4400
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_5:CC,4299
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_5:S,4299
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_5:UB,4400
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_126:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_126:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_126:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_126:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_126:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[12]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[12]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[12]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[12]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[12]:Y,261
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[7]:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[7]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[7]:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[7]:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[7]:Y,-247
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:CLK,3562
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:Q,3562
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[8]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[18]:A,3820
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[18]:B,5286
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[18]:C,3370
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[18]:D,4179
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[18]:Y,3370
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_31:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_31:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17_FCINST1:CC,4652
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17_FCINST1:CO,4652
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:CLK,6810
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:Q,6810
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:C,6818
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_3:A,7108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_3:B,6907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_3:CC,7123
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_3:P,7036
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_3:S,7123
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_3:UB,6907
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:CLK,7246
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:Q,7246
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[9]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_39:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_39:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_39:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_39:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_39:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8:B,2843
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8:CC,2752
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8:P,2843
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8:S,2752
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[9]:A,5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[9]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[9]:C,5702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[9]:Y,5240
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_13:A,5142
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_13:B,4411
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_13:CC,4114
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_13:S,4114
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_13:UB,4411
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[12]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[12]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[12]:C,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[12]:Y,5196
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[41]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[41]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[41]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[41]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[41]:Y,224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[14]:A,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[14]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[14]:C,5696
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[14]:Y,5060
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:CLK,4219
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:Q,4219
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[3]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_3:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_3:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_3:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_3:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_3:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_3:IPC,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m14_0_03_0_1:A,3751
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m14_0_03_0_1:B,3667
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m14_0_03_0_1:C,3355
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m14_0_03_0_1:D,3268
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m14_0_03_0_1:Y,3268
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:CC[0],6781
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:CC[1],6703
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:CC[2],6645
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:CC[3],6735
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:CC[4],6664
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:CC[5],6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:CC[6],6732
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:CI,6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[0],7077
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[1],7161
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[2],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[3],7332
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[6],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[7],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[8],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:P[9],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_2:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__N_447_i:A,7990
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__N_447_i:B,7870
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__N_447_i:C,7796
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__N_447_i:Y,7796
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:CLK,6434
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:Q,6434
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_4:B,6105
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_4:UB,6105
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_163:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_163:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_163:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_163:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_163:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO:A,5457
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO:B,5409
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO:C,3526
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO:D,3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO:Y,3324
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[6]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[6]:B,5176
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[6]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[6]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[6]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[6]:A,6277
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[6]:B,6193
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[6]:C,5493
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[6]:Y,5493
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_22:EN,9019
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_22:IPENn,9019
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:D,8867
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:Q,8867
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:CLK,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:Q,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[5]:SLn,
A0_ADC_SDO_O_obuf/U0/U_IOOUTFF:A,4354
A0_ADC_SDO_O_obuf/U0/U_IOOUTFF:Y,4354
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_9:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_9:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_9:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_9:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_9:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_9:IPC,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:CLK,6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:Q,6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:CLK,3483
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:D,6439
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:Q,3483
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o_1_sqmuxa_0_a2:A,5350
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o_1_sqmuxa_0_a2:B,5422
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o_1_sqmuxa_0_a2:C,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o_1_sqmuxa_0_a2:D,4933
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o_1_sqmuxa_0_a2:Y,2990
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_6:A,6942
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_6:B,6774
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_6:CC,7057
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_6:P,6876
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_6:S,7057
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_6:UB,6774
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:CC[0],6618
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:CC[1],6548
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:CC[2],6502
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:CC[3],6566
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:CC[4],6502
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:CC[5],6453
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:CC[6],6554
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:CI,6453
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[0],6668
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[1],6746
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[3],6917
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[0],6614
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[1],6583
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[2],6712
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[3],6765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[4],6806
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[5],6899
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:CLK,7130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:Q,7130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:D,5390
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:CLK,6844
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:Q,6844
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[21]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[21]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[21]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[21]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_7:A,7130
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_7:B,7000
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_7:CC,6974
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_7:P,7088
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_7:S,6974
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_7:UB,7000
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[0]:A,1673
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[0]:B,2545
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[0]:C,4849
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[0]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[0]:D,4688
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[0]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[0]:Y,1673
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9:B,1722
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9:CC,1663
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9:P,1722
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9:S,1663
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_1:A,3674
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_1:B,4530
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_1:C,3552
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_1:Y,3552
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:C,6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPC,6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPD,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_23_0:A,2947
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_23_0:B,1380
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_23_0:C,1453
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_23_0:CC,268
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_23_0:D,212
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_23_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_23_0:S,268
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_23_0:UB,212
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[11]:A,5507
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[11]:B,5804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[11]:C,4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[11]:D,5245
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[11]:Y,4407
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_30:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_30:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:CLK,7787
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:Q,7787
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[9]:A,7808
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[9]:B,5767
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[9]:C,5065
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[9]:CC,4705
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[9]:D,6841
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[9]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[9]:S,4705
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[9]:UB,5065
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:CLK,1604
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:Q,1604
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[8]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_17:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_17:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_17:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_17:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_17:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[14]:A,3287
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[14]:B,3280
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[14]:C,2279
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[14]:D,2206
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[14]:Y,2206
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_31:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_31:IPENn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_227:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_227:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_227:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_227:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_227:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4:B,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4:S,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[3]:A,1624
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[3]:B,5341
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[3]:Y,1624
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:CLK,287
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:D,7034
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:Q,287
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17_FCINST1:CC,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17_FCINST1:CO,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[31]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[31]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[31]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[31]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[12]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[12]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[12]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[12]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:D,5187
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[13]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_206:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_206:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_206:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_206:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_206:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[1]:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[1]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[1]:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[1]:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[1]:Y,-247
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:CLK,6709
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:Q,6709
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[4]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_26:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_26:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_26:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_26:IPA,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:CLK,6277
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:Q,6277
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[1]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[1]:B,5170
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[1]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[1]:Y,91
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_15:A,3133
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_15:B,4726
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_15:P,3133
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_15:UB,4726
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[5]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[5]:B,7103
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[5]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[5]:CC,7168
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[5]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[5]:P,7103
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[5]:S,7168
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:CLK,3290
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:Q,3290
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[11]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[11]:A,1696
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[11]:B,4396
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[11]:C,2875
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[11]:Y,1696
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:C,6859
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPC,6859
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:CLK,5597
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:D,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:Q,5597
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2:A,7997
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2:B,7913
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2:C,4992
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2:D,5687
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2:Y,4992
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[12]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[12]:B,4494
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[12]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[12]:Y,91
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:D,5257
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[16]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[16]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[16]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_21:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_21:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:CC[6],2538
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:CI,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[0],2656
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[1],2538
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[3],2727
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[0],2606
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[1],2624
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[2],2692
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[3],2711
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[4],2681
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[5],2564
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIQM2U8[6]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIQM2U8[6]:B,3808
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIQM2U8[6]:C,7042
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIQM2U8[6]:CC,3860
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIQM2U8[6]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIQM2U8[6]:P,3808
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIQM2U8[6]:S,3860
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIQM2U8[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:B,7694
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:C,6847
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:D,7727
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPB,7694
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPC,6847
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPD,7727
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:CLK,5999
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:Q,5999
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:C,6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPC,6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_11:IPD,
A0_ADC_SDO_O_obuf/U0/U_IOPAD:D,4354
A0_ADC_SDO_O_obuf/U0/U_IOPAD:E,
A0_ADC_SDO_O_obuf/U0/U_IOPAD:PAD,4354
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_2:A,6915
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_2:B,6843
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_2:CC,7480
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_2:P,6879
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_2:S,7480
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_2:UB,6843
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_o2[8]:A,4069
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_o2[8]:B,5114
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_o2[8]:C,3954
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_o2[8]:Y,3954
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:CLK,5665
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:D,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:Q,5665
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[2]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_262:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_262:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_262:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_262:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_262:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:CLK,7856
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:Q,7856
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[12]:A,3341
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[12]:B,3328
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[12]:C,2350
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[12]:D,2269
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[12]:Y,2269
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[3]:A,2589
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[3]:B,988
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[3]:C,7816
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[3]:D,7689
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[3]:Y,988
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:CLK,2131
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:D,7029
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:Q,2131
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:CLK,2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:D,8673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:Q,2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m21_3:A,4664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m21_3:B,1891
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m21_3:C,4774
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m21_3:Y,1891
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[25]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[25]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[25]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[25]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:CLK,1821
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:D,8679
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:Q,1821
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3_RNO:A,5117
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3_RNO:B,3642
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3_RNO:C,4995
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3_RNO:Y,3642
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16:B,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:CLK,4803
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:Q,4803
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:CLK,7168
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:Q,7168
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:IPENn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_159:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_159:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_159:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_159:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_159:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRAGM[4]:A,3937
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRAGM[4]:B,3627
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRAGM[4]:C,3815
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRAGM[4]:Y,3627
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:CLK,4178
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:Q,4178
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[18]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[18]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[18]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_12:A,1804
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_12:B,1698
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_12:C,1712
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_12:D,1540
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_12:Y,1540
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:CLK,6750
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:D,7447
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:Q,6750
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:D,3206
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:B,7856
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:C,6818
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:IPB,7856
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI97T9[3]:A,3661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI97T9[3]:B,3584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI97T9[3]:C,3150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI97T9[3]:Y,3150
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]:A,2392
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]:B,1673
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]:C,3946
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]:D,3815
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]:Y,1673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:CLK,4394
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:Q,4394
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[13]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[13]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[13]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_1_sqmuxa_i:A,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_1_sqmuxa_i:B,7740
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_1_sqmuxa_i:Y,7414
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_14_107_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_14_107_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_14_107_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_14_107_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNII6NV[33]:A,5687
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNII6NV[33]:B,5884
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNII6NV[33]:C,5565
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNII6NV[33]:Y,5565
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_18:A,7087
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_18:B,6883
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_18:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_18:CC,7048
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_18:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_18:P,7001
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_18:S,7048
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_18:UB,6883
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:CLK,1921
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:D,5931
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:Q,1921
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[13]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:CLK,4970
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:Q,4970
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:CLK,6099
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:D,3501
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:Q,6099
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[1]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_68:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_68:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_68:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_68:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_68:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:CLK,4931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:D,8706
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:Q,4931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:CC[6],2930
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:CI,3044
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[0],3056
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[1],2930
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[3],3133
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[0],4575
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[1],4671
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[2],4797
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[3],4726
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[4],4767
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[5],2937
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:CLK,3922
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:EN,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:Q,3922
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:CLK,1952
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:D,8678
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:Q,1952
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:CLK,1816
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:D,8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:Q,1816
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[20]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[20]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[20]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[20]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:CLK,5074
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:Q,5074
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:D,3704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[4]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_213:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_213:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_213:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_213:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_213:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK[2]:A,3945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK[2]:B,3842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK[2]:C,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK[2]:Y,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_16_0:A,7841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_16_0:B,6912
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_16_0:C,5228
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_16_0:CC,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_16_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_16_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_16_0:S,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_16_0:UB,5228
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:CLK,4549
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:Q,4549
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0:A,6032
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0:B,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0:P,6006
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0:UB,5897
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:CLK,4545
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:Q,4545
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[12]:A,4931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[12]:B,4851
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[12]:C,4432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[12]:Y,4432
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:D,5045
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:CLK,5129
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:D,6801
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:Q,5129
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:CLK,2242
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:Q,2242
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[2]:A,6609
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[2]:B,5939
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[2]:C,7449
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[2]:Y,5939
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:CLK,4283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:Q,4283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:CLK,1459
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:Q,1459
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_12:B,2160
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_12:C,1776
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_12:CC,988
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_12:P,2924
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_12:S,988
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[34]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[34]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[34]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[34]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[34]:Y,224
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:CLK,4995
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:D,6849
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:Q,4995
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[6]:A,4635
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[6]:B,2099
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[6]:C,2055
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[6]:Y,2055
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:CLK,6771
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:Q,6771
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:CLK,2139
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:D,2886
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:Q,2139
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0_RNO:A,5563
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0_RNO:B,2839
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0_RNO:C,1825
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0_RNO:Y,1825
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[43]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_192:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_192:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_192:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_192:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_192:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_192:IPC,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:CLK,6762
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:D,8488
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:Q,6762
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_14:B,2382
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_14:C,1998
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_14:CC,1242
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_14:P,3096
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_14:S,1242
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_9_0:A,5599
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_9_0:B,6549
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_9_0:C,5390
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_9_0:CC,5319
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_9_0:D,6850
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_9_0:P,5476
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_9_0:S,5319
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_9_0:UB,5390
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en_RNO_0:A,7521
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en_RNO_0:B,7571
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en_RNO_0:C,7805
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en_RNO_0:D,7669
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en_RNO_0:Y,7521
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[21]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[21]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[21]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[21]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[21]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_14:B,6286
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_14:UB,6286
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_3:A,5849
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_3:B,5806
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_3:Y,5806
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_6:A,2101
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_6:B,1934
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_6:P,2015
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_6:UB,1934
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:CLK,4087
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:Q,4087
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:ARSHFT17,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:ARSHFT17_AD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:ARSHFT17_AL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:ARSHFT17_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:ARSHFT17_CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:ARSHFT17_EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:ARSHFT17_SD_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:ARSHFT17_SL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[0],4275
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[10],4336
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[11],4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[12],4432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[13],4380
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[14],4374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[15],4400
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[16],4414
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[17],4431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[1],4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[2],4242
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[3],4211
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[4],4227
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[5],4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[6],4290
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[7],4265
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[8],4273
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A[9],4256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_EN[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_EN[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:A_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[0],5401
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[10],5445
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[12],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[13],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[14],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[15],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[16],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[17],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[1],4483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[2],4489
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[3],4474
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[5],5431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[6],4413
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[7],5454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B[9],4451
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_EN[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_EN[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:B_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CARRYIN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[12],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[13],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[14],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[15],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[16],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[17],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[18],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[19],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[20],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[21],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[22],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[23],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[24],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[25],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[26],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[27],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[28],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[29],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[30],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[31],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[32],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[33],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[34],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[35],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[36],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[37],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[38],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[39],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[40],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[41],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[42],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[43],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDIN[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDSEL,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:CDSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[10],6385
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[11],6334
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[12],6339
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[13],6361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[14],6357
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[15],6432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[16],6458
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[17],6449
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[18],6452
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[19],6509
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[20],6506
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[21],6492
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[22],6499
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[23],6496
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[24],6475
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[25],6576
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[26],6562
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[27],6421
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[28],6483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[29],6432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[30],6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[31],6426
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[32],6406
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[33],6369
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[34],6354
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[35],6416
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[36],6401
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[37],6364
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[38],6408
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[39],6374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[40],6389
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[41],6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[42],6446
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[43],6486
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_EN[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_EN[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:C_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:DOTP,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:FDBKSEL,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:FDBKSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:FDBKSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:FDBKSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:FDBKSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:FDBKSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:FDBKSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:FDBKSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:OVFL_CARRYOUT_SEL,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[10],8711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[11],8706
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[12],8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[13],8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[14],8703
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[15],8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[16],8699
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[17],8697
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[18],8673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[19],8668
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[20],8671
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[21],8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[22],8670
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[23],8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[24],8664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[25],8663
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[26],8667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[27],8686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[28],8686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P[9],8712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_CLK[0],8697
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_CLK[1],8663
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_EN[0],6525
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_EN[1],6548
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:P_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SIMD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SUB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SUB_AD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SUB_AL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SUB_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SUB_CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SUB_EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SUB_SD_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP:SUB_SL_N,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:CLK,364
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:D,8682
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:Q,364
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[21]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:CLK,6208
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:Q,6208
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIMFM7B[8]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIMFM7B[8]:B,7167
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIMFM7B[8]:C,2902
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIMFM7B[8]:CC,2972
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIMFM7B[8]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIMFM7B[8]:P,2902
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIMFM7B[8]:S,2972
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIMFM7B[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:CLK,7129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:Q,7129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI6BM15[4]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI6BM15[4]:B,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI6BM15[4]:C,7716
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI6BM15[4]:CC,7001
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI6BM15[4]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI6BM15[4]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI6BM15[4]:S,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI6BM15[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[14]:A,5474
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[14]:B,5771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[14]:C,4374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[14]:D,5212
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[14]:Y,4374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[7]:A,3461
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[7]:B,3307
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[7]:C,3384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[7]:Y,3307
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:CLK,723
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:D,8673
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:Q,723
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[38]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]:A,1841
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]:B,2326
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]:C,4042
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]:D,3910
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]:Y,1841
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_3:B,4561
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_3:C,3642
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_3:CC,3794
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_3:P,3642
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_3:S,3794
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_3:UB,4561
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVUKU[1]:A,6811
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVUKU[1]:B,6445
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVUKU[1]:C,6357
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVUKU[1]:Y,6357
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:CLK,4059
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:D,8677
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:Q,4059
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI9NRS[2]:A,2523
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI9NRS[2]:B,2420
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI9NRS[2]:C,2052
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI9NRS[2]:Y,2052
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_5:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_5:C,4489
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_5:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_5:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_5:IPC,4489
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_5:IPD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:CLK,1187
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:D,1417
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:Q,1187
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:CLK,4252
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:D,7415
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:Q,4252
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_28:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_28:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_s_17:B,7661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_s_17:C,7598
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_s_17:CC,6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_s_17:S,6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:CLK,5682
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:D,3674
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:Q,5682
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:CLK,5285
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:D,8687
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:Q,5285
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[6]:A,5850
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[6]:B,6046
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[6]:C,2870
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[6]:D,2895
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[6]:Y,2870
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:CLK,4402
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:Q,4402
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:CLK,5834
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:D,6692
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:Q,5834
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5:D,6054
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5:UB,6054
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[18]:A,6578
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[18]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[18]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[18]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[18]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11_0[6]:A,3807
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11_0[6]:B,3723
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11_0[6]:C,3411
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11_0[6]:D,3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11_0[6]:Y,3324
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:CLK,6841
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:Q,6841
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:CLK,4146
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:Q,4146
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:CLK,6835
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:Q,6835
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:CLK,5124
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:D,8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:Q,5124
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_1_0:A,5322
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_1_0:B,6357
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_1_0:C,5199
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_1_0:CC,5846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_1_0:D,6658
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_1_0:P,5199
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_1_0:S,5846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_1_0:UB,5217
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[1]:A,4336
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[1]:B,4252
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[1]:C,4074
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[1]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[1]:Y,4074
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_115:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_115:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_115:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_115:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_115:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0:A,6032
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0:B,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0:P,6006
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0:UB,5897
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[19]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[19]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[19]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:CC[0],2192
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:CC[1],2114
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:CC[2],2056
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:CC[3],2146
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:CC[4],2075
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:CC[5],2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:CC[6],2143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:CI,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[0],2369
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[1],2440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[3],2733
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[0],2326
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[1],2267
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[2],2598
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[3],2587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[4],2624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[5],2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14:B,3496
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14:CC,2692
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14:S,2692
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_8_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_8_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_8_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_8_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_8_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:CLK,5254
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:Q,5254
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:CLK,6818
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:Q,6818
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[9]:A,6484
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[9]:B,7181
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[9]:C,6718
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[9]:CC,5666
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[9]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[9]:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[9]:S,5666
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[9]:UB,6718
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[5]:A,6167
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[5]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[5]:Y,6167
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_4:B,6037
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_4:UB,6037
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/un1_s_mas_en_0_sqmuxa_0:A,8004
BLDC_Encoder_Axis_0/MSC_i_27/un1_s_mas_en_0_sqmuxa_0:B,7920
BLDC_Encoder_Axis_0/MSC_i_27/un1_s_mas_en_0_sqmuxa_0:C,7842
BLDC_Encoder_Axis_0/MSC_i_27/un1_s_mas_en_0_sqmuxa_0:D,6720
BLDC_Encoder_Axis_0/MSC_i_27/un1_s_mas_en_0_sqmuxa_0:Y,6720
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[17]:A,2409
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[17]:B,2373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[17]:Y,2373
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:CLK,6303
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:D,8673
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:Q,6303
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_10:B,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_10:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_11:B,6089
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_11:C,6197
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_11:CC,6067
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_11:P,6089
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_11:S,6067
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_11:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:CLK,4519
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:Q,4519
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[7]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_98:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_98:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_98:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_98:IPA,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[16]:A,5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[16]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[16]:C,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[16]:Y,5079
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i_o4[0]:A,4518
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i_o4[0]:B,2764
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i_o4[0]:C,4626
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i_o4[0]:Y,2764
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_22:EN,9019
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_22:IPENn,9019
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:CLK,7784
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:D,8342
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:Q,7784
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[8]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[8]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[8]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[8]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_15:A,6349
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_15:B,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_15:P,6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_15:UB,6183
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_12:A,3522
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_12:B,988
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_12:P,1135
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_12:UB,988
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o_1_sqmuxa_0_a2:A,5499
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o_1_sqmuxa_0_a2:B,5084
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o_1_sqmuxa_0_a2:C,5229
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o_1_sqmuxa_0_a2:D,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o_1_sqmuxa_0_a2:Y,2867
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[8]:A,6198
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[8]:B,6153
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[8]:C,5438
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[8]:Y,5438
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[29]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[29]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[29]:Y,7440
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:CLK,6112
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:Q,6112
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:CLK,6698
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:D,6928
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:Q,6698
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:CLK,3317
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:Q,3317
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[1]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[4]:A,6940
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[4]:B,5824
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[4]:C,7836
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[4]:D,7722
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[4]:Y,5824
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_1[2]:A,3940
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_1[2]:B,3851
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_1[2]:C,1825
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_1[2]:Y,1825
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:CLK,1575
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:Q,1575
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CC[0],5767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CC[1],5689
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CC[2],5631
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CC[3],5721
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CC[4],5650
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CC[5],5589
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CC[6],5710
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CC[7],5588
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:CI,5588
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[0],5775
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[1],5761
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[2],5934
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[3],5919
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[6],6256
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[0],6499
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[1],6562
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[2],6688
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[3],6637
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[4],6675
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[5],6767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[6],6998
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:CLK,7130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:Q,7130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:D,5174
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[16]:A,6111
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[16]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[16]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[16]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[16]:Y,2538
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:CLK,6882
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:Q,6882
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:CLK,2689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:D,1716
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:Q,2689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_7:A,6952
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_7:B,6828
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_7:CC,6987
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_7:P,6916
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_7:S,6987
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_7:UB,6828
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:CLK,7730
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:Q,7730
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[15]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:CLK0,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:CLK0_PAD,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:CLK1,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:CLK1_PAD,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:CLK2,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:CLK2_PAD,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:CLK3,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:CLK3_PAD,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GL0,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GPD0_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GPD1_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GPD2_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:GPD3_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:LOCK,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX0_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX0_HOLD_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX0_SEL,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX1_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX1_HOLD_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX1_SEL,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX2_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX2_HOLD_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX2_SEL,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX3_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX3_HOLD_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:NGMUX3_SEL,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PADDR[2],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PADDR[3],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PADDR[4],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PADDR[5],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PADDR[6],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PADDR[7],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PCLK,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PENABLE,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PLL_ARST_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PLL_BYPASS_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PLL_POWERDOWN_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PRESET_N,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PSEL,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWDATA[0],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWDATA[1],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWDATA[2],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWDATA[3],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWDATA[4],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWDATA[5],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWDATA[6],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWDATA[7],
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:PWRITE,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:RCOSC_1MHZ,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:RCOSC_25_50MHZ,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP:XTLOSC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[22]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[22]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[22]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[22]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:CLK,4494
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:Q,4494
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_15_0:A,3274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_15_0:B,7207
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_15_0:C,6745
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_15_0:CC,1645
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_15_0:D,4587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_15_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_15_0:S,1645
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_15_0:UB,4587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO_0:A,3151
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO_0:B,2184
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO_0:C,5007
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO_0:D,4814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO_0:Y,2184
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[0]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_0_sqmuxa_i_o3:A,7890
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_0_sqmuxa_i_o3:B,7874
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_0_sqmuxa_i_o3:Y,7874
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[3]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[3]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[3]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[26]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[26]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[26]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_1:A,4269
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_1:B,5956
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_1:P,4269
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_1:UB,5956
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]_CC_0:UB[9],
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:CLK,5335
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:Q,5335
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6_RNIJ44P1:A,6329
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6_RNIJ44P1:B,4644
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6_RNIJ44P1:C,4500
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6_RNIJ44P1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6_RNIJ44P1:D,5914
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6_RNIJ44P1:P,4500
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6_RNIJ44P1:UB,5914
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[11]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[11]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[11]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[11]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:CLK,3702
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:D,6926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:Q,3702
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[19]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_17:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_17:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:CLK,6791
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:Q,6791
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:CLK,2629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:Q,2629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_27:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_27:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[14]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[14]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[14]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[14]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[14]:Y,261
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_27:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_27:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_s_17:A,7841
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_s_17:B,5254
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_s_17:C,6101
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_s_17:CC,5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_s_17:D,7038
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_s_17:S,5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_s_17:UB,
A0_PWM_WH_O_obuf/U0/U_IOENFF:A,
A0_PWM_WH_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_9:A,1218
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_9:B,1397
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_9:P,1218
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_9:UB,1397
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_axb_0_i_0:A,6630
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_axb_0_i_0:B,6897
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_axb_0_i_0:Y,6630
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_13:A,3089
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_13:B,2997
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_13:P,2997
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_13:UB,3015
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:CLK,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:Q,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[7]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[17]:A,3385
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[17]:B,2615
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[17]:C,2834
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[17]:D,2525
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[17]:Y,2525
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16:B,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16:S,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:CLK,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:Q,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[41]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[41]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[41]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:CLK,6029
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:D,8675
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:Q,6029
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:CLK,7220
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:Q,7220
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMUVR8[26]:A,2596
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMUVR8[26]:B,1597
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMUVR8[26]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMUVR8[26]:CC,1591
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMUVR8[26]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMUVR8[26]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMUVR8[26]:S,1591
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMUVR8[26]:UB,1597
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[4]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[4]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[4]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[5]:A,1431
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[5]:B,5159
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[5]:Y,1431
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:CLK,6183
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:Q,6183
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:CLK,3682
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:D,2525
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:Q,3682
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[3]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[3]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[3]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[3]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_22:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_22:B,7786
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_22:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_22:CC,6753
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_22:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_22:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_22:S,6753
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_22:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i[7]:A,8010
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i[7]:B,3954
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i[7]:C,3847
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i[7]:D,2373
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i[7]:Y,2373
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNID48V1[8]:A,4130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNID48V1[8]:B,3113
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNID48V1[8]:C,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNID48V1[8]:Y,3068
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:CLK,7718
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:Q,7718
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[6]:A,5184
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[6]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[6]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[6]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[6]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:CLK,6969
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:Q,6969
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:D,3501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:D,6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:CLK,4368
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:D,4792
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:Q,4368
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:B,7718
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:C,6771
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:IPB,7718
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:IPC,6771
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:CLK,7718
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:Q,7718
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:C,6733
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:IPC,6733
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:CLK,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:Q,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIJPJKI[43]:A,2205
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIJPJKI[43]:B,1093
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIJPJKI[43]:C,1792
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIJPJKI[43]:Y,1093
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:CLK,2053
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:D,2491
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:Q,2053
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[40]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[40]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[40]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[40]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[40]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_2:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_2:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_2:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_2:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[16]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[16]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[16]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[14]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[14]:B,4358
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[14]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[14]:Y,91
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[17]:A,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[17]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[17]:C,5685
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[17]:Y,5018
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[17]:A,6010
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[17]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[17]:Y,6010
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_33:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_33:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:CLK,3050
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:D,2297
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:Q,3050
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[14]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[14]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[14]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:CLK,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:D,6967
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:Q,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]:A,2302
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]:B,1795
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]:C,4055
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]:D,3937
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]:Y,1795
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI1QNK[0]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI1QNK[0]:B,6925
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI1QNK[0]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI1QNK[0]:CC,7448
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI1QNK[0]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI1QNK[0]:P,6925
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI1QNK[0]:S,7448
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI1QNK[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:CLK,1927
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:D,8676
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:Q,1927
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:D,1226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[28]:A,294
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[28]:B,217
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[28]:C,-323
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[28]:Y,-323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[2]:A,3686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[2]:B,5061
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[2]:C,2624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[2]:D,3396
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[2]:Y,2624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:CC[0],6953
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:CC[1],6875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:CC[2],6817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:CC[3],6907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:CC[4],6836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:CC[5],6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:CI,6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[0],7077
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[1],6992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[2],7143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[3],7395
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[4],7540
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]:A,2579
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]:B,2072
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]:C,4332
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]:D,4214
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]:Y,2072
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:CLK,6117
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:D,8668
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:Q,6117
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:D,3336
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_12:A,5208
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_12:B,5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_12:CC,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_12:P,5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_12:S,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_0:A,5474
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_0:B,5436
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_0:C,3408
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_0:D,3463
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO_0:Y,3408
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:B,7856
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:C,6818
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:IPB,7856
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_6:A,1408
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_6:B,3044
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_6:P,1408
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_6:UB,3044
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:CLK,4804
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:Q,4804
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1[1]:A,7009
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1[1]:B,7000
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1[1]:C,5416
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1[1]:D,5608
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1[1]:Y,5416
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_7:A,7180
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_7:B,7103
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_7:C,6681
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_7:CC,6557
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_7:P,6715
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_7:S,6557
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_7:UB,6681
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:CLK,2366
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:D,6010
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:Q,2366
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10_RNIL2RG1:A,951
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10_RNIL2RG1:B,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10_RNIL2RG1:C,1775
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10_RNIL2RG1:D,698
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_10_RNIL2RG1:Y,-247
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:CLK,1461
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:D,1407
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:Q,1461
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[21]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[21]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[21]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[11]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[11]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[11]:Y,7555
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:CLK,1616
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:Q,1616
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:CLK,4003
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:Q,4003
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_230:A,6008
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_230:B,4523
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_230:C,5886
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_230:Y,4523
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:CLK,1471
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:D,8717
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:Q,1471
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:D,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]:A,2722
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]:B,2003
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]:C,4269
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]:D,4145
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]:Y,2003
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:B,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:C,6841
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:D,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPC,6841
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_5_0:A,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_5_0:B,6926
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_5_0:C,6456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_5_0:CC,2385
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_5_0:D,4298
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_5_0:P,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_5_0:S,2315
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_5_0:UB,4298
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_9:A,7808
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_9:B,7088
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_9:C,6642
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_9:CC,6570
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_9:P,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_9:S,6570
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_9:UB,6642
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[11]:A,5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[11]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[11]:C,5742
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[11]:Y,5095
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:CLK,7049
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:Q,7049
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:C,6795
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:IPC,6795
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:CLK,4158
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:Q,4158
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:CLK,6763
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:D,3661
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:Q,6763
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[9]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[9]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[9]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[9]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_3:A,6161
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_3:B,6029
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_3:P,6115
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_3:UB,6029
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_148:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_148:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_148:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_148:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_148:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[11]:A,5761
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[11]:B,6992
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[11]:C,6562
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[11]:CC,5689
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[11]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[11]:P,5761
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[11]:S,5689
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[11]:UB,6562
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]:A,1684
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]:B,2194
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]:C,3889
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]:D,3765
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]:Y,1684
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_160:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_160:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_160:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_160:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_160:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[15]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[15]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[15]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[15]:CC,7015
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[15]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[15]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[15]:S,7015
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[15]:UB,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:CLK,6370
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:Q,6370
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:CLK,1898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:D,8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:Q,1898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:CLK,6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:Q,6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:CLK,7884
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:Q,7884
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[17]:A,3142
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[17]:B,3129
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[17]:C,2144
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[17]:D,2070
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[17]:Y,2070
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_3:A,7029
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_3:B,6787
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_3:CC,7002
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_3:P,6916
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_3:S,7002
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_3:UB,6787
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[15]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[15]:B,7661
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[15]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[15]:CC,6857
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[15]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[15]:P,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[15]:S,6857
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[15]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]:A,1902
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]:B,2412
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]:C,4100
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]:D,3983
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]:Y,1902
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_11:A,7848
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_11:B,7205
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_11:CC,6850
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_11:S,6850
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_11:UB,7205
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[0]:A,1697
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[0]:B,2569
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[0]:C,4866
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[0]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[0]:D,4712
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[0]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[0]:Y,1697
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[0],7105
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[10],6878
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[11],6817
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[1],7027
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[2],6969
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[3],7059
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[4],6988
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[5],6927
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[6],7048
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[7],6926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[8],6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CC[9],6962
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CI,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:CO,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[0],6915
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[1],6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[2],6995
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[3],7023
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[6],7001
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[7],7014
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[8],7096
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:P[9],7099
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[10],7008
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[11],7129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[4],6900
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[5],6992
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[6],6883
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[7],6941
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[8],7049
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_1:UB[9],6990
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_16:B,3100
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_16:UB,3100
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:D,5545
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[1]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[1]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[1]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[25]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[25]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[25]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[10],5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[11],5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[1],6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[2],6139
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[3],5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[4],5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[5],5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[6],5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[7],5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[8],5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CC[9],5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:CO,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[0],5599
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[1],5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[2],5324
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[3],5239
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[6],5181
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[7],5157
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[8],5315
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:P[9],5232
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[0],5472
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[10],5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[11],5308
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[1],5512
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[2],5292
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[3],5141
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[4],5118
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[5],5262
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[6],5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[7],5103
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[8],5282
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_0:UB[9],5144
GPIO_0_M2F_obuf/U0/U_IOOUTFF:A,
GPIO_0_M2F_obuf/U0/U_IOOUTFF:Y,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:CC[0],1407
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:CC[1],1333
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:CC[2],1275
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:CC[3],1355
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:CC[4],1291
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:CC[5],1233
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:CC[6],1343
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:CI,1233
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[0],1441
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[1],1519
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[3],1690
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[0],1403
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[1],1356
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[2],1501
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[3],1554
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[4],1591
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[5],1688
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:CLK,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:D,8684
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:Q,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:D,6710
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1_RNIQUH71:A,6104
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1_RNIQUH71:B,6038
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1_RNIQUH71:C,5732
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1_RNIQUH71:Y,5732
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_4:B,2202
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_4:C,2014
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_4:CC,1381
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_4:S,1381
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIMBIB3[0]:A,7377
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIMBIB3[0]:B,6276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIMBIB3[0]:C,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIMBIB3[0]:Y,4796
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[8]:A,6175
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[8]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[8]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[8]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[8]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI22LU[1]:A,6903
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI22LU[1]:B,6535
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI22LU[1]:C,6449
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI22LU[1]:Y,6449
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:CLK,3425
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:D,8667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:Q,3425
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:D,5045
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_4:B,4823
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_4:UB,4823
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[25]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[25]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[25]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[25]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[25]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv[17]:A,1384
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv[17]:B,3645
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv[17]:C,1226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv[17]:Y,1226
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_11:B,4825
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_11:UB,4825
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:D,6732
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:D,5478
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:CLK,6220
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:D,8671
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:Q,6220
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_s_17:B,3675
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_s_17:C,7703
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_s_17:CC,2723
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_s_17:D,5320
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_s_17:S,2723
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_s_17:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o_1_sqmuxa_0_a2:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o_1_sqmuxa_0_a2:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o_1_sqmuxa_0_a2:C,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o_1_sqmuxa_0_a2:D,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o_1_sqmuxa_0_a2:Y,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:CLK,6274
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:Q,6274
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_5:B,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_5:S,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGVEHC[33]:A,2391
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGVEHC[33]:B,1898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGVEHC[33]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGVEHC[33]:CC,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGVEHC[33]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGVEHC[33]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGVEHC[33]:S,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGVEHC[33]:UB,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[12]:A,2269
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[12]:B,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[12]:C,5495
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[12]:Y,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17_RNO:A,6744
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17_RNO:B,6770
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17_RNO:Y,6744
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17:B,2937
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17:UB,2937
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17:S,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[5]:A,5546
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[5]:B,2897
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[5]:C,3264
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[5]:D,3134
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[5]:Y,2897
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[5]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[5]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[5]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[5]:CC,7077
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[5]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[5]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[5]:S,7077
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:CLK,2938
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:D,2175
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:Q,2938
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:CLK,5777
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:D,6949
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:Q,5777
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:CLK,6082
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:D,8847
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:Q,6082
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly1:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:D,7524
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_1:A,2928
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_1:B,2836
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_1:P,2836
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_1:UB,2859
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_214:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_214:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_214:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_214:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_214:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[0],1598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[10],2205
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[1],1477
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[2],1307
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[3],1354
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[4],2266
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[5],1422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[6],1471
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[7],1311
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[8],1294
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CC[9],1347
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:CI,1294
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[0],1818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[1],1768
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[2],1941
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[3],1926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[6],1947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[7],2353
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[0],1680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[1],1768
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[2],1899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[3],1817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[4],1855
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[5],1947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[6],1846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[7],1899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[8],1989
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_2:UB[9],3136
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:CLK,2514
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:D,8674
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:Q,2514
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0:B,2610
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0:P,2610
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[16]:A,1233
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[16]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[16]:Y,1233
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[12]:A,5752
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[12]:B,5949
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[12]:C,2773
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[12]:D,2798
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[12]:Y,2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:CLK,4145
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:Q,4145
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV5O43[14]:A,2836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV5O43[14]:B,2603
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV5O43[14]:C,2759
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV5O43[14]:Y,2603
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:CLK,4108
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:D,5284
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:Q,4108
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha_0_sqmuxa_0_a3:A,7669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha_0_sqmuxa_0_a3:B,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha_0_sqmuxa_0_a3:Y,7578
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:C,6747
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:IPC,6747
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:CLK,4508
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:Q,4508
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[27]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[27]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[27]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_32_0:A,2992
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_32_0:B,1927
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_32_0:C,2002
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_32_0:CC,185
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_32_0:D,715
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_32_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_32_0:S,185
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_32_0:UB,715
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:CLK,217
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:D,6965
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:Q,217
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:CLK,3646
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:D,6962
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:Q,3646
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[21]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:CLK,7171
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:Q,7171
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_1:A,5096
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_1:B,5019
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_1:C,3277
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_1:D,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_1:Y,3068
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:CLK,6762
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:D,6793
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:Q,6762
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5L4O[2]:A,3989
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5L4O[2]:B,3912
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5L4O[2]:C,3461
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5L4O[2]:Y,3461
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:CLK,5053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:D,8671
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:Q,5053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:CLK,4086
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:Q,4086
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_11_0:A,7149
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_11_0:B,6666
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_11_0:C,2870
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_11_0:CC,2787
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_11_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_11_0:P,2920
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_11_0:S,2787
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_11_0:UB,2870
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:C,6833
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPC,6833
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_9:A,3205
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_9:B,3030
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_9:P,3113
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_9:UB,3030
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITPIT[32]:A,4061
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITPIT[32]:B,3904
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITPIT[32]:C,3672
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITPIT[32]:Y,3672
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10_0:A,6219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10_0:B,7274
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10_0:C,7014
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10_0:CC,5453
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10_0:S,5453
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10_0:UB,7014
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0:A,6920
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0:B,6659
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0:P,6811
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0:UB,6659
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0:Y,7794
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:D,7018
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_12:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_12:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:D,8697
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_9:B,6798
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_9:C,6873
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_9:CC,6027
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_9:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_9:S,6027
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12:A,6950
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12:B,3579
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12:C,3456
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12:CC,3501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12:P,3577
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12:S,3501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12:UB,3456
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_14:B,3141
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_14:UB,3141
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_23:A,598
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_23:B,450
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_23:C,344
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_23:D,395
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_23:Y,344
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_1:A,5176
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_1:B,5089
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_1:CC,5472
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_1:P,5097
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_1:S,5472
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_1:UB,5089
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:CLK,6016
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:Q,6016
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_14_0:A,1787
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_14_0:B,1011
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_14_0:C,1423
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_14_0:CC,695
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_14_0:D,-157
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_14_0:P,87
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_14_0:S,695
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_14_0:UB,-157
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_11:B,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_11:CC,5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_11:S,5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_11:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_167:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_167:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_167:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_167:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:CLK,6023
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:Q,6023
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_0:A,1294
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_0:B,1347
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_0:C,166
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_0:D,783
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_0:Y,166
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__un1_s_ia_0_sqmuxa_0_0:A,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__un1_s_ia_0_sqmuxa_0_0:B,6588
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__un1_s_ia_0_sqmuxa_0_0:Y,6398
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:CLK,4948
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:Q,4948
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_183:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_183:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_183:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_183:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_183:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:CLK,1411
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:D,8716
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:Q,1411
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:D,6645
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:CLK,4930
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:D,7077
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:Q,4930
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[17]:A,2501
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[17]:B,3373
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[17]:C,5670
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[17]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[17]:D,5516
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[17]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[17]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[17]:Y,2501
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_12:A,6315
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_12:B,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_12:P,4273
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_12:UB,4108
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:CLK,7884
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:Q,7884
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[3]:A,7827
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[3]:B,7493
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[3]:C,5967
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[3]:D,4964
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[3]:Y,4964
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:D,8668
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11:A,7808
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11:B,7211
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11:CC,6857
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11:S,6857
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11:UB,7211
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:C,6709
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:IPC,6709
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:CLK,3668
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:D,1540
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:Q,3668
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5:B,3387
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5:CC,2712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5:S,2712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:CLK,4370
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:D,6790
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:Q,4370
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNO[13]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNO[13]:B,7786
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNO[13]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNO[13]:CC,6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNO[13]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNO[13]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNO[13]:S,6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNO[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:CLK,4553
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:D,8691
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:Q,4553
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14:A,7808
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14:B,5211
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14:CC,5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14:S,5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14:UB,5211
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7:A,1576
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7:B,1459
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7:CC,1273
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7:P,1527
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7:S,1273
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7:UB,1459
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:D,3245
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0:A,7143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0:B,6573
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0:C,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0:CC,1945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0:P,1968
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0:S,1945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0:UB,1898
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[42]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[42]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[42]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:B,7869
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:C,6705
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:IPB,7869
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:IPC,6705
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_26:A,7237
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_26:B,7130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_26:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_26:CC,6784
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_26:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_26:P,7181
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_26:S,6784
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_26:UB,7130
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[17]:A,1343
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[17]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[17]:Y,1343
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:CLK,4369
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:Q,4369
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3UGT[26]:A,3900
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3UGT[26]:B,3580
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3UGT[26]:C,3773
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3UGT[26]:Y,3580
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:CLK,1817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:D,8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:Q,1817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:B,7806
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:C,6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:D,7809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPB,7806
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPD,7809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:CLK,1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:D,8681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:Q,1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:CLK,4284
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:Q,4284
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]:B,6846
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]:C,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]:CC,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]:P,6846
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_18:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_18:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:CLK,6724
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:Q,6724
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_11:B,6385
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_11:C,5431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_11:D,6334
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_11:IPB,6385
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_11:IPC,5431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_11:IPD,6334
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[2]:A,3059
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[2]:B,4452
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[2]:C,1668
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[2]:D,1762
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[2]:Y,1668
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[12]:A,4786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[12]:B,2346
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[12]:C,2265
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[12]:D,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[12]:Y,2119
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_14:A,1367
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_14:B,3291
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_14:P,1367
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_14:UB,3291
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[7]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[7]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[7]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_10:B,2289
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_10:C,1905
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_10:CC,1122
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_10:S,1122
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_10:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[7]:A,7964
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[7]:B,7893
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[7]:Y,7893
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_28:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_28:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_28:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_28:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_28:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o_1_sqmuxa_0_a2:A,5477
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o_1_sqmuxa_0_a2:B,5105
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o_1_sqmuxa_0_a2:C,5188
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o_1_sqmuxa_0_a2:D,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o_1_sqmuxa_0_a2:Y,2867
ip_interface_inst:A,
ip_interface_inst:B,
ip_interface_inst:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_28:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_28:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[16]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[16]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[16]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[16]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_4:B,1381
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_4:UB,1381
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:CLK,7876
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:D,8854
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:EN,7832
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:Q,7876
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_enable:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:CLK,3247
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:Q,3247
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_29:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_29:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o_1_sqmuxa_0_a2:A,5477
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o_1_sqmuxa_0_a2:B,5871
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o_1_sqmuxa_0_a2:C,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o_1_sqmuxa_0_a2:D,5008
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o_1_sqmuxa_0_a2:Y,3090
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_124:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_124:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_124:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_124:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_124:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:CLK,6183
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:Q,6183
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:CLK,5972
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:D,5824
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:EN,7664
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:Q,5972
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:CLK,1732
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:D,8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:Q,1732
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[30]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_282:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_282:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_282:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_282:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_282:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6:A,2912
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6:B,2710
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6:CC,2722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6:P,2800
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6:S,2722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6:UB,2710
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:CLK,6833
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:Q,6833
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[3]:A,4143
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[3]:B,1607
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[3]:C,1563
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[3]:Y,1563
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_9:B,4704
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_9:C,3760
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_9:CC,3705
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_9:P,3760
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_9:S,3705
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_9:UB,4704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:CLK,4907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:Q,4907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:CLK,4835
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:D,4608
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:Q,4835
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_s_34:A,4577
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_s_34:B,4156
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_s_34:C,3964
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_s_34:CC,1775
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_s_34:D,2771
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_s_34:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_s_34:S,1775
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_s_34:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:CLK,4995
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:Q,4995
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:IPENn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_250:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_250:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_250:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_250:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_250:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:D,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2:B,1575
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2:CC,1887
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2:P,1575
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2:S,1887
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[6]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[21]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[21]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[21]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[21]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[21]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_14/s_state_ns_0[0]:A,7951
BLDC_Encoder_Axis_0/MSC_i_14/s_state_ns_0[0]:B,7916
BLDC_Encoder_Axis_0/MSC_i_14/s_state_ns_0[0]:C,7711
BLDC_Encoder_Axis_0/MSC_i_14/s_state_ns_0[0]:D,7749
BLDC_Encoder_Axis_0/MSC_i_14/s_state_ns_0[0]:Y,7711
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_14:B,6286
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_14:UB,6286
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[16]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[16]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[16]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[16]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_13:A,7848
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_13:B,7028
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_13:CC,6888
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_13:S,6888
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_13:UB,7028
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:CLK,4560
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:Q,4560
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[10]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[10]:B,7661
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[10]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[10]:CC,6873
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[10]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[10]:P,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[10]:S,6873
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_0_0_0[7]:A,3650
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_0_0_0[7]:B,5766
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_0_0_0[7]:Y,3650
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:CLK,6762
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:D,5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:Q,6762
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:CLK,4767
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:D,8729
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:Q,4767
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[35]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[35]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[35]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[35]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[35]:Y,88
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:CLK,6835
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:Q,6835
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:CLK,5233
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:Q,5233
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:CLK,6754
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:Q,6754
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[8]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:CLK,5082
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:Q,5082
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[8]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[8]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[8]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[8]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12:B,1826
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12:CC,1573
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12:P,1826
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12:S,1573
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_8:A,3496
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_8:B,5168
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_8:P,3496
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_8:UB,5168
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[1]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[1]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[1]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[6]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[6]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[6]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[6]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_3_228_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_3_228_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_3_228_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_3_228_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_8:A,5427
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_8:B,5310
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_8:CC,5103
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_8:P,5378
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_8:S,5103
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_8:UB,5310
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CC[0],4786
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CC[1],4708
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CC[2],4650
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CC[3],4740
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CC[4],4669
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CC[5],4608
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CC[6],4737
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CC[7],4627
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:CI,4608
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[0],4956
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[1],4942
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[2],5118
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[3],5100
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[6],5437
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[0],4846
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[1],4909
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[2],5035
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[3],4984
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[4],5022
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[5],5114
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[6],5345
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_2_sqmuxa_i:A,5895
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_2_sqmuxa_i:B,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_2_sqmuxa_i:C,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_2_sqmuxa_i:Y,4108
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:D,6502
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[13]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:CLK,2186
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:D,6167
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:Q,2186
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[5]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[5]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[5]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:C,6711
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:IPC,6711
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[17]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:CLK,5956
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:D,8704
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:Q,5956
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[14]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[14]:B,4949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[14]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[14]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[14]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_4:B,4596
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_4:UB,4596
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[0]:A,4131
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[0]:B,1741
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[0]:C,4012
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[0]:Y,1741
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[6]:A,3823
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[6]:B,2725
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[6]:C,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[6]:D,3755
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[6]:Y,2725
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[15]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[15]:B,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[15]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:CLK,4891
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:D,7467
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:Q,4891
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO:A,5703
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO:B,5655
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO:C,3798
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO:D,3557
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO:Y,3557
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:CLK,2323
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:Q,2323
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_31:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_31:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[6]:A,4453
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[6]:B,4365
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[6]:C,4169
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[6]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[6]:Y,4169
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:CLK,1905
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:D,6982
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:Q,1905
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:CLK,4254
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:Q,4254
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:CLK,2779
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:D,1684
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:Q,2779
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_7:A,2111
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_7:B,1992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_7:P,2055
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_7:UB,1992
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[4]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[4]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[4]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[13]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[13]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[13]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[13]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_11:B,5064
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_11:UB,5064
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[13]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[13]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[13]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[13]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[17]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[17]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[17]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[17]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[17]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[16]:A,5514
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[16]:B,5811
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[16]:C,4414
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[16]:D,5252
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[16]:Y,4414
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]:A,2548
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]:B,1818
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]:C,4100
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]:D,3961
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]:Y,1818
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o[0]:A,6973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o[0]:B,6384
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o[0]:C,5207
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o[0]:Y,5207
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:CLK,1257
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:D,1333
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:Q,1257
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_19:A,871
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_19:B,734
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_19:C,787
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_19:D,631
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_19:Y,631
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[10]:A,2901
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[10]:B,2840
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[10]:C,2561
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[10]:D,2532
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[10]:Y,2532
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:CLK,2323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:D,4964
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:Q,2323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_1:A,5722
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_1:B,5679
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_1:C,5597
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_1:D,5496
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_1:Y,5496
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_1_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_1_PAD/U_IOINFF:Y,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_54:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_54:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_54:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_54:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_54:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_156:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_156:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_156:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_156:IPA,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:D,8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIC9J32[6]:A,4557
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIC9J32[6]:B,3529
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIC9J32[6]:C,3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIC9J32[6]:Y,3324
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_12:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_12:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:CLK,440
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:D,8676
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:Q,440
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_9_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_9_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_9_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_9_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_9_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:CLK,5246
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:Q,5246
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:CLK,6807
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:Q,6807
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_1:A,6073
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_1:B,4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_1:P,4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_1:UB,4640
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17:B,3767
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17:C,3724
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17:CC,3336
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17:S,3336
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17:UB,3724
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:CLK,6828
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:D,6987
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:Q,6828
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13_1:A,-277
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13_1:B,-393
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13_1:C,-331
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13_1:Y,-393
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:CLK,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:Q,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_13:A,7808
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_13:B,7156
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_13:C,6712
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_13:CC,6502
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_13:S,6502
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_13:UB,6712
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:CLK,6020
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:Q,6020
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:CLK,7805
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:D,8544
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:Q,7805
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:CLK,6738
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:D,5174
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:Q,6738
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[10]:A,2948
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[10]:B,4217
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[10]:C,6056
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[10]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[10]:D,5902
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[10]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[10]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[10]:Y,2948
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:CLK,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:D,6817
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:Q,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_6:B,1576
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_6:C,1387
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_6:CC,1330
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_6:P,1387
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_6:S,1330
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_29:B,6369
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_29:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_29:D,6354
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_29:IPB,6369
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_29:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_29:IPD,6354
A0_ADC_CS_O_obuf/U0/U_IOENFF:A,
A0_ADC_CS_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AL_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SD_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SL_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[0],6757
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[10],6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[11],6738
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[12],6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[13],6711
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[14],6705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[15],6731
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[16],6745
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[17],6762
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[1],6733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[2],6724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[3],6697
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[4],6709
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[5],6733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[6],6772
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[7],6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[8],6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[9],6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_EN[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_EN[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[0],6791
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[10],6802
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[11],6844
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[12],6795
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[13],6814
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[14],6833
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[15],6859
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[16],6835
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[17],6804
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[1],6841
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[2],6847
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[3],6807
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[4],6810
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[5],6828
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[6],6771
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[7],6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[8],6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[9],6809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_EN[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_EN[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CARRYIN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[12],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[13],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[14],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[15],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[16],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[17],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[18],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[19],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[20],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[21],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[22],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[23],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[24],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[25],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[26],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[27],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[28],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[29],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[30],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[31],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[32],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[33],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[34],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[35],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[36],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[37],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[38],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[39],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[40],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[41],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[42],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[43],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[0],7662
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[10],7742
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[11],7691
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[12],7689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[13],7718
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[14],7714
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[15],7787
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[16],7815
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[17],7806
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[18],7809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[19],7866
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[1],7694
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[20],7863
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[21],7849
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[22],7856
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[23],7853
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[24],7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[25],7933
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[26],7919
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[27],7884
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[28],7946
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[29],7895
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[2],7727
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[30],7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[31],7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[32],7869
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[33],7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[34],7817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[35],7879
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[36],7864
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[37],7827
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[38],7871
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[39],7837
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[3],7685
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[40],7852
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[41],7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[42],7909
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[43],7949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[4],7657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[5],7641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[6],7686
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[7],7671
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[8],7661
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[9],7730
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_EN[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_EN[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:DOTP,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:OVFL_CARRYOUT_SEL,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[0],8721
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[10],8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[11],8719
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[12],8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[13],8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[14],8716
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[15],8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[16],8712
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[17],8710
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[18],8686
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[19],8681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[1],8725
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[20],8684
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[21],8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[22],8683
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[23],8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[24],8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[25],8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[26],8680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[27],8679
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[28],8679
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[29],8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[2],8725
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[30],8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[31],8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[32],8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[33],8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[34],8681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[35],8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[36],8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[37],8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[38],8673
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[39],8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[3],8729
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[40],8673
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[41],8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[42],8668
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[43],8678
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[4],8724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[5],8724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[6],8728
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[7],8728
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[8],8730
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[9],8725
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_CLK[0],8710
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_CLK[1],8668
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_EN[0],8996
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_EN[1],9019
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SIMD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_AD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_AL_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_SD_N,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_SL_N,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:D,8725
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:CLK,3760
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:D,6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:Q,3760
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:D,6203
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:CLK,5633
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:D,5423
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:Q,5633
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[11]:A,3337
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[11]:B,4712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[11]:C,2282
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[11]:D,3027
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[11]:Y,2282
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_46:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_46:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_46:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_46:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:D,2841
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[5]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[5]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[5]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[2]:A,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[2]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[2]:C,5882
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[2]:Y,5614
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:CLK,3759
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:D,2254
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:Q,3759
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[5]:A,6124
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[5]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[5]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[5]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[5]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:CLK,5150
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:Q,5150
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_11:B,3290
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_11:UB,3290
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_12:B,6940
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_12:CC,6966
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_12:P,6940
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_12:S,6966
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:CLK,4066
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:Q,4066
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:CLK,4518
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:D,5835
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:Q,4518
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:CLK,3854
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:D,8717
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:Q,3854
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:D,3431
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:CO,4207
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[0],4641
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[1],4523
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[2],4424
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[3],4345
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[6],4260
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[7],4207
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[8],4367
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:P[9],4310
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[0],5861
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[10],6145
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[11],6266
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[1],5956
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[2],6080
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[3],5999
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[4],6037
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[5],6129
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[6],6020
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[7],6078
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[8],6186
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_0:UB[9],6127
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[0]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[0]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[0]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[0]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:C,6677
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:IPC,6677
A0_PWM_WH_O_obuf/U0/U_IOOUTFF:A,4354
A0_PWM_WH_O_obuf/U0/U_IOOUTFF:Y,4354
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:D,8725
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[10],6803
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[11],6742
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[1],7415
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[2],7351
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[3],7002
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[4],6932
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[5],6871
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[6],6928
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[7],6850
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[8],6790
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CC[9],6887
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:CO,6659
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[0],6811
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[1],6756
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[2],6929
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[3],6916
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[6],6926
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[7],6966
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[8],7032
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:P[9],7026
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[0],6659
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[10],6921
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[11],7023
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[1],6748
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[2],6893
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[3],6787
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[4],6818
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[5],6925
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[6],6824
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[7],6878
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[8],6964
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_0_CC_0:UB[9],6933
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[39]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[39]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[39]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[39]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[39]:Y,224
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:CLK,5091
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:Q,5091
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:C,6847
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPC,6847
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:CLK,5233
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:Q,5233
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_1:B,1544
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_1:C,1128
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_1:CC,1468
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_1:P,1128
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_1:S,1468
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_1:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_257:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_257:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_257:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_257:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_257:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:C,6833
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPC,6833
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPD,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_1:A,6969
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_1:B,6877
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_1:CC,7524
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_1:P,6877
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_1:S,7524
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_1:UB,6895
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[5]:A,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[5]:B,5454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[5]:C,5343
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[5]:D,4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[5]:Y,4251
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:CLK,5712
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:D,6788
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:Q,5712
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_12:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_12:IPENn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_199:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_199:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_199:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_199:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_199:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy:A,6624
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy:B,4998
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy:C,6857
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy:D,6321
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy:P,4998
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy:UB,6321
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_2:B,4409
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_2:C,4248
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_2:CC,4424
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_2:P,4248
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_2:S,4424
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_2:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[6]:A,4214
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[6]:B,1891
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[6]:C,1902
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[6]:Y,1891
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:C,6738
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:IPC,6738
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:CLK,1125
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:D,8717
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:Q,1125
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:CLK,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:D,4220
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:Q,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AL_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SD_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SL_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[0],6757
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[10],6818
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[11],6738
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[12],6763
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[13],6711
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[14],6705
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[15],6731
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[16],6745
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[17],6762
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[1],6733
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[2],6724
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[3],6697
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[4],6709
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[5],6733
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[6],6772
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[7],6747
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[8],6754
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[9],6747
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_EN[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_EN[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[0],6791
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[10],6802
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[11],6844
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[12],6795
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[13],6814
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[14],6833
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[15],6859
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[16],6835
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[17],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[1],6841
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[2],6847
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[3],6807
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[4],6810
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[5],6828
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[6],6771
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[7],6818
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[8],6754
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[9],6809
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_EN[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_EN[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CARRYIN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[10],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[11],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[12],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[13],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[14],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[15],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[16],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[17],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[18],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[19],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[20],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[21],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[22],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[23],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[24],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[25],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[26],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[27],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[28],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[29],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[2],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[30],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[31],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[32],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[33],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[34],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[35],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[36],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[37],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[38],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[39],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[3],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[40],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[41],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[42],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[43],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[4],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[5],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[6],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[7],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[8],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[9],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[10],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[11],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[12],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[13],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[14],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[15],7774
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[16],7808
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[17],7799
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[18],7802
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[19],7859
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[20],7856
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[21],7842
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[22],7849
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[23],7846
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[24],7825
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[25],7926
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[26],7912
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[27],7877
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[28],7939
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[29],7888
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[2],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[30],7879
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[31],7882
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[32],7862
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[33],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[34],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[35],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[36],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[37],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[38],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[39],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[3],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[40],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[41],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[42],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[43],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[4],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[5],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[6],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[7],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[8],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[9],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_EN[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_EN[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:DOTP,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:OVFL_CARRYOUT_SEL,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[16],8706
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[17],8704
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[18],8680
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[19],8675
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[20],8678
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[21],8676
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[22],8677
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[23],8676
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[24],8671
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[25],8670
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[26],8674
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[27],8673
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[28],8673
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[29],8668
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[30],8670
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[31],8670
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[32],8671
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[33],8676
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_CLK[0],8704
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_CLK[1],8668
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_EN[0],8996
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_EN[1],9019
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SIMD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_AD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_AL_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_SD_N,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_SL_N,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:CLK,2845
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:D,2723
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:Q,2845
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[5]:A,2844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[5]:B,2648
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[5]:C,2783
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[5]:Y,2648
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:CLK,422
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:D,7910
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:Q,422
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:CLK,4373
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:Q,4373
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[16]:A,5932
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[16]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[16]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[16]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[16]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6_RNO:A,5129
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6_RNO:B,3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6_RNO:C,5007
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_6_RNO:Y,3654
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[7]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[7]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[7]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[7]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[39]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[39]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[39]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_13:B,2242
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_13:C,2085
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_13:CC,1239
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_13:S,1239
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:CLK,1371
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:D,8717
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:Q,1371
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_5:B,4930
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_5:UB,4930
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:D,5899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:D,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:D,6059
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_6:A,4389
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_6:B,4258
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_6:P,4317
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_6:UB,4258
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_8:A,3562
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_8:B,1290
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_8:P,1332
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_8:UB,1290
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[31]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[31]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[31]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[31]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[31]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_23:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_23:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[9]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_16:B,4174
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_16:UB,4174
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:C,6807
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPC,6807
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:CLK,5007
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:D,6801
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:Q,5007
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32[2]:A,2052
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32[2]:B,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32[2]:Y,2014
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_0_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_0_PAD/U_IOINFF:Y,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260:B,1081
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260:C,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260:CC,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260:P,1081
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:CLK,6833
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:Q,6833
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[1]:A,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[1]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[1]:C,6154
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[1]:Y,5675
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:CLK,6843
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:D,7480
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:Q,6843
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[2]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:CLK,7140
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:Q,7140
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_8:A,6324
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_8:B,4244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_8:P,4278
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_8:UB,4244
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_15:A,969
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_15:B,991
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_15:C,6
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_15:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_15:Y,-247
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNII8KB1[7]:A,2506
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNII8KB1[7]:B,2273
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNII8KB1[7]:C,2384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNII8KB1[7]:Y,2273
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16:A,7808
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16:B,5442
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16:CC,5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16:S,5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16:UB,5442
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17_FCINST1:CC,3828
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17_FCINST1:CO,3828
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[17]:A,5717
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[17]:B,2310
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[17]:C,2373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[17]:D,2108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[17]:Y,2108
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:CLK,7061
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:Q,7061
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]:A,2819
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]:B,3213
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]:C,5037
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]:D,4913
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]:Y,2819
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:C,6810
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPC,6810
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:C,6841
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPC,6841
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPD,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[17]:A,7160
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[17]:B,6578
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[17]:C,7039
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[17]:Y,6578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_10_151_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_10_151_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_10_151_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_10_151_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_9:A,1460
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_9:B,3151
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_9:P,1460
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_9:UB,3151
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO_0:A,4872
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO_0:B,2250
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO_0:C,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO_0:D,4871
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO_0:Y,2250
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:CLK,5100
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:Q,5100
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[16]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[16]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[16]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_axb_0_1:A,5940
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_axb_0_1:B,5620
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_axb_0_1:C,3866
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_axb_0_1:D,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_axb_0_1:Y,2622
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_34:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_34:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:D,8697
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219:B,4182
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219:C,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219:P,4182
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[16]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[16]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[16]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[16]:Y,6423
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start_RNO:A,7871
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start_RNO:B,7867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start_RNO:Y,7867
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12_1:A,1497
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12_1:B,1372
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12_1:C,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12_1:Y,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[39]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[39]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[39]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_8:B,3621
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_8:CC,3496
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_8:P,3621
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_8:S,3496
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:CLK,6763
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:Q,6763
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_5_206_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_5_206_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_5_206_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_5_206_i_m2:Y,7698
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:CLK,6810
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:Q,6810
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:CLK,7013
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:Q,7013
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]:Y,4589
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[4]:A,1943
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[4]:B,4088
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[4]:C,1585
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[4]:D,1779
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[4]:Y,1585
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[16]:A,4477
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[16]:B,2587
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[16]:C,1795
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[16]:Y,1795
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_218:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_218:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_218:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_218:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_218:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_12:A,2525
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_12:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_12:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_12:IPA,2525
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:C,6762
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:IPC,6762
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:CLK,6804
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:Q,6804
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:CLK,3815
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:Q,3815
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:CLK,7573
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:D,8834
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:EN,7861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:Q,7573
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_done:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:CLK,1920
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:D,7448
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:Q,1920
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9:A,3018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9:B,2817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9:CC,2766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9:P,2906
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9:S,2766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9:UB,2817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:CLK,1777
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:D,8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:Q,1777
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0:A,4853
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0:B,4652
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0:P,4761
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0:UB,4652
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[10]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[10]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[10]:C,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[10]:Y,5156
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:CLK,2280
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:D,5889
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:Q,2280
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[6]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[6]:B,7054
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[6]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[6]:CC,7161
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[6]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[6]:P,7054
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[6]:S,7161
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[18]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[18]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[18]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[18]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_27_0:A,1994
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_27_0:B,1292
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_27_0:C,1365
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_27_0:CC,217
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_27_0:D,78
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_27_0:P,213
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_27_0:S,217
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_27_0:UB,78
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:CC[6],988
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:CI,1100
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[0],1135
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[1],1029
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[3],1219
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[0],988
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[1],1026
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[2],1242
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[3],1100
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[4],1080
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[5],3581
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:CLK,6828
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:Q,6828
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:CLK,4853
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:Q,4853
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[3]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[3]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[3]:C,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[3]:Y,5342
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:CLK,6080
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:Q,6080
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:CLK,7657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:Q,7657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_2:A,5650
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_2:B,5292
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_2:CC,6139
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_2:P,5324
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_2:S,6059
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_2:UB,5292
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o_1_sqmuxa_0_a2:A,5477
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o_1_sqmuxa_0_a2:B,5871
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o_1_sqmuxa_0_a2:C,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o_1_sqmuxa_0_a2:D,4961
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o_1_sqmuxa_0_a2:Y,3090
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_5:B,4299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_5:UB,4299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_9:A,6350
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_9:B,4308
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_9:P,4362
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_9:UB,4308
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[15]:A,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[15]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[15]:C,5625
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[15]:Y,5150
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:CLK,4042
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:D,8710
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:Q,4042
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_7:B,1649
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_7:C,1460
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_7:CC,1323
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_7:P,1460
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_7:S,1323
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:CLK,4438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:Q,4438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:CLK,2768
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:Q,2768
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[33]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:CLK,7842
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:D,7876
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:Q,7842
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:CLK,6709
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:D,7078
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:Q,6709
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_2:A,3093
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_2:B,3036
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_2:P,3088
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_2:UB,3036
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[41]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[41]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[41]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[41]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[41]:Y,88
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_13:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_13:B,6992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_13:CC,6875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_13:S,6875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_13:UB,6992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0:A,7130
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0:B,6573
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0:C,4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0:CC,2223
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0:D,2282
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0:P,2378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0:S,2223
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0:UB,2282
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:CLK,6726
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:D,7386
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:Q,6726
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:CLK,4185
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:D,8724
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:Q,4185
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[11]:A,3420
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[11]:B,3382
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[11]:C,2397
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[11]:D,2323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[11]:Y,2323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEKTI2_0[17]:A,4248
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEKTI2_0[17]:B,2681
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEKTI2_0[17]:C,2561
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEKTI2_0[17]:Y,2561
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o_1_sqmuxa_0_a2:A,5591
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o_1_sqmuxa_0_a2:B,5963
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o_1_sqmuxa_0_a2:C,3182
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o_1_sqmuxa_0_a2:D,5100
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o_1_sqmuxa_0_a2:Y,3182
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:CLK,5932
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:D,7816
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:EN,7664
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:Q,5932
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9:A,6992
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9:B,3586
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9:C,3536
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9:CC,3538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9:P,3619
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9:S,3538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9:UB,3536
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_15:A,3275
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_15:B,3063
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_15:P,3183
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_15:UB,3063
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[4]:A,2094
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[4]:B,1002
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[4]:C,6922
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[4]:D,2760
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[4]:Y,1002
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_64:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_64:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_64:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_64:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_64:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_4:B,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_4:CC,7127
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_4:S,7127
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_4:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[0]:A,4022
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[0]:B,2564
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[0]:C,3096
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[0]:D,1673
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[0]:Y,1673
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[37]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[37]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[37]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[37]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[37]:Y,224
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_211:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_211:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_211:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_211:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_211:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy:B,4891
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy:C,6765
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy:CC,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy:P,4891
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_81:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_81:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_81:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_81:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_81:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:CLK,4132
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:Q,4132
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:CLK,6145
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:Q,6145
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:CLK,5220
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:Q,5220
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[14]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[14]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[14]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[14]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIC6A11[11]:A,1402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIC6A11[11]:B,1323
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIC6A11[11]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIC6A11[11]:CC,5663
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIC6A11[11]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIC6A11[11]:P,1323
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIC6A11[11]:S,5663
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIC6A11[11]:UB,1330
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:CLK,2876
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:Q,2876
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[0]:A,7846
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[0]:B,7926
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[0]:C,7526
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[0]:D,6817
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[0]:Y,6817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[11]:A,5968
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[11]:B,5896
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[11]:C,4395
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[11]:D,5384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[11]:Y,4395
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0:A,7219
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0:B,6634
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0:C,4468
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0:CC,2246
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0:D,2336
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0:P,2439
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0:S,2246
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0:UB,2336
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:CLK,5347
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:Q,5347
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:CLK,4007
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:D,7794
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:Q,4007
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_180:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_180:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_180:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_180:IPA,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[15]:A,5713
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[15]:B,5928
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[15]:C,2747
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[15]:D,2764
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[15]:Y,2747
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:CLK,6841
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:Q,6841
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s[17]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s[17]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s[17]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s[17]:CC,6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s[17]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s[17]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s[17]:S,6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[9]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[9]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[9]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[9]:Y,6423
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_249:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_249:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_249:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_249:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_249:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_1:A,4604
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_1:B,6024
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_1:P,4604
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_1:UB,6024
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_7:A,3468
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_7:B,5060
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_7:P,3468
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_7:UB,5060
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_11:A,6077
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_11:B,5401
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_11:CC,5114
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_11:S,5114
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_11:UB,5401
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:B,7815
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:C,6754
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:IPB,7815
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:CLK,3729
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:D,6842
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:Q,3729
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:D,3074
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:CLK,6117
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:D,8668
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:Q,6117
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[9]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[9]:B,5139
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[9]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[9]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[9]:Y,3584
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]_CC_0:UB[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_36:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_36:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_36:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_36:IPA,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_13:B,3915
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_13:CC,3384
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_13:P,3915
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_13:S,3384
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_13:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o_1_sqmuxa_0_a2:A,5611
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o_1_sqmuxa_0_a2:B,5196
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o_1_sqmuxa_0_a2:C,5300
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o_1_sqmuxa_0_a2:D,2979
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o_1_sqmuxa_0_a2:Y,2979
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEKTI2[17]:A,5555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEKTI2[17]:B,3980
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEKTI2[17]:C,3868
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEKTI2[17]:Y,3868
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:CLK,6122
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:Q,6122
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:B,7886
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:C,6711
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:IPB,7886
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:IPC,6711
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:CLK,7806
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:Q,7806
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:D,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[15]:A,6182
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[15]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[15]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[15]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[15]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry:B,5371
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry:C,5320
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry:CC,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry:P,5588
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry:UB,5606
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry:Y,5320
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:D,5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_14:A,7749
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_14:B,6986
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_14:CC,6701
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_14:S,6701
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_14:UB,6986
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_adc_start_o_3_iv_0:A,7918
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_adc_start_o_3_iv_0:B,6943
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_adc_start_o_3_iv_0:C,6894
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_adc_start_o_3_iv_0:D,5496
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_adc_start_o_3_iv_0:Y,5496
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO:A,5643
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO:B,5595
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO:C,3738
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO:D,3658
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO:Y,3658
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:CLK,4113
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:Q,4113
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:CLK,4465
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:Q,4465
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[17]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_178:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_178:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_178:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_178:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:CLK,3384
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:Q,3384
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[1]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_5:A,1445
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_5:B,1760
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_5:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_5:IPA,1445
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_5:IPB,1760
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_14_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_14_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_14_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_14_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_14_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFDT9[6]:A,2692
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFDT9[6]:B,2615
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFDT9[6]:C,2181
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFDT9[6]:Y,2181
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[12]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[12]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[12]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_16_85_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_16_85_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_16_85_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_16_85_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17:A,3684
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17:B,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17:C,3562
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17:D,3484
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17:Y,2622
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:CLK,4958
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:D,7021
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:Q,4958
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:CLK,3061
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:Q,3061
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:CLK,6370
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:Q,6370
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8:A,1646
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8:B,1569
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8:CC,1303
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8:P,1597
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8:S,1303
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8:UB,1569
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_9:B,5219
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_9:C,5048
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_9:CC,4310
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_9:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_9:S,4310
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:CLK,7686
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:Q,7686
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_5:B,4299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_5:UB,4299
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/un1_s_pout_0_sqmuxa_0:A,7401
BLDC_Encoder_Axis_0/MSC_i_11/un1_s_pout_0_sqmuxa_0:B,6935
BLDC_Encoder_Axis_0/MSC_i_11/un1_s_pout_0_sqmuxa_0:C,7246
BLDC_Encoder_Axis_0/MSC_i_11/un1_s_pout_0_sqmuxa_0:D,7177
BLDC_Encoder_Axis_0/MSC_i_11/un1_s_pout_0_sqmuxa_0:Y,6935
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[4]:A,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[4]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[4]:C,5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[4]:Y,5274
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:CLK,3245
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:D,8717
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:Q,3245
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:CLK,2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:Q,2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[2]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[14]:A,4223
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[14]:B,4139
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[14]:C,3950
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[14]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[14]:Y,3950
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_10:A,7808
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_10:B,7194
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_10:C,6763
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_10:CC,6509
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_10:S,6509
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_10:UB,6763
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[1]:A,6614
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[1]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[1]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[1]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[1]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO:A,5517
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO:B,5469
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO:C,3464
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO:D,3552
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2_RNO:Y,3464
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[5]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[5]:B,4716
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[5]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[5]:Y,91
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[11]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[11]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[11]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[11]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[11]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[11]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[11]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:CLK,4218
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:Q,4218
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:CLK,5127
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:D,6835
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:Q,5127
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO_0:A,5518
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO_0:B,5424
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO_0:C,3567
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO_0:D,3487
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7_RNO_0:Y,3487
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_3:A,4426
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_3:B,6067
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_3:P,4426
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_3:UB,6067
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[11]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[11]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[11]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_14:B,4221
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_14:UB,4221
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[2]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[2]:B,5363
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[2]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[2]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[2]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[15]:A,3601
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[15]:B,3588
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[15]:C,2603
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[15]:D,2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[15]:Y,2456
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:D,5112
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[10]:A,4286
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[10]:B,1963
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[10]:C,1974
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[10]:Y,1963
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:CO,4288
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[0],4722
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[1],4604
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[2],4505
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[3],4426
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[6],4341
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[7],4288
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[8],4448
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:P[9],4391
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[0],5929
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[10],6213
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[11],6334
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[1],6024
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[2],6148
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[3],6067
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[4],6105
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[5],6197
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[6],6088
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[7],6146
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[8],6254
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_0:UB[9],6195
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset_0_sqmuxa:A,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset_0_sqmuxa:B,7483
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset_0_sqmuxa:Y,7426
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[10],4310
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[1],4641
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[2],4523
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[3],4424
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[4],4345
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[7],4260
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[8],4207
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CC[9],4367
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:CO,4089
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[0],4182
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[1],4089
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[2],4229
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[3],4248
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[6],4260
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[7],4266
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[8],4336
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:P[9],4366
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDM0J[14]:A,2766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDM0J[14]:B,2689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDM0J[14]:C,2255
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDM0J[14]:Y,2255
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_187:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_187:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_187:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_187:IPA,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:D,4130
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_6:A,3999
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_6:B,6020
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_6:P,3999
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_6:UB,6020
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_21:A,796
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_21:B,673
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_21:C,698
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_21:D,541
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_21:Y,541
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_5:A,7835
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_5:B,6875
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_5:CC,7005
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_5:S,7005
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_5:UB,6875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_25:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_25:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0:A,4181
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0:B,4843
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0:P,4181
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0:UB,4843
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIGI45L[16]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIGI45L[16]:B,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIGI45L[16]:C,7716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIGI45L[16]:CC,3674
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIGI45L[16]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIGI45L[16]:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIGI45L[16]:S,3674
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIGI45L[16]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0:A,6758
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0:B,4244
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0:C,4096
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0:D,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0:P,3256
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0:UB,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0:Y,4495
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:D,3150
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_8:B,4602
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_8:C,4447
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_8:CC,4448
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_8:P,4447
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_8:S,4448
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:CLK,4798
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:Q,4798
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:CLK,4962
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:Q,4962
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:C,6791
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:IPC,6791
A0_ADC_SDI_I_ibuf/U0/U_IOPAD:PAD,6138
A0_ADC_SDI_I_ibuf/U0/U_IOPAD:Y,6138
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21:A,7178
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21:B,3845
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21:C,3722
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21:CC,3351
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21:P,3805
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21:S,3351
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21:UB,3722
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:CLK,4309
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:Q,4309
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_13:A,4170
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_13:B,6180
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_13:P,4170
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_13:UB,6180
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[15]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o_1_sqmuxa_0_a2:A,7844
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o_1_sqmuxa_0_a2:B,7759
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o_1_sqmuxa_0_a2:C,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o_1_sqmuxa_0_a2:Y,6734
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:CLK,6667
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:D,8814
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:EN,7792
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:Q,6667
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_17/done_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_29:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_29:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:Q,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[13]:A,5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[13]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[13]:C,5606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[13]:Y,5118
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[6]:A,5929
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[6]:B,5852
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[6]:C,4356
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[6]:D,5340
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[6]:Y,4356
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[7]:A,2211
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[7]:B,4281
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[7]:C,3714
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[7]:Y,2211
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[37]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[37]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[37]:Y,7440
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o_1_sqmuxa_0_a2:A,7836
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o_1_sqmuxa_0_a2:B,7759
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o_1_sqmuxa_0_a2:C,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o_1_sqmuxa_0_a2:Y,6734
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5:A,2186
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5:B,1514
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5:CC,1378
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5:S,1378
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5:UB,1514
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:CLK,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:Q,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[9]:A,2684
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[9]:B,2766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[9]:C,2635
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[9]:Y,2635
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRLGT[22]:A,3813
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRLGT[22]:B,3500
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRLGT[22]:C,3691
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRLGT[22]:Y,3500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:B,6154
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:C,7716
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:CC,5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:D,6025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:S,5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0:A,6814
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0:B,6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0:P,6755
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0:UB,6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0:Y,7923
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:CLK,3474
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:Q,3474
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[2]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[2]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[2]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[2]:Y,1256
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[8]:A,2072
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[8]:B,2944
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[8]:C,5233
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[8]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[8]:D,5081
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[8]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[8]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[8]:Y,2072
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[12]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[12]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[12]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[12]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:B,7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:C,6711
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:IPB,7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:IPC,6711
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:CLK,6078
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:Q,6078
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_5:B,4299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_5:UB,4299
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:CLK,6711
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:Q,6711
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_29:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_29:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:CLK,4886
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:Q,4886
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_11:A,7835
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_11:B,7009
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_11:CC,6879
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_11:S,6879
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_11:UB,7009
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_11:B,6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_11:UB,6303
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]:A,2343
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]:B,1836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]:C,4096
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]:D,3978
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]:Y,1836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:D,8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[35]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[35]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[35]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[35]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:CC[0],6781
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:CC[1],6703
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:CC[2],6645
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:CC[3],6735
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:CC[4],6664
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:CC[5],6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:CC[6],6732
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:CI,6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[0],7077
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[1],7161
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[2],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[3],7332
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[6],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[7],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[8],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:P[9],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_2:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:CLK,6818
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:Q,6818
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[17]:A,6978
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[17]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[17]:C,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[17]:Y,5018
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:CLK,6771
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:Q,6771
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_9:B,5294
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_9:C,5129
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_9:CC,4391
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_9:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_9:S,4391
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIB6J5F[38]:A,3410
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIB6J5F[38]:B,1855
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIB6J5F[38]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIB6J5F[38]:CC,2266
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIB6J5F[38]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIB6J5F[38]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIB6J5F[38]:S,2266
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIB6J5F[38]:UB,1855
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_5:B,4496
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_5:C,4341
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_5:P,4341
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_5:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[14]:A,6119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[14]:B,6042
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[14]:C,4546
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[14]:D,5530
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[14]:Y,4546
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[10],6918
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[11],6857
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[1],7531
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[2],7467
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[3],7151
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[4],7084
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[5],7034
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[6],7056
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[7],6965
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[8],6905
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CC[9],7002
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:CO,6800
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[0],6927
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[1],6883
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[2],7057
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[3],7042
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[6],7054
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[7],7094
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[8],7164
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:P[9],7160
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[0],6800
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[10],7090
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[11],7211
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[1],6901
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[2],7025
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[3],6944
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[4],6982
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[5],7074
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[6],6965
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[7],7023
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[8],7131
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_0:UB[9],7072
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[29]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[29]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[29]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[29]:Y,6423
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[7]:A,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[7]:B,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[7]:C,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[7]:Y,7659
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_24:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_24:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUULU[1]:A,6953
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUULU[1]:B,6587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUULU[1]:C,6499
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUULU[1]:Y,6499
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:B,7871
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:C,6745
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:IPB,7871
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:IPC,6745
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:CLK,4562
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:D,4669
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:Q,4562
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[14]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_225:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_225:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_225:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_225:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_225:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:CLK,2917
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:D,2717
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:Q,2917
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_14:B,7060
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_14:CC,6830
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_14:P,7060
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_14:S,6830
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_14:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_162:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_162:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_162:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_162:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_162:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:CLK,4879
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:D,6888
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:Q,4879
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]:A,2258
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]:B,1539
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]:C,3805
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]:D,3681
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[3]:Y,1539
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_28:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_28:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:CLK,5820
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:D,6914
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:Q,5820
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15:B,3425
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15:CC,2711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15:S,2711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_4:A,7911
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_4:B,7296
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_4:C,7876
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_4:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_4:Y,7296
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[6]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[6]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[6]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:CLK,263
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:D,8683
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:Q,263
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO:A,5768
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO:B,6004
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO:C,3863
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO:D,5548
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO:Y,3863
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:CC[0],6958
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:CC[1],6888
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:CC[2],6844
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:CC[3],6906
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:CC[4],6842
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:CC[5],6793
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:CI,6793
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[0],7077
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[1],7028
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[2],7154
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[3],7409
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[4],7537
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:C,6733
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:IPC,6733
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_5:B,1291
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_5:UB,1291
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[10]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[10]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[10]:Y,5366
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_111:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_111:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_111:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_111:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_111:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:CLK,6286
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:Q,6286
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[15]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[15]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[15]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:CLK,6957
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:Q,6957
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIPLSR6[5]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIPLSR6[5]:B,4226
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIPLSR6[5]:C,7056
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIPLSR6[5]:CC,4288
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIPLSR6[5]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIPLSR6[5]:P,4226
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIPLSR6[5]:S,4288
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIPLSR6[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_16:A,7848
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_16:B,6900
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_16:CC,6988
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_16:S,6988
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_16:UB,6900
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:D,8730
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:CLK,6918
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:D,6927
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:Q,6918
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]:A,2727
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]:B,1997
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]:C,4279
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]:D,4140
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]:Y,1997
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[0]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[0]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[0]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[0]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:CLK,1640
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:D,8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:Q,1640
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5_0:A,6219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5_0:B,7274
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5_0:C,6998
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5_0:CC,5509
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5_0:S,5509
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5_0:UB,6998
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:D,8724
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI5T1P6[6]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI5T1P6[6]:B,6057
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI5T1P6[6]:C,7158
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI5T1P6[6]:CC,5964
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI5T1P6[6]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI5T1P6[6]:P,6057
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI5T1P6[6]:S,5964
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI5T1P6[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[17]:A,6050
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[17]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[17]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[17]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[17]:Y,2538
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:CLK,3874
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:EN,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:Q,3874
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:CLK,6183
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:Q,6183
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:D,3449
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy:B,6743
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy:C,6457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy:P,6457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0_cy:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_8_0:A,5598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_8_0:B,6578
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_8_0:C,5438
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_8_0:CC,5222
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_8_0:D,6879
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_8_0:P,5472
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_8_0:S,5222
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_8_0:UB,5438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:CLK,6729
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:D,6363
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:Q,6729
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3:A,8004
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3:B,7920
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3:C,7464
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3:D,6373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3:Y,6373
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:CLK,6763
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:D,6958
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:Q,6763
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:D,3772
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:CLK,1445
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:Q,1445
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_3:A,2089
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_3:B,1913
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_3:P,2003
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_3:UB,1913
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[36]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[36]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[36]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[36]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in_1_sqmuxa_i:A,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in_1_sqmuxa_i:B,7553
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in_1_sqmuxa_i:Y,5058
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:CLK,1787
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:D,8677
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:Q,1787
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[24]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]:A,2450
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]:B,1943
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]:C,4203
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]:D,4085
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]:Y,1943
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:D,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[5]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[5]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[5]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_1:B,3384
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_1:CC,3743
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_1:P,3384
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_1:S,3743
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_1:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:CLK,4046
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:D,5810
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:Q,4046
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_RNO[17]:A,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_RNO[17]:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_RNO[17]:C,3501
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_RNO[17]:CC,2886
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_RNO[17]:D,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_RNO[17]:P,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_RNO[17]:S,2886
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_RNO[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:Q,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11]:SLn,
CFG0_GND_INST:Y,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:D,5627
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[3]:A,3862
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[3]:B,1539
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[3]:C,1550
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[3]:Y,1539
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[1]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_6:A,1585
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_6:B,1696
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_6:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_6:IPA,1585
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_6:IPB,1696
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7:A,7110
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7:B,5103
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7:CC,5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7:P,5157
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7:S,5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7:UB,5103
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_138:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_138:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_138:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_138:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_138:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:CLK,2107
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:D,5950
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:Q,2107
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0:A,6966
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0:B,5472
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0:P,5599
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0:UB,5472
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_14:A,5927
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_14:B,5211
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_14:CC,5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_14:S,5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_14:UB,5211
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:CLK,7028
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:Q,7028
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:CLK,5564
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:D,4196
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:Q,5564
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[0]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[0]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[0]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[0]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:CLK,6924
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:D,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:Q,6924
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[14]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[15]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[15]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[15]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[15]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:CLK,5060
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:D,3799
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:Q,5060
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:CLK,6697
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:D,7544
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:Q,6697
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[1]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:CLK,4624
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:D,4669
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:Q,4624
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[9]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[9]:B,7661
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[9]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[9]:CC,6934
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[9]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[9]:P,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[9]:S,6934
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI3FUTH[16]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI3FUTH[16]:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI3FUTH[16]:C,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI3FUTH[16]:CC,2765
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI3FUTH[16]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI3FUTH[16]:P,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI3FUTH[16]:S,2765
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI3FUTH[16]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_7:A,6254
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_7:B,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_7:P,4268
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_7:UB,4214
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[22]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNIMSE31[0]:A,7783
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNIMSE31[0]:B,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNIMSE31[0]:C,7674
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNIMSE31[0]:Y,6808
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_48:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_48:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_48:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_48:IPA,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18:B,2477
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18:CC,1774
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18:P,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18:S,1774
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_25:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_25:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:CLK,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:D,2671
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:Q,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:CLK,5495
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:D,5888
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:EN,5030
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:Q,5495
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[40]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[40]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[40]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:B,7685
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:C,6697
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:IPB,7685
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:IPC,6697
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_57:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_57:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_57:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_57:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_57:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_15:B,7527
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_15:C,7552
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_15:CC,6679
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_15:S,6679
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:CLK,4978
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:Q,4978
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_15:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_15:C,7716
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_15:CC,3615
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_15:D,5763
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_15:S,3615
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_15:UB,5763
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:CLK,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:Q,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:CLK,5685
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:D,6193
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:Q,5685
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_17:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_17:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:CLK,3524
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:D,8670
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:Q,3524
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:CLK,6795
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:Q,6795
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:C,6731
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:IPC,6731
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1:An,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1:ENn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1:YL,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:CLK,7863
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:Q,7863
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:C,6847
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPC,6847
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:CLK,5109
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:D,3812
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:Q,5109
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[38]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[38]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[38]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[38]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[38]:Y,224
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:D,8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:CLK,8854
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:D,7796
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:EN,6808
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:Q,8854
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mas_en:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12:A,7129
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12:B,5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12:CC,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12:P,5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12:S,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:CLK,972
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:D,1002
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:Q,972
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO_0:A,3110
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO_0:B,2022
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO_0:C,4856
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO_0:Y,2022
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14:B,2336
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14:CC,1532
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14:S,1532
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_1_0:A,1312
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_1_0:B,1225
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_1_0:C,694
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_1_0:CC,581
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_1_0:D,972
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_1_0:P,702
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_1_0:S,581
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_1_0:UB,694
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4:A,2094
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4:B,1422
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4:CC,1339
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4:S,1339
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4:UB,1422
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_axb_0_i_0:A,7924
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_axb_0_i_0:B,7910
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_axb_0_i_0:Y,7910
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_32:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_32:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:CLK,2207
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:Q,2207
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_12:A,4604
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_12:B,4485
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_12:CC,4108
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_12:P,4485
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_12:S,4108
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNIKN4I[1]:A,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNIKN4I[1]:B,7707
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNIKN4I[1]:Y,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_26:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_26:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:CC[6],4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:CI,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[0],4273
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[1],4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[3],4332
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[0],4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[1],4130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[2],4221
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[3],4208
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[4],4174
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[5],6370
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO:A,5660
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO:B,5612
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO:C,3755
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO:D,3672
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO:Y,3672
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:CLK,4982
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:Q,4982
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:CLK,6724
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:D,4066
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:Q,6724
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:CLK,5931
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:Q,5931
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:CLK,7332
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:D,6735
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:Q,7332
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:CLK,2923
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:D,2787
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:Q,2923
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_RNO[0]:A,7958
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_RNO[0]:Y,7958
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12_0:A,5515
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12_0:B,6565
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12_0:C,7040
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12_0:CC,5493
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12_0:P,5515
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12_0:S,5493
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12_0:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:D,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[10],4391
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[1],4722
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[2],4604
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[3],4505
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[4],4426
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[7],4341
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[8],4288
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CC[9],4448
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:CO,4170
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[0],4263
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[1],4170
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[2],4310
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[3],4329
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[6],4341
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[7],4347
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[8],4417
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:P[9],4447
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3A9P1[14]:A,2486
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3A9P1[14]:B,2246
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3A9P1[14]:C,2412
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3A9P1[14]:Y,2246
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:C,6771
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:IPC,6771
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_154:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_154:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_154:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_154:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_7_184_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_7_184_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_7_184_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_7_184_i_m2:Y,7698
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]:A,2610
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]:B,1891
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]:C,4157
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]:D,4033
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[6]:Y,1891
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO:A,5623
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO:B,5575
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO:C,3811
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO:D,3644
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8_RNO:Y,3644
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_143:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_143:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_143:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_143:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:CLK,7919
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:Q,7919
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:D,5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:D,6509
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:CLK,6809
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:Q,6809
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[9]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_108:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_108:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_108:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_108:IPA,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:B,7886
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:C,6762
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:IPB,7886
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:IPC,6762
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:D,5222
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[8]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_9:A,1809
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_9:B,1836
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_9:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_9:IPA,1809
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_9:IPB,1836
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[17]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[17]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[17]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[17]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27_RNO:A,5765
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27_RNO:B,6001
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27_RNO:C,3860
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27_RNO:D,5545
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27_RNO:Y,3860
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en_RNO:A,7869
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en_RNO:B,7714
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en_RNO:C,7787
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en_RNO:Y,7714
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_3:B,5177
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_3:CC,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_3:P,5177
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_3:S,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_3:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]:A,2147
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]:B,2654
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]:C,4345
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]:D,4228
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]:Y,2147
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0:B,6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0:C,6717
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0:CC,7313
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0:P,6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0:S,7313
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[2]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[2]:B,7066
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[2]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[2]:CC,7467
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[2]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[2]:P,7066
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[2]:S,7467
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:CLK,4877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:Q,4877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:CLK,5956
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:D,8704
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:Q,5956
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_12:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_12:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[1]:A,6143
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[1]:B,6331
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[1]:C,3155
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[1]:D,3180
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[1]:Y,3155
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI48T68[4]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI48T68[4]:B,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI48T68[4]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI48T68[4]:CC,4950
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI48T68[4]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI48T68[4]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI48T68[4]:S,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI48T68[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_21:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_21:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[5]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[5]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[5]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[0]:A,4777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[0]:B,4734
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[0]:C,4275
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[0]:Y,4275
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[3]:A,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[3]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[3]:C,5814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[3]:Y,5342
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:CLK,4258
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:Q,4258
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[6]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_196:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_196:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_196:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_196:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_196:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[2]:A,4739
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[2]:B,4691
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[2]:C,4242
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[2]:Y,4242
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[3]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[3]:B,5261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[3]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[3]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[3]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[0]:A,6820
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[0]:B,5800
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[0]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[0]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[0]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:CLK,7107
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:D,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:Q,7107
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in_1_sqmuxa_i:A,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in_1_sqmuxa_i:B,7573
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in_1_sqmuxa_i:Y,5058
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNI8L252[0]:A,6231
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNI8L252[0]:B,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNI8L252[0]:C,7133
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNI8L252[0]:Y,5666
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[10],5453
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[11],5392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[1],5963
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[2],5899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[3],5627
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[4],5559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[5],5509
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[6],5593
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[7],5501
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[8],5440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CC[9],5537
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:CO,5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[0],5359
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[1],5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[2],5484
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[3],5474
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[6],5486
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[7],5521
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[8],5591
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:P[9],5592
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[0],6724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[10],7014
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[11],7135
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[1],6825
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[2],6949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[3],6868
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[4],6906
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[5],6998
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[6],6889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[7],6947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[8],7055
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_0:UB[9],6996
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:CLK,4089
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:D,8676
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:Q,4089
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11:B,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11:S,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11:UB,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIMDGO6[3]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIMDGO6[3]:B,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIMDGO6[3]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIMDGO6[3]:CC,5011
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIMDGO6[3]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIMDGO6[3]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIMDGO6[3]:S,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIMDGO6[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:CLK,1983
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:D,8668
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:Q,1983
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[42]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:CLK,5829
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:Q,5829
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:CLK,2756
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:D,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:Q,2756
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_12:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_12:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_12:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_12:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_12:IPC,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[5]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_24:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_24:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_24:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_24:IPA,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_30:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_30:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AD,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AL_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SD_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SL_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[0],6757
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[10],6818
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[11],6738
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[12],6763
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[13],6711
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[14],6705
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[15],6731
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[16],6745
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[17],6762
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[1],6733
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[2],6724
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[3],6697
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[4],6709
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[5],6733
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[6],6772
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[7],6747
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[8],6754
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[9],6747
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_EN[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_EN[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[0],6791
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[10],6802
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[11],6844
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[12],6795
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[13],6814
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[14],6833
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[15],6859
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[16],6835
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[17],6804
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[1],6841
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[2],6847
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[3],6807
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[4],6810
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[5],6828
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[6],6771
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[7],6818
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[8],6754
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[9],6809
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_EN[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_EN[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CARRYIN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[10],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[11],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[12],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[13],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[14],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[15],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[16],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[17],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[18],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[19],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[20],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[21],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[22],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[23],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[24],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[25],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[26],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[27],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[28],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[29],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[2],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[30],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[31],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[32],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[33],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[34],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[35],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[36],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[37],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[38],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[39],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[3],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[40],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[41],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[42],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[43],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[4],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[5],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[6],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[7],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[8],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[9],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[10],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[11],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[12],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[13],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[14],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[15],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[16],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[17],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[18],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[19],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[20],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[21],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[22],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[23],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[24],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[25],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[26],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[27],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[28],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[29],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[2],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[30],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[31],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[32],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[33],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[34],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[35],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[36],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[37],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[38],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[39],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[3],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[40],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[41],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[42],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[43],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[4],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[5],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[6],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[7],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[8],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[9],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_EN[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_EN[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:DOTP,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:OVFL_CARRYOUT_SEL,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[10],8717
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[11],8719
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[12],8717
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[13],8717
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[14],8716
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[15],8717
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[16],8712
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[17],8710
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[18],8686
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[19],8681
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[20],8684
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[21],8682
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[22],8683
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[23],8682
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[24],8677
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[25],8676
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[8],8723
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[9],8718
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_CLK[0],8710
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_CLK[1],8676
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_EN[0],8996
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_EN[1],9019
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SIMD,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_AD,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_AL_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_SD_N,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_SL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:D,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_FCINST1:CC,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_FCINST1:CO,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIN7339[11]:A,6293
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIN7339[11]:B,1364
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIN7339[11]:C,1434
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIN7339[11]:CC,1407
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIN7339[11]:D,5936
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIN7339[11]:P,1435
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIN7339[11]:S,1407
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIN7339[11]:UB,1364
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_11:B,6266
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_11:UB,6266
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:CLK,2039
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:Q,2039
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIRU1B[2]:A,1947
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIRU1B[2]:B,3874
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIRU1B[2]:Y,1947
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_11:B,2922
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_11:UB,2922
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[10]:A,5896
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[10]:B,6113
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[10]:C,2930
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[10]:D,2947
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[10]:Y,2930
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[15]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[15]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[15]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[15]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[15]:Y,261
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:CLK,7661
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:Q,7661
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:CLK,7653
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:D,6679
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:Q,7653
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:CLK,4131
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:Q,4131
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_242:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_242:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_242:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_242:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_242:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_72:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_72:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_72:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_72:IPA,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[10]:A,1760
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[10]:B,4469
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[10]:C,2948
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[10]:Y,1760
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_iv_0_o3[1]:A,4927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_iv_0_o3[1]:B,4522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_iv_0_o3[1]:C,4413
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_iv_0_o3[1]:Y,4413
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17:B,6299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17:UB,6299
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_4_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_4_0:B,6678
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_4_0:C,2882
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_4_0:CC,2752
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_4_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_4_0:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_4_0:S,2752
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_4_0:UB,2882
BLDC_Encoder_Axis_0/MSC_i_27/un1_s_state_3_0_a3:A,7805
BLDC_Encoder_Axis_0/MSC_i_27/un1_s_state_3_0_a3:B,7762
BLDC_Encoder_Axis_0/MSC_i_27/un1_s_state_3_0_a3:Y,7762
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_22:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_22:B,7786
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_22:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_22:CC,6753
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_22:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_22:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_22:S,6753
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_22:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:B,7863
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:C,6809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:D,7849
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPB,7863
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPC,6809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPD,7849
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[33]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[33]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[33]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[33]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[33]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:CLK,7657
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:Q,7657
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_19:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_19:IPENn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:CLK,5677
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:D,6818
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:Q,5677
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[15]:A,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[15]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[15]:C,5625
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[15]:Y,5150
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:C,6810
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPC,6810
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:CLK,6275
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:Q,6275
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o_1_sqmuxa_0_a2:A,5402
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o_1_sqmuxa_0_a2:B,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o_1_sqmuxa_0_a2:C,5469
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o_1_sqmuxa_0_a2:D,5025
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o_1_sqmuxa_0_a2:Y,3082
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[3]:A,6183
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[3]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[3]:Y,6183
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:CLK,6106
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:Q,6106
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]:C,4158
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]:D,4034
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[1]:Y,4034
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_15:A,7848
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_15:B,7409
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_15:CC,6906
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_15:S,6906
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_15:UB,7409
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[1]:A,5416
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[1]:B,5076
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[1]:C,7449
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[1]:Y,5076
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:CLK,4105
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:D,6720
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:Q,4105
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[0]:A,7938
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[0]:B,2525
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[0]:C,7829
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[0]:Y,2525
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[7]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[7]:B,7033
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[7]:C,7131
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[7]:CC,6921
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[7]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[7]:P,7033
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[7]:S,6921
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[19]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[19]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[19]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_29:A,1070
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_29:B,738
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_29:C,631
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_29:D,518
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_29:Y,518
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:CLK,5811
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:Q,5811
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:CLK,7352
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:Q,7352
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_4:B,6062
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_4:UB,6062
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1FL0C[32]:A,2473
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1FL0C[32]:B,1777
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1FL0C[32]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1FL0C[32]:CC,1372
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1FL0C[32]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1FL0C[32]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1FL0C[32]:S,1372
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI1FL0C[32]:UB,1777
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_8:B,6166
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_8:C,6274
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_8:CC,6111
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_8:P,6166
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_8:S,6111
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_8:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2_i_m2[11]:A,4634
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2_i_m2[11]:B,2098
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2_i_m2[11]:C,2054
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2_i_m2[11]:Y,2054
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[15]:A,2307
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[15]:B,2386
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[15]:Y,2307
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:D,8668
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:D,8671
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:C,6807
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPC,6807
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_14:B,7067
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_14:C,7126
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_14:CC,6750
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_14:P,7067
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_14:S,6750
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:CLK,3846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:Q,3846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:CO,3468
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[0],4181
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[1],3743
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[2],3824
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[3],3570
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[6],3559
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[7],3468
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[8],3496
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:P[9],3601
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[0],4843
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[10],5127
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[11],5248
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[1],4938
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[2],5062
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[3],4981
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[4],5019
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[5],5111
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[6],5002
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[7],5060
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[8],5168
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_0:UB[9],5109
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIG02IF[13]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIG02IF[13]:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIG02IF[13]:C,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIG02IF[13]:CC,2807
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIG02IF[13]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIG02IF[13]:P,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIG02IF[13]:S,2807
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIG02IF[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIHJ862[18]:A,4535
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIHJ862[18]:B,3553
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIHJ862[18]:C,3509
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIHJ862[18]:Y,3509
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[13]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[13]:B,5007
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[13]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[13]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[13]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[10]:A,1298
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[10]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[10]:Y,1298
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[6]:A,6139
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[6]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[6]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[6]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[6]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[15]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[15]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[15]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[15]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[1]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[1]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[1]:C,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[1]:Y,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0:B,6754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0:C,4588
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0:CC,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0:D,2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0:S,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0:UB,2456
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNI9UPU1[3]:A,6885
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNI9UPU1[3]:B,5829
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNI9UPU1[3]:C,6770
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNI9UPU1[3]:Y,5829
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[12]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[12]:B,7083
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[12]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[12]:CC,7061
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[12]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[12]:P,7083
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[12]:S,7061
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[12]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_16:A,5946
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_16:B,5442
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_16:CC,5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_16:S,5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_16:UB,5442
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_67:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_67:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_67:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_67:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_67:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[7]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[7]:B,7103
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[7]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[7]:CC,7069
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[7]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[7]:P,7103
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[7]:S,7069
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:CLK,7714
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:Q,7714
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[4]:A,4344
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[4]:B,4253
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[4]:C,4057
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[4]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[4]:Y,4057
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14]:B,6013
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14]:C,6291
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14]:CC,5696
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14]:P,6013
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14]:S,5696
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14]:UB,
MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2[0]:A,4345
MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2[0]:B,4210
MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2[0]:C,4046
MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2[0]:D,3090
MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2[0]:Y,3090
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:CLK,4669
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:D,5759
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:Q,4669
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[15]:A,5950
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[15]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[15]:Y,5950
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_53:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_53:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_53:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_53:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_53:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[13]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[13]:B,4416
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[13]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[13]:Y,91
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:CLK,6810
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:Q,6810
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[0],6966
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[10],6753
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[11],6692
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[1],6888
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[2],6830
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[3],6920
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[4],6849
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[5],6788
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[6],6917
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[7],6801
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[8],6740
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CC[9],6835
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CI,6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:CO,6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[0],6940
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[1],6877
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[2],7060
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[3],7036
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[6],7048
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[7],7097
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[8],7167
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:P[9],7154
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[10]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[10]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[10]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[10]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_33_0:A,2965
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_33_0:B,2401
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_33_0:C,2472
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_33_0:CC,235
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_33_0:D,1124
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_33_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_33_0:S,235
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_33_0:UB,2519
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_11_0:A,2595
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_11_0:B,7024
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_11_0:C,6553
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_11_0:CC,1762
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_11_0:D,4395
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_11_0:P,2595
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_11_0:S,1762
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_11_0:UB,4395
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_13:B,5173
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_13:C,5008
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_13:CC,4170
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_13:S,4170
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_183:A,5727
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_183:B,5685
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_183:C,5371
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_183:Y,5371
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_38:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_38:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_38:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_38:IPA,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux:A,5015
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux:B,4731
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux:C,2010
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux:D,1877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux:Y,1877
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_ia_0_sqmuxa_0_a3_0_a3:A,6731
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_ia_0_sqmuxa_0_a3_0_a3:B,6628
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_ia_0_sqmuxa_0_a3_0_a3:C,6588
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_ia_0_sqmuxa_0_a3_0_a3:Y,6588
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:CLK,6062
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:D,7873
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:Q,6062
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_start_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI72HT[28]:A,3953
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI72HT[28]:B,3643
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI72HT[28]:C,3831
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI72HT[28]:Y,3643
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:CLK,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:Q,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:CLK,3581
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:Q,3581
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9ALM9[27]:A,1657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9ALM9[27]:B,324
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9ALM9[27]:C,1023
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9ALM9[27]:Y,324
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_5:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_5:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_5:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_5:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[32]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[32]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[32]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[32]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[9]:A,4348
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[9]:B,4264
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[9]:C,4107
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[9]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[9]:Y,4107
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:CLK,6859
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:Q,6859
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]:A,3568
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]:B,2849
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]:C,5115
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]:D,4991
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[13]:Y,2849
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[6]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_279:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_279:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_279:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_279:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_279:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_9:A,4049
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_9:B,6127
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_9:P,4049
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_9:UB,6127
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:C,6833
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPC,6833
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_29:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[37]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[37]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[37]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[37]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:C,6818
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_15:IPC,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_0:B,1374
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_0:C,1213
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_0:CC,1670
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_0:P,1213
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_0:S,1670
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13:A,3524
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13:B,2794
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13:CC,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13:S,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13:UB,2794
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[4]:A,5413
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[4]:B,2764
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[4]:C,3131
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[4]:D,3001
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[4]:Y,2764
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_4:B,5019
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_4:UB,5019
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[5]:A,4753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[5]:B,4706
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[5]:C,4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[5]:Y,4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_0_sqmuxa_0_a3:A,6540
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_0_sqmuxa_0_a3:B,6460
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_0_sqmuxa_0_a3:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_0_sqmuxa_0_a3:D,6640
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_0_sqmuxa_0_a3:Y,6460
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:CLK,6795
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:Q,6795
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[12]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[12]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[12]:C,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[12]:Y,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:CLK,3946
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:D,8854
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:Q,3946
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[8]:A,1908
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[8]:B,2780
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[8]:C,5069
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[8]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[8]:D,4923
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[8]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[8]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[8]:Y,1908
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_NXT_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_NXT_PAD/U_IOINFF:Y,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8:A,6959
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8:B,3644
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8:C,3582
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8:CC,3441
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8:P,3582
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8:S,3441
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_8:UB,3594
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[37]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[37]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[37]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[37]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[37]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0:A,1980
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0:B,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0:P,1894
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0:UB,1775
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[11]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[11]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[11]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[11]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[11]:Y,261
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI25PR1[8]:A,4569
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI25PR1[8]:B,3587
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI25PR1[8]:C,3543
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI25PR1[8]:Y,3543
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[33]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[33]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[33]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[33]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o_0_sqmuxa_0_a2:A,5611
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o_0_sqmuxa_0_a2:B,5983
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o_0_sqmuxa_0_a2:C,3202
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o_0_sqmuxa_0_a2:D,5073
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o_0_sqmuxa_0_a2:Y,3202
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_3_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_3_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_3_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_3_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT4N33[1]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT4N33[1]:B,3789
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT4N33[1]:C,7023
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT4N33[1]:CC,5320
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT4N33[1]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT4N33[1]:P,3789
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT4N33[1]:S,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT4N33[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_11:B,6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_11:UB,6303
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[10],3454
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[11],3393
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[1],4108
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[2],4044
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[3],3772
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[4],3704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[5],3654
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[6],3592
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[7],3501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[8],3441
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CC[9],3538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:CO,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[0],3256
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[1],3348
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[2],3434
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[3],3456
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[6],3384
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[7],3500
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[8],3582
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:P[9],3619
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[0],3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[10],3516
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[11],3651
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[1],3372
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[2],3408
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[3],3341
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[4],3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[5],3520
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[6],3268
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[7],3487
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[8],3594
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_0:UB[9],3536
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o_0_sqmuxa:A,7688
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o_0_sqmuxa:B,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o_0_sqmuxa:Y,7611
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:D,5257
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:CLK,2323
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:D,6067
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:Q,2323
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:CLK,4389
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:D,4348
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:Q,4389
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[9]:A,5996
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[9]:B,5925
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[9]:C,4423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[9]:D,5415
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[9]:Y,4423
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[0],3315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[1],3245
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[2],3197
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[3],3263
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[4],3199
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[5],3150
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[6],3251
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[7],3129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[8],3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CC[9],3165
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:CI,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[0],3764
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[1],3775
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[2],3940
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[3],3959
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[6],4995
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[7],5194
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[0],3643
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[1],3762
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[2],3942
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[3],3860
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[4],3898
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[5],4968
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[6],4897
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[7],4771
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[8],5701
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_2:UB[9],
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[2]:A,6137
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[2]:B,7896
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[2]:C,4624
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[2]:D,5829
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[2]:Y,4624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[5]:A,5871
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[5]:B,5798
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[5]:C,4298
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[5]:D,5286
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[5]:Y,4298
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:CLK,5316
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:Q,5316
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[11]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_15:A,2441
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_15:B,2458
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_15:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_15:IPA,2441
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_15:IPB,2458
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:CLK,6903
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:D,6940
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:Q,6903
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIVPGT[24]:A,3855
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIVPGT[24]:B,3536
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIVPGT[24]:C,3729
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIVPGT[24]:Y,3536
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:CLK,6833
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:Q,6833
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_7:A,3109
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_7:B,2981
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_7:P,3047
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_7:UB,2981
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_12:B,4680
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_12:C,4525
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_12:CC,4276
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_12:P,4525
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_12:S,4276
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CC[6],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CC[7],1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:CI,1273
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[0],1375
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[1],1249
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[2],1362
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[3],1432
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[6],1793
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[0],1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[1],1258
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[2],1328
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[3],1314
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[4],1282
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[5],1334
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[6],1774
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[12]:A,6048
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[12]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[12]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[12]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[12]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_18:B,6509
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_18:C,4256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_18:IPB,6509
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_18:IPC,4256
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:CLK,4829
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:D,7161
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:Q,4829
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[4]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[4]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[4]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[4]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[4]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[4]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[4]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:D,6618
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:CLK,4012
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:Q,4012
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_12:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_12:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[5]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[5]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[5]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_30:A,7316
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_30:B,7130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_30:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_30:CC,6862
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_30:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_30:P,7230
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_30:S,6862
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_30:UB,7130
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:CLK,6717
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:D,7114
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:Q,6717
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[2]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_50:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_50:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_50:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_50:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_97:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_97:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_97:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_97:IPA,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[4]:A,6985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[4]:B,6901
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[4]:C,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[4]:Y,6226
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_9:B,5295
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_9:CC,5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_9:P,5295
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_9:S,5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_12:A,3056
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_12:B,4575
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_12:P,3056
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_12:UB,4575
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI77662[11]:A,4441
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI77662[11]:B,3459
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI77662[11]:C,3341
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI77662[11]:Y,3341
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:C,6717
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:IPC,6717
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:CLK,2005
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:D,1817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:Q,2005
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:CLK,6804
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:Q,6804
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_21:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_21:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[13]:A,5853
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[13]:B,6058
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[13]:C,2882
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[13]:D,2904
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[13]:Y,2882
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_15:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_15:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_15:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_15:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_15:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_15:IPC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[15]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[15]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[15]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[1]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[1]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[1]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_4:B,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_4:S,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:CLK,6149
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:Q,6149
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI89NK1[9]:A,2575
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI89NK1[9]:B,2342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI89NK1[9]:C,2453
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI89NK1[9]:Y,2342
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:CLK,4004
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:D,8717
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:Q,4004
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6:A,7100
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6:B,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6:CC,5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6:P,5181
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6:S,5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6:UB,5092
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[11]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[11]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[11]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[11]:CC,6960
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[11]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[11]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[11]:S,6960
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o[17]:A,1671
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o[17]:B,705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o[17]:C,2219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o[17]:D,2139
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o[17]:Y,705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[15]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17_FCINST1:CC,4089
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17_FCINST1:CO,4089
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]:A,2561
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]:B,2054
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]:C,4314
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]:D,4196
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[11]:Y,2054
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[23]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[23]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[23]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[23]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[23]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_16:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_16:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:B,7837
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:C,6835
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:D,7852
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPB,7837
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPC,6835
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPD,7852
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:CLK,3522
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:Q,3522
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[1]:A,4823
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[1]:C,5816
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[1]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[1]:D,5683
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[1]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[1]:Y,4823
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:CLK,5606
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:Q,5606
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:CLK,6802
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:Q,6802
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_5:A,7911
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_5:B,7408
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_5:C,7836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_5:D,7801
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_5:Y,7408
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:CLK,1699
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:D,8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:Q,1699
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[3]:Y,4589
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[4]:A,4523
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[4]:B,1987
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[4]:C,1943
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[4]:Y,1943
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[14]:A,1379
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[14]:B,5107
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[14]:Y,1379
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:CLK,5956
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:D,8704
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:Q,5956
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_0_sqmuxa:A,4478
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_0_sqmuxa:B,5891
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_0_sqmuxa:Y,4478
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[16]:A,1795
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[16]:B,2667
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[16]:C,4964
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[16]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[16]:D,4804
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[16]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[16]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[16]:Y,1795
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[0]:A,7938
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[0]:B,6809
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[0]:C,7856
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count_3[0]:Y,6809
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:CLK,4176
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:D,8677
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:Q,4176
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_12:B,7127
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_12:C,7047
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_12:CC,3661
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_12:D,5453
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_12:P,5453
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_12:S,3661
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:D,5440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_15:A,6834
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_15:B,6791
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_15:C,5623
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_15:D,5543
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_15:Y,5543
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_17:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_17:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_o2[18]:A,3820
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_o2[18]:B,6096
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_o2[18]:Y,3820
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:CC[0],3511
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:CC[1],3384
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:CC[2],3469
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:CC[3],3574
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:CC[6],3755
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:CI,3384
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[0],3764
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[1],3915
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[3],4086
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_iout_i_m2[16]:A,499
BLDC_Encoder_Axis_0/MSC_i_11/s_iout_i_m2[16]:B,422
BLDC_Encoder_Axis_0/MSC_i_11/s_iout_i_m2[16]:C,-143
BLDC_Encoder_Axis_0/MSC_i_11/s_iout_i_m2[16]:Y,-143
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_182:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_182:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_182:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_182:IPA,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[4]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[4]:B,7661
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[4]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[4]:CC,6996
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[4]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[4]:P,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[4]:S,6996
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_11:A,2957
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_11:B,2830
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_11:C,2690
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_11:D,2687
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_11:Y,2687
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:CLK,2277
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:Q,2277
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:CLK,477
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:D,8677
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:Q,477
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:IPENn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_2:A,1579
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_2:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_2:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_2:IPA,1579
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:CLK,1226
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:D,1407
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:Q,1226
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:CLK,6047
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:D,7781
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:Q,6047
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]:A,2988
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]:B,3382
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]:C,5206
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]:D,5082
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]:Y,2988
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:CLK,5064
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:Q,5064
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_s_17:B,6434
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_s_17:C,6389
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_s_17:CC,5442
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_s_17:S,5442
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_s_17:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:CLK,4615
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:Q,4615
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:D,3315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:CLK,6757
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:D,5483
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:Q,6757
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_30:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_30:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[10],2739
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[11],2678
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[1],5602
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[2],3272
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[3],2872
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[4],2805
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[5],2752
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[6],2879
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[7],2787
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[8],2726
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CC[9],2823
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:CO,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[0],4998
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[1],2637
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[2],2864
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[3],2879
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[6],2891
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[7],2901
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[8],2971
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:P[9],2997
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[0],6321
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[10],2898
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[11],3019
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[1],2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[2],2833
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[3],2747
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[4],2780
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[5],2882
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[6],2773
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[7],2831
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[8],2930
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_0:UB[9],2880
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISSLU[1]:A,6960
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISSLU[1]:B,6588
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISSLU[1]:C,6506
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISSLU[1]:Y,6506
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:CLK,1722
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:Q,1722
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:Q,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_11:B,2180
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_11:UB,2180
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIO86S[1]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIO86S[1]:B,7108
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIO86S[1]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIO86S[1]:CC,7384
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIO86S[1]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIO86S[1]:P,7108
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIO86S[1]:S,7384
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIO86S[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[16]:A,1978
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[16]:B,3348
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[16]:C,5091
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[16]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[16]:D,4938
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[16]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[16]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[16]:Y,1978
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[7]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[7]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[7]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[7]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_34:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_34:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRO7H5[14]:A,6991
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRO7H5[14]:B,1304
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRO7H5[14]:C,1379
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRO7H5[14]:CC,1417
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRO7H5[14]:D,5876
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRO7H5[14]:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRO7H5[14]:S,1417
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRO7H5[14]:UB,1304
BLDC_Encoder_Axis_0/MSC_i_11/s_error_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_s_17:B,7786
BLDC_Encoder_Axis_0/MSC_i_11/s_error_s_17:C,7723
BLDC_Encoder_Axis_0/MSC_i_11/s_error_s_17:CC,6793
BLDC_Encoder_Axis_0/MSC_i_11/s_error_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_s_17:S,6793
BLDC_Encoder_Axis_0/MSC_i_11/s_error_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_30:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_30:IPENn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:CLK,5902
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:Q,5902
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_5:B,6060
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_5:C,6168
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_5:CC,6167
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_5:P,6060
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_5:S,6167
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[8]:A,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[8]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[8]:C,5786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[8]:Y,5143
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:CLK,3275
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:Q,3275
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[5]:A,1912
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[5]:B,2784
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[5]:C,5078
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[5]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[5]:D,4927
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[5]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[5]:Y,1912
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[17]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[17]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[17]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[17]:Y,3435
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_4_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_4_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_4_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_4_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_17:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_17:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15:A,3695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15:B,3197
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15:CC,2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15:S,2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15:UB,3197
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_63:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_63:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_63:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_63:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_63:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO[0]:A,5067
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO[0]:B,7483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO[0]:Y,5067
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[10]:A,7964
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[10]:B,7880
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[10]:Y,7880
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state_0_sqmuxa:A,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state_0_sqmuxa:B,7444
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state_0_sqmuxa:Y,6699
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[1]:A,5928
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[1]:B,5821
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[1]:C,4669
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[1]:Y,4669
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:CC[0],3661
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:CC[1],3583
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:CC[2],3525
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:CC[3],3615
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:CC[4],3544
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:CC[5],3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:CI,3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[0],5453
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[1],5360
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[2],5511
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[3],5763
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[4],5908
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:B,7895
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:C,6795
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:IPB,7895
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:IPC,6795
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:CLK,6828
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:Q,6828
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_8:A,7022
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_8:B,6918
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_8:CC,6927
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_8:P,6986
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_8:S,6927
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_8:UB,6918
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[6]:A,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[6]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[6]:C,5750
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[6]:Y,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_1_0:A,7106
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_1_0:B,6588
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_1_0:C,1877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_1_0:CC,2430
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_1_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_1_0:P,1908
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_1_0:S,2430
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_1_0:UB,1877
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_15:A,4360
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_15:B,6235
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_15:P,4360
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_15:UB,6235
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:CLK,7203
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:Q,7203
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[14]:A,5611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[14]:B,2206
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[14]:C,2251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[14]:D,2047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[14]:Y,2047
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:CLK,6286
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:Q,6286
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m22:A,4976
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m22:B,1991
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m22:C,1926
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m22:Y,1926
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[0]:A,6926
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[0]:B,7926
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[0]:C,2491
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[0]:D,4638
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[0]:Y,2491
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[1]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[1]:B,7115
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[1]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[1]:CC,7504
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[1]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[1]:P,7115
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[1]:S,7504
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:CLK,4942
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:D,8682
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:Q,4942
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[13]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_140:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_140:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_140:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_140:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_140:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7_RNO[17]:A,2199
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7_RNO[17]:B,2274
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7_RNO[17]:C,6860
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7_RNO[17]:CC,1343
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7_RNO[17]:D,6686
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7_RNO[17]:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7_RNO[17]:S,1343
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7_RNO[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o_1_sqmuxa_i:A,7792
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o_1_sqmuxa_i:B,7749
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o_1_sqmuxa_i:C,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o_1_sqmuxa_i:D,7584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o_1_sqmuxa_i:Y,5103
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_169:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_169:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_169:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_169:IPA,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_10:B,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_10:UB,4242
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4:A,3696
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4:B,2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4:CC,2916
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4:S,2916
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4:UB,2727
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_32:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_32:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_bm[12]:A,4413
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_bm[12]:B,1875
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_bm[12]:C,1830
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_bm[12]:Y,1830
BLDC_Encoder_Axis_0/MSC_i_27/done_o_RNO:A,7909
BLDC_Encoder_Axis_0/MSC_i_27/done_o_RNO:B,7839
BLDC_Encoder_Axis_0/MSC_i_27/done_o_RNO:Y,7839
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_239:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_239:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_239:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_239:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_239:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:CLK,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:D,6990
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:Q,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:CLK,5064
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:D,6960
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:Q,5064
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[26]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[26]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[26]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[26]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:CLK,2770
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:D,1629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:Q,2770
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[5]:A,2120
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[5]:B,4190
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[5]:C,3623
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[5]:Y,2120
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2:A,6122
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2:B,6074
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2:C,3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2:D,4496
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2:Y,3654
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[27]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[27]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[27]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[27]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[27]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:C,6754
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_16:IPC,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]:A,2014
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]:B,2524
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]:C,4212
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]:D,4095
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]:Y,2014
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[10],3621
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[11],3560
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[1],4130
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[2],4066
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[3],3794
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[4],3726
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[5],3676
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[6],3761
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[7],3669
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[8],3608
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CC[9],3705
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:CO,3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[0],3526
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[1],3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[2],3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[3],3642
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[6],3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[7],3691
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[8],3761
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:P[9],3760
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[0],4429
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[10],4722
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[11],4835
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[1],4523
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[2],4657
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[3],4561
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[4],4594
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[5],4701
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[6],4597
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[7],4654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[8],4744
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_CC_0:UB[9],4704
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:CLK,7869
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:Q,7869
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:B,7866
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:C,6747
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:IPB,7866
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:IPC,6747
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:CLK,180
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:D,7084
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:Q,180
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[8]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[2]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[2]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[2]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_12:A,1144
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_12:B,1213
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_12:P,1144
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_12:UB,1213
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto34:A,259
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto34:B,182
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto34:C,1200
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto34:D,1093
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto34:Y,182
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_12_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_12_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_12_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_12_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_12_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:CLK,6062
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:D,8678
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:Q,6062
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:CLK,6096
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:Q,6096
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[14]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[14]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[14]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_21:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_21:B,7154
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_21:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_21:CC,6835
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_21:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_21:P,7154
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_21:S,6835
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_21:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o_1_sqmuxa_0_a2_0:A,2368
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o_1_sqmuxa_0_a2_0:B,2368
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o_1_sqmuxa_0_a2_0:Y,2368
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[8]:A,5031
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[8]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[8]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[8]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[8]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[3]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[3]:B,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[3]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[3]:CC,7164
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[3]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[3]:P,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[3]:S,7164
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:CLK,7480
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:D,7068
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:Q,7480
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:C,6705
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:IPC,6705
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[1]:A,6655
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[1]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[1]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[1]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[1]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[8]:A,5978
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[8]:B,5907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[8]:C,4405
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[8]:D,5401
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[8]:Y,4405
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[17]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[17]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[17]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[17]:Y,6726
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[19]:A,224
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[19]:B,147
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[19]:C,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[19]:Y,-393
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_34:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_34:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]:A,2686
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]:B,1967
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]:C,4233
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]:D,4109
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]:Y,1967
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:B,7774
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:C,6818
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:IPB,7774
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:CLK,4214
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:Q,4214
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[3]:A,3868
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[3]:B,6237
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[3]:C,2896
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[3]:D,3625
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[3]:Y,2896
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:CLK,4664
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:Q,4664
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:C,6705
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:IPC,6705
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_RNO:A,5320
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_RNO:Y,5320
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:CC[6],5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:CI,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[0],6198
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[1],6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[3],6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[0],6037
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[1],6137
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[2],6286
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[3],6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[4],6220
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[5],6299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:CLK,6697
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:Q,6697
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:CLK,1553
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:D,8679
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:Q,1553
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_11:B,6334
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_11:UB,6334
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:CLK,7742
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:Q,7742
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_15_0:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_15_0:B,6883
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_15_0:C,5733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_15_0:CC,5230
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_15_0:D,7184
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_15_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_15_0:S,5230
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_15_0:UB,5733
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_4:A,7808
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_4:B,7060
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_4:C,6626
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_4:CC,6583
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_4:S,6583
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_4:UB,6626
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIRQKU[1]:A,6826
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIRQKU[1]:B,6468
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIRQKU[1]:C,6385
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIRQKU[1]:Y,6385
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_60:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_60:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_60:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_60:IPA,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIU0MTE[11]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIU0MTE[11]:B,3876
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIU0MTE[11]:C,7040
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIU0MTE[11]:CC,3852
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIU0MTE[11]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIU0MTE[11]:P,3876
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIU0MTE[11]:S,3852
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIU0MTE[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_24:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_24:B,7077
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_24:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_24:CC,6781
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_24:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_24:P,7077
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_24:S,6781
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_24:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[5]:A,4516
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[5]:B,2120
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[5]:C,4391
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[5]:Y,2120
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8]:B,5841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8]:C,6112
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8]:CC,5786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8]:P,5841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8]:S,5786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:CLK,6212
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:D,8671
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:Q,6212
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:B,7671
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:C,6810
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:D,7661
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPB,7671
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPC,6810
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPD,7661
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[5]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_ac0_3:A,7034
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_ac0_3:B,6950
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_ac0_3:C,6892
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_ac0_3:Y,6892
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_93:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_93:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_93:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_93:IPA,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:CLK,1440
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:D,1233
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:Q,1440
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:D,8854
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/s_mas_done_dly[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0:A,-143
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0:B,1125
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0:C,600
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0:CC,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0:D,871
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0:P,-143
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0:UB,600
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0:Y,870
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:CLK,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:Q,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[12]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_147:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_147:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_147:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_147:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_147:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:B,7859
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:C,6747
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:IPB,7859
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:IPC,6747
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_9_162_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_9_162_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_9_162_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_9_162_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:CLK,6810
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:Q,6810
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_1:B,6792
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_1:C,6853
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_1:CC,7252
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_1:P,6792
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_1:S,7252
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_1:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[2]:A,4226
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[2]:B,1830
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[2]:C,4101
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[2]:Y,1830
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:C,6745
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:IPC,6745
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[2]:A,7017
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[2]:B,6962
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[2]:C,1540
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[2]:Y,1540
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:CLK,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:D,7028
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:Q,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[17]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[17]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[17]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[22]:A,263
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[22]:B,186
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[22]:C,-354
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[22]:Y,-354
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO:A,5579
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO:B,5528
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO:C,3657
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO:D,3570
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO:Y,3570
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:C,6733
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:IPC,6733
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[6]:A,1902
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[6]:B,3272
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[6]:C,5016
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[6]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[6]:D,4862
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[6]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[6]:Y,1902
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_255:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_255:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_255:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_255:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_255:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_8:A,6253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_8:B,6212
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_8:P,6237
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_8:UB,6212
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:CLK,6724
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:D,7460
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:Q,6724
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[2]:A,5837
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[2]:B,5759
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[2]:C,4271
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[2]:D,5247
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[2]:Y,4271
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:CLK,3904
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:Q,3904
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNILCCG2[8]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNILCCG2[8]:B,7202
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNILCCG2[8]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNILCCG2[8]:CC,7066
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNILCCG2[8]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNILCCG2[8]:P,7202
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNILCCG2[8]:S,7066
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNILCCG2[8]:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_209:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_209:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_209:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_209:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_209:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:CLK,4387
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:D,5767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:Q,4387
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:CLK,1994
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:D,8677
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:Q,1994
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_22:B,6576
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_22:C,4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_22:IPB,6576
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_22:IPC,4407
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:CLK,2074
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:Q,2074
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:CLK,5712
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:D,6781
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:Q,5712
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:D,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:D,5257
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:CLK,7815
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:Q,7815
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[4]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[4]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[4]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:D,5143
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_16_0:A,2254
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_16_0:B,1028
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_16_0:C,1440
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_16_0:CC,-277
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_16_0:D,-140
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_16_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_16_0:S,-277
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_16_0:UB,-140
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:D,6566
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_13:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_13:IPENn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:CLK,5718
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:Q,5718
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17:B,5100
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_17:UB,5100
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[15]:A,1971
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[15]:B,2843
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[15]:C,5132
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[15]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[15]:D,4986
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[15]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[15]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[15]:Y,1971
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:C,6804
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPC,6804
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:CLK,6036
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:Q,6036
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_15:B,5344
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_15:C,5179
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_15:CC,4360
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_15:S,4360
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_15:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_173:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_173:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_173:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_173:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_173:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:CLK,7884
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:Q,7884
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13:A,6900
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13:B,3570
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13:C,3527
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13:CC,3431
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13:P,3527
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13:S,3431
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13:UB,3551
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:D,4108
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_13:A,6234
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_13:B,4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_13:P,4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_13:UB,4130
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[3]:A,2587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[3]:B,5813
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[3]:Y,2587
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:CLK,2202
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:D,5966
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:Q,2202
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:CLK,7841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:D,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:Q,7841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[17]:A,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[17]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[17]:C,5685
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[17]:Y,5018
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2:A,1539
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2:B,1465
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2:CC,1748
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2:P,1490
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2:S,1748
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2:UB,1465
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m10_0_03_1_1:A,3915
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m10_0_03_1_1:B,3838
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m10_0_03_1_1:C,3565
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m10_0_03_1_1:D,3463
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m10_0_03_1_1:Y,3463
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:CLK,421
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:D,6857
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:Q,421
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:CLK,3919
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:D,2745
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:Q,3919
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]:A,2674
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]:B,2167
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]:C,4427
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]:D,4309
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]:Y,2167
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[26]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[26]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[26]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[26]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[14]:A,6092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[14]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[14]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[14]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[14]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:D,2865
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:CLK,2804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:D,1678
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:Q,2804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:C,6698
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:IPC,6698
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[10]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[10]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[10]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[10]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_6_195_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_6_195_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_6_195_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_6_195_i_m2:Y,7698
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1_1[13]:A,4295
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1_1[13]:B,4998
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1_1[13]:C,2803
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1_1[13]:D,4326
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1_1[13]:Y,2803
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_3:A,4855
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_3:B,2948
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_3:P,3065
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_3:UB,2948
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:CLK,1908
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:Q,1908
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[5]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[5]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[5]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[5]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[13]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[13]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[13]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[13]:CC,6983
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[13]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[13]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[13]:S,6983
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIPLIT[30]:A,3998
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIPLIT[30]:B,3687
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIPLIT[30]:C,3876
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIPLIT[30]:Y,3687
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[13]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[13]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[13]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:CLK,6757
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:Q,6757
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:CLK,3904
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:D,6776
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:Q,3904
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:CLK,7299
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:Q,7299
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:CLK,4923
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:Q,4923
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir_47_1:A,5981
BLDC_Encoder_Axis_0/MSC_i_23/s_dir_47_1:B,6801
BLDC_Encoder_Axis_0/MSC_i_23/s_dir_47_1:C,5835
BLDC_Encoder_Axis_0/MSC_i_23/s_dir_47_1:Y,5835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:CLK,3773
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:D,6874
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:Q,3773
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[27]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_223:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_223:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_223:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_223:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_223:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI34MU[1]:A,6808
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI34MU[1]:B,6450
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI34MU[1]:C,6354
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI34MU[1]:Y,6354
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7:A,6877
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7:B,3543
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7:C,3487
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7:CC,3501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7:P,3500
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7:S,3501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_7:UB,3487
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:B,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:C,6791
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:IPC,6791
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en_RNO:A,6834
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en_RNO:B,7517
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en_RNO:Y,6834
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[3]:A,6484
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[3]:B,7047
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[3]:C,6581
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[3]:CC,5753
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[3]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[3]:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[3]:S,5753
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[3]:UB,6581
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:CLK,6811
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:D,6873
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:Q,6811
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[2]:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[2]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[2]:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[2]:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[2]:Y,-247
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[1]:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[1]:C,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[1]:D,4034
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[1]:Y,4034
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:B,7849
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:C,6818
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:IPB,7849
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_9:B,3661
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_9:CC,3601
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_9:P,3661
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_9:S,3601
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:CLK,186
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:D,7056
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:Q,186
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:CLK,4657
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:D,7123
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:Q,4657
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:CO,3044
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[0],4554
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[1],3280
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[2],3361
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[3],3107
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[6],3135
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[7],3044
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[8],3072
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:P[9],3177
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[0],4407
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[10],4704
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[11],4825
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[1],4515
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[2],4639
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[3],4558
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[4],4596
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[5],4688
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[6],4579
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[7],4637
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[8],4745
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0_CC_0:UB[9],4686
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:CLK,3322
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:EN,3182
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:Q,3322
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[1]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_27:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_27:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_27:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_27:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_27:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[4]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[4]:B,4766
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[4]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[4]:Y,91
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[5]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_90:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_90:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_90:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_90:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_90:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:D,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]:A,2893
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]:B,3287
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]:C,5111
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]:D,4987
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]:Y,2893
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_7:A,6952
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_7:B,6828
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_7:CC,6987
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_7:P,6916
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_7:S,6987
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_7:UB,6828
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:CLK,5332
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:Q,5332
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[7]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15:A,2107
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15:B,1908
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15:CC,1314
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15:P,2028
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15:S,1314
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15:UB,1908
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:C,6762
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:IPC,6762
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[2]:A,6594
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[2]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[2]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[2]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[2]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:CLK,1840
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:D,8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:Q,1840
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[41]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_12:A,5384
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_12:B,5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_12:CC,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_12:P,5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_12:S,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_12:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_272:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_272:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_272:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_272:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_272:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:D,6583
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[0]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[0]:B,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[0]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[0]:CC,7565
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[0]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[0]:P,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[0]:S,7565
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:CLK,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:Q,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:CLK,4228
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:D,8683
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:Q,4228
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_14:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_14:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[16]:A,3830
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[16]:B,3753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[16]:C,3315
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[16]:Y,3315
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_194:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_194:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_194:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_194:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_194:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_1:A,3743
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_1:B,4938
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_1:P,3743
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_1:UB,4938
A0_PWM_VL_O_obuf/U0/U_IOOUTFF:A,2345
A0_PWM_VL_O_obuf/U0/U_IOOUTFF:Y,2345
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO:A,5474
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO:B,5436
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO:C,3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO:D,3503
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO:Y,3324
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:CLK,6745
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:D,5166
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:Q,6745
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:CLK,4454
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:D,8689
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:Q,4454
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:B,7714
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:C,6747
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:IPB,7714
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:IPC,6747
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[13]:A,5199
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[13]:B,2803
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[13]:C,5074
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[13]:Y,2803
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[9]:A,6027
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[9]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[9]:Y,6027
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:CLK,695
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:D,8678
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:Q,695
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[43]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:CLK,5002
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:D,3860
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:Q,5002
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:CLK,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:Q,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_226:A,6181
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_226:B,4701
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_226:C,6059
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_226:Y,4701
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:CLK,6731
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:D,3615
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:Q,6731
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[3]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[3]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[3]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[3]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:D,3538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:B,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:C,6791
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_1:IPC,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:CLK,6828
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:Q,6828
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:CLK,6603
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:D,7923
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:Q,6603
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_15:A,2682
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_15:B,2763
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_15:C,1540
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_15:D,1870
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_15:Y,1540
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[9]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[9]:B,7160
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[9]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[9]:CC,7105
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[9]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[9]:P,7160
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[9]:S,7105
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[8]:A,3534
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[8]:B,4909
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[8]:C,2472
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[8]:D,3224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[8]:Y,2472
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[6]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[6]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[6]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:CLK,7086
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:Q,7086
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:CC[0],2943
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:CC[1],2865
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:CC[2],2807
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:CC[3],2897
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:CC[4],2826
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:CC[5],2765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:CC[6],2886
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:CI,2765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[0],2825
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[1],2903
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[3],3074
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:B,7946
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:C,6763
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:IPB,7946
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:IPC,6763
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc1:A,7938
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc1:B,7903
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc1:Y,7903
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]:Y,4589
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_125:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_125:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_125:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_125:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_125:IPB,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:CLK,1953
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:D,6944
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:Q,1953
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_9:A,3177
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_9:B,4686
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_9:P,3177
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_9:UB,4686
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[0]:A,1741
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[0]:B,3811
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[0]:C,3244
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[0]:Y,1741
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:CLK,4756
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:D,6813
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:Q,4756
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[43]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[43]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[43]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:CLK,7836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:D,7682
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:Q,7836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_park_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:CLK,1512
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:Q,1512
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:CLK,5112
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:Q,5112
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:CLK,3551
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:Q,3551
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO_0:A,5646
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO_0:B,5552
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO_0:C,3672
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO_0:D,3615
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18_RNO_0:Y,3615
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:CLK,6802
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:Q,6802
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:CLK,7723
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:Q,7723
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:CLK,1831
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:D,7066
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:Q,1831
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:D,8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_7:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_7:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_7:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_7:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_7:IPC,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIJBK8B[8]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIJBK8B[8]:B,3953
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIJBK8B[8]:C,7117
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIJBK8B[8]:CC,3896
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIJBK8B[8]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIJBK8B[8]:P,3953
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIJBK8B[8]:S,3896
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIJBK8B[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:CLK,4269
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:Q,4269
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_2_sqmuxa_i:A,5895
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_2_sqmuxa_i:B,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_2_sqmuxa_i:C,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_2_sqmuxa_i:Y,4108
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:CLK,6738
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:D,3560
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:Q,6738
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO:A,5393
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO:B,5345
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO:C,3427
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO:D,3411
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO:Y,3411
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:CLK,5839
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:Q,5839
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:CLK,6834
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:D,7473
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:Q,6834
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[3]:A,5870
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[3]:B,5792
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[3]:C,4304
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[3]:D,5280
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[3]:Y,4304
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[6]:A,6100
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[6]:B,6023
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[6]:C,5637
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[6]:D,4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[6]:Y,4407
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_44:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_44:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_44:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_44:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_44:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_227:A,6085
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_227:B,4594
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_227:C,5960
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_227:Y,4594
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_27:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_27:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:B,7694
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:C,6847
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:D,7727
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPB,7694
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPC,6847
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPD,7727
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:C,6690
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:IPC,6690
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:CLK,499
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:D,8712
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:Q,499
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:CLK,7832
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:Q,7832
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:CLK,7809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:Q,7809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_4:A,6027
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_4:B,5118
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_4:CC,5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_4:S,5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_4:UB,5118
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:D,5283
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_7:A,5357
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_7:B,5220
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_7:CC,5092
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_7:P,5308
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_7:S,5092
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_7:UB,5220
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:CLK,7866
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:Q,7866
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[12]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[12]:B,4861
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[12]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[12]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[12]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_9:A,2766
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_9:B,2771
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_9:P,2766
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_9:UB,2771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o_0_sqmuxa_0_a3:A,7669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o_0_sqmuxa_0_a3:B,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o_0_sqmuxa_0_a3:Y,7591
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_1:A,1806
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_1:B,1688
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_1:P,1688
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_1:UB,1699
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_11:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_11:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_11:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_11:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:CLK,5008
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:Q,5008
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:CLK,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:Q,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17:B,3581
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17:UB,3581
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:CLK,4537
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:Q,4537
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[3]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:CLK,5073
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:Q,5073
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:D,2950
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:CLK,6772
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:D,7049
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:Q,6772
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_3_0:A,1471
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_3_0:B,775
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_3_0:C,1187
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_3_0:CC,1323
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_3_0:D,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_3_0:P,-257
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_3_0:S,1323
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_3_0:UB,-393
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:D,5427
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[20]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[20]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[20]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[16]:A,5686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[16]:B,2285
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[16]:C,2342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[16]:D,2122
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[16]:Y,2122
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[9]:A,6272
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[9]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[9]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[9]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[9]:Y,2538
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]:A,1978
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]:B,2488
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]:C,4176
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]:D,4059
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]:Y,1978
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[11]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[11]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[11]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:B,7912
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:C,6844
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:D,7877
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPB,7912
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPC,6844
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPD,7877
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3_RNILBQT:A,7918
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3_RNILBQT:B,7896
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3_RNILBQT:C,6439
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3_RNILBQT:D,7702
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3_RNILBQT:Y,6439
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[7]:A,6287
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[7]:B,6203
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[7]:C,5528
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[7]:Y,5528
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_24:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_24:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[4]:A,7100
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[4]:B,5052
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[4]:C,4819
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[4]:CC,4883
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[4]:D,6595
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[4]:P,4927
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[4]:S,4883
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[4]:UB,4819
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[11]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[11]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[11]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[17]:A,6861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[17]:B,6814
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[17]:C,6101
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[17]:Y,6101
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[8]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[8]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[8]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[8]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[8]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[8]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[8]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_1:A,5574
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_1:B,5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_1:CC,6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_1:P,5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_1:S,6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_1:UB,5512
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[32]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:CLK,4858
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:Q,4858
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[36]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[36]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[36]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[36]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[36]:Y,224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[6]:A,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[6]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[6]:C,5750
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[6]:Y,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:CLK,5670
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:D,8667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:Q,5670
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:CLK,1524
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:Q,1524
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_2:A,4170
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_2:B,6080
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_2:P,4170
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_2:UB,6080
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2:A,5182
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2:B,5434
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2:C,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2:D,5150
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2:Y,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]:A,2583
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]:B,2076
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]:C,4336
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]:D,4218
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[5]:Y,2076
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4:B,5216
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4:CC,4619
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4:S,4619
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10:A,7808
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10:B,7090
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10:CC,6918
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10:S,6918
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_10:UB,7090
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNO[18]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNO[18]:B,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNO[18]:C,7716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNO[18]:CC,3674
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNO[18]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNO[18]:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNO[18]:S,3674
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNO[18]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:D,8854
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/s_mas_done_dly[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_75:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_75:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_75:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_75:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_75:IPB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[11]:A,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[11]:B,7920
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[11]:C,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[11]:Y,7659
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14:A,7808
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14:B,7160
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14:CC,6851
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14:S,6851
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_14:UB,7160
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_133:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_133:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_133:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_133:IPA,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_20:A,7152
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_20:B,7049
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_20:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_20:CC,6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_20:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_20:P,7096
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_20:S,6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_20:UB,7049
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIB8IB2[17]:A,3069
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIB8IB2[17]:B,2785
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIB8IB2[17]:C,4224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIB8IB2[17]:Y,2785
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:CLK,6156
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:Q,6156
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[2]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:CLK,5956
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:Q,5956
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI6SG0E[8]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI6SG0E[8]:B,4459
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI6SG0E[8]:C,7295
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI6SG0E[8]:CC,4351
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI6SG0E[8]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI6SG0E[8]:P,4459
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI6SG0E[8]:S,4351
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI6SG0E[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0:A,4387
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0:B,5861
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0:P,4387
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0:UB,5861
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[6]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[6]:B,4952
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[6]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[6]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[6]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_8:A,7206
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_8:B,7074
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_8:C,6624
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_8:CC,6654
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_8:P,6745
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_8:S,6654
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_8:UB,6624
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:D,6630
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:CLK,4724
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:D,6974
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:Q,4724
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:CLK,6697
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:D,3794
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:Q,6697
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO:A,2015
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO:B,5698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO:C,1967
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO:D,1885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO:Y,1885
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_15:A,5150
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_15:B,4944
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_15:P,5064
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_15:UB,4944
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[16]:A,4290
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[16]:B,1967
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[16]:C,1978
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[16]:Y,1967
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:C,6755
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_34:IPC,6755
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[15]:A,6485
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[15]:B,6437
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[15]:C,5733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[15]:Y,5733
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_1:A,4218
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_1:B,4146
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_1:P,4146
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_1:UB,4181
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_3:A,6232
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_3:B,4290
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_3:P,4380
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_3:UB,4290
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[2]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[2]:B,7091
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[2]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[2]:CC,7232
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[2]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[2]:P,7091
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[2]:S,7232
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[26]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[26]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[26]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1_0[7]:A,3880
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1_0[7]:B,2684
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1_0[7]:C,4193
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1_0[7]:D,4108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1_0[7]:Y,2684
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO:A,5701
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO:B,5653
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO:C,3796
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO:D,3716
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO:Y,3716
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0:A,4633
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0:B,4407
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0:P,4554
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_0:UB,4407
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[10]:A,6001
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[10]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[10]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[10]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[10]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:CLK,3087
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:Q,3087
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:CO,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[0],5948
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[1],4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[2],4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[3],4380
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[6],4293
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[7],4268
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[8],4278
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:P[9],4362
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[0],5796
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[10],4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[11],4287
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[1],4640
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[2],4722
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[3],4290
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[4],4253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[5],4299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[6],4230
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[7],4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[8],4244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_0:UB[9],4308
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:C,6685
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_28:IPC,6685
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIK3RN2[9]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIK3RN2[9]:B,7792
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIK3RN2[9]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIK3RN2[9]:CC,6982
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIK3RN2[9]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIK3RN2[9]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIK3RN2[9]:S,6982
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIK3RN2[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:D,5114
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[3]:A,5178
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[3]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[3]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[3]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[3]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNILCVH1[12]:A,1546
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNILCVH1[12]:B,1454
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNILCVH1[12]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNILCVH1[12]:CC,5599
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNILCVH1[12]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNILCVH1[12]:P,1497
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNILCVH1[12]:S,5599
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNILCVH1[12]:UB,1454
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:CLK,6889
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:D,7020
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:Q,6889
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[9]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:CLK,5942
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:Q,5942
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:CLK,5846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:Q,5846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:CO,1088
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[0],1188
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[1],1088
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[2],1275
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[3],1190
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[6],1154
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[7],1127
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[8],1270
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:P[9],1218
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[0],1670
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[10],1350
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[11],1557
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[1],1700
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[2],1574
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[3],1398
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[4],1381
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[5],1523
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[6],1330
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[7],1323
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[8],1510
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_0:UB[9],1397
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:CC[6],4089
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:CI,4207
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[0],4195
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[1],4089
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[3],4279
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[0],6016
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[1],6112
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[2],6238
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[3],6167
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[4],6208
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[5],4283
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:CLK,7009
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:D,6879
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:Q,7009
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[7]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[7]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[7]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[7]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:CLK,6774
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:D,7057
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:Q,6774
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:CLK,6818
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:Q,6818
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:CLK,6001
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:Q,6001
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[9]:A,3395
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[9]:B,4773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[9]:C,2336
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[9]:D,3088
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[9]:Y,2336
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_23:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_23:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_23:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_23:IPB,
QB_I_ibuf/U0/U_IOINFF:A,6192
QB_I_ibuf/U0/U_IOINFF:Y,6192
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:CLK,7144
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:D,6840
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:Q,7144
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[6]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[6]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[6]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[6]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[6]:Y,261
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:CLK,5033
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:Q,5033
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:CLK,7584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:D,8847
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:EN,7398
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:Q,7584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/done_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:CLK,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:D,7164
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:Q,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:CLK,8854
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:D,7485
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:EN,7714
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:Q,8854
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mas_en:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9]:B,6473
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9]:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9]:CC,5702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9]:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9]:S,5702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:CLK,3973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:Q,3973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[10],5727
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[11],5666
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[2],6277
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[3],5877
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[4],5810
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[5],5753
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[6],5867
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[7],5775
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[8],5714
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CC[9],5811
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:CO,5588
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[0],6667
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[1],5588
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[2],5748
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[3],5732
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[6],5746
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[7],5767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[8],5849
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:P[9],5852
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[0],6533
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[10],6597
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[11],6718
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[1],5606
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[2],6532
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[3],6451
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[4],6489
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[5],6581
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[6],6472
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[7],6530
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[8],6638
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy_CC_0:UB[9],6579
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[4]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[4]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[4]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[4]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:D,5376
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[12]:A,6011
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[12]:B,2800
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[12]:C,2626
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[12]:D,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[12]:Y,1584
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_4:B,2916
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_4:UB,2916
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_7:A,1544
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_7:B,1273
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_7:P,1322
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_7:UB,1273
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:CLK,7879
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:Q,7879
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[15]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_232:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_232:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_232:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_232:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_232:IPB,
A0_PWM_UH_O_obuf/U0/U_IOENFF:A,
A0_PWM_UH_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[9]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[9]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[9]:C,5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[9]:Y,5240
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CC[6],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CC[7],3384
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:CI,3468
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[0],3511
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[1],3384
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[2],3469
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[3],3574
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[6],3829
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[0],5029
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[1],5124
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[2],5249
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[3],5167
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[4],5205
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[5],5297
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[6],3755
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_29:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_29:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:D,5143
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:CLK,6757
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:Q,6757
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[4]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[4]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[4]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[4]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_3:A,4508
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_3:B,4260
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_3:CC,4290
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_3:P,4389
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_3:S,4290
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_3:UB,4260
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_16:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_16:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:CO,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[0],6006
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[1],5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[2],6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[3],6115
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[6],6127
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[7],6167
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[8],6237
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:P[9],6233
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[0],5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[10],6197
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[11],6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[1],5991
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[2],6137
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[3],6029
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[4],6062
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[5],6169
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[6],6068
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[7],6122
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[8],6212
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0_CC_0:UB[9],6183
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[0]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[0]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[0]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[0]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m31_0:A,4575
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m31_0:B,1947
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m31_0:C,4684
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m31_0:Y,1947
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:CLK,6771
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:Q,6771
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[6]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[5]:A,7055
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[5]:B,6005
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[5]:C,6986
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[5]:Y,6005
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_3:A,4962
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_3:B,4790
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_3:P,4876
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_3:UB,4790
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_8_0:A,7226
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_8_0:B,6676
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_8_0:C,2880
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_8_0:CC,2823
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_8_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_8_0:P,2997
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_8_0:S,2823
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_8_0:UB,2880
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1[16]:A,2718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1[16]:B,2725
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1[16]:C,1799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1[16]:D,2468
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1[16]:Y,1799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[13]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[13]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[13]:C,5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[13]:Y,5118
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO:A,5703
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO:B,5655
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO:C,3798
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO:D,3651
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO:Y,3651
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:CLK,4105
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:Q,4105
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[3]:A,3888
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[3]:B,2430
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[3]:C,2962
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[3]:D,1539
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_0[3]:Y,1539
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0:A,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0:B,4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0:C,5511
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0:P,5150
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0:UB,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0:Y,4087
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_14:B,4791
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_14:C,4630
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_14:P,4630
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_14:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[26]:A,392
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[26]:B,315
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[26]:C,-225
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[26]:Y,-225
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:D,5257
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[9]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_1_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_1_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_1_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_1_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[10],6940
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[11],6879
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[1],7544
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[2],7480
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[3],7136
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[4],7066
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[5],7005
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[6],7057
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[7],6987
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[8],6927
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CC[9],7020
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:CO,6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[0],6755
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[1],6705
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[2],6879
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[3],6864
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[6],6876
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[7],6916
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[8],6986
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:P[9],6982
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[0],6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[10],6903
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[11],7009
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[1],6697
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[2],6843
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[3],6735
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[4],6768
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[5],6875
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[6],6774
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[7],6828
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[8],6918
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0_CC_0:UB[9],6889
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0:A,4734
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0:B,3535
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0:P,3682
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0:UB,3535
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_19:A,2442
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_19:B,2480
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_19:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_19:IPA,2442
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_19:IPB,2480
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:CLK,4276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:Q,4276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:CLK,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:Q,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[11]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_103:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_103:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_103:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_103:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_103:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIO6FH2[10]:A,3463
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIO6FH2[10]:B,4474
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIO6FH2[10]:C,3488
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIO6FH2[10]:Y,3463
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:D,3654
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_2:A,4645
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_2:B,4555
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_2:C,4244
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_2:Y,4244
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:CLK,3764
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:Q,3764
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:CC[6],5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:CI,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[0],6198
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[1],6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[3],6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[0],6037
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[1],6137
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[2],6286
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[3],6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[4],6220
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[5],6299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:D,3251
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:CLK,7694
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:Q,7694
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[1]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:CLK,5277
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:Q,5277
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_7:B,6899
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_7:C,6959
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_7:CC,6743
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_7:P,6899
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_7:S,6743
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:D,2807
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[14]:A,4877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[14]:B,4793
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[14]:C,4374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[14]:Y,4374
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP:B,2319
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP:C,1248
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP:P,1248
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP:UB,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[3]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[3]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[3]:Y,7568
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[7]:A,2167
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[7]:B,4312
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[7]:C,1809
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[7]:D,2003
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[7]:Y,1809
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN:A,
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN:B,5950
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN:C,5855
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN:CC,
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN:D,
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN:P,6928
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN:UB,
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN:Y,5855
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:CLK,6802
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:Q,6802
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[4]:A,4102
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[4]:B,1779
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[4]:C,1790
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[4]:Y,1779
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:CLK,6828
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:Q,6828
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[5]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_260:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_260:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_260:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_260:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_260:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:CLK,3726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:D,7027
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:Q,3726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIPEBLI[14]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIPEBLI[14]:B,4020
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIPEBLI[14]:C,7184
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIPEBLI[14]:CC,3806
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIPEBLI[14]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIPEBLI[14]:P,4020
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIPEBLI[14]:S,3806
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIPEBLI[14]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI33LU[1]:A,6906
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI33LU[1]:B,6533
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI33LU[1]:C,6452
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI33LU[1]:Y,6452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:D,8716
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[14]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_189:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_189:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_189:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_189:IPA,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_1:A,6002
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_1:B,5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_1:P,5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_1:UB,5991
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:CLK,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:D,6759
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:Q,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sckctr_done:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[32]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[32]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[32]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[3]:A,4705
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[3]:B,4657
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[3]:C,4211
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[3]:Y,4211
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o_1_sqmuxa_0_a2_0:A,6851
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o_1_sqmuxa_0_a2_0:B,6816
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o_1_sqmuxa_0_a2_0:C,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o_1_sqmuxa_0_a2_0:Y,6734
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:CLK,6037
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:D,8673
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:Q,6037
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22:B,3863
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22:C,3740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22:CC,3267
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22:S,3267
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22:UB,3740
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_224:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_224:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_224:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_224:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_224:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:CLK,7879
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:Q,7879
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[13]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[13]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[13]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[13]:Y,6732
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[8]:A,5542
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[8]:B,2893
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[8]:C,3260
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[8]:D,3130
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[8]:Y,2893
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_20:A,2469
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_20:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_20:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_20:IPA,2469
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_20:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_3:B,6837
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_3:CC,7195
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_3:P,6837
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_3:S,7195
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[34]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[34]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[34]:Y,7555
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o_0_sqmuxa_0_a2:A,7844
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o_0_sqmuxa_0_a2:B,7801
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o_0_sqmuxa_0_a2:C,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o_0_sqmuxa_0_a2:Y,6734
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0:B,6513
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0:C,4347
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0:CC,2254
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0:D,2047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0:S,2254
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0:UB,2047
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[2]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[2]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[2]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[2]:Y,6726
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_34:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_34:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_34:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_34:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:CLK,6810
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:Q,6810
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_17:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_17:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_10:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_10:B,7075
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_10:CC,6927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_10:S,6927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_10:UB,7075
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[3]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[3]:B,4834
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[3]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[3]:Y,91
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:D,5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[4]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[4]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[4]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[4]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_15:A,1438
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_15:B,3209
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_15:P,1438
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_15:UB,3209
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[12]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[12]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[12]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[12]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[12]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[12]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[12]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[12]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[4]:A,1356
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[4]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[4]:Y,1356
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:CLK,6735
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:D,7136
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:Q,6735
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:CLK,4931
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:Q,4931
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[12]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_202:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_202:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_202:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_202:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_202:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv[16]:A,1384
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv[16]:B,3571
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv[16]:C,1226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv[16]:Y,1226
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_170:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_170:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_170:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_170:IPA,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_3:A,7808
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_3:B,6953
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_3:C,6531
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_3:CC,6636
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_3:P,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_3:S,6636
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_3:UB,6531
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_32:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_32:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_20:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_20:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIV3B62[26]:A,4641
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIV3B62[26]:B,3659
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIV3B62[26]:C,3615
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIV3B62[26]:Y,3615
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:CLK,6711
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:D,3583
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:Q,6711
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[27]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[27]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[27]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[3]:A,6265
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[3]:B,6181
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[3]:C,5481
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[3]:Y,5481
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:CLK,1501
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:D,8681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:Q,1501
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_20:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_20:IPENn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:C,6807
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPC,6807
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1_0:A,5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1_0:B,6365
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1_0:C,6825
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1_0:CC,5963
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1_0:P,5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1_0:S,5963
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1_0:UB,6825
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[13]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[13]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[13]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:C,6754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:D,5222
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:CLK,5037
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:D,8711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:Q,5037
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:CLK,6940
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:D,6966
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:Q,6940
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[12]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_166:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_166:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_166:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_166:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[10]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_4:A,1668
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_4:B,1606
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_4:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_4:IPA,1668
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_4:IPB,1606
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:CLK,7444
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:D,6800
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:Q,7444
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:C,6807
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPC,6807
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_7:IPD,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_11_0:A,3246
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_11_0:B,1049
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_11_0:C,1461
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_11_0:CC,734
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_11_0:D,-119
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_11_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_11_0:S,734
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_11_0:UB,-119
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0:B,5889
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0:C,5997
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0:CC,6584
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0:P,5889
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0:S,6584
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:CLK,6046
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:Q,6046
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:CLK,3982
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:D,8681
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:Q,3982
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_12:A,6315
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_12:B,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_12:P,4273
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_12:UB,4108
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[14]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[14]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[14]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[14]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:B,7866
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:C,6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:IPB,7866
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:IPC,6747
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:CLK,2981
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:D,2726
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:Q,2981
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[0]:A,5907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[0]:B,5478
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[0]:C,5367
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[0]:D,4275
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[0]:Y,4275
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:CLK,6265
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:Q,6265
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIDT4O[6]:A,2938
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIDT4O[6]:B,2466
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIDT4O[6]:C,2823
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIDT4O[6]:Y,2466
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILRC62[28]:A,4669
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILRC62[28]:B,3687
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILRC62[28]:C,3643
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILRC62[28]:Y,3643
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIU5N97[23]:A,1589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIU5N97[23]:B,1510
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIU5N97[23]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIU5N97[23]:CC,5007
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIU5N97[23]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIU5N97[23]:P,1510
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIU5N97[23]:S,5007
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIU5N97[23]:UB,1516
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[15]:A,6484
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[15]:B,7242
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[15]:C,6767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[15]:CC,5589
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[15]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[15]:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[15]:S,5589
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[15]:UB,6767
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_9:A,2845
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_9:B,2797
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_9:C,2723
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_9:D,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_9:Y,2622
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[4]:A,2589
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[4]:B,1002
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[4]:C,7856
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[4]:D,7689
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0[4]:Y,1002
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:CLK,3048
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:D,2678
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:Q,3048
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_22:EN,8894
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_22:IPENn,8894
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[0]:A,5869
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[0]:B,5821
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[0]:C,5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[0]:Y,5116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:CLK,1830
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:D,5076
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:Q,1830
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:D,8671
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:D,6630
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:CLK,7113
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:Q,7113
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_26:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_26:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:CLK,2254
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:D,8680
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:Q,2254
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[12]:A,5934
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[12]:B,7143
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[12]:C,6688
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[12]:CC,5631
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[12]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[12]:P,5934
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[12]:S,5631
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[12]:UB,6688
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:C,6754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_17:IPD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:CLK,3543
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:Q,3543
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_7:A,4288
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_7:B,6146
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_7:P,4288
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_7:UB,6146
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done_RNO:A,7871
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done_RNO:B,7854
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_all_ch_done_RNO:Y,7854
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[10]:A,1529
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[10]:B,5257
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[10]:Y,1529
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:CLK,6772
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:D,5373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:Q,6772
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:C,6765
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:IPC,6765
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[23]:A,317
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[23]:B,240
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[23]:C,-300
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[23]:Y,-300
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[5]:A,5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[5]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[5]:C,5842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[5]:Y,5224
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIMN762[17]:A,4562
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIMN762[17]:B,3580
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIMN762[17]:C,3536
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIMN762[17]:Y,3536
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8:A,7180
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8:B,7131
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8:CC,6905
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8:P,7164
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8:S,6905
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8:UB,7131
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:CLK,4181
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:D,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:Q,4181
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_2_sqmuxa_i:A,5895
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_2_sqmuxa_i:B,4378
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_2_sqmuxa_i:C,5701
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_2_sqmuxa_i:D,5543
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_2_sqmuxa_i:Y,4378
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_267:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_267:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_267:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_267:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_267:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:CLK,6807
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:Q,6807
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12:A,7129
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12:B,7083
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12:CC,6965
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12:P,7083
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12:S,6965
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_12:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_177:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_177:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_177:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_177:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_177:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0:A,4641
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0:B,5861
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0:P,4641
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_0:UB,5861
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[15]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[15]:B,4448
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[15]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[15]:Y,91
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[14]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[14]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[14]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[14]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[4]:A,4729
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[4]:B,4686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[4]:C,4227
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[4]:Y,4227
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_3:A,3087
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_3:B,2902
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_3:P,2995
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_3:UB,2902
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CC[6],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CC[7],1261
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:CI,1352
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[0],1381
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[1],1261
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[2],1367
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[3],1438
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[6],1676
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[0],3071
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[1],3166
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[2],3291
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[3],3209
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[4],3247
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[5],3325
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[6],1592
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:C,6811
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:IPC,6811
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:D,5392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc_1_sqmuxa_1_i:A,5058
BLDC_Encoder_Axis_0/MSC_i_11/s_acc_1_sqmuxa_1_i:B,7250
BLDC_Encoder_Axis_0/MSC_i_11/s_acc_1_sqmuxa_1_i:C,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc_1_sqmuxa_1_i:D,247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc_1_sqmuxa_1_i:Y,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[0],463
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[10],1775
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[1],308
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[2],205
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[3],217
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[4],7
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[5],-102
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[6],-47
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[7],-247
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[8],185
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CC[9],235
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:CI,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[0],150
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[10],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[11],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[1],100
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[2],273
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[3],213
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[4],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[5],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[6],532
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[7],1036
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[8],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:P[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[0],-9
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[10],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[11],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[1],86
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[2],228
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[3],78
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[4],110
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[5],218
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[6],432
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[7],625
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[8],715
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_2:UB[9],2519
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:D,6570
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[11]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[11]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[11]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[11]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:CLK,7852
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:Q,7852
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[40]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:CLK,7916
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:D,8847
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:EN,7839
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:Q,7916
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_27/done_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[4]:A,5977
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[4]:B,5899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[4]:C,4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[4]:D,5387
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[4]:Y,4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[10]:A,2413
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[10]:B,5713
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[10]:C,2372
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[10]:Y,2372
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_4:A,5075
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_4:B,4293
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_4:CC,4253
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_4:S,4253
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_4:UB,4293
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_3_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_3_PAD/U_IOINFF:Y,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:CLK,5116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:Q,5116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:D,4995
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy:B,6667
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy:C,6863
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy:CC,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy:D,6533
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy:P,6667
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_lcry_cy:UB,6533
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:C,6752
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_12:IPC,6752
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:CLK,2831
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:D,3017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:Q,2831
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:B,7889
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:C,6814
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:IPB,7889
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:IPC,6814
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[3]:A,7808
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[3]:B,5767
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[3]:C,4928
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[3]:CC,4731
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[3]:D,6704
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[3]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[3]:S,4731
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[3]:UB,4928
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:D,8699
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:CLK,6705
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:D,3525
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:Q,6705
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11:S,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[16]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[16]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[16]:Y,5366
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:CLK,5907
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:Q,5907
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[7]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[7]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[7]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[4]:A,6254
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[4]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[4]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[4]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[4]:Y,2538
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_142:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_142:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_142:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_142:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:CLK,6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:D,5222
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:Q,6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:CLK,4140
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:Q,4140
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_5:B,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_5:CC,5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_5:S,5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_5:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:CLK,2336
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:Q,2336
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[13]:A,5919
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[13]:B,7112
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[13]:C,6637
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[13]:CC,5721
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[13]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[13]:P,5919
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[13]:S,5721
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[13]:UB,6637
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27:A,7245
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27:B,5740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27:C,3860
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27:CC,3263
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27:D,4651
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27:P,3959
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27:S,3263
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_27:UB,3860
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[10]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[10]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[10]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16:A,2280
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16:B,1945
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16:CC,1282
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16:S,1282
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16:UB,1945
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:CLK,7048
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:Q,7048
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SD_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[0],6737
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[10],6798
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[11],6718
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[12],6743
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[13],6691
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[14],6685
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[15],6711
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[16],6725
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[17],6742
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[1],6713
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[2],6704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[3],6677
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[4],6689
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[5],6713
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[6],6752
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[7],6727
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[8],6734
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[9],6727
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_EN[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_EN[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[0],6791
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[10],6802
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[11],6844
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[12],6795
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[13],6814
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[14],6833
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[15],6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[16],6835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[17],6804
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[1],6841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[2],6847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[3],6807
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[4],6810
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[5],6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[6],6771
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[7],6818
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[8],6754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[9],6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_EN[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_EN[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CARRYIN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[12],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[13],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[14],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[15],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[16],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[17],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[18],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[19],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[20],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[21],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[22],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[23],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[24],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[25],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[26],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[27],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[28],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[29],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[2],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[30],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[31],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[32],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[33],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[34],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[35],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[36],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[37],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[38],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[39],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[3],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[40],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[41],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[42],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[43],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[6],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[7],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[12],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[13],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[14],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[15],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[16],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[17],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[18],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[19],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[20],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[21],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[22],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[23],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[24],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[25],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[26],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[27],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[28],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[29],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[2],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[30],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[31],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[32],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[33],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[34],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[35],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[36],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[37],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[38],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[39],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[3],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[40],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[41],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[42],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[43],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[6],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[7],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_EN[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_EN[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:DOTP,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:OVFL_CARRYOUT_SEL,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[10],6893
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[11],6787
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[12],6818
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[13],6925
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[14],6824
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[15],6878
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[16],6964
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[17],6933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[18],6921
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[19],7023
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[20],6922
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[21],6834
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[22],6986
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[23],7237
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[24],7376
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[25],7547
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[8],6659
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[9],6748
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_CLK[0],6659
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_CLK[1],6834
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_EN[0],8969
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_EN[1],8992
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SIMD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_AD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_AL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_SD_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_SL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIBK0J[13]:A,2831
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIBK0J[13]:B,2754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIBK0J[13]:C,2318
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIBK0J[13]:Y,2318
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_15_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_15_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_15_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_15_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_15_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:CLK,6709
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:D,3726
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:Q,6709
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:CLK,4379
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:Q,4379
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[1]:A,4151
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[1]:C,5159
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[1]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[1]:D,5035
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[1]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[1]:Y,4151
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:CLK,7815
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:Q,7815
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU:A,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU:B,4220
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU:C,5637
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU:P,5159
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU:UB,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU:Y,4220
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:CLK,315
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:D,6918
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:Q,315
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:IPENn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:CLK,6068
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:D,8677
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:Q,6068
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:CLK,6973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:D,5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:Q,6973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9_0:A,5592
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9_0:B,6642
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9_0:C,6996
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9_0:CC,5537
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9_0:P,5592
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9_0:S,5537
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9_0:UB,6996
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_17:B,7786
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_17:CC,6788
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_17:S,6788
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_17:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:CLK,2337
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:Q,2337
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[9]:A,1359
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[9]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[9]:Y,1359
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[7]:A,6048
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[7]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[7]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[7]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[7]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[16]:A,3792
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[16]:B,2661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[16]:C,3830
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[16]:D,3753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[16]:Y,2661
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_6:A,3099
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_6:B,2923
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_6:P,3007
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_6:UB,2923
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm_RNO[13]:A,3647
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm_RNO[13]:B,5037
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm_RNO[13]:C,2598
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm_RNO[13]:D,3413
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm_RNO[13]:Y,2598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:CLK,5002
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:Q,5002
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12:A,2266
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12:B,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12:C,1028
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12:D,1645
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_12:Y,1028
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_27:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_27:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[40]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[40]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[40]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[40]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:CLK,3699
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:D,7796
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:Q,3699
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_state[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[7]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[7]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[7]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_27/s_state_108:A,7879
BLDC_Encoder_Axis_0/MSC_i_27/s_state_108:B,7876
BLDC_Encoder_Axis_0/MSC_i_27/s_state_108:C,7751
BLDC_Encoder_Axis_0/MSC_i_27/s_state_108:Y,7751
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_6:A,1613
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_6:B,1306
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_6:P,1402
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_6:UB,1306
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[36]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[36]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[36]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[36]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[14]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[14]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[14]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[14]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:CLK,4151
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:Q,4151
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[8]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[8]:B,7173
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[8]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[8]:CC,7008
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[8]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[8]:P,7173
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[8]:S,7008
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_s_17:B,7792
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_s_17:C,7547
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_s_17:CC,6659
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_s_17:S,6659
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0:A,5359
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0:B,6415
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0:C,6724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0:P,5359
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0:UB,6724
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_15:A,6420
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_15:B,4208
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_15:P,4332
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_15:UB,4208
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[31]:A,440
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[31]:B,363
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[31]:C,-177
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[31]:Y,-177
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[7]:A,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[7]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[7]:C,5689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[7]:Y,5204
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1:B,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1:CC,4893
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1:P,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1:S,4893
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1:UB,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_9_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_9_0:B,6694
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_9_0:C,2898
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_9_0:CC,2739
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_9_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_9_0:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_9_0:S,2739
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_9_0:UB,2898
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:CLK,6818
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:D,6911
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:Q,6818
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI5P7J[1]:A,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI5P7J[1]:B,1830
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI5P7J[1]:Y,1584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:D,8728
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:D,8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_16:A,7710
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_16:B,7540
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_16:CC,6836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_16:S,6836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_16:UB,7540
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFO0J[15]:A,2968
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFO0J[15]:B,2891
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFO0J[15]:C,2457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFO0J[15]:Y,2457
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_35:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_35:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[9]:A,6175
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[9]:B,6098
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[9]:C,5704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[9]:D,4482
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[9]:Y,4482
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:CLK,4054
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:Q,4054
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17:B,3204
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17:UB,3204
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:CLK,7057
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:Q,7057
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI6FI5G[12]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI6FI5G[12]:B,3860
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI6FI5G[12]:C,7026
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI6FI5G[12]:CC,3774
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI6FI5G[12]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI6FI5G[12]:P,3860
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI6FI5G[12]:S,3774
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI6FI5G[12]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[5]:A,6046
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[5]:B,5969
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[5]:C,5579
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[5]:D,4353
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[5]:Y,4353
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]:B,7013
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]:C,6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]:CC,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]:P,6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[13]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[15]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[15]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[15]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:CLK,4391
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:Q,4391
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:CLK,7853
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:Q,7853
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13:A,7808
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13:B,7034
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13:CC,6895
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13:S,6895
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13:UB,7034
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:CC[0],1945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:CC[1],1875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:CC[2],1817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:CC[3],1893
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:CC[4],1829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:CC[5],1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:CC[6],1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:CI,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[0],1870
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[1],3292
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[3],3432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[0],1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[1],6522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[2],6673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[3],6720
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[4],5116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[5],5228
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[22]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[22]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[22]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_15:EN,8996
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_15:IPENn,8996
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[13]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[13]:B,4791
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[13]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[13]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[13]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_23:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_23:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_3:A,5441
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_3:B,5141
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_3:CC,5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_3:P,5239
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_3:S,5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_3:UB,5141
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_216:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_216:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_216:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_216:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_216:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_216:IPC,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_130:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_130:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_130:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_130:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:CLK,4975
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:Q,4975
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[12]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[9]:A,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[9]:B,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[9]:C,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[9]:Y,7659
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_14:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_14:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_14:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_14:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_14:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_14:IPC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[8]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[8]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[8]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[8]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:CLK,5949
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:Q,5949
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0:A,7108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0:B,6480
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0:C,4314
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0:CC,2324
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0:D,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0:P,2153
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0:S,2324
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0:UB,2014
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:CLK,4984
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:Q,4984
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:CLK,3645
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:Q,3645
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4_0:A,6219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4_0:B,7274
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4_0:C,6906
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4_0:CC,5559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4_0:S,5559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4_0:UB,6906
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]:A,2631
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]:B,1912
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]:C,4178
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]:D,4054
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]:Y,1912
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:CLK,5830
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:Q,5830
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_RNO:A,2196
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_RNO:Y,2196
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[11]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[11]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[11]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[1]:A,6099
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[1]:B,6022
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[1]:C,5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[1]:Y,5315
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_6:A,2094
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_6:B,2006
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_6:Y,2006
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[9]:A,1841
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[9]:B,3215
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[9]:C,4918
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[9]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[9]:D,4794
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[9]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[9]:Y,1841
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[17]:A,2677
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[17]:B,3549
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[17]:C,5846
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[17]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[17]:D,5574
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[17]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[17]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[17]:Y,2677
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0:A,7149
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0:B,6617
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0:C,4451
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0:CC,2192
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0:D,2326
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0:P,2369
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0:S,2192
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0:UB,2326
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[10]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[10]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[10]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_17:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_17:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_0[2]:A,2264
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_0[2]:B,2251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_0[2]:Y,2251
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:CLK,7882
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:Q,7882
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:CLK,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:D,6743
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:Q,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_231:A,5913
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_231:B,4429
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_231:C,5791
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_231:Y,4429
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_14:B,6306
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_14:UB,6306
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[17]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[17]:B,7554
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[17]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[14]:A,6230
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[14]:B,6182
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[14]:C,5478
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[14]:Y,5478
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[4]:A,6048
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[4]:B,6004
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[4]:C,5288
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[4]:Y,5288
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:CLK,6238
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:Q,6238
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:B,7888
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:C,6795
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:IPB,7888
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:IPC,6795
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:CLK,6809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:Q,6809
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_s_17:B,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_s_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_s_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_s_17:S,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:CLK,1280
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:D,1346
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:Q,1280
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:CLK,3655
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:D,6988
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:Q,3655
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:CC[0],5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:CC[1],5212
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:CC[2],5158
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:CC[3],5230
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:CC[4],5166
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:CC[5],5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:CI,5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[0],5399
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[1],5340
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[2],5478
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[3],5733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[4],5861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5]:B,5735
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5]:C,6013
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5]:CC,5842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5]:P,5735
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5]:S,5842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_19_0:A,1818
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_19_0:B,1199
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_19_0:C,1272
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_19_0:CC,6
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_19_0:D,31
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_19_0:P,111
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_19_0:S,6
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_19_0:UB,31
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:D,6262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]:A,2627
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]:B,1908
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]:C,4174
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]:D,4050
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[8]:Y,1908
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:C,6737
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:IPC,6737
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_3:A,4034
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_3:B,1712
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_3:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_3:IPA,4034
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_3:IPB,1712
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[31]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[31]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[31]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[15]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[15]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[15]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[26]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[26]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[26]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[26]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[26]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_10:A,7835
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_10:B,6903
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_10:CC,6940
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_10:S,6940
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_10:UB,6903
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:CLK,3158
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:Q,3158
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:CLK,7714
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:Q,7714
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_axb_4_1:A,5422
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_axb_4_1:B,3564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_axb_4_1:C,3575
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_axb_4_1:Y,3564
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[15]:A,4231
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[15]:B,4147
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[15]:C,3957
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[15]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[15]:Y,3957
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0:A,4268
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0:B,4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0:P,4196
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0:UB,4087
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:CLK,4645
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:D,8854
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:Q,4645
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_47:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_47:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_47:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_47:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_2_0:A,5491
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_2_0:B,6503
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_2_0:C,5343
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_2_0:CC,5782
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_2_0:D,6804
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_2_0:P,5365
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_2_0:S,5782
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_2_0:UB,5343
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_5:B,1378
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_5:UB,1378
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_31:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_31:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_o2[5]:A,5073
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_o2[5]:B,1002
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_o2[5]:C,4976
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_o2[5]:Y,1002
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[16]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[9]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[9]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[9]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[41]:A,703
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[41]:B,560
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[41]:C,86
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[41]:Y,86
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6:B,2777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6:CC,2722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6:P,2777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6:S,2722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_3:A,5335
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_3:B,5127
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_3:CC,5292
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_3:P,5256
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_3:S,5292
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_3:UB,5127
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:B,7862
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:C,6705
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:IPB,7862
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:IPC,6705
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:CC[0],4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:CI,4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_13:A,5836
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_13:B,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_13:CC,5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_13:S,5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_13:UB,4995
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_3:A,6232
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_3:B,4290
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_3:P,4380
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_3:UB,4290
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[10],6940
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[11],6879
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[1],7544
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[2],7480
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[3],7136
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[4],7066
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[5],7005
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[6],7057
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[7],6987
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[8],6927
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CC[9],7020
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:CO,6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[0],6755
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[1],6705
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[2],6879
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[3],6864
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[6],6876
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[7],6916
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[8],6986
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:P[9],6982
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[0],6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[10],6903
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[11],7009
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[1],6697
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[2],6843
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[3],6735
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[4],6768
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[5],6875
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[6],6774
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[7],6828
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[8],6918
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_0_CC_0:UB[9],6889
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:CLK,2057
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:D,7120
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:Q,2057
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0_RNO:A,3893
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0_RNO:B,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0_RNO:C,6441
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0_RNO:D,4644
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0_RNO:Y,3893
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:CLK,6900
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:Q,6900
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:CLK,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:Q,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[12]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[12]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[12]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_11_0:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_11_0:B,6669
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_11_0:C,5529
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_11_0:CC,5174
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_11_0:D,6970
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_11_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_11_0:S,5174
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_11_0:UB,5529
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:CLK,5144
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:D,6920
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:Q,5144
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_14_0:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_14_0:B,6631
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_14_0:C,5478
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_14_0:CC,5158
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_14_0:D,6932
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_14_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_14_0:S,5158
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_14_0:UB,5478
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:D,8854
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/s_mas_done_dly[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:CLK,7611
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:D,7617
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:Q,7611
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:CLK,4400
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:D,4814
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:Q,4400
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:CO,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[0],6006
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[1],5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[2],6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[3],6115
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[6],6127
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[7],6167
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[8],6237
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:P[9],6233
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[0],5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[10],6197
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[11],6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[1],5991
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[2],6137
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[3],6029
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[4],6062
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[5],6169
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[6],6068
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[7],6122
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[8],6212
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_0_CC_0:UB[9],6183
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:CLK,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:D,7630
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:EN,7328
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:Q,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_137:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_137:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_137:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_137:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_137:IPB,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_9:A,5453
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_9:B,5281
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_9:CC,5282
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_9:P,5374
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_9:S,5282
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_9:UB,5281
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[11]:A,4983
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[11]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[11]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[11]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[11]:Y,2639
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_253:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_253:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_253:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_253:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_253:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_253:IPC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[20]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[20]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[20]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[20]:Y,3435
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:CLK,5984
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:Q,5984
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3SN81[10]:A,3008
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3SN81[10]:B,2931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3SN81[10]:C,2484
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3SN81[10]:Y,2484
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:CLK,2177
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:Q,2177
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:B,7853
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:C,6802
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:D,7832
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPB,7853
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPC,6802
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPD,7832
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[3]:A,4003
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[3]:B,1607
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[3]:C,3878
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[3]:Y,1607
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[9]:A,4750
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[9]:B,4702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[9]:C,4256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[9]:Y,4256
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_228:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_228:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_228:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_228:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_228:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_228:IPC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9:A,1672
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9:B,1512
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9:CC,1359
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9:P,1593
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9:S,1359
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9:UB,1512
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:C,6809
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPC,6809
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[12]:A,5532
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[12]:B,5829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[12]:C,4432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[12]:D,5270
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[12]:Y,4432
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_26:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_26:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO_0[0]:A,6140
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO_0[0]:B,5067
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO_0[0]:C,6849
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO_0[0]:D,6474
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO_0[0]:Y,5067
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[3]:A,7918
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[3]:B,7867
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[3]:C,6818
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[3]:D,6837
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[3]:Y,6818
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_100:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_100:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_100:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_100:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_100:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:C,6733
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:IPC,6733
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16:B,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_7:B,6170
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_7:C,6244
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_7:CC,6014
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_7:P,6170
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_7:S,6014
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:C,6798
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:IPC,6798
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_28_0:A,2730
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_28_0:B,1324
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_28_0:C,1397
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_28_0:CC,7
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_28_0:D,110
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_28_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_28_0:S,7
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_28_0:UB,110
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:CLK,3593
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:D,7467
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:Q,3593
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[41]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[41]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[41]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:CLK,1641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:D,8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:Q,1641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9P4O[4]:A,3067
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9P4O[4]:B,2990
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9P4O[4]:C,2543
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9P4O[4]:Y,2543
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[9]:A,4565
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[9]:B,2027
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[9]:C,1982
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[9]:Y,1982
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3RHI1[4]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3RHI1[4]:B,7792
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3RHI1[4]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3RHI1[4]:CC,6994
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3RHI1[4]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3RHI1[4]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3RHI1[4]:S,6994
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI3RHI1[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:CLK,5182
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:Q,5182
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:D,5283
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[6]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[6]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[6]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[30]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[30]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[30]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[30]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[10]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[10]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[10]:C,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[10]:Y,5156
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:CLK,5816
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:Q,5816
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[2]:A,7984
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[2]:B,7893
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[2]:C,6891
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[2]:Y,6891
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:CLK,4260
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:D,4731
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:Q,4260
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[9]:A,1818
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[9]:B,2697
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[9]:C,4963
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[9]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[9]:D,4839
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[9]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[9]:Y,1818
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2_RNO:A,5144
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2_RNO:B,3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2_RNO:C,5020
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_2_RNO:Y,3654
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[11]:A,1434
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[11]:B,5151
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[11]:Y,1434
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[20]:A,257
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[20]:B,180
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[20]:C,-360
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[20]:Y,-360
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0:A,3292
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0:B,6998
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0:C,6522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0:CC,1875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0:P,3292
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0:S,1875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_12_0:UB,6522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO:A,2108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO:B,2143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO:C,1947
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO:D,1875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO:Y,1875
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a2_2[4]:A,988
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a2_2[4]:B,4000
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a2_2[4]:Y,988
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:CLK,4358
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:D,8834
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:EN,7819
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:Q,4358
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_pi_done:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[0]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[0]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[0]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4_RNO:A,5834
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4_RNO:B,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4_RNO:C,5712
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_4_RNO:Y,4359
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[1]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:CLK,6738
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:Q,6738
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:CLK,2817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:Q,2817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:CLK,3748
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:D,8719
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:Q,3748
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI44LU[1]:A,6963
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI44LU[1]:B,6604
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI44LU[1]:C,6509
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI44LU[1]:Y,6509
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:CLK,6638
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:D,5637
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:Q,6638
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_present_state[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_13:A,2930
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_13:B,4671
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_13:P,2930
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_13:UB,4671
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[13]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[13]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[13]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[16]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[16]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[16]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_14:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_14:C,7716
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_14:CC,3525
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_14:D,5511
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_14:S,3525
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_14:UB,5511
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:D,6603
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:CLK,4991
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:Q,4991
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92O81[13]:A,3432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92O81[13]:B,3355
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92O81[13]:C,2892
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92O81[13]:Y,2892
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:CLK,6127
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:Q,6127
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:CLK,7716
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:D,6645
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:Q,7716
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:CLK,1651
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:Q,1651
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_221:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_221:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_221:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_221:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_221:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[1]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[1]:B,5663
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[1]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[1]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[1]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_s_30:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_s_30:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_s_30:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_s_30:CC,6732
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_s_30:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_s_30:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_s_30:S,6732
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_s_30:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[7]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_82:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_82:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_82:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_82:IPB,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_1:A,3317
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_1:B,1468
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_1:P,1470
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_1:UB,1468
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:B,7689
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:C,6772
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:IPB,7689
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:IPC,6772
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[16]:A,1839
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[16]:B,3909
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[16]:C,3342
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[16]:Y,1839
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_155:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_155:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_155:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_155:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:CLK,1612
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:Q,1612
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_10:B,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_10:CC,7065
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_10:S,7065
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:CLK,3169
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:D,2787
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:Q,3169
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNISVEE[9]:A,2895
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNISVEE[9]:B,2818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNISVEE[9]:C,2384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNISVEE[9]:Y,2384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIR19P1[12]:A,2377
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIR19P1[12]:B,2144
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIR19P1[12]:C,2255
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIR19P1[12]:Y,2144
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[5]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[5]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[5]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:CLK,1651
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:Q,1651
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[16]:A,4375
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[16]:B,1839
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[16]:C,1795
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[16]:Y,1795
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:CLK,4269
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:Q,4269
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[22]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[22]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[22]:Y,7440
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_107:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_107:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_107:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_107:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:B,7787
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:C,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:IPB,7787
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:C,6726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:IPC,6726
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]:A,2293
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]:B,1786
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]:C,4046
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]:D,3928
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]:Y,1786
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[2]:A,6484
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[2]:B,6940
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[2]:C,6489
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[2]:CC,5810
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[2]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[2]:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[2]:S,5810
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[2]:UB,6489
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_24:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_24:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[8]:A,6161
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[8]:B,6084
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[8]:C,5686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[8]:D,4468
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[8]:Y,4468
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_8:A,5411
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_8:B,5282
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_8:CC,5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_8:P,5315
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_8:S,5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_8:UB,5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:B,7730
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:C,6733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:IPB,7730
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:IPC,6733
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_28:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_28:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0:A,6814
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0:B,6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0:P,6755
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0:UB,6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_0:Y,7923
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:D,4995
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:CC[0],1573
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:CC[1],1445
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:CC[2],1532
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:CC[3],1636
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:CC[6],1774
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:CI,1445
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[0],1826
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[1],1935
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[3],2121
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_2_sqmuxa_i:A,5895
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_2_sqmuxa_i:B,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_2_sqmuxa_i:C,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_2_sqmuxa_i:Y,4108
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_16:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_16:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_16:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_16:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_16:IPC,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:CLK,1576
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:D,6014
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:Q,1576
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[36]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[36]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[36]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[36]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[36]:Y,88
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:CLK,6837
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:Q,6837
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_s_17:B,5691
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_s_17:C,5611
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_s_17:CC,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_s_17:S,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[2]:A,6033
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[2]:B,6238
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[2]:C,3062
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[2]:D,3084
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[2]:Y,3062
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[2]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m26_i_i_o2_i_o2:A,3741
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m26_i_i_o2_i_o2:B,3919
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m26_i_i_o2_i_o2:C,3851
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m26_i_i_o2_i_o2:Y,3741
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_79:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_79:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_79:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_79:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_79:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:D,5846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[7]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[7]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[7]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[7]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[7]:Y,261
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_9:A,2331
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_9:B,1877
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_9:C,1870
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_9:D,2041
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_9:Y,1870
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_24:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_24:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_4:A,5931
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_4:B,5160
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_4:CC,5141
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_4:S,5141
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_4:UB,5160
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[1]:A,6106
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[1]:B,6022
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[1]:C,5322
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[1]:Y,5322
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7:A,7110
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7:B,7023
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7:CC,6965
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7:P,7094
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7:S,6965
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_7:UB,7023
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:CLK,4691
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:D,7467
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:Q,4691
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_32:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_32:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:CLK,6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:Q,6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[7]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[7]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[7]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[7]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[7]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[7]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[7]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIPGLA1[0]:A,4964
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIPGLA1[0]:B,6424
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIPGLA1[0]:Y,4964
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_280:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_280:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_280:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_280:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_280:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_15:B,4086
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_15:CC,3574
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_15:P,4086
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_15:S,3574
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_15:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:CLK,7862
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:Q,7862
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[9]:A,1982
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[9]:B,2861
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[9]:C,5127
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[9]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[9]:D,4997
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[9]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[9]:Y,1982
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:CLK,5679
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:D,5855
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:Q,5679
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[34]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o_1_sqmuxa_0_a2:A,5499
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o_1_sqmuxa_0_a2:B,5886
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o_1_sqmuxa_0_a2:C,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o_1_sqmuxa_0_a2:D,5008
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o_1_sqmuxa_0_a2:Y,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:CLK,5077
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:D,8683
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:Q,5077
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[14]:A,3396
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[14]:B,3373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[14]:C,2208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[14]:D,3080
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[14]:Y,2208
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_14:B,1242
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_14:UB,1242
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:CLK,4937
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:D,5588
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:Q,4937
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_2:B,6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_2:CC,7467
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_2:P,6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_2:S,7467
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:B,7662
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:C,6724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:IPB,7662
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:IPC,6724
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17:B,6370
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17:UB,6370
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI7N4O[3]:A,3836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI7N4O[3]:B,3759
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI7N4O[3]:C,3284
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI7N4O[3]:Y,3284
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:CLK,6807
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:Q,6807
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[18]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[18]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[18]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[2]:A,6007
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[2]:B,5930
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[2]:C,5551
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[2]:D,4314
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[2]:Y,4314
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[17]:A,3919
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[17]:B,3440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[17]:C,3804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[17]:Y,3440
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:CLK,7867
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:D,6005
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:Q,7867
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_16:B,3247
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_16:UB,3247
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5_FCINST1:CC,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5_FCINST1:CO,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_2:A,1561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_2:B,1378
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_2:C,259
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_2:D,913
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_2:Y,259
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[1]:A,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[1]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[1]:C,6154
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[1]:Y,5675
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:D,4044
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_1:A,6073
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_1:B,4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_1:P,4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_1:UB,4640
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:CLK,6220
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:D,8671
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:Q,6220
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:CLK,6661
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:D,7699
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:Q,6661
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:D,8725
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:CLK,4753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:Q,4753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:CLK,7920
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:D,8814
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:EN,7792
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:Q,7920
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0:A,3132
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0:B,2901
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0:C,2843
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0:P,3010
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_0:UB,2843
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_0:B,4257
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_0:C,4089
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_0:CC,4641
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_0:P,4089
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_0:S,4641
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_0:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_43:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_43:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_43:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_43:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_43:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:CLK,1546
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:D,8686
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:Q,1546
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[7]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[7]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[7]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[7]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_s_17:B,7527
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_s_17:C,7547
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_s_17:CC,6739
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_s_17:S,6739
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_15:B,7036
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_15:CC,6920
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_15:P,7036
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_15:S,6920
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:CLK,6754
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:Q,6754
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[8]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:CLK,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:D,7880
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:EN,7792
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:Q,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_3[6]:A,3644
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_3[6]:B,2465
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_3[6]:C,6855
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_3[6]:D,3391
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2_3[6]:Y,2465
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:D,5427
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:CLK,1573
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:Q,1573
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[8]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[8]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[8]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0:A,5993
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0:B,5472
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0:P,5599
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0:UB,5472
A0_RUNNING_LED_obuf/U0/U_IOPAD:D,2053
A0_RUNNING_LED_obuf/U0/U_IOPAD:E,
A0_RUNNING_LED_obuf/U0/U_IOPAD:PAD,2053
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:CC[0],5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:CC[1],5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:CC[2],5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:CC[3],5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:CC[4],5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:CC[5],4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:CI,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[0],5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[1],4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[2],5211
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[3],5395
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[4],5442
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[4]:A,6940
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[4]:B,5912
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[4]:C,5826
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_0[4]:Y,5826
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:CLK,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:Q,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[6]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[6]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[6]:C,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[6]:Y,5296
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_19:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_19:B,7097
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_19:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_19:CC,6801
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_19:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_19:P,7097
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_19:S,6801
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_19:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:CLK,2765
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:D,8703
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:Q,2765
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[3]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_37:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_37:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_37:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_37:IPA,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[2]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[2]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[2]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[2]:Y,6726
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[8]:A,4512
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[8]:B,2116
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[8]:C,4387
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[8]:Y,2116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_3:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_3:C,4483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_3:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_3:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_3:IPC,4483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_3:IPD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[7]:A,6236
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[7]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[7]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[7]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[7]:Y,2538
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc5:A,7938
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc5:B,6892
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc5:C,7842
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc5:D,7742
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc5:Y,6892
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:CLK,1225
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:D,8719
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:Q,1225
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[11]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_186:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_186:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_186:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_186:IPA,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:D,8724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:CLK,6802
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:Q,6802
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[13]:A,3378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[13]:B,6667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[13]:C,3266
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[13]:Y,3266
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un109_s_state_0:A,7977
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un109_s_state_0:B,7893
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un109_s_state_0:C,7849
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un109_s_state_0:D,3828
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un109_s_state_0:Y,3828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9:B,2883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9:CC,2771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9:P,2883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9:S,2771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:CLK,4958
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:D,6830
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:Q,4958
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[11]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[11]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[11]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[11]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:CLK,5024
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:Q,5024
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:CLK,4819
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:Q,4819
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[5]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0_i_0:A,7951
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0_i_0:B,7903
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0_i_0:C,5483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0_i_0:D,6332
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0_i_0:Y,5483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:CLK,4851
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:D,6953
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:Q,4851
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:C,6762
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:IPC,6762
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_10:B,6145
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_10:UB,6145
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIFNCQ9[8]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIFNCQ9[8]:B,4465
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIFNCQ9[8]:C,7295
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIFNCQ9[8]:CC,4232
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIFNCQ9[8]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIFNCQ9[8]:P,4465
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIFNCQ9[8]:S,4232
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIFNCQ9[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[5]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[5]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[5]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[27]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[27]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[27]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[27]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_s_18:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_s_18:B,4465
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_s_18:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_s_18:CC,3755
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_s_18:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_s_18:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_s_18:S,3755
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_s_18:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:CLK,4734
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:D,7910
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:Q,4734
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[29]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[29]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[29]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[29]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[29]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[19]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[19]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[19]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[19]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:CLK,7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:Q,7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINHGT[20]:A,3768
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINHGT[20]:B,3456
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINHGT[20]:C,3646
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINHGT[20]:Y,3456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[2]:A,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[2]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[2]:C,5882
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[2]:Y,5614
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:CLK,4332
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:D,5727
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:Q,4332
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_16:B,7527
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_16:C,7548
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_16:CC,6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_16:S,6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16_FCINST1:CC,4283
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16_FCINST1:CO,4283
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_16_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[13]:A,2357
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[13]:B,5670
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[13]:C,2248
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[13]:Y,2248
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16:B,2274
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16:C,1882
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16:CC,1002
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16:S,1002
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:CLK,5226
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:Q,5226
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:CLK,1759
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:D,8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:Q,1759
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:CLK,1589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:D,8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:Q,1589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:CLK,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:Q,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI46ES2[9]:A,2761
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI46ES2[9]:B,2528
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI46ES2[9]:C,2639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI46ES2[9]:Y,2528
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:CLK,2088
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:D,7112
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:Q,2088
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:CLK,6711
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:D,5212
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:Q,6711
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[9]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[9]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[9]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[9]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[9]:Y,261
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:CLK,6640
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:D,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:Q,6640
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[34]:A,594
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[34]:B,451
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[34]:C,-23
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[34]:Y,-23
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15:S,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:C,6702
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_8:IPC,6702
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[6]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[6]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[6]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[6]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:CLK,6697
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:Q,6697
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:B,7815
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:C,6754
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:IPB,7815
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_16:B,4174
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_16:UB,4174
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNO[11]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNO[11]:B,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNO[11]:C,7703
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNO[11]:CC,4188
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNO[11]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNO[11]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNO[11]:S,4188
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNO[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_14:A,1532
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_14:B,1328
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_14:P,1362
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_14:UB,1328
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[7]:A,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[7]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[7]:C,5689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[7]:Y,5204
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[7]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[7]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[7]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[7]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:B,7714
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:C,6747
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:IPB,7714
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:IPC,6747
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_287:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_287:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_287:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_287:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_287:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNISKOKE[37]:A,1952
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNISKOKE[37]:B,1817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNISKOKE[37]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNISKOKE[37]:CC,1354
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNISKOKE[37]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNISKOKE[37]:P,1926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNISKOKE[37]:S,1354
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNISKOKE[37]:UB,1817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:D,6262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:CLK,6287
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:Q,6287
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:C,6747
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:IPC,6747
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_7:B,6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_7:CC,7112
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_7:P,6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_7:S,7112
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:CLK,7485
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:D,7607
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:Q,7485
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[15]:A,5578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[15]:B,2179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[15]:C,2234
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[15]:D,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[15]:Y,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16]:B,6473
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16]:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16]:CC,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16]:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16]:S,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:D,5319
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:CLK,5897
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:D,8706
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:Q,5897
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIPRTEF[9]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIPRTEF[9]:B,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIPRTEF[9]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIPRTEF[9]:CC,4269
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIPRTEF[9]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIPRTEF[9]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIPRTEF[9]:S,4269
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIPRTEF[9]:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:CLK,7916
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:D,7742
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:Q,7916
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_5:B,3032
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_5:UB,3032
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_11:B,4835
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_11:C,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_11:CC,3560
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_11:S,3560
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_11:UB,4835
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:CLK,2682
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:D,8674
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:Q,2682
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:D,8717
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:CLK,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:Q,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_5_0:A,3245
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_5_0:B,915
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_5_0:C,1327
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_5_0:CC,1070
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_5_0:D,-253
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_5_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_5_0:S,1070
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_5_0:UB,-253
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:CLK,7128
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:Q,7128
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO:A,5809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO:B,5761
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO:C,3904
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO:D,3822
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO:Y,3822
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[0]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[0]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[0]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIAR043[15]:A,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIAR043[15]:B,1503
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIAR043[15]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIAR043[15]:CC,5130
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIAR043[15]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIAR043[15]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIAR043[15]:S,5130
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIAR043[15]:UB,1503
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:CLK,4095
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:D,8717
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:Q,4095
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1[3]:A,5967
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1[3]:B,6529
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1[3]:Y,5967
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_40:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_40:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_40:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_40:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_40:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_121:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_121:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_121:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_121:IPA,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15:A,7058
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15:B,3637
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15:C,3594
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15:CC,3449
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15:P,3685
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15:S,3449
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15:UB,3594
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[10],7028
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[11],6967
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[1],7565
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[2],7504
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[3],7232
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[4],7164
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[5],7114
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[6],7168
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[7],7076
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[8],7015
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CC[9],7112
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:CO,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[0],7006
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[1],6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[2],7115
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[3],7091
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[6],7103
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[7],7152
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[8],7222
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:P[9],7209
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:CLK,5861
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:D,6056
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:Q,5861
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:CLK,4600
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:Q,4600
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:C,6844
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPC,6844
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_164:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_164:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_164:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_164:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_164:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:CLK,5873
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:Q,5873
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:CLK,6402
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:Q,6402
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[9]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:C,6757
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:IPC,6757
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:CLK,4792
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:Q,4792
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_20_0:A,1900
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_20_0:B,1289
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_20_0:C,1362
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_20_0:CC,525
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_20_0:D,121
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_20_0:P,193
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_20_0:S,525
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_20_0:UB,121
A0_ADC_SCK_O_obuf/U0/U_IOOUTFF:A,4288
A0_ADC_SCK_O_obuf/U0/U_IOOUTFF:Y,4288
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[15]:A,2154
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[15]:B,4273
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[15]:C,1971
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[15]:Y,1971
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_1:A,1712
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_1:B,2962
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_1:P,1712
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_1:UB,2980
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0_m2[1]:A,7047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0_m2[1]:B,6845
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0_m2[1]:C,5533
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0_m2[1]:Y,5533
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o_1_sqmuxa_0_a2:A,5351
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o_1_sqmuxa_0_a2:B,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o_1_sqmuxa_0_a2:C,5352
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o_1_sqmuxa_0_a2:D,4933
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o_1_sqmuxa_0_a2:Y,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17:A,2366
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17:B,2039
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17:CC,1334
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17:S,1334
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17:UB,2039
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_26:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_26:IPENn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:CLK,5111
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:Q,5111
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_3:A,6232
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_3:B,4290
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_3:P,4380
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_3:UB,4290
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[8]_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:CLK,6266
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:Q,6266
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12:B,4931
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12:CC,4499
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12:P,4931
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12:S,4499
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[17]:A,6578
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[17]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[17]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[17]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[17]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1:A,6929
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1:B,5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1:CC,6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1:P,5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1:S,6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1:UB,5512
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:C,6713
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_2:IPC,6713
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[3]:A,6040
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[3]:B,5963
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[3]:C,5584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[3]:D,4347
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[3]:Y,4347
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:D,8664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_254:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_254:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_254:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_254:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_254:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:CLK,4443
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:D,4762
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:Q,4443
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[14]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[14]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[14]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[14]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[20]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[20]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[20]:Y,7440
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[41]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[41]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[41]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[41]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:B,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:C,6757
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:IPC,6757
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[17]:A,2513
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[17]:B,2831
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[17]:C,2780
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_2[17]:Y,2513
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[33]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[33]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[33]:Y,7555
A0_ADC_CS_O_obuf/U0/U_IOPAD:D,4164
A0_ADC_CS_O_obuf/U0/U_IOPAD:E,
A0_ADC_CS_O_obuf/U0/U_IOPAD:PAD,4164
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:CLK,2753
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:D,6453
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:Q,2753
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_13:A,6163
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_13:B,6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_13:P,6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_13:UB,6137
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_2:A,4493
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_2:B,4368
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_2:CC,4719
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_2:P,4404
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_2:S,4719
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_2:UB,4368
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[0]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[0]:B,5543
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[0]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[0]:Y,91
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11:B,4493
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11:UB,4493
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:CLK,6357
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:Q,6357
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_s_17:A,5392
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_s_17:B,7359
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_s_17:C,7585
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_s_17:CC,1713
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_s_17:D,3044
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_s_17:S,1713
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_axb_0_i_0:A,6630
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_axb_0_i_0:B,7870
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_axb_0_i_0:Y,6630
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:B,7919
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:C,6844
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:D,7884
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPB,7919
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPC,6844
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPD,7884
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:CLK,6250
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:Q,6250
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[10],5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[11],5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[1],6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[2],6139
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[3],5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[4],5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[5],5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[6],5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[7],5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[8],5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CC[9],5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:CO,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[0],5599
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[1],5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[2],5324
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[3],5239
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[6],5181
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[7],5157
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[8],5315
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:P[9],5232
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[0],5472
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[10],5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[11],5308
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[1],5512
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[2],5292
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[3],5141
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[4],5118
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[5],5262
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[6],5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[7],5103
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[8],5282
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_0:UB[9],5144
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[37]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[37]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[37]:Y,7555
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:CLK,4626
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:Q,4626
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[9]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_172:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_172:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_172:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_172:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_172:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:D,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:CC[0],4499
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:CC[1],4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:CI,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[0],4931
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:CLK,4979
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:Q,4979
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14]:SLn,
A0_PWM_VH_O_obuf/U0/U_IOOUTFF:A,4315
A0_PWM_VH_O_obuf/U0/U_IOOUTFF:Y,4315
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI408TJ[15]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI408TJ[15]:B,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI408TJ[15]:C,7716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI408TJ[15]:CC,3735
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI408TJ[15]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI408TJ[15]:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI408TJ[15]:S,3735
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI408TJ[15]:UB,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGI4O7[5]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGI4O7[5]:B,7061
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGI4O7[5]:C,2796
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGI4O7[5]:CC,3074
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGI4O7[5]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGI4O7[5]:P,2796
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGI4O7[5]:S,3074
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGI4O7[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:CLK,6738
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:D,6850
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:Q,6738
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15]:B,6473
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15]:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15]:CC,5625
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15]:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15]:S,5625
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15]:UB,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:CLK,6738
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:D,7751
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:Q,6738
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:CLK,6768
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:D,7066
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:Q,6768
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:CLK,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:Q,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[4]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[4]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[4]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:CLK,7837
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:Q,7837
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[39]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[10]:A,2127
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[10]:B,4272
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[10]:C,1760
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[10]:D,1963
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[10]:Y,1760
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_8:A,4942
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_8:B,2890
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_8:P,2913
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_8:UB,2890
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:CLK,6331
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:Q,6331
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[11]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[11]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[11]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[11]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI8NFH2[16]:A,4501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI8NFH2[16]:B,3473
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI8NFH2[16]:C,3268
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI8NFH2[16]:Y,3268
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:CLK,2777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:D,8697
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:Q,2777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[41]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[41]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[41]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[41]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[0]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[0]:B,7886
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[0]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_11:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7O271[6]:A,2415
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7O271[6]:B,2179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7O271[6]:C,2291
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7O271[6]:Y,2179
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_5:B,2947
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_5:UB,2947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:CLK,7671
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:Q,7671
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_30:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_30:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:CC[0],7061
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:CC[1],6983
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:CC[2],6925
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:CC[3],7015
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:CC[4],6944
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:CC[5],6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:CI,6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[0],7083
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[39]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[39]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[39]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[39]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[39]:Y,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_16:B,6220
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_16:UB,6220
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_149:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_149:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_149:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_149:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_149:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:CLK,2391
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:D,8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:Q,2391
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:CLK,7252
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:D,6796
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:Q,7252
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8:A,6229
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8:B,6181
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8:C,3761
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8:D,4603
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8:Y,3761
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:CLK,3427
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:Q,3427
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:CLK,2136
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:D,7044
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:Q,2136
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0:A,6999
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0:B,6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0:P,6927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0:UB,6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0:Y,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_35:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_35:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_27:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_27:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[10]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[10]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[10]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[10]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[10]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[10]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[10]:Y,4589
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[0]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[0]:A,2970
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[0]:B,4363
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[0]:C,1579
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[0]:D,1673
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[0]:Y,1579
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_11:A,5927
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_11:B,5884
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_11:C,5802
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_11:D,5701
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_11:Y,5701
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[5]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[5]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[5]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[5]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[5]:Y,261
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:CLK,4320
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:Q,4320
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[0]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[0]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[0]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIF8O81[16]:A,3166
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIF8O81[16]:B,2759
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIF8O81[16]:C,3116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIF8O81[16]:Y,2759
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_33:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_33:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_33:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_33:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_33:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:CLK,7718
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:Q,7718
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_30:A,7309
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_30:B,5809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_30:C,4897
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_30:CC,3251
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_30:D,5565
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_30:P,4995
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_30:S,3251
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_30:UB,4897
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:CLK,6859
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:Q,6859
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:CLK,4028
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:Q,4028
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18:A,5682
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18:B,3755
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18:P,3829
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18:UB,3755
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:D,6618
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[0]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[0]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[0]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[0]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[0]:Y,261
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[4]:A,5859
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[4]:B,5430
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[4]:C,5319
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[4]:D,4227
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[4]:Y,4227
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:CLK,2318
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:D,5939
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:Q,2318
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[15]:A,6985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[15]:B,6901
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[15]:C,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[15]:Y,6226
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:CLK,3876
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:D,6740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:Q,3876
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[5]:A,7091
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[5]:B,5049
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[5]:C,4877
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[5]:CC,4814
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[5]:D,6653
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[5]:P,4951
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[5]:S,4814
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[5]:UB,4877
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:D,5187
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:D,8719
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:CLK,6847
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:Q,6847
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:C,6757
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:IPC,6757
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_13_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_13_0:B,6764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_13_0:C,2968
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_13_0:CC,2671
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_13_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_13_0:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_13_0:S,2671
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_13_0:UB,2968
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_4_iv_0[17]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_4_iv_0[17]:B,4303
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_4_iv_0[17]:C,708
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_4_iv_0[17]:Y,91
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[9]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[9]:B,4898
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[9]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[9]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[9]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3:A,6872
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3:B,3471
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3:C,3341
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3:CC,3772
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3:P,3456
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3:S,3772
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3:UB,3341
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:CLK,5020
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:D,6920
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:Q,5020
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_15:A,2727
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_15:B,2711
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_15:P,2727
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_15:UB,2711
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[22]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[22]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[22]:Y,5379
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:B,7686
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:C,6709
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:IPB,7686
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:IPC,6709
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_29:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_29:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:D,8728
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_19:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_19:B,7097
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_19:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_19:CC,6801
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_19:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_19:P,7097
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_19:S,6801
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_19:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_6:A,7140
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_6:B,6959
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_6:CC,7049
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_6:P,7048
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_6:S,7049
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_6:UB,6959
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[14]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[14]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[14]:C,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[14]:Y,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:CLK,6640
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:D,6418
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:Q,6640
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[7]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[7]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[7]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:D,5478
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[4]_CC_0:UB[9],
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:CLK,5790
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:Q,5790
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:CLK,5281
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:Q,5281
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIFUEDH[13]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIFUEDH[13]:B,3975
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIFUEDH[13]:C,7209
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIFUEDH[13]:CC,3716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIFUEDH[13]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIFUEDH[13]:P,3975
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIFUEDH[13]:S,3716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIFUEDH[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i[2]:A,5084
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i[2]:B,4022
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i[2]:C,7836
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i[2]:D,5601
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i[2]:Y,4022
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI01MU[1]:A,6929
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI01MU[1]:B,6555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI01MU[1]:C,6475
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI01MU[1]:Y,6475
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:CLK,4732
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:Q,4732
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[24]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[24]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[24]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:B,7832
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:C,6833
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:D,7817
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPB,7832
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPC,6833
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPD,7817
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_8:A,7121
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_8:B,6964
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_8:CC,6790
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_8:P,7032
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_8:S,6790
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_8:UB,6964
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16:B,3672
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16:C,3629
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16:CC,3385
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16:S,3385
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16:UB,3629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0:A,7227
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0:B,6565
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0:C,4399
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0:CC,2114
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0:D,2267
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0:P,2440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0:S,2114
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0:UB,2267
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[7]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_FCINST1:CC,4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_FCINST1:CO,4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:CLK,4272
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:Q,4272
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[16]:A,5821
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[16]:B,6009
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[16]:C,2833
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[16]:D,2858
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[16]:Y,2833
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2_i_m2[2]:A,4366
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2_i_m2[2]:B,1830
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2_i_m2[2]:C,1786
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2_i_m2[2]:Y,1786
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_11:B,6818
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_11:C,6875
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_11:CC,6796
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_11:P,6818
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_11:S,6796
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_11:UB,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_27:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_27:B,7332
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_27:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_27:CC,6735
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_27:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_27:P,7332
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_27:S,6735
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_27:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO_0:A,5585
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO_0:B,5491
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO_0:C,3634
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO_0:D,3554
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO_0:Y,3554
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:CO,1352
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[0],2196
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[1],1712
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[2],1788
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[3],1498
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[6],1408
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[7],1352
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[8],1362
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:P[9],1460
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[0],2802
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[10],3169
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[11],3290
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[1],2980
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[2],3104
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[3],3023
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[4],3061
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[5],3153
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[6],3044
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[7],3102
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[8],3210
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0_CC_0:UB[9],3151
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:CLK,2502
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:D,8678
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:Q,2502
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[16]:A,2661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[16]:B,1799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[16]:C,5887
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[16]:D,2544
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[16]:Y,1799
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:CLK,5904
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:Q,5904
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18:A,7080
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18:B,3658
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18:C,3615
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18:CC,3437
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18:P,3707
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18:S,3437
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_18:UB,3615
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIE4U3E[36]:A,1983
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIE4U3E[36]:B,1899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIE4U3E[36]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIE4U3E[36]:CC,1307
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIE4U3E[36]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIE4U3E[36]:P,1941
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIE4U3E[36]:S,1307
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIE4U3E[36]:UB,1899
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:CLK,7853
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:Q,7853
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14:S,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:CLK,2730
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:D,8673
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:Q,2730
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:CLK,1844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:D,2430
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:Q,1844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:CLK,4109
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:Q,4109
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_30:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_30:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_30:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_30:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_30:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_5:A,1740
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_5:B,1636
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_5:C,365
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_5:D,982
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_5:Y,365
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:CLK,5059
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:D,8682
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:Q,5059
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[4]:A,6174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[4]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[4]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[4]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[4]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:C,6844
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPC,6844
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPD,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_7:A,3480
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_7:B,1104
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_7:P,1153
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_7:UB,1104
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNIH1TF1:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNIH1TF1:B,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNIH1TF1:C,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNIH1TF1:CC,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNIH1TF1:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNIH1TF1:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNIH1TF1:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_31:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_31:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0_RNO:A,6072
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0_RNO:B,5995
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0_RNO:C,5825
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0_RNO:D,5483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0_RNO:Y,5483
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_4:B,2682
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_4:UB,2682
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_6:A,2722
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_6:B,2722
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_6:P,2722
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_6:UB,2722
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:CLK,5054
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:Q,5054
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFSISF[6]:A,6312
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFSISF[6]:B,1403
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFSISF[6]:C,1473
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFSISF[6]:CC,1407
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFSISF[6]:D,5980
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFSISF[6]:P,1441
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFSISF[6]:S,1407
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFSISF[6]:UB,1403
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_2:A,6217
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_2:B,4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_2:P,4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_2:UB,4722
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:CLK,4427
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:D,5811
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:Q,4427
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_RNIURLK:A,4753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_RNIURLK:B,4440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_RNIURLK:C,2776
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_RNIURLK:Y,2776
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_16:A,2421
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_16:B,2452
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_16:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_16:IPA,2421
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_16:IPB,2452
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[6]:A,2055
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[6]:B,4200
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[6]:C,1697
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[6]:D,1891
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[6]:Y,1697
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_2:A,4362
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_2:B,4320
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_2:P,4320
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_2:UB,4327
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1_RNO[1]:A,5608
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1_RNO[1]:B,5756
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_1_RNO[1]:Y,5608
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[7]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[7]:B,7222
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[7]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[7]:CC,7015
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[7]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[7]:P,7222
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[7]:S,7015
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[10]:A,5967
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[10]:B,5539
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[10]:C,5428
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[10]:D,4336
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[10]:Y,4336
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[3]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[3]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[3]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[3]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_s_17:B,5724
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_s_17:C,7283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_s_17:CC,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_s_17:D,7556
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_s_17:S,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_s_17:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_17:B,6449
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_17:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_17:D,6452
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_17:IPB,6449
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_17:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_17:IPD,6452
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[7]:A,2988
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[7]:B,4257
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[7]:C,6096
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[7]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[7]:D,5942
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[7]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[7]:Y,2988
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:CLK,4406
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:Q,4406
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:CLK,7049
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:Q,7049
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17_FCINST1:CC,2764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17_FCINST1:CO,2764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_5:B,4688
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_5:UB,4688
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_8:A,6253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_8:B,6212
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_8:P,6237
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_8:UB,6212
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[35]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[35]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[35]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[35]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[35]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[15]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[15]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[15]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[15]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:CLK,7723
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:D,6739
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:Q,7723
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[17]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n_RNO:A,7958
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n_RNO:Y,7958
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[11]:A,6985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[11]:B,6901
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[11]:C,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[11]:Y,6226
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[11]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[11]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[11]:C,5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[11]:Y,5095
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[39]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[39]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[39]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[39]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_8:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_8:C,4227
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_8:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_8:IPC,4227
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_132:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_132:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_132:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_132:IPA,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]:A,2562
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]:B,2055
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]:C,4315
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]:D,4197
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]:Y,2055
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:CLK,330
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:D,6905
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:Q,330
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[9]:A,4144
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[9]:B,1818
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[9]:C,1841
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[9]:Y,1818
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18:A,1793
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18:B,1774
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18:P,1793
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18:UB,1774
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_7:A,7051
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_7:B,6878
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_7:CC,6850
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_7:P,6966
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_7:S,6850
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_7:UB,6878
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:CLK,1394
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:D,8712
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:Q,1394
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_2:B,4484
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_2:C,4329
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_2:CC,4505
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_2:P,4329
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_2:S,4505
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIK0SFB[31]:A,1931
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIK0SFB[31]:B,1759
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIK0SFB[31]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIK0SFB[31]:CC,1497
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIK0SFB[31]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIK0SFB[31]:P,1859
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIK0SFB[31]:S,1497
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIK0SFB[31]:UB,1759
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[15]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[12]:A,1376
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[12]:B,5093
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[12]:Y,1376
A0_PWM_VL_O_obuf/U0/U_IOPAD:D,2345
A0_PWM_VL_O_obuf/U0/U_IOPAD:E,
A0_PWM_VL_O_obuf/U0/U_IOPAD:PAD,2345
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:CLK,7662
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:Q,7662
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:CLK,4156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:Q,4156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_20:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_20:B,7167
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_20:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_20:CC,6740
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_20:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_20:P,7167
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_20:S,6740
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_20:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI8JDG8[8]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI8JDG8[8]:B,6155
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI8JDG8[8]:C,7217
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI8JDG8[8]:CC,6000
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI8JDG8[8]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI8JDG8[8]:P,6155
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI8JDG8[8]:S,6000
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNI8JDG8[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:CLK,4709
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:D,7531
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:Q,4709
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1:A,2741
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1:B,2629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1:CC,3017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1:P,2629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1:S,3017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1:UB,2646
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:CLK,2324
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:D,6021
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:Q,2324
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[0]:A,7052
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[0]:B,5030
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[0]:C,4879
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[0]:CC,5284
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[0]:D,6655
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[0]:P,4932
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[0]:S,5284
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[0]:UB,4879
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:D,8840
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:EN,7480
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:CLK,3514
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:Q,3514
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[2]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o_1_sqmuxa_0_a2_0:A,2545
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o_1_sqmuxa_0_a2_0:B,2522
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o_1_sqmuxa_0_a2_0:Y,2522
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[7]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[18]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[18]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[18]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[18]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_13:A,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_13:B,2624
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_13:P,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_13:UB,2624
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_3:A,1688
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_3:B,1533
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_3:C,337
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_3:D,991
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_3:Y,337
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[7]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[7]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[7]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[16]:A,6985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[16]:B,6901
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[16]:C,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[16]:Y,6226
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_3:A,6930
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_3:B,6735
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_3:CC,7136
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_3:P,6864
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_3:S,7136
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_3:UB,6735
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIVTPO7[5]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIVTPO7[5]:B,3847
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIVTPO7[5]:C,7011
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIVTPO7[5]:CC,3951
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIVTPO7[5]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIVTPO7[5]:P,3847
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIVTPO7[5]:S,3951
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIVTPO7[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]:A,2682
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]:B,1963
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]:C,4229
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]:D,4105
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]:Y,1963
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:CLK,4453
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:D,8688
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:Q,4453
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o_1_sqmuxa_0_a2:A,5182
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o_1_sqmuxa_0_a2:B,5422
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o_1_sqmuxa_0_a2:C,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o_1_sqmuxa_0_a2:D,5150
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o_1_sqmuxa_0_a2:Y,2945
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_17:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_17:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_225:A,6072
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_225:B,4597
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_225:C,5950
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_225:Y,4597
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[2]:A,4402
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[2]:B,3274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[2]:C,5786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[2]:D,4323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[2]:Y,3274
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[15]:A,4525
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[15]:B,2635
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[15]:C,1843
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[15]:Y,1843
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:CLK,6865
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:Q,6865
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_3:B,5174
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_3:C,5009
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_3:CC,4426
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_3:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_3:S,4426
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[5]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[5]:B,4937
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[5]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[5]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[5]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:C,6704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:IPC,6704
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:CLK,7103
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:D,7168
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:Q,7103
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:CLK,3910
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:D,6862
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:Q,3910
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:CLK,7332
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:D,6735
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:Q,7332
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[9]:A,3481
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[9]:B,3443
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[9]:C,2458
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[9]:D,2378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[9]:Y,2378
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[17]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[17]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[17]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0_RNO:A,5731
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0_RNO:B,2016
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0_RNO:C,1926
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0_RNO:Y,1926
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:CLK,4348
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:D,8690
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:Q,4348
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:CLK,6117
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:D,8668
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:Q,6117
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:D,8711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[32]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[32]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[32]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:CLK,871
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:D,1852
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:Q,871
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_state_RNIM0BA1[0]:A,3992
BLDC_Encoder_Axis_0/MSC_i_0/s_state_RNIM0BA1[0]:B,7611
BLDC_Encoder_Axis_0/MSC_i_0/s_state_RNIM0BA1[0]:C,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_state_RNIM0BA1[0]:D,3515
BLDC_Encoder_Axis_0/MSC_i_0/s_state_RNIM0BA1[0]:Y,3475
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_19:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_19:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_o2_0[7]:A,3869
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_o2_0[7]:B,3913
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_o2_0[7]:C,4853
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_o2_0[7]:D,3650
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_o2_0[7]:Y,3650
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNINT8P1[11]:A,2442
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNINT8P1[11]:B,2206
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNINT8P1[11]:C,2318
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNINT8P1[11]:Y,2206
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[1]:A,6953
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[1]:B,6892
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[1]:C,5857
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[1]:D,4669
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[1]:Y,4669
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3_0:A,5474
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3_0:B,6524
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3_0:C,6868
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3_0:CC,5627
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3_0:P,5474
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3_0:S,5627
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_3_0:UB,6868
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:CLK,1213
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:Q,1213
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_10_0:A,3307
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_10_0:B,7161
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_10_0:C,6702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_10_0:CC,1629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_10_0:D,4544
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_10_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_10_0:S,1629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_10_0:UB,4544
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2[0]:A,2402
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2[0]:B,2341
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2[0]:C,6047
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2[0]:Y,2341
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[16]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[16]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[16]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[16]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[16]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[16]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[16]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[16]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_14:B,7060
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_14:CC,6830
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_14:P,7060
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_14:S,6830
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_14:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o_1_sqmuxa_0_a2:A,5483
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o_1_sqmuxa_0_a2:B,5137
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o_1_sqmuxa_0_a2:C,5235
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o_1_sqmuxa_0_a2:D,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o_1_sqmuxa_0_a2:Y,2873
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[2]:A,6251
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[2]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[2]:Y,6251
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_13:B,2256
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_13:C,1872
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_13:CC,1026
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_13:S,1026
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12_RNIP1IO3:A,6296
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12_RNIP1IO3:B,4499
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12_RNIP1IO3:C,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12_RNIP1IO3:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12_RNIP1IO3:D,5911
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12_RNIP1IO3:P,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12_RNIP1IO3:UB,5911
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_32:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_32:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[13]:A,4343
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[13]:B,4333
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[13]:C,3340
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[13]:D,3266
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[13]:Y,3266
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[5]:A,2897
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[5]:B,4166
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[5]:C,6005
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[5]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[5]:D,5851
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[5]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[5]:Y,2897
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:CLK,3089
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:D,2823
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:Q,3089
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:CLK,1925
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:D,1875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:Q,1925
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_0:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16:A,3950
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16:B,3866
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16:C,2765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16:Y,2765
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:CLK,7716
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:D,6603
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:Q,7716
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI00LU[1]:A,6886
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI00LU[1]:B,6508
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI00LU[1]:C,6432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI00LU[1]:Y,6432
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:CLK,5166
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:Q,5166
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[1]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[1]:B,6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[1]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[1]:CC,7531
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[1]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[1]:P,6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[1]:S,7531
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIRFH32[4]:A,2543
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIRFH32[4]:B,2310
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIRFH32[4]:C,2466
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIRFH32[4]:Y,2310
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[0]:A,2341
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[0]:B,1579
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[0]:C,3994
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[0]:D,1697
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[0]:Y,1579
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_258:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_258:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_258:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_258:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_258:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_16:B,1282
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_16:UB,1282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[4]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[4]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[4]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[4]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_34:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_34:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:CLK,7526
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:D,7879
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:Q,7526
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_8:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_8:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_8:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_8:IPENn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:CLK,6370
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:Q,6370
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[3]:A,6940
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[3]:B,6889
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[3]:C,5826
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[3]:D,5759
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[3]:Y,5759
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_22:EN,9019
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_22:IPENn,9019
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:CLK,6804
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:Q,6804
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:D,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_13:B,6798
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_13:C,6873
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_13:CC,5931
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_13:S,5931
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:CLK,6212
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:D,8671
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:Q,6212
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:CLK,6136
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:D,6891
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:Q,6136
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_24:A,581
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_24:B,334
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_24:C,243
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_24:D,235
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_24:Y,235
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:CLK,6910
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:Q,6910
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:CLK,6940
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:D,6966
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:Q,6940
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[12]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_102:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_102:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_102:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_102:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_102:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:CLK,4495
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:Q,4495
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO:A,2214
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO:B,2131
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO:C,2250
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO:D,2159
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0_RNO:Y,2131
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m35_3:A,4648
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m35_3:B,1875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m35_3:C,4758
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m35_3:Y,1875
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]:A,3184
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]:B,2677
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]:C,4937
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]:D,4819
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_0_wmux[17]:Y,2677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[6]:Y,4589
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[8]:A,7964
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[8]:B,7880
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[8]:Y,7880
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[0]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[0]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[0]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[7]:A,5987
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[7]:B,6195
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[7]:C,3019
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[7]:D,3038
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[7]:Y,3019
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16:B,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16:S,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[10]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[10]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[10]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[10]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:CLK,4034
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:Q,4034
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[10],5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[11],5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[1],6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[2],6139
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[3],5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[4],5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[5],5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[6],5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[7],5283
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[8],5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CC[9],5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:CO,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[0],5599
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[1],5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[2],5324
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[3],5239
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[6],5181
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[7],5157
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[8],5224
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:P[9],5232
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[0],5472
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[10],5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[11],5308
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[1],5512
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[2],5292
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[3],5141
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[4],5118
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[5],5262
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[6],5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[7],5103
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[8],5282
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_0:UB[9],5144
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_8:A,7022
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_8:B,6918
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_8:CC,6927
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_8:P,6986
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_8:S,6927
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_8:UB,6918
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_195:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_195:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_195:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_195:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_195:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:CLK,6844
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:Q,6844
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m24_0_a2_0_a2_3:A,5106
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m24_0_a2_0_a2_3:B,5008
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m24_0_a2_0_a2_3:Y,5008
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[4]:A,6147
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[4]:B,6070
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[4]:C,5688
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[4]:D,4454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[4]:Y,4454
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:CC[6],2777
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:CI,2842
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[0],2927
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[1],2803
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[3],2998
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[0],2777
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[1],2800
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[2],2868
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[3],2871
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[4],2844
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[5],4961
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:CLK,5712
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:D,6917
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:Q,5712
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_2_0:A,2276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_2_0:B,6887
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_2_0:C,6435
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_2_0:CC,2378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_2_0:D,4271
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_2_0:P,2276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_2_0:S,2378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_2_0:UB,4271
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[10]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[10]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[10]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[18]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[18]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[18]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_3[2]:A,4137
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_3[2]:B,4038
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_3[2]:C,2012
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_3[2]:Y,2012
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_a2_1[11]:A,5524
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_a2_1[11]:B,2875
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_a2_1[11]:C,3242
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_a2_1[11]:D,3112
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_a2_1[11]:Y,2875
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_11:B,4708
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_11:C,4553
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_11:P,4553
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_11:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_11:UB,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[11]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[11]:B,6996
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[11]:C,7040
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[11]:CC,6974
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[11]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[11]:P,6996
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[11]:S,6974
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[23]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[23]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[23]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2_0:A,5484
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2_0:B,6539
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2_0:C,6949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2_0:CC,5899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2_0:P,5484
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2_0:S,5899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2_0:UB,6949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[40]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[40]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[40]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[40]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_16:B,6458
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_16:C,4273
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_16:IPB,6458
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_16:IPC,4273
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[12]:A,5084
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[12]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[12]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[12]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[12]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:CLK,6167
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:Q,6167
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[4]:A,5746
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[4]:B,6946
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[4]:C,6472
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[4]:CC,5867
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[4]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[4]:P,5746
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[4]:S,5867
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[4]:UB,6472
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_1:B,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_1:CC,7531
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_1:P,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_1:S,7531
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_1:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6]:B,5775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6]:C,6019
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6]:CC,5750
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6]:P,5775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6]:S,5750
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:D,8724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:CLK,3964
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:D,8719
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:Q,3964
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:CLK,6911
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:Q,6911
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[24]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[2]:A,4085
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[2]:B,1762
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[2]:C,1773
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[2]:Y,1762
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:CLK,6892
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:D,6809
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:EN,7664
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:Q,6892
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[8]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[8]:B,7073
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[8]:C,7117
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[8]:CC,7018
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[8]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[8]:P,7073
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[8]:S,7018
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[8]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[10]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[10]:B,4814
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[10]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[10]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[10]:Y,2538
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:CLK,6063
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:D,6892
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:EN,7664
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:Q,6063
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[25]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_251:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_251:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_251:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_251:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_251:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:D,7028
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[5]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/START_SIG_PROC_un1_s_sckctr_done:A,7909
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/START_SIG_PROC_un1_s_sckctr_done:B,7832
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/START_SIG_PROC_un1_s_sckctr_done:Y,7832
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_85:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_85:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_85:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_85:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_85:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:CLK,4345
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:D,8683
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:Q,4345
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_2:A,6146
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_2:B,6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_2:P,6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_2:UB,6137
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:CLK,4702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:D,7007
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:Q,4702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_5:A,7749
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_5:B,6925
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_5:CC,6871
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_5:S,6871
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_5:UB,6925
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI50HT[27]:A,3963
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI50HT[27]:B,3659
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI50HT[27]:C,3841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI50HT[27]:Y,3659
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:CLK,6844
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:Q,6844
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:CLK,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:Q,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[13]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[13]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[13]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:C,6795
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:IPC,6795
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:CLK,3295
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:D,7004
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:Q,3295
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[6]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_20:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_20:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:CLK,3461
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:Q,3461
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_2:A,4947
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_2:B,4891
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_2:P,4891
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_2:UB,4898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:D,5415
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[12]:A,5922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[12]:B,5844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[12]:C,4356
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[12]:D,5332
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[12]:Y,4356
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:CLK,7688
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:D,8834
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:EN,5533
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:Q,7688
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[25]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[25]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[25]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[25]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[25]:Y,-45
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[1]:A,7964
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[1]:B,7910
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[1]:C,7876
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[1]:Y,7876
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:CLK,7091
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:D,7232
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:Q,7091
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:Q,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:CLK,2853
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:Q,2853
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[4]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17:B,4961
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17:UB,4961
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:CLK,6130
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:D,8680
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:Q,6130
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:D,3441
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[8]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:CLK,5019
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:D,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:Q,5019
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:CLK,6197
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:D,8674
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:Q,6197
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[2]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[2]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[2]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[2]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:C,6724
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:IPC,6724
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_5:A,7848
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_5:B,7068
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_5:CC,7028
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_5:S,7028
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_5:UB,7068
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_12:A,6244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_12:B,6037
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_12:P,6198
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_12:UB,6037
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:CLK,5160
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:Q,5160
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:CLK,6066
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:D,7165
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:Q,6066
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir0_tmp10_0_0:A,6232
BLDC_Encoder_Axis_0/MSC_i_23/s_dir0_tmp10_0_0:B,6135
BLDC_Encoder_Axis_0/MSC_i_23/s_dir0_tmp10_0_0:C,6103
BLDC_Encoder_Axis_0/MSC_i_23/s_dir0_tmp10_0_0:D,5981
BLDC_Encoder_Axis_0/MSC_i_23/s_dir0_tmp10_0_0:Y,5981
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[0]:A,6953
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[0]:B,6879
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[0]:C,5857
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[0]:D,4615
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_0[0]:Y,4615
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_10:B,6197
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_10:UB,6197
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o_1_sqmuxa_0_a2:A,5499
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o_1_sqmuxa_0_a2:B,5105
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o_1_sqmuxa_0_a2:C,5229
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o_1_sqmuxa_0_a2:D,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o_1_sqmuxa_0_a2:Y,2867
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_184:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_184:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_184:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_184:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_184:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[23]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[23]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[23]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[23]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[23]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9K2VA[30]:A,1898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9K2VA[30]:B,1699
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9K2VA[30]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9K2VA[30]:CC,1636
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9K2VA[30]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9K2VA[30]:P,1856
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9K2VA[30]:S,1636
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI9K2VA[30]:UB,1699
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:CLK,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:Q,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[38]:A,723
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[38]:B,580
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[38]:C,106
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[38]:Y,106
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:CLK,2797
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:D,2872
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:Q,2797
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:CLK,5010
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:Q,5010
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[15]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_265:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_265:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_265:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_265:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_265:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_265:IPC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13:A,7808
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13:B,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13:CC,5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13:S,5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13:UB,4995
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:CLK,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:Q,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:CLK,3656
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:D,7127
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:Q,3656
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_16:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_16:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_18:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_18:B,7048
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_18:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_18:CC,6917
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_18:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_18:P,7048
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_18:S,6917
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_18:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_10:B,2059
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_10:UB,2059
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_1:A,4349
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_1:B,4222
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_1:CC,4620
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_1:P,4230
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_1:S,4620
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_1:UB,4222
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:D,5045
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:CLK,4931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:Q,4931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:CLK,4387
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:Q,4387
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_25:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_25:B,7161
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_25:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_25:CC,6703
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_25:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_25:P,7161
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_25:S,6703
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_25:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[16]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[16]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[16]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[16]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[16]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_3:B,7527
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_3:C,7590
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_3:CC,6912
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_3:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_3:S,6912
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[38]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[38]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[38]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[38]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[8]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[8]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[8]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[8]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[8]:Y,261
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_4:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_4:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_4:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_4:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_1:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_1:C,5401
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_1:IPC,5401
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:CLK,6183
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:Q,6183
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:C,6802
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPC,6802
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPD,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_29:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_29:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_29:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_29:CC,6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_29:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_29:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_29:S,6603
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_29:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_15:B,6798
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_15:C,6873
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_15:CC,5950
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_15:S,5950
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:CLK,6772
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:Q,6772
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9B9B4[15]:A,6271
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9B9B4[15]:B,1271
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9B9B4[15]:C,1346
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9B9B4[15]:CC,1487
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9B9B4[15]:D,5843
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9B9B4[15]:P,1400
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9B9B4[15]:S,1487
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9B9B4[15]:UB,1271
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:CLK,4717
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:D,7531
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:Q,4717
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[1]:SLn,
A0_PWM_UL_O_obuf/U0/U_IOPAD:D,2345
A0_PWM_UL_O_obuf/U0/U_IOPAD:E,
A0_PWM_UL_O_obuf/U0/U_IOPAD:PAD,2345
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:CLK,1855
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:D,8673
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:Q,1855
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0:A,7841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0:B,6513
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0:C,1908
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0:CC,1959
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0:S,1959
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0:UB,1908
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[4]:A,7977
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[4]:B,7857
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[4]:C,5826
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[4]:D,5650
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[4]:Y,5650
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:C,6691
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_26:IPC,6691
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[7]:A,6020
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[7]:B,5942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[7]:C,4454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[7]:D,5430
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[7]:Y,4454
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[16]:A,6613
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[16]:B,6565
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[16]:C,5861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[16]:Y,5861
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:CLK,4354
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:EN,8623
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:Q,4354
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:C,6711
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:IPC,6711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[9]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[9]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[9]:C,5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[9]:Y,5240
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_7:A,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_7:B,2698
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_7:P,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_7:UB,2698
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_17:B,7786
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_17:CC,6788
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_17:S,6788
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_17:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:D,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[15]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[15]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[15]:Y,5366
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:CLK,6186
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:Q,6186
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[8]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:CLK,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:Q,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:CLK,1652
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:D,5989
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:Q,1652
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:CLK,6920
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:Q,6920
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_1:A,4697
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_1:B,3268
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_1:P,3270
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_1:UB,3268
flash_freeze_inst/INST_FLASH_FREEZE_IP:FF_TO_START,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[42]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[42]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[42]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[42]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:D,8667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[12]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[12]:B,7074
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[12]:C,7118
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[12]:CC,6896
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[12]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[12]:P,7074
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[12]:S,6896
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[12]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:D,8670
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_10:B,4387
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_10:UB,4387
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_16:B,6208
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_16:UB,6208
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_240:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_240:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_240:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_240:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_240:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_240:IPC,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[0]:A,6584
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[0]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[0]:Y,6584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_RNIPUHA[1]:A,705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_RNIPUHA[1]:Y,705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_ns[1]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_ns[1]:B,6261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_ns[1]:C,7862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_ns[1]:D,7728
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_ns[1]:Y,6261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[30]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[30]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[30]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[6]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[6]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[6]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[6]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17:B,4283
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17:UB,4283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:CLK,4991
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:Q,4991
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[11]:A,6127
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[11]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[11]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[11]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[11]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIPJGT[21]:A,3831
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIPJGT[21]:B,3527
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIPJGT[21]:C,3709
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIPJGT[21]:Y,3527
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:CLK,4732
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:D,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:EN,8779
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:Q,4732
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:CLK,5168
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:D,8699
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:Q,5168
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o_1_sqmuxa_0_a2:A,5253
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o_1_sqmuxa_0_a2:B,5514
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o_1_sqmuxa_0_a2:C,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o_1_sqmuxa_0_a2:D,5202
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o_1_sqmuxa_0_a2:Y,3082
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[14]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[14]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[14]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_2_239_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_2_239_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_2_239_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_2_239_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:CC[0],6067
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:CC[1],5989
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:CC[2],5931
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:CC[3],6021
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:CC[4],5950
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:CC[5],5889
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:CC[6],6010
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:CI,5889
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[0],6089
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[1],6167
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[3],6338
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:CLK,5897
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:Q,5897
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_13:A,382
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_13:B,337
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_13:C,247
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_13:D,182
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_13:Y,182
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[10]:A,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[10]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[10]:C,5641
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[10]:Y,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:CLK,5117
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:D,8668
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:Q,5117
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[10],1293
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[11],1346
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[1],1688
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[2],1748
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[3],1373
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[4],1339
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[5],1378
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[6],1306
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[7],1273
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[8],1303
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CC[9],1359
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:CO,1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[0],1353
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[1],1316
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[2],1490
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[3],1475
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[6],1487
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[7],1527
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[8],1597
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:P[9],1593
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[0],1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[10],1530
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[11],1651
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[1],1339
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[2],1465
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[3],1384
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[4],1422
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[5],1514
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[6],1400
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[7],1459
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[8],1569
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_0:UB[9],1512
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[8]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[8]:B,4801
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[8]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[8]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[8]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:CLK,1989
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:D,8668
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:Q,1989
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[10]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[10]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[10]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[10]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10_RNIR4HV2:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10_RNIR4HV2:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10_RNIR4HV2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10_RNIR4HV2:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10_RNIR4HV2:D,6044
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10_RNIR4HV2:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10_RNIR4HV2:UB,6044
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:CLK,1565
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:D,8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:Q,1565
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14:A,7044
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14:B,3557
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14:C,3667
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14:CC,3382
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14:P,3609
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14:S,3382
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14:UB,3557
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3_1_1:A,6879
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3_1_1:B,6484
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3_1_1:C,6373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3_1_1:Y,6373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[0]:A,4016
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[0]:B,6360
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[0]:C,3044
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[0]:D,3766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[0]:Y,3044
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14_RNIV2JH4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14_RNIV2JH4:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14_RNIV2JH4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14_RNIV2JH4:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14_RNIV2JH4:D,5964
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14_RNIV2JH4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14_RNIV2JH4:UB,5964
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_4:B,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_4:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_4:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DIR_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DIR_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:B,7879
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:C,6731
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:IPB,7879
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:IPC,6731
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:CLK,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:Q,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[13]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_179:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_179:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_179:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_179:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[41]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIM0Q65[19]:A,1680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIM0Q65[19]:B,1501
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIM0Q65[19]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIM0Q65[19]:CC,5139
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIM0Q65[19]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIM0Q65[19]:P,1601
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIM0Q65[19]:S,5139
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIM0Q65[19]:UB,1501
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr_RNIGFTM:A,7679
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr_RNIGFTM:B,7700
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr_RNIGFTM:Y,7679
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[12]:A,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[12]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[12]:C,5664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[12]:Y,5196
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[7]:A,6014
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[7]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[7]:Y,6014
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:CC[0],5956
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:CC[1],5878
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:CI,5878
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[0],6432
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3_RNI7OD94[1]:A,2105
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3_RNI7OD94[1]:B,1445
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3_RNI7OD94[1]:Y,1445
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[38]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[38]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[38]:Y,5366
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:CLK,3661
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:Q,3661
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_2:B,6777
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_2:C,6870
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_2:CC,6980
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_2:P,6777
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_2:S,6980
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:CLK,4229
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:Q,4229
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_9:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:CLK,1403
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:D,1291
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:Q,1403
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[2]_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]:A,2876
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]:B,3270
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]:C,5094
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]:D,4970
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]:Y,2876
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:CLK,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:D,6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:Q,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset_fedg:A,6590
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset_fedg:B,6909
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset_fedg:Y,6590
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:CLK,1826
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:D,3828
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:Q,1826
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_13/cl_status_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[38]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[38]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[38]:Y,7555
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_146:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_146:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_146:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_146:IPA,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:CLK,703
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:D,8674
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:Q,703
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23:B,3984
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23:C,3861
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23:CC,3206
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23:S,3206
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23:UB,3861
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:CLK,3417
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:D,7065
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:Q,3417
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[33]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[33]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[33]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[33]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[33]:Y,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]:A,1452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]:B,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]:P,1367
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]:UB,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]:Y,6042
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:CLK,5884
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:Q,5884
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:CLK,6697
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:D,5469
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:Q,6697
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_4:B,3061
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_4:UB,3061
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:CLK,7087
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:D,6980
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:Q,7087
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[38]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[38]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[38]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[38]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_10:B,4722
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_10:C,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_10:CC,3621
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_10:S,3621
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_10:UB,4722
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:B,7806
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:C,6754
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:D,7809
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPB,7806
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPD,7809
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_151:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_151:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_151:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_151:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_151:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[14]:A,1880
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[14]:B,3950
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[14]:C,3383
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[14]:Y,1880
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIBTAA3[2]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIBTAA3[2]:B,6013
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIBTAA3[2]:C,7075
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIBTAA3[2]:CC,7119
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIBTAA3[2]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIBTAA3[2]:P,6013
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIBTAA3[2]:S,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIBTAA3[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:CLK,2942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:Q,2942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:B,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:C,6841
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPC,6841
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPD,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_223:A,6235
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_223:B,4744
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_223:C,6110
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_223:Y,4744
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:CLK,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:Q,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[11]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI2QAV_0[1]:A,6859
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI2QAV_0[1]:B,6837
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI2QAV_0[1]:Y,6837
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_1:A,5613
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_1:B,5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_1:CC,6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_1:P,5494
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_1:S,6203
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_1:UB,5512
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:CLK,3767
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:D,4089
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:Q,3767
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_17/over_current_fault_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:CLK,6754
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:D,6898
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:Q,6754
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI7HEU1[0]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI7HEU1[0]:B,3674
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI7HEU1[0]:C,6839
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI7HEU1[0]:CC,5378
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI7HEU1[0]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI7HEU1[0]:P,3674
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI7HEU1[0]:S,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI7HEU1[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0:B,6800
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0:C,4634
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0:CC,2075
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0:D,2624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0:S,2075
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0:UB,2624
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[24]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[24]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[24]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:C,6814
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:IPC,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[8]:A,2116
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[8]:B,4186
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[8]:C,3619
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[8]:Y,2116
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:CLK,6029
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:D,8675
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:Q,6029
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:CLK,1535
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:D,8682
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:Q,1535
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[23]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:CLK,6852
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:Q,6852
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17_FCINST1:CC,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17_FCINST1:CO,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[16]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[16]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[16]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[16]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[12]:A,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[12]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[12]:C,5664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[12]:Y,5196
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:C,6795
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_25:IPC,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI6F886[21]:A,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI6F886[21]:B,1640
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI6F886[21]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI6F886[21]:CC,4998
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI6F886[21]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI6F886[21]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI6F886[21]:S,4998
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI6F886[21]:UB,1640
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:B,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:C,6814
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:IPB,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_27:IPC,6814
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:CLK,7949
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:Q,7949
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:CLK,2766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:D,1645
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:Q,2766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:CLK,3099
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:Q,3099
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:CLK,3631
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:D,8719
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:Q,3631
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_35:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_35:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_0[7]:A,3523
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_0[7]:B,2373
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_0[7]:C,3650
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_0[7]:D,3254
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_a3_0[7]:Y,2373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[15]:A,2752
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[15]:B,2718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[15]:Y,2718
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[15]:A,7808
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[15]:B,5767
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[15]:C,5114
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[15]:CC,4608
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[15]:D,6890
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[15]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[15]:S,4608
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[15]:UB,5114
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:CLK,4534
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:D,4708
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:Q,4534
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:CLK,6745
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:D,3544
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:Q,6745
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:CLK,5712
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:D,6692
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:Q,5712
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[6]:A,7173
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[6]:B,5131
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[6]:C,4985
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[6]:CC,4753
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[6]:D,6760
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[6]:P,5033
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[6]:S,4753
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[6]:UB,4985
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_16:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_16:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:CLK,7714
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:Q,7714
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[14]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_247:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_247:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_247:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_247:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_247:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_13:A,6234
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_13:B,4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_13:P,4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_13:UB,4130
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[0]:A,5870
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[0]:B,5780
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[0]:C,4819
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[0]:D,4615
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_1[0]:Y,4615
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:CO,1100
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[0],1595
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[1],1470
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[2],1377
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[3],1310
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[6],1218
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[7],1153
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[8],1332
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:P[9],1261
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[0],1448
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[10],1122
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[11],1316
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[1],1468
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[2],1349
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[3],1193
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[4],1169
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[5],1291
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[6],1100
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[7],1104
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[8],1290
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0_CC_0:UB[9],1152
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:CLK,4839
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:Q,4839
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rrce:A,6923
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rrce:B,7799
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rrce:Y,6923
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_12:B,6896
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_12:C,6956
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_12:CC,6718
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_12:P,6896
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_12:S,6718
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_5_0:A,7120
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_5_0:B,6569
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_5_0:C,2773
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_5_0:CC,2879
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_5_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_5_0:P,2891
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_5_0:S,2879
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_5_0:UB,2773
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:CLK,7849
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:Q,7849
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_16:B,4767
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_16:UB,4767
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_12:A,1381
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_12:B,3071
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_12:P,1381
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_12:UB,3071
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_2:A,7088
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_2:B,6920
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_2:C,6496
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_2:CC,6703
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_2:P,6627
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_2:S,6703
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_2:UB,6496
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_3:A,1190
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_3:B,1398
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_3:P,1190
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_3:UB,1398
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:CLK,7185
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:D,6896
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:Q,7185
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11:A,2323
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11:B,1651
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11:CC,1346
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11:S,1346
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11:UB,1651
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNISLSQ8[7]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNISLSQ8[7]:B,4449
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNISLSQ8[7]:C,7309
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNISLSQ8[7]:CC,4135
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNISLSQ8[7]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNISLSQ8[7]:P,4449
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNISLSQ8[7]:S,4135
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNISLSQ8[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13]:B,6473
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13]:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13]:CC,5606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13]:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13]:S,5606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[10]:A,5966
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[10]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[10]:Y,5966
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:CLK,3889
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:D,8723
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:Q,3889
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2[0]:A,4846
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2[0]:B,4815
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2[0]:Y,4815
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_11_140_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_11_140_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_11_140_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_11_140_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_14:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_14:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17:B,5691
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17:C,7683
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17:CC,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17:S,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:CLK,7209
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:D,7112
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:Q,7209
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:CLK,392
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:D,8680
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:Q,392
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_9:A,3601
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_9:B,5109
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_9:P,3601
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_9:UB,5109
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m0_2_03_1_0:A,4178
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m0_2_03_1_0:B,4096
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m0_2_03_1_0:Y,4096
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_18:A,2368
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_18:B,2393
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_18:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_18:IPA,2368
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_18:IPB,2393
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1:B,1445
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1:CC,1806
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1:P,1445
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1:S,1806
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[1]:A,6523
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[1]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[1]:Y,6523
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20:B,6927
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20:CC,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20:P,6927
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:CLK,5953
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:D,6192
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:Q,5953
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_qb_dly:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:C,6724
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_4:IPC,6724
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:CLK,6756
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:D,6896
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:Q,6756
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[25]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[25]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[25]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[25]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_27:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_27:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:CLK,4516
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:Q,4516
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4:B,3295
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4:CC,2682
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4:S,2682
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:CLK,4196
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:Q,4196
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO_0:A,5625
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO_0:B,5531
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO_0:C,3674
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO_0:D,3594
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_15_RNO_0:Y,3594
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[6]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[6]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[6]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_s_piout_1:A,338
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_s_piout_1:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_s_piout_1:Y,261
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:CLK,6814
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:Q,6814
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:D,7659
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:Q,7920
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_10:B,3048
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_10:UB,3048
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_13:B,6877
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_13:CC,6888
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_13:P,6877
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_13:S,6888
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_13:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_76:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_76:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_76:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_76:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_76:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]:A,1773
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]:B,2283
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]:C,3971
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]:D,3854
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]:Y,1773
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_1:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_1:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_1:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_1:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_14:A,6912
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_14:B,6869
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_14:C,5701
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_14:D,5806
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_14:Y,5701
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:B,7808
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:C,6754
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:IPB,7808
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:C,6740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:IPC,6740
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:C,6791
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_1:IPC,6791
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:CLK,2754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:D,1626
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:Q,2754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:CLK,2723
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:D,8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:Q,2723
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:IPENn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:C,6828
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPC,6828
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[43]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[43]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[43]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[43]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[43]:Y,88
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[1]:A,6137
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[1]:B,7896
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[1]:C,4669
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[1]:D,5829
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[1]:Y,4669
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2[2]:A,2491
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2[2]:B,2430
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2[2]:C,6136
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2[2]:Y,2430
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_0_sqmuxa_0_a4:A,6918
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_0_sqmuxa_0_a4:B,6834
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_0_sqmuxa_0_a4:Y,6834
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:C,6802
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPC,6802
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:CLK,4112
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:D,6837
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:Q,4112
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_12:A,4195
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_12:B,6016
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_12:P,4195
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_12:UB,6016
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13:A,1921
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13:B,1524
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13:CC,1249
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13:P,1842
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13:S,1249
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13:UB,1524
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_9:A,7147
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_9:B,6933
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_9:CC,6887
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_9:P,7026
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_9:S,6887
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_9:UB,6933
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[0]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[0]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[0]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9_RNO:A,5235
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9_RNO:B,3760
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9_RNO:C,5113
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9_RNO:Y,3760
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:CLK,7869
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:Q,7869
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0:B,6716
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0:C,2598
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0:CC,2056
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0:D,5483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0:S,2056
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0:UB,2598
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:CLK,6879
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:D,7672
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:Q,6879
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:CLK,4878
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:D,6983
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:Q,4878
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_19:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_19:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_33:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_33:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2[6]:A,3057
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2[6]:B,2974
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2[6]:C,2922
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_o2[6]:Y,2922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:CLK,4279
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:Q,4279
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[13]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[13]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[13]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[10]:A,5775
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[10]:B,6974
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[10]:C,6499
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[10]:CC,5767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[10]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[10]:P,5775
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[10]:S,5767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[10]:UB,6499
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:CLK,4626
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:D,7711
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:Q,4626
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count_incr:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:CLK,6731
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:D,5230
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:Q,6731
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_29:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_29:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_29:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_29:CC,6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_29:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_29:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_29:S,6603
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_29:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:B,7657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:C,6807
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:D,7641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPB,7657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPC,6807
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPD,7641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[19]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[19]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[19]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[19]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[19]:Y,1300
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[10]:A,2127
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[10]:B,2999
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[10]:C,5281
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[10]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[10]:D,5136
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[10]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[10]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[10]:Y,2127
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:C,6727
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_14:IPC,6727
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:CLK,4099
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:D,8681
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:Q,4099
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[11]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_118:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_118:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_118:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_118:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:D,3315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[24]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]:A,2836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]:B,3230
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]:C,5054
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]:D,4930
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[3]:Y,2836
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_19:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_19:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17_FCINST1:CC,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17_FCINST1:CO,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:CLK,7005
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:Q,7005
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[25]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[13]:A,2854
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[13]:B,3726
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[13]:C,6023
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[13]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[13]:D,5863
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[13]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[13]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[13]:Y,2854
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_axb_0_i_0:A,6336
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_axb_0_i_0:B,6368
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_axb_0_i_0:C,7836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_axb_0_i_0:Y,6336
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:D,8427
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:EN,5910
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:Q,7882
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_13:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_13:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[5]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[5]:B,6967
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[5]:C,7011
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[5]:CC,7074
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[5]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[5]:P,6967
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[5]:S,7074
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_21:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_21:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[4]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[4]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[4]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[4]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:D,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15]:SLn,
QA_I_ibuf/U0/U_IOINFF:A,6193
QA_I_ibuf/U0/U_IOINFF:Y,6193
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_9:A,4626
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_9:B,4414
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_9:CC,4308
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_9:P,4507
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_9:S,4308
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_9:UB,4414
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_3:A,1634
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_3:B,1373
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_3:P,1484
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_3:UB,1373
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:CLK,5248
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:D,3852
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:Q,5248
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:C,6841
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPC,6841
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_3:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:CLK,1645
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:Q,1645
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[12]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[12]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[12]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_11:A,4096
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_11:B,4048
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_11:C,3974
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_11:D,3866
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_11:Y,3866
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:CLK,5111
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:D,3951
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:Q,5111
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[0]:A,7977
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[0]:B,7880
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[0]:C,7862
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[0]:D,7781
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[0]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:D,5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un103_s_state_i_a3_0_a2:A,2053
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un103_s_state_i_a3_0_a2:B,2909
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un103_s_state_i_a3_0_a2:Y,2053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_4:B,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_4:CC,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_4:S,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:CLK,1514
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:Q,1514
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO_0:A,5460
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO_0:B,5366
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO_0:C,3509
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO_0:D,3268
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6_RNO_0:Y,3268
A0_PWM_VL_O_obuf/U0/U_IOENFF:A,
A0_PWM_VL_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AL_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SD_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SL_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[0],6757
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[10],6818
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[11],6738
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[12],6763
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[13],6711
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[14],6705
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[15],6731
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[16],6745
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[17],6762
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[1],6733
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[2],6724
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[3],6697
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[4],6709
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[5],6733
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[6],6772
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[7],6747
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[8],6754
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[9],6747
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_EN[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_EN[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[0],6791
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[10],6802
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[11],6844
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[12],6795
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[13],6814
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[14],6833
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[15],6859
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[16],6835
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[17],6804
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[1],6841
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[2],6847
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[3],6807
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[4],6810
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[5],6828
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[6],6771
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[7],6818
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[8],6754
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[9],6809
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_EN[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_EN[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CARRYIN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[10],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[11],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[12],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[13],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[14],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[15],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[16],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[17],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[18],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[19],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[20],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[21],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[22],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[23],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[24],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[25],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[26],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[27],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[28],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[29],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[2],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[30],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[31],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[32],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[33],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[34],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[35],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[36],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[37],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[38],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[39],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[3],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[40],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[41],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[42],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[43],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[4],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[5],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[6],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[7],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[8],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[9],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[10],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[11],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[12],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[13],7718
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[14],7714
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[15],7787
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[16],7815
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[17],7806
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[18],7809
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[19],7866
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[20],7863
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[21],7849
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[22],7856
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[23],7853
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[24],7832
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[25],7933
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[26],7919
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[27],7884
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[28],7946
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[29],7895
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[2],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[30],7886
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[31],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[32],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[33],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[34],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[35],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[36],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[37],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[38],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[39],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[3],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[40],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[41],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[42],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[43],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[4],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[5],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[6],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[7],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[8],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[9],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_EN[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_EN[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:DOTP,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:OVFL_CARRYOUT_SEL,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[13],8724
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[14],8723
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[15],8724
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[16],8719
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[17],8717
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[18],8693
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[19],8688
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[20],8691
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[21],8689
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[22],8690
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[23],8689
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[24],8684
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[25],8683
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[26],8687
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[27],8686
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[28],8686
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[29],8681
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[30],8683
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_CLK[0],8717
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_CLK[1],8681
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_EN[0],8996
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_EN[1],9019
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SIMD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_AD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_AL_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_SD_N,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_SL_N,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0:A,4379
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0:B,4108
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0:P,4260
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0:UB,4108
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[10]:A,6188
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[10]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[10]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[10]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[10]:Y,2538
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:CLK,5037
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:Q,5037
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[9]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_139:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_139:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_139:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_139:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_139:IPB,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[5]:A,1718
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[5]:B,4418
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[5]:C,2897
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[5]:Y,1718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3]:B,6473
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3]:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3]:CC,5814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3]:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3]:S,5814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_2:B,1529
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_2:C,1147
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_2:CC,1349
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_2:P,1147
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_2:S,1349
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[7]:A,2014
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[7]:B,3384
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[7]:C,5123
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[7]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[7]:D,4974
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[7]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[7]:Y,2014
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[14]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[14]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[14]:Y,5379
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_9:A,6279
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_9:B,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_9:P,6233
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_9:UB,6183
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:CLK,5281
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:Q,5281
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUTKU[1]:A,6815
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUTKU[1]:B,6439
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUTKU[1]:C,6361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUTKU[1]:Y,6361
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIJ3AL9[5]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIJ3AL9[5]:B,4220
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIJ3AL9[5]:C,7056
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIJ3AL9[5]:CC,4453
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIJ3AL9[5]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIJ3AL9[5]:P,4220
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIJ3AL9[5]:S,4453
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIJ3AL9[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_10:B,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_10:UB,4242
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[3]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[3]:B,5054
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[3]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[3]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[3]:Y,2538
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:CLK,4823
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:Q,4823
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_25:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_25:IPENn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[13]:A,4470
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[13]:B,2803
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[13]:C,2849
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[13]:D,2468
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[13]:Y,2468
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:D,5559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_15:EN,8996
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_15:IPENn,8996
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[23]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[23]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[23]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:CLK,4554
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:Q,4554
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:CLK,7070
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:D,6912
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:Q,7070
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:D,5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_9:A,5509
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_9:B,5144
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_9:CC,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_9:P,5232
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_9:S,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_9:UB,5144
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_4_0:A,3266
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_4_0:B,7027
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_4_0:C,6565
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_4_0:CC,2256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_4_0:D,4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_4_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_4_0:S,2256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_4_0:UB,4407
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:B,7742
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:C,6828
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:D,7691
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPB,7742
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPC,6828
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPD,7691
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:CLK,7662
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:Q,7662
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHPOD5[3]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHPOD5[3]:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHPOD5[3]:C,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHPOD5[3]:CC,3964
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHPOD5[3]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHPOD5[3]:P,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHPOD5[3]:S,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHPOD5[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI993B1[3]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI993B1[3]:B,7792
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI993B1[3]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI993B1[3]:CC,7044
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI993B1[3]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI993B1[3]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI993B1[3]:S,7044
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNI993B1[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[10],4242
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[11],4287
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[1],4620
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[2],4719
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[3],4290
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[4],4253
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[5],4299
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[6],4230
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[7],4214
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[8],4244
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CC[9],4308
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:CO,4108
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[0],4260
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[1],4230
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[2],4404
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[3],4389
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[6],4401
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[7],4430
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[8],4511
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:P[9],4507
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[0],4108
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[10],4428
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[11],4534
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[1],4222
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[2],4368
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[3],4260
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[4],4293
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[5],4400
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[6],4299
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[7],4353
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[8],4443
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_0:UB[9],4414
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[4]:A,3506
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[4]:B,5953
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[4]:Y,3506
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17_FCINST1:CC,2777
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17_FCINST1:CO,2777
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:CLK,6796
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:D,4992
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:Q,6796
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_reset_speed_counter:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:CLK,3988
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:D,8717
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:Q,3988
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[27]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[27]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[27]:Y,7555
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:CLK,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:D,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:Q,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:CLK,6844
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:Q,6844
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:C,6841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPC,6841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPD,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[13]:A,2803
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[13]:B,2854
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[13]:C,5268
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[13]:D,5193
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[13]:Y,2803
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:CLK,3667
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:D,7059
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:Q,3667
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_8_0:A,2635
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_8_0:B,7041
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_8_0:C,6563
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_8_0:CC,1760
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_8_0:D,4405
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_8_0:P,2635
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_8_0:S,1760
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_8_0:UB,4405
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:CLK,5913
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:D,8801
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:Q,5913
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[5]:A,5767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[5]:B,7000
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[5]:C,6530
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[5]:CC,5775
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[5]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[5]:P,5767
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[5]:S,5775
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[5]:UB,6530
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_10:B,1350
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_10:UB,1350
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:D,8664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:CLK,6870
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:D,8716
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:EN,8389
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:Q,6870
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_1:A,1930
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_1:B,1844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_1:P,1844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_1:UB,1870
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_5:B,4421
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_5:C,4260
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_5:P,4260
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_5:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:B,7787
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:C,6818
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:IPB,7787
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[10],5059
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[11],4998
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[1],5663
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[2],5599
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[3],5261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[4],5191
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[5],5130
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[6],5176
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[7],5106
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[8],5046
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CC[9],5139
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:CO,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[0],1367
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[1],1323
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[2],1497
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[3],1481
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[6],1503
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[7],1516
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[8],1598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:P[9],1601
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[0],1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[10],1519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[11],1640
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[1],1330
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[2],1454
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[3],1373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[4],1411
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[5],1503
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[6],1394
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[7],1452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[8],1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_0:UB[9],1501
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:D,5545
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[4]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[4]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[4]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:CLK,1539
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:D,6251
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:Q,1539
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:C,6731
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:IPC,6731
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:CLK,6195
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:Q,6195
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[12]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[12]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[12]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[12]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_13/config_reg_i_RNI30RC[3]:A,6908
BLDC_Encoder_Axis_0/MSC_i_13/config_reg_i_RNI30RC[3]:B,6864
BLDC_Encoder_Axis_0/MSC_i_13/config_reg_i_RNI30RC[3]:Y,6864
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[2]:A,4857
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[2]:B,4809
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[2]:C,4722
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[2]:D,4624
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO_2[2]:Y,4624
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_1:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_16:A,6402
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_16:B,6207
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_16:CC,5395
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_16:S,5395
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_16:UB,6207
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:CLK,4174
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:Q,4174
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:B,7895
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:C,6795
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:IPB,7895
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:IPC,6795
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:CLK,2219
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:D,6554
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:Q,2219
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_o2_RNIFRD03[1]:A,3088
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_o2_RNIFRD03[1]:B,2914
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_o2_RNIFRD03[1]:C,2083
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_o2_RNIFRD03[1]:D,1445
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_o2_RNIFRD03[1]:Y,1445
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[4]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[4]:B,5191
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[4]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[4]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[4]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:C,6844
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPC,6844
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_23:IPD,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_24_0:A,1885
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_24_0:B,1159
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_24_0:C,1232
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_24_0:CC,463
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_24_0:D,-9
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_24_0:P,150
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_24_0:S,463
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_24_0:UB,-9
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_23:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_23:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[15]:A,5038
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[15]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[15]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[15]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[15]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:CLK,1355
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:D,1298
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:Q,1355
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_0_i_0:A,6342
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_0_i_0:B,6368
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_0_i_0:C,5207
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_0_i_0:Y,5207
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[3]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[3]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[3]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[29]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[29]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[29]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_s[13]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_s[13]:B,7779
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_s[13]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_s[13]:CC,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_s[13]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_s[13]:P,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_s[13]:S,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_s[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[10]:A,4833
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[10]:B,4785
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[10]:C,4336
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[10]:Y,4336
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:CLK,972
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:D,1788
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:Q,972
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_1:B,4499
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_1:C,4310
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_1:CC,4604
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_1:P,4310
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_1:S,4604
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_1:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_6_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_6_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_6_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_6_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_4:A,7848
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_4:B,6976
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_4:CC,7078
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_4:S,7078
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_4:UB,6976
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[29]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[29]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[29]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[29]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_33:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_33:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:CLK,4607
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:Q,4607
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[13]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[13]:B,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[13]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:D,3676
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[11]:A,4901
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[11]:B,4824
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[11]:C,4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[11]:Y,4407
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNICF962[19]:A,4593
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNICF962[19]:B,3611
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNICF962[19]:C,3567
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNICF962[19]:Y,3567
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:CLK,3723
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:D,7112
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:Q,3723
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[14]:A,6985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[14]:B,6901
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[14]:C,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[14]:Y,6226
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_109:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_109:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_109:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_109:IPA,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_start_i_0_a2:A,4233
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_start_i_0_a2:B,4358
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_start_i_0_a2:Y,4233
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[13]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[13]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[13]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[13]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[3]:A,2922
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[3]:B,1737
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[3]:C,4791
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[3]:D,3710
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[3]:Y,1737
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_33:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_33:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[7]:A,7206
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[7]:B,5158
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[7]:C,4926
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[7]:CC,4840
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[7]:D,6702
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[7]:P,5033
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[7]:S,4840
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[7]:UB,4926
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[9]:A,4406
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[9]:B,2027
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[9]:C,4284
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[9]:Y,2027
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[10]:A,1963
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[10]:B,2835
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[10]:C,5117
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[10]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[10]:D,4978
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[10]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[10]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[10]:Y,1963
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:CLK,3564
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:D,1540
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:Q,3564
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:CLK,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:D,4341
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:Q,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[13]:A,6100
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[13]:B,6056
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[13]:C,5340
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[13]:Y,5340
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[9]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_6:B,3555
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_6:CC,3559
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_6:P,3555
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_6:S,3559
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[10],7065
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[11],7004
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[1],7531
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[2],7467
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[3],7195
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[4],7127
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[5],7077
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[6],7203
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[7],7112
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[8],7052
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CC[9],7149
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:CO,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[0],6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[1],6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[2],6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[3],6837
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[6],6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[7],6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[8],6910
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:P[9],6957
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[13]:A,2849
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[13]:B,3721
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[13]:C,6018
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[13]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[13]:D,5864
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[13]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[13]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[13]:Y,2849
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[8]:A,1501
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[8]:B,5218
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[8]:Y,1501
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[33]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[33]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[33]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:CLK,3983
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:D,8716
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:Q,3983
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:CLK,7787
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:Q,7787
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_0[6]:A,6840
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_0[6]:B,6822
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_0[6]:C,3564
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_0[6]:D,5705
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_0[6]:Y,3564
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o_1_sqmuxa_0_a2:A,5294
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o_1_sqmuxa_0_a2:B,5534
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o_1_sqmuxa_0_a2:C,3102
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o_1_sqmuxa_0_a2:D,5222
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o_1_sqmuxa_0_a2:Y,3102
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_24:A,7144
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_24:B,6911
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_24:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_24:CC,6920
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_24:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_24:P,7058
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_24:S,6920
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_24:UB,6911
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIKJVI1[0]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIKJVI1[0]:B,5855
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIKJVI1[0]:C,6917
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIKJVI1[0]:CC,7455
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIKJVI1[0]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIKJVI1[0]:P,5855
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIKJVI1[0]:S,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIKJVI1[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[3]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[3]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[3]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[3]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:D,5447
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIQUIU[0]:A,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIQUIU[0]:B,7355
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIQUIU[0]:Y,6366
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:CLK,3709
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:D,6878
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:Q,3709
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:CLK,2100
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:D,1981
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:Q,2100
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_7_0:A,2514
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_7_0:B,7070
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_7_0:C,6620
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_7_0:CC,1923
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_7_0:D,4454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_7_0:P,2514
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_7_0:S,1923
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_7_0:UB,4454
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[10]:A,6160
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[10]:B,6112
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[10]:C,5408
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[10]:Y,5408
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:CLK,3403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:D,8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:Q,3403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_8:A,5224
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_8:B,5282
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_8:CC,5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_8:P,5224
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_8:S,5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_8:UB,5282
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[8]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[8]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[8]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_29:A,7848
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_29:B,7178
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_29:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_29:CC,6742
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_29:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_29:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_29:S,6742
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_29:UB,7178
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[5]:A,6985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[5]:B,6901
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[5]:C,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[5]:Y,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[2]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[2]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[2]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[2]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:CLK,6704
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:D,6838
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:Q,6704
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:D,5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:CLK,7856
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:Q,7856
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0:A,6123
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0:B,5879
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0:C,5796
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0:P,5948
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0:UB,5796
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_13:A,4964
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_13:B,4878
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_13:P,4878
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_13:UB,4898
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_3:A,5686
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_3:B,5609
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_3:C,5564
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_3:D,5486
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_3:Y,5486
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_24:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_24:B,7077
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_24:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_24:CC,6781
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_24:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_24:P,7077
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_24:S,6781
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_24:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[3]:A,6014
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[3]:B,5966
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[3]:C,5255
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[3]:Y,5255
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO:A,5566
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO:B,5518
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO:C,3668
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO:D,3520
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO:Y,3520
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_285:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_285:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_285:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_285:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_285:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI37LDM[1]:A,6991
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI37LDM[1]:B,1688
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI37LDM[1]:C,1758
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI37LDM[1]:CC,1233
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI37LDM[1]:D,6272
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI37LDM[1]:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI37LDM[1]:S,1233
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI37LDM[1]:UB,1688
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:CLK,5097
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:Q,5097
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:CLK,1503
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:D,8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:Q,1503
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_3:A,4084
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_3:B,5999
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_3:P,4084
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_3:UB,5999
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17:B,4022
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_17:UB,4022
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:CLK,2928
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:Q,2928
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[2]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[2]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[2]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[2]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[1]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[1]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[1]:Y,7440
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_wmux_0[11]:A,2875
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_wmux_0[11]:B,4144
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_wmux_0[11]:C,5983
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_wmux_0[11]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_wmux_0[11]:D,5829
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_wmux_0[11]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_wmux_0[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_wmux_0[11]:Y,2875
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_5_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_5_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_5_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_5_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_10_0:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_10_0:B,6563
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_10_0:C,5408
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_10_0:CC,5235
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_10_0:D,6864
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_10_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_10_0:S,5235
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_10_0:UB,5408
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:CLK,3323
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:D,8684
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:Q,3323
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:CLK,301
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:D,7002
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:Q,301
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[2]:A,6550
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[2]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[2]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[2]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[2]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[3]:A,1417
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[3]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[3]:Y,1417
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:CLK,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:Q,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1_FCINST1:CC,1002
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1_FCINST1:CO,1002
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_RNI7K2Q1_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_16:B,2844
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_16:UB,2844
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[10]:A,1974
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[10]:B,3344
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[10]:C,5072
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[10]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[10]:D,4934
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[10]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[10]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[10]:Y,1974
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:CLK,1395
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:D,6523
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:Q,1395
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:CLK,6197
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:D,8674
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:Q,6197
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[10]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[10]:B,4449
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[10]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[10]:Y,91
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_12:A,2163
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_12:B,1925
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_12:P,2077
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_12:UB,1925
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10:B,3516
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10:C,3554
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10:CC,3454
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10:S,3454
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10:UB,3516
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_13:B,5098
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_13:C,4927
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_13:CC,4089
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_13:S,4089
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_13:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[13]:A,2861
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[13]:B,4231
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[13]:C,5975
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[13]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[13]:D,5821
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[13]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[13]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[13]:Y,2861
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_27:A,7252
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_27:B,7048
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_27:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_27:CC,6874
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_27:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_27:P,7166
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_27:S,6874
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_27:UB,7048
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:CLK,4353
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:D,4840
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:Q,4353
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:CLK,1529
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:D,8683
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:Q,1529
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[22]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:CLK,6807
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:Q,6807
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:CLK,6754
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:Q,6754
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5:B,3520
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5:C,3538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5:CC,3654
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5:S,3654
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5:UB,3520
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16_FCINST1:CC,4364
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16_FCINST1:CO,4364
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_16_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:CLK,6839
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:D,5878
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:Q,6839
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNIIL4Q[1]:A,7792
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNIIL4Q[1]:B,7631
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNIIL4Q[1]:C,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNIIL4Q[1]:Y,6283
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:CLK,7553
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:D,8834
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:EN,7861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:Q,7553
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_pi_done:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:CLK,7871
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:Q,7871
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:IPENn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[10]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[10]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[10]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_7:A,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_7:B,6122
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_7:P,6167
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_7:UB,6122
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNI3VQE[6]:A,3751
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNI3VQE[6]:B,3674
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNI3VQE[6]:Y,3674
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:CLK,6724
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:Q,6724
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[13]:A,5480
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[13]:B,5777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[13]:C,4380
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[13]:D,5218
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[13]:Y,4380
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1:A,6714
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1:B,3411
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1:C,3348
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1:CC,4108
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1:P,3348
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1:S,4108
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1:UB,3372
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[11]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[11]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[11]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[5]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[5]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[5]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[5]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[16]:A,4967
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[16]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[16]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[16]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[16]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:C,6835
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPC,6835
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:CLK,6740
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:D,6921
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:Q,6740
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_3:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:CLK,7864
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:Q,7864
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_7:A,2136
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_7:B,2088
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_7:C,2014
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_7:D,1920
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_7:Y,1920
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[14]:A,6290
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[14]:B,6213
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[14]:C,5827
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[14]:D,4597
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[14]:Y,4597
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO_0:A,5658
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO_0:B,5620
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO_0:C,3723
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO_0:D,3673
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19_RNO_0:Y,3673
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11_RNO:A,5834
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11_RNO:B,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11_RNO:C,5712
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11_RNO:Y,4359
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:CLK,6757
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:D,8820
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:Q,6757
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_51:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_51:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_51:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_51:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_51:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[9]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[3]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[3]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[3]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18_FCINST1:CC,1261
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18_FCINST1:CO,1261
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_18_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:CLK,6286
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:Q,6286
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_18:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_18:IPENn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_89:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_89:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_89:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_89:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_89:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:CLK,4121
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:D,8717
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:Q,4121
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:CLK,7740
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:D,8847
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:EN,
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:Q,7740
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_olmng_done:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_16_0:A,3351
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_16_0:B,7319
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_16_0:C,6838
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_16_0:CC,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_16_0:D,4673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_16_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_16_0:S,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_16_0:UB,4673
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:CLK,4273
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:D,8718
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:Q,4273
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[27]:A,498
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[27]:B,421
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[27]:C,-119
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[27]:Y,-119
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_5:B,2712
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_5:UB,2712
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:CLK,5094
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:Q,5094
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_axb_0_i_0:A,6630
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_axb_0_i_0:B,7870
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_axb_0_i_0:Y,6630
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:C,6835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPC,6835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPD,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_9:B,2271
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_9:C,1887
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_9:CC,1152
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_9:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_9:S,1152
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[30]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[30]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[30]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[30]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[30]:Y,-45
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIO3N22[9]:A,3425
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIO3N22[9]:B,4333
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIO3N22[9]:C,3348
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIO3N22[9]:Y,3348
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_2:A,7093
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_2:B,7015
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_2:CC,7467
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_2:P,7051
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_2:S,7467
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_2:UB,7015
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[11]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[11]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[11]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[11]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_14:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_14:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_6:A,4974
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_6:B,4829
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_6:P,4888
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_6:UB,4829
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[10]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[10]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[10]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[10]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[10],2710
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[11],2783
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[1],2975
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[2],3036
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[3],2712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[4],2682
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[5],2712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[6],2722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[7],2698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[8],2752
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CC[9],2771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:CO,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[0],2610
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[1],2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[2],2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[3],2765
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[6],2777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[7],2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[8],2843
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:P[9],2883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_0_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:CLK,5897
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:D,8706
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:Q,5897
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_axb_25_1:A,5710
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_axb_25_1:B,3836
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_axb_25_1:C,3762
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_axb_25_1:Y,3762
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:C,6841
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPC,6841
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:D,6557
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:CLK,6244
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:Q,6244
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_22:EN,9019
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_22:IPENn,9019
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:B,7919
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:C,6844
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:D,7884
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPB,7919
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPC,6844
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPD,7884
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[14]:A,6744
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[14]:B,3431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[14]:C,3290
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[14]:D,2208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[14]:Y,2208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:CLK,4927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:Q,4927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:CLK,7074
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:Q,7074
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:CLK,6841
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:Q,6841
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_21:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_21:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[13]:A,5931
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[13]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[13]:Y,5931
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_16:B,5205
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_16:UB,5205
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:CLK,5057
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:D,6740
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:Q,5057
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[20]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o_1_sqmuxa_0_a2:A,7836
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o_1_sqmuxa_0_a2:B,7801
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o_1_sqmuxa_0_a2:C,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o_1_sqmuxa_0_a2:Y,6734
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3:B,4537
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3:CC,4468
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3:P,4537
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3:S,4468
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_3_0:A,5481
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_3_0:B,6395
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_3_0:C,5255
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_3_0:CC,5469
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_3_0:D,6696
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_3_0:P,5358
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_3_0:S,5469
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_3_0:UB,5255
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[11]:A,7115
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[11]:B,5067
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[11]:C,4909
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[11]:CC,4708
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[11]:D,6662
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[11]:P,4942
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[11]:S,4708
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[11]:UB,4909
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_12:B,4605
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_12:C,4444
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_12:CC,4195
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_12:P,4444
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_12:S,4195
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:D,6548
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:CLK,3130
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:D,2167
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:Q,3130
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:CLK,7556
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:D,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:Q,7556
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_13:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_13:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:CLK,6875
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:D,7005
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:Q,6875
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_4:B,4253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_4:UB,4253
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI0FBBG[14]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI0FBBG[14]:B,7339
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI0FBBG[14]:C,3074
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI0FBBG[14]:CC,2897
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI0FBBG[14]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI0FBBG[14]:P,3074
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI0FBBG[14]:S,2897
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI0FBBG[14]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_12:A,2656
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_12:B,2606
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_12:P,2656
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_12:UB,2606
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:CLK,1316
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:Q,1316
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:CLK,2723
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:D,3272
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:Q,2723
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:CLK,147
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:D,7151
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:Q,147
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[6]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[6]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[6]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[6]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:CLK,4253
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:D,6932
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:Q,4253
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[4]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_270:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_270:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_270:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_270:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_270:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:CLK,1400
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:Q,1400
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[22]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[22]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[22]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[22]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_6:A,6244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_6:B,4230
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_6:P,4293
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_6:UB,4230
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]_CC_0:UB[9],
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:CLK,5093
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:Q,5093
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_8:B,1645
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_8:C,1490
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_8:CC,1510
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_8:P,1490
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_8:S,1510
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_8:A,4367
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_8:B,6186
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_8:P,4367
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_8:UB,6186
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[1]:A,4753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[1]:B,4709
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[1]:C,4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[1]:Y,4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI5E0J[10]:A,2847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI5E0J[10]:B,2770
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI5E0J[10]:C,2327
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI5E0J[10]:Y,2327
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12]:B,5842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12]:C,6120
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12]:CC,5664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12]:P,5842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12]:S,5664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[2]:A,1773
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[2]:B,3143
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[2]:C,4886
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[2]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[2]:D,4733
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[2]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[2]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[2]:Y,1773
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_i_a3_0_0[1]:A,5987
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_i_a3_0_0[1]:B,5998
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_i_a3_0_0[1]:Y,5987
A0_PWM_VH_O_obuf/U0/U_IOPAD:D,4315
A0_PWM_VH_O_obuf/U0/U_IOPAD:E,
A0_PWM_VH_O_obuf/U0/U_IOPAD:PAD,4315
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]:A,2070
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]:B,1563
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]:C,3823
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]:D,3705
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]:Y,1563
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[27]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[27]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[27]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[27]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:CLK,4604
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:Q,4604
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:CLK,4055
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:D,5710
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:Q,4055
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_4:A,1779
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_4:B,1422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_4:C,288
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_4:D,905
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_4:Y,288
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_i[1]:A,7931
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_i[1]:B,6939
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_i[1]:C,5987
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_i[1]:D,4843
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_i[1]:Y,4843
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[12]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[12]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[12]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[12]:Y,7507
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:CC[6],1002
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:CI,1088
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[0],1144
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[1],1002
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[3],1484
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[0],1213
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[1],1255
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[2],1494
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[15]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[15]:B,5039
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[15]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[15]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[15]:Y,3584
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[8]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITTLU[1]:A,6946
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITTLU[1]:B,6595
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITTLU[1]:C,6492
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITTLU[1]:Y,6492
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:CLK,7681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:D,8458
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:Q,7681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6:A,7100
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6:B,6965
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6:CC,7056
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6:P,7054
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6:S,7056
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6:UB,6965
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:CLK,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:D,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:Q,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17_FCINST1:CC,4170
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17_FCINST1:CO,4170
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:CLK,2089
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:Q,2089
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:CLK,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:Q,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:CLK,1118
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:D,1487
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:Q,1118
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[23]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[23]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[23]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[23]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_13:A,5985
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_13:B,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_13:CC,5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_13:S,5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_13:UB,4995
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc3:A,6940
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc3:B,7890
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc3:Y,6940
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNIGRSG1:A,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNIGRSG1:B,7748
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNIGRSG1:C,4298
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNIGRSG1:D,4309
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNIGRSG1:Y,3420
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[10]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[10]:B,5059
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[10]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[10]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[10]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[4]:A,3945
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[4]:B,2760
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[4]:C,5854
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[4]:D,4733
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3[4]:Y,2760
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[13]:A,3510
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[13]:B,3390
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[13]:C,2444
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[13]:D,2357
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[13]:Y,2357
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:CLK,3797
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:EN,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:Q,3797
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_28:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_28:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_28:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_28:CC,6664
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_28:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_28:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_28:S,6664
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_28:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4]:B,6473
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4]:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4]:CC,5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4]:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4]:S,5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITCGM[5]:A,3788
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITCGM[5]:B,3705
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITCGM[5]:C,3427
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITCGM[5]:Y,3427
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0[2]:A,4111
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0[2]:B,2653
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0[2]:C,3185
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0[2]:D,1762
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0[2]:Y,1762
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[14]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[14]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[14]:Y,5379
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:CLK,6859
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:Q,6859
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:CC[0],4341
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:CI,4341
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_4:B,1169
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_4:UB,1169
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_6:B,5189
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_6:CC,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_6:P,5189
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_6:S,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_6:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]:C,4947
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]:D,4823
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]:Y,4823
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:CLK,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:D,7893
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:EN,7792
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:Q,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_6:A,7041
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_6:B,6824
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_6:CC,6928
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_6:P,6926
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_6:S,6928
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_6:UB,6824
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:CLK,4986
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:D,6659
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:Q,4986
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[9]:A,1982
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[9]:B,4138
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[9]:C,1606
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[9]:D,1818
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[9]:Y,1606
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8:B,4615
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8:P,4615
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8:S,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[8]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[8]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[8]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:CLK,1828
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:Q,1828
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_9:B,2323
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_9:C,2135
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_9:CC,1397
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_9:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_9:S,1397
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_5:B,1539
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_5:C,1384
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_5:CC,1523
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_5:P,1384
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_5:S,1523
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[8]:A,6111
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[8]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[8]:Y,6111
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[2]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[2]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[2]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[2]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[2]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[2]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[2]:Y,4589
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_176:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_176:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_176:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_176:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_176:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:CLK,6709
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:D,5401
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:Q,6709
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:CLK,5797
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:Q,5797
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_16:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_16:B,7376
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_16:CC,6720
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_16:S,6720
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_16:UB,7376
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:D,5340
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:CLK,4106
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:D,5631
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:Q,4106
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[7]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[7]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[7]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[7]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:CLK,7012
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:Q,7012
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[42]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[42]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[42]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10:A,2202
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10:B,1530
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10:CC,1293
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10:S,1293
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10:UB,1530
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:CLK,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:Q,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:CO,4652
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[0],4761
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[1],4717
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[2],4891
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[3],4876
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[6],4888
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[7],4928
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[8],4998
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:P[9],4994
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[0],4652
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[10],4958
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[11],5064
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[1],4752
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[2],4898
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[3],4790
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[4],4823
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[5],4930
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[6],4829
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[7],4883
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[8],4973
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_0:UB[9],4944
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:CLK,7703
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:D,4087
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:Q,7703
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:CLK,6130
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:D,8680
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:Q,6130
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:D,5453
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_27:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_27:B,7332
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_27:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_27:CC,6735
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_27:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_27:P,7332
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_27:S,6735
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_27:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_6:A,4875
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_6:B,2875
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_6:P,2991
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_6:UB,2875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNISCVC2[2]:A,5806
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNISCVC2[2]:B,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNISCVC2[2]:C,6518
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNISCVC2[2]:D,6185
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNISCVC2[2]:Y,4796
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIJNA62[23]:A,4620
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIJNA62[23]:B,3638
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIJNA62[23]:C,3594
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIJNA62[23]:Y,3594
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:CLK,6834
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:D,6261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:Q,6834
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[3]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:CLK,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:D,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:Q,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:CLK,6791
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:Q,6791
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:D,3197
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:CLK,4096
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:D,7351
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:Q,4096
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKAISG[10]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKAISG[10]:B,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKAISG[10]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKAISG[10]:CC,4220
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKAISG[10]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKAISG[10]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKAISG[10]:S,4220
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKAISG[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[11]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[11]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[11]:C,5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[11]:Y,5095
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2:A,308
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2:B,-393
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2:C,268
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2:D,205
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2:Y,-393
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:CLK,2063
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:D,5650
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:Q,2063
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_20:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_20:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:B,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:C,6757
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_0:IPC,6757
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:CLK,738
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:D,8682
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:Q,738
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[17]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[34]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[34]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[34]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:CLK,4237
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:Q,4237
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT51DM[17]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT51DM[17]:B,4308
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT51DM[17]:C,7521
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT51DM[17]:CC,3796
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT51DM[17]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT51DM[17]:P,4308
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT51DM[17]:S,3796
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIT51DM[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[14]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[14]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[14]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_12:A,5606
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_12:B,5527
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_12:CC,5308
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_12:P,5527
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_12:S,5308
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:CLK,6918
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:D,8867
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:Q,6918
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/mas_done_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:CLK,6807
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:Q,6807
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_4:B,6798
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_4:C,6873
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_4:CC,6133
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_4:S,6133
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_10:B,6798
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_10:C,6873
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_10:CC,5966
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_10:S,5966
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_3:A,6161
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_3:B,6029
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_3:P,6115
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_3:UB,6029
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:CLK,7691
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:Q,7691
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[11]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_4:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_4:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_4:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_4:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_4:IPC,
MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0:An,
MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0:ENn,
MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0:YNn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_144:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_144:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_144:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_144:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_277:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_277:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_277:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_277:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_277:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_11:B,4287
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_11:UB,4287
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_263:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_263:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_263:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_263:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_263:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_12:A,1573
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_12:B,1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_12:P,1375
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_12:UB,1233
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8_RNO:A,5251
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8_RNO:B,3761
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8_RNO:C,5127
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_8_RNO:Y,3761
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0_0[17]:A,3914
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0_0[17]:B,6212
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0_0[17]:C,4453
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_0_0[17]:Y,3914
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_4_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_4_PAD/U_IOINFF:Y,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_78:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_78:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_78:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_78:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_78:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[5]:A,5798
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[5]:B,6015
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[5]:C,2832
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[5]:D,2849
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[5]:Y,2832
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:CLK,3715
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:D,7531
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:Q,3715
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_13:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_13:C,7716
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_13:CC,3583
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_13:D,5360
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_13:S,3583
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_13:UB,5360
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_26:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_26:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_2:A,3072
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_2:B,2983
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_2:P,3010
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_2:UB,2983
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:D,2826
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[5]_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[8]:A,1919
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[8]:B,3289
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[8]:C,5024
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[8]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[8]:D,4879
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[8]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[8]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[8]:Y,1919
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_15:A,1636
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_15:B,1314
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_15:P,1432
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_15:UB,1314
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17:B,3783
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17:CC,2937
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17:S,2937
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_0:A,6922
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_0:B,6882
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_0:C,6453
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_0:CC,7165
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_0:P,6468
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_0:S,7165
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_0:UB,6453
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:CLK,4085
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:Q,4085
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_19:B,6506
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_19:C,4451
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_19:D,6492
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_19:IPB,6506
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_19:IPC,4451
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_19:IPD,6492
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:CLK,1721
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:D,8676
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:Q,1721
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[25]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0_0[11]:A,2054
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0_0[11]:B,4199
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0_0[11]:C,1696
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0_0[11]:D,1890
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0_0[11]:Y,1696
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:CLK,6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:Q,6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:CO,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[0],3436
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[1],2977
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[2],3088
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[3],2802
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[6],2722
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[7],2639
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[8],2661
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:P[9],2766
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[0],4183
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[10],2710
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[11],2783
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[1],2975
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[2],3036
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[3],2712
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[4],2682
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[5],2712
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[6],2722
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[7],2698
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[8],2752
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_0_CC_0:UB[9],2771
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_9:B,7527
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_9:C,7582
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_9:CC,6756
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_9:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_9:S,6756
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[10],1152
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[11],1122
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[1],1448
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[2],1468
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[3],1349
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[4],1188
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[5],1088
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[6],1275
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[7],1100
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[8],1104
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CC[9],1290
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:CO,988
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[0],1081
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[1],988
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[2],1128
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[3],1147
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[6],1159
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[7],1165
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[8],1235
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:P[9],1265
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMNNK7[7]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMNNK7[7]:B,6130
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMNNK7[7]:C,7231
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMNNK7[7]:CC,5903
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMNNK7[7]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMNNK7[7]:P,6130
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMNNK7[7]:S,5903
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMNNK7[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI7R7J[2]:A,4854
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI7R7J[2]:B,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI7R7J[2]:Y,4796
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:CLK,1885
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:D,8681
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:Q,1885
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[34]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_61:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_61:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_61:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_61:IPA,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO_0:A,5487
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO_0:B,5393
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO_0:C,3536
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO_0:D,3456
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO_0:Y,3456
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:CLK,4299
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:D,4753
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:Q,4299
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[6]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:CLK,4615
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:D,4624
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:Q,4615
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:CLK,3788
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:D,7077
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:Q,3788
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:CLK,4045
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:Q,4045
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[20]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[20]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[20]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[20]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[20]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_15:A,6420
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_15:B,4208
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_15:P,4332
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_15:UB,4208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[16]:A,4354
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[16]:B,4306
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[16]:C,3830
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[16]:Y,3830
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_226:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_226:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_226:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_226:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_226:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[7]:A,1620
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[7]:B,5339
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[7]:Y,1620
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:CLK,3787
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:D,2525
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:Q,3787
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:CLK,5124
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:Q,5124
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:CLK,6859
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:Q,6859
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12:A,1652
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12:B,1573
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12:CC,1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12:P,1573
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12:S,1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12:UB,1760
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:CLK,6485
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:D,4478
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:EN,4378
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:Q,6485
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[5]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[5]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[5]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[5]:Y,5421
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0_0[1]:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0_0[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0_0[1]:C,4074
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0_0[1]:D,4066
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_0_0[1]:Y,4066
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[33]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[33]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[33]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[33]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIV59P1[13]:A,2579
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIV59P1[13]:B,2346
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIV59P1[13]:C,2457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIV59P1[13]:Y,2346
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:CLK,4096
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:D,5650
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:Q,4096
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:CLK,1493
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:D,8710
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:Q,1493
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[8]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[8]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[8]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[8]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[16]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[16]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[16]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[16]:Y,6726
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_219:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_219:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_219:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_219:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_219:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:CLK,7806
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:Q,7806
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_15:A,7808
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_15:B,7240
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_15:C,6806
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_15:CC,6502
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_15:S,6502
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_15:UB,6806
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:CLK,7240
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:Q,7240
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0:A,1432
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0:B,1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0:P,1353
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0:UB,1233
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a2_0[2]:A,5931
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a2_0[2]:B,5893
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a2_0[2]:Y,5893
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_8:A,4469
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_8:B,4402
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_8:P,4427
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_8:UB,4402
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:CLK,6145
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:Q,6145
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[5]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[5]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[5]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[5]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[10]:A,2171
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[10]:B,4241
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[10]:C,3674
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[10]:Y,2171
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[28]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[28]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[28]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[28]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261:B,1306
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261:C,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261:CC,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261:P,1306
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261:UB,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:D,5257
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:CLK,6077
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:Q,6077
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:CLK,7039
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:D,7467
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:Q,7039
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[2]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_165:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_165:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_165:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_165:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_165:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_a2[13]:A,2849
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_a2[13]:B,2861
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_a2[13]:C,4982
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_a2[13]:D,3854
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_a2[13]:Y,2849
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_230:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_230:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_230:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_230:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_230:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:D,8725
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:D,1226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:CLK,1488
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:Q,1488
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[4]:A,1943
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[4]:B,2815
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[4]:C,5112
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[4]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[4]:D,4952
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[4]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[4]:Y,1943
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[8]:A,6484
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[8]:B,7072
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[8]:C,6597
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[8]:CC,5727
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[8]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[8]:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[8]:S,5727
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[8]:UB,6597
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNITO5G1[8]:A,2455
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNITO5G1[8]:B,2215
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNITO5G1[8]:C,2327
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNITO5G1[8]:Y,2215
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2_i_o2_i_o2[11]:A,3131
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2_i_o2_i_o2[11]:B,3278
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2_i_o2_i_o2[11]:C,3339
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2_i_o2_i_o2[11]:D,3151
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2_i_o2_i_o2[11]:Y,3131
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:CLK,1846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:D,8673
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:Q,1846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:CLK,1680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:D,8681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:Q,1680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:CLK,5235
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:Q,5235
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11]:B,5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11]:C,6042
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11]:CC,5742
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11]:P,5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11]:S,5742
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:CLK,4264
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:D,6887
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:Q,4264
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:CLK,4493
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:Q,4493
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:CLK,7641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:Q,7641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16_FCINST1:CC,2763
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16_FCINST1:CO,2763
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_16_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:CLK,4779
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:Q,4779
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:CLK,5029
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:D,3774
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:Q,5029
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_2:A,6217
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_2:B,4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_2:P,4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_2:UB,4722
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:D,6203
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:CLK,5176
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:Q,5176
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[0]:A,5748
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[0]:B,7000
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[0]:C,6532
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[0]:CC,6277
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[0]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[0]:P,5748
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[0]:S,6277
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[0]:UB,6532
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:D,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILDET[10]:A,3417
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILDET[10]:B,3113
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILDET[10]:C,3295
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNILDET[10]:Y,3113
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:D,5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:CLK,4686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:D,7053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:Q,4686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[13]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[13]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[13]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[13]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[13]:Y,261
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:D,8721
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[0]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:CLK,5188
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:Q,5188
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0:A,7398
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0:B,6763
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0:C,4597
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0:CC,2146
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0:D,2587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0:P,2733
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0:S,2146
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0:UB,2587
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:CLK,5080
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:Q,5080
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[11]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[11]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[11]:Y,7440
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[13]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[13]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[13]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_23:B,6562
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_23:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_23:D,6421
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_23:IPB,6562
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_23:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_23:IPD,6421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11_0:A,6219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11_0:B,7274
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11_0:C,7135
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11_0:CC,5392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11_0:S,5392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_11_0:UB,7135
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:CLK,4378
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:Q,4378
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[1]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_91:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_91:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_91:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_91:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_91:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[6]:A,5849
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[6]:B,7090
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[6]:C,6638
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[6]:CC,5714
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[6]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[6]:P,5849
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[6]:S,5714
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[6]:UB,6638
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:CLK,6835
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:Q,6835
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[16]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[0]:A,8004
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[0]:B,7910
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count_3[0]:Y,7910
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:CLK,4793
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:D,6817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:Q,4793
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:CLK,6014
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:Q,6014
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:CLK,4973
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:D,7008
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:Q,4973
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_30_0:A,2292
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_30_0:B,1640
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_30_0:C,1722
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_30_0:CC,-47
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_30_0:D,432
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_30_0:P,532
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_30_0:S,-47
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_30_0:UB,432
A0_PWM_UH_O_obuf/U0/U_IOPAD:D,4315
A0_PWM_UH_O_obuf/U0/U_IOPAD:E,
A0_PWM_UH_O_obuf/U0/U_IOPAD:PAD,4315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:D,3382
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_23:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_23:B,7786
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_23:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_23:CC,6692
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_23:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_23:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_23:S,6692
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_23:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_14:A,365
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_14:B,288
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_14:C,243
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_14:D,165
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_14:Y,165
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[7]:A,2003
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[7]:B,2875
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[7]:C,5168
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[7]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[7]:D,5018
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[7]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[7]:Y,2003
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_2:A,7014
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_2:B,6893
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_2:CC,7351
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_2:P,6929
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_2:S,7351
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_2:UB,6893
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_15:B,5269
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_15:C,5098
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_15:CC,4279
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_15:S,4279
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:CLK,1609
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:D,8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:Q,1609
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__m8_0:A,7990
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__m8_0:B,7870
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__m8_0:C,7796
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__m8_0:Y,7796
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[8]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[8]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[8]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[8]:Y,7507
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_136:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_136:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_136:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_136:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_136:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_14:B,4273
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_14:CC,3469
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_14:S,3469
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_14:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:CLK,3205
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:Q,3205
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIO992D[34]:A,1890
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIO992D[34]:B,1680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIO992D[34]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIO992D[34]:CC,1598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIO992D[34]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIO992D[34]:P,1818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIO992D[34]:S,1598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIO992D[34]:UB,1680
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:CC[0],1557
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:CC[1],1213
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:CC[2],1239
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:CC[3],1494
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:CC[4],1484
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:CC[6],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:CI,1213
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[0],1673
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:CLK,2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:D,1760
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:Q,2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:CLK,6772
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:D,3761
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:Q,6772
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[6]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:CLK,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:D,7893
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:EN,7792
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:Q,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_2:A,4505
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_2:B,6148
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_2:P,4505
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_2:UB,6148
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_8:A,2181
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_8:B,2100
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_8:P,2125
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_8:UB,2100
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]:A,2481
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]:B,1762
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]:C,4028
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]:D,3904
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[2]:Y,1762
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_8:B,5255
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_8:CC,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_8:P,5255
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_8:S,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_19:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_19:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[9]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[9]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[9]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[9]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[9]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[9]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[9]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_0/s_state_ns_0_a2[0]:A,7617
BLDC_Encoder_Axis_0/MSC_i_0/s_state_ns_0_a2[0]:B,7933
BLDC_Encoder_Axis_0/MSC_i_0/s_state_ns_0_a2[0]:C,7836
BLDC_Encoder_Axis_0/MSC_i_0/s_state_ns_0_a2[0]:Y,7617
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_12:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_12:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[12]:A,3583
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[12]:B,3463
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[12]:C,2528
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[12]:D,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[12]:Y,1584
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_5:B,3153
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_5:UB,3153
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:CLK,3978
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:Q,3978
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[16]:A,1967
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[16]:B,2839
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[16]:C,5136
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[16]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[16]:D,4982
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[16]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[16]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[16]:Y,1967
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:CC[0],2787
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:CC[1],2717
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:CC[2],2671
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:CC[3],2735
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:CC[4],2671
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:CC[5],2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:CC[6],2723
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:CI,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[0],2920
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[1],2998
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[3],3169
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[0],2870
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[1],2832
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[2],2968
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[3],3021
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[4],3062
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[5],3155
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0_cy_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[17]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[17]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[17]:Y,5366
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:CLK,4969
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:Q,4969
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:CLK,6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:Q,6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_12_0:A,1529
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_12_0:B,845
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_12_0:C,1257
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_12_0:CC,787
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_12_0:D,-323
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_12_0:P,-199
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_12_0:S,787
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_12_0:UB,-323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[11]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[11]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[11]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[11]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_16:B,7786
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_16:CC,6849
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_16:S,6849
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_12:A,6315
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_12:B,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_12:P,4273
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_12:UB,4108
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_4:B,2940
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_4:UB,2940
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:D,8667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:CLK,5166
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:Q,5166
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[10]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_200:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_200:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_200:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_200:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_200:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[8]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[8]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[8]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[40]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[40]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[40]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:D,8670
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:B,7909
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:C,6804
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:D,7949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPB,7909
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPC,6804
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPD,7949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:CLK,1566
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:D,6075
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:Q,1566
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO_0:A,5755
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO_0:B,5661
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO_0:C,3804
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO_0:D,3724
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO_0:Y,3724
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[5]:A,5060
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[5]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[5]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[5]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[5]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:B,7879
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:C,6731
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:IPB,7879
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_30:IPC,6731
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7_RNO:A,5181
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7_RNO:B,3691
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7_RNO:C,5057
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7_RNO:Y,3691
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:CLK,2741
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:D,2378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:Q,2741
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0:A,7239
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0:B,6634
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0:C,1875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0:CC,1981
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0:P,1996
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0:S,1981
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0:UB,1875
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[6]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[6]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[6]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[6]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:CLK,4336
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:D,8723
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:Q,4336
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:CLK,2931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:D,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:Q,2931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[15]:A,1843
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[15]:B,2715
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[15]:C,5010
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[15]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[15]:D,4852
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[15]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[15]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[15]:Y,1843
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[0]:A,6149
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[0]:B,6065
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[0]:C,5365
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[0]:Y,5365
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[36]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[36]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[36]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[36]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[36]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_9:A,5322
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_9:B,5144
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_9:CC,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_9:P,5232
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_9:S,5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_9:UB,5144
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0:A,7213
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0:B,6663
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0:C,1885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0:CC,1884
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0:P,1917
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0:S,1884
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0:UB,1885
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_237:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_237:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_237:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_237:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_237:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:CLK,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:Q,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:CLK,7115
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:D,7504
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:Q,7115
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[7]:A,6190
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[7]:B,6113
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[7]:C,5734
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[7]:D,4497
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[7]:Y,4497
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:CLK,3765
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:D,8723
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:Q,3765
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_6:B,4461
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_6:C,4266
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_6:CC,4260
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_6:P,4266
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_6:S,4260
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[28]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[28]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[28]:Y,7555
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[4]:A,1790
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[4]:B,3160
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[4]:C,4904
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[4]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[4]:D,4750
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[4]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[4]:Y,1790
A0_RUNNING_LED_obuf/U0/U_IOOUTFF:A,2053
A0_RUNNING_LED_obuf/U0/U_IOOUTFF:Y,2053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_20:B,6499
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_20:C,4336
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_20:IPB,6499
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_20:IPC,4336
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o_1_sqmuxa_0_a2:A,5351
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o_1_sqmuxa_0_a2:B,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o_1_sqmuxa_0_a2:C,5352
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o_1_sqmuxa_0_a2:D,4933
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o_1_sqmuxa_0_a2:Y,3035
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_7_0:A,5528
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_7_0:B,6488
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_7_0:C,5341
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_7_0:CC,5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_7_0:D,6789
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_7_0:P,5402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_7_0:S,5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_7_0:UB,5341
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0:A,6123
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0:B,5879
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0:C,5796
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0:P,5948
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0:UB,5796
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:CLK,7005
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:Q,7005
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:CLK,5310
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:Q,5310
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[8]:SLn,
A0_ADC_SCK_O_obuf/U0/U_IOENFF:A,
A0_ADC_SCK_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:CLK,1384
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:Q,1384
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12:A,2965
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12:B,2853
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12:CC,2656
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12:P,2853
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12:S,2656
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]_CC_0:UB[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_14:A,2452
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_14:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_14:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_14:IPA,2452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:CLK,4955
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:Q,4955
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[27]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[27]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[27]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:CLK,4151
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:D,8718
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:Q,4151
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:D,8706
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_9:A,1663
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_9:B,1359
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_9:P,1454
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_9:UB,1359
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[2]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[3]:A,6137
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[3]:B,7896
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[3]:C,5759
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[3]:D,5829
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[3]:Y,5759
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:CLK,5072
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:Q,5072
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[14]:A,3552
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[14]:B,3452
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[14]:C,3290
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[14]:Y,3290
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:CLK,7152
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:D,7076
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:Q,7152
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:B,7879
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:C,6711
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:IPB,7879
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:IPC,6711
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:CLK,4349
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:Q,4349
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:CLK,4231
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:D,8686
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:Q,4231
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[43]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[43]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[43]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:B,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:C,6833
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:D,7817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPB,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPC,6833
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_29:IPD,7817
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[3]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[3]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[3]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16:B,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16:S,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:B,7846
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:C,6802
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:D,7825
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPB,7846
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPC,6802
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPD,7825
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGLUI6[4]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGLUI6[4]:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGLUI6[4]:C,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGLUI6[4]:CC,3914
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGLUI6[4]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGLUI6[4]:P,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGLUI6[4]:S,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIGLUI6[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0:A,6014
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0:B,5937
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0:C,3526
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0:D,4360
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_0:Y,3526
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI9I0J[12]:A,2856
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI9I0J[12]:B,2779
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI9I0J[12]:C,2345
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI9I0J[12]:Y,2345
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[11]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[11]:B,4998
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[11]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[11]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[11]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:D,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_7:B,4654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_7:C,3691
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_7:CC,3669
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_7:P,3691
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_7:S,3669
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_7:UB,4654
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[10]:A,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[10]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[10]:C,5641
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[10]:Y,5156
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_106:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_106:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_106:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_106:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[30]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[30]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[30]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[30]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:B,7714
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:C,6747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:IPB,7714
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_14:IPC,6747
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:C,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPC,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[14]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[14]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[14]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[14]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[14]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[14]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[14]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[14]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_24:B,6483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_24:C,4432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_24:IPB,6483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_24:IPC,4432
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2[3]:A,2268
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2[3]:B,2207
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2[3]:C,5913
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_2[3]:Y,2207
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:CLK,5224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:Q,5224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[6]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_12_0:A,7227
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_12_0:B,6638
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_12_0:C,2832
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_12_0:CC,2717
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_12_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_12_0:P,2998
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_12_0:S,2717
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_12_0:UB,2832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:CLK,705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:D,7408
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:Q,705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_3:A,4345
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_3:B,5999
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_3:P,4345
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_3:UB,5999
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_2:A,3461
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_2:B,1349
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_2:P,1377
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_2:UB,1349
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[8]:A,4296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[8]:B,6667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[8]:C,3098
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[8]:D,3219
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[8]:Y,3098
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:CLK,4203
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:D,5867
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:Q,4203
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_284:A,7997
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_284:B,7890
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_284:C,7517
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_284:D,6291
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_284:Y,6291
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_15:A,6349
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_15:B,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_15:P,6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_15:UB,6183
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:CLK,2181
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:Q,2181
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[8]:A,2072
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[8]:B,4217
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[8]:C,1712
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[8]:D,1908
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[8]:Y,1712
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:CLK,4103
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:D,5589
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:Q,4103
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17:A,6744
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17:B,7359
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17:C,7631
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17:CC,2143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17:D,4971
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17:S,2143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[1]:A,7938
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[1]:B,2525
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[1]:C,7836
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[1]:D,7735
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[1]:Y,2525
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[1]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[1]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[1]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[1]:Y,6726
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:CLK,6810
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:Q,6810
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:C,6804
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPC,6804
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_23:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_23:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[0]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[0]:B,6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[0]:C,6840
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[0]:CC,7447
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[0]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[0]:P,6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[0]:S,7447
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_16:B,6208
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_16:UB,6208
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:CLK,240
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:D,6965
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:Q,240
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[42]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[42]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[42]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[42]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[42]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_15:A,2277
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_15:B,2071
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_15:P,2191
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_15:UB,2071
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_29:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_29:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[0]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[0]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[0]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[0]:Y,1256
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_2_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_2_PAD/U_IOINFF:Y,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:CLK,7694
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:Q,7694
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_23:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_23:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_1:A,3525
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_1:B,4449
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_1:C,3471
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO_1:Y,3471
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:CLK,6883
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:Q,6883
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_14:B,6995
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_14:CC,6969
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_14:P,6995
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_14:S,6969
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[10],6927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[11],6866
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[1],7531
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[2],7467
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[3],7123
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[4],7053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[5],6992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[6],7044
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[7],6974
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[8],6914
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CC[9],7007
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:CO,6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[0],6927
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[1],6877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[2],7051
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[3],7036
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[6],7048
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[7],7088
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[8],7158
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:P[9],7154
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[0],6775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[10],7075
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[11],7181
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[1],6869
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[2],7015
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[3],6907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[4],6940
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[5],7047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[6],6946
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[7],7000
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[8],7090
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_0_CC_0:UB[9],7061
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:CLK,3480
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:Q,3480
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:CLK,1647
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:D,8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:Q,1647
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:CLK,4944
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:D,7015
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:Q,4944
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[14]:A,1964
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[14]:B,4109
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[14]:C,1836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[14]:Y,1836
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_4:B,6062
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_4:UB,6062
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:CLK,7150
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:Q,7150
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[3]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[3]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[3]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[3]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_32:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_32:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:CLK,3910
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:D,8710
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:Q,3910
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_14:B,6338
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_14:C,6446
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_14:CC,6021
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_14:P,6338
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_14:S,6021
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_19:A,7070
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_19:B,6941
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_19:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_19:CC,6926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_19:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_19:P,7014
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_19:S,6926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_19:UB,6941
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_s_17:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_s_17:C,7716
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_s_17:CC,3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_s_17:D,6144
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_s_17:S,3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_s_17:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_207:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_207:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_207:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_207:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_207:IPB,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_8:A,4106
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_8:B,6186
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_8:P,4106
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_8:UB,6186
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:CLK,5944
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:Q,5944
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5:A,7808
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5:B,7074
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5:CC,7034
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5:S,7034
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_5:UB,7074
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:CLK,6771
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:Q,6771
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:CLK,849
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:D,8668
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:Q,849
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:CLK,257
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:D,8684
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:Q,257
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17:B,6370
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17:UB,6370
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[9]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[9]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[9]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[13]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[13]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[13]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[13]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3K271[5]:A,2502
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3K271[5]:B,2269
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3K271[5]:C,2380
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3K271[5]:Y,2269
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_12_0:A,5522
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_12_0:B,6565
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_12_0:C,5399
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_12_0:CC,5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_12_0:D,6878
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_12_0:P,5399
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_12_0:S,5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_12_0:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:B,7657
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:C,6807
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:D,7641
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPB,7657
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPC,6807
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPD,7641
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_16:B,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_16:CC,5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_16:S,5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:CLK,5834
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:D,6917
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:Q,5834
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_25:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_25:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[14]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[14]:B,7245
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[14]:C,7289
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[14]:CC,6928
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[14]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[14]:P,7245
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[14]:S,6928
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[14]:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_264:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_264:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_264:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_264:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_264:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_264:IPC,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_s[17]:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_s[17]:B,6407
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_s[17]:C,7710
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_s[17]:CC,5588
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_s[17]:D,7146
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_s[17]:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_s[17]:S,5588
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_s[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:D,8721
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:CLK,7809
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:Q,7809
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[6]:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[6]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[6]:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[6]:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[6]:Y,-247
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[17]:A,6929
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[17]:B,6852
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[17]:C,6154
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[17]:Y,6154
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_25:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_25:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:CLK,7866
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:Q,7866
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[19]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:CLK,4508
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:Q,4508
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_11:A,5804
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_11:B,5308
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_11:CC,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_11:S,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_11:UB,5308
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:CLK,6843
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:D,7480
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:Q,6843
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:D,6636
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[8]:A,2472
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[8]:B,2179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[8]:C,5624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[8]:Y,2179
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_17:A,7848
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_17:B,6992
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_17:CC,6927
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_17:S,6927
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_17:UB,6992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:CLK,3804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:D,2968
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:Q,3804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:CLK,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:D,6660
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:Q,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_16:B,6798
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_16:C,6873
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_16:CC,5889
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_16:S,5889
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_16:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:CLK,5153
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:Q,5153
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in_1_sqmuxa_i:A,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in_1_sqmuxa_i:B,7441
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in_1_sqmuxa_i:Y,5058
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0:A,7841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0:B,6648
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0:C,1926
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0:CC,1897
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0:S,1897
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_9_0:UB,1926
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_0_sqmuxa:A,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_0_sqmuxa:B,5891
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_0_sqmuxa:Y,4242
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:D,8716
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_7:A,4860
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_7:B,2842
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_7:P,2891
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_7:UB,2842
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_8:A,2661
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_8:B,2752
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_8:P,2661
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_8:UB,2752
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQB7U1[0]:A,3793
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQB7U1[0]:B,6890
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQB7U1[0]:C,6468
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQB7U1[0]:CC,4368
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQB7U1[0]:D,6526
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQB7U1[0]:P,3793
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQB7U1[0]:S,4368
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQB7U1[0]:UB,6526
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13:B,3370
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13:CC,2624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13:S,2624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[9]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[9]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[9]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[9]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_RNO[4]:A,7562
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_RNO[4]:B,6935
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_RNO[4]:C,7836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_RNO[4]:D,7801
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state_RNO[4]:Y,6935
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:C,6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPC,6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:D,3501
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[9]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[9]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[9]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[9]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:CLK,2830
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:D,2765
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:Q,2830
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[12]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[12]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[12]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:CLK,4050
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:Q,4050
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_30:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_30:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI12MU[1]:A,7030
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI12MU[1]:B,6676
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI12MU[1]:C,6576
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI12MU[1]:Y,6576
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[11]:A,6067
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[11]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[11]:Y,6067
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[19]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[19]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[19]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[19]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[30]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[30]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[30]:Y,5366
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/done_o:A,5731
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/done_o:B,5650
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/done_o:Y,5650
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[6]:A,2099
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[6]:B,4169
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[6]:C,3602
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[6]:Y,2099
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_2_0:A,1456
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_2_0:B,1371
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_2_0:C,840
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_2_0:CC,1521
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_2_0:D,1118
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_2_0:P,842
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_2_0:S,1521
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_2_0:UB,840
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o_1_sqmuxa_0_a2:A,5589
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o_1_sqmuxa_0_a2:B,5196
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o_1_sqmuxa_0_a2:C,5300
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o_1_sqmuxa_0_a2:D,2979
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o_1_sqmuxa_0_a2:Y,2979
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[11]:A,1407
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[11]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[11]:Y,1407
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:CLK,5168
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:D,3896
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:Q,5168
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_2:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[10],5144
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[11],5114
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[1],5472
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[2],5494
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[3],5292
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[4],5141
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[5],5118
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[6],5262
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[7],5092
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[8],5103
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CC[9],5282
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:CO,4995
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[0],5147
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[1],5097
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[2],5271
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[3],5256
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[6],5268
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[7],5308
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[8],5378
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:P[9],5374
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[0],4995
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[10],5295
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[11],5401
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[1],5089
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[2],5235
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[3],5127
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[4],5160
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[5],5267
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[6],5166
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[7],5220
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[8],5310
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_0:UB[9],5281
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:CLK,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:Q,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_16_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_16_0:B,6951
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_16_0:C,3155
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_16_0:CC,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_16_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_16_0:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_16_0:S,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_16_0:UB,3155
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[25]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[25]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[25]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_25:A,7087
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_25:B,6919
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_25:C,3762
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_25:CC,3245
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_25:D,6438
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_25:P,3775
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_25:S,3245
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_25:UB,3762
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_4:A,7835
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_4:B,6768
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_4:CC,7066
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_4:S,7066
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_4:UB,6768
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[8]:A,5881
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[8]:B,6074
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[8]:C,2898
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[8]:D,2923
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[8]:Y,2898
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:CLK,7316
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:D,6750
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:Q,7316
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:CLK,6835
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:Q,6835
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[16]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_113:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_113:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_113:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_113:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_113:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_s_17:B,5778
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_s_17:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_s_17:CC,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_s_17:S,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:CLK,4906
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:Q,4906
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:CLK,6058
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:Q,6058
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:CLK,5251
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:D,6835
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:Q,5251
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[26]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[26]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[26]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[26]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[26]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:CLK,3985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:Q,3985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:D,8712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_0_sqmuxa_0_a3:A,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_0_sqmuxa_0_a3:B,7693
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_0_sqmuxa_0_a3:Y,7679
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[15]:A,2154
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[15]:B,3524
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[15]:C,5254
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[15]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[15]:D,5114
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[15]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[15]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[15]:Y,2154
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0:A,6032
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0:B,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0:P,6006
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_0:UB,5897
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[1]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[1]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[1]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[1]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_5:B,6789
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_5:C,6882
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_5:CC,6896
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_5:P,6789
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_5:S,6896
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209:A,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209:B,6561
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209:C,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209:CC,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209:P,6561
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:CLK,6705
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:Q,6705
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:D,6373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[15]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[15]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[15]:C,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[15]:Y,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO_0:A,5219
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO_0:B,5069
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO_0:C,2229
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO_0:D,2015
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_7_0_RNO_0:Y,2015
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:CLK,5997
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:Q,5997
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_3:B,6798
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_3:C,6873
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_3:CC,6183
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_3:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_3:S,6183
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[4]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[4]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[4]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[4]:CC,7127
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[4]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[4]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[4]:S,7127
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQGSCC[9]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQGSCC[9]:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQGSCC[9]:C,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQGSCC[9]:CC,2890
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQGSCC[9]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQGSCC[9]:P,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQGSCC[9]:S,2890
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIQGSCC[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot_RNO:A,5030
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot_RNO:B,7454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot_RNO:Y,5030
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5:B,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5:S,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:CLK,1728
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:D,8681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:Q,1728
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:D,5390
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[6]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_21:A,2506
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_21:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_21:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_21:IPA,2506
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_21:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[1]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[1]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[1]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[1]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[1]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[1]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[1]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[1]:A,1788
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[1]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[1]:Y,1788
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_5:B,4359
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_5:UB,4359
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_32:B,6408
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_32:C,4414
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_32:IPB,6408
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_32:IPC,4414
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI8JCV1[17]:A,6099
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI8JCV1[17]:B,1233
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI8JCV1[17]:C,1308
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI8JCV1[17]:CC,1852
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI8JCV1[17]:D,5792
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI8JCV1[17]:P,1241
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI8JCV1[17]:S,1852
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNI8JCV1[17]:UB,1233
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:CLK,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:D,6804
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:Q,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[8]:A,5988
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[8]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[8]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[8]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[8]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:CLK,5777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:Q,5777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:CLK,6918
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:D,8867
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:Q,6918
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/mas_done_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[11]:A,6144
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[11]:B,6067
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[11]:C,5676
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[11]:D,4451
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[11]:Y,4451
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:D,8703
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[42]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[42]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[42]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:CLK,2737
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:D,2256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:Q,2737
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_212:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_212:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_212:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_212:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_212:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[7]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[7]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[7]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_8:A,1362
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_8:B,3210
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_8:P,1362
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_8:UB,3210
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:CLK,7909
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:Q,7909
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[16]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[16]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[16]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:C,6804
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPC,6804
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:CLK,5042
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:Q,5042
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[11]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[11]:B,7480
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[11]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[11]:CC,7068
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[11]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[11]:P,7480
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[11]:S,7068
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o_1_sqmuxa_0_a2:A,5422
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o_1_sqmuxa_0_a2:B,3147
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o_1_sqmuxa_0_a2:C,5464
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o_1_sqmuxa_0_a2:D,5045
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o_1_sqmuxa_0_a2:Y,3147
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_283:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_283:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_283:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_283:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_283:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO:A,2184
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO:B,5592
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO:C,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO:D,1947
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_6_0_RNO:Y,1898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[0]:A,6143
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[0]:B,6066
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[0]:C,5359
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[0]:Y,5359
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_11:A,3710
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_11:B,3663
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_11:C,3585
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_11:D,3484
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_11:Y,3484
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[0]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[0]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[0]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[0]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[0]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[0]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[0]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:CLK,4158
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:Q,4158
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[4]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[4]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[4]:Y,5366
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_1[4]:A,6832
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_1[4]:B,6824
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_1[4]:C,5677
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_1[4]:D,5650
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO_1[4]:Y,5650
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_245:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_245:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_245:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_245:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_245:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[6]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[6]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[6]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[6]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_21:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_21:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:D,8725
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_a3_0[8]:A,5963
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_a3_0[8]:B,5829
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_a3_0[8]:C,5769
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_a3_0[8]:Y,5769
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:D,8725
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[12]:A,1333
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[12]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[12]:Y,1333
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_0:A,3797
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_0:B,3749
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_0:C,3668
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_0:D,3564
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_0:Y,3564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_9:A,7226
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_9:B,7061
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_9:CC,7007
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_9:P,7154
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_9:S,7007
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_9:UB,7061
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]:A,3059
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]:B,3453
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]:C,5277
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]:D,5153
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[2]:Y,3059
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[5]:A,1923
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[5]:B,3293
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[5]:C,5033
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[5]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[5]:D,4883
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[5]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[5]:Y,1923
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO_0:A,5569
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO_0:B,5475
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO_0:C,3618
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO_0:D,3538
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_5_RNO_0:Y,3538
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2M3JD[35]:A,1840
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2M3JD[35]:B,1768
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2M3JD[35]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2M3JD[35]:CC,1477
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2M3JD[35]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2M3JD[35]:P,1768
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2M3JD[35]:S,1477
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI2M3JD[35]:UB,1768
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[17]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[17]:B,4696
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[17]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[17]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[17]:Y,2538
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_1:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_1:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_1:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_1:IPA,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[10],1897
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[11],1836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[1],5503
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[2],2430
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[3],2029
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[4],1959
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[5],1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[6],2037
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[7],1945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[8],1884
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CC[9],1981
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:CO,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[0],4899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[1],1786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[2],1908
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[3],1956
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[6],2013
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[7],1968
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[8],1917
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:P[9],1996
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[10],1926
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[11],2131
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[1],1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[2],1877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[3],1825
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[4],1908
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[5],1955
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[6],1891
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[7],1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[8],1885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy_CC_0:UB[9],1875
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:CLK,4354
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:D,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:EN,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:Q,4354
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_Z:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_6_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_6_PAD/U_IOINFF:Y,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[3]:A,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[3]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[3]:C,5814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[3]:Y,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3:A,2900
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3:B,2689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3:CC,2802
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3:P,2788
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3:S,2802
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3:UB,2689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[15]:A,3254
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[15]:B,3241
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[15]:C,2246
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[15]:D,2179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[15]:Y,2179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0:A,7121
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0:B,6480
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0:C,1825
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0:CC,2029
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0:P,1956
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0:S,2029
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_2_0:UB,1825
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:CLK,6809
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:Q,6809
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[3]:A,5996
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[3]:B,6197
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[3]:C,3021
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[3]:D,3046
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[3]:Y,3021
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_16:A,7808
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_16:B,7352
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_16:C,6899
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_16:CC,6453
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_16:S,6453
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_16:UB,6899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDBT9[5]:A,3013
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDBT9[5]:B,2936
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDBT9[5]:C,2502
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDBT9[5]:Y,2502
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_174:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_174:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_174:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_174:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_174:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:CC[6],4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:CI,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[0],4273
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[1],4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[3],4332
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[0],4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[1],4130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[2],4221
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[3],4208
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[4],4174
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[5],6370
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[2]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[2]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[2]:C,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[2]:Y,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_13_118_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_13_118_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_13_118_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_13_118_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[4]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[4]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[4]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[4]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[10]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[10]:B,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[10]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[10]:CC,6967
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[10]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[10]:P,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[10]:S,6967
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6:B,4549
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6:CC,4644
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6:P,4549
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6:S,4644
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:CLK,3841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:D,6803
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:Q,3841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:CLK,1582
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:D,8683
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:Q,1582
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[22]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:CC[0],6796
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:CC[1],6718
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:CC[2],6660
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:CC[3],6750
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:CC[4],6679
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:CC[5],6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:CC[6],6739
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:CI,6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[0],6818
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[1],6896
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[3],7067
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:CLK,3666
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:D,6927
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:Q,3666
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s_RNO[17]:A,4652
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s_RNO[17]:B,6485
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s_RNO[17]:Y,4652
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:CLK,5609
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:D,4232
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:Q,5609
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:CLK,7101
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:Q,7101
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:C,6847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPC,6847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4CFQ7[24]:A,1732
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4CFQ7[24]:B,1641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4CFQ7[24]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4CFQ7[24]:CC,4949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4CFQ7[24]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4CFQ7[24]:P,1683
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4CFQ7[24]:S,4949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4CFQ7[24]:UB,1641
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:CC[0],7068
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:CC[1],6990
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:CC[2],6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:CI,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[0],7480
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_10:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:CLK,4340
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:D,6647
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:EN,6923
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:Q,4340
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[14]:A,4416
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[14]:B,1880
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[14]:C,1836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[14]:Y,1836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[4]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[4]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[4]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[4]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[4]:Y,261
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:CLK,1980
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:Q,1980
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:CLK,5964
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:Q,5964
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_s_17:B,6798
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_s_17:C,6873
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_s_17:CC,6010
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_s_17:S,6010
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[8]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[8]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[8]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[8]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:CLK,2041
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:D,1897
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:Q,2041
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_0_sqmuxa_i_o3_i:A,7763
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_0_sqmuxa_i_o3_i:B,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_0_sqmuxa_i_o3_i:Y,7713
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:D,3385
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:CLK,6169
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:Q,6169
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:CLK,7008
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:Q,7008
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_3:B,5099
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_3:C,4928
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_3:CC,4345
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_3:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_3:S,4345
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:CLK,7886
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:Q,7886
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[41]:SLn,
A0_ADC_SDI_I_ibuf/U0/U_IOINFF:A,6138
A0_ADC_SDI_I_ibuf/U0/U_IOINFF:Y,6138
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0:B,4429
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0:C,3526
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0:P,3526
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0:UB,4429
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:CLK,6754
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:D,3608
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:Q,6754
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_220:A,6318
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_220:B,4835
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_220:C,6196
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_220:Y,4835
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:CLK,5235
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:D,6753
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:Q,5235
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_8:A,6324
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_8:B,4244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_8:P,4278
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_8:UB,4244
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:D,8706
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_185:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_185:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_185:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_185:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_185:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[43]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[43]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[43]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_10:A,3907
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_10:B,3859
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_10:C,3785
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_10:D,3684
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_10:Y,3684
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_1:A,1088
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_1:B,1669
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_1:P,1088
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_1:UB,1700
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:CO,2764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[0],2886
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[1],2836
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[2],3010
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[3],2995
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[6],3007
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[7],3047
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[8],3117
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:P[9],3113
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[0],2764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[10],3048
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[11],3169
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[1],2859
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[2],2983
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[3],2902
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[4],2940
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[5],3032
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[6],2923
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[7],2981
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[8],3089
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0_CC_0:UB[9],3030
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:CLK,5194
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:D,6759
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:Q,5194
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[14]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[14]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[14]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:CLK,5078
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:D,8703
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:Q,5078
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[17]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[17]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[17]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[17]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_7:A,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_7:B,6122
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_7:P,6167
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_7:UB,6122
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12:A,2434
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12:B,1425
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12:C,1200
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12:D,1854
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_12:Y,1200
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_23:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_23:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2_RNI72CU:A,6171
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2_RNI72CU:B,4780
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2_RNI72CU:C,4468
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2_RNI72CU:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2_RNI72CU:D,5871
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2_RNI72CU:P,4468
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2_RNI72CU:UB,5871
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[8]:A,4301
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[8]:B,3219
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[8]:C,4322
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[8]:D,4222
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[8]:Y,3219
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_4:B,6062
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_4:UB,6062
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[25]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[25]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[25]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26:A,7230
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26:B,5822
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26:C,3940
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26:CC,3197
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26:D,4733
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26:P,3940
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26:S,3197
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26:UB,3942
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIOJ064[3]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIOJ064[3]:B,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIOJ064[3]:C,7716
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIOJ064[3]:CC,7051
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIOJ064[3]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIOJ064[3]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIOJ064[3]:S,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIOJ064[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:CLK,2426
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:Q,2426
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[13]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[13]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[13]:C,5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[13]:Y,5118
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa:A,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa:B,6697
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa:Y,3384
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:CLK,6765
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:D,6982
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:Q,6765
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO:A,1921
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO:B,1891
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO:C,5480
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO:D,2782
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO:Y,1891
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_8_173_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_8_173_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_8_173_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_8_173_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:D,5257
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[40]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[40]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[40]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[40]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[40]:Y,224
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:CLK,6903
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:D,6940
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:Q,6903
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_7:B,4531
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_7:C,4336
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_7:CC,4207
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_7:P,4336
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_7:S,4207
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_15:EN,8969
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_15:IPENn,8969
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[1]:A,5951
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[1]:B,5903
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[1]:C,5199
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[1]:Y,5199
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:CLK,4938
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:D,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:Q,4938
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[6]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[6]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[6]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_16:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_16:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]:A,2347
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]:B,1830
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]:C,4106
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]:D,3973
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[12]:Y,1830
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_14:B,6286
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_14:UB,6286
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_12:A,5849
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_12:B,5806
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_12:C,5724
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_12:D,5623
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_12:Y,5623
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a2[2]:A,4022
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a2[2]:B,5958
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a2[2]:C,4904
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a2[2]:Y,4022
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIL3CT5[5]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIL3CT5[5]:B,5994
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIL3CT5[5]:C,7056
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIL3CT5[5]:CC,6056
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIL3CT5[5]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIL3CT5[5]:P,5994
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIL3CT5[5]:S,6056
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIL3CT5[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28:B,5778
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28:C,3898
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28:CC,3199
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28:D,5533
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28:S,3199
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28:UB,3898
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_4:B,6037
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_4:UB,6037
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_14:A,7848
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_14:B,7154
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_14:CC,6844
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_14:S,6844
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_14:UB,7154
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[32]:A,477
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[32]:B,400
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[32]:C,-140
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[32]:Y,-140
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:CLK,1934
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:D,1945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:Q,1934
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:CLK,6844
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:Q,6844
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o_1_sqmuxa_0_a2:A,5350
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o_1_sqmuxa_0_a2:B,5422
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o_1_sqmuxa_0_a2:C,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o_1_sqmuxa_0_a2:D,4933
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o_1_sqmuxa_0_a2:Y,2945
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[11]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[11]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[11]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_3:A,6930
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_3:B,6735
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_3:CC,7136
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_3:P,6864
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_3:S,7136
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_3:UB,6735
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:CLK,4846
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:EN,2979
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:Q,4846
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/start_motor_o:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:CLK,5917
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:Q,5917
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18_FCINST1:CC,3384
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18_FCINST1:CO,3384
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:CLK,6809
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:Q,6809
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:CLK,7888
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:Q,7888
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:CLK,4495
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:D,4269
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:Q,4495
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[7]:A,4767
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[7]:B,4724
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[7]:C,4265
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[7]:Y,4265
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_3:B,3543
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_3:CC,3570
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_3:P,3543
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_3:S,3570
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_14:B,4797
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_14:UB,4797
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_8:B,4527
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_8:C,4366
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_8:CC,4367
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_8:P,4366
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_8:S,4367
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[2]:A,5450
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[2]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[2]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[2]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[2]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[4]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[4]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[4]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[4]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_2_0:A,7108
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_2_0:B,6548
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_2_0:C,2747
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_2_0:CC,2872
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_2_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_2_0:P,2879
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_2_0:S,2872
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_2_0:UB,2747
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[13]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[13]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[13]:Y,7555
A0_PWM_WL_O_obuf/U0/U_IOENFF:A,
A0_PWM_WL_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:CLK,8854
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:D,6834
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:EN,7406
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:Q,8854
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[29]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[29]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[29]:Y,5379
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_268:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_268:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_268:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_268:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_268:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0[0]:A,8010
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0[0]:B,7890
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0[0]:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0[0]:D,6363
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_ns_0[0]:Y,6363
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[12]:A,5989
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[12]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[12]:Y,5989
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[16]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[17]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[17]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[17]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:CLK,2596
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:D,8677
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:Q,2596
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12:B,2899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12:CC,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12:P,2899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12:S,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[2]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[2]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[2]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[4]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[4]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[4]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_1:A,6949
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_1:B,6869
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_1:CC,7531
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_1:P,6877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_1:S,7531
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_1:UB,6869
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:CLK,6137
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:Q,6137
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_8:A,5054
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_8:B,4973
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_8:P,4998
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_8:UB,4973
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:CLK,6918
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:D,6927
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:Q,6918
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI5UET[18]:A,3830
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI5UET[18]:B,3509
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI5UET[18]:C,3702
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI5UET[18]:Y,3509
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[9]:A,1606
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[9]:B,4323
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[9]:C,2819
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[9]:Y,1606
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:CLK,5127
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:Q,5127
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:CLK,4833
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:Q,4833
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc2:A,7958
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc2:B,7903
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc2:C,7816
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/un2_s_sck_count_1_axbxc2:Y,7816
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_256:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_256:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_256:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_256:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_256:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_0_sqmuxa:A,5808
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_0_sqmuxa:B,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_0_sqmuxa:Y,5692
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_RNIGFL51:A,7836
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_RNIGFL51:B,7759
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_RNIGFL51:C,4842
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_RNIGFL51:D,5486
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9_RNIGFL51:Y,4842
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[23]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[23]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[23]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[23]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_16:B,6276
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_16:UB,6276
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:CLK,7339
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:Q,7339
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO:A,5484
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO:B,5436
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO:C,3579
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO:D,3592
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_12_RNO:Y,3579
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:C,6771
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_13:IPC,6771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:CLK,2794
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:Q,2794
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:B,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:C,6733
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:IPC,6733
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:C,6847
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPC,6847
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_5:IPD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:CLK,4293
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:D,4883
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:Q,4293
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[42]:A,849
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[42]:B,706
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[42]:C,228
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[42]:Y,228
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_11:A,7749
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_11:B,7023
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_11:CC,6742
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_11:S,6742
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_11:UB,7023
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:C,6704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_4:IPC,6704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_INCR_SIGNAL_GEN_s_angle_count_incr_1_0:A,7958
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_INCR_SIGNAL_GEN_s_angle_count_incr_1_0:B,7890
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_INCR_SIGNAL_GEN_s_angle_count_incr_1_0:C,7829
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_INCR_SIGNAL_GEN_s_angle_count_incr_1_0:D,7711
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_INCR_SIGNAL_GEN_s_angle_count_incr_1_0:Y,7711
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:CLK,6804
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:Q,6804
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:CLK,6992
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:Q,6992
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[3]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[3]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[3]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[3]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[3]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[3]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[3]:Y,4589
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_261:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_261:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_261:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_261:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_261:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_134:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_134:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_134:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_134:IPA,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir_47:A,5835
BLDC_Encoder_Axis_0/MSC_i_23/s_dir_47:B,7782
BLDC_Encoder_Axis_0/MSC_i_23/s_dir_47:C,6590
BLDC_Encoder_Axis_0/MSC_i_23/s_dir_47:Y,5835
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[29]:A,309
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[29]:B,232
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[29]:C,-308
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[29]:Y,-308
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_86:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_86:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_86:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_86:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_86:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_74:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_74:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_74:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_74:IPA,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_6:A,5459
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_6:B,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_6:CC,5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_6:P,5181
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_6:S,5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_6:UB,5092
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[31]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[31]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[31]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[31]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[6]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[6]:B,7152
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[6]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[6]:CC,7076
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[6]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[6]:P,7152
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[6]:S,7076
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[41]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[41]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[41]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[41]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[41]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIERVR1[13]:A,2840
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIERVR1[13]:B,2892
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIERVR1[13]:Y,2840
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P:A,
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P:B,3674
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P:C,5633
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P:CC,
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P:D,
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P:P,4799
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P:UB,
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P:Y,3674
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_35:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_35:IPENn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state_ns_i_o3[0]:A,6738
BLDC_Encoder_Axis_0/MSC_i_27/s_state_ns_i_o3[0]:B,6661
BLDC_Encoder_Axis_0/MSC_i_27/s_state_ns_i_o3[0]:Y,6661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_10:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_10:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_10:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_10:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:CLK,6705
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:D,6844
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:Q,6705
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[2]:A,1487
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[2]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[2]:Y,1487
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[16]:A,4190
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[16]:B,4105
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[16]:C,3909
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[16]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[16]:Y,3909
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[3]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[3]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[3]:C,5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[3]:Y,5342
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[26]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_17:A,2416
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_17:B,2389
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_17:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_17:IPA,2416
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_17:IPB,2389
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_13:A,3474
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_13:B,1026
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_13:P,1029
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_13:UB,1026
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un101_s_state_i_a2_0_a3:A,2063
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un101_s_state_i_a2_0_a3:B,2053
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un101_s_state_i_a2_0_a3:Y,2053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:CLK,7047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:D,6463
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:Q,7047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:CLK,7909
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:D,7873
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:EN,7867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:Q,7909
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_start:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m33_3:A,4948
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m33_3:B,4639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m33_3:C,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m33_3:Y,1898
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:CLK,6697
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:D,7544
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:Q,6697
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15:B,2121
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15:CC,1636
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15:P,2121
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15:S,1636
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_12:B,3764
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_12:CC,3511
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_12:P,3764
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_12:S,3511
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO_0:A,5803
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO_0:B,5718
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO_0:C,4671
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO_0:D,3768
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20_RNO_0:Y,3768
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[17]:A,6907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[17]:B,6604
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[17]:C,5754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[17]:Y,5754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[19]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[19]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[19]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[19]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[0]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4:B,3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4:C,3564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4:CC,3704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4:D,6143
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4:S,3704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4:UB,3324
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_15_0:A,1721
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_15_0:B,991
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_15_0:C,1403
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_15_0:CC,708
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_15_0:D,-177
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_15_0:P,-7
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_15_0:S,708
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_15_0:UB,-177
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:CLK,4918
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:Q,4918
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:CLK,3179
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:Q,3179
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_16:A,5233
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_16:B,5144
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_16:CC,4174
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_16:S,4174
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_14:B,2868
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_14:UB,2868
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17_FCINST1:CC,2930
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17_FCINST1:CO,2930
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[25]:A,378
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[25]:B,301
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[25]:C,-239
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[25]:Y,-239
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_25:A,7094
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_25:B,7005
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_25:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_25:CC,6842
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_25:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_25:P,7008
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_25:S,6842
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_25:UB,7005
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIVCNRB[10]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIVCNRB[10]:B,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIVCNRB[10]:C,7703
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIVCNRB[10]:CC,4087
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIVCNRB[10]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIVCNRB[10]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIVCNRB[10]:S,4087
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIVCNRB[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[26]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[26]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[26]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[26]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:D,8728
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:CLK,4512
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:Q,4512
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_un1_olmng_done_i:A,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_un1_olmng_done_i:B,7740
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_un1_olmng_done_i:Y,5225
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_110:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_110:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_110:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_110:IPA,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:CLK,7863
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:Q,7863
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_25:B,6432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_25:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_25:IPB,6432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_25:IPC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_12:A,3934
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_12:B,6016
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_12:P,3934
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_12:UB,6016
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_25:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_25:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_3:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_3:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_3:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_3:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[7]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[7]:B,5106
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[7]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[7]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[7]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITNGT[23]:A,3876
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITNGT[23]:B,3572
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITNGT[23]:C,3754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNITNGT[23]:Y,3572
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:CLK,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:D,7565
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:Q,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[12]:A,4254
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[12]:B,1875
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[12]:C,4132
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[12]:Y,1875
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:CLK,460
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:D,8676
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:Q,460
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[30]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[3]:A,1607
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[3]:B,3677
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[3]:C,3110
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[3]:Y,1607
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:CLK,4139
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:D,6701
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:Q,4139
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:CLK,5486
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:D,4288
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:Q,5486
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICG4OG[41]:A,2353
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICG4OG[41]:B,1899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICG4OG[41]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICG4OG[41]:CC,1311
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICG4OG[41]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICG4OG[41]:P,2353
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICG4OG[41]:S,1311
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICG4OG[41]:UB,1899
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIFJA62[22]:A,4660
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIFJA62[22]:B,3678
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIFJA62[22]:C,3634
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIFJA62[22]:Y,3634
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:CLK,5963
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:D,8867
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:Q,5963
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_fault_clear_sync1:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[14]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[14]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[14]:C,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[14]:Y,5060
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:D,3129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[5]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[5]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[5]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[5]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[5]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[5]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[5]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[5]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_26:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_26:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_26:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_26:CC,6645
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_26:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_26:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_26:S,6645
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_26:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO:A,4519
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO:B,4283
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO:C,5295
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO:D,4244
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO:Y,4244
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_6:A,5270
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_6:B,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_6:CC,5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_6:P,5181
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_6:S,5390
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_6:UB,5092
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_284:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_284:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_284:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_284:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_284:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:CLK,2847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:D,1762
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:Q,2847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:CLK,3072
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:Q,3072
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:D,3254
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:CLK,1639
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:D,8679
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:Q,1639
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[35]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]:A,2020
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]:B,2505
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]:C,4221
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]:D,4089
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[12]:Y,2020
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:CLK,4963
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:D,8673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:Q,4963
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:CLK,5242
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:Q,5242
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[5]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1:An,
MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1:ENn,
MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1:YL,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:CLK,7127
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:D,6703
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:Q,7127
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[25]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[0]:A,6137
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[0]:B,7896
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[0]:C,4615
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[0]:D,5829
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index_RNO[0]:Y,4615
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:C,6810
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPC,6810
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHFT9[7]:A,2891
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHFT9[7]:B,2814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHFT9[7]:C,2380
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHFT9[7]:Y,2380
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_104:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_104:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_104:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_104:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_104:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:CLK,4705
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:Q,4705
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:CLK,4463
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:D,8693
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:Q,4463
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:CLK,2487
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:Q,2487
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[15]:A,4898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[15]:B,4819
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[15]:C,4400
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[15]:Y,4400
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:CLK,7064
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:Q,7064
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:CLK,6771
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:Q,6771
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[9]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[9]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[9]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0LK22[13]:A,1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0LK22[13]:B,1373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0LK22[13]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0LK22[13]:CC,5261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0LK22[13]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0LK22[13]:P,1481
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0LK22[13]:S,5261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0LK22[13]:UB,1373
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[10],6570
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[11],6509
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[1],7165
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[2],7101
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[3],6703
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[4],6636
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[5],6583
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[6],6710
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[7],6618
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[8],6557
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CC[9],6654
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:CO,6453
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[0],6561
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[1],6468
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[2],6608
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[3],6627
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[6],6639
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[7],6645
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[8],6715
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:P[9],6745
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[10],6642
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[11],6763
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[1],6453
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[2],6577
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[3],6496
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[4],6531
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[5],6626
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[6],6517
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[7],6575
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[8],6681
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_0_209_CC_0:UB[9],6624
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:CLK,5847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:Q,5847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:CLK,5089
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:Q,5089
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[1]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[3]:A,2836
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[3]:B,4229
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[3]:C,1445
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[3]:D,1539
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[3]:Y,1445
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0]:B,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0]:C,5849
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0]:CC,6262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0]:P,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0]:S,6262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:CLK,6724
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:D,6857
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:Q,6724
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_13_0:A,3319
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_13_0:B,7123
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_13_0:C,6651
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_13_0:CC,1626
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_13_0:D,4493
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_13_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_13_0:S,1626
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_13_0:UB,4493
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_6_0:A,1483
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_6_0:B,814
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_6_0:C,1226
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_6_0:CC,1059
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_6_0:D,-354
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_6_0:P,-245
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_6_0:S,1059
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_6_0:UB,-354
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:B,7730
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:C,6733
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:IPB,7730
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_10:IPC,6733
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_1_sqmuxa_i_0:A,7602
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_1_sqmuxa_i_0:B,7522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_1_sqmuxa_i_0:C,7780
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_1_sqmuxa_i_0:D,7639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_1_sqmuxa_i_0:Y,7522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[1]:A,3795
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[1]:B,5173
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[1]:C,2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[1]:D,3508
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[1]:Y,2736
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0:B,4422
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0:P,4422
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[1]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[1]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[1]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[1]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_3:A,1598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_3:B,1477
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_3:C,243
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_3:D,860
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_3:Y,243
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[2]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[2]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[2]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:D,6630
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:CLK,1527
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:Q,1527
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_23:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_23:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[0]:A,3044
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[0]:B,5524
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[0]:Y,3044
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_10:B,4958
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_10:UB,4958
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:CLK,2899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:D,8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:Q,2899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[9]:A,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[9]:B,6094
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[9]:C,5390
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[9]:Y,5390
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[11]:A,2613
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[11]:B,2686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[11]:C,2564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[11]:Y,2564
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[14]:A,7808
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[14]:B,5767
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[14]:C,5022
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[14]:CC,4669
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[14]:D,6798
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[14]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[14]:S,4669
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[14]:UB,5022
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_5:B,6129
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_5:UB,6129
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_117:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_117:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_117:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_117:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_117:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO:A,5752
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO:B,5704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO:C,3847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO:D,3767
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_17_RNO:Y,3767
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_224:A,6130
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_224:B,4654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_224:C,6008
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_224:Y,4654
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:B,7909
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:C,6804
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:D,7949
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPB,7909
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPC,6804
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_35:IPD,7949
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[9]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:CLK,4913
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:Q,4913
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:CLK,4235
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:D,8682
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:Q,4235
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:D,8729
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_22:EN,8992
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_22:IPENn,8992
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18:B,2436
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18:C,2391
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18:CC,1592
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18:S,1592
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:CLK,2997
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:D,2671
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:Q,2997
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMTV8H[42]:A,2548
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMTV8H[42]:B,1989
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMTV8H[42]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMTV8H[42]:CC,1294
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMTV8H[42]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMTV8H[42]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMTV8H[42]:S,1294
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIMTV8H[42]:UB,1989
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:CLK,6807
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:Q,6807
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:D,5143
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[2]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[2]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[2]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[2]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINN662[16]:A,4513
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINN662[16]:B,3531
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINN662[16]:C,3487
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINN662[16]:Y,3487
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_15_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_15_0:B,6858
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_15_0:C,3062
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_15_0:CC,2671
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_15_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_15_0:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_15_0:S,2671
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_15_0:UB,3062
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:CC[1],4195
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:CC[2],4089
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:CC[4],4279
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:CC[6],4283
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:CI,4089
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[0],4472
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[1],4444
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[3],4630
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_s_0_219_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNO[11]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNO[11]:B,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNO[11]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNO[11]:CC,4341
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNO[11]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNO[11]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNO[11]:S,4341
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNO[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNICGVP[9]:A,3652
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNICGVP[9]:B,3348
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNICGVP[9]:C,3530
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNICGVP[9]:Y,3348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:CLK,5864
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:Q,5864
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIUNFT[19]:A,3888
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIUNFT[19]:B,3567
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIUNFT[19]:C,3760
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIUNFT[19]:Y,3567
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[8]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[8]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[8]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:CLK,5733
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:D,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:Q,5733
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:CLK,6212
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:D,8671
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:Q,6212
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0_a2_0:A,5068
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0_a2_0:B,4982
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0_a2_0:Y,4982
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[11]:A,3718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[11]:B,3680
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[11]:C,2695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[11]:D,2548
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[11]:Y,2548
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:CLK,7879
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:Q,7879
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:CLK,6207
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:Q,6207
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:CLK,3950
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:D,6277
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:Q,3950
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:CC[0],5308
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:CC[1],5102
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:CC[2],4995
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:CC[3],5211
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:CC[4],5395
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:CC[5],5442
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:CI,4995
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[0],5527
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[1],5427
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[2],5578
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[3],6036
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[4],6207
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:CLK,4125
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:Q,4125
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[37]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[37]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[37]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[37]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:CLK,5907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:Q,5907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[10],3812
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[11],3751
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[1],5378
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[2],5320
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[3],5068
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[4],5000
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[5],4950
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[6],3951
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[7],3860
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[8],3799
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CC[9],3896
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:CO,3674
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[0],4799
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[1],3674
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[2],3789
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[3],3833
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[6],3847
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[7],3808
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[8],3890
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:P[9],3953
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:CC[6],1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:CI,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[0],2077
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[1],2005
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[3],2191
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[0],1925
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[1],2025
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[2],2152
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[3],2071
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:CLK,5062
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:D,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:Q,5062
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:CLK,4904
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:Q,4904
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[8]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[8]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[8]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[8]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIQEE01[9]:A,3285
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIQEE01[9]:B,3208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIQEE01[9]:C,2761
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIQEE01[9]:Y,2761
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1:B,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1:CC,2975
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1:P,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1:S,2975
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:D,5493
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:CLK,2770
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:Q,2770
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:CLK,7919
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:Q,7919
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:CLK,4055
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:D,8686
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:Q,4055
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:CC[0],1270
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:CC[1],988
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:CC[2],1026
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:CC[3],1242
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:CC[4],1100
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:CC[5],1002
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:CC[6],2763
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:CI,988
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[0],1206
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[1],2924
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[3],3096
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_s_0_1260_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_26_0:A,1980
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_26_0:B,1390
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_26_0:C,1472
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_26_0:CC,205
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_26_0:D,228
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_26_0:P,273
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_26_0:S,205
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_26_0:UB,228
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]:A,3361
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]:B,2854
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]:C,5114
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]:D,4996
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[13]:Y,2854
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[16]:A,5889
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[16]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[16]:Y,5889
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CC[9],4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[0],4893
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[1],4468
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[2],4504
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[3],4500
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[6],4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[0],5761
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[1],5871
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[2],5996
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[3],5914
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[4],5953
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[5],6044
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[6],5911
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[7],5964
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[8],6054
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_9_0:A,1589
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_9_0:B,929
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_9_0:C,1341
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_9_0:CC,877
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_9_0:D,-239
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_9_0:P,-139
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_9_0:S,877
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_9_0:UB,-239
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[6]:A,6328
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[6]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[6]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[6]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[6]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_12:A,3158
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_12:B,2917
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_12:P,3066
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_12:UB,2917
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:D,3592
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]:A,1923
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]:B,2433
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]:C,4121
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]:D,4004
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[5]:Y,1923
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_161:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_161:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_161:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_161:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_161:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:CLK,4258
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:Q,4258
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AD,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AL_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SD_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SL_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[0],6757
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[10],6818
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[11],6738
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[12],6763
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[13],6711
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[14],6705
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[15],6731
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[16],6745
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[17],6762
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[1],6733
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[2],6724
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[3],6697
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[4],6709
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[5],6733
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[6],6772
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[7],6747
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[8],6754
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A[9],6747
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_EN[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_EN[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:A_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[0],6791
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[10],6802
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[11],6844
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[12],6795
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[13],6814
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[14],6833
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[15],6859
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[16],6835
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[17],6804
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[1],6841
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[2],6847
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[3],6807
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[4],6810
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[5],6828
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[6],6771
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[7],6818
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[8],6754
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B[9],6809
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_EN[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_EN[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:B_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CARRYIN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[10],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[11],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[12],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[13],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[14],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[15],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[16],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[17],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[18],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[19],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[20],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[21],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[22],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[23],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[24],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[25],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[26],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[27],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[28],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[29],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[2],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[30],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[31],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[32],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[33],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[34],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[35],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[36],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[37],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[38],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[39],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[3],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[40],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[41],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[42],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[43],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[4],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[5],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[6],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[7],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[8],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDIN[9],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:CDSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[0],7662
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[10],7742
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[11],7691
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[12],7689
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[13],7718
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[14],7714
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[15],7787
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[16],7815
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[17],7806
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[18],7809
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[19],7866
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[1],7694
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[20],7863
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[21],7849
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[22],7856
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[23],7853
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[24],7832
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[25],7933
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[26],7919
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[27],7884
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[28],7946
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[29],7895
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[2],7727
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[30],7886
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[31],7889
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[32],7869
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[33],7832
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[34],7817
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[35],7879
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[36],7864
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[37],7827
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[38],7871
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[39],7837
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[3],7685
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[40],7852
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[41],7886
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[42],7909
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[43],7949
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[4],7657
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[5],7641
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[6],7686
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[7],7671
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[8],7661
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C[9],7730
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_EN[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_EN[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:C_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:DOTP,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:OVFL_CARRYOUT_SEL,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[0],8721
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[10],8717
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[11],8719
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[12],8717
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[13],8717
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[14],8716
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[15],8717
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[16],8712
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[17],8710
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[18],8686
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[19],8681
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[1],8725
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[20],8684
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[21],8682
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[22],8683
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[23],8682
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[24],8677
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[25],8676
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[26],8680
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[27],8679
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[28],8679
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[29],8674
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[2],8725
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[30],8676
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[31],8676
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[32],8677
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[33],8682
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[34],8681
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[35],8674
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[36],8682
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[37],8677
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[38],8673
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[39],8674
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[3],8729
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[40],8673
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[41],8674
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[42],8668
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[43],8678
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[4],8724
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[5],8724
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[6],8728
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[7],8728
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[8],8730
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P[9],8725
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_CLK[0],8710
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_CLK[1],8668
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_EN[0],8996
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_EN[1],9019
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:P_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SIMD,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_AD,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_AL_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_SD_N,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP:SUB_SL_N,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:CLK,3008
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:D,2192
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:Q,3008
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_3:A,7128
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_3:B,6938
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_3:CC,7145
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_3:P,7036
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_3:S,7145
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_3:UB,6938
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3SET[17]:A,3847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3SET[17]:B,3531
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3SET[17]:C,3724
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3SET[17]:Y,3531
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[34]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[34]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[34]:Y,5366
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o_1_sqmuxa_0_a2:A,5477
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o_1_sqmuxa_0_a2:B,5084
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o_1_sqmuxa_0_a2:C,5229
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o_1_sqmuxa_0_a2:D,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o_1_sqmuxa_0_a2:Y,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:CLK,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:Q,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1[0]:A,6818
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1[0]:B,5769
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1[0]:C,4649
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1[0]:D,4638
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1[0]:Y,4638
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:CLK,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:Q,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[14]:A,2147
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[14]:B,4266
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[14]:C,1964
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_am[14]:Y,1964
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_13:A,2501
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_13:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_13:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_13:IPA,2501
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[9]:A,1483
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[9]:B,5200
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[9]:Y,1483
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[36]:A,738
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[36]:B,595
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[36]:C,121
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[36]:Y,121
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:CLK,6807
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:Q,6807
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[1]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[1]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[1]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[1]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_2:B,3514
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_2:CC,3824
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_2:P,3514
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_2:S,3824
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:CLK,3116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:D,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:Q,3116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINFET[11]:A,3722
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINFET[11]:B,3639
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINFET[11]:C,3341
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINFET[11]:Y,3341
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:CLK,2473
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:D,8673
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:Q,2473
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:CLK,6147
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:Q,6147
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[3]:A,2207
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[3]:B,1445
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[3]:C,3860
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[3]:D,1563
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[3]:Y,1445
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[7]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_11:A,7129
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_11:B,7057
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_11:C,6614
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_11:CC,6618
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_11:P,6668
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_11:S,6618
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_11:UB,6614
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:CLK,5295
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:Q,5295
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:CLK,6169
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:Q,6169
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[4]:A,3506
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[4]:B,3319
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[4]:C,6622
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[4]:D,4261
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[4]:Y,3319
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10]:B,6473
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10]:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10]:CC,5641
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10]:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10]:S,5641
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:CLK,7849
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:Q,7849
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[1],1806
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[2],1887
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[3],1634
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[6],1613
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[7],1544
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[8],1565
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CC[9],1663
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:CO,1445
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[0],1488
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[1],1445
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[2],1575
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[3],1604
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[6],1616
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[7],1612
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[8],1682
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:P[9],1722
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:CLK,4422
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:Q,4422
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0:A,6972
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0:B,6800
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0:P,6927
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0:UB,6800
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:CLK,7742
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:D,7910
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:Q,7742
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sys_clk_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_4:B,4253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_4:UB,4253
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:CLK,6816
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:Q,6816
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_0[2]:A,3869
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_0[2]:B,3795
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_0[2]:C,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIURLK_0[2]:Y,1775
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:CLK,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:Q,6795
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s[17]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s[17]:B,5767
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s[17]:C,7683
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s[17]:CC,4627
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s[17]:D,4652
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s[17]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s[17]:S,4627
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_s[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_8:A,3179
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_8:B,3089
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_8:P,3117
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_8:UB,3089
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_0:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_0:C,4275
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_0:IPC,4275
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5:A,6847
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5:B,6770
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5:C,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5:D,5186
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_5:Y,4359
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24:A,7137
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24:B,3766
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24:C,3643
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24:CC,3315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24:P,3764
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24:S,3315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24:UB,3643
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7G0J[11]:A,2953
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7G0J[11]:B,2876
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7G0J[11]:C,2442
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7G0J[11]:Y,2442
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[14]:A,1964
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[14]:B,2836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[14]:C,5124
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[14]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[14]:D,4979
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[14]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[14]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[14]:Y,1964
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_9:A,4310
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_9:B,6127
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_9:P,4310
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_9:UB,6127
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:D,3501
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_12:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_12:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_5:A,5964
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_5:B,5267
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_5:CC,5118
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_5:S,5118
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_5:UB,5267
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_7:A,1718
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_7:B,1830
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_7:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_7:IPA,1718
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_7:IPB,1830
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_12:A,5045
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_12:B,4798
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_12:P,4959
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_12:UB,4798
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:CLK,4767
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:Q,4767
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:CLK,5196
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:Q,5196
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:CLK,7805
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:D,7794
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:Q,7805
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_275:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_275:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_275:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_275:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_275:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_32:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_32:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[6]:A,1407
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[6]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[6]:Y,1407
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_5:B,6169
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_5:UB,6169
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_15:A,7749
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_15:B,7237
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_15:CC,6791
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_15:S,6791
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_15:UB,7237
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:CLK,1597
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:D,8680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:Q,1597
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_3:A,2802
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_3:B,2712
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_3:P,2802
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_3:UB,2712
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16_0:A,6219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16_0:B,7274
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16_0:C,7467
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16_0:CC,5376
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16_0:S,5376
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16_0:UB,7467
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_14:B,6238
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_14:UB,6238
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[0]:A,6641
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[0]:B,6852
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[0]:C,3675
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[0]:D,3692
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[0]:Y,3675
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_222:A,6179
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_222:B,4704
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_222:C,6057
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_222:Y,4704
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[7]:A,4747
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[7]:B,2211
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[7]:C,2167
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[7]:Y,2167
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:CLK,5738
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:EN,2979
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:Q,5738
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/direction_config_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIKT6GI[4]:A,6991
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIKT6GI[4]:B,1501
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIKT6GI[4]:C,1571
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIKT6GI[4]:CC,1275
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIKT6GI[4]:D,6079
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIKT6GI[4]:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIKT6GI[4]:S,1275
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIKT6GI[4]:UB,1501
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:C,6835
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPC,6835
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_6:A,7120
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_6:B,6946
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_6:CC,7044
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_6:P,7048
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_6:S,7044
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_6:UB,6946
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[33]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[33]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[33]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[33]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[33]:Y,224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10:A,3804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10:B,2835
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10:CC,2862
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10:S,2862
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10:UB,2835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_1:A,3526
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_1:B,4389
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_1:C,3411
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_1_RNO_1:Y,3411
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[16]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[16]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[16]:C,5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[16]:Y,5079
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:CLK,4100
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:D,8716
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:Q,4100
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:CLK,1589
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:D,8681
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:Q,1589
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:D,5222
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0:B,3427
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0:P,3427
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[10]:A,7129
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[10]:B,5081
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[10]:C,4846
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[10]:CC,4786
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[10]:D,6622
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[10]:P,4956
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[10]:S,4786
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[10]:UB,4846
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNICLE93[12]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNICLE93[12]:B,7792
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNICLE93[12]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNICLE93[12]:CC,6944
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNICLE93[12]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNICLE93[12]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNICLE93[12]:S,6944
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNICLE93[12]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[2]_CC_0:UB[9],
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[10]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[10]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[10]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[10]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:CLK,5834
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:D,6781
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:Q,5834
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_2:A,1275
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_2:B,1574
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_2:P,1275
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_2:UB,1574
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:D,5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_0_sqmuxa_0_a3:A,6540
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_0_sqmuxa_0_a3:B,6418
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_0_sqmuxa_0_a3:C,6718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_0_sqmuxa_0_a3:D,6640
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_0_sqmuxa_0_a3:Y,6418
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_11:B,1557
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_11:UB,1557
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[16]:A,6134
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[16]:B,6175
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[16]:C,4673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[16]:D,5672
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[16]:Y,4673
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_41:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_41:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_41:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_41:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_41:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:CLK,1373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:D,8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:Q,1373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:CC[0],5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:CC[1],5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:CC[2],5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:CC[3],5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:CC[4],5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:CC[5],4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:CI,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[0],5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[1],4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[2],5211
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[3],5395
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[4],5442
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[5]:A,6144
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[5]:B,6096
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[5]:C,5392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[5]:Y,5392
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:CLK,4986
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:Q,4986
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:CLK,4964
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:Q,4964
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[4]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[4]:B,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[4]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[4]:CC,7114
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[4]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[4]:P,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[4]:S,7114
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[2]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_10:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_10:B,1843
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_10:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_10:IPB,1843
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[15]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_5_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_5_PAD/U_IOINFF:Y,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_0:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_0:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_0:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_0:IPA,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_2_2:A,4165
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_2_2:B,4100
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_2_2:C,3987
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o_1_sqmuxa_0_a2_2_2:Y,3987
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:CLK,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:D,8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:Q,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:CLK,6833
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:Q,6833
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:B,7671
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:C,6810
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:D,7661
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPB,7671
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPC,6810
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPD,7661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel_RNO:A,7630
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_sel_RNO:Y,7630
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:CLK,5124
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:D,3716
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:Q,5124
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[13]:SLn,
MC_System_0/MC_System_sb_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_14:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_14:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:CLK,1074
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:D,4022
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:Q,1074
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:CLK,5142
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:D,8669
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:Q,5142
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_12:B,6339
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_12:C,4290
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_12:IPB,6339
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_12:IPC,4290
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[33]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[33]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[33]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_15:A,4018
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_15:B,6167
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_15:P,4018
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_15:UB,6167
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_6:A,6173
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_6:B,6068
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_6:P,6127
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_6:UB,6068
A0_PWM_UL_O_obuf/U0/U_IOOUTFF:A,2345
A0_PWM_UL_O_obuf/U0/U_IOOUTFF:Y,2345
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_14:A,3713
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_14:B,4004
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_14:C,2843
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_14:D,2765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_14:Y,2765
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_1:A,3017
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_1:B,2975
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_1:P,2977
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_1:UB,2975
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_18:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_18:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_15:A,5025
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_15:B,2871
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_15:P,2998
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_15:UB,2871
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_13_0:A,1535
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_13_0:B,860
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_13_0:C,1272
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_13_0:CC,631
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_13_0:D,-308
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_13_0:P,-193
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_13_0:S,631
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_13_0:UB,-308
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[8]:A,4779
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[8]:B,4384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[8]:C,4273
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_1_0[8]:Y,4273
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:CLK,4032
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:Q,4032
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNICF8E5[3]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNICF8E5[3]:B,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNICF8E5[3]:C,7716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNICF8E5[3]:CC,5000
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNICF8E5[3]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNICF8E5[3]:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNICF8E5[3]:S,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNICF8E5[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_4:A,7749
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_4:B,6818
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_4:CC,6932
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_4:S,6932
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_4:UB,6818
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[3]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[3]:B,7661
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[3]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[3]:CC,7046
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[3]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[3]:P,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[3]:S,7046
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[5]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[5]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[5]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0:B,1488
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0:P,1488
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:CLK,1272
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:D,1275
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:Q,1272
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_4:B,7527
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_4:C,7588
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_4:CC,6862
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_4:S,6862
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:CLK,1980
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:D,8682
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:Q,1980
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:CLK,4898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:Q,4898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:CLK,6953
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:Q,6953
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:CC[6],5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:CI,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[0],6198
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[1],6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[3],6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[0],6037
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[1],6137
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[2],6286
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[3],6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[4],6220
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[5],6299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:D,6958
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[7]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:CLK,5297
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:D,3796
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:Q,5297
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_4_0:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_4_0:B,6428
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_4_0:C,5288
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_4_0:CC,5401
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_4_0:D,6729
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_4_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_4_0:S,5401
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_4_0:UB,5288
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17:B,6299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_17:UB,6299
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[9]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[9]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[9]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[9]:Y,6726
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_2_0[1]:A,2413
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_2_0[1]:B,2766
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_2_0[1]:C,2522
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_2_0[1]:D,2268
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_2_0[1]:Y,2268
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[12]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[12]:B,5085
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[12]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[12]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[12]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done_129:A,7977
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done_129:B,7811
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done_129:C,7869
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done_129:Y,7811
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[0]:A,5415
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[0]:B,6042
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[0]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[0]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[0]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:B,7869
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:C,6705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:IPB,7869
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_28:IPC,6705
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[10],1397
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[11],1350
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[1],1670
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[2],1669
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[3],1574
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[4],1398
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[5],1381
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[6],1523
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[7],1330
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[8],1323
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CC[9],1510
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:CO,1213
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[0],1306
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[1],1213
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[2],1353
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[3],1372
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[6],1384
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[7],1387
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[8],1460
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:P[9],1490
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_s_0_1261_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_18:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_18:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[33]:A,589
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[33]:B,446
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[33]:C,-28
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[33]:Y,-28
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:CLK,2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:Q,2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0:A,3367
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0:B,1448
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0:P,1595
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_0:UB,1448
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:D,5478
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[35]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[35]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[35]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2:A,7073
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2:B,7025
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2:CC,7467
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2:P,7057
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2:S,7467
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_2:UB,7025
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_1[2]:A,2141
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_1[2]:B,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_1[2]:Y,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[14]:A,3178
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[14]:B,2047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[14]:C,3237
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[14]:D,3150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[14]:Y,2047
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:CLK,3928
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:Q,3928
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[16]:A,6256
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[16]:B,7456
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[16]:C,6998
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[16]:CC,5710
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[16]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[16]:P,6256
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[16]:S,5710
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[16]:UB,6998
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:CC[6],3828
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:CI,3946
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[0],3934
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[1],3828
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[3],4018
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[0],6016
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[1],6112
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[2],6238
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[3],6167
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[4],6208
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[5],4022
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[11]:A,2323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[11]:B,5623
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[11]:C,2282
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[11]:Y,2282
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:CC[1],4276
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:CC[2],4170
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:CC[4],4360
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:CC[6],4364
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:CI,4170
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[0],4553
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[1],4525
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[3],4711
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3_1[4]:A,5083
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3_1[4]:B,6032
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3_1[4]:C,1002
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3_1[4]:D,1827
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a3_1[4]:Y,1002
QB_I_ibuf/U0/U_IOPAD:PAD,6192
QB_I_ibuf/U0/U_IOPAD:Y,6192
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:CLK,1452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:D,8712
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:Q,1452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]:A,2861
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]:B,3371
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]:C,5059
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]:D,4942
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[13]:Y,2861
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[2]:A,2430
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[2]:B,1668
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[2]:C,4083
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[2]:D,1786
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_0[2]:Y,1668
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[14]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[14]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[14]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[14]:CC,6925
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[14]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[14]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[14]:S,6925
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[14]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[8]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[8]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[8]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[8]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_13_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_13_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_13_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_13_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_13_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[17]:A,6978
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[17]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[17]:C,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[17]:Y,5018
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_RNIHAGU:A,7797
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_RNIHAGU:B,7720
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_RNIHAGU:C,6719
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_RNIHAGU:D,5430
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_RNIHAGU:Y,5430
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:CLK,3971
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:D,8717
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:Q,3971
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_7:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11:A,7808
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11:B,5308
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11:CC,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11:S,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11:UB,5308
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:CLK,6122
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:Q,6122
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_34:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_34:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:CLK,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:D,7711
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:Q,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_state[0]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[6]:A,7827
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[6]:B,7920
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[6]:Y,7827
MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2_1[0]:A,3129
MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2_1[0]:B,3090
MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2_1[0]:Y,3090
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:CLK,1452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:D,8710
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:Q,1452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[16]:A,6432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[16]:B,6355
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[16]:C,5954
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[16]:D,4739
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[16]:Y,4739
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_FCINST1:CC,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_FCINST1:CO,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_16_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:CLK,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:D,5067
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:Q,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1SGT[25]:A,3918
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1SGT[25]:B,3614
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1SGT[25]:C,3796
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1SGT[25]:Y,3614
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[15]:A,1346
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[15]:B,5072
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[15]:Y,1346
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_19:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_19:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/en_o:A,1402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/en_o:B,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/en_o:C,1826
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/en_o:D,1298
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/en_o:Y,88
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:CLK,7839
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:D,6661
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:Q,7839
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a2[0]:A,4036
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a2[0]:B,3962
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a2[0]:C,2922
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a2[0]:Y,2922
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_5:B,4701
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_5:C,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_5:CC,3676
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_5:S,3676
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_5:UB,4701
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_7:A,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_7:B,6122
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_7:P,6167
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_7:UB,6122
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[10]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[10]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[10]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[10]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[8]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[8]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[8]:C,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[8]:Y,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_15_0:A,7841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_15_0:B,6821
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_15_0:C,5116
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_15_0:CC,1829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_15_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_15_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_15_0:S,1829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_15_0:UB,5116
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_243:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_243:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_243:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_243:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_243:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_281:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_281:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_281:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_281:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_281:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:CLK,1747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:D,8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:Q,1747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:CLK,6183
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:Q,6183
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_34:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_34:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_13:A,4854
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_13:B,2800
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_13:P,2803
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_13:UB,2800
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[3]:A,6322
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[3]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[3]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[3]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[3]:Y,2538
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[9]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_88:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_88:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_88:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_88:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_88:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:CLK,6768
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:D,4135
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:Q,6768
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[43]:A,695
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[43]:B,552
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[43]:C,78
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[43]:Y,78
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state_RNO[0]:A,7997
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state_RNO[0]:B,7906
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state_RNO[0]:C,6418
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_state_RNO[0]:Y,6418
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:CLK,6802
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:Q,6802
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:CLK,3197
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:Q,3197
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_128:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_128:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_128:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_128:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_128:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:CLK,5114
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:D,5721
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:Q,5114
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIT6HN5[20]:A,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIT6HN5[20]:B,1519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIT6HN5[20]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIT6HN5[20]:CC,5059
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIT6HN5[20]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIT6HN5[20]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIT6HN5[20]:S,5059
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIT6HN5[20]:UB,1519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:B,7689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:C,6772
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:IPB,7689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:IPC,6772
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o_1_sqmuxa_i:A,7784
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o_1_sqmuxa_i:B,7749
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o_1_sqmuxa_i:C,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o_1_sqmuxa_i:D,7584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o_1_sqmuxa_i:Y,5103
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_s_33:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_s_33:B,7713
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_s_33:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_s_33:CC,3165
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_s_33:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_s_33:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_s_33:S,3165
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_s_33:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/un1_s_acc_in_0_sqmuxa_0:A,7401
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/un1_s_acc_in_0_sqmuxa_0:B,7324
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/un1_s_acc_in_0_sqmuxa_0:C,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/un1_s_acc_in_0_sqmuxa_0:Y,5621
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[2]:A,7931
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[2]:B,7880
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[2]:C,6918
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[2]:D,6813
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[2]:Y,6813
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_235:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_235:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_235:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_235:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_235:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:D,8730
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:CLK,2091
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:Q,2091
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_6:A,4260
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_6:B,6020
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_6:P,4260
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_6:UB,6020
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:CLK,4929
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:Q,4929
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_7:A,3044
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_7:B,4637
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_7:P,3044
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_7:UB,4637
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:CLK,7727
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:Q,7727
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15_0:A,6219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15_0:B,7274
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15_0:C,7339
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15_0:CC,5447
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15_0:S,5447
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15_0:UB,7339
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:B,7864
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:C,6859
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:D,7827
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPB,7864
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPC,6859
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPD,7827
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_18:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_18:B,7048
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_18:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_18:CC,6917
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_18:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_18:P,7048
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_18:S,6917
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_18:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:CLK,4190
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:D,8681
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:Q,4190
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_9_0:A,2991
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_9_0:B,2948
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_9_0:C,2866
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_9_0:D,2765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_9_0:Y,2765
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0:A,7012
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0:B,6793
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0:P,6920
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_0:UB,6793
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[2]:A,4323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[2]:B,6667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[2]:C,3274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[2]:D,4073
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[2]:Y,3274
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:CLK,4991
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:Q,4991
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:CLK,5069
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:D,8697
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:Q,5069
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:CLK,6835
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:Q,6835
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[17]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:CLK,6851
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:D,6843
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:EN,7854
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:Q,6851
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_result_done:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO:A,5671
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO:B,5907
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO:C,3766
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO:D,5451
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO:Y,3766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[16]:A,4909
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[16]:B,4832
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[16]:C,4414
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[16]:Y,4414
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[18]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[18]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[18]:Y,7555
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[3]:A,1550
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[3]:B,2920
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[3]:C,4664
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[3]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[3]:D,4510
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[3]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[3]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[3]:Y,1550
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:CLK,4981
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:D,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:Q,4981
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:CLK,7817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:Q,7817
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:CLK,6847
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:Q,6847
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:CLK,6814
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:Q,6814
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_10_i_a3_0_a2_RNII7NQ[1]:A,1074
BLDC_Encoder_Axis_0/MSC_i_13/state_o_10_i_a3_0_a2_RNII7NQ[1]:B,88
BLDC_Encoder_Axis_0/MSC_i_13/state_o_10_i_a3_0_a2_RNII7NQ[1]:C,972
BLDC_Encoder_Axis_0/MSC_i_13/state_o_10_i_a3_0_a2_RNII7NQ[1]:D,887
BLDC_Encoder_Axis_0/MSC_i_13/state_o_10_i_a3_0_a2_RNII7NQ[1]:Y,88
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:CLK,6068
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:D,8677
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:Q,6068
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_17:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_17:IPENn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:CO,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[0],5948
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[1],4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[2],4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[3],4380
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[6],4293
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[7],4268
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[8],4278
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:P[9],4362
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[0],5796
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[10],4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[11],4287
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[1],4640
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[2],4722
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[3],4290
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[4],4253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[5],4299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[6],4230
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[7],4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[8],4244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_0_CC_0:UB[9],4308
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_10:A,7835
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_10:B,6903
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_10:CC,6940
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_10:S,6940
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_10:UB,6903
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_77:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_77:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_77:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_77:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_77:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_6:B,6100
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_6:C,6174
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_6:CC,6075
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_6:P,6100
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_6:S,6075
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:CLK,1899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:D,8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:Q,1899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_20:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_20:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_17:B,3325
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_17:UB,3325
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]:A,2875
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]:B,3269
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]:C,5093
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]:D,4969
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_i_m2_0_0_wmux[11]:Y,2875
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_1:A,3922
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_1:B,3874
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_1:C,3787
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_1:D,3682
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_1:Y,3682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ID_PI_DONE_PROC_op_eq_un15_clear_buffer_i:A,7904
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ID_PI_DONE_PROC_op_eq_un15_clear_buffer_i:B,7819
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ID_PI_DONE_PROC_op_eq_un15_clear_buffer_i:Y,7819
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[34]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[34]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[34]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[34]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:B,7866
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:C,6747
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:IPB,7866
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_18:IPC,6747
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:CLK,2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:D,1713
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:Q,2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[18]:A,3370
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[18]:B,2458
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[18]:C,2677
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[18]:D,2368
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[18]:Y,2368
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:CLK,5167
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:D,3735
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:Q,5167
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI70O81[12]:A,3141
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI70O81[12]:B,3064
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI70O81[12]:C,2617
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI70O81[12]:Y,2617
BLDC_Encoder_Axis_0/MSC_i_27/s_state_ns[1]:A,8004
BLDC_Encoder_Axis_0/MSC_i_27/s_state_ns[1]:B,7920
BLDC_Encoder_Axis_0/MSC_i_27/s_state_ns[1]:C,7751
BLDC_Encoder_Axis_0/MSC_i_27/s_state_ns[1]:D,7699
BLDC_Encoder_Axis_0/MSC_i_27/s_state_ns[1]:Y,7699
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[13]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[13]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[13]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[13]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[13]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[13]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[13]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[3]:A,7938
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[3]:B,1540
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[3]:C,7842
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[3]:D,7742
BLDC_Encoder_Axis_0/MSC_i_13/s_restart_count_RNO[3]:Y,1540
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1_RNIM6421:A,4756
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1_RNIM6421:B,4699
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1_RNIM6421:C,4640
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1_RNIM6421:Y,4640
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_31:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_31:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[5]:A,6204
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[5]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[5]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[5]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[5]:Y,2538
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_24:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_24:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:CLK,7047
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:D,6703
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:Q,7047
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:CLK,4794
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:Q,4794
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[4]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[1]:A,6979
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[1]:B,6949
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[1]:C,7836
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[1]:D,7755
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[1]:Y,6949
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[8]:A,1443
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[8]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[8]:Y,1443
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:CLK,1563
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:D,8686
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:Q,1563
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[3]:A,3649
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[3]:B,5024
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[3]:C,2587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[3]:D,3359
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[3]:Y,2587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_7:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_7:C,4474
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_7:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_7:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_7:IPC,4474
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_7:IPD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:CLK,6859
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:Q,6859
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:CLK,3754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:D,6920
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:Q,3754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI9NCS5[4]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI9NCS5[4]:B,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI9NCS5[4]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI9NCS5[4]:CC,5223
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI9NCS5[4]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI9NCS5[4]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI9NCS5[4]:S,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI9NCS5[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_1_0:A,7093
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_1_0:B,6629
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_1_0:C,2833
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_1_0:CC,3272
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_1_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_1_0:P,2864
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_1_0:S,3272
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_1_0:UB,2833
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI8K3M4[18]:A,1647
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI8K3M4[18]:B,1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI8K3M4[18]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI8K3M4[18]:CC,5046
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI8K3M4[18]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI8K3M4[18]:P,1598
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI8K3M4[18]:S,5046
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI8K3M4[18]:UB,1560
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:CLK,5136
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:D,8663
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:Q,5136
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_31:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_31:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_31:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_31:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_31:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[7]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[7]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[7]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:CC[6],4170
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:CI,4288
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[0],4276
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[1],4170
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[3],4360
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[0],6084
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[1],6180
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[2],6306
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[3],6235
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[4],6276
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[5],4364
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:CLK,4379
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:D,6871
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:Q,4379
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:D,8717
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[13]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:CLK,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:Q,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[16]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_145:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_145:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_145:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_145:IPA,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_7:A,4399
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_7:B,4312
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_7:P,4357
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_7:UB,4312
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un103_s_state_i_a3_0_a2_i:A,5058
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un103_s_state_i_a3_0_a2_i:B,5910
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_un103_s_state_i_a3_0_a2_i:Y,5058
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[11]:A,6046
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[11]:B,2548
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[11]:C,2564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[11]:Y,2548
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[15]:A,5996
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[15]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[15]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[15]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[15]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[3]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:CLK,6828
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:D,6987
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:Q,6828
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:CLK,5216
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:Q,5216
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[24]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[24]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[24]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[24]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10_RNO:A,5834
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10_RNO:B,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10_RNO:C,5712
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10_RNO:Y,4359
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:CLK,7056
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:D,4453
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:Q,7056
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[10],4148
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[11],4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[1],5677
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[2],5613
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[3],5341
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[4],5273
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[5],5223
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[6],4288
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[7],4196
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[8],4135
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CC[9],4232
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:CO,4188
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[0],5150
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[1],4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[2],4240
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[3],4245
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[6],4226
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[7],4368
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[8],4449
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:P[9],4465
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_7:A,1127
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_7:B,1323
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_7:P,1127
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_7:UB,1323
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o_1_sqmuxa_0_a2:A,5499
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o_1_sqmuxa_0_a2:B,5105
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o_1_sqmuxa_0_a2:C,5188
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o_1_sqmuxa_0_a2:D,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o_1_sqmuxa_0_a2:Y,2867
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:CLK,4370
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:Q,4370
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[15]:A,1291
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[15]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[15]:Y,1291
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_25:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_25:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[10]:A,6985
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[10]:B,6901
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[10]:C,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[10]:Y,6226
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_0_a3[7]:A,5936
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_0_a3[7]:B,5516
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_0_a3[7]:C,5445
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_0_a3[7]:Y,5445
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[2]:A,2624
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[2]:B,5850
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[2]:Y,2624
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_205:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_205:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_205:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_205:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_205:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_205:IPC,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:CLK,4469
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:D,6850
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:Q,4469
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/op_eq_un3_init_o:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/op_eq_un3_init_o:B,5423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/op_eq_un3_init_o:Y,4589
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[1]:A,1758
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[1]:B,5475
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[1]:Y,1758
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19:A,7063
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19:B,3716
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19:C,3673
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19:CC,3315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19:P,3686
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19:S,3315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_19:UB,3673
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:CLK,7225
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:Q,7225
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_16_0:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_16_0:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_16_0:C,5861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_16_0:CC,5166
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_16_0:D,7329
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_16_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_16_0:S,5166
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_16_0:UB,5861
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO:A,2121
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO:B,1955
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO:C,5581
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0_RNO:Y,1955
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOUA53[16]:A,6256
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOUA53[16]:B,1366
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOUA53[16]:C,1436
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOUA53[16]:CC,1788
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOUA53[16]:D,5950
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOUA53[16]:P,1398
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOUA53[16]:S,1788
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOUA53[16]:UB,1366
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0:A,2196
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0:B,2853
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0:C,2802
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0:P,2196
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_0:UB,2802
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_15:B,7023
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_15:CC,7059
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_15:P,7023
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_15:S,7059
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:D,8703
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:CLK,6795
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:Q,6795
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:B,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:C,6733
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_2:IPC,6733
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[13]:A,3320
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[13]:B,3307
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[13]:C,2329
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[13]:D,2248
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[13]:Y,2248
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[1]:A,5732
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[1]:B,6907
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[1]:C,6451
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[1]:CC,5877
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[1]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[1]:P,5732
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[1]:S,5877
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[1]:UB,6451
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8:A,7180
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8:B,5282
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8:CC,5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8:P,5315
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8:S,5222
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8:UB,5282
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:CC[0],1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:CC[1],1249
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:CC[2],1328
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:CC[3],1314
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:CC[4],1282
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:CC[5],1334
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:CC[6],1592
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:CI,1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[0],1573
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[1],1842
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[3],2028
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[0],1760
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[1],1524
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[2],1651
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[3],1908
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[4],1945
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[5],2039
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o_1_sqmuxa_i:A,7792
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o_1_sqmuxa_i:B,7707
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o_1_sqmuxa_i:C,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o_1_sqmuxa_i:D,7584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o_1_sqmuxa_i:Y,5103
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:CLK,4106
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:Q,4106
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:D,5174
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_4:B,4252
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_4:UB,4252
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO_0:A,5702
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO_0:B,5612
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO_0:C,3754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO_0:D,3667
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_14_RNO_0:Y,3667
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:CLK,3372
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:EN,3182
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:Q,3372
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[2]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[3]:A,1563
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[3]:B,2435
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[3]:C,4732
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[3]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[3]:D,4572
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[3]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[3]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[3]:Y,1563
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_21_0:A,1927
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_21_0:B,1250
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_21_0:C,1332
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_21_0:CC,518
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_21_0:D,88
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_21_0:P,192
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_21_0:S,518
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_21_0:UB,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[11]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[11]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[11]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[11]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[9]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[9]:B,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[9]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[9]:CC,7028
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[9]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[9]:P,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[9]:S,7028
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_s[17]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_s[17]:B,7661
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_s[17]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_s[17]:CC,6917
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_s[17]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_s[17]:P,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_s[17]:S,6917
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_s[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[13]:A,5006
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[13]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[13]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[13]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[13]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:CLK,6835
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:Q,6835
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:CLK,5123
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:Q,5123
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[7]:SLn,
A0_ADC_CS_O_obuf/U0/U_IOOUTFF:A,4164
A0_ADC_CS_O_obuf/U0/U_IOOUTFF:Y,4164
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[30]:A,460
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[30]:B,383
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[30]:C,-157
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[30]:Y,-157
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:CLK,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:Q,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[8]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[8]:B,4457
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[8]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[8]:Y,91
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO_0:A,5706
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO_0:B,5612
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO_0:C,3755
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO_0:D,3675
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_11_RNO_0:Y,3675
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:CC[0],5257
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:CC[1],5187
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:CC[2],5143
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:CC[3],5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:CC[4],5045
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:CC[5],4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:CI,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[0],5102
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[1],4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[2],5211
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[3],5395
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[4],5442
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_24:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_24:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[10],5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[11],5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[1],5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[2],5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[3],5342
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[4],5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[5],5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[6],5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[7],5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[8],5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CC[9],5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:CO,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[0],5074
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[1],5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[2],5148
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[3],5177
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[6],5189
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[7],5185
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[8],5255
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:P[9],5295
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_12:A,546
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_12:B,408
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_12:C,492
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_12:D,308
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_12:Y,308
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[2]:A,1830
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[2]:B,3900
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[2]:C,3333
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[2]:Y,1830
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:D,3454
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[8]:A,7808
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[8]:B,5767
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[8]:C,4944
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[8]:CC,4762
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[8]:D,6720
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[8]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[8]:S,4762
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[8]:UB,4944
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_3:A,6161
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_3:B,6029
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_3:P,6115
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_3:UB,6029
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7:B,1612
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7:CC,1544
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7:P,1612
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7:S,1544
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:CLK,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:Q,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:CLK,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:D,4995
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:Q,6951
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/va3h_o_Z[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0:A,7120
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0:B,6519
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0:C,4353
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0:CC,2297
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0:D,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0:P,2231
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0:S,2297
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0:UB,2119
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o_0_sqmuxa:A,7688
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o_0_sqmuxa:B,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o_0_sqmuxa:Y,7653
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_NXT_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_NXT_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:CLK,7740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:D,8639
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:Q,7740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/done_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[7]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[7]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[7]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[7]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:CLK,6847
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:Q,6847
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20:A,7145
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20:B,3822
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20:C,3768
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20:CC,3254
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20:P,3768
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20:S,3254
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_20:UB,3779
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[2]:A,6095
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[2]:B,6047
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[2]:C,5343
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[2]:Y,5343
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:C,6772
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:IPC,6772
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:CLK,6828
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:Q,6828
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:CLK,1682
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:Q,1682
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNICTCT3[2]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNICTCT3[2]:B,4245
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNICTCT3[2]:C,7082
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNICTCT3[2]:CC,5341
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNICTCT3[2]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNICTCT3[2]:P,4245
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNICTCT3[2]:S,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNICTCT3[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[19]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[19]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[19]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_13:A,1261
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_13:B,3147
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_13:P,1261
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_13:UB,3166
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_35:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_35:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:CLK,4233
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:D,8840
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:EN,7522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:Q,4233
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:CLK,6733
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:Q,6733
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:CLK,1890
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:D,8673
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:Q,1890
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:CLK,1402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:D,8710
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:Q,1402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[7]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[7]:B,4518
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[7]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[7]:Y,91
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:D,8717
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:CLK,6828
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:Q,6828
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[5]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_181:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_181:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_181:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_181:IPA,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[11]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[11]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[11]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:B,7933
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:C,6738
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:IPB,7933
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:IPC,6738
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_13:A,6234
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_13:B,4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_13:P,4114
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_13:UB,4130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2:A,6858
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2:B,3464
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2:C,3408
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2:CC,4044
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2:P,3434
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2:S,4044
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_2:UB,3408
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJFG2A[7]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJFG2A[7]:B,7171
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJFG2A[7]:C,2872
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJFG2A[7]:CC,2889
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJFG2A[7]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJFG2A[7]:P,2872
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJFG2A[7]:S,2889
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJFG2A[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[6]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[6]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[6]:C,5296
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[6]:Y,5296
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:C,6814
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:IPC,6814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_18:A,7531
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_18:B,7592
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_18:C,5754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_18:D,6291
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_18:Y,5754
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:CLK,4377
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:D,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:Q,4377
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_21:B,6496
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_21:C,5445
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_21:D,6475
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_21:IPB,6496
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_21:IPC,5445
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_21:IPD,6475
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:CLK,6705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:D,5158
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:Q,6705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[14]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_XCLK_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_XCLK_PAD/U_IOINFF:Y,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_10:B,7527
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_10:C,7556
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_10:CC,6695
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_10:S,6695
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_1:B,6063
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_1:C,6137
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_1:CC,6523
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_1:P,6063
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_1:S,6523
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_1:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_112:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_112:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_112:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_112:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_112:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:CLK,1402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:D,7296
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:Q,1402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:C,6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPC,6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:CLK,6603
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:D,7923
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:Q,6603
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[3]:A,3964
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[3]:B,3873
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[3]:C,3677
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[3]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[3]:Y,3677
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:CO,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[0],1894
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[1],1844
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[2],2018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[3],2003
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[6],2015
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[7],2055
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[8],2125
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:P[9],2121
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[0],1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[10],2059
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[11],2180
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[1],1870
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[2],1994
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[3],1913
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[4],1950
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[5],2043
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[6],1934
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[7],1992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[8],2100
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_0_CC_0:UB[9],2041
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:CLK,1454
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:D,8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:Q,1454
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:CLK,4643
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:Q,4643
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_11:B,2783
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_11:UB,2783
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:CO,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[0],6006
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[1],5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[2],6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[3],6115
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[6],6127
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[7],6167
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[8],6237
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:P[9],6233
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[0],5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[10],6197
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[11],6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[1],5991
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[2],6137
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[3],6029
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[4],6062
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[5],6169
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[6],6068
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[7],6122
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[8],6212
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_0_CC_0:UB[9],6183
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[12]:A,6306
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[12]:B,6222
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[12]:C,5522
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[12]:Y,5522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17]:B,6473
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17]:C,6646
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17]:CC,5685
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17]:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17]:S,5685
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17]:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_73:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_73:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_73:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_73:IPA,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:CLK,7693
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:D,8867
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:Q,7693
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/mas_done_o_Z:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_52:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_52:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_52:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_52:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_52:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_16:B,4981
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_16:UB,4981
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:CLK,4315
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:D,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:EN,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:Q,4315
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_AH_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state_RNO[0]:A,7984
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state_RNO[0]:B,7906
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state_RNO[0]:C,6460
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state_RNO[0]:Y,6460
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[10],7021
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[11],6960
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[1],7531
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[2],7467
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[3],7195
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[4],7127
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[5],7077
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[6],7161
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[7],7069
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[8],7008
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CC[9],7105
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:CO,6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[0],6927
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[1],6883
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[2],7066
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[3],7042
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[6],7054
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[7],7103
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[8],7173
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:P[9],7160
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_s_20_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_11:B,6303
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_11:UB,6303
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:B,7895
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:C,6795
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:IPB,7895
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_25:IPC,6795
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[23]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[23]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[23]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:CLK,6935
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:D,8840
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:EN,8765
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:Q,6935
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_state[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9:A,6248
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9:B,6171
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9:C,3760
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9:D,4587
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_9:Y,3760
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:D,5963
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[11]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[11]:B,4753
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[11]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[11]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[11]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[40]:A,608
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[40]:B,465
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[40]:C,-9
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[40]:Y,-9
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[1]:A,4272
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[1]:B,4074
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[1]:C,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[1]:Y,4074
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:B,7856
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:C,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:IPB,7856
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_20:IPC,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[0]:A,5619
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[0]:B,2970
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[0]:C,3337
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[0]:D,3207
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[0]:Y,2970
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:CLK,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:D,5754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:Q,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[12]:A,6151
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[12]:B,6103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[12]:C,5399
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[12]:Y,5399
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:CLK,6731
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:D,8867
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:Q,6731
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/mas_done_o_Z:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o_1_sqmuxa_0_a2:A,5516
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o_1_sqmuxa_0_a2:B,5925
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o_1_sqmuxa_0_a2:C,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o_1_sqmuxa_0_a2:D,5000
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o_1_sqmuxa_0_a2:Y,3129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:C,6731
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:IPC,6731
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[9]:A,6085
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[9]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[9]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[9]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[9]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:C,6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPC,6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_19:IPD,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7:A,6159
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7:B,6111
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7:C,3691
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7:D,4533
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_7:Y,3691
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_27:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_27:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[13]:A,5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[13]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[13]:C,5606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[13]:Y,5118
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:CLK,5527
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:Q,5527
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc_1_sqmuxa_0_a2_0:A,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_acc_1_sqmuxa_0_a2_0:B,6533
BLDC_Encoder_Axis_0/MSC_i_11/s_acc_1_sqmuxa_0_a2_0:Y,-247
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:CLK,5516
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:Q,5516
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[6]:A,2725
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[6]:B,2595
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[6]:C,5918
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[6]:D,3582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[6]:Y,2595
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIVNET[16]:A,3771
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIVNET[16]:B,3473
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIVNET[16]:C,3655
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIVNET[16]:Y,3473
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:C,6810
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPC,6810
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_9:IPD,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[11]:A,2098
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[11]:B,4168
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[11]:C,3601
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2[11]:Y,2098
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[3]:A,2836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[3]:B,4105
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[3]:C,5944
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[3]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[3]:D,5790
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[3]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[3]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[3]:Y,2836
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:CLK,7852
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:Q,7852
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[10],871
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[11],734
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[1],581
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[2],1521
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[3],1323
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[4],1332
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[5],1070
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[6],1059
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[7],908
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[8],738
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CC[9],877
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:CO,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[0],-143
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[1],702
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[2],842
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[3],-257
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[6],-245
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[7],-207
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[8],-137
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:P[9],-139
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[0],600
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[10],-225
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[11],-119
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[1],694
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[2],840
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[3],-393
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[4],-360
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[5],-253
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[6],-354
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[7],-300
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[8],-210
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_0_0_CC_0:UB[9],-239
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_13:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_13:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:CLK,5113
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:D,6753
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:Q,5113
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[0]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[0]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[0]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[0]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_0:B,1363
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_0:C,988
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_0:CC,1448
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_0:P,988
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_0:S,1448
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_0:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_10:B,1293
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_10:UB,1293
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[16]:A,4235
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[16]:B,1839
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[16]:C,4110
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[16]:Y,1839
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:CLK,6804
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:Q,6804
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[17]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[1]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[1]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[1]:Y,7781
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[1]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17:B,6299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17:UB,6299
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:CLK,2059
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:D,1836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:Q,2059
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[9]:A,2819
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[9]:B,4088
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[9]:C,5907
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[9]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[9]:D,5773
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[9]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[9]:Y,2819
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:CLK,7094
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:D,6756
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:Q,7094
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[2]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[2]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[2]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_12:B,5218
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_12:CC,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_12:P,5218
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_12:S,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[0]:A,4098
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[0]:B,4007
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[0]:C,3811
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[0]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[0]:Y,3811
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:CLK,3153
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:Q,3153
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:CLK,7716
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:D,6664
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:Q,7716
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:CLK,2835
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:Q,2835
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_14:B,4221
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_14:UB,4221
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:C,6818
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_20:IPC,6818
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[3]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_10:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_10:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_10:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_10:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_10:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28_RNO:A,5803
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28_RNO:B,6039
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28_RNO:C,3898
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28_RNO:D,5583
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_28_RNO:Y,3898
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7:A,2922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7:B,2768
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7:CC,2639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7:P,2840
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7:S,2639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7:UB,2768
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[7]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[7]:B,4861
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[7]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[7]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[7]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:D,8699
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:CLK,2615
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:D,1984
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:Q,2615
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_244:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_244:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_244:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_244:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_244:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:CLK,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:Q,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_21:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_21:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux:A,4659
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux:B,4817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux:C,1995
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux:D,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux:Y,1775
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3:A,6130
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3:B,6053
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3:C,3642
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3:D,4469
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_3:Y,3642
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_7:A,4207
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_7:B,6078
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_7:P,4207
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_7:UB,6078
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:CLK,1312
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:D,8710
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:Q,1312
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_11:B,4633
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_11:C,4472
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_11:P,4472
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_11:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_11:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:D,8711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:CLK,7716
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:D,6732
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:Q,7716
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1]:B,5738
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1]:C,5982
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1]:CC,6154
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1]:P,5738
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1]:S,6154
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[18]:A,7160
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[18]:B,6578
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[18]:C,7039
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[18]:Y,6578
BLDC_Encoder_Axis_0/MSC_i_11/s_error_axb_0_i_0:A,7951
BLDC_Encoder_Axis_0/MSC_i_11/s_error_axb_0_i_0:B,7916
BLDC_Encoder_Axis_0/MSC_i_11/s_error_axb_0_i_0:Y,7916
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:CLK,4312
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:Q,4312
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_3:A,4377
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_3:B,4219
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_3:P,4305
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_3:UB,4219
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_9:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_9:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_9:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_9:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_9:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_9:IPD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:CLK,6855
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:EN,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:Q,6855
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_8:A,6324
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_8:B,4244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_8:P,4278
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_8:UB,4244
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_9:A,1953
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_9:B,1905
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_9:C,1831
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_9:D,1737
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_9:Y,1737
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_15:EN,8996
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_15:IPENn,8996
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHGAT8[6]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHGAT8[6]:B,7101
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHGAT8[6]:C,2802
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHGAT8[6]:CC,2950
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHGAT8[6]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHGAT8[6]:P,2802
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHGAT8[6]:S,2950
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIHGAT8[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]:A,2897
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]:B,3291
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]:C,5115
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]:D,4991
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[5]:Y,2897
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[27]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[27]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[27]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[27]:Y,6423
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_70:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_70:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_70:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_70:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:CC[0],6965
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:CC[1],6895
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:CC[2],6851
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:CC[3],6913
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:CC[4],6849
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:CC[5],6800
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:CI,6800
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[0],7083
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[1],7034
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[2],7160
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[3],7415
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[4],7543
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_9:A,5080
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_9:B,4944
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_9:P,4994
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_9:UB,4944
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIPM4K2[9]:A,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIPM4K2[9]:B,2373
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIPM4K2[9]:C,2484
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIPM4K2[9]:Y,2373
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:CLK,5824
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:D,7903
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:EN,7664
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:Q,5824
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[36]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[36]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[36]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:CLK,5995
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:D,8867
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:Q,5995
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_6:A,4520
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_6:B,4299
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_6:CC,4230
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_6:P,4401
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_6:S,4230
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_6:UB,4299
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[12]:A,6228
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[12]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[12]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[12]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[12]:Y,2538
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:CLK,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:Q,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_15:B,7036
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_15:CC,6920
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_15:P,7036
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_15:S,6920
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[15]:A,2307
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[15]:B,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[15]:C,3204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[15]:D,2919
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[15]:Y,2014
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[26]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[26]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[26]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7]:B,5845
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7]:C,6082
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7]:CC,5689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7]:P,5845
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7]:S,5689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o_1_sqmuxa_0_a2:A,5477
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o_1_sqmuxa_0_a2:B,5105
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o_1_sqmuxa_0_a2:C,5229
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o_1_sqmuxa_0_a2:D,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o_1_sqmuxa_0_a2:Y,2867
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[12]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_14:B,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_14:CC,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_14:S,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m33_2:A,4854
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m33_2:B,4537
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m33_2:C,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m33_2:Y,1816
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[2]:A,5708
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[2]:B,3059
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[2]:C,3426
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[2]:D,3296
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_1[2]:Y,3059
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_10_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_10_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_10_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_10_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_10_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[4]:A,5110
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[4]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[4]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[4]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[4]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[1]:A,4151
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[1]:C,4034
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2_i_m2[1]:Y,4034
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6:A,1566
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6:B,1400
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6:CC,1306
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6:P,1487
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6:S,1306
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6:UB,1400
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_14:A,7378
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_14:B,7203
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_14:C,6765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_14:CC,6566
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_14:P,6917
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_14:S,6566
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_cry_14:UB,6765
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[6]:A,3426
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[6]:B,5667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[6]:C,2326
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[6]:D,3124
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[6]:Y,2326
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux:A,3322
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux:B,3277
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux:C,3453
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux:CC,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux:D,3314
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m12_0_03_1_0_wmux:Y,3277
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_29_0:A,2682
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_29_0:B,1432
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_29_0:C,1505
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_29_0:CC,-102
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_29_0:D,218
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_29_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_29_0:S,-102
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_29_0:UB,218
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[7]:A,4326
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[7]:B,2003
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[7]:C,2014
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[7]:Y,2003
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_11:B,1828
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_11:C,1673
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_11:CC,1557
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_11:P,1673
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_11:S,1557
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_11:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:CLK,6844
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:Q,6844
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:CLK,7849
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:Q,7849
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_0_261_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_0_261_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_0_261_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_0_261_i_m2:Y,7698
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[10]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[10],5235
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[11],5174
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[1],5846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[2],5782
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[3],5469
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[4],5401
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[5],5340
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[6],5373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[7],5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[8],5222
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CC[9],5319
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:CO,5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[0],5242
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[1],5199
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[2],5365
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[3],5358
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[6],5370
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[7],5402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[8],5472
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:P[9],5476
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[0],5116
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[10],5408
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[11],5529
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[1],5217
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[2],5343
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[3],5255
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[4],5288
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[5],5392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[6],5283
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[7],5341
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[8],5438
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_0_0_CC_0:UB[9],5390
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[9]:A,5867
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[9]:B,6056
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[9]:C,2880
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[9]:D,2905
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[9]:Y,2880
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO_0:A,5567
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO_0:B,5473
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO_0:C,3616
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO_0:D,3536
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO_0:Y,3536
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_18:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_18:IPENn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:CLK,6068
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:D,8677
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:Q,6068
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__OVER_CURRENT_FAULT_DET_PROC_over_current_fault_o2_0_a3:A,7964
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__OVER_CURRENT_FAULT_DET_PROC_over_current_fault_o2_0_a3:B,7880
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__OVER_CURRENT_FAULT_DET_PROC_over_current_fault_o2_0_a3:C,4170
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__OVER_CURRENT_FAULT_DET_PROC_over_current_fault_o2_0_a3:D,4089
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__OVER_CURRENT_FAULT_DET_PROC_over_current_fault_o2_0_a3:Y,4089
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2:A,7073
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2:B,5292
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2:CC,6139
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2:P,5324
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2:S,6059
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2:UB,5292
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:CLK,6995
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:Q,6995
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11:B,3524
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11:CC,2783
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11:S,2783
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:CLK,2902
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:D,2805
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:Q,2902
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_10:B,6213
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_10:UB,6213
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:CLK,4739
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:Q,4739
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1:A,6929
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1:B,6883
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1:CC,7531
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1:P,6883
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1:S,7531
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_1:UB,6901
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:D,3165
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:CLK,7178
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:Q,7178
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:CLK,1542
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:Q,1542
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:B,7420
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:C,7716
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:CC,6800
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:S,6800
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:CLK,5127
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:Q,5127
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[14]:A,4948
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[14]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[14]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[14]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[14]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2_1:A,4203
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2_1:B,4102
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2_1:C,3851
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2_1:D,3843
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2_1:Y,3843
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:CLK,5047
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:D,6925
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:Q,5047
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:D,2897
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:D,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13:A,455
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13:B,-393
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13:C,494
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13:D,185
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_13:Y,-393
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIVF271[4]:A,2303
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIVF271[4]:B,2070
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIVF271[4]:C,2181
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIVF271[4]:Y,2070
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_6:A,6244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_6:B,4230
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_6:P,4293
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_6:UB,4230
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[16]:A,3566
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[16]:B,2544
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[16]:C,3587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[16]:D,3487
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[16]:Y,2544
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[17]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[17]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[17]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[2]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[2]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[2]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:CLK,4883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:Q,4883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:CLK,3745
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:D,7195
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:Q,3745
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6:B,1616
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6:CC,1613
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6:P,1616
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6:S,1613
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[43]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[43]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[43]:C,6757
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[43]:D,6621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[43]:Y,224
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_13:A,3828
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_13:B,6112
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_13:P,3828
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_13:UB,6112
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[30]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[30]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[30]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:CLK,2180
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:D,1945
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:Q,2180
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[12]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[12]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[12]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_high:A,6699
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_high:B,6802
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_high:Y,6699
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_7:A,6254
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_7:B,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_7:P,4268
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_7:UB,4214
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:CLK,2169
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:Q,2169
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:CLK,6810
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:Q,6810
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[7]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[7]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[7]:C,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[7]:Y,5204
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[17]:A,1308
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[17]:B,5022
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[17]:Y,1308
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:CLK,7716
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:Q,7716
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[33]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[5]:A,4656
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[5]:B,2120
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[5]:C,2076
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[5]:Y,2076
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:D,5174
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:CLK,4230
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:Q,4230
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:C,6814
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:IPC,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:CLK,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:Q,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]:A,2204
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]:B,1697
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]:C,3950
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]:D,3846
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[0]:Y,1697
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_6:A,6173
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_6:B,6068
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_6:P,6127
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_6:UB,6068
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISRKU[1]:A,6788
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISRKU[1]:B,6449
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISRKU[1]:C,6334
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISRKU[1]:Y,6334
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:CLK,6726
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:D,7074
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:Q,6726
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[31]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[31]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[31]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_1:B,4523
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_1:C,3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_1:CC,4130
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_1:P,3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_1:S,4130
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_1:UB,4523
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_11:B,4287
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_11:UB,4287
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[14]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_62:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_62:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_62:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_62:IPA,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_15:EN,8996
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_15:IPENn,8996
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:CLK,8004
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:D,5547
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:Q,8004
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[19]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[19]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[19]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218:B,4263
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218:C,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218:P,4263
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_s_0_218:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_30:A,541
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_30:B,353
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_30:C,344
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_30:D,235
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_30:Y,235
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[17]:A,5540
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[17]:B,2078
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[17]:C,2070
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[17]:Y,2070
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:CLK,7895
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:Q,7895
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_20:A,695
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_20:B,708
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_20:C,518
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_20:D,576
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_20:Y,518
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:CLK,4223
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:D,8686
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:Q,4223
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_20:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_20:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_5:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_5:B,7047
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_5:CC,6992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_5:S,6992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_5:UB,7047
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15:B,2487
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15:C,2299
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15:CC,1484
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15:S,1484
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:CLK,6059
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:Q,6059
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3JGM[8]:A,3372
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3JGM[8]:B,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3JGM[8]:C,3250
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI3JGM[8]:Y,3068
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17_FCINST1:CC,988
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17_FCINST1:CO,988
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHQ0J[16]:A,2773
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHQ0J[16]:B,2412
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHQ0J[16]:C,2756
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHQ0J[16]:Y,2412
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]:A,2970
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]:B,3364
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]:C,5188
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]:D,5064
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[0]:Y,2970
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0:A,7133
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0:B,6519
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0:C,1891
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0:CC,2037
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0:P,2013
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0:S,2037
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0:UB,1891
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m24_0_a2_0_a2_2:A,5249
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m24_0_a2_0_a2_2:B,5229
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m24_0_a2_0_a2_2:Y,5229
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:C,6724
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:IPC,6724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[35]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[35]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[35]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10:A,6847
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10:B,6770
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10:C,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10:D,5186
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_10:Y,4359
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[7]:A,3518
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[7]:B,4893
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[7]:C,2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[7]:D,3222
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[7]:Y,2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:CLK,4777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:Q,4777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[11]:A,5940
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[11]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[11]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[11]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[11]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:CLK,3246
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:D,8682
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:Q,3246
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[25]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_229:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_229:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_229:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_229:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_229:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_229:IPC,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:C,6718
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:IPC,6718
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[4]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[4]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[4]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[4]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/MAS_PI_INST_mas_done_o_RNI605I:A,7519
BLDC_Encoder_Axis_0/MSC_i_11/MAS_PI_INST_mas_done_o_RNI605I:B,7540
BLDC_Encoder_Axis_0/MSC_i_11/MAS_PI_INST_mas_done_o_RNI605I:Y,7519
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[0]:A,7977
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[0]:B,7867
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[0]:C,6791
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[0]:D,5650
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[0]:Y,5650
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:CLK,4101
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:Q,4101
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:CLK,1559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:D,8676
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:Q,1559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:CLK,5804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:Q,5804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_14:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_14:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO_0:A,5562
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO_0:B,5485
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO_0:C,3614
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO_0:D,3527
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_13_RNO_0:Y,3527
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_4:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:B,7864
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:C,6859
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:D,7827
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPB,7864
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPC,6859
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPD,7827
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[13]:A,6066
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[13]:B,5995
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[13]:C,4493
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[13]:D,5483
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[13]:Y,4493
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:CLK,3387
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:D,8699
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:Q,3387
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[5]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[8]:A,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[8]:B,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[8]:C,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[8]:Y,7659
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CAN_RXBUS_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CAN_RXBUS_USBA_DATA1_MGPIO3A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CAN_TXBUS_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CAN_TXBUS_USBA_DATA0_MGPIO2A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CAN_TX_EBL_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CAN_TX_EBL_USBA_DATA2_MGPIO4A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CLK_BASE,1445
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CLK_MDDR_APB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:COLF,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:CRSF,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DM_IN[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DM_IN[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DM_IN[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQS_IN[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQS_IN[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQS_IN[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[16],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[17],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_DQ_IN[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_FIFO_WE_IN[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:DRAM_FIFO_WE_IN[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2HCALIB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2H_INTERRUPT[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2_DMAREADY[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F2_DMAREADY[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_AVALID,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_HOSTDISCON,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_IDDIG,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_LINESTATE[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_LINESTATE[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_M3_RESET_N,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_PLL_LOCK,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_RXACTIVE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_RXERROR,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_RXVALID,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_RXVALIDH,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_SESSEND,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_TXREADY,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VBUSVALID,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VSTATUS[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VSTATUS[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VSTATUS[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VSTATUS[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VSTATUS[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VSTATUS[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VSTATUS[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_VSTATUS[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_XDATAIN[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_XDATAIN[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_XDATAIN[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_XDATAIN[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_XDATAIN[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_XDATAIN[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_XDATAIN[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FAB_XDATAIN[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:FPGA_MDDR_ARESET_N,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[16],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[17],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[18],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[19],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[20],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[21],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[22],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[23],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[24],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[25],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[26],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[27],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[28],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[29],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[30],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[31],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARADDR_HADDR1[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARBURST_HTRANS1[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARBURST_HTRANS1[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARID_HSEL1[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARID_HSEL1[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARID_HSEL1[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARID_HSEL1[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARLEN_HBURST1[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARLEN_HBURST1[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARLEN_HBURST1[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARLEN_HBURST1[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARLOCK_HMASTLOCK1[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARLOCK_HMASTLOCK1[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARSIZE_HSIZE1[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARSIZE_HSIZE1[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_ARVALID_HWRITE1,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[16],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[17],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[18],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[19],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[20],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[21],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[22],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[23],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[24],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[25],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[26],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[27],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[28],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[29],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[30],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[31],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWADDR_HADDR0[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWBURST_HTRANS0[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWBURST_HTRANS0[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWID_HSEL0[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWID_HSEL0[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWID_HSEL0[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWID_HSEL0[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWLEN_HBURST0[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWLEN_HBURST0[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWLEN_HBURST0[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWLEN_HBURST0[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWLOCK_HMASTLOCK0[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWLOCK_HMASTLOCK0[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWSIZE_HSIZE0[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWSIZE_HSIZE0[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_AWVALID_HWRITE0,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_BREADY,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_DMAREADY[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_DMAREADY[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[16],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[17],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[18],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[19],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[20],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[21],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[22],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[23],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[24],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[25],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[26],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[27],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[28],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[29],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[30],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[31],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ADDR[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_ENABLE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_MASTLOCK,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_READY,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_SEL,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_SIZE[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_SIZE[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_TRANS1,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[16],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[17],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[18],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[19],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[20],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[21],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[22],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[23],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[24],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[25],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[26],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[27],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[28],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[29],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[30],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[31],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WDATA[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_FM0_WRITE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[0],2411
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[10],2105
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[11],2815
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[12],4046
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[13],3090
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[14],3129
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[15],4210
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[1],2333
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[2],1445
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[3],2070
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[4],2059
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[5],1905
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[6],2368
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[7],2368
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[8],3194
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ADDR[9],1898
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_ENABLE,4165
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[0],1579
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[10],1760
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[11],1696
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[12],1830
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[13],2468
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[14],1836
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[15],1843
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[16],1795
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[17],2525
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[18],2501
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[19],2452
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[1],4034
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[20],2441
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[21],2421
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[22],2416
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[23],2368
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[24],2442
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[25],2469
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[26],2506
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[27],2458
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[28],2452
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[29],2389
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[2],1668
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[30],2393
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[31],2480
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[3],1445
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[4],1585
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[5],1718
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[6],1697
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[7],1809
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[8],1712
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RDATA[9],1606
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_READY,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_RESP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_SEL,4345
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[0],7215
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[10],7390
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[11],7194
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[12],7198
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[13],7180
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[14],7250
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[15],7165
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[16],7296
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[17],7105
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[1],7156
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[2],7145
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[3],7110
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[4],7317
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[5],7241
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[6],7273
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[7],7050
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[8],7329
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WDATA[9],7247
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_HM0_WRITE,3987
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_RMW_AXI,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_RREADY,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[16],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[17],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[18],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[19],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[20],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[21],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[22],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[23],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[24],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[25],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[26],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[27],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[28],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[29],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[30],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[31],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[32],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[33],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[34],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[35],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[36],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[37],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[38],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[39],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[40],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[41],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[42],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[43],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[44],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[45],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[46],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[47],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[48],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[49],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[50],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[51],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[52],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[53],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[54],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[55],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[56],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[57],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[58],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[59],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[60],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[61],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[62],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[63],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WDATA_HWDATA01[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WID_HREADY01[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WID_HREADY01[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WID_HREADY01[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WID_HREADY01[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WLAST,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WSTRB[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WSTRB[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WSTRB[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WSTRB[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WSTRB[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WSTRB[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WSTRB[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WSTRB[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:F_WVALID,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:GTX_CLKPF,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C0_BCLK,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C0_SCL_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C0_SCL_USBC_DATA1_MGPIO31B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C0_SDA_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C0_SDA_USBC_DATA0_MGPIO30B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C1_BCLK,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C1_SCL_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C1_SCL_USBA_DATA4_MGPIO1A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C1_SDA_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C1_SDA_MGPIO0A_H2F_B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:I2C1_SDA_USBA_DATA3_MGPIO0A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PADDR[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PENABLE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PSEL,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWDATA[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDDR_FABRIC_PWRITE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MDIF,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO0A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO10A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO11A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO11B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO12A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO13A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO14A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO15A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO16A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO17B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO18B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO19B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO1A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO20B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO21B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO22B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO24B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO25B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO26B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO27B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO28B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO29B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO2A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO30B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO31B_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO3A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO4A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO5A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO6A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO7A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO8A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MGPIO9A_F2H_GPIN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_CTS_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_CTS_USBC_DATA7_MGPIO19B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_DCD_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_DCD_MGPIO22B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_DSR_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_DSR_MGPIO20B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_DTR_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_DTR_USBC_DATA6_MGPIO18B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_RI_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_RI_MGPIO21B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_RTS_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_RTS_USBC_DATA5_MGPIO17B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_RXD_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_RXD_USBC_STP_MGPIO28B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_SCK_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_SCK_USBC_NXT_MGPIO29B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_TXD_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART0_TXD_USBC_DIR_MGPIO27B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_CTS_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_DCD_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_DSR_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_RI_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_RTS_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_RXD_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_RXD_USBC_DATA3_MGPIO26B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_SCK_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_SCK_USBC_DATA4_MGPIO25B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_TXD_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:MMUART1_TXD_USBC_DATA2_MGPIO24B_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[10],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[11],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[12],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[13],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[14],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[15],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[16],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[17],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[18],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[19],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[20],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[21],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[22],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[23],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[24],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[25],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[26],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[27],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[28],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[29],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[30],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[31],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PRDATA[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PREADY,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PER2_FABRIC_PSLVERR,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:PRESET_N,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[8],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RCGF[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_GTX_CLK_RMII_CLK_USBB_XCLK_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_MDC_RMII_MDC_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_MDIO_RMII_MDIO_USBB_DATA7_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_MDIO_RMII_MDIO_USBB_DATA7_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_MDIO_RMII_MDIO_USBB_DATA7_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD0_RMII_RXD0_USBB_DATA0_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD0_RMII_RXD0_USBB_DATA0_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD0_RMII_RXD0_USBB_DATA0_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD1_RMII_RXD1_USBB_DATA1_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD1_RMII_RXD1_USBB_DATA1_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD1_RMII_RXD1_USBB_DATA1_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD2_RMII_RX_ER_USBB_DATA3_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD2_RMII_RX_ER_USBB_DATA3_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD2_RMII_RX_ER_USBB_DATA3_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD3_USBB_DATA4_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD3_USBB_DATA4_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RXD3_USBB_DATA4_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RX_CLK_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RX_CTL_RMII_CRS_DV_USBB_DATA2_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RX_CTL_RMII_CRS_DV_USBB_DATA2_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_RX_CTL_RMII_CRS_DV_USBB_DATA2_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD0_RMII_TXD0_USBB_DIR_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD1_RMII_TXD1_USBB_STP_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD1_RMII_TXD1_USBB_STP_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD1_RMII_TXD1_USBB_STP_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD2_USBB_DATA5_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD2_USBB_DATA5_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD2_USBB_DATA5_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD3_USBB_DATA6_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD3_USBB_DATA6_OE,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TXD3_USBB_DATA6_OUT,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TX_CLK_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RGMII_TX_CTL_RMII_TX_EN_USBB_NXT_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RXDF[0],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RXDF[1],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RXDF[2],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RXDF[3],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RXDF[4],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RXDF[5],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RXDF[6],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RXDF[7],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RX_CLKPF,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RX_DVF,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RX_ERRF,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:RX_EV,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SLEEPHOLDREQ,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SMBALERT_NI0,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SMBALERT_NI1,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SMBSUS_NI0,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SMBSUS_NI1,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_CLK_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SCK_USBA_XCLK_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SDI_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SDI_USBA_DIR_MGPIO5A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SDO_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SDO_USBA_STP_MGPIO6A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SS0_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SS0_USBA_NXT_MGPIO7A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SS1_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SS1_USBA_DATA5_MGPIO8A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SS2_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SS2_USBA_DATA6_MGPIO9A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SS3_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI0_SS3_USBA_DATA7_MGPIO10A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_CLK_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SCK_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SDI_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SDI_MGPIO11A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SDO_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SDO_MGPIO12A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS0_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS0_MGPIO13A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS1_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS1_MGPIO14A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS2_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS2_MGPIO15A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS3_F2H_SCP,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS3_MGPIO16A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS4_MGPIO17A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS5_MGPIO18A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS6_MGPIO23A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:SPI1_SS7_MGPIO24A_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:TX_CLKPF,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:USBC_XCLK_IN,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:USER_MSS_GPIO_RESET_N,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:USER_MSS_RESET_N,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP:XCLK_FAB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[0]:A,7737
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[0]:B,6262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[0]:C,7862
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[0]:Y,6262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[15]:A,5999
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[15]:B,2718
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[15]:C,2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[15]:D,2276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[15]:Y,2276
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_10:B,2862
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_10:UB,2862
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_273:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_273:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_273:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_273:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_273:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:CLK,6303
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:D,8673
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:Q,6303
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[28]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[28]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[28]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[28]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[1],4893
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[2],4780
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[3],4468
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[4],4619
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[5],4504
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[6],4644
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[7],4500
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:CO,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[0],4422
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[1],4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[2],4508
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[3],4537
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[6],4549
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[7],4545
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[8],4615
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:P[9],4655
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_0_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[15]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[15]:B,4809
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[15]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[15]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[15]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4:A,7808
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4:B,6982
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4:CC,7084
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4:S,7084
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_4:UB,6982
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[6]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[6]:B,4599
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[6]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[6]:Y,91
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:CLK,5144
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:D,4737
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:Q,5144
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:CLK,6802
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:Q,6802
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[5]:A,6005
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[5]:B,6066
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[5]:C,7809
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[5]:D,6815
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[5]:Y,6005
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[9]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[9]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[9]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[9]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:D,5283
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:CLK,1947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:D,8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:Q,1947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:CLK,4866
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:Q,4866
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[35]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[35]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[35]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_5:B,5111
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_5:UB,5111
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:CC[0],7022
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:CC[1],6944
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:CC[2],6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:CI,6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[0],7473
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[15]:A,1887
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[15]:B,3957
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[15]:C,3390
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[15]:Y,1887
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[13]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[13]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[13]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[13]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIB9T9[4]:A,2814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIB9T9[4]:B,2737
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIB9T9[4]:C,2303
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIB9T9[4]:Y,2303
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[4]:A,1987
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[4]:B,4057
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[4]:C,3490
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[4]:Y,1987
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_13:A,1445
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_13:B,1249
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_13:P,1249
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_13:UB,1258
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[6]:A,2876
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[6]:B,4145
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[6]:C,5984
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[6]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[6]:D,5830
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[6]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[6]:Y,2876
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:CLK,5872
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:Q,5872
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:D,5501
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[10],6756
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[11],6695
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[1],7313
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[2],7252
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[3],6980
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[4],6912
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[5],6862
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[6],6896
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[7],6804
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[8],6743
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CC[9],6840
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:CO,6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[0],6712
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[1],6618
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[2],6792
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[3],6777
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[6],6789
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[7],6829
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[8],6899
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:P[9],6895
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[12]:A,3672
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[12]:B,2626
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[12]:C,3711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[12]:D,3604
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[12]:Y,2626
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:CLK,7871
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:Q,7871
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[38]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:CLK,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:D,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:Q,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[12]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[12]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[12]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[7]:A,1346
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[7]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[7]:Y,1346
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:CLK,988
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:D,1343
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:Q,988
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:CLK,7837
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:Q,7837
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIKPV84[2]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIKPV84[2]:B,3833
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIKPV84[2]:C,6997
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIKPV84[2]:CC,5068
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIKPV84[2]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIKPV84[2]:P,3833
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIKPV84[2]:S,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIKPV84[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_9:A,5771
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_9:B,5728
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_9:C,5646
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_9:D,5543
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un9_en_pwm_i_9:Y,5543
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:CLK,5829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:Q,5829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_4:B,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_4:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[4]:A,1571
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[4]:B,5288
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[4]:Y,1571
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:CO,4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[0],4196
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[1],4146
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[2],4320
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[3],4305
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[6],4317
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[7],4357
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[8],4427
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:P[9],4423
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[0],4087
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[10],4387
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[11],4493
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[1],4181
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[2],4327
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[3],4219
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[4],4252
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[5],4359
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[6],4258
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[7],4312
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[8],4402
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_0_CC_0:UB[9],4373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/PI_SEL_PROC_un1_id_pi_start_i:A,7997
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/PI_SEL_PROC_un1_id_pi_start_i:B,7873
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/PI_SEL_PROC_un1_id_pi_start_i:C,7876
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/PI_SEL_PROC_un1_id_pi_start_i:Y,7873
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0A9EA[29]:A,1816
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0A9EA[29]:B,1609
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0A9EA[29]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0A9EA[29]:CC,1740
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0A9EA[29]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0A9EA[29]:P,1774
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0A9EA[29]:S,1740
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI0A9EA[29]:UB,1609
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_2:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[1]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_92:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_92:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_92:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_92:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_92:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:CLK,7827
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:Q,7827
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_dir1_tmp5_0_0:A,6082
BLDC_Encoder_Axis_0/MSC_i_23/s_dir1_tmp5_0_0:B,6014
BLDC_Encoder_Axis_0/MSC_i_23/s_dir1_tmp5_0_0:C,5953
BLDC_Encoder_Axis_0/MSC_i_23/s_dir1_tmp5_0_0:D,5835
BLDC_Encoder_Axis_0/MSC_i_23/s_dir1_tmp5_0_0:Y,5835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_24:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_24:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[9]:A,3808
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[9]:B,3776
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[9]:C,2785
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[9]:D,2711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[9]:Y,2711
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:CLK,6446
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:Q,6446
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]:A,2499
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]:B,1982
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]:C,4258
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]:D,4125
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[9]:Y,1982
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:CLK,1576
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:Q,1576
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[1]:A,4323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[1]:B,6667
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[1]:C,3351
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[1]:D,4073
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[1]:Y,3351
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_11:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_11:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_11:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_11:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_11:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNINTN43[12]:A,2617
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNINTN43[12]:B,2384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNINTN43[12]:C,2495
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNINTN43[12]:Y,2384
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_11:A,5990
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_11:B,5308
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_11:CC,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_11:S,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_11:UB,5308
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:CLK,3497
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:Q,3497
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_12:A,4902
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_12:B,2777
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_12:P,2927
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_12:UB,2777
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_2:A,6146
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_2:B,6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_2:P,6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_2:UB,6137
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:CLK,3831
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:D,6742
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:Q,3831
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICQMAI[43]:A,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICQMAI[43]:B,3397
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICQMAI[43]:C,3367
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICQMAI[43]:CC,2205
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICQMAI[43]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICQMAI[43]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICQMAI[43]:S,2205
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICQMAI[43]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_7:A,4519
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_7:B,4353
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_7:CC,4214
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_7:P,4430
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_7:S,4214
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_7:UB,4353
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:CLK,3823
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:D,5753
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:Q,3823
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:CLK,4273
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:Q,4273
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_17:A,1332
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_17:B,1323
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_17:C,1521
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_17:D,1070
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_17:Y,1070
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_28:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_28:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_7:A,3946
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_7:B,6078
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_7:P,3946
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_7:UB,6078
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_iv_0[1]:A,5476
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_iv_0[1]:B,4413
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_iv_0[1]:C,5752
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_iv_0[1]:Y,4413
BLDC_Encoder_Axis_0/MSC_i_13/state_o_10_i_a3_0_a2[1]:A,136
BLDC_Encoder_Axis_0/MSC_i_13/state_o_10_i_a3_0_a2[1]:B,88
BLDC_Encoder_Axis_0/MSC_i_13/state_o_10_i_a3_0_a2[1]:Y,88
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[17]:A,3231
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[17]:B,3203
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[17]:C,2215
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[17]:D,2078
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[17]:Y,2078
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIT2R3L[2]:A,6991
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIT2R3L[2]:B,1591
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIT2R3L[2]:C,1665
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIT2R3L[2]:CC,1291
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIT2R3L[2]:D,6163
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIT2R3L[2]:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIT2R3L[2]:S,1291
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIT2R3L[2]:UB,1591
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO_0:A,5725
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO_0:B,5677
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO_0:C,3797
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO_0:D,3740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_22_RNO_0:Y,3740
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_175:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_175:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_175:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_175:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_175:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[10],6027
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[11],5966
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[1],6584
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[2],6523
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[3],6251
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[4],6183
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[5],6133
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[6],6167
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[7],6075
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[8],6014
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CC[9],6111
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:CO,5889
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[0],5983
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[1],5889
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[2],6063
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[3],6048
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[6],6060
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[7],6100
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[8],6170
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:P[9],6166
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:CLK,6754
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:Q,6754
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:CLK,224
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:D,8681
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:Q,224
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:CLK,5401
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:Q,5401
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0_RNO:A,3432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0_RNO:B,6288
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0_RNO:C,5986
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0_RNO:D,4214
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_14_0_RNO:Y,3432
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[5]:A,3829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[5]:B,6066
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[5]:C,2648
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[5]:D,3527
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[5]:Y,2648
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26_RNO:A,5847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26_RNO:B,6083
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26_RNO:C,3940
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26_RNO:D,5627
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_26_RNO:Y,3940
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:CLK,1826
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:Q,1826
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_4:IPENn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:CLK,5054
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:Q,5054
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[10],2862
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[11],2922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[1],3017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[2],3093
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[3],2802
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[4],2916
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[5],2947
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[6],2722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[7],2639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[8],2661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CC[9],2766
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:CO,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[0],2666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[1],2629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[2],2803
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[3],2788
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[6],2800
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[7],2840
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[8],2910
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:P[9],2906
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[0],2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[10],2835
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[11],2956
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[1],2646
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[2],2770
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[3],2689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[4],2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[5],2819
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[6],2710
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[7],2768
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[8],2876
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0_CC_0:UB[9],2817
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:EN,7740
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data_reg[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[29]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[29]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[29]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[29]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:D,4495
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[8]:A,4454
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[8]:B,4370
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[8]:C,4186
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[8]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[8]:Y,4186
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:CLK,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:D,6138
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:Q,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdi:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:CLK,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:Q,6986
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_ki_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:CLK,7167
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:D,7329
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:Q,7167
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:CLK,7169
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:Q,7169
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[9]:A,5128
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[9]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[9]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[9]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[9]:Y,2639
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:CLK,6208
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:Q,6208
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_8:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns_a4_0[0]:A,6898
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns_a4_0[0]:B,6817
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns_a4_0[0]:Y,6817
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIFF662[16]:A,4471
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIFF662[16]:B,3473
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIFF662[16]:C,3428
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIFF662[16]:Y,3428
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[25]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[25]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[25]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[25]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:CLK,1220
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:D,1356
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:Q,1220
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[4]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[9]:A,7964
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[9]:B,7893
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi_RNO[9]:Y,7893
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_28:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_28:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_28:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_28:CC,6664
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_28:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_28:P,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_28:S,6664
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_28:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_34:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_34:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:B,7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:C,6762
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:IPB,7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_34:IPC,6762
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIM4D33[1]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIM4D33[1]:B,7064
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIM4D33[1]:C,2765
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIM4D33[1]:CC,4304
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIM4D33[1]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIM4D33[1]:P,2765
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIM4D33[1]:S,3501
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIM4D33[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_3:A,5360
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_3:B,5141
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_3:CC,5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_3:P,5239
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_3:S,5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_3:UB,5141
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[14]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[14]:B,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_TRANSMIT_PROC_s_sdo_reg_6[14]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:CLK,7863
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:Q,7863
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_17_0:A,2199
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_17_0:B,1140
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_17_0:C,1213
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_17_0:CC,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_17_0:D,-28
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_17_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_17_0:S,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_17_0:UB,-28
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:CC[0],4188
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:CI,4188
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un8_sensor_reset_i_cry_11_RNI8ETU_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_4:B,4594
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_4:C,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_4:CC,3726
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_4:S,3726
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_4:UB,4594
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]:A,2764
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]:B,3158
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]:C,4982
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]:D,4858
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[4]:Y,2764
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[15]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_248:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_248:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_248:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_248:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_248:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_158:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_158:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_158:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_158:IPA,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1_RNO:A,4958
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1_RNO:B,3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1_RNO:C,4836
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1_RNO:Y,3483
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:B,7718
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:C,6771
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:IPB,7718
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_13:IPC,6771
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:D,2972
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO_0:A,4955
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO_0:B,2012
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO_0:C,1921
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_5_0_RNO_0:Y,1921
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_6:A,6244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_6:B,4230
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_6:P,4293
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_6:UB,4230
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[1]:A,2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[1]:B,5955
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[1]:Y,2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_9:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_9:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_9:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_9:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[16]:A,1967
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[16]:B,4068
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[16]:C,1795
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[16]:Y,1795
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_20:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_20:B,7167
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_20:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_20:CC,6740
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_20:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_20:P,7167
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_20:S,6740
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_20:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:CLK,7919
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:Q,7919
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[26]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:CLK,6129
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:Q,6129
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[15]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[15]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[15]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[15]:Y,6726
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[0]:A,4277
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[0]:B,1741
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[0]:C,1697
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[0]:Y,1697
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_8:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_8:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_8:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_8:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_8:IPB,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_8:IPC,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:CLK,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:Q,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[9]:A,5468
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[9]:B,2819
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[9]:C,3173
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[9]:D,3056
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[9]:Y,2819
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:B,7919
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:C,6844
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:D,7884
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPB,7919
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPC,6844
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_23:IPD,7884
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17_FCINST1:CC,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17_FCINST1:CO,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:CLK,5142
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:Q,5142
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o[13]:SLn,
A0_ADC_SCK_O_obuf/U0/U_IOPAD:D,4288
A0_ADC_SCK_O_obuf/U0/U_IOPAD:E,
A0_ADC_SCK_O_obuf/U0/U_IOPAD:PAD,4288
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:CLK,1432
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:D,6584
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:Q,1432
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_op_eq_un5_clear_buffer_i:A,7904
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_op_eq_un5_clear_buffer_i:B,7861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_op_eq_un5_clear_buffer_i:Y,7861
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGPGT9[28]:A,1728
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGPGT9[28]:B,1553
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGPGT9[28]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGPGT9[28]:CC,1779
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGPGT9[28]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGPGT9[28]:P,1656
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGPGT9[28]:S,1779
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIGPGT9[28]:UB,1553
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:CLK,7222
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:D,7015
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:Q,7222
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_11:A,463
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_11:B,308
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_11:C,205
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_11:D,217
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_11:Y,205
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[8]:A,5904
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[8]:B,5820
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[8]:C,5364
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[8]:D,4273
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[8]:Y,4273
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count:A,1963
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count:B,1920
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count:C,2006
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count:D,1737
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count:Y,1737
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:CLK,6817
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:D,8840
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:EN,8669
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:Q,6817
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_done:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:D,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:CLK,4482
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:Q,4482
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_13:B,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_13:CC,5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_13:S,5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[4]:A,6133
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[4]:B,6864
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref_4[4]:Y,6133
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:CLK,4974
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:Q,4974
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[9]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:CLK,7671
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:Q,7671
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_29:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_29:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[5]:A,3374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[5]:B,5615
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[5]:C,2267
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[5]:D,3072
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[5]:Y,2267
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_1:A,6002
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_1:B,5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_1:P,5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_1:UB,5991
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_12:B,6167
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_12:C,6275
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_12:CC,5989
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_12:P,6167
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_12:S,5989
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[12]:A,7258
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[12]:B,5216
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[12]:C,5035
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[12]:CC,4650
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[12]:D,6811
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[12]:P,5118
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[12]:S,4650
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[12]:UB,5035
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:C,6810
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPC,6810
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_9:IPD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:CLK,1539
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:Q,1539
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[28]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[28]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[28]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[20]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:CLK,6804
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:Q,6804
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:CLK,407
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:D,8677
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:Q,407
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_18:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_18:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_am[12]:A,4323
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_am[12]:B,1997
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_am[12]:C,2020
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_am[12]:Y,1997
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_2:B,1527
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_2:C,1372
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_2:CC,1574
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_2:P,1372
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_2:S,1574
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO:A,2076
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO:B,5652
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO:C,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO:D,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_11_0_RNO:Y,1816
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[5]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[5]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[5]:C,5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[5]:Y,5224
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO:A,5436
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO:B,5388
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO:C,3544
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO:D,3471
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_3_RNO:Y,3471
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:CLK,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:Q,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_4:A,7835
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_4:B,6768
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_4:CC,7066
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_4:S,7066
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_4:UB,6768
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_3_0:A,2208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_3_0:B,6920
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_3_0:C,6470
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_3_0:CC,2311
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_3_0:D,4304
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_3_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_3_0:S,2208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_3_0:UB,4304
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_8:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:C,6847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPC,6847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_5:IPD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:CLK,6757
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:D,7916
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:Q,6757
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:CLK,6424
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:D,5683
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:Q,6424
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:CLK,6771
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:Q,6771
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[7]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_241:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_241:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_241:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_241:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_241:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_241:IPC,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[0],6920
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[1],6842
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[2],6784
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[3],6874
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[4],6803
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[5],6742
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[6],6862
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[7],6740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[8],6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CC[9],6776
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:CI,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[0],7058
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[1],7008
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[2],7181
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[3],7166
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[6],7230
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[7],7595
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[0],6911
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[1],7005
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[2],7130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[3],7048
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[4],7086
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[5],7178
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[6],7130
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[7],7225
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[8],7299
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_0_CC_2:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:CLK,1649
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:Q,1649
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9:A,7206
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9:B,7072
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9:CC,7002
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9:P,7160
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9:S,7002
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_9:UB,7072
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_84:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_84:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_84:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_84:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_84:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_233:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_233:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_233:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_233:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_233:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_1[1]:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_1[1]:B,5212
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_1[1]:C,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_a2_2_1[1]:Y,5212
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:CLK,6724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:D,5782
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:Q,6724
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:CC[0],5742
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:CC[1],5664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:CC[2],5606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:CC[3],5696
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:CC[4],5625
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:CC[5],5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:CC[6],5685
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:CI,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[0],5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[1],5842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[3],6013
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[22]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:CLK,7926
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:Q,7926
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:CLK,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:D,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:Q,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10:B,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10:S,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3:B,1604
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3:CC,1634
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3:P,1604
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3:S,1634
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_3:B,2169
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_3:C,1981
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_3:CC,1398
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_3:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_3:S,1398
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:CLK,6197
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:D,8674
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:Q,6197
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Va_o_Z[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:CLK,3166
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:D,2143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:Q,3166
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIQPSS4[3]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIQPSS4[3]:B,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIQPSS4[3]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIQPSS4[3]:CC,5273
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIQPSS4[3]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIQPSS4[3]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIQPSS4[3]:S,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNIQPSS4[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[6]:A,6926
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[6]:B,7916
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[6]:C,2465
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[6]:D,3564
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0[6]:Y,2465
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:CLK,7023
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:Q,7023
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_17:A,7531
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_17:B,7699
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_17:C,5754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_17:D,6291
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_17:Y,5754
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]:A,1919
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]:B,2429
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]:C,4117
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]:D,4000
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[8]:Y,1919
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:CLK,7088
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:Q,7088
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[9]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_7_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_7_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_7_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_7_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:CLK,5205
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:D,3674
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:Q,5205
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:CLK,6169
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:D,8676
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:Q,6169
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]:A,2350
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]:B,1843
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]:C,4103
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]:D,3985
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[15]:Y,1843
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[1]:A,5931
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[1]:B,5860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[1]:C,4358
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[1]:D,5355
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[1]:Y,4358
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:D,8663
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[17]:A,3977
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[17]:B,3914
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[17]:C,4430
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[17]:D,3385
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_0[17]:Y,3385
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[14]:A,1355
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[14]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[14]:Y,1355
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[1]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[1]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[1]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:D,8854
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/s_mas_done_dly[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:C,6807
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPC,6807
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_7:IPD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:CLK,6005
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:Q,6005
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[6]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[6]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[6]:Y,5764
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[11]:A,4494
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[11]:B,2098
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[11]:C,4369
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[11]:Y,2098
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]:C,4273
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]:D,4151
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[1]:Y,4151
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2:A,5161
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2:B,5434
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2:C,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2:D,5110
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2:Y,2990
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_15:A,6420
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_15:B,4208
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_15:P,4332
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_15:UB,4208
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[0]:A,6820
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[0]:B,6777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[0]:C,3031
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[0]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[0]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_s_33:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_s_33:B,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_s_33:C,7723
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_s_33:CC,6776
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_s_33:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_s_33:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_s_33:S,6776
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_s_33:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[14]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[14]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[14]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[14]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_12:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_12:B,2177
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_12:C,1989
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_12:CC,1213
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_12:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_12:S,1213
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_12:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_119:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_119:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_119:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_119:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[8]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[8]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[8]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[3]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[3]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[3]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIN6GM[2]:A,3873
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIN6GM[2]:B,3552
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIN6GM[2]:C,3745
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIN6GM[2]:Y,3552
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[2]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[2]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[2]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_8:B,4744
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_8:C,3761
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_8:CC,3608
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_8:P,3761
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_8:S,3608
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_8:UB,4744
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[3]:A,2058
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[3]:B,6956
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[3]:C,988
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[3]:D,1898
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_1[3]:Y,988
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:CLK,1994
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:D,2029
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:Q,1994
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[12]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[12]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[12]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[12]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14:B,2426
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14:C,2238
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14:CC,1494
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14:S,1494
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14:UB,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[6]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[6]:B,6963
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[6]:C,7061
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[6]:CC,6982
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[6]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[6]:P,6963
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[6]:S,6982
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:CLK,1327
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:D,1499
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:Q,1327
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_12:A,3779
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_12:B,3731
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_12:C,3657
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_12:D,3562
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_12:Y,3562
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en_RNO:A,6834
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en_RNO:B,7402
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en_RNO:Y,6834
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_10:B,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_10:CC,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_10:S,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:C,6841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPC,6841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_3:IPD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[23]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[0]:A,1684
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[0]:B,3054
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[0]:C,4798
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[0]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[0]:D,4644
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[0]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[0]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[0]:Y,1684
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_STP_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_STP_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_STP_PAD/U_IOPAD:PAD,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNITB0PB[9]:A,6389
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNITB0PB[9]:B,1413
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNITB0PB[9]:C,1483
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNITB0PB[9]:CC,1443
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNITB0PB[9]:D,5997
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNITB0PB[9]:P,1518
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNITB0PB[9]:S,1443
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNITB0PB[9]:UB,1413
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_2_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_2_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_2_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_2_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:CLK,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:Q,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_6:B,4536
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_6:C,4347
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_6:CC,4341
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_6:P,4347
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_6:S,4341
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_6:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:CLK,7689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:Q,7689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIGOK31[2]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIGOK31[2]:B,7084
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIGOK31[2]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIGOK31[2]:CC,7112
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIGOK31[2]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIGOK31[2]:P,7084
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIGOK31[2]:S,7112
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIGOK31[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:CLK,3370
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:D,8664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:Q,3370
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17_FCINST1:CC,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17_FCINST1:CO,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:C,6738
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:IPB,7933
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_22:IPC,6738
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO:A,5564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO:B,5516
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO:C,3659
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO:D,3586
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_9_RNO:Y,3586
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[33]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_135:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_135:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_135:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_135:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_135:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:C,6697
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_6:IPC,6697
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_1:A,1307
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_1:B,1354
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_1:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_1:D,705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_1:Y,88
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10:B,3403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10:CC,2710
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10:S,2710
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:CLK,3961
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:Q,3961
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[31]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[0]:A,6987
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[0]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[0]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[0]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[0]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:D,8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:CLK,3915
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:Q,3915
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:D,8513
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:Q,7920
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_0/done_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[12]:A,2800
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[12]:B,5168
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[12]:Y,2800
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0:A,6942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0:B,6442
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0:C,2108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0:CC,7061
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0:D,4233
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0:P,2108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0:S,3017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0:UB,2128
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_14:B,5047
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_14:UB,5047
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:CLK,6757
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:D,5207
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:Q,6757
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIPGLA1_0[0]:A,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIPGLA1_0[0]:B,7184
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state_RNIPGLA1_0[0]:Y,5695
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2_i:A,7844
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2_i:B,7801
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2_i:C,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2_i:D,5504
BLDC_Encoder_Axis_0/MSC_i_23/count1_1_sqmuxa_0_a2_i:Y,4842
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_23:A,7848
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_23:B,7129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_23:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_23:CC,6817
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_23:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_23:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_23:S,6817
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_23:UB,7129
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:CLK,6197
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:Q,6197
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[28]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[28]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[28]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[28]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[28]:Y,1300
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_123:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_123:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_123:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_123:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_123:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_11:A,1213
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_11:B,1087
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_11:C,955
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_11:D,951
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_11:Y,951
A0_PWM_UH_O_obuf/U0/U_IOOUTFF:A,4315
A0_PWM_UH_O_obuf/U0/U_IOOUTFF:Y,4315
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_203:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_203:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_203:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_203:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_203:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:CLK,7685
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:Q,7685
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_1:B,4424
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_1:C,4229
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_1:CC,4523
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_1:P,4229
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_1:S,4523
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs0_cry_1:UB,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI1JOOE[12]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI1JOOE[12]:B,7168
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI1JOOE[12]:C,2903
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI1JOOE[12]:CC,2865
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI1JOOE[12]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI1JOOE[12]:P,2903
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI1JOOE[12]:S,2865
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNI1JOOE[12]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_12_0:A,2648
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_12_0:B,6972
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_12_0:C,6522
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_12_0:CC,1684
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_12_0:D,4356
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_12_0:P,2648
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_12_0:S,1684
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_12_0:UB,4356
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_0_sqmuxa:A,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_0_sqmuxa:B,5891
BLDC_Encoder_Axis_0/MSC_i_29/PWM_CH_o_0_sqmuxa:Y,4242
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[14]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[14]:B,4747
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[14]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[14]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[14]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:CLK,5001
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:D,6888
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:Q,5001
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[13]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:CLK,5683
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:Q,5683
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[1]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIMGB3A[7]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIMGB3A[7]:B,3890
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIMGB3A[7]:C,7124
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIMGB3A[7]:CC,3799
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIMGB3A[7]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIMGB3A[7]:P,3890
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIMGB3A[7]:S,3799
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIMGB3A[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[16]:A,3253
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[16]:B,2122
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[16]:C,3315
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[16]:D,3225
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[16]:Y,2122
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:CLK,1913
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:D,1959
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:Q,1913
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:CLK,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:D,7880
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:EN,7792
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:Q,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_spi_mosi[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2:A,2885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2:B,2770
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2:CC,3093
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2:P,2803
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2:S,3093
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2:UB,2770
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:CLK,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:D,7313
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:Q,7848
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_12:A,4276
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_12:B,6084
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_12:P,4276
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_12:UB,6084
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:CLK,5045
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:Q,5045
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_delay_time_val_o[12]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_274:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_274:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_274:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_274:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_274:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[4]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[4]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[4]:C,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[4]:Y,5274
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:CLK,4000
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:D,8712
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:Q,4000
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:CLK,3019
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:D,2075
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:Q,3019
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_2[2]:A,2265
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_2[2]:B,2276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNINDB32_2[2]:Y,2265
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:D,5112
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[6]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[6]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[6]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:CLK,4753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:Q,4753
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:CLK,5773
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:Q,5773
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state_RNO[4]:A,7958
BLDC_Encoder_Axis_0/MSC_i_27/s_state_RNO[4]:B,7903
BLDC_Encoder_Axis_0/MSC_i_27/s_state_RNO[4]:C,7869
BLDC_Encoder_Axis_0/MSC_i_27/s_state_RNO[4]:D,6661
BLDC_Encoder_Axis_0/MSC_i_27/s_state_RNO[4]:Y,6661
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:D,5537
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:CLK,7832
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:Q,7832
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[24]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_1[18]:A,4179
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_1[18]:B,4258
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_1[18]:Y,4179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11:A,3925
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11:B,2956
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11:CC,2922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11:S,2922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11:UB,2956
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16:B,3466
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16:CC,2681
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16:S,2681
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:CLK,4336
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:D,5775
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:Q,4336
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIJ1AO1[5]:A,4527
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIJ1AO1[5]:B,3529
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIJ1AO1[5]:C,3427
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIJ1AO1[5]:Y,3427
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:CLK,6859
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:D,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:Q,6859
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult1_input[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:CLK,2071
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:D,1829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:Q,2071
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:C,6859
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:D,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPC,6859
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:CLK,3063
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:D,2671
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:Q,3063
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_10:B,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_10:S,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[43]:A,6451
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[43]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[43]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[43]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[43]:Y,-45
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[11]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_0:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_0:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_0:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_0:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:B,7686
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:C,6709
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:IPB,7686
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_8:IPC,6709
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:CLK,4233
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:Q,4233
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0:B,6648
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0:C,4482
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0:CC,2167
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0:D,2179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0:S,2167
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0:UB,2179
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17:B,2564
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_17:UB,2564
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_22:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_22:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_22:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_22:IPB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:CLK,6096
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:Q,6096
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_2:B,4657
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_2:C,3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_2:CC,4066
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_2:P,3654
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_2:S,4066
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_2:UB,4657
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNITRMR3[1]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNITRMR3[1]:B,4252
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNITRMR3[1]:C,7100
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNITRMR3[1]:CC,5503
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNITRMR3[1]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNITRMR3[1]:P,4252
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNITRMR3[1]:S,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNITRMR3[1]:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:CLK,6013
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:Q,6013
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch1_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1HGM[8]:A,3827
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1HGM[8]:B,3529
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1HGM[8]:C,3711
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1HGM[8]:Y,3529
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_11:B,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_11:S,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_11:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:CLK,6697
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:D,7145
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:Q,6697
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_13:A,6070
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_13:B,5427
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_13:CC,5102
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_13:S,5102
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_13:UB,5427
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_0:A,1877
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_0:B,5594
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_0:C,3031
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_0:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_0:D,2731
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_0:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m16_1_0_wmux_0:Y,1877
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[11]:A,5806
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[11]:B,6007
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[11]:C,2831
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[11]:D,2856
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[11]:Y,2831
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[35]:A,3561
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[35]:B,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[35]:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[35]:D,6655
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1[35]:Y,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[36]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[36]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[36]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:CLK,7806
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:Q,7806
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[17]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_222:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_222:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_222:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_222:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_222:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_8:A,1565
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_8:B,1303
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_8:P,1337
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_8:UB,1303
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[14]:A,6484
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[14]:B,7148
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[14]:C,6675
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[14]:CC,5650
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[14]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[14]:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[14]:S,5650
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[14]:UB,6675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:CLK,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:Q,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[10]:A,2831
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[10]:B,6039
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[10]:C,2532
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[10]:D,2514
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[10]:Y,2514
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:CLK,6130
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:D,8680
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:Q,6130
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[15]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[15]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[15]:C,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[15]:Y,5150
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[2]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_55:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_55:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_55:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_55:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_55:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:D,8724
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_1:A,6771
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_1:B,6697
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_1:CC,7544
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_1:P,6705
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_1:S,7544
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_1:UB,6697
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[10]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5:A,7808
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5:B,5262
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5:CC,5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5:S,5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5:UB,5262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:CLK,4799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:D,6875
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:Q,4799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_105:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_105:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_105:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_105:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_105:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:CLK,4028
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:D,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:Q,4028
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_285:A,7951
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_285:B,7890
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_285:C,7554
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_285:D,6370
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_285:Y,6370
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11:A,6847
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11:B,6770
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11:C,4359
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11:D,5186
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_11:Y,4359
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[10]:A,3899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[10]:B,2831
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[10]:C,5280
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[10]:D,3820
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[10]:Y,2831
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0:A,5226
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0:B,4995
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0:P,5147
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_0:UB,4995
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0:A,6966
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0:B,5472
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0:P,5599
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_0:UB,5472
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[7]:A,5852
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[7]:B,7054
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[7]:C,6579
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[7]:CC,5811
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[7]:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[7]:P,5852
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[7]:S,5811
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count_cry[7]:UB,6579
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI3QSPA[9]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI3QSPA[9]:B,4900
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI3QSPA[9]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI3QSPA[9]:CC,4148
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI3QSPA[9]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI3QSPA[9]:P,
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI3QSPA[9]:S,4148
BLDC_Encoder_Axis_0/MSC_i_23/count2_RNI3QSPA[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_11:B,6266
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_11:UB,6266
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[8]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[8]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[8]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[9]:A,6383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[9]:B,6299
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[9]:C,5599
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/ref_input_o_0_cZ[9]:Y,5599
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[6]:A,3381
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[6]:B,4756
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[6]:C,2326
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[6]:D,3133
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[6]:Y,2326
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIB4O81[14]:A,3019
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIB4O81[14]:B,2942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIB4O81[14]:C,2495
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIB4O81[14]:Y,2495
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:CLK,6266
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:Q,6266
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13_0:A,6219
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13_0:B,7274
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13_0:C,6958
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13_0:CC,5415
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13_0:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13_0:S,5415
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_13_0:UB,6958
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel_RNIVIG21[0]:A,4724
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel_RNIVIG21[0]:B,4732
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel_RNIVIG21[0]:C,4615
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_channel_sel_RNIVIG21[0]:Y,4615
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[7]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[7]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[7]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[7]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_6:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_6:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_6:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_6:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_272_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_272_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_272_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_272_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_7:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:CLK,4117
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:D,8712
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:Q,4117
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:CLK,2622
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:D,3513
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:Q,2622
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:CLK,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:D,7692
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:Q,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_141:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_141:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_141:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_141:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_141:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_0_sqmuxa_0_a3:A,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_0_sqmuxa_0_a3:B,7693
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_0_sqmuxa_0_a3:Y,7679
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_13:A,3823
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_13:B,3775
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_13:C,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un17_s_angle_count_incrlto17_13:Y,2622
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIUD0Q1[5]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIUD0Q1[5]:B,7096
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIUD0Q1[5]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIUD0Q1[5]:CC,7120
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIUD0Q1[5]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIUD0Q1[5]:P,7096
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIUD0Q1[5]:S,7120
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIUD0Q1[5]:UB,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:CLK,7836
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:Q,7836
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[13]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:CLK,8854
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:D,6834
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:EN,7521
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:Q,8854
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mas_en:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:CLK,5453
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:Q,5453
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o_1_sqmuxa_0_a2:A,5351
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o_1_sqmuxa_0_a2:B,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o_1_sqmuxa_0_a2:C,5377
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o_1_sqmuxa_0_a2:D,4933
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o_1_sqmuxa_0_a2:Y,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:CLK,6809
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:Q,6809
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:CLK,6833
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:Q,6833
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[14]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:CLK,5861
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:Q,5861
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:CLK,4655
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:Q,4655
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:D,3199
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:CLK,3681
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:Q,3681
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[3]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[3]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[3]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:CLK,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:D,8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:Q,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0:A,6962
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0:B,6442
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0:C,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0:CC,5503
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0:P,1786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0:S,2671
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0:UB,1775
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]:A,2498
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]:B,1779
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]:C,4045
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]:D,3921
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[4]:Y,1779
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[2]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[2]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[2]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_7:B,4606
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_7:C,4417
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_7:CC,4288
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_7:P,4417
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_7:S,4288
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[10],5916
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[11],5855
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[1],7455
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[2],7391
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[3],7119
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[4],7051
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[5],7001
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[6],6056
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[7],5964
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[8],5903
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CC[9],6000
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:CO,5878
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[0],6928
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[1],5855
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[2],5999
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[3],6013
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[6],5994
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[7],6057
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[8],6130
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:P[9],6155
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/calib_done_i_RNIA0AN_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[1]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[1]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[1]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[1]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:CLK,7866
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:Q,7866
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[19]:SLn,
A0_PWM_WL_O_obuf/U0/U_IOPAD:D,2345
A0_PWM_WL_O_obuf/U0/U_IOPAD:E,
A0_PWM_WL_O_obuf/U0/U_IOPAD:PAD,2345
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_4:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_4:B,6940
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_4:CC,7053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_4:S,7053
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_4:UB,6940
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:CLK,7617
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:D,8854
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:Q,7617
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_state[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_5:B,6169
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_5:UB,6169
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_ib_0_sqmuxa_0_a3_0_a3:A,7790
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_ib_0_sqmuxa_0_a3_0_a3:B,7729
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_ib_0_sqmuxa_0_a3_0_a3:C,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_ib_0_sqmuxa_0_a3_0_a3:Y,7642
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]:A,2154
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]:B,2662
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]:C,4352
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]:D,4235
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[15]:Y,2154
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_9:A,7048
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_9:B,6889
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_9:CC,7020
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_9:P,6982
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_9:S,7020
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_9:UB,6889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:B,7886
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:C,6711
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:IPB,7886
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_26:IPC,6711
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[1]:A,7964
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[1]:B,6965
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[1]:C,7862
BLDC_Encoder_Axis_0/MSC_i_13/state_o_RNO[1]:Y,6965
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:CLK,4089
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:D,8684
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:EN,7642
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:Q,4089
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ib[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[38]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[38]:B,7910
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[38]:C,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[38]:D,224
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[38]:Y,88
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:B,7946
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:C,6763
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:IPB,7946
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:IPC,6763
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy:B,4899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy:C,6457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy:P,4899
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_0_0_cy:Y,5888
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:D,5593
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_25:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_25:B,7161
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_25:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_25:CC,6703
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_25:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_25:P,7161
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_25:S,6703
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_25:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_a3_0[5]:A,7035
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_a3_0[5]:B,6998
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o3_0_i_a3_0[5]:Y,6998
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:CLK,3046
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:D,2246
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:Q,3046
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJHT9[8]:A,2804
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJHT9[8]:B,2727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJHT9[8]:C,2291
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJHT9[8]:Y,2291
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:C,6835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPC,6835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_33:IPD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_15:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_15:B,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_15:CC,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_15:S,5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_15:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:CLK,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:Q,6791
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[9]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[9]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[9]:Y,5379
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[7]:A,2167
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[7]:B,3039
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[7]:C,5332
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[7]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[7]:D,5176
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[7]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[7]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[7]:Y,2167
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_266:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_266:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_266:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_266:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_266:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[5]:A,4235
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[5]:B,1912
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[5]:C,1923
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[5]:Y,1912
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in_0_sqmuxa_0_a4:A,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in_0_sqmuxa_0_a4:B,6062
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in_0_sqmuxa_0_a4:Y,5621
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:CLK,4750
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:Q,4750
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_15:EN,8996
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_15:IPENn,8996
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_9:A,6350
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_9:B,4308
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_9:P,4362
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_9:UB,4308
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_8:A,1697
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_8:B,2468
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_8:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_8:IPA,1697
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_8:IPB,2468
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[28]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[28]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[28]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:CLK,4352
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:D,8682
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:Q,4352
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:CLK,1465
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:Q,1465
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:C,6745
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:IPC,6745
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:CLK,3057
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:D,988
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:Q,3057
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[2]:A,5873
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[2]:B,5445
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[2]:C,5334
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[2]:D,4242
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[2]:Y,4242
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:CO,2842
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[0],3682
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[1],3270
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[2],3369
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[3],3065
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[6],2991
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[7],2891
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[8],2913
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:P[9],3037
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[0],3535
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[10],2862
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[11],2922
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[1],3268
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[2],3317
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[3],2948
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[4],2916
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[5],2947
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[6],2875
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[7],2842
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[8],2890
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_0_CC_0:UB[9],2928
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[17]:A,5883
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[17]:B,3957
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[17]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[17]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns[17]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKT3IC[7]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKT3IC[7]:B,4461
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKT3IC[7]:C,7309
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKT3IC[7]:CC,4287
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKT3IC[7]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKT3IC[7]:P,4461
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKT3IC[7]:S,4287
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNIKT3IC[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:CLK,5496
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:D,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:Q,5496
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[5]:A,3329
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[5]:B,4704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[5]:C,2267
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[5]:D,3081
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[5]:Y,2267
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_4:B,2113
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_4:C,1721
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_4:CC,1088
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_4:S,1088
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_4:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:CLK,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:D,77
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:Q,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:CLK,3912
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:D,2324
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:Q,3912
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_6:A,3497
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_6:B,1100
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_6:P,1218
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_6:UB,1100
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:CLK,6841
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:Q,6841
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[27]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:CLK,3475
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:Q,3475
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_0_0:A,581
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_0_0:B,870
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_0_0:Y,581
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[3]:A,5485
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[3]:B,2836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[3]:C,3203
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[3]:D,3073
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[3]:Y,2836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[14]:A,5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[14]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[14]:C,5696
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[14]:Y,5060
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:CLK,6303
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:D,8673
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:Q,6303
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:CLK,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:EN,3147
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:Q,8867
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/fault_clr_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIBFA62[21]:A,4577
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIBFA62[21]:B,3572
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIBFA62[21]:C,3527
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIBFA62[21]:Y,3527
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:CLK,3325
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:Q,3325
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:CLK,5777
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:D,5903
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:Q,5777
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:CLK,6640
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:D,6460
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:Q,6640
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_state[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO_0:A,4615
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO_0:B,3627
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO_0:C,3421
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO_0:D,3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_4_RNO_0:Y,3324
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_3:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0:B,6912
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0:C,4739
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0:CC,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0:D,2736
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0:S,2014
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0:UB,2736
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_3:A,3570
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_3:B,4981
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_3:P,3570
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_3:UB,4981
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17:B,6370
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17:UB,6370
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_234:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_234:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_234:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_234:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_234:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:CLK,1370
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:D,1443
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:Q,1370
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:CLK,7853
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:Q,7853
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:CLK,4172
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:D,8686
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:EN,7640
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:Q,4172
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_ia[10]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:CLK,7912
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:Q,7912
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_period_val_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIV7LE2[1]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIV7LE2[1]:B,5999
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIV7LE2[1]:C,7100
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIV7LE2[1]:CC,7391
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIV7LE2[1]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIV7LE2[1]:P,5999
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIV7LE2[1]:S,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIV7LE2[1]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15:A,7808
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15:B,7415
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15:CC,6913
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15:S,6913
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_15:UB,7415
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJ6FVD[11]:A,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJ6FVD[11]:B,7090
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJ6FVD[11]:C,2825
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJ6FVD[11]:CC,2943
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJ6FVD[11]:D,
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJ6FVD[11]:P,2825
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJ6FVD[11]:S,2943
BLDC_Encoder_Axis_0/MSC_i_14/iq_ref_in_i_RNIJ6FVD[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[5]:A,5224
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[5]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[5]:C,5842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[5]:Y,5224
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[0]:A,1852
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[0]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[0]:Y,1852
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:CLK,7661
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:Q,7661
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[10]:A,6281
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[10]:B,6204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[10]:C,5825
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[10]:D,4588
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[10]:Y,4588
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIRTMT2[10]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIRTMT2[10]:B,7792
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIRTMT2[10]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIRTMT2[10]:CC,6921
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIRTMT2[10]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIRTMT2[10]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIRTMT2[10]:S,6921
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIRTMT2[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:CLK,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:Q,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_1:A,6870
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_1:B,6748
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_1:CC,7415
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_1:P,6756
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_1:S,7415
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_1:UB,6748
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:CLK,3445
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:D,8716
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:Q,3445
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:CLK,5777
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:D,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:Q,5777
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:CLK,2947
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:D,8682
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:Q,2947
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:CLK,3030
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:D,2739
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:Q,3030
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[6]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[6]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[6]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[6]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[6]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[6]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[6]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[6]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:CLK,7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:Q,7886
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_13:A,1002
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_13:B,1239
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_13:P,1002
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_13:UB,1255
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:CLK,4196
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:D,8683
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:Q,4196
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[12]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[14]:A,4276
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[14]:B,1880
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[14]:C,4151
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[14]:Y,1880
A0_ADC_SDO_O_obuf/U0/U_IOENFF:A,
A0_ADC_SDO_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3OH32[6]:A,2807
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3OH32[6]:B,2685
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3OH32[6]:C,2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3OH32[6]:Y,2456
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_en_o_6_0:A,7820
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_en_o_6_0:B,5547
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_en_o_6_0:C,7882
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_en_o_6_0:D,7722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_en_o_6_0:Y,5547
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:CLK,6902
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:D,8840
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:Q,6902
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_sync:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[28]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[28]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[28]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:CO,3946
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[0],4387
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[1],4269
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[2],4170
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[3],4084
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[6],3999
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[7],3946
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[8],4106
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:P[9],4049
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[0],5861
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[10],6145
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[11],6266
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[1],5956
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[2],6080
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[3],5999
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[4],6037
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[5],6129
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[6],6020
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[7],6078
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[8],6186
BLDC_Encoder_Axis_0/MSC_i_13/EN_SPEED_PI_PROC_un108_s_state_cry_0_CC_0:UB[9],6127
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:CLK,4218
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:D,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:Q,4218
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_1:A,6002
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_1:B,5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_1:P,5956
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_1:UB,5991
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[3]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[3]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[3]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[3]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[3]:Y,261
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[10],6982
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[11],6921
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[1],7448
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[2],7384
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[3],7112
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[4],7044
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[5],6994
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[6],7120
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[7],7029
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[8],6969
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CC[9],7066
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:CO,6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[0],6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[1],6925
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[2],7108
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[3],7084
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[6],7096
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[7],7145
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[8],7215
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:P[9],7202
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNIBC9D[13]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:D,5156
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_2:A,3824
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_2:B,5062
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_2:P,3824
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_2:UB,5062
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[11]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[25]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_65:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_65:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_65:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_65:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_65:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNI6TPE1:A,7798
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNI6TPE1:B,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNI6TPE1:C,4417
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNI6TPE1:Y,3384
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO:A,5889
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO:B,6125
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO:C,3984
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO:D,5669
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_23_RNO:Y,3984
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:D,6059
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[2]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n_3:A,6063
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n_3:B,5972
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n_3:C,5932
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n_3:D,5824
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_un10_s_cs_n_3:Y,5824
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[34]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[34]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[34]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[34]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:B,7787
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:C,6818
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:IPB,7787
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_15:IPC,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:B,7815
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:C,6754
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:IPB,7815
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_16:IPC,6754
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15:A,1261
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15:B,1233
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15:Y,1233
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:CLK,1554
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:D,6183
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:Q,1554
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[0]:A,7964
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[0]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[0]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[0]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[0]:Y,2538
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[5]:A,2076
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[5]:B,4221
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[5]:C,1718
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[5]:D,1912
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_0_0[5]:Y,1718
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17:B,3559
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17:C,3481
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17:CC,2564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17:S,2564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:CLK,5117
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:D,6849
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:Q,5117
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO:A,5582
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO:B,5534
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO:C,3516
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO:D,3571
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_10_RNO:Y,3516
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:CLK,4909
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:Q,4909
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[17]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[17]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[17]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[17]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:CLK,1456
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:D,8686
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:Q,1456
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:CLK,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:Q,6985
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8:A,2992
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8:B,2876
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8:CC,2661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8:P,2910
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8:S,2661
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8:UB,2876
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3:B,2765
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3:CC,2712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3:P,2765
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3:S,2712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3:UB,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:D,5112
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[11]:A,2054
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[11]:B,2926
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[11]:C,5217
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[11]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[11]:D,5063
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[11]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_i_m2_0_wmux_0[11]:Y,2054
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[12]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:CLK,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:Q,7933
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:CLK,7856
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:Q,7856
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:CLK,4315
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:D,5714
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:Q,4315
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:CLK,4365
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:D,6928
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:Q,4365
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:CLK,3805
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:Q,3805
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3]:SLn,
A0_PWM_UL_O_obuf/U0/U_IOENFF:A,
A0_PWM_UL_O_obuf/U0/U_IOENFF:Y,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:CLK,5212
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:D,6965
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:Q,5212
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/state_o_Z[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[8]:A,5143
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[8]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[8]:C,5786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[8]:Y,5143
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_259:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_259:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_259:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_259:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_259:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[17]:A,4929
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[17]:B,4850
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[17]:C,4431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[17]:Y,4431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_done_to_cordic_o_0_a3:A,5995
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_done_to_cordic_o_0_a3:B,5610
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_done_to_cordic_o_0_a3:C,5533
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mas_done_to_cordic_o_0_a3:Y,5533
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO:A,2022
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO:B,1908
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO:C,5474
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO:D,2776
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_3_0_RNO:Y,1908
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[10],5702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[11],5641
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[1],6262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[2],6154
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[3],5882
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[4],5814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[5],5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[6],5842
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[7],5750
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[8],5689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CC[9],5786
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:CO,5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[0],5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[1],5564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[2],5738
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[3],5723
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[6],5735
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[7],5775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[8],5845
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:P[9],5841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_28:B,6406
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_28:C,4374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_28:IPB,6406
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_28:IPC,4374
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:C,6814
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_27:IPC,6814
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13:B,1935
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13:CC,1445
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13:P,1935
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13:S,1445
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[14]:A,5746
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[14]:B,5963
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[14]:C,2780
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[14]:D,2797
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[14]:Y,2780
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:CLK,5727
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:D,8827
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:Q,5727
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_qa_dly1:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIHPVO6[22]:A,1639
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIHPVO6[22]:B,1422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIHPVO6[22]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIHPVO6[22]:CC,5085
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIHPVO6[22]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIHPVO6[22]:P,1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIHPVO6[22]:S,5085
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIHPVO6[22]:UB,1422
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_204:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_204:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_204:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_204:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_204:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_204:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1_0[8]:A,5880
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1_0[8]:B,3401
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1_0[8]:C,3283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1_0[8]:D,3098
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_1_0[8]:Y,3098
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:CLK,3100
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:D,2622
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:Q,3100
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_2:A,6146
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_2:B,6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_2:P,6130
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_2:UB,6137
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[26]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]:A,1790
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]:B,2300
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]:C,3988
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]:D,3871
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[4]:Y,1790
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[7]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_10:B,2337
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_10:C,2149
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_10:CC,1350
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_10:S,1350
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:CLK,5267
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:Q,5267
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[10]:A,4707
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[10]:B,2171
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[10]:C,2127
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_16_i_m2[10]:Y,2127
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_11:A,5316
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_11:B,4534
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_11:CC,4287
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_11:S,4287
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_11:UB,4534
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[7]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[7]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[7]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNINMT82[7]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNINMT82[7]:B,7215
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNINMT82[7]:C,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNINMT82[7]:CC,6969
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNINMT82[7]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNINMT82[7]:P,7215
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNINMT82[7]:S,6969
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count_RNINMT82[7]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:C,6738
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_22:IPC,6738
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_7:A,5861
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_7:B,5777
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_7:C,5733
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_7:D,5665
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_7:Y,5665
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:CLK,2689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:Q,2689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_278:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_278:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_278:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_278:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_278:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:CLK,594
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:D,8681
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:Q,594
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0:B,5074
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0:P,5074
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[14]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_0_sqmuxa:A,4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_0_sqmuxa:B,5891
BLDC_Encoder_Axis_0/MSC_i_29/PWM_BH_o_0_sqmuxa:Y,4242
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:CLK,2965
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:D,8678
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:Q,2965
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_10:B,4704
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_10:UB,4704
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:CLK,1569
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:Q,1569
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]:B,7006
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]:CC,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]:P,7006
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry_cy[0]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:CLK,4964
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:Q,4964
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:CLK,1737
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:D,6969
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:Q,1737
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[12]:A,1875
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[12]:B,3955
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[12]:C,3393
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[12]:Y,1875
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_RNIT6M81:A,2451
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_RNIT6M81:B,518
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_RNIT6M81:C,235
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_RNIT6M81:D,-393
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_RNIT6M81:Y,-393
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIH15O[9]:A,3130
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIH15O[9]:B,3046
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIH15O[9]:C,2606
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIH15O[9]:Y,2606
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[16]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[16]:B,7661
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[16]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[16]:CC,6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[16]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[16]:P,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[16]:S,6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[16]:UB,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_10:A,6059
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_10:B,5295
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_10:CC,5144
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_10:S,5144
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_10:UB,5295
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:CLK,6183
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:D,8670
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:Q,6183
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[7]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[7]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[7]:C,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[7]:Y,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:CLK,4157
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:Q,4157
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]:A,2690
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]:B,1971
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]:C,4237
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]:D,4113
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[15]:Y,1971
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[15]:A,5500
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[15]:B,5797
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[15]:C,4400
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[15]:D,5238
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[15]:Y,4400
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_2:B,5148
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_2:CC,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_2:P,5148
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_2:S,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_2:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_120:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_120:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_120:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_120:IPA,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:CLK,4944
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:D,7105
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:Q,4944
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_o2[1]:A,2154
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_o2[1]:B,2083
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_o2[1]:Y,2083
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:CLK,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:D,7659
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:Q,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:CLK,7039
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:D,7531
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:Q,7039
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[13]:A,4883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[13]:B,4799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[13]:C,4380
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[13]:Y,4380
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:C,6828
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPC,6828
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_24:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_24:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4:A,7808
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4:B,5118
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4:CC,5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4:S,5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4:UB,5118
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CC[0],3852
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CC[1],3774
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CC[2],3716
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CC[3],3806
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CC[4],3735
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CC[5],3674
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CC[6],3796
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CC[7],3674
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:CI,3674
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[0],3876
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[1],3860
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[2],3975
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[3],4020
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[6],4308
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1:A,5971
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1:B,5894
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1:C,3483
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1:D,4310
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_axb_1:Y,3483
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[20]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[20]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[20]:Y,7555
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[0]:A,3996
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[0]:B,1673
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[0]:C,1684
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_15_i_m2[0]:Y,1673
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:CLK,3453
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:D,7105
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:Q,3453
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:CLK,4688
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:Q,4688
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_RNIQRNV:A,2943
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_RNIQRNV:B,1825
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_RNIQRNV:C,4688
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_RNIQRNV:Y,1825
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:B,7853
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:C,6802
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:D,7832
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPB,7853
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPC,6802
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPD,7832
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[36]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[36]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[36]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:CLK,3149
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:D,7811
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:EN,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:Q,3149
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_done:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:CC[0],1762
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:CC[1],1684
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:CC[2],1626
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:CC[3],1716
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:CC[4],1645
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:CC[5],1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:CC[6],1713
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:CI,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[0],2595
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[1],2648
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[3],2896
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[0],4395
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[1],4356
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[2],4493
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[3],4546
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[4],4587
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[5],4673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[10]:A,4560
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[10]:B,2171
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[10]:C,4438
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[10]:Y,2171
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_271:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_271:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_271:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_271:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_271:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:CC[0],5493
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:CC[1],5415
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:CC[2],5357
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:CC[3],5447
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:CC[4],5376
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:CC[5],5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:CI,5315
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[0],5515
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[1],6958
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[2],7084
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[3],7339
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[4],7467
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_0_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[3]:A,5839
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[3]:B,5418
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[3]:C,5307
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[3]:D,4211
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[3]:Y,4211
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO_0:A,4855
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO_0:B,2108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO_0:C,4970
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_8_0_RNO_0:Y,2108
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_87:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_87:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_87:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_87:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_87:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:CLK,6809
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:Q,6809
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[11]:A,4438
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[11]:B,4354
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[11]:C,4168
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[11]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[11]:Y,4168
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:CLK,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:D,8840
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:EN,8765
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:Q,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[2]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:CLK,6833
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:Q,6833
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[1]:A,7990
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[1]:B,7873
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[1]:C,7473
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[1]:D,7719
BLDC_Encoder_Axis_0/MSC_i_11/s_state_ns[1]:Y,7473
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[1]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[1]:B,5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[1]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[1]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[1]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[16]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[16]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3_0_a2[16]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:D,8717
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[10]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_7_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_7_PAD/U_IOINFF:Y,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:CLK,4502
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:D,8689
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:Q,4502
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[10]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_210:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_210:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_210:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_210:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_210:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:CLK,2121
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:D,7165
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:Q,2121
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m11_0_03_1_1_tz:A,3726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m11_0_03_1_1_tz:B,3428
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m11_0_03_1_1_tz:C,3604
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/m11_0_03_1_1_tz:Y,3428
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[9]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[9]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[9]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:CLK,4819
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:D,6907
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:Q,4819
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:CLK,3555
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:D,7273
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:Q,3555
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[6]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:CLK,4288
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:D,8860
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:Q,4288
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_6:A,4341
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_6:B,6088
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_6:P,4341
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_6:UB,6088
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_3:A,3475
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_3:B,1193
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_3:P,1310
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_3:UB,1193
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_5_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_5_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_5_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_5_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_5_m1_0_a2:Y,-247
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_198:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_198:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_198:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_198:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_198:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[11]:A,1901
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[11]:B,3271
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[11]:C,5008
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[11]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[11]:D,4861
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[11]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_wmux_0[11]:Y,1901
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:CLK,6771
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:Q,6771
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:CLK,4098
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:D,8724
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:EN,8654
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:Q,4098
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_theta_ol[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:CLK,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:Q,7848
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:CLK,7787
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:Q,7787
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P:A,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P:B,2765
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P:C,5738
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P:CC,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P:D,5407
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P:P,3764
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P:UB,6195
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_RNIVJ1P:Y,2765
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:CC[0],5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:CC[1],5118
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:CC[2],5060
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:CC[3],5150
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:CC[4],5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:CC[5],5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:CI,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[0],5218
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]:A,1550
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]:B,2060
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]:C,3748
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]:D,3631
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[3]:Y,1550
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18_FCINST1:CC,1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18_FCINST1:CO,1233
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:CLK,4362
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:D,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:Q,4362
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:CLK,4901
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:Q,4901
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_15:A,6147
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_15:B,6036
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_15:CC,5211
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_15:S,5211
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_15:UB,6036
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_15:A,5860
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_15:B,5395
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_15:CC,5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_15:S,5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_15:UB,5395
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]:A,2683
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]:B,1964
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]:C,4230
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]:D,4106
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[14]:Y,1964
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[7]:A,5092
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[7]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[7]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[7]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[7]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_15:A,5196
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_15:B,4835
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_15:CC,4208
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_15:S,4208
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_15:UB,4835
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIS9D54[17]:A,1565
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIS9D54[17]:B,1452
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIS9D54[17]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIS9D54[17]:CC,5106
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIS9D54[17]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIS9D54[17]:P,1516
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIS9D54[17]:S,5106
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNIS9D54[17]:UB,1452
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_13:A,2091
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_13:B,2005
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_13:P,2005
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_13:UB,2025
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m32_i_i_o2_0:A,1445
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m32_i_i_o2_0:B,2059
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m32_i_i_o2_0:C,1898
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m32_i_i_o2_0:D,1905
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_sn_m32_i_i_o2_0:Y,1445
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_5:B,1541
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_5:C,1159
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_5:CC,1275
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_5:P,1159
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_5:S,1275
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:B,7853
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:C,6802
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:D,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPB,7853
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPC,6802
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_21:IPD,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[19]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:CLK,3878
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:Q,3878
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:CLK,2814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:D,2315
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:Q,2814
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:CLK,2990
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:D,2193
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:Q,2990
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:CLK,3141
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:D,2735
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:Q,3141
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_6_0:A,7130
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_6_0:B,6627
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_6_0:C,2831
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_6_0:CC,2787
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_6_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_6_0:P,2901
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_6_0:S,2787
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_6_0:UB,2831
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:CC[0],6974
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:CC[1],6896
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:CC[2],6838
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:CC[3],6928
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:CC[4],6857
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:CC[5],6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:CC[6],6917
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:CI,6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[0],6996
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[1],7074
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[3],7245
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_1:UB[9],
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_127:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_127:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_127:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_127:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_127:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO_0:A,5663
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO_0:B,5569
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO_0:C,3712
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO_0:D,3629
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_16_RNO_0:Y,3629
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_17_1:A,6906
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_17_1:B,6865
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_17_1:C,5254
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_17_1:D,6060
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_axb_17_1:Y,5254
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:CLK,6016
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:D,7198
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:Q,6016
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_oc_thresh_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__un1_s_state_3_0_0:A,7884
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__un1_s_state_3_0_0:B,7812
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__un1_s_state_3_0_0:C,6808
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__un1_s_state_3_0_0:D,7617
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__un1_s_state_3_0_0:Y,6808
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[4]:A,5949
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[4]:B,6144
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[4]:C,2968
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[4]:D,2993
BLDC_Encoder_Axis_0/MSC_i_23/un1_s_angle_count_i[4]:Y,2968
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[16]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[16]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[16]:C,5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3_2[16]:Y,5079
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[14]_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[2]:A,3059
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[2]:B,4328
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[2]:C,6167
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[2]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[2]:D,6013
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[2]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[2]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[2]:Y,3059
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:C,6757
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_0:IPC,6757
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[14]:A,4518
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[14]:B,2628
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[14]:C,1836
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[14]:Y,1836
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_a2[1]:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_a2[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_a2[1]:C,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_a2[1]:D,4823
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_0_0_a2[1]:Y,4823
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en_RNO_0:A,7406
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en_RNO_0:B,7485
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en_RNO_0:C,7794
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en_RNO_0:D,7681
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mas_en_RNO_0:Y,7406
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_AL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SD_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:ARSHFT17_SL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[0],6750
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[10],6811
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[11],6731
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[12],6756
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[13],6704
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[14],6698
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[15],6724
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[16],6738
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[17],6755
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[1],6726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[2],6717
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[3],6690
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[4],6702
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[5],6726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[6],6765
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[7],6740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[8],6747
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A[9],6740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_EN[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_EN[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:A_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[0],6791
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[10],6802
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[11],6844
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[12],6795
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[13],6814
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[14],6833
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[15],6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[16],6835
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[17],6804
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[1],6841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[2],6847
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[3],6807
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[4],6810
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[5],6828
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[6],6771
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[7],6818
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[8],6754
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B[9],6809
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_EN[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_EN[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:B_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CARRYIN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[12],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[13],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[14],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[15],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[16],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[17],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[18],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[19],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[20],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[21],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[22],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[23],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[24],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[25],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[26],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[27],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[28],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[29],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[2],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[30],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[31],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[32],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[33],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[34],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[35],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[36],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[37],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[38],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[39],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[3],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[40],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[41],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[42],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[43],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[6],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[7],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDIN[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:CDSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[12],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[13],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[14],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[15],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[16],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[17],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[18],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[19],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[20],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[21],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[22],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[23],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[24],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[25],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[26],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[27],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[28],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[29],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[2],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[30],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[31],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[32],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[33],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[34],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[35],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[36],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[37],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[38],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[39],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[3],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[40],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[41],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[42],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[43],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[6],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[7],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[8],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_CLK[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_CLK[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_EN[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_EN[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:C_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:DOTP,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_AL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SD_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:FDBKSEL_SL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:OVFL_CARRYOUT_SEL,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[10],6870
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[11],7590
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[12],7588
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[13],6882
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[14],6889
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[15],6959
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[16],6983
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[17],7582
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[18],7556
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[19],6875
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[20],6956
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[21],7552
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[22],7126
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[23],7552
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[24],7548
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[25],7547
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[8],6717
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P[9],6853
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_ARST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_ARST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_BYPASS[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_BYPASS[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_CLK[0],6717
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_CLK[1],6875
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_EN[0],8871
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_EN[1],8894
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_SRST_N[0],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:P_SRST_N[1],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SIMD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_AD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_AL_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_BYPASS,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_SD_N,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP:SUB_SL_N,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[2]:A,1786
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[2]:B,2658
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[2]:C,4955
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[2]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[2]:D,4795
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[2]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[2]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[2]:Y,1786
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[13]:A,6150
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[13]:B,4216
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[13]:C,3756
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[13]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns[13]:Y,2538
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:CLK,4640
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:Q,4640
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_done_dly1:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI9K3A5[2]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI9K3A5[2]:B,4239
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI9K3A5[2]:C,7075
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI9K3A5[2]:CC,5081
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI9K3A5[2]:D,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI9K3A5[2]:P,4239
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI9K3A5[2]:S,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNI9K3A5[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:CLK,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:D,6336
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:Q,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_i_init_ds[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:CLK,6731
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:Q,6731
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_13:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_13:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[25]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[25]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[25]:Y,7555
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_116:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_116:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_116:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_116:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_116:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:C,6725
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_32:IPC,6725
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:CLK,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:D,6654
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:Q,6142
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_iqpi_o_Z[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o_1_sqmuxa_0_a2:A,5350
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o_1_sqmuxa_0_a2:B,5434
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o_1_sqmuxa_0_a2:C,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o_1_sqmuxa_0_a2:D,4933
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_dead_time_val_o_1_sqmuxa_0_a2:Y,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[11]:A,1890
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[11]:B,2762
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[11]:C,5053
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[11]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[11]:D,4905
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[11]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[11]:Y,1890
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:CLK,4147
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:D,6791
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:Q,4147
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNII4KQB[11]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNII4KQB[11]:B,6432
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNII4KQB[11]:C,7494
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNII4KQB[11]:CC,5956
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNII4KQB[11]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNII4KQB[11]:P,6432
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNII4KQB[11]:S,5956
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNII4KQB[11]:UB,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_221:A,6197
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_221:B,4722
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_221:C,6075
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_0_221:Y,4722
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_1:B,1542
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_1:C,1353
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_1:CC,1669
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_1:P,1353
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_1:S,1669
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_1:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_8:A,3069
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_8:B,3026
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_8:C,2944
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_8:D,2843
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_8:Y,2843
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:CLK,2202
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:Q,2202
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6:A,6894
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6:B,3324
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6:C,3268
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6:CC,3592
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6:P,3384
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6:S,3592
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_6:UB,3268
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[0]_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_1[17]:A,5151
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_1[17]:B,4826
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_1[17]:C,2501
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_1[17]:D,2368
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_0_a2_1[17]:Y,2368
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:CLK,7886
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:Q,7886
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[30]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_17:B,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_17:S,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_17:UB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:C,6733
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:IPC,6733
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[10]:A,6111
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[10]:B,6033
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[10]:C,4544
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[10]:D,5521
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[10]:Y,4544
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_7:A,7150
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_7:B,7017
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_7:CC,6958
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_7:P,7088
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_7:S,6958
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_7:UB,7017
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]:A,3220
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]:B,2501
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]:C,4767
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]:D,4643
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[17]:Y,2501
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[15]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[15]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[15]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[39]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:CLK,2909
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:D,4843
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:Q,2909
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2_0:A,5073
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2_0:B,4961
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2_0:Y,4961
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNII1NK3[16]:A,1582
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNII1NK3[16]:B,1394
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNII1NK3[16]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNII1NK3[16]:CC,5176
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNII1NK3[16]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNII1NK3[16]:P,1503
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNII1NK3[16]:S,5176
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNII1NK3[16]:UB,1394
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:CLK,6802
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:Q,6802
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3:A,3699
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3:B,3585
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3:C,3612
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3:D,3483
BLDC_Encoder_Axis_0/MSC_i_17/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3:Y,3483
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_11:B,1316
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_11:UB,1316
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:CLK,2043
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:D,2037
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:Q,2043
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[0]:A,7737
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[0]:B,6262
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[0]:C,7862
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[0]:Y,6262
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H:A,6221
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H:B,4893
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H:C,6126
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H:D,5761
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H:P,4893
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1_RNID70H:UB,5761
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[4]:A,4450
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[4]:B,3319
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[4]:C,4489
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[4]:D,4382
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[4]:Y,3319
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]:A,2634
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]:B,2127
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]:C,4387
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]:D,4269
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[10]:Y,2127
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[15]:A,4283
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[15]:B,1887
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[15]:C,4158
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[15]:Y,1887
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_0_PAD/U_IOPAD:D,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_0_PAD/U_IOPAD:E,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_0_PAD/U_IOPAD:PAD,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DATA_0_PAD/U_IOPAD:Y,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[1],3743
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[2],3824
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[3],3570
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[6],3559
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[7],3468
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[8],3496
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CC[9],3601
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:CO,3384
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[0],3427
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[1],3384
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[2],3514
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[3],3543
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[6],3555
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[7],3551
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[8],3621
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:P[9],3661
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_0_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:CLK,4211
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:D,6291
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:Q,4211
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[10]:A,3427
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[10]:B,4802
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[10]:C,2372
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[10]:D,3117
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[10]:Y,2372
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:CLK,3873
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:D,7002
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:Q,3873
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_out_f[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIRF3C9[9]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIRF3C9[9]:B,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIRF3C9[9]:C,7716
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIRF3C9[9]:CC,5916
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIRF3C9[9]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIRF3C9[9]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIRF3C9[9]:S,5916
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIRF3C9[9]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:CLK,6847
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:EN,2873
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:Q,6847
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/pwm_gain_val_o[3]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2:A,5499
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2:B,5886
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2:C,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2:D,4961
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2:Y,3090
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_13:A,6163
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_13:B,6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_13:P,6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_13:UB,6137
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:CLK,4359
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:EN,3129
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:Q,4359
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_window_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[39]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[39]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[39]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_4_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_4_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_4_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_4_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_4_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_0_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_0_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_0_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_0_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_0_m1_0_a2:Y,-247
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_217:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_217:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_217:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_217:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_217:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_217:IPC,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:CLK,5975
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:D,7568
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:EN,7414
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:Q,5975
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/omega_out_o_Z[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[1]:A,5511
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[1]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[1]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[1]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[1]:Y,2639
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:D,2890
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_13:B,6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_13:CC,7027
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_13:P,6865
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_13:S,7027
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6_0:A,5486
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6_0:B,6536
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6_0:C,6889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6_0:CC,5593
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6_0:P,5486
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6_0:S,5593
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_6_0:UB,6889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_10:A,525
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_10:B,518
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_10:C,394
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_10:D,268
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_10:Y,268
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29_RNO:A,5748
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29_RNO:B,5671
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29_RNO:C,5900
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29_RNO:Y,5671
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_238:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_238:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_238:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_238:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_238:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:CLK,2692
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:D,1923
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:Q,2692
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[14]:A,3323
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[14]:B,2208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[14]:C,3364
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[14]:D,3284
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[14]:Y,2208
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:CLK,7864
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:Q,7864
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[36]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:CLK,1899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:D,8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:Q,1899
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNO[12]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNO[12]:B,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNO[12]:C,7716
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNO[12]:CC,5878
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNO[12]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNO[12]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNO[12]:S,5878
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNO[12]:UB,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:CLK,6802
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:D,8729
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:Q,6802
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_midmatch_dly:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_s_30:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_s_30:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_s_30:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_s_30:CC,6732
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_s_30:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_s_30:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_s_30:S,6732
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_s_30:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:CLK,6841
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:Q,6841
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:CLK,7946
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:Q,7946
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[28]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[13]:A,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[13]:B,7661
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[13]:C,7716
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[13]:CC,6838
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[13]:D,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[13]:P,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[13]:S,6838
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry[13]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNID6O81[15]:A,4045
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNID6O81[15]:B,3968
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNID6O81[15]:C,3487
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNID6O81[15]:Y,3487
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:CLK,1233
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:Q,1233
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:CLK,6062
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:D,8678
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:Q,6062
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vb_o_Z[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:CLK,6909
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:D,8464
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:Q,6909
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_sensor_reset:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIANVR1[11]:A,2818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIANVR1[11]:B,2915
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIANVR1[11]:Y,2818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_7:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_7:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_7:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_7:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0:A,7841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0:B,6620
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0:C,1955
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0:CC,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0:S,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_4_0:UB,1955
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:CLK,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_5:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_1:A,3280
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_1:B,4515
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_1:P,3280
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_1:UB,4515
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_16:B,6220
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_16:UB,6220
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9:A,6768
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9:B,6684
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9:C,6640
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9:D,5486
BLDC_Encoder_Axis_0/MSC_i_23/WAIT_PERIOD_PROC_un9_sensor_reset_ilto9:Y,5486
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_20:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_20:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_28:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_28:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_22:EN,9019
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_22:IPENn,9019
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:CLK,1900
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:D,8676
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:Q,1900
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[30]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:CLK,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:D,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:EN,7733
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:Q,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_miso_data[13]:SLn,
QA_I_ibuf/U0/U_IOPAD:PAD,6193
QA_I_ibuf/U0/U_IOPAD:Y,6193
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[0]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[0]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[0]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:CLK,6889
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:D,7020
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:Q,6889
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[38]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[12]:A,4492
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[12]:B,2606
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[12]:C,1830
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[12]:Y,1830
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0:A,7193
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0:B,6663
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0:C,4497
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0:CC,2175
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0:D,2372
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0:P,2448
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0:S,2175
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0:UB,2372
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:CLK,6774
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:D,7057
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:Q,6774
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:CLK,6168
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:Q,6168
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]:A,2609
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]:B,1890
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]:C,4156
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]:D,4032
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_0_wmux[11]:Y,1890
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_9:A,6279
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_9:B,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_9:P,6233
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_9:UB,6183
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset_RNO[16]:A,7820
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_offset_RNO[16]:Y,7820
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:CLK,3025
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:D,8677
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:Q,3025
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[32]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0:A,3893
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0:B,7149
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0:C,6673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0:CC,1817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0:S,1817
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_13_0:UB,6673
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:CLK,2978
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:Q,2978
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:C,6804
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPC,6804
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_35:IPD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2_1:A,3218
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2_1:B,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2_1:C,4794
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2_1:D,4110
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_theta_factor_o_1_sqmuxa_0_a2_1:Y,2990
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13:B,5124
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13:CC,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13:S,4378
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:CLK,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_0:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:CLK,4314
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:D,5689
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:Q,4314
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_line_count[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_10:A,5865
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_10:B,5114
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_10:CC,5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_10:S,5174
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_1_cry_10:UB,5114
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_1:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_1:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_1:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_1:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIRU1B_0[2]:A,3031
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIRU1B_0[2]:B,4958
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIRU1B_0[2]:Y,3031
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[37]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:CLK,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:D,7827
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:EN,7557
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:Q,8017
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sdo_reg[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_7:A,6254
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_7:B,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_7:P,4268
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_7:UB,4214
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO:A,5750
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO:B,5986
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO:C,3845
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO:D,5567
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO:Y,3845
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8_0:A,5591
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8_0:B,6646
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8_0:C,7055
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8_0:CC,5440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8_0:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8_0:P,5591
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8_0:S,5440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_8_0:UB,7055
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_231:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_231:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_231:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_231:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_231:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:CLK,6383
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:D,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:EN,8469
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:Q,6383
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y[9]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_83:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_83:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_83:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_83:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:CLK,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:EN,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:Q,6818
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_factor_o[7]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_171:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_171:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_171:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_171:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_171:IPB,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:CLK,6835
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:D,7296
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:Q,6835
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_factor_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:CLK,7792
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:D,6664
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:Q,7792
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI75T9[2]:A,2818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI75T9[2]:B,2741
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI75T9[2]:C,2304
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI75T9[2]:Y,2304
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_28:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_28:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_10:B,2710
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_10:UB,2710
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[15]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[15]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[15]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[15]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:CLK,3466
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:D,8686
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:Q,3466
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[16]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[9]:A,2027
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[9]:B,4107
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[9]:C,3545
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2[9]:Y,2027
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:CLK,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_5:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[37]:A,709
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[37]:B,566
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[37]:C,88
BLDC_Encoder_Axis_0/MSC_i_11/s_iout[37]:Y,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[20]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[20]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[20]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[20]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_16:A,7848
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_16:B,7537
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_16:CC,6842
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_16:S,6842
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_16:UB,7537
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:CLK,1950
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:D,1898
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:EN,4796
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:Q,1950
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17:B,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17:S,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_31:A,7646
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_31:B,5898
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_31:C,5788
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_31:CC,3129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_31:D,4771
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_31:P,5194
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_31:S,3129
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_31:UB,4771
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:CLK,4383
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:Q,4383
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIETOIE[7]:A,6991
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIETOIE[7]:B,1545
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIETOIE[7]:C,1620
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIETOIE[7]:CC,1298
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIETOIE[7]:D,6117
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIETOIE[7]:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIETOIE[7]:S,1298
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIETOIE[7]:UB,1545
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[1]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[1]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[1]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11[6]:A,3892
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11[6]:B,3815
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11[6]:C,3542
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11[6]:D,3421
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIKIP11[6]:Y,3421
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:C,6835
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPC,6835
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPD,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[17]:A,4906
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[17]:B,6790
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[17]:C,2639
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[17]:D,2930
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_4_3_ns_1[17]:Y,2639
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_6:A,6942
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_6:B,6774
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_6:CC,7057
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_6:P,6876
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_6:S,7057
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_6:UB,6774
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_286:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_286:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_286:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_286:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_286:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MAS_PI_INST_mas_done_o_RNIKUNB:A,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MAS_PI_INST_mas_done_o_RNIKUNB:B,7540
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MAS_PI_INST_mas_done_o_RNIKUNB:Y,7519
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[6]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[6]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[6]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o_RNO:A,5533
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o_RNO:B,7743
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o_RNO:Y,5533
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_17:B,5297
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_17:UB,5297
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_29:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_29:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_9:A,2207
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_9:B,2041
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_9:P,2121
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_9:UB,2041
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_153:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_153:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_153:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_153:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_153:IPB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[39]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_42:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_42:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_42:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_42:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_42:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:CLK,4411
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:D,4740
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:Q,4411
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[2]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[2]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[2]:C,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[2]:Y,5614
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_208:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_208:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_208:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_208:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_208:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[1]:A,7086
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[1]:B,5038
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[1]:C,4798
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[1]:CC,4862
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[1]:D,6574
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[1]:P,4913
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[1]:S,4862
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_cry[1]:UB,4798
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_32:A,7848
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_32:B,7299
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_32:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_32:CC,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_32:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_32:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_32:S,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_32:UB,7299
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16:A,7808
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16:B,7543
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16:CC,6849
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16:S,6849
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_i_init_ds_1_cry_16:UB,7543
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_31_0:A,2514
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_31_0:B,1839
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_31_0:C,1912
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_31_0:CC,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_31_0:D,625
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_31_0:P,1036
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_31_0:S,-247
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_31_0:UB,625
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_1[6]:A,5928
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_1[6]:B,5814
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_1[6]:C,5714
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_1[6]:D,3564
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_1[6]:Y,3564
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[9]:A,5240
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[9]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[9]:C,5702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3[9]:Y,5240
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto34:A,165
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto34:B,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto34:C,1144
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto34:D,1028
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto34:Y,88
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:CLK,3068
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:EN,3182
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:Q,3068
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIEVU8D[8]:A,6991
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIEVU8D[8]:B,1431
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIEVU8D[8]:C,1501
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIEVU8D[8]:CC,1359
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIEVU8D[8]:D,6011
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIEVU8D[8]:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIEVU8D[8]:S,1359
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIEVU8D[8]:UB,1431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:D,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[14]:A,2251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[14]:B,2273
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[14]:Y,2251
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:CLK,3595
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:Q,3595
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[6]:A,1891
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[6]:B,2763
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[6]:C,5060
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[6]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[6]:D,4906
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[6]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[6]:Y,1891
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:CLK,3705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:Q,3705
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[6]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[6]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[6]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[6]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMPBJA[10]:A,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMPBJA[10]:B,6659
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMPBJA[10]:C,7716
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMPBJA[10]:CC,5855
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMPBJA[10]:D,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMPBJA[10]:P,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMPBJA[10]:S,5855
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count_RNIMPBJA[10]:UB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_59:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_59:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_59:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_59:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:B,7856
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:C,6809
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:D,7842
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPB,7856
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPC,6809
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_19:IPD,7842
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNINJPLD[10]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNINJPLD[10]:B,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNINJPLD[10]:C,7716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNINJPLD[10]:CC,3751
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNINJPLD[10]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNINJPLD[10]:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNINJPLD[10]:S,3751
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNINJPLD[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:D,8729
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:CLK,7006
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:D,6932
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:Q,7006
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[8]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[8]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[8]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:CLK,2292
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:D,8673
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:Q,2292
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[40]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:C,6740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:IPC,6740
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIH7TDC[9]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIH7TDC[9]:B,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIH7TDC[9]:C,7716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIH7TDC[9]:CC,3812
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIH7TDC[9]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIH7TDC[9]:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIH7TDC[9]:S,3812
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNIH7TDC[9]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:C,6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPC,6859
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_31:IPD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_5:B,2043
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_5:UB,2043
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[11]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[11]:B,4396
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[11]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[11]:Y,91
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[6]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[6]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[6]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_10:A,5210
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_10:B,4428
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_10:CC,4242
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_10:S,4242
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_10:UB,4428
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[2]:A,1762
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[2]:B,2634
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[2]:C,4931
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[2]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[2]:D,4777
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[2]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[2]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_i_m2_0_wmux_0[2]:Y,1762
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIDP19A[10]:A,6363
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIDP19A[10]:B,1454
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIDP19A[10]:C,1529
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIDP19A[10]:CC,1346
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIDP19A[10]:D,6026
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIDP19A[10]:P,1505
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIDP19A[10]:S,1346
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIDP19A[10]:UB,1454
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[16]:A,77
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[16]:B,4371
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[16]:C,708
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[16]:Y,77
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:CLK,6197
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:D,7194
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:Q,6197
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:D,3437
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:CLK,2992
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:D,8668
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:Q,2992
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[42]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:D,5079
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_25:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_25:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_25:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_25:IPA,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:CLK,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:Q,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy:B,6712
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy:C,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy:CC,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy:P,6712
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_0_cy:UB,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_2:A,6915
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_2:B,6843
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_2:CC,7480
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_2:P,6879
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_2:S,7480
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_2:UB,6843
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:CLK,3710
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:EN,3102
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:Q,3710
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/stop_motor_o:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_0:A,1532
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_0:B,1525
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_0:C,382
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_0:D,1036
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_0:Y,382
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:C,6756
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:IPC,6756
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[38]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[38]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[38]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[31]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[31]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[31]:Y,7555
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:CLK,4164
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:D,7958
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:EN,7832
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:Q,4164
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_cs_n:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[15]:A,4423
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[15]:B,1887
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[15]:C,1843
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_bm[15]:Y,1843
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o_1_sqmuxa_0_a2:A,5477
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o_1_sqmuxa_0_a2:B,5886
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o_1_sqmuxa_0_a2:C,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o_1_sqmuxa_0_a2:D,4982
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ref_o_1_sqmuxa_0_a2:Y,3090
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:CLK,5206
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:Q,5206
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_9:A,4975
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_9:B,2928
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_9:P,3037
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_9:UB,2928
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:CLK,3372
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:D,7052
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:Q,3372
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:CLK,6824
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:D,5496
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:Q,6824
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_13/adc_start_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:CLK,6735
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:D,7136
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:Q,6735
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_0:A,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_0:B,4325
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_0:C,4170
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_0:CC,4722
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_0:P,4170
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_0:S,4722
BLDC_Encoder_Axis_0/MSC_i_17/inf_abs1_cry_0:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_2:A,7113
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_2:B,7019
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_2:CC,7460
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_2:P,7051
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_2:S,7460
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_2:UB,7019
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_252:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_252:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_252:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_252:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_252:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_252:IPC,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:CLK,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:D,5545
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:Q,6994
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vb3h_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[16]:A,3357
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[16]:B,3344
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[16]:C,2354
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[16]:D,2285
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[16]:Y,2285
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_11:IPENn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_201:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_201:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_201:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_201:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_201:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_80:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_80:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_80:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_80:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_80:IPB,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1_1[0]:A,5861
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1_1[0]:B,5756
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1_1[0]:C,4815
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1_1[0]:D,4649
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_1_1[0]:Y,4649
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0:B,6620
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0:C,4454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0:CC,2193
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0:D,2248
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0:S,2193
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0:UB,2248
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_5:B,7792
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_5:CC,7077
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_5:S,7077
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_5:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:C,6727
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_18:IPC,6727
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[0]:A,5799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[0]:B,5721
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[0]:C,4233
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[0]:D,5209
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_yi[0]:Y,4233
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:CC[0],4108
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:CC[1],4114
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:CC[2],4221
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:CC[3],4208
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:CC[4],4174
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:CI,4108
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[0],4485
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[1],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[3],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[0],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[1],4411
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[2],4562
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[3],4835
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[4],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[5],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:CLK,3100
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:D,7156
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:EN,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:Q,3100
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[15]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[15]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[15]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[15]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[6]:A,5525
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[6]:B,2876
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[6]:C,3243
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[6]:D,3113
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_1_a2_1[6]:Y,2876
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]:A,1974
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]:B,2480
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]:C,4172
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]:D,4055
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_0_wmux[10]:Y,1974
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[12]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[12]:B,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[12]:C,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i[12]:Y,1256
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[12]:A,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[12]:B,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[12]:C,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[12]:CC,6990
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[12]:D,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[12]:P,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[12]:S,6990
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt_cry[12]:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[39]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[39]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[39]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[39]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[39]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:CLK,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:Q,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:CLK,4100
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:D,8847
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:Q,4100
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICK7B8[25]:A,1747
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICK7B8[25]:B,1559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICK7B8[25]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICK7B8[25]:CC,5039
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICK7B8[25]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICK7B8[25]:P,1668
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICK7B8[25]:S,5039
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNICK7B8[25]:UB,1559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_6_0:A,5493
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_6_0:B,6434
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_6_0:C,5283
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_6_0:CC,5373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_6_0:D,6735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_6_0:P,5370
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_6_0:S,5373
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_error_cry_6_0:UB,5283
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[1]:A,4692
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[1]:B,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[1]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[1]:D,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[1]:Y,261
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_6:IPENn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:CLK,5821
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:D,5650
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:Q,5821
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state[4]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:CLK,6122
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:Q,6122
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_33:B,6374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_33:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_33:D,6389
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_33:IPB,6374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_33:IPC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_33:IPD,6389
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_19:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_19:IPENn,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_13:B,6877
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_13:CC,6888
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_13:P,6877
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_13:S,6888
BLDC_Encoder_Axis_0/MSC_i_17/un3_s_adc_ch0_offset_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:CLK,7009
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:D,6879
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:Q,7009
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch1_offset[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRNIT[31]:A,4118
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRNIT[31]:B,4028
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRNIT[31]:C,3723
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRNIT[31]:Y,3723
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[0],3501
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[10],3267
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[11],3206
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[1],3431
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[2],3382
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[3],3449
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[4],3385
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[5],3336
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[6],3437
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[7],3315
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[8],3254
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CC[9],3351
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CI,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:CO,3068
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[0],3577
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[1],3527
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[2],3609
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[3],3685
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[6],3707
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[7],3686
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[8],3768
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:P[9],3805
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[0],3456
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[10],3740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[11],3861
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[1],3551
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[2],3557
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[3],3594
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[4],3629
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[5],3724
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[6],3615
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[7],3673
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[8],3779
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_CC_1:UB[9],3722
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:CLK,3749
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:D,7145
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:EN,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:Q,3749
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/auto_restart_no_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:CLK,4790
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:D,7195
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:EN,5692
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:Q,4790
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:CLK,1945
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:D,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:EN,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:Q,1945
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_12:A,3511
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_12:B,5029
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_12:P,3511
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_12:UB,5029
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[4]:A,7083
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[4]:B,6690
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[4]:C,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_4_3_1[4]:Y,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:CLK,2163
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:Q,2163
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_16:B,2681
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_bc_cry_16:UB,2681
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_8:A,2179
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_8:B,2131
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_8:C,2057
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_8:D,1963
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_op_eq_un1_s_sensor_calib_count_8:Y,1963
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:D,8719
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:D,8663
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0:A,2745
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0:B,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0:P,2666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_0:UB,2538
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:B,7799
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:C,6754
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:D,7802
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPB,7799
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPD,7802
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[39]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[39]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[39]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[39]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:B,7871
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:C,6745
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:IPB,7871
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_32:IPC,6745
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_14:A,3469
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_14:B,5249
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_14:P,3469
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_14:UB,5249
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[15]:A,1971
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[15]:B,4116
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[15]:C,1843
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_i_m2_i_m2_ns[15]:Y,1843
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:D,7390
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[10]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[3]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[3]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[3]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:CLK,2956
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:Q,2956
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[17]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[17]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_RNO[17]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[17]:A,3461
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[17]:B,3440
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[17]:C,2108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[17]:D,3058
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[17]:Y,2108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:CLK,2818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:D,2208
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:Q,2818
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:CLK,3141
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:D,2056
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:Q,3141
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:CLK,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:Q,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[5]:A,1499
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[5]:B,7789
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out_7[5]:Y,1499
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:CLK,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:Q,7799
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_iq_ref_in_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_33:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_33:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_13:A,7749
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_13:B,6834
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_13:CC,6759
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_13:S,6759
BLDC_Encoder_Axis_0/MSC_i_23/un3_s_angle_out_f_cry_13:UB,6834
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_1:A,4523
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_1:B,5956
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_1:P,4523
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_1:UB,5956
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[5]:A,8017
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[5]:B,7507
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[5]:C,7889
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_mult1_input_5[5]:Y,7507
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:CLK,4197
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:Q,4197
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/id_pi_output_y_o[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:CLK,3089
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:Q,3089
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/angle_count_max_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_8:A,4600
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_8:B,4443
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_8:CC,4244
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_8:P,4511
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_8:S,4244
BLDC_Encoder_Axis_0/MSC_i_29/un1_dead_time_i_cry_8:UB,4443
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:CLK,4414
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:D,4705
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:Q,4414
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:CLK,5686
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:D,4148
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:Q,5686
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:CLK,317
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:D,8682
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:Q,317
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm[13]:A,5996
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm[13]:B,6035
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm[13]:C,2598
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm[13]:D,3405
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_bm[13]:Y,2598
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:CLK,4428
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:D,4786
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:Q,4428
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:CLK,6738
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:D,6726
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:EN,7762
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:Q,6738
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_mult_in0[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[13]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[13]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[13]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:D,5196
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_13:A,324
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_13:B,207
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_13:C,166
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_13:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un10_s_pioutlto33_13:Y,88
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_14:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_14:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_ns[12]:A,1997
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_ns[12]:B,4108
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_ns[12]:C,1830
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_18_i_m2_ns[12]:Y,1830
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:CLK,6731
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:D,6906
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:Q,6731
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_12:A,7
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_12:B,-102
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_12:C,-47
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_12:D,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_12:Y,-247
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[10]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[10]:B,7933
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[10]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0:A,6949
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0:B,6505
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0:C,2622
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0:CC,5602
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0:D,6654
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0:P,2637
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0:S,3513
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_0_0:UB,2622
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[1]:A,6115
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[1]:B,6038
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[1]:C,5639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[1]:D,4422
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[1]:Y,4422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:CLK,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:D,5282
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:Q,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[12]:SLn,
GPIO_0_M2F_obuf/U0/U_IOPAD:D,
GPIO_0_M2F_obuf/U0/U_IOPAD:E,
GPIO_0_M2F_obuf/U0/U_IOPAD:PAD,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3:A,1554
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3:B,1384
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3:CC,1373
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3:P,1475
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3:S,1373
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3:UB,1384
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5:A,3788
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5:B,2819
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5:CC,2947
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5:S,2947
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5:UB,2819
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:CLK,1835
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:D,8674
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:Q,1835
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:CLK,7689
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:Q,7689
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1_RNI5U1P[0]:A,5934
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1_RNI5U1P[0]:B,5512
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1_RNI5U1P[0]:C,5401
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1_RNI5U1P[0]:Y,5401
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0:A,4722
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0:B,5929
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0:P,4722
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_0:UB,5929
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_19:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_19:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_8:B,6910
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_8:CC,7052
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_8:P,6910
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_8:S,7052
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[15]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[15]:B,7392
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[15]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[15]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[15]:D,7735
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[15]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[15]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux_0[15]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:CLK,2179
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:D,7022
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:Q,2179
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:CLK,400
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:D,6849
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:Q,400
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_35:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_35:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:CLK,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:Q,6862
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_ki_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:C,6731
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_30:IPC,6731
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[14]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_131:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_131:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_131:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_131:IPB,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[16]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[16]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[16]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[16]:CC,6944
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[16]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[16]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[16]:S,6944
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[16]:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_16:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:CLK,4824
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:D,6866
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:Q,4824
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:CLK,6740
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:D,6934
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:Q,6740
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_30:B,6416
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_30:C,4400
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_30:IPB,6416
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_30:IPC,4400
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_22:EN,6548
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_22:IPENn,6548
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[18]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[18]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[18]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[18]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[18]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_o2[4]:A,3100
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_o2[4]:B,1737
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_o2[4]:C,3870
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_o2[4]:D,3736
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_o2[4]:Y,1737
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[18]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[18]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[18]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[18]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:CLK,2819
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:Q,2819
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_6:A,3559
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_6:B,5002
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_6:P,3559
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_6:UB,5002
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNILFPJ[0]:A,6066
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNILFPJ[0]:B,6939
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNILFPJ[0]:Y,6066
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[1]:A,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[1]:B,6783
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/DELAY_PROC_theta_scl_buff_o_3[1]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:CLK,5859
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:D,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:EN,6283
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:Q,5859
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_8:A,4448
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_8:B,6254
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_8:P,4448
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_8:UB,6254
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_s_sckctr_done_2:A,6872
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_s_sckctr_done_2:B,6759
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_s_sckctr_done_2:C,7816
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_s_sckctr_done_2:D,7722
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/SCK_CTR_PROC_s_sckctr_done_2:Y,6759
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_13:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_13:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:CLK,3705
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:D,7203
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:Q,3705
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_9:IPENn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_10:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_11_m1_0_a2:A,7522
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_11_m1_0_a2:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_11_m1_0_a2:C,-247
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_11_m1_0_a2:D,-139
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2_11_m1_0_a2:Y,-247
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:CLK,7103
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:Q,7103
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:CLK,7703
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:D,4188
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:Q,7703
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count2[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[16]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[16]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[16]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[3]:A,6951
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[3]:B,6998
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[3]:C,2870
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[3]:D,3651
BLDC_Encoder_Axis_0/MSC_i_13/s_state_RNO[3]:Y,2870
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0:A,7841
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0:B,6754
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0:C,2131
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0:CC,1836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0:S,1836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_8_cry_10_0:UB,2131
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CC[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:CO,4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[0],5948
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[1],4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[2],4719
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[3],4380
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[6],4293
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[7],4268
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[8],4278
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:P[9],4362
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[0],5796
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[10],4242
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[11],4287
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[1],4640
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[2],4722
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[3],4290
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[4],4253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[5],4299
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[6],4230
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[7],4214
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[8],4244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_0_CC_0:UB[9],4308
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:C,6802
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:D,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPC,6802
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_21:IPD,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[1]:A,4066
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[1]:C,5073
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[1]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[1]:D,4933
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[1]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[1]:Y,4066
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI3497G[40]:A,1973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI3497G[40]:B,1846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI3497G[40]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI3497G[40]:CC,1471
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI3497G[40]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI3497G[40]:P,1947
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI3497G[40]:S,1471
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI3497G[40]:UB,1846
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_16:B,1080
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_16:UB,1080
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_1:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_1:B,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_1:CC,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_1:P,5018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_1:S,5675
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_1:UB,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI56HJ6[4]:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI56HJ6[4]:B,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI56HJ6[4]:C,7716
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI56HJ6[4]:CC,4950
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI56HJ6[4]:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI56HJ6[4]:P,
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI56HJ6[4]:S,4526
BLDC_Encoder_Axis_0/MSC_i_9/s_count_RNI56HJ6[4]:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:CLK,7946
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:Q,7946
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[28]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_11:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_11:B,5248
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_11:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_11:UB,5248
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_34:B,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_34:C,4431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_34:IPB,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_34:IPC,4431
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_32:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_32:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_32:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_32:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_32:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:CLK,7895
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:Q,7895
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[29]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_69:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_69:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_69:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_69:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_69:IPB,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[5]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[5]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[5]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:CLK,4832
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:D,6836
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:EN,7578
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:Q,4832
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:CLK,5983
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:Q,5983
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:D,8673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:D,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:CLK,6915
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:Q,6915
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[28]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[12]:A,1830
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[12]:B,2709
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[12]:C,4975
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[12]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[12]:D,4845
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[12]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[12]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[12]:Y,1830
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:CLK,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:D,3267
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:EN,8564
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:Q,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_out_scale[22]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]:A,4589
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]:B,6500
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]:C,6986
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]:CC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]:D,6862
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_mult1_input_5_0_0_wmux[2]:Y,4589
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:CLK,5181
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:D,6740
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:Q,5181
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[20]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[41]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:CLK,4033
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:Q,4033
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:D,7247
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[9]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[7]:A,4607
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[7]:B,2211
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[7]:C,4482
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_1_1[7]:Y,2211
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29:A,7841
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29:B,5857
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29:C,4968
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29:CC,3150
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29:D,5671
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29:S,3150
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_29:UB,4968
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_20:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_20:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_14:A,459
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_14:B,382
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_14:C,337
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_14:D,259
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_un1_ymax_ilto33_14:Y,259
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:CLK,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:D,5379
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:EN,5225
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:Q,8867
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_15/theta_scl_buff_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[15]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[15]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[15]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[15]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:CLK,6533
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:D,7607
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:Q,6533
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_state[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_8:A,6253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_8:B,6212
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_8:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_8:P,6237
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_8:UB,6212
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17_FCINST1:CC,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17_FCINST1:CO,5897
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:CLK,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:EN,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_6:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_4:B,1950
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_4:UB,1950
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_7:A,1352
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_7:B,3102
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_7:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_7:P,1352
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_7:UB,3102
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:CLK,7727
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:Q,7727
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:CLK,4708
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:D,8704
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:EN,7403
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:Q,4708
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state:A,6839
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state:B,5709
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state:C,5665
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state:D,5496
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state:Y,5496
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:Q,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[37]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:C,6743
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_24:IPC,6743
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:CLK,4399
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:D,4287
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:EN,4842
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:Q,4399
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/count1[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:CLK,2940
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:D,2752
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:Q,2940
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/s_angle_count[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:CLK,378
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:D,8676
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:Q,378
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[25]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]:B,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]:P,5614
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_RNI0KP4[17]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[24]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[24]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[24]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[24]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:CLK,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:D,7114
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:EN,8680
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:Q,7799
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_calib_cnt[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_6:A,1154
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_6:B,1330
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_6:P,1154
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_6:UB,1330
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:CLK,5578
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:D,2639
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:Q,5578
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_min_value[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:CLK,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:Q,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_speed_pi_acc_in[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_14:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_14:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_9_0:A,3098
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_9_0:B,7055
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_9_0:C,6581
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_9_0:CC,1678
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_9_0:D,4423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_9_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_9_0:S,1678
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_9_0:UB,4423
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_101:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_101:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_101:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_101:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_101:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[29]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[29]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[29]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[29]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[29]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_1_sqmuxa_i_0:A,7602
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_1_sqmuxa_i_0:B,7480
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_1_sqmuxa_i_0:C,7780
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_1_sqmuxa_i_0:D,7639
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_1_sqmuxa_i_0:Y,7480
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[7]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[7]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[7]:Y,7555
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:CLK,4809
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:D,4615
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:EN,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:Q,4809
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_index[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:CLK,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:Q,7735
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/speed_pi_kp_o[14]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:CLK,7759
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:D,8867
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:EN,6808
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:Q,7759
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/s_data_miso[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:CLK,7949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:Q,7949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:CLK,887
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:D,2870
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:Q,887
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:D,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[8]:A,4915
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[8]:B,2482
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[8]:C,2359
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[8]:D,2179
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_1[8]:Y,2179
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[16]:A,1436
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[16]:B,5153
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[16]:Y,1436
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:B,7806
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:C,6754
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:D,7809
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPB,7806
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPC,6754
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_17:IPD,7809
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_11:A,7828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_11:B,7181
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_11:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_11:CC,6866
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_11:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_11:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_11:S,6866
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_3/un8_mul_a_to_mas_o_cry_11:UB,7181
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2:A,4158
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2:B,4227
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2:C,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2:D,3843
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o_1_sqmuxa_0_a2_2:Y,3090
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[0],5085
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[10],1372
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[11],1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[1],5007
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[2],4949
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[3],5039
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[4],1591
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[5],1657
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[6],1779
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[7],1740
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[8],1636
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CC[9],1497
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CI,1229
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:CO,1294
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[0],1560
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[1],1510
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[2],1683
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[3],1668
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[6],1656
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[7],1774
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[8],1856
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:P[9],1859
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[0],1422
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[10],1777
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[11],1898
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[1],1516
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[2],1641
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[3],1559
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[4],1597
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[5],1689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[6],1553
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[7],1609
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[8],1699
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew_RNI52LG[16]_CC_1:UB[9],1759
A0_PWM_WH_O_obuf/U0/U_IOPAD:D,4354
A0_PWM_WH_O_obuf/U0/U_IOPAD:E,
A0_PWM_WH_O_obuf/U0/U_IOPAD:PAD,4354
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_26:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_26:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:CLK,6238
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:D,7250
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:Q,6238
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_13:A,6163
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_13:B,6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_13:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_13:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_13:P,6117
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_13:UB,6137
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[17]:A,2513
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[17]:B,2304
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[17]:C,2078
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[17]:Y,2078
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:CLK,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:EN,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[11]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[11]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[11]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[11]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_16:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_16:IPENn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:CLK,1510
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:D,8682
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:Q,1510
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[23]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout_0_sqmuxa_0_a4:A,6918
BLDC_Encoder_Axis_0/MSC_i_11/s_pout_0_sqmuxa_0_a4:B,6834
BLDC_Encoder_Axis_0/MSC_i_11/s_pout_0_sqmuxa_0_a4:Y,6834
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[10],6934
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[11],6873
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[1],7447
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[2],7386
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[3],7114
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[4],7046
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[5],6996
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[6],7074
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[7],6982
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[8],6921
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CC[9],7018
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:CO,6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[0],6846
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[1],6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[2],6926
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[3],6955
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[6],6967
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[7],6963
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[8],7033
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:P[9],7073
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[10],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[11],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[1],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[2],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[3],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[4],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[5],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[6],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[7],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[8],
BLDC_Encoder_Axis_0/MSC_i_23/speed_count_cry_cy[0]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[9]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[9]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[9]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[9]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_5:A,6056
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_5:B,5262
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_5:CC,5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_5:S,5427
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_5:UB,5262
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_12:A,6244
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_12:B,6037
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_12:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_12:P,6198
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_12:UB,6037
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_9:A,260
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_9:B,144
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_9:C,206
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_9:D,6
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un1_ymax_ilto34_i_a2_9:Y,6
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:D,2889
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[7]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:CLK,-393
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:EN,3202
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:Q,-393
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_en_o:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[3]:A,1539
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[3]:B,2411
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[3]:C,4708
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[3]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[3]:D,4554
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[3]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[3]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[3]:Y,1539
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_10:B,6197
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vb_i_cry_10:UB,6197
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[12]:A,4196
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[12]:B,4112
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[12]:C,3955
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[12]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[12]:Y,3955
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:CLK,1423
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:D,1355
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:Q,1423
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:CLK,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:D,2943
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:EN,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:Q,6226
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/init_speedpi_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_2:A,4841
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_2:B,3317
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_2:P,3369
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ab_cry_2:UB,3317
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[36]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_33:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_33:IPENn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_o2[7]:A,3954
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_o2[7]:B,5017
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_3_i_o2[7]:Y,3954
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14_RNI6SHR:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14_RNI6SHR:B,1494
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14_RNI6SHR:C,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14_RNI6SHR:CC,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14_RNI6SHR:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14_RNI6SHR:P,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_14_RNI6SHR:UB,1494
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_3:A,3107
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_3:B,4558
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_3:P,3107
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_3:UB,4558
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_39:A,6973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_39:B,3548
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_39:C,182
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_39:D,88
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_39:Y,88
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI150F1[0]:A,5825
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI150F1[0]:B,5777
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI150F1[0]:C,5677
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNI150F1[0]:Y,5677
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_99:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_99:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_99:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_99:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_99:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:CLK,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:D,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:Q,6679
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[7]:A,4553
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[7]:B,4469
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[7]:C,4281
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[7]:D,
BLDC_Encoder_Axis_0/MSC_i_14/theta_o_cZ[7]:Y,4281
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:CLK,1930
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:Q,1930
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:CLK,2843
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:D,8668
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:Q,2843
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:CLK,6037
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:D,7317
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:Q,6037
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_cl_omega_o[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_16:B,6220
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_16:UB,6220
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:CLK,7742
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:Q,7742
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a3_0[2]:A,7043
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a3_0[2]:B,6992
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a3_0[2]:C,4022
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a3_0[2]:D,5893
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_i_4_i_a3_0[2]:Y,4022
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:CLK,6844
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:Q,6844
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_17:A,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_17:B,7799
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_17:C,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_17:CC,6554
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_17:D,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_17:P,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_17:S,6554
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_init_iqpi_o_3_s_17:UB,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[10],1359
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[11],1298
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[1],1852
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[2],1788
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[3],1487
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[4],1417
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[5],1356
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[6],1499
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[7],1407
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[8],1346
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CC[9],1443
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:CO,1233
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[0],1248
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[1],1241
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[2],1398
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[3],1400
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[6],1412
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[7],1435
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[8],1505
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:P[9],1518
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[10],1431
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[11],1545
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[1],1233
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[2],1366
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[3],1271
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[4],1304
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[5],1411
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[6],1306
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[7],1364
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[8],1454
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out15_RNIP8EP_CC_0:UB[9],1413
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_13:A,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_13:B,7527
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_13:C,7552
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_13:CC,6660
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_13:D,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_13:P,
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_13:S,6660
BLDC_Encoder_Axis_0/MSC_i_23/s_omega_fil_inp_3_cry_13:UB,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:CLK,5834
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:D,6788
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:EN,7426
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:Q,5834
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_adc_ch0_offset[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:CLK,6738
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:D,6796
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:Q,6738
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[16]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_5:B,1523
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_5:UB,1523
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_1_0:A,1799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_1_0:B,6995
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_1_0:C,6516
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_1_0:CC,2778
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_1_0:D,4358
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_1_0:P,1799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_1_0:S,2534
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_1_0:UB,4358
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_6:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_6:B,1581
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_6:C,1165
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_6:CC,1100
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_6:P,1165
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_6:S,1100
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs0_cry_6:UB,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[40]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[40]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[40]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:D,5274
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:CLK,5115
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:Q,5115
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch2_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:B,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:C,6697
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:IPB,
BLDC_Encoder_Axis_0/MSC_i_17/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_6:IPC,6697
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:CLK,2199
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:D,8679
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:Q,2199
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_pout[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_31:A,7653
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_31:B,7225
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_31:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_31:CC,6740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_31:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_31:P,7595
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_31:S,6740
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_31:UB,7225
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[3]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[3]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[3]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[3]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[38]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[38]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[38]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[38]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[38]:Y,-45
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_6:A,3135
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_6:B,4579
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_6:P,3135
BLDC_Encoder_Axis_0/MSC_i_0/s_cmp_ca_cry_6:UB,4579
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:D,7050
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_9:A,4391
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_9:B,6195
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_9:P,4391
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_9:UB,6195
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_150:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_150:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_150:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_150:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_150:IPB,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:B,7837
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:C,6835
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:D,7852
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPB,7837
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPC,6835
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_33:IPD,7852
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_1_250_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_1_250_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_1_250_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_1_250_i_m2:Y,7698
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:D,5114
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:EN,8438
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/vc3h_o_Z[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[10],4762
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[11],4705
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[2],5284
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[3],4862
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[4],4792
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[5],4731
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[6],4883
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[7],4814
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[8],4753
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CC[9],4840
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:CO,4608
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[0],4891
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[1],4627
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[2],4932
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[3],4913
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[6],4927
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[7],4951
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[8],5033
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:P[9],5033
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[10],4944
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[11],5065
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[1],4608
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[2],4879
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[3],4798
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[4],4836
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[5],4928
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[6],4819
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[7],4877
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[8],4985
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter_lcry_cy_CC_0:UB[9],4926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:CLK,5217
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:Q,5217
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/speed_pi_output_y_o[11]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_122:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_122:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_122:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_122:IPA,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:CLK,1646
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:D,6111
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:Q,1646
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[8]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:CLK,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:Q,6873
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_ref_in_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:CLK,2094
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:D,6133
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:EN,5402
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:Q,2094
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_set_ref[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[12]:A,1997
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[12]:B,2876
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[12]:C,5142
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[12]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[12]:D,5018
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[12]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[12]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[12]:Y,1997
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:CLK,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:D,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:EN,7107
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:Q,7781
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_acc_in[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:CLK,5828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:Q,5828
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:CLK,4976
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:D,7215
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:EN,3082
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:Q,4976
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/seq_cntl_config_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:CLK,498
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:D,8679
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:Q,498
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:CLK,4222
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:D,4862
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:EN,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:Q,4222
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_29/s_pwm_counter[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:CLK,7685
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:Q,7685
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:CLK,4729
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:Q,4729
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]:A,1901
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]:B,2411
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]:C,4099
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]:D,3982
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_i_m2_0_0_wmux[11]:Y,1901
BLDC_Encoder_Axis_0/MSC_i_14/s_state_RNO[1]:A,7879
BLDC_Encoder_Axis_0/MSC_i_14/s_state_RNO[1]:B,7926
BLDC_Encoder_Axis_0/MSC_i_14/s_state_RNO[1]:Y,7879
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:CLK,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_1:IPENn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_17:A,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_17:B,1334
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_17:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_17:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_17:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_17:P,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_17:UB,1334
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:D,3705
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1[7]:A,2809
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1[7]:B,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1[7]:C,3082
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1[7]:D,2995
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1[7]:Y,1584
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_114:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_114:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_114:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_114:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_114:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_13:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_13:IPENn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[17]:A,5116
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[17]:B,2720
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[17]:C,4991
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_14_i_m2_i_m2_1_1[17]:Y,2720
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[22]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[22]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[22]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[22]:Y,3435
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[13]:A,1485
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[13]:B,5202
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out[13]:Y,1485
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:CLK,2101
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:D,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:EN,6366
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:Q,2101
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[16]_CC_0:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:CLK,7809
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:Q,7809
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:CLK,1689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:D,8679
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:Q,1689
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:CLK,5249
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:D,3806
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:EN,3420
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:Q,5249
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_count[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_6:A,6173
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_6:B,6068
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_6:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_6:P,6127
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_vc_i_cry_6:UB,6068
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[30]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0:A,6956
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0:B,6442
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0:C,4276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0:CC,7061
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0:D,2070
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0:P,2088
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0:S,2968
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0:UB,2070
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:D,8673
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:EN,6438
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_27:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_27:IPENn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:CLK,6029
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:D,8675
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:EN,7713
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:Q,6029
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/Vc_o_Z[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:B,7946
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:C,6763
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:IPB,7946
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/MSC_i_21/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_24:IPC,6763
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:CLK,5709
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:D,5964
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:Q,5709
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:CLK,363
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:D,6913
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:Q,363
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[15]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[4]:A,1779
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[4]:B,2651
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[4]:C,4948
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[4]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[4]:D,4794
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[4]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[4]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_wmux_0[4]:Y,1779
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_15:A,3574
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_15:B,5167
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_15:P,3574
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_15:UB,5167
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1QET[16]:A,3794
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1QET[16]:B,3473
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1QET[16]:C,3666
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI1QET[16]:Y,3473
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[32]:A,6896
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[32]:B,6846
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[32]:C,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2_1_0[32]:Y,3435
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:CLK,3324
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:EN,3182
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:Q,3324
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/en_filter_factor_omega_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_3:A,1498
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_3:B,3023
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_3:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_3:P,1498
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_3:UB,3023
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[2]:A,91
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[2]:B,5106
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[2]:C,704
BLDC_Encoder_Axis_0/MSC_i_11/s_output_y_RNO[2]:Y,91
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO_0:A,5628
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO_0:B,5580
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO_0:C,4533
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO_0:D,3643
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_24_RNO_0:Y,3643
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:CLK,6711
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:D,8827
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:Q,6711
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult0_input[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_6:A,5347
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_6:B,5166
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_6:C,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_6:CC,5262
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_6:D,
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_6:P,5268
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_6:S,5262
BLDC_Encoder_Axis_0/MSC_i_0/un2_s_v3h_cry_6:UB,5166
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[12]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[12]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[12]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[12]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[2]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[2]:B,5599
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[2]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[2]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[2]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:CLK,7641
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:Q,7641
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:D,3669
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[7]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[21]:A,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[21]:B,7926
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_s_add_cin_4[21]:Y,7440
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_8:A,7220
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_8:B,7125
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_8:CC,6898
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_8:P,7158
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_8:S,6898
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_8:UB,7125
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_22:A,616
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_22:B,612
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_22:C,489
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_22:D,353
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_un10_s_pioutlto34_i_a2_0_22:Y,353
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[21]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[21]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[21]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[21]:Y,6423
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[12]:A,2020
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[12]:B,3396
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[12]:C,5097
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[12]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[12]:D,4973
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[12]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[12]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_12_i_m2_0_wmux_0[12]:Y,2020
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:CLK,88
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:D,2465
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:Q,88
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_state[2]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[5]:A,8017
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[5]:B,7785
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[5]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4[5]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[2]:A,6226
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[2]:B,6142
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[2]:C,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/init_o_0_cZ[2]:Y,5421
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15_RNIREN51:A,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15_RNIREN51:B,1484
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15_RNIREN51:C,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15_RNIREN51:CC,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15_RNIREN51:D,
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15_RNIREN51:P,1484
BLDC_Encoder_Axis_0/MSC_i_13/inf_abs1_cry_15_RNIREN51:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[10],1678
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[11],1629
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[1],7061
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[2],2778
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[3],2378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[4],2311
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[5],2256
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[6],2385
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[7],1984
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[8],1923
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CC[9],1760
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CI,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:CO,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[0],6457
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[10],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[11],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[1],2108
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[2],1799
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[3],2276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[4],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[5],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[6],1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[7],2548
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[8],2514
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:P[9],2635
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[0],
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[10],4423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[11],4544
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[1],2128
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[2],4358
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[3],4271
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[4],4304
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[5],4407
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[6],4298
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[7],4356
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[8],4454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_6_cry_0_0_cy_CC_0:UB[9],4405
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIC1VA1[17]:A,2519
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIC1VA1[17]:B,2279
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIC1VA1[17]:C,3676
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIC1VA1[17]:Y,2279
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO_0:A,5707
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO_0:B,5659
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO_0:C,3802
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO_0:D,3722
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_21_RNO_0:Y,3722
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:CLK,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:D,5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:EN,5695
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:Q,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[10]:A,3510
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[10]:B,3472
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[10]:C,2487
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[10]:D,2413
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[10]:Y,2413
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[8]:A,5421
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[8]:B,5046
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[8]:C,3584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[8]:D,5310
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_4_iv_i_RNO[8]:Y,3584
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:CLK,6828
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:Q,6828
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[8]:A,2893
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[8]:B,4162
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[8]:C,6001
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[8]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[8]:D,5847
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[8]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[8]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_wmux_0[8]:Y,2893
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:CLK,4387
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:Q,4387
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_15:EN,8871
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_15:IPENn,8871
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[17]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[17]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[17]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[17]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_21:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_21:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[15]:A,2276
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[15]:B,2234
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[15]:Y,2234
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:CLK,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:D,8712
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:EN,6431
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:Q,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_157:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_157:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_157:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_157:IPA,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[6]:A,6035
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[6]:B,5987
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[6]:C,5283
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/act_input_o_1_1_cZ[6]:Y,5283
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:CLK,6859
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:Q,6859
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_mult1_input[15]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_1:A,6073
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_1:B,4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_1:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_1:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_1:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_1:P,4620
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_1:UB,4640
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]:A,2948
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]:B,3342
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]:C,5166
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]:D,5042
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_10_i_m2_0_0_wmux[10]:Y,2948
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:CLK,8680
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:D,8867
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:Q,8680
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/mas_done_o_Z:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:B,7742
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:C,6828
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:D,7691
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPB,7742
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPC,6828
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_11:IPD,7691
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_0:CLK,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_0:EN,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_0:IPCLKn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_0:IPENn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[24]:A,5379
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[24]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_buffer_3[24]:Y,5379
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:CLK,6809
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:D,7507
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:Q,6809
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult1_input[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_22:A,7848
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_22:B,7008
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_22:C,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_22:CC,6878
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_22:D,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_22:P,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_22:S,6878
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/FILTER_FSM_PROC_s_filter_incr_1_cry_22:UB,7008
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[13]:A,7446
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[13]:B,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[13]:C,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o[13]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[20]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[20]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[20]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[20]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[20]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:CLK,5722
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:D,5956
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:EN,5430
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:Q,5722
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_adctrig_count[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:C,6726
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:IPC,6726
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[4]:A,6833
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[4]:B,4987
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[4]:C,2777
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[4]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_3_3_ns_1[4]:Y,2538
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:D,1256
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/output_y_o_1[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_16:B,7786
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_16:CC,6849
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_16:S,6849
BLDC_Encoder_Axis_0/MSC_i_17/un2_s_adc_ch1_offset_cry_16:UB,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_un1_rl_done_i:A,5610
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_un1_rl_done_i:B,7680
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_un1_rl_done_i:Y,5610
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_14:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_14:B,4221
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_14:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_14:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_14:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_14:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_14:UB,4221
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:CLK,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:D,5235
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:Q,6818
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_mult0_input[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_9:A,6279
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_9:B,6183
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_9:P,6233
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_va_i_cry_9:UB,6183
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_0:A,4470
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_0:B,5326
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_0:C,4180
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_0:D,4096
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/un2_s_out_scale_cry_0_RNO_0:Y,4096
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:CLK,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:Q,2538
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10]:SLn,
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[4]:A,1585
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[4]:B,4285
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[4]:C,2764
MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[4]:Y,1585
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_2:A,1788
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_2:B,3104
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_2:P,1788
BLDC_Encoder_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out15_cry_2:UB,3104
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[10]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[10]:B,7792
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[10]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[10]:CC,7021
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[10]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[10]:P,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[10]:S,7021
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[10]:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:CLK,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:Q,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_iq_acc_in[18]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[12]:A,6092
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[12]:B,6015
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[12]:C,5636
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[12]:D,4399
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_xi[12]:Y,4399
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[9]:A,6117
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[9]:B,2711
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[9]:C,2635
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[9]:Y,2635
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:CLK,3724
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:D,7048
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:EN,6699
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:Q,3724
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr[18]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:CLK,2477
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:D,7105
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:EN,3035
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:Q,2477
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_rate_cnt_o[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr_RNIBO351:A,4838
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr_RNIBO351:B,4747
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr_RNIBO351:C,4340
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr_RNIBO351:D,3674
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_rr_RNIBO351:Y,3674
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_7:A,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_7:B,5185
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_7:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_7:CC,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_7:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_7:P,5185
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_7:S,5204
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_cry_7:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:CLK,7707
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:D,8230
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:EN,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:Q,7707
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_pi_sel_dly[0]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_kp_o[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_9:A,6350
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_9:B,4308
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_9:P,4362
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_9:UB,4308
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[10]:A,2829
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[10]:B,2684
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[10]:C,2514
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[10]:Y,2514
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:ADn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:ALn,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:CLK,7886
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:D,8867
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:EN,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:LAT,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:Q,7886
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:SD,
BLDC_Encoder_Axis_0/MSC_i_14/s_addc_input[30]:SLn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:CLK,6056
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:Q,6056
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch0_o[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[6]:A,5922
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[6]:B,5493
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[6]:C,5382
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[6]:D,4290
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[6]:Y,4290
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy:A,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy:B,5983
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy:C,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy:CC,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy:D,
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy:P,5983
BLDC_Encoder_Axis_0/MSC_i_9/s_rl_in_cry_0_cy:UB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:B,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:C,6713
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:IPB,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_25/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/CFG_10:IPC,6713
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:CC[0],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:CC[1],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:CC[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:CC[3],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:CC[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:CC[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:CC[6],4652
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:CI,4652
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[0],4959
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[1],4878
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[2],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[3],5064
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[4],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[5],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:P[9],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[0],4798
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[10],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[11],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[1],4898
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[2],5047
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[3],4944
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[4],4981
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[5],5100
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[6],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[7],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[8],
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_un14_en_pwm_i_cry_0_CC_1:UB[9],
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[26]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[26]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[26]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINRA62[24]:A,4562
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINRA62[24]:B,3580
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINRA62[24]:C,3536
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNINRA62[24]:Y,3536
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:CLK,2094
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:D,6886
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:EN,6500
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:Q,2094
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_sensor_calib_count[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI7BA62[20]:A,4482
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI7BA62[20]:B,3500
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI7BA62[20]:C,3456
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNI7BA62[20]:Y,3456
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8:A,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8:B,1682
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8:C,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8:CC,1565
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8:D,
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8:P,1682
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8:S,1565
BLDC_Encoder_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8:UB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:B,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:C,6859
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:D,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPB,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPC,6859
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_31:IPD,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_10:A,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_10:B,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_10:C,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_10:CC,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_10:D,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_10:P,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_10:S,
BLDC_Encoder_Axis_0/MSC_i_9/un1_slew_count_i_cry_10:UB,
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[10]:A,5764
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[10]:B,7893
BLDC_Encoder_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[10]:Y,5764
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_33:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_33:IPENn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0:A,7093
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0:B,6588
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0:C,4422
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0:CC,2745
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0:D,2122
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0:P,2187
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0:S,2745
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0:UB,2122
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[7]:SLn,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_13:A,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_13:B,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_13:C,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_13:IPA,
MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/IP_INTERFACE_13:IPC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_16:B,4174
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_16:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_16:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_16:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_16:UB,4174
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRVA62[25]:A,4657
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRVA62[25]:B,3659
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRVA62[25]:C,3614
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_24/s_filter_incr_RNIRVA62[25]:Y,3614
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2:B,4508
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2:CC,4780
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2:P,4508
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2:S,4780
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2:UB,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:CLK,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:D,261
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:EN,8383
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:Q,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/acc_out_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:CLK,7817
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:D,7555
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:Q,7817
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_add_cin[34]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:CLK,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:D,-45
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:EN,-393
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:Q,7933
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_acc[43]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[28]:A,6497
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[28]:B,7610
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[28]:C,-45
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[28]:D,614
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5[28]:Y,-45
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[9]:A,7781
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[9]:B,7926
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/DATA_COLLECTION_PROC_s_miso_data_2[9]:Y,7781
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_2:A,2074
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_2:B,1994
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_2:C,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_2:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_2:D,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_2:P,2018
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_2:UB,1994
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_0:A,1775
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_0:B,5702
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_0:C,2762
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_0:CC,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_0:D,2619
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_0:P,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_0:UB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/m11_0_0_wmux_0:Y,1775
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_0_0[1]:A,2413
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_0_0[1]:B,2815
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_0_0[1]:Y,2413
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:CLK,6959
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:Q,6959
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/olmng_dv_o[5]:SLn,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[3]:A,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[3]:B,7042
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[3]:C,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[3]:CC,7195
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[3]:D,
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[3]:P,7042
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[3]:S,7195
BLDC_Encoder_Axis_0/MSC_i_29/s_delay_counter_cry[3]:UB,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:ADn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:ALn,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:CLK,6702
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:D,6996
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:EN,7679
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:LAT,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:Q,6702
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:SD,
BLDC_Encoder_Axis_0/MSC_i_23/speed_count[4]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0:A,2978
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0:B,2764
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0:P,2886
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_un13_s_angle_count_incr_cry_0:UB,2764
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:CLK,2942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:D,2146
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:Q,2942
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:CLK,4905
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:Q,4905
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_3_0:A,7828
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_3_0:B,6586
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_3_0:C,2780
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_3_0:CC,2805
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_3_0:D,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_3_0:P,
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_3_0:S,2805
BLDC_Encoder_Axis_0/MSC_i_23/ANGLE_COUNT_PROC_s_angle_count_7_cry_3_0:UB,2780
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:CLK,1374
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:EN,5103
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:Q,1374
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/iq_pi_output_y_o[0]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:ADn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:ALn,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:CLK,7713
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:D,8729
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:EN,8745
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:LAT,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:Q,7713
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:SD,
BLDC_Encoder_Axis_0/MSC_i_27/s_state[1]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:CLK,3064
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:D,2114
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:EN,5666
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:Q,3064
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_15:EN,6525
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/FF_15:IPENn,6525
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[1]:A,5883
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[1]:B,5454
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[1]:C,5343
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[1]:D,4251
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[1]:Y,4251
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[20]:A,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[20]:B,7920
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[20]:Y,5366
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17_FCINST1:CC,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17_FCINST1:CO,4108
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17_FCINST1:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17_FCINST1:UB,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_12:A,7169
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_12:B,7077
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_12:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_12:CC,6958
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_12:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_12:P,7077
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_12:S,6958
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_12:UB,
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_10:A,4176
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_10:B,4132
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_10:C,4051
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_10:D,3950
BLDC_Encoder_Axis_0/MSC_i_14/SPEED_IQ_PI_INIT_GEN_PROC_op_eq_init_iqpi_o16_10:Y,3950
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[14]:A,7885
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[14]:B,7582
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[14]:C,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/s_theta_1[14]:Y,6732
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4DPM2[7]:A,1584
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4DPM2[7]:B,2603
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4DPM2[7]:C,2374
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4DPM2[7]:Y,1584
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:CLK,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:D,8680
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:Q,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_inew[26]:SLn,
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOV0QJ[3]:A,6561
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOV0QJ[3]:B,1554
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOV0QJ[3]:C,1624
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOV0QJ[3]:CC,1355
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOV0QJ[3]:D,6126
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOV0QJ[3]:P,1690
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOV0QJ[3]:S,1355
BLDC_Encoder_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOV0QJ[3]:UB,1554
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[32]:A,7555
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[32]:B,7933
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_add_cin_4[32]:Y,7555
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9:B,4655
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9:P,4655
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9:S,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9:UB,
BLDC_Encoder_Axis_0/MSC_i_14/s_state_s0_0_a2:A,7451
BLDC_Encoder_Axis_0/MSC_i_14/s_state_s0_0_a2:B,7526
BLDC_Encoder_Axis_0/MSC_i_14/s_state_s0_0_a2:Y,7451
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]:A,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]:B,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]:C,4184
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]:D,4066
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_0_wmux[1]:Y,4066
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:CLK,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:EN,3090
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:Q,8017
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/position_pi_ki_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[15]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[15]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[15]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[15]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[9]:A,2378
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[9]:B,5680
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[9]:C,2336
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[9]:Y,2336
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:CLK,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:D,7110
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:EN,2867
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:Q,7889
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/idq_pi_kp_o[3]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_193:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_193:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_193:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_193:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_193:IPB,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_193:IPC,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:CLK,1768
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:D,8674
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:Q,1768
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[35]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:CLK,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:Q,7832
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[24]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:CLK,3496
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:D,8663
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:EN,7361
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:Q,3496
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/s_vc[14]:SLn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15:A,7808
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15:B,5395
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15:CC,5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15:S,5112
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15:UB,5395
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[6]:A,2055
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[6]:B,2927
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[6]:C,5224
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[6]:CC,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[6]:D,5064
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[6]:P,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[6]:UB,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_11_i_m2_0_wmux_0[6]:Y,2055
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_35:EN,
BLDC_Encoder_Axis_0/MSC_i_23/MSC_i_26/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/FF_35:IPENn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[0]:A,7990
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[0]:B,7906
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[0]:C,6911
BLDC_Encoder_Axis_0/adc_interface_795x_0/state_RNO[0]:Y,6911
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:ADn,
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:ALn,
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:CLK,4815
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:D,8860
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:EN,
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:LAT,
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:Q,4815
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:SD,
BLDC_Encoder_Axis_0/MSC_i_13/s_start_motor_dly:SLn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_35:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_35:IPENn,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_14:EN,
BLDC_Encoder_Axis_0/MSC_i_14/MSC_i_16/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_14:IPENn,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_22_0:A,3025
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_22_0:B,1268
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_22_0:C,1347
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_22_0:CC,394
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_22_0:D,106
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_22_0:P,
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_22_0:S,394
BLDC_Encoder_Axis_0/MSC_i_11/s_piout_cry_22_0:UB,106
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:CLK,589
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:D,8682
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:Q,589
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[33]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_0[3]:A,6026
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_0[3]:B,5994
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_0[3]:C,988
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_0[3]:D,1737
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_0[3]:Y,988
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:CLK,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:D,7241
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:EN,2990
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:Q,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/rate_limit_slew_cnt_o[5]:SLn,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:CC[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:CC[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:CI,
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:P[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[0],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[10],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[11],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[1],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[2],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[3],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[4],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[5],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[6],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[7],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[8],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_13_i_m2_0_0_wmux[12]_CC_0:UB[9],
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3[1]:A,2411
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3[1]:B,2105
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3[1]:C,2333
BLDC_Encoder_Axis_0/apb3_en_if_0/prdata_o_1_0_a2_2_a2_1_a2_3[1]:Y,2105
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_4:A,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_4:B,4253
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_4:CC,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_29/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_4:UB,4253
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:CLK,1323
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:D,8719
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:EN,7603
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:Q,1323
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout[11]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:CLK,446
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:D,6800
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:EN,8667
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:Q,446
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_i_init_ds[17]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:CLK,7686
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:D,7440
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:EN,5621
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:Q,7686
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_add_cin[6]:SLn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[22]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[22]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[22]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[22]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[22]:Y,1300
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[17]:A,3382
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[17]:B,3369
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[17]:C,2384
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[17]:D,2310
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[17]:Y,2310
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_0_1[6]:A,7120
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_0_1[6]:B,7026
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_0_1[6]:C,6926
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_0_a3_0_1[6]:Y,6926
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:CLK,1341
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:D,1359
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:EN,3384
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:Q,1341
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_9/s_ramp_out[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNII4AD2[0]:A,
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNII4AD2[0]:B,6960
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNII4AD2[0]:C,6528
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNII4AD2[0]:CC,5686
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNII4AD2[0]:D,4912
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNII4AD2[0]:P,4918
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNII4AD2[0]:S,5686
BLDC_Encoder_Axis_0/MSC_i_23/count1_RNII4AD2[0]:UB,4912
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[16]:A,830
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[16]:B,29
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[16]:C,7566
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[16]:D,6301
BLDC_Encoder_Axis_0/MSC_i_11/PI_CONT_FSM_PROC_s_acc_5_0_a2[16]:Y,29
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[17]:A,7568
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[17]:B,7926
BLDC_Encoder_Axis_0/MSC_i_23/OMEGA_GEN1_PROC_omega_out_o_3[17]:Y,7568
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4NAJ2[14]:A,5973
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4NAJ2[14]:B,1411
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4NAJ2[14]:C,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4NAJ2[14]:CC,5191
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4NAJ2[14]:D,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4NAJ2[14]:P,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4NAJ2[14]:S,5191
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/s_pout_RNI4NAJ2[14]:UB,1411
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DIR_PAD/U_IOINFF:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/USB_ULPI_DIR_PAD/U_IOINFF:Y,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[10]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[10]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[10]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[10]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_4:B,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_4:C,4242
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_4:IPB,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/CFG_4:IPC,4242
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_34:EN,
BLDC_Encoder_Axis_0/MSC_i_11/MSC_i_12/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/FF_34:IPENn,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3:A,7088
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3:B,5141
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3:CC,5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3:P,5239
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3:S,5545
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3:UB,5141
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[31]:A,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[31]:B,7025
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[31]:C,6943
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/acc_in_o_1_1[31]:Y,6423
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[30]:A,1348
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[30]:B,1300
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[30]:C,7882
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[30]:D,3435
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_20/PI_CONT_FSM_PROC_acc_out_o_2[30]:Y,1300
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_11:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_11:B,1795
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_11:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_11:IPB,1795
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:CLK,7035
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:D,6940
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:EN,7664
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:Q,7035
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/spi_engine_inst/s_sck_count[3]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:CLK,3481
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:EN,7591
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:Q,3481
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_16:A,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_16:B,7792
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_16:C,7716
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_16:CC,3544
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_16:D,5908
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_16:P,
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_16:S,3544
BLDC_Encoder_Axis_0/MSC_i_17/un1_s_mult0_in_1_cry_16:UB,5908
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:CLK,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:D,5366
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:EN,5058
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:Q,7889
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_19/MSC_i_22/s_id_acc_in[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_12_129_i_m2:A,8017
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_12_129_i_m2:B,7933
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_12_129_i_m2:C,7698
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_12_129_i_m2:Y,7698
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:ADn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:ALn,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:CLK,4987
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:D,8847
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:EN,6734
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:LAT,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:Q,4987
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:SD,
BLDC_Encoder_Axis_0/adc_interface_795x_0/result_ch3_o[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0:A,1188
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0:B,1670
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0:C,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0:CC,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0:D,
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0:P,1188
BLDC_Encoder_Axis_0/MSC_i_13/FSM_SEQ_CONTROLLER_PROC_un12_s_vq_i_abs_cry_0:UB,1670
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_29:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_29:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_29:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_29:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_29:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[6]:A,6994
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[6]:B,6951
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[6]:C,6726
BLDC_Encoder_Axis_0/MSC_i_27/MUL_INP_GEN_PROC_s_mult_in0_4_1_1[6]:Y,6726
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:ADn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:ALn,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:CLK,6818
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:D,3621
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:EN,6398
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:LAT,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:Q,6818
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:SD,
BLDC_Encoder_Axis_0/MSC_i_17/s_mult0_in[10]:SLn,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_15:A,4279
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_15:B,6167
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_15:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_15:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_15:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_15:P,4279
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_15:UB,6167
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:CLK,4235
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:EN,7653
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:Q,4235
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16]:SLn,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_45:A,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_45:B,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_45:C,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_45:IPA,
MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/IP_INTERFACE_45:IPB,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:ADn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:ALn,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:CLK,5427
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:D,2538
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:EN,3475
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:LAT,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:Q,5427
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:SD,
BLDC_Encoder_Axis_0/MSC_i_0/s_max_value[8]:SLn,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:B,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:C,6772
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:IPB,
BLDC_Encoder_Axis_0/MSC_i_27/MSC_i_28/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/CFG_12:IPC,6772
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_4:A,6118
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_4:B,5118
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_4:C,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_4:CC,5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_4:D,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_4:P,
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_4:S,5478
BLDC_Encoder_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_1_cry_4:UB,5118
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_8:A,5905
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_8:B,5821
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_8:C,5777
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_8:D,5709
BLDC_Encoder_Axis_0/MSC_i_13/ADC_START_PROC_op_eq_un98_s_state_8:Y,5709
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:ADn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:ALn,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:CLK,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:D,7180
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:EN,2945
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:LAT,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:Q,6814
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:SD,
BLDC_Encoder_Axis_0/apb3_en_if_0/adc_scale_val_o[13]:SLn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:CLK,6747
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:D,6995
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:EN,6935
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:Q,6747
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_mult0_input[9]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[11]:A,5095
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[11]:B,7689
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[11]:C,5742
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_2_1_3[11]:Y,5095
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_5:A,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_5:B,6129
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_5:C,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_5:CC,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_5:D,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_5:P,
BLDC_Encoder_Axis_0/MSC_i_17/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_5:UB,6129
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a2_0_0[4]:A,3149
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a2_0_0[4]:B,3100
BLDC_Encoder_Axis_0/MSC_i_13/s_state_ns_o2_0_a2_0_0[4]:Y,3100
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:ADn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:ALn,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:CLK,309
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:D,8674
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:EN,7519
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:LAT,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:Q,309
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:SD,
BLDC_Encoder_Axis_0/MSC_i_11/s_inew[29]:SLn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI23MU[1]:A,7016
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI23MU[1]:B,6664
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI23MU[1]:C,6562
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI23MU[1]:Y,6562
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_9:A,7246
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_9:B,7066
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_9:C,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_9:CC,6995
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_9:D,
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_9:P,7154
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_9:S,6995
BLDC_Encoder_Axis_0/MSC_i_11/s_error_cry_9:UB,7066
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:ADn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:ALn,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:CLK,4777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:D,8860
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:EN,7611
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:LAT,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:Q,4777
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:SD,
BLDC_Encoder_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2]:SLn,
USB_ULPI_DATA[7],
USB_ULPI_DATA[6],
USB_ULPI_DATA[5],
USB_ULPI_DATA[4],
USB_ULPI_DATA[3],
USB_ULPI_DATA[2],
USB_ULPI_DATA[1],
USB_ULPI_DATA[0],
A0_ADC_SDI_I,6138
QA_I,6193
QB_I,6192
USB_ULPI_DIR,
USB_ULPI_NXT,
USB_ULPI_XCLK,
A0_ADC_CS_O,4164
A0_ADC_SCK_O,4288
A0_ADC_SDO_O,4354
A0_PWM_UH_O,4315
A0_PWM_UL_O,2345
A0_PWM_VH_O,4315
A0_PWM_VL_O,2345
A0_PWM_WH_O,4354
A0_PWM_WL_O,2345
A0_RUNNING_LED,2053
GPIO_0_M2F,
USB_ULPI_STP,
DEVRST_N,
