@W: MO129 :"d:\svn solutions\motor control\development\mcsk\sk2ablstsl10_4_1\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":781:8:781:9|Sequential instance MC_System_sb_0.CORERESETP_0.sm1_areset_n_q1 reduced to a combinational gate by constant propagation
@W: MO129 :"d:\svn solutions\motor control\development\mcsk\sk2ablstsl10_4_1\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":781:8:781:9|Sequential instance MC_System_sb_0.CORERESETP_0.sm1_areset_n_clk_base reduced to a combinational gate by constant propagation
@W: MO129 :"d:\svn solutions\motor control\development\mcsk\sk2ablstsl10_4_1\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1331:8:1331:9|Sequential instance MC_System_sb_0.CORERESETP_0.RESET_N_F2M_int reduced to a combinational gate by constant propagation
@W: MT246 :"d:\svn solutions\motor control\development\mcsk\sk2ablstsl10_4_1\component\work\mc_system_sb\ccc_0\mc_system_sb_ccc_0_fccc.vhd":110:4:110:11|Blackbox CCC is missing a user supplied timing model. This may have a negative effect on timing analysis and optimizations (Quality of Results) 
@W: MT420 |Found inferred clock MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock with period 10.00ns. Please declare a user-defined clock on object "n:MC_System_sb_0.CCC_0.GL0_net"
