@P:  Worst Slack : 2.048
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Estimated Frequency : 125.7 MHz
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Requested Frequency : 100.0 MHz
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Estimated Period : 7.952
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Requested Period : 10.000
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Slack : 2.048
@P:  System - Estimated Frequency : 1029.4 MHz
@P:  System - Requested Frequency : 100.0 MHz
@P:  System - Estimated Period : 0.971
@P:  System - Requested Period : 10.000
@P:  System - Slack : 9.029
@P:  Worst Slack(min analysis) : 0.680
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Estimated Frequency(min analysis) : 125.7 MHz
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Requested Frequency(min analysis) : 100.0 MHz
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Estimated Period(min analysis) : 7.952
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Requested Period(min analysis) : 10.000
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Slack(min analysis) : 2.048
@P:  System - Estimated Frequency(min analysis) : 1029.4 MHz
@P:  System - Requested Frequency(min analysis) : 100.0 MHz
@P:  System - Estimated Period(min analysis) : 0.971
@P:  System - Requested Period(min analysis) : 10.000
@P:  System - Slack(min analysis) : 9.029
@P: MC_System Part : m2s010fbga484-1
@P: MC_System Register bits  : 0 
@P: MC_System DSP Blocks  : 0
@P: MC_System I/O primitives : 219
@P:  CPU Time : 0h:00m:01s
