@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\clarke.vhd":161:8:161:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[9],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[6]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\clarke.vhd":161:8:161:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[6],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[0]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.s_va[17:0],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.add_c_to_mas_o_1[27:10]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[9],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[5]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[5],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[1]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1059:8:1059:9|Removing sequential instance MC_System_sb_0.CORERESETP_0.MDDR_DDR_AXI_S_CORE_RESET_N_int,  because it is equivalent to instance MC_System_sb_0.CORERESETP_0.FDDR_CORE_RESET_N_int
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":703:8:703:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF0_PERST_N_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":719:8:719:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF1_PERST_N_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":735:8:735:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF2_PERST_N_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":751:8:751:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF3_PERST_N_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":703:8:703:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF0_PERST_N_q2 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":719:8:719:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF1_PERST_N_q2 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":735:8:735:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF2_PERST_N_q2 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":751:8:751:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF3_PERST_N_q2 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":781:8:781:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm1_areset_n_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":703:8:703:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF0_PERST_N_q3 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":719:8:719:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF1_PERST_N_q3 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":735:8:735:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF2_PERST_N_q3 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":751:8:751:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF3_PERST_N_q3 reduced to a combinational gate by constant propagation 
@W: MO160 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Register bit state[0] is always 0, optimizing ...
@W: MO160 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\clarke.vhd":161:8:161:9|Register bit state[0] is always 0, optimizing ...
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":781:8:781:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm1_areset_n_clk_base reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1331:8:1331:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.RESET_N_F2M_int reduced to a combinational gate by constant propagation 
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":894:8:894:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif3_areset_n_rcosc_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif2_areset_n_rcosc_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":883:8:883:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif2_areset_n_rcosc_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif1_areset_n_rcosc_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":872:8:872:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif1_areset_n_rcosc_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_areset_n_rcosc_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":850:8:850:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm0_areset_n_rcosc_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_areset_n_rcosc_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":836:8:836:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif3_areset_n_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif2_areset_n_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":825:8:825:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif2_areset_n_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif1_areset_n_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":814:8:814:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif1_areset_n_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_areset_n_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":836:8:836:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif3_areset_n_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif2_areset_n_clk_base
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":825:8:825:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif2_areset_n_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif1_areset_n_clk_base
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":814:8:814:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif1_areset_n_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_areset_n_clk_base
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":770:8:770:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm0_areset_n_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_areset_n_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":803:8:803:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_areset_n_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm0_areset_n_clk_base
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":936:8:936:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif3_spll_lock_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.CONFIG2_DONE_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":922:8:922:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.CONFIG2_DONE_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.CONFIG1_DONE_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":922:8:922:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.CONFIG2_DONE_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif3_spll_lock_q2
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":908:8:908:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.CONFIG1_DONE_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif3_spll_lock_q2
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":883:8:883:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif2_areset_n_rcosc,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm0_areset_n_rcosc
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":894:8:894:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif3_areset_n_rcosc,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm0_areset_n_rcosc
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":872:8:872:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif1_areset_n_rcosc,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm0_areset_n_rcosc
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":861:8:861:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_areset_n_rcosc,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm0_areset_n_rcosc
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1471:8:1471:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif2_core,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.ddr_settled
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1495:8:1495:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif3_core,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.ddr_settled
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1447:8:1447:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif1_core,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.ddr_settled
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1423:8:1423:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif0_core,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.ddr_settled
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1544:8:1544:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif1_core_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif0_core_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1544:8:1544:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif3_core_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif0_core_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1544:8:1544:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif2_core_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif0_core_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1544:8:1544:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif0_core_q1,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.ddr_settled_q1
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1544:8:1544:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif3_core_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif2_core_clk_base
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1544:8:1544:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif2_core_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif1_core_clk_base
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1544:8:1544:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif1_core_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif0_core_clk_base
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1544:8:1544:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.release_sdif0_core_clk_base,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.ddr_settled_clk_base
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1252:8:1252:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif2_state[0:3],  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_state[0:3]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1311:8:1311:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif3_state[0:3],  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_state[0:3]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1193:8:1193:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif1_state[0:3],  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.sdif0_state[0:3]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1311:8:1311:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF3_PHY_RESET_N_int,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF2_PHY_RESET_N_int
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1252:8:1252:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF2_PHY_RESET_N_int,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF1_PHY_RESET_N_int
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1193:8:1193:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF1_PHY_RESET_N_int,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF0_PHY_RESET_N_int
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1311:8:1311:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF3_CORE_RESET_N_0,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF2_CORE_RESET_N_0
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1252:8:1252:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF2_CORE_RESET_N_0,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF1_CORE_RESET_N_0
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1193:8:1193:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF1_CORE_RESET_N_0,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF0_CORE_RESET_N_0
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Stepper_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[1],  because it is equivalent to instance Stepper_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[0]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1059:8:1059:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.SDIF_RELEASED_int,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.DDR_READY_int
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[1] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[2] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[0] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[2] reduced to a combinational gate by constant propagation
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Removing instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[1],  because it is equivalent to instance Stepper_Axis_0.adc_measurements_0.s_r_sck_max_count[3]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Removing instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[0],  because it is equivalent to instance Stepper_Axis_0.adc_measurements_0.s_r_sck_max_count[3]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\mas.vhd":210:16:210:17|Removing instance Stepper_Axis_0.FOC_transforms_0.MAS_INST.MAS_PROC.op_mult.un3_product_o_mac.product_o[29],  because it is equivalent to instance Stepper_Axis_0.FOC_transforms_0.MAS_INST.MAS_PROC.op_mult.un3_product_o_mac.product_o[28]
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\seq_controller.vhd":289:2:289:3|Sequential instance I_Stepper_Axis_0.seq_controller_0.state_0_7cc.Stepper_Axis_0.seq_controller_0.state[1] reduced to a combinational gate by constant propagation
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\clarke.vhd":161:8:161:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[9],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[6]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\clarke.vhd":161:8:161:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[6],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[0]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.s_va[17:0],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.add_c_to_mas_o_1[27:10]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[9],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[5]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[5],  because it is equivalent to instance Bldc_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[1]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1059:8:1059:9|Removing sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.MDDR_DDR_AXI_S_CORE_RESET_N_int,  because it is equivalent to instance MC_System_0.MC_System_sb_0.CORERESETP_0.FDDR_CORE_RESET_N_int
@W: MO160 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Register bit state[0] is always 0, optimizing ...
@W: MO160 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\clarke.vhd":161:8:161:9|Register bit state[0] is always 0, optimizing ...
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":781:8:781:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm1_areset_n_q1 reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":781:8:781:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.sm1_areset_n_clk_base reduced to a combinational gate by constant propagation 
@W: MO171 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\actel\directcore\coreresetp\7.0.104\rtl\vhdl\core\coreresetp.vhd":1331:8:1331:9|Sequential instance MC_System_0.MC_System_sb_0.CORERESETP_0.RESET_N_F2M_int reduced to a combinational gate by constant propagation 
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\inverse_clarke.vhd":166:8:166:9|Removing sequential instance Stepper_Axis_0.FOC_transforms_0.ICLARKE_INST.mul_b_to_mas_o_1[1],  because it is equivalent to instance Stepper_Axis_0.FOC_transforms_0.CLARKE_INST.mul_b_to_mas_o_1[0]
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[1] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[2] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[0] reduced to a combinational gate by constant propagation
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Sequential instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[2] reduced to a combinational gate by constant propagation
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Removing instance Stepper_Axis_0.adc_measurements_0.s_r_sck_sel[1],  because it is equivalent to instance Stepper_Axis_0.adc_measurements_0.s_r_sck_max_count[3]
@W: BN132 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\adc_measurements.vhd":469:8:469:9|Removing instance Stepper_Axis_0.adc_measurements_0.s_r_adc_chnls_4_samp[0],  because it is equivalent to instance Stepper_Axis_0.adc_measurements_0.s_r_sck_max_count[3]
@W: MO129 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\hdl\seq_controller.vhd":289:2:289:3|Sequential instance Stepper_Axis_0.seq_controller_0.state[1] reduced to a combinational gate by constant propagation
@W: MT246 :"e:\solutions_repo\motor control\development\mcsk\sk2ablslst10_bup\sk2ablsl10_5_0\component\work\mc_system_sb\ccc_0\mc_system_sb_ccc_0_fccc.vhd":110:4:110:11|Blackbox CCC is missing a user supplied timing model. This may have a negative effect on timing analysis and optimizations (Quality of Results) 

