F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(0): WARNING: net ** does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(34417): WARNING: net N_2969 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(34418): WARNING: net N_2970 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(34419): WARNING: net N_2971 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(34420): WARNING: net N_2972 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(34421): WARNING: net N_2973 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(34422): WARNING: net N_2974 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(35515): WARNING: net N_2978 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(35516): WARNING: net N_2979 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(36712): WARNING: net N_2980 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(36713): WARNING: net N_2981 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(36991): WARNING: net N_2982 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(36992): WARNING: net N_2983 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(37199): WARNING: net N_2984 does not have a driver (VDB-1002)

F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/synthesis/MC_System_top_1.vm(37200): WARNING: net N_2985 does not have a driver (VDB-1002)

Warning: CMPG4-007: Top level port DEVRST_N is not connected to any IO pad



===============================================================================.



Info: Global design data: 

      Total globals:                       2 

      Globals that cannot be demoted:      1 

      Globals considered for demotion:     1 





Info: List of globals that cannot be demoted: 

    CLK    ASYN   DATA   Instance Name 

    ---    ----   ----   ------------- 

    2289   0      0      'MC_System_0/MC_System_sb_0/CCC_0/GL0_INST' 



Info: List of globals considered for demotion: 

    CLK    ASYN   DATA   Instance Name 

    ---    ----   ----   ------------- 

    0      2288   19     'MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF' 



Info: Demotion information: 

      Disconnected 19 data pins from global 'MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF'. 

Info: CMPG4-302: Added 0 row global instances.

Info: CMPG4-303: Deleted 0 global instances.



===============================================================================.



Warning:   Your design contains a Fabric CCC block with the selected Lock Window setting too low when using the On-Chip 25/50 MHz RC oscillator as the reference clock. The PLL may not lock for 'MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP' instance. Select a Lock Window setting of '16000' ppm or higher in the PLL Options tab of the CCC block.

INFO: Reading User PDC file F:/SVN/MotorControl/Release/WebRelease/LiberoProjects/SK1ABLHL10/LiberoProject/SK1ABLHL10_5_1/constraint/io/MC_System_top.io.pdc. 0 error(s) and 0 warning(s)

