Design: MC_System_top
Fam: SmartFusion2
Die: PA4M1000_N
Pkg: fg484
Debug: 0
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[11] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[11] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[10] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[10] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[9] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[9] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[8] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[8] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[7] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[7] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[6] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[6] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[5] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[5] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[4] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[4] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[3] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[3] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[2] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[2] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[1] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[1] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PADDR[0] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[0] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[17] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[17] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[16] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[16] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[15] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[15] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[14] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[14] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[13] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[13] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[12] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[12] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[11] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[11] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[10] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[10] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[9] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[9] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[8] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[8] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[7] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[7] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[6] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[6] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[5] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[5] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[4] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[4] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[3] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[3] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[2] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[2] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[1] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[1] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWDATA[0] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WDATA[0] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PRDATA[19] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.ADC_SCALING_0_ia_adc_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.ADC_SCALING_0_ia_adc_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.ADC_SCALING_0_ia_adc_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.ADC_SCALING_0_ia_adc_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.FOC_TRANSFORMS_0_iq_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.RATE_LIMITER_0_rl_out_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.HALL_INTERFACE_1_omega_out_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.prdata_o_0_1_0[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.prdata_o_0_6[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_13[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_13[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_14[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_14[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_14[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_14[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_15[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_15[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_15[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_15[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_15[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_15[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_15[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_15[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_5[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_5[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_5[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_5[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_5[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_6[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_6[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_6[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_6[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_6[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_16[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_16_cZ[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_16[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_16_cZ[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_16[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_16_cZ[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_16[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_16_cZ[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_4[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_4[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_4[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_4[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_11[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_11_cZ[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_11[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_11_cZ[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_11[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_11_cZ[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_11[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_11_cZ[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_10[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_10_cZ[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_11[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_11_cZ[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_12[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_12_cZ[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_14[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_cZ[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_14[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_cZ[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_14[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_cZ[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_14[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_cZ[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_14[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_cZ[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_14[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_cZ[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_14[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_cZ[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_15[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_15_cZ[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_15[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_15_cZ[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_15[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_15_cZ[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_15[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_15_cZ[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_15[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_15_cZ[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_15[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_15_cZ[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_15[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_15_cZ[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_16[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_16_cZ[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_16[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_16_cZ[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_16[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_16_cZ[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_16[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_16_cZ[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_16[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_16_cZ[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_16[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_16_cZ[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_iv_16[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_16_cZ[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.prdata_o_1_0_iv_2[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PENABLE Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ENABLE Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PWRITE Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_WRITE Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_YNn Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0 Pin=YNn Type=GB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_YNn Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0 Pin=YNn Type=GB PkgPin= Port=
ProbePoint: Net=MC_System_0_AMBA_SLAVE_0_PSELx Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.READ_DECODE_PROC.prdata_o257 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o257 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.READ_DECODE_PROC.prdata_o262 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o262 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.READ_DECODE_PROC.prdata_o277 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o277 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.READ_DECODE_PROC.prdata_o265_1_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o257_1_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.READ_DECODE_PROC.prdata_o265 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o265 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.adc_channel_ch0_o_1_sqmuxa_8 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o257_2_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=A0_ADC_CS_O_c Inst=BLDC_HALL_Axis_0/adc_interface_0/s_slave_select Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=A0_ADC_SCK_O_c Inst=BLDC_HALL_Axis_0/adc_interface_0/sck_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=A0_ADC_SDO_O_c Inst=BLDC_HALL_Axis_0/adc_interface_0/sdo_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=A0_PWM_UH_O_c Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_AH_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=A0_PWM_VH_O_c Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_BH_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=A0_PWM_VL_O_c Inst=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC_un105_s_state_i_a3_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=A0_PWM_WH_O_c Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_CH_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=GPIO_0_M2F_c Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=I2C1_SDA_MGPIO0A_H2F_B Type=MSS PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.ADC_SCALING_0_ia_adc_o_m_out_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o257_1_1_0_RNI4NDC1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0.apb3_hall_if_0.HALL_INTERFACE_1_angle_out_raw_o_m_out Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o275_1_0_RNIKUFD1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PADDR[15] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[15] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PADDR[14] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[14] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PADDR[13] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[13] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PADDR[12] Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_ADDR[12] Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[31] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[17] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[16] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[15] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[14] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[13] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[12] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[11] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[10] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[9] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[8] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[7] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[6] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[5] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[4] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[3] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[2] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[1] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PRDATA[0] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_TMP_0_FIC_0_APB_MASTER_PSELx Inst=MC_System_0/MC_System_sb_0/MC_System_sb_MSS_0/MSS_ADLIB_INST/INST_MSS_010_IP Pin=F_HM0_SEL Type=MSS PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2_1[0] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/iPSELS_raw_0_a2_1_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[16] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[15] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[14] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[13] Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_N_4L5_Z Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_N_4L5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_N_7L13_Z Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_N_7L13 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_N_8L15_Z Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_N_8L15 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_N_9L19_Z Inst=MC_System_0/MC_System_sb_0/CoreAPB3_0/u_mux_p_to_b3/PRDATA_N_9L19 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/LOCK Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST/INST_CCC_IP Pin=LOCK Type=CCC PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_va_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/add_c_to_mas_o_1[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vb_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vb_output_o_axb_0_i_0_c Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/vc_output_o_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vc_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_va3h_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/va3h_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vb3h_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/vb3h_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_vc3h_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/vc3h_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_speedpi_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_init_iqpi_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_iqpi_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_out_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_omega_out_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/omega_out_o_1_cry_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_kp_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_speed_pi_ki_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_id_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_kp_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_idq_pi_ki_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_speed_pi_output_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iq_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_park_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_id_pi_output_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_0_iq_pi_output_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_cl_omega_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_auto_restart_no_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_auto_restart_no_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_auto_restart_no_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_auto_restart_no_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_config_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_config_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_config_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_seq_cntl_config_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_state_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/state_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_state_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/state_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_state_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/state_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_state_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/state_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_slew_cnt_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_rate_cnt_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_rate_limit_ref_in_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_period_val_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_gain_val_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Va_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vb_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_0_Vc_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_dead_time_val_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_pwm_delay_time_val_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_theta_factor_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_dv_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_theta_output_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_olmng_iq_ref_in_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/theta_o_cZ[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol_RNIJB1M[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol_RNIIA1M[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol_RNIH91M[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol_RNIG81M[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/OLMNG_0_theta_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol_RNIF71M[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_filter_factor_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_filter_factor_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_filter_factor_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_filter_factor_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_filter_factor_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_filter_factor_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_filter_factor_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_filter_factor_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_speed_factor_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_angle_out_raw_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/hall_sensor_pol_i_RNIOPV71 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_angle_out_raw_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_angle_out_raw_12_0__m4_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_angle_out_raw_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_angle_out_raw_12_0__m5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_angle_out_raw_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_angle_out_raw_12_0__m4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/HALL_INTERFACE_1_angle_out_raw_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_angle_out_raw_12_0__m1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ia_adc_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ia[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_ib_adc_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_ib[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ialpha_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ibeta_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ibeta[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_valpha_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_vbeta_o[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/yo_ipark_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_scale_val_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch0_o[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch1_o[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_oc_thresh_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_control_reg_val_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_control_reg_val_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_control_reg_val_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_control_reg_val_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_control_reg_val_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_control_reg_val_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch2_o[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_result_ch3_o[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch2_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch0_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch1_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_adc_channel_ch3_o[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_iclarke_done_o Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SVM_0_done_o Inst=BLDC_HALL_Axis_0/MSC_i_0/done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_motor_stopped_o Inst=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC_un105_s_state_i_a3_0_a3_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_cl_status_o Inst=BLDC_HALL_Axis_0/MSC_i_11/cl_status_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_en_idq_pi_o Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_o2_1_RNIQANQ[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/RATE_LIMITER_0_rl_done_o Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_1_iq_pi_done_o Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_pi_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_park_done_o Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/done_park_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SPEED_ID_IQ_PI_1_id_pi_done_o Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_pi_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_1_over_current_fault_o Inst=BLDC_HALL_Axis_0/MSC_i_19/over_current_fault_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_start_motor_o Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/start_motor_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_stop_motor_o Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/stop_motor_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_1_fault_clr_o Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_calib_done_o Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM3PH_0_midmatch_o Inst=BLDC_HALL_Axis_0/MSC_i_27/midmatch_o_c Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/PWM_SCALING_1_done_o Inst=BLDC_HALL_Axis_0/MSC_i_25/done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_1_adc_start_o Inst=BLDC_HALL_Axis_0/MSC_i_11/adc_start_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_reset_rl_o Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_rr_RNIBO351 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/SEQ_CONTROLLER_0_soft_stop_o Inst=BLDC_HALL_Axis_0/MSC_i_11/config_reg_i_RNI30RC[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/ADC_SCALING_0_done_o Inst=BLDC_HALL_Axis_0/MSC_i_19/done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_en_if_0_direction_config_o Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/direction_config_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0_hall_sensor_polarity_o Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_sensor_polarity_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_1_clarke_done_o_0 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/FOC_TRANSFORMS_0_ipark_done_o Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/done_ipark_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0_results_rdy_o Inst=BLDC_HALL_Axis_0/adc_interface_0/results_rdy_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[16] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[15] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[14] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[13] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[12] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[11] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[10] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[9] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[8] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[7] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[6] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[5] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[4] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[3] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[2] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[1] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[0] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[17] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[16] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[15] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[14] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[13] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[12] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[11] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[10] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[9] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[8] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[7] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[6] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[5] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[4] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[3] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[2] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[1] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[0] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[17] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[16] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[15] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[14] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[13] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[12] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[11] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[10] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[9] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[8] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[7] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[6] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[5] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[4] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[3] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[2] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i_a_4[1] Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[17] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[16] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[15] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[14] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[13] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[12] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[11] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[10] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[9] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[8] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[7] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[6] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[5] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[4] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[3] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[2] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[1] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s[0] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_cry[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[17] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[16] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[15] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[14] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[13] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[12] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[11] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[10] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[9] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[8] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[7] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[6] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[5] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[4] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[3] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[2] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[1] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_cry[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_s[0] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_delay_counter_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_Z[17] Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_283 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_284 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_285 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_286 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_287 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_288 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_289 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_290 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_291 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_292 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_293 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_294 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_295 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_296 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_297 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_298 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_299 Inst=BLDC_HALL_Axis_0/MSC_i_27/un1_dead_time_i_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_300 Inst=BLDC_HALL_Axis_0/MSC_i_27/s_midmatch Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_301 Inst=BLDC_HALL_Axis_0/MSC_i_27/s_midmatch_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.un19_en_pwm_i Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_un19_en_pwm_i_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC.va_i Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC_va_i_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC.vb_i Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC_vb_i_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC.vc_i Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC_vc_i_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_307 Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC.pwm_ah_o2 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC_pwm_ah_o2_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC.pwm_bh_o2 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC_pwm_bh_o2_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC.pwm_ch_o2 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_OUTPUT_GEN_PROC_pwm_ch_o2_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un6_en_pwm_i Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un6_en_pwm_i_a_4_s_17_RNIIS8A5_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_315 Inst=BLDC_HALL_Axis_0/MSC_i_27/s_pwm_counter_s_RNO[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_435 Inst=BLDC_HALL_Axis_0/MSC_i_27/s_midmatch_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_436 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_BH_o_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_437 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_AH_o_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_438 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_CH_o_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un12_en_pwm_i_3_Z Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un12_en_pwm_i_3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un12_en_pwm_i_9_Z Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un12_en_pwm_i_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un12_en_pwm_i_11_Z Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un12_en_pwm_i_11 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un12_en_pwm_i_12_Z Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un12_en_pwm_i_12 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un12_en_pwm_i_14_Z Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un12_en_pwm_i_14 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC.op_eq.un12_en_pwm_i_15_Z Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_MIDMATCH_GEN_PROC_op_eq_un12_en_pwm_i_15 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_480 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_AH_o_2_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_481 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_BH_o_2_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_482 Inst=BLDC_HALL_Axis_0/MSC_i_27/PWM_CH_o_2_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_27/MSC_net_483 Inst=BLDC_HALL_Axis_0/MSC_i_27/s_midmatch_2_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_max_value[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_state[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/s_state_ns[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/s_state_ns_0_a2[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_min_value_5_3_ns_1[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_min_value_5_3_ns_1[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[17] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[16] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[15] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[14] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[13] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[12] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[11] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[10] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[9] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[8] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[7] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[6] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[5] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[4] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[3] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[2] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[1] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.s_max_value_4_3_ns_1[0] Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_s_max_value_4_3_ns_1[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_273 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_274 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_275 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_276 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_277 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_278 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_279 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_280 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_281 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_282 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_283 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_284 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_285 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_286 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_287 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_288 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_289 Inst=BLDC_HALL_Axis_0/MSC_i_0/un2_s_v3h_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_292 Inst=BLDC_HALL_Axis_0/MSC_i_0/s_cmp_ab_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_293 Inst=BLDC_HALL_Axis_0/MSC_i_0/s_cmp_bc_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_294 Inst=BLDC_HALL_Axis_0/MSC_i_0/s_cmp_ca_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_295 Inst=BLDC_HALL_Axis_0/MSC_i_0/s_min_value[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/MSC_net_418 Inst=BLDC_HALL_Axis_0/MSC_i_0/s_state_RNIM0BA1[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vc3h_o_2_axb_0_i_0_Z Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vc3h_o_2_axb_0_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.vb3h_o_2_axb_0_i_0_Z Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_vb3h_o_2_axb_0_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC.va3h_o_2_axb_0_i_0_Z Inst=BLDC_HALL_Axis_0/MSC_i_0/SVM_FSM_PROC_va3h_o_2_axb_0_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[17] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mult0_in[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[25] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[25] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[24] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[24] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[23] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[23] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[22] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[22] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[21] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[21] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[20] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[20] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[19] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[19] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[18] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[18] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[17] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[17] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[16] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[15] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[14] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[13] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[12] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[11] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[10] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[9] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_product[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[8] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[30] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[29] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[28] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[27] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[26] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[25] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[24] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[23] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[22] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[21] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[20] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[19] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[18] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[17] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[30] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[29] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[28] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[27] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[26] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[25] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[24] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[23] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[22] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[21] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[20] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[19] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[18] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[17] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_state[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__m8_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3_RNILBQT Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[17] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_16_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs1_cry_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[17] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_16_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/inf_abs0_cry_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[5] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[4] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[3] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[2] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[1] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_s[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/s_calib_cnt_cry[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[16] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_230 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[15] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_229 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[14] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_228 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[13] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_227 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[12] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_226 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[11] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_225 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[10] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_224 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[9] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_223 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[8] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_222 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[7] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_221 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_0[6] Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_220 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_353 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__un1_s_ia_0_sqmuxa_0_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_354 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch0_offset_RNIJJH41[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_355 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_1_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_356 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_2_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_357 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_3_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_358 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_4_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_359 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_5_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_360 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_6_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_361 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_7_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_362 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_8_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_363 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_9_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_364 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_10_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_365 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_11_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_366 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__un1_s_state_3_0_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_367 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_368 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_369 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_370 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_371 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_372 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_373 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_374 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_375 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_376 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_377 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_378 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_379 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_380 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_381 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_382 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_383 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_384 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_18 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_385 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_19 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_386 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_20 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_387 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_21 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_388 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_22 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_389 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_23 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_390 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_24 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_391 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_25 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_392 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_26 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_393 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_27 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_394 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_28 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_395 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_29 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_396 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_s_30 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_397 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_398 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_399 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_400 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_401 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_402 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_403 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_404 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_405 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_406 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_407 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_408 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_409 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_410 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_411 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_412 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_413 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_414 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_18 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_415 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_19 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_416 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_20 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_417 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_21 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_418 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_22 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_419 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_23 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_420 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_24 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_421 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_25 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_422 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_26 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_423 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_27 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_424 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_28 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_425 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_29 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_426 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_s_30 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_427 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_mas_en Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_429 Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/mas_done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_431 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_adc_ch1_offset_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/OVER_CURRENT_FAULT_DET_PROC.un1_fault_threshold_i Inst=BLDC_HALL_Axis_0/MSC_i_19/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/OVER_CURRENT_FAULT_DET_PROC.un1_fault_threshold_i_1 Inst=BLDC_HALL_Axis_0/MSC_i_19/OVER_CURRENT_FAULT_DET_PROC_un1_fault_threshold_i_1_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/OVER_CURRENT_FAULT_DET_PROC.over_current_fault_o2 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__OVER_CURRENT_FAULT_DET_PROC_over_current_fault_o2_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_439 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__s_ib_0_sqmuxa_0_a3_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_440 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__s_ia_0_sqmuxa_0_a3_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_441 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__s_mas_en_1_sqmuxa_1_0_a3_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_476 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__m6_0_o2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_569 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_570 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_571 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_572 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_573 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_574 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_575 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_576 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_577 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_578 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_579 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_580 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_581 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_582 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_583 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_584 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_585 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_586 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_588 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_590 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_592 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_594 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_596 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_598 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_600 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_7 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_602 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_8 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_604 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_606 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_10 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_608 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_11 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_615 Inst=BLDC_HALL_Axis_0/MSC_i_19/s_state_ns_1_0__N_448_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_616 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_axb_0_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_762 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch0_offset_cry_0 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_795 Inst=BLDC_HALL_Axis_0/MSC_i_19/un3_s_adc_ch1_offset_cry_0 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_net_814 Inst=BLDC_HALL_Axis_0/MSC_i_19/un1_s_mult0_in_1_cry_0_231 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/s_mas_done_dly[0] Inst=BLDC_HALL_Axis_0/MSC_i_19/MSC_i_20/s_mas_done_dly[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult0_input[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mult1_input[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[30] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[29] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[28] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[27] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[26] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[25] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[24] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[23] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[22] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[21] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[20] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[19] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[18] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_addc_input[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[30] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[30] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[29] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[29] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[28] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[28] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[27] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[27] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[26] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[26] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[25] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[25] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[24] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[24] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[23] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[23] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[22] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[22] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[21] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[21] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[20] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[20] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[19] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[19] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[18] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[18] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[17] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[16] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[15] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[14] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_product[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[13] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_buff[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_theta_ol[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_state[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_state_d[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_state_s0_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/s_state_ns[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/s_state_ns_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIAVOD1_S[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIAVOD1[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_RNO[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIJUS9D[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNI9KQOC[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNI0BO7C[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIO2MMB[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIHRJ5B[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIBLHKA[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNI6GF3A[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNI2CDI9[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNI6HEL8[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIBNFO7[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIHUGR6[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIO6IU5[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNI0GJ15[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNI9QK44[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIJ5M73[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/init_speedpi_o_5[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/iq_ref_in_i_RNIUHNA2[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_344 Inst=BLDC_HALL_Axis_0/MSC_i_12/s_olmng_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_345 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_346 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_347 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_348 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_349 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_350 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_351 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_352 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_353 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_354 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_355 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_356 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_357 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_358 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_359 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_360 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_361 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_362 Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mas_en Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_363 Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/mas_done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_402 Inst=BLDC_HALL_Axis_0/MSC_i_12/un1_init_speedpi_o18_tz_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_403 Inst=BLDC_HALL_Axis_0/MSC_i_12/un1_init_speedpi_o18_tz_10 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_404 Inst=BLDC_HALL_Axis_0/MSC_i_12/un1_init_speedpi_o18_tz_11 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_405 Inst=BLDC_HALL_Axis_0/MSC_i_12/un1_init_speedpi_o18_tz_12 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_406 Inst=BLDC_HALL_Axis_0/MSC_i_12/un1_init_speedpi_o18_tz_15 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_407 Inst=BLDC_HALL_Axis_0/MSC_i_12/s_mas_en_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_408 Inst=BLDC_HALL_Axis_0/MSC_i_12/s_state_RNO[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_429 Inst=BLDC_HALL_Axis_0/MSC_i_12/un3_init_iqpi_o_cry_0 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_net_431 Inst=BLDC_HALL_Axis_0/MSC_i_12/un1_init_speedpi_o18_tz_10_RNINDQG Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/s_mas_done_dly[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_14/s_mas_done_dly[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[17] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[16] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[15] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[14] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[13] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[12] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[11] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[10] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[9] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[8] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[7] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[6] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[5] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[4] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[3] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[2] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[1] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/theta_scl_buff_o_3[0] Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_theta_scl_buff_o_3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/MSC_net_59 Inst=BLDC_HALL_Axis_0/MSC_i_12/MSC_i_13/DELAY_PROC_un1_olmng_done_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ref_val_buf[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[18] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_present_state[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_present_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_present_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_present_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_present_state_ns[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_present_state_ns_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_set_ref_5[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.op_minus.un1_s_set_ref[18] Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_s_18 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[18] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNO[18] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIT51DM[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIGI45L[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNI408TJ[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIPEBLI[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIFUEDH[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNI6FI5G[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIU0MTE[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNINJPLD[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIH7TDC[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIJBK8B[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIMGB3A[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIQM2U8[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIVTPO7[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNI56HJ6[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNICF8E5[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIKPV84[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNIT4N33[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_s[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_RNI7HEU1[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/rate_count_i_i[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out20_cry_0_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/s_count_i[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_0_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_1 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_2 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_3 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_4 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_5 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_6 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_7 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_8 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_9 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_10 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_11 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_12 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_13 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_14 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_15 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_16 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count_17 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_cry_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_305 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_slew_count_i_s_18 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_s_ramp_out20_cry_18_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_set_ref_cry_18_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_count Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_un1_s_count_cry_18_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_314 Inst=BLDC_HALL_Axis_0/MSC_i_9/s_count_1_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_315 Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNIGRSG1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_370 Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_371 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out20 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_372 Inst=BLDC_HALL_Axis_0/MSC_i_9/s_rl_in_cry_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_1 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_2 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_3 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_4 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_5 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_6 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_7 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_8 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_9 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_10 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_11 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_12 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_13 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_14 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_15 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_16 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.un1_s_set_ref_17 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_cry_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_407 Inst=BLDC_HALL_Axis_0/MSC_i_9/un2_s_rate_count_minus_s_18 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_1 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_2 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_3 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_4 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_5 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_6 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_7 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_8 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_9 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_10 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_11 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_12 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_13 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_14 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_15 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_16 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC.s_ramp_out20_17 Inst=BLDC_HALL_Axis_0/MSC_i_9/FSM_RATE_LIM_PROC_op_minus_un1_s_set_ref_cry_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_479 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNI3IH71[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_480 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIFUFD2[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_481 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNISBEJ3[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_482 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIAQCP4[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_483 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIP9BV5[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_484 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNI9Q957[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_485 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIQB8B8[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_486 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNICU6H9[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_487 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIOH51B[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_488 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNI564HC[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_489 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNI15UQD[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_490 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIU4O4F[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_491 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIS5IEG[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_492 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIR7COH[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_493 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIRA62J[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_494 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNISE0CK[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_495 Inst=BLDC_HALL_Axis_0/MSC_i_9/un1_s_ramp_out_RNIUJQLL[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_496 Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_8_RNO[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_514 Inst=BLDC_HALL_Axis_0/MSC_i_9/s_ramp_out_3_sqmuxa_RNI6TPE1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_net_698 Inst=BLDC_HALL_Axis_0/MSC_i_9/reset_rl_i_RNIIU5P Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[17] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[16] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[15] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[14] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[13] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[12] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[11] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[10] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[9] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[8] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[7] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[6] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[5] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[4] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[3] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[2] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[1] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/rl_out_prev_o_3[0] Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_rl_out_prev_o_3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/MSC_net_59 Inst=BLDC_HALL_Axis_0/MSC_i_9/MSC_i_10/DELAY_PROC_un1_rl_done_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[43] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[42] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[41] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[40] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[39] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[38] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[37] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[36] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[35] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[34] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_out[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_output_y[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/PI_SCHEDULER_INST.s_pi_sel[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_pi_sel_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/PI_SCHEDULER_INST.s_pi_sel[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_pi_sel_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[43] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[42] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[41] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[40] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[39] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[38] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[37] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[36] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[35] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[34] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[30] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_acc_in[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/s_act_input[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/PI_SCHEDULER_INST.s_pi_sel_i_0[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_pi_sel_RNIPUHA[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_517 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/done_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_518 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/en_o Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_519 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_start_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/PI_SCHEDULER_INST.op_eq.un3_init_o Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/op_eq_un3_init_o Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_522 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_523 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_524 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_525 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_526 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_527 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_528 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_529 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_530 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_531 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_532 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_533 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_534 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_535 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_536 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_537 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_538 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_539 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/init_o_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_540 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_541 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_542 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_543 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_544 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_545 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_546 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_547 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_548 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_549 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_550 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_551 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_552 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_553 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_554 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_555 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_556 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ref_input_o_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_557 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_558 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_559 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_560 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_561 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_562 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_563 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_564 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_565 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_566 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_567 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_568 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_569 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_570 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_571 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_572 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_573 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_net_574 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/act_input_o_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIPN949[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIGEHJ8[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI97P28[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIRP1I7[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIFEA17[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI55JG6[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIMM866[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI79IL5[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIQTR45[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIFK5K4[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI6DF34[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIV7PI3[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIQ4323[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIERDH2[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI4KO02[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew_RNISE3G1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_i[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un12_s_piout_cry_16_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_i[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un12_s_piout_cry_0_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[43] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[42] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[41] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[40] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[39] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[38] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[37] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[36] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[35] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[34] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[43] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[42] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[41] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[40] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[39] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[38] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[37] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[36] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[35] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[34] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[43] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[42] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[41] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[40] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[39] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[38] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[37] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[36] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[35] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[34] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[33] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[32] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[31] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[30] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[29] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[28] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[27] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[26] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[25] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[24] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[23] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[22] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[21] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[20] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[19] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[18] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[17] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[16] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[15] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[14] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[13] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[12] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[11] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[10] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[9] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[8] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[7] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[6] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[5] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[4] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[3] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[2] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[1] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_product[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[0] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[43] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[42] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[41] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[40] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[39] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[38] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[37] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[36] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[35] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[34] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[43] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[42] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[41] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[40] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[39] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[38] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[37] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[36] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[35] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[34] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[43] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[42] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[41] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[40] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[39] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[38] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[37] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[36] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[35] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[34] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[30] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_add_cin_5[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_add_cin_5[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_16_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_15_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_14_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_13_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_12_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_11_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_10_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_9_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_8_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_7_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_6_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_5_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_4_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_3_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_2_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_i_init_ds_2[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_cry_1_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult0_input[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_16_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_15_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_14_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_13_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_12_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_11_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_10_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_9_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_8_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_7_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_6_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_5_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_4_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_3_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_2_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_cry_1_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[43] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[42] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[41] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[40] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[39] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[38] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[37] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[36] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[35] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[34] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[30] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_acc_out_o_3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_5[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state_ns[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state_ns[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew_RNI52LG_Y[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_inew_RNI52LG[16] Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIC6A11_S[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIC6A11[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNILCVH1_S[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNILCVH1[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI0LK22_S[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI0LK22[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI4NAJ2_S[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI4NAJ2[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIAR043_S[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIAR043[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNII1NK3_S[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNII1NK3[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIS9D54_S[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIS9D54[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI8K3M4_S[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI8K3M4[18] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIM0Q65_S[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIM0Q65[19] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIT6HN5_S[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIT6HN5[20] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI6F886_S[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI6F886[21] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIHPVO6_S[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIHPVO6[22] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIU5N97_S[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIU5N97[23] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI4CFQ7_S[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI4CFQ7[24] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNICK7B8_S[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNICK7B8[25] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIMUVR8_S[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIMUVR8[26] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI2BOC9_S[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI2BOC9[27] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIGPGT9_S[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIGPGT9[28] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI0A9EA_S[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI0A9EA[29] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI9K2VA_S[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI9K2VA[30] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIK0SFB_S[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIK0SFB[31] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI1FL0C_S[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI1FL0C[32] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIGVEHC_S[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIGVEHC[33] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIO992D_S[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIO992D[34] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI2M3JD_S[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI2M3JD[35] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIE4U3E_S[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIE4U3E[36] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNISKOKE_S[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNISKOKE[37] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIB6J5F_S[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIB6J5F[38] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIRODMF_S[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIRODMF[39] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI3497G_S[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI3497G[40] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNICG4OG_S[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNICG4OG[41] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIMTV8H_S[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNIMTV8H[42] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNICQMAI_S[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNICQMAI[43] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI1CRPH_S[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_RNI1CRPH[43] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_640 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_641 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_642 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_643 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_644 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_645 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_646 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_647 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_648 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_649 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_650 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_651 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_652 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_653 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_654 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_0_Z[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_655 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_i_0_0[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_0_639 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_piout_i_0[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_34_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_6_1_1[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mult1_input_RNO_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state_ns_i_0[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state_ns_i_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[42] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[41] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[40] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[39] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[38] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[37] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[36] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[35] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[34] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[30] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/acc_out_o_3_b_A[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_iout[43] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_872 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_16 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_874 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_acc_in_0_sqmuxa_0_a4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_876 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MAS_PI_INST_mas_done_o_RNIKUNB Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_877 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout_0_sqmuxa_0_a4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_878 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/un1_s_acc_in_0_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_879 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_pout[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_880 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_s_i_init_ds_2_axb_0_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_881 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_axb_0_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_882 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/output_y_o_1_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_883 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mas_en Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_884 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mas_en_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_885 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_mas_en_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_886 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/done_o_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_887 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/mas_done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_888 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_state_RNO[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_958 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/s_error_s_17_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1001 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_0_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1005 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_1_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1009 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_2_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1013 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_3_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1017 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_4_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1021 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_5_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1025 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_6_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1029 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_7_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1033 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_8_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1037 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_9_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1041 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_10_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1045 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_11_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1049 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_12_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1053 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_13_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1057 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_14_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1061 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_axb_15_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1066 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_17 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1115 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un1_ymax_i_cry_34_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_net_1220 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/PI_CONT_FSM_PROC_un12_s_piout_cry_34_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/s_mas_done_dly[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_22/MSC_i_23/s_mas_done_dly[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[43] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[42] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[41] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[40] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[39] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[38] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[37] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[36] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[35] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[34] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[43] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[42] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[41] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[40] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[39] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[38] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[37] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[36] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[35] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[34] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[30] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_4[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_ACC_IN_PROC_s_speed_pi_acc_in_4[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_pi_sel_dly[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_pi_sel_dly[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_pi_sel_dly[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_pi_sel_dly[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[43] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[42] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[41] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[40] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[39] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[38] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[37] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[36] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[35] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[34] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[43] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[43] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[42] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[42] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[41] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[41] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[40] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[40] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[39] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[39] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[38] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[38] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[37] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[37] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[36] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[36] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[35] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[35] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[34] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[34] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[33] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[32] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[31] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[30] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[29] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[28] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[27] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[26] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[25] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[24] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[23] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[22] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[21] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[20] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[19] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[18] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[17] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[16] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[15] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[14] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[13] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[12] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[11] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[10] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[9] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[8] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[7] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[6] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[5] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[4] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[3] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[2] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[1] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_5[0] Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_speed_pi_output_y_o_5[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_535 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_acc_in_1_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_537 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/PI_SEL_PROC_un2_iq_pi_start_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_538 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/PI_SEL_PROC_un1_id_pi_start_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_539 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/un1_speed_pi_start_i_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_540 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_iq_acc_in_1_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_541 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_id_acc_in_1_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_542 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/speed_pi_output_y_o_1_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_543 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/iq_pi_output_y_o_1_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_544 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/id_pi_output_y_o_1_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_545 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/ID_PI_DONE_PROC_op_eq_un19_clear_buffer_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_546 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/IQ_PI_DONE_PROC_op_eq_un11_clear_buffer_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_547 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/s_speed_pi_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_548 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/SPEED_PI_DONE_PROC_op_eq_un5_clear_buffer_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_549 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[37] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_550 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[38] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_551 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[39] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_552 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[40] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_553 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[41] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_554 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[42] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_555 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[43] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_556 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[36] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_557 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[35] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_558 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[34] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_559 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_560 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_561 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_562 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[30] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_563 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_564 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_565 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_566 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_567 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_568 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_569 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_570 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_571 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_572 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_573 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_574 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_575 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_576 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_577 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_578 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_579 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_580 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_581 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_582 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_583 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_584 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_585 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_586 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_587 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_588 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_589 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_590 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_591 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/MSC_net_592 Inst=BLDC_HALL_Axis_0/MSC_i_21/MSC_i_24/acc_in_o_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state[8] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state[5] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[12] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[11] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[10] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[9] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[8] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[5] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_a2[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_a2[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a2[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a2[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_a2[8] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_a2[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[17] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_16_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[16] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[15] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[14] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[13] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[12] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[11] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[10] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[9] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[8] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[5] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[17] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_16_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[16] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[15] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[14] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[13] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[12] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[11] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[10] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[9] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[8] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[5] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs0_cry_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[12] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNO[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[11] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNII4KQB[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[10] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNIMPBJA[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[9] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNIRF3C9[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[8] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNI8JDG8[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNIMNNK7[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNI5T1P6[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[5] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNIL3CT5[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNI6BM15[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNIOJ064[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNIBTAA3[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNIV7LE2[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_s[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_adctrig_count_RNIKJVI1[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[13] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[12] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[11] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[10] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[9] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[8] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[5] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[13] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNO[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[12] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNICLE93[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[11] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNI3PI33[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[10] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNIRTMT2[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[9] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNIK3RN2[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[8] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNILCCG2[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNINMT82[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNIQ1F12[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[5] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNIUD0Q1[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNI3RHI1[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNI993B1[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNIGOK31[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[1] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNIO86S[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_s[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_count_RNI1QNK[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2_6[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2_6[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2_7[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2_7[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2_8[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2_8[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2_9[2] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2_9[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_3_i_a3_1[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_3_i_a3_1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_3_i_a3_0_0[7] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_3_i_a3_0_0_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o3_0_i_a3_0[5] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o3_0_i_a3_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_1[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_1[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_0[6] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_0[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_0[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_2[4] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_2[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_2[3] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_2[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_1_1[0] Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_1_1[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_265 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_rr Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_266 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_267 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_start_motor_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_268 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_fault_clear_sync1 Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_270 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_fault_clear_sync Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC.adc_start_o_3 Inst=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC_adc_start_o_3_iv_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.un13_s_speed_ref_abs Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_un13_s_speed_ref_abs_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/EN_SPEED_PI_PROC.un110_s_state Inst=BLDC_HALL_Axis_0/MSC_i_11/EN_SPEED_PI_PROC_un110_s_state_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.un12_s_vq_i_abs Inst=BLDC_HALL_Axis_0/MSC_i_11/inf_abs1_cry_16_RNI7K2Q1_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/EN_SPEED_PI_PROC.un111_s_state Inst=BLDC_HALL_Axis_0/MSC_i_11/EN_SPEED_PI_PROC_un111_s_state_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un8_fault_i_NE_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un8_fault_i_1 Inst=BLDC_HALL_Axis_0/MSC_i_11/un1_s_restart_count_1_FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_338 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_3_i[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_339 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_340 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_i[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_341 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o3_0_i_o3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_342 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_o2_1[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_343 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_o2[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_344 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_3_i_o2_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_345 Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_346 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_RNI3VQE[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_347 Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_s_restart_count_4_i_o2[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_348 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_o2[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_349 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_o2[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_350 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_3_i_o2[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_351 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_o2_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_352 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o3_0_i_a3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_353 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_a3_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_354 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_3_i_a3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_355 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_0_a3_1[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_356 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_a2_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_357 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a3_3_2[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC.op_eq.un98_s_state_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC_op_eq_un98_s_state Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_359 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a3[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_360 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a2_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_361 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a3_0_1[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_362 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a3_2[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_363 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a3_2[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_364 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o2_0_a3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_397 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_i_tz[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_398 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_i_4_i_tz[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un8_fault_i_NE_0_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_op_eq_un8_fault_i_NE_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC.op_eq.un98_s_state_7_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC_op_eq_un98_s_state_7 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC.op_eq.un98_s_state_8_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC_op_eq_un98_s_state_8 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un6_s_soft_stop_9_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un6_s_soft_stop_10_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_10 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un6_s_soft_stop_11_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_11 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un6_s_soft_stop_12_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_12 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un6_s_soft_stop_14_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_14 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC.op_eq.un6_s_soft_stop_15_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/FSM_SEQ_CONTROLLER_PROC_op_eq_un6_s_soft_stop_15 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_408 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_ns_o3_0_i_o3_RNIS1LL[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_409 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_410 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_state_RNO[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_411 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_sensor_calib_rr_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_412 Inst=BLDC_HALL_Axis_0/MSC_i_11/state_o_RNO[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_413 Inst=BLDC_HALL_Axis_0/MSC_i_11/state_o_RNO[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_414 Inst=BLDC_HALL_Axis_0/MSC_i_11/state_o_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_415 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count_RNO[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_416 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count_RNO[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_417 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count_RNO[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_418 Inst=BLDC_HALL_Axis_0/MSC_i_11/s_restart_count_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC.op_eq.un98_s_state_1_Z Inst=BLDC_HALL_Axis_0/MSC_i_11/ADC_START_PROC_op_eq_un98_s_state_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_11/MSC_net_571 Inst=BLDC_HALL_Axis_0/MSC_i_11/calib_done_i_RNIA0AN Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_clarke[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_a_to_mas_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_b_from_clarke[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_cordic[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_mul_a_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_from_iclarke[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_b_from_iclarke[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_b_to_mas_o_1[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_a_to_mas[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_3_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_b_to_mas[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_b_to_mas_o_iv_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_b_to_mas[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_mul_b_from_iclarke_m_0_a2[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_b_to_mas[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_b_to_mas_o_iv_0_o2[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_mul_b_to_mas[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mul_b_to_mas_o_1_RNI5U1P[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[43] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI34MU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[26] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI23MU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[25] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI12MU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[24] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI01MU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[23] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVVLU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[22] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUULU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[21] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITTLU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[20] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISSLU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[19] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI44LU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[18] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI33LU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI22LU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI11LU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNI00LU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIVUKU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIUTKU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNITSKU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNISRKU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_add_c_to_mas[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_RNIRQKU[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[28] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[28] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[27] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[27] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[26] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[26] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[25] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[25] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[24] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[24] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[23] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[23] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[22] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[22] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[21] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[21] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[20] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[20] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[19] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[19] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[18] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[18] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[17] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[16] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[15] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[14] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[13] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[12] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[11] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[10] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/s_product_from_mas[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/MAS_PROC_op_mult_un3_product_o_muladd_0[29_0]/U0/INST_MACC_IP Pin=P[9] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MAS_SCHEDULER_INST.s_mas_sel[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MAS_SCHEDULER_INST.s_mas_sel[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/s_mas_sel_Z[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_net_518 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/mas_en_to_mas_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_net_519 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mas_done_to_cordic_o_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_net_520 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/mas_en_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_net_521 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mas_en_to_mas_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_net_522 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_3_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_net_523 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/mas_done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_net_526 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/start_park_i_i_0_c Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo_scale[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/x_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo_scale[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xi[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yi[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_xo[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_yo[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_313 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_park_o_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_315 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/xo_ipark_o_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_316 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_sel Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_317 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_start Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_318 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_319 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_320 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_321 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_322 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_323 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_324 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_325 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_326 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_327 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_328 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_329 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_330 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_331 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_332 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_333 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_334 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_335 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/s_theta_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_336 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/done_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_net_337 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/x_o_5[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_0[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNO[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_0[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i_0[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_7_iv_i[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3_1[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_16_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_15_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_14_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_13_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_12_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_11_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_10_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_9_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_8_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_7_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_6_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_5_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_4_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_3_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_2_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_1_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_c_9[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_0_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_theta_c3_1_i_0[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un4_s_theta_c_14_1_RNIVU3K Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_16_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_15_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_14_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_13_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_12_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_11_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_10_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_9_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_8_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_7_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_6_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_5_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_4_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_3_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_2_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_1_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_7[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_xi_rot_7_cry_0_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_theta_c3_i_0[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un4_s_theta_c_14_RNISQ9A1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_16_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_15_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_14_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_13_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_12_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_11_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_10_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_9_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_8_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_7_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_6_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_5_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_4_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_3_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_2_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_1_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_7[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_yi_rot_7_cry_0_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un4_s_theta_c[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un4_s_theta_c_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un4_s_theta_c[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un4_s_theta_c_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un4_s_theta_c[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un4_s_theta_c_3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/y_o_3[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un4_s_theta_c_1[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un4_s_theta_c_14_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_345 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_347 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_348 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_theta_i_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_349 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_350 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_351 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_s_theta_c_9_cry_0_0_cy Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_352 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_dir_rot_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_353 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/done_o_1_sqmuxa_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_434 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un9_s_index_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_437 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_440 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m11_ns Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_443 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m13 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_446 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m16 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_449 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m19_ns Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_452 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m21 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_455 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m25 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_458 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m27_ns Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_461 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m29 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_464 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m30 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_467 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m32 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_470 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m34_ns Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_574 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVHRG[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_576 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIVGTS[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_578 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI0HV81[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_580 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI2I1L1[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_582 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5K312[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_584 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI9N5D2[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_586 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIER7P2[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_588 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK0A53[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_590 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR6CH3[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_592 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3EET3[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_594 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIJ1QH4[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_596 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI4M565[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_598 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIMBHQ5[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_600 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92TE6[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_602 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNITP837[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_604 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIIKN7[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_605 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV6C09[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_607 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8C0C8[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_608 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIEMF61[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_609 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNINIB67[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_610 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIPM4K2[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_611 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIMCB1_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_612 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI9NRS[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_613 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIEICB1[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_614 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_615 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un4_s_theta_c_14 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_616 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIDGKS[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_617 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNISRF21[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_618 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIHUVR1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_619 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV5O43[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_620 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI5P7J[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_621 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIP5LF1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_622 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIJG861[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_623 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI3A9P1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_624 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m11_ns_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_625 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI7R7J[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_626 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m19_ns_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_627 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m27_ns_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_628 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/FSM_CORDIC_ROT_PROC_un4_s_theta_c_14_1_RNIPURO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_629 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_630 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_631 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_632 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_633 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_634 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_635 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_636 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_637 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_638 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_639 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_640 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_641 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_642 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_643 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_644 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_645 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_646 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_647 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_648 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_649 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_x_o_5_2[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_650 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_651 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_652 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_653 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_654 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_655 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_656 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_657 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_658 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_659 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_660 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_661 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_662 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/OUTPUT_PROC_y_o_3_1_1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_663 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNID6O81[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_664 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFO0J[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_665 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI70O81[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_666 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI3SN81[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_667 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI7G0J[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_668 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIBK0J[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_669 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI92O81[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_670 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5UN81[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_671 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIFDT9[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_672 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIFV4O[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_673 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHFT9[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_674 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIQEE01[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_675 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNISVEE[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_676 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIH15O[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_677 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIB9T9[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_678 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI7N4O[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_679 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_680 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m28 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_681 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m22 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_682 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m24 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_683 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un5_s_theta_c_11_0__m31 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_684 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIGTVR1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_685 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNICPVR1[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_686 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIA7861_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_687 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIOA5T[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_688 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIEB861[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_689 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIA7861[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_690 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIGD861[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_691 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIC9861[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_692 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIERVR1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_693 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIANVR1[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_694 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKOCB1[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_695 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIGKCB1[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_696 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIOA5T_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_697 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNII45T[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_698 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIIMCB1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_699 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_700 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_701 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_702 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_703 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_704 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_705 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_706 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_707 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_708 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_709 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_710 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_711 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_712 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_713 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI5T1M1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_714 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI89NK1[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_715 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNII8KB1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_716 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNICHAQ1[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_717 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI8DAQ1[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_718 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIVF271[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_719 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIMJ861[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_720 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIC1VA1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_721 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIV59P1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_722 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_723 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIK10S1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_724 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI96IB2[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_725 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIR1O43[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_726 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIFLN43[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_727 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI46ES2[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_728 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIE7RB2[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_729 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI8HPM2[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_730 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO_2[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_731 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNIG6SA4[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_732 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_733 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNI940O3[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_734 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_735 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_736 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_737 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIRV5H4[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_738 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_739 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI4HRQ2[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_740 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_741 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNID8HC2[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_742 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_743 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIKVD83[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_744 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_745 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIHFBK4[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_746 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_747 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI4KL25[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_748 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_749 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIU4097[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_750 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_751 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI4FUF4[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_752 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_753 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIAGD07[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_754 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIPFRG6[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_755 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNI0DRQ2[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_756 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_xout_RNO[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_757 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNINQQ72[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_758 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_xi_rot_RNIV36H4[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_759 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_760 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_index_RNI8V1U6[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_761 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/un1_s_yout_RNO[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/MSC_net_762 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_7/s_yi_rot_RNIOGPI3[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_120 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/un1_s_state_1_i_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_122 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/y_o_0_sqmuxa_i_i_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_123 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_272_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_124 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNI1VN8[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_125 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_0_261_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_126 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_1_250_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_127 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_2_239_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_128 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_3_228_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_129 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_4_217_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_130 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_5_206_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_131 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_6_195_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_132 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_7_184_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_133 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_8_173_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_134 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_9_162_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_135 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_10_151_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_136 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_11_140_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_137 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_12_129_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_138 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_13_118_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_139 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_14_107_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_140 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_15_96_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_141 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_mul_a_o_5_16_85_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_142 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/un1_s_state_3_i_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_143 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/CORDIC_SCALE_FSM_PROC_mas_en_o_6_0_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/MSC_net_144 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_5/MSC_i_6/s_state_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_122 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_0_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_124 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_ialpha_0_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_125 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_126 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_127 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_128 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_129 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_130 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_131 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_132 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_133 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_134 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_135 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_136 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_137 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_0 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_138 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_139 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_140 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_141 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_142 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/un9_mul_a_to_mas_o_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_143 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/clarke_done_o_1_sqmuxa_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/MSC_net_144 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_3/s_state_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[17] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[16] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[15] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[14] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[13] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[12] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[11] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[10] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[9] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[8] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[7] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[6] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[5] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[4] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[3] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[2] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[1] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_vc[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/MSC_net_154 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_0_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/MSC_net_156 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/mul_a_to_mas_o_0_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/MSC_net_157 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/iclarke_done_o_1_sqmuxa_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/MSC_net_158 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_2/s_state_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_128 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MAS_SEL_PROC_un2_start_iclarke_i_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_129 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/un1_start_clarke_i_1_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_131 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/un1_start_clarke_i_2_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_132 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_133 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_134 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_135 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_136 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_137 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_138 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_139 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_140 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_141 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_142 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_143 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_144 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1_i_m2[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_145 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1_i_m2[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_146 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1_i_m2[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_147 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1_i_m2[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_148 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1_i_m2[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_149 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mas_en_to_mas_o_1_i_m2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/MSC_net_150 Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_8/mul_a_to_mas_o_1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0] Inst=BLDC_HALL_Axis_0/MSC_i_1/MSC_i_4/s_mas_done_dly[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt_5[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/CHANNEL_CNT_PROC_s_channel_cnt_5[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt_5[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/CHANNEL_CNT_PROC_s_channel_cnt_5[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt_5[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/CHANNEL_CNT_PROC_s_channel_cnt_5[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_chnls_4_samp[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_chnls_4_samp[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_chnls_4_samp[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_chnls_4_samp[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_chnls_4_samp[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_chnls_4_samp[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_sel[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_sel[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_sel[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_sel[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_sel[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_sel[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[15] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[14] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[13] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[12] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[15] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[14] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[13] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[12] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_data_4[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_CLOLLECTION_PROC_s_r_adc_data_4[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[15] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[14] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[13] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[12] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[15] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[14] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[13] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[12] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_ns[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/next_state[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/next_state_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns_i_m4[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/next_state_i_0[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/next_state_0_i[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_max_count[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_max_count[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_cry[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_cry[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_cry[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_cry[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_cry[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_cry[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_s[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_clock_count_cry[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[15] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[14] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[13] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[12] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_bm[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_bm[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[15] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[14] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[13] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[12] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_am[0] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_am[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns_a3_1[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns_a3_1[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[15] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[14] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[13] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[12] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[11] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[10] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[9] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[8] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[7] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[6] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[5] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[4] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[3] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[2] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0[1] Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_n2_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_n2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_counte Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns_o4_RNINP6U[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_n3_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_n3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_n4_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_n4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/N_1595_i_0 Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_n1_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_n1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_0_sqmuxa_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o_1_sqmuxa Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch1_o_1_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o_0_sqmuxa Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch0_o_0_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o_1_sqmuxa Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch2_o_1_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o_1_sqmuxa Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o_1_sqmuxa_0_a2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_1_sqmuxa_3_i_0 Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_1_sqmuxa_3_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_start_sig_ext_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_start_sig_ext Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/un13_s_r_adc_results_ready Inst=BLDC_HALL_Axis_0/adc_interface_0/START_SIG_PROC_un13_s_r_adc_results_ready_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_adc_sdi_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_adc_sdi Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/N_154_i_0 Inst=BLDC_HALL_Axis_0/adc_interface_0/s_adc_sdi_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/N_173_i_0 Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_enable_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_enable Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/adc_sdo_dly_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/adc_sdo_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_slave_select_2 Inst=BLDC_HALL_Axis_0/adc_interface_0/SS_GEN_PROC_s_slave_select_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_10 Inst=BLDC_HALL_Axis_0/adc_interface_0/SCK_GEN_PROC_s_r_sck_10_7_ns Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_results_ready_1_sqmuxa_1 Inst=BLDC_HALL_Axis_0/adc_interface_0/next_state_0_a3_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/un13_s_r_sck Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns_o4[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_10_7_am_1_1 Inst=BLDC_HALL_Axis_0/adc_interface_0/SCK_GEN_PROC_s_r_sck_10_7_am_1_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_10_7_am Inst=BLDC_HALL_Axis_0/adc_interface_0/SCK_GEN_PROC_s_r_sck_10_7_am Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_10_7_bm_1_1 Inst=BLDC_HALL_Axis_0/adc_interface_0/SCK_GEN_PROC_s_r_sck_10_7_bm_1_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_10_7_bm Inst=BLDC_HALL_Axis_0/adc_interface_0/SCK_GEN_PROC_s_r_sck_10_7_bm Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_sm2 Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14s2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_0_sqmuxa_1_1_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_0_sqmuxa_1_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/un1_s_r_sck Inst=BLDC_HALL_Axis_0/adc_interface_0/ADC_FSM_NS_PROC_un1_s_r_sck Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt_0_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt_0_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o_1_sqmuxa_0_a2_0_3_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o_1_sqmuxa_0_a2_0_3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o_1_sqmuxa_0_a2_0_2_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o_1_sqmuxa_0_a2_0_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/un10_s_start_sig_ext_0_a3_2 Inst=BLDC_HALL_Axis_0/adc_interface_0/SS_GEN_PROC_un10_s_start_sig_ext_0_a3_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_c2_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_sck_count_c2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/N_188 Inst=BLDC_HALL_Axis_0/adc_interface_0/present_state_ns_a3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/un1_s_sdo_2_sqmuxa_tz_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/un1_s_sdo_2_sqmuxa_tz Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_14_m0s2 Inst=BLDC_HALL_Axis_0/adc_interface_0/DATA_TRANSMIT_PROC_s_sdo_14_m0s2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_3_sqmuxa_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/s_sdo_3_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/N_1605 Inst=BLDC_HALL_Axis_0/adc_interface_0/result_ch3_o_1_sqmuxa_0_a2_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/CO1 Inst=BLDC_HALL_Axis_0/adc_interface_0/ADC_FSM_NS_PROC_un22_s_r_sck_1_CO1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/un1_s_sdo_1_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/adc_interface_0/un1_s_sdo_1_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/un22_s_r_sck Inst=BLDC_HALL_Axis_0/adc_interface_0/ADC_FSM_NS_PROC_un22_s_r_sck_1_CO2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_results_ready_0_sqmuxa_1 Inst=BLDC_HALL_Axis_0/adc_interface_0/s_r_adc_results_ready_0_sqmuxa_1_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/adc_interface_0/CO0 Inst=BLDC_HALL_Axis_0/adc_interface_0/s_channel_cnt_0_sqmuxa_1_RNIME6D3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[17] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[16] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[15] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[14] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[13] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[12] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[11] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[10] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[9] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[8] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[7] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[6] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[5] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[4] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[3] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[2] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[1] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[0] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mult_in0[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[33] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[33] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[32] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[32] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[31] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[31] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[30] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[30] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[29] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[29] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[28] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[28] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[27] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[27] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[26] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[26] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[25] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[25] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[24] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[24] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[23] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[23] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[22] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[22] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[21] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[21] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[20] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[20] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[19] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[19] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[18] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[18] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[17] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[17] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_product[16] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/MAS_PROC_op_mult_un3_product_o_muladd_0[35_0]/U0/INST_MACC_IP Pin=P[16] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_state[4] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_state[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_state[3] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_state[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_state[2] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_state[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_state[1] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_state[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/s_state_ns[1] Inst=BLDC_HALL_Axis_0/MSC_i_25/s_state_ns[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[17] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[16] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[15] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[14] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[13] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[12] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[11] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[10] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[9] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[8] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[7] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[6] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[5] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[4] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[3] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[2] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[1] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC.s_mult_in0_5[0] Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_252 Inst=BLDC_HALL_Axis_0/MSC_i_25/un1_s_mas_en_0_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_253 Inst=BLDC_HALL_Axis_0/MSC_i_25/s_mas_en Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_255 Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/mas_done_o_Z Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_262 Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_0_sqmuxa_i_o3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_263 Inst=BLDC_HALL_Axis_0/MSC_i_25/Vb_o_0_sqmuxa_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_264 Inst=BLDC_HALL_Axis_0/MSC_i_25/Va_o_0_sqmuxa_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_265 Inst=BLDC_HALL_Axis_0/MSC_i_25/un1_s_state_3_0_a3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_266 Inst=BLDC_HALL_Axis_0/MSC_i_25/s_state_ns_i_o3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_267 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_268 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_269 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_270 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_271 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_272 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_273 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_274 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_275 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_276 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_277 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_278 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_279 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_280 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_281 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_282 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_283 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_284 Inst=BLDC_HALL_Axis_0/MSC_i_25/MUL_INP_GEN_PROC_s_mult_in0_5_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_285 Inst=BLDC_HALL_Axis_0/MSC_i_25/s_state_RNO[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_286 Inst=BLDC_HALL_Axis_0/MSC_i_25/done_o_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_net_287 Inst=BLDC_HALL_Axis_0/MSC_i_25/Vc_o_0_sqmuxa_i_o3_i Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/s_mas_done_dly[0] Inst=BLDC_HALL_Axis_0/MSC_i_25/MSC_i_26/s_mas_done_dly[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[33] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[32] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[31] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[30] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[29] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[28] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[27] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[26] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[25] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[24] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[23] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[22] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[21] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[20] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[19] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[18] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_out[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_out_scale[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/un14_0_iv[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/un14_0_iv[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/un14_0_iv[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/un14_0_iv[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[25] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[25] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[24] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[24] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[23] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[23] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[22] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[22] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[21] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[21] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[20] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[20] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[19] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[19] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[18] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[18] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[17] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[16] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[15] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[14] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[13] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[12] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[11] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[10] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[9] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_result[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_18/MAS_PROC_op_mult_un3_product_o_mulonly_0[35_0]/U0/INST_MACC_IP Pin=P[8] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[33] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[32] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[31] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[30] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[29] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[28] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[27] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[26] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[25] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[24] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[23] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[22] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[21] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[20] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[19] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[18] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_filter_val_prev[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[33] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[26] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[25] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[24] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[23] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[22] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[21] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[20] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[19] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[18] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_omega_out[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/product_o_Z[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_buff[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_buff[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_count_buff[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_output[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly1[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly1[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly1[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly1[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly1[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly1[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly1[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_dly1[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[33] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[32] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[31] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[30] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[30] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[29] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[28] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[27] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[26] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[25] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[24] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[23] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[22] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[21] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[20] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[19] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[18] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC.s_filter_val_prev_3[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/FILTER_ACC_PROC_s_filter_val_prev_3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig_RNO[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_0_iv[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_0_iv[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_sig_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us_3[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us_3[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us_3[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_raw_m[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_RNO[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_angle_out_raw[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_angle_out_raw_12_0__m6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_11_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/op_abs.inf_abs0[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/op_abs_inf_abs0_cry_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_s_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNI5T0M1_S[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNI5T0M1[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIIGCS1_S[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIIGCS1[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNI05O22_S[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNI05O22[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIFQ392_S[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIFQ392[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIVGFF2_S[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIVGFF2[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIG8RL2_S[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIG8RL2[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNI217S2_S[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNI217S2[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNILQI23_S[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNILQI23[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNI9LU83_S[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNI9LU83[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIUGAF3_S[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIUGAF3[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIR58H3_S[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIR58H3[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIPR5J3_S[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIPR5J3[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIOI3L3_S[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIOI3L3[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIOA1N3_S[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIOA1N3[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIP3VO3_S[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIP3VO3[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIRTSQ3_S[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIRTSQ3[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIUOQS3_S[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNIUOQS3[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNO_S[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win_RNO[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_in_spd_win[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI8ITU_S[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI8ITU[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI8K5V_S[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI8K5V[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI9NDV_S[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI9NDV[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIBRLV_S[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIBRLV[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIE0UV_S[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIE0UV[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNII6601_S[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNII6601[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNINDE01_S[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNINDE01[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNITLM01_S[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNITLM01[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI4VU01_S[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI4VU01[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIC9711_S[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIC9711[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNISVF91_S[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNISVF91[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIDNOH1_S[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIDNOH1[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIVF1Q1_S[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIVF1Q1[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNII9A22_S[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNII9A22[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI64JA2_S[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNI64JA2[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIRVRI2_S[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIRVRI2[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIHS4R2_S[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle_RNIHS4R2[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_limit_angle_6_RNO_S[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_limit_angle_6_RNO[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_limit_angle[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[17] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[16] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[15] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[14] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[13] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[12] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[11] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[10] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[9] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[8] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[7] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[6] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[5] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[4] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[3] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[2] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[1] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_s[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_speed_count_cry[0] Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_iv_0[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_iv_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.s_speed_raw_sig_13_0_iv_0[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_s_speed_raw_sig_13_0_iv_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_i_0[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal_RNO[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_i_0[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal_RNO[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us_i_0[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_1us_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/un14_0_iv_0[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_0_0_504 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/un14_0_iv_1[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_0_0_505 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/un14_0_iv_2[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_0_0_506 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/un14_0_iv_3[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_0_0_507 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_733 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_734 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_2_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_735 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_3_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_736 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_737 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_5_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_738 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_739 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_7_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_740 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_741 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_9_0 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_742 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_743 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_744 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_s_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_745 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_calc_done_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_746 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_edge_det Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_748 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_ha_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_749 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hb_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_750 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_win_term_flag Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_751 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr_calc_done_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_752 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_roll_calc_done_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_753 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_win_term_flag_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_754 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_ha_dly1 Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_755 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hb_dly1 Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_756 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hc_dly1 Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_757 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hc_dly Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_758 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_dir Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.un5_s_spd_win_term_flag_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_un5_s_spd_win_term_flag Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_ROLL_PROC.un5_s_theta_incr_calc_done_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_ROLL_PROC_un5_s_theta_incr_calc_done Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_761 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_incr_calc_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC.un5_s_theta_roll_calc_done_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC_un5_s_theta_roll_calc_done Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_763 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_roll_calc_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN.un20_s_spd_win_term_flag_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/ANGLE_CNT_INCR_SIGNAL_DLY_GEN_un20_s_spd_win_term_flag Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/SPD_WINDOW_TIME_GEN.un1_s_spd_window_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/SPD_WINDOW_TIME_GEN_un1_s_spd_window Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_766 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_calc_done Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/EDGE_DETECT_PROC.s_hall_edge_det_1_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/EDGE_DETECT_PROC_s_hall_edge_det_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un22_s_trigger_1us Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un22_s_trigger_1us_cry_17_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/COUNT_TERM_PROC.op_eq.s_count_in_spd_win7 Inst=BLDC_HALL_Axis_0/MSC_i_15/COUNT_TERM_PROC_op_eq_s_count_in_spd_win7_0_I_9_FCINST1 Pin=CO Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un16_s_hall_edge_det Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_op_eq_un13_s_hall_edge_det_10_RNIJCQ81 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un25_s_trigger_1us Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un25_s_trigger_1uslto17 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/COUNT_TERM_PROC.un14_s_trigger_1us_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/COUNT_TERM_PROC_un14_s_trigger_1us Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/DIR_DETECT_PROC.un9_s_tmp5_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/DIR_DETECT_PROC_un9_s_tmp5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_774 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_hall_edge_det_RNISQRL1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_775 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_3_0_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_776 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_5_0_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_777 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_7_0_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_778 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_9_0_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_779 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_axb_11_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un25_s_trigger_1uslt7 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un25_s_trigger_1uslto6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un25_s_trigger_1uslt4 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un25_s_trigger_1uslto3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_count_output_6_iv_10_262_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_10_262 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_count_output_6_iv_6_298_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_6_298 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_count_output_6_iv_4_316_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_4_316 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.s_count_output_6_iv_1_343_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_1_343 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_803 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_3_325 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_804 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_0_352 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_805 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_806 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un18_s_trigger_1us_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un18_s_trigger_1us Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un19_s_trigger_1us_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un19_s_trigger_1us Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_809 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_theta_output_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_810 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_16_208 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_811 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_15_217 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_812 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_14_226 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_813 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_13_235 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_814 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_12_244 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_815 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_11_253 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_816 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_9_271 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_817 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_8_280 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_818 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_7_289 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_819 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_5_307 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_820 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_2_334 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_821 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_s_count_output_6_iv_361 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC.un20_s_theta_roll_calc_done_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC_un20_s_theta_roll_calc_done Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC.un14_s_theta_roll_calc_done_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC_un14_s_theta_roll_calc_done Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC.un9_s_theta_roll_calc_done Inst=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC_un9_s_theta_roll_calc_donelto17 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/EDGE_DETECT_PROC.s_hall_edge_det_1_4_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/EDGE_DETECT_PROC_s_hall_edge_det_1_4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_858 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_axb_4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_861 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_axb_6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_864 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_axb_8 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_867 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_axb_10 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_869 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_axb_11 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_883 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_884 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_885 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_886 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_887 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_888 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_889 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_890 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_891 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_892 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_893 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_894 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_895 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_896 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_897 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_898 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_899 Inst=BLDC_HALL_Axis_0/MSC_i_15/un5_s_count_output_s_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_950 Inst=BLDC_HALL_Axis_0/MSC_i_15/un2_s_count_1us_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_951 Inst=BLDC_HALL_Axis_0/MSC_i_15/un2_s_count_1us_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_952 Inst=BLDC_HALL_Axis_0/MSC_i_15/un2_s_count_1us_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_953 Inst=BLDC_HALL_Axis_0/MSC_i_15/un2_s_count_1us_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_954 Inst=BLDC_HALL_Axis_0/MSC_i_15/un2_s_count_1us_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_955 Inst=BLDC_HALL_Axis_0/MSC_i_15/un2_s_count_1us_s_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.op_eq.un13_s_hall_edge_det_9_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_op_eq_un13_s_hall_edge_det_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.op_eq.un13_s_hall_edge_det_10_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_op_eq_un13_s_hall_edge_det_10 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.op_eq.un13_s_hall_edge_det_11_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_op_eq_un13_s_hall_edge_det_11 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.op_eq.un13_s_hall_edge_det_12_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_op_eq_un13_s_hall_edge_det_12 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.op_eq.un13_s_hall_edge_det_15_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_op_eq_un13_s_hall_edge_det_15 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un25_s_trigger_1uslto16_4_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un25_s_trigger_1uslto16_4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un25_s_trigger_1uslto16_5_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un25_s_trigger_1uslto16_5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un25_s_trigger_1uslto16_7_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un25_s_trigger_1uslto16_7 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_969 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_dir_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC.un22_s_trigger_1us_i_0 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un22_s_trigger_1us_cry_17_RNIRIHB Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/SPD_WIN_PROC.un18_s_theta_roll_calc_done_i_0 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_spd_window_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_972 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal_RNO[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_973 Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_SMOOTHEN_PROC_un18_s_trigger_1us_RNILPG31 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_974 Inst=BLDC_HALL_Axis_0/MSC_i_15/s_count_terminal_RNO[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC.s_theta_incr_2_axb_0_i_0_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/THETA_INCR_PROC_s_theta_incr_2_axb_0_i_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/COUNT_1MS_PROC.s_count_1us7lto6_1_Z Inst=BLDC_HALL_Axis_0/MSC_i_15/COUNT_1MS_PROC_s_count_1us7lto6_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_1102 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_0_0_503 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_net_1117 Inst=BLDC_HALL_Axis_0/MSC_i_15/un1_s_angle_out_raw_1_cry_0_0 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/COUNT_1MS_PROC.s_count_1us7lto6_1_RNIPALF1_Y Inst=BLDC_HALL_Axis_0/MSC_i_15/COUNT_1MS_PROC_s_count_1us7lto6_1_RNIPALF1 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[32] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[32] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[31] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[31] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[30] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[30] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[29] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[29] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[28] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[28] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[27] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[27] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[26] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[26] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[25] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[25] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[24] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[24] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[23] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[23] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[22] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[22] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[21] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[21] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[20] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[20] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[19] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[19] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[18] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[18] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[17] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[16] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[15] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[14] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[13] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[12] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[11] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[10] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[9] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[8] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[7] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[6] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[5] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[4] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[3] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[2] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[1] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[33] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_s_33 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[32] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_32 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[31] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_31 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[30] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_30 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[29] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_29 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[28] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_28 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[27] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_27 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[26] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_26 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[25] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_25 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[24] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_24 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[23] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_23 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[22] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_22 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[21] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_21 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[20] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_20 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[19] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_19 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[18] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_18 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[15] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[14] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[13] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[12] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[11] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[10] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[9] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[8] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[7] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[6] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[5] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[4] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[3] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[2] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_2[1] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/FILTER_FSM_PROC_s_filter_incr_2_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_state[0] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_state[0] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_161 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_state_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_163 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr[33] Pin=Q Type=SEQ PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_164 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_28 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_165 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_29 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_166 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_30 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_167 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_31 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_168 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_32 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_169 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_s_33 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_170 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_13 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_171 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_14 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_172 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_15 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_173 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_16 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_174 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_17 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_175 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_18 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_176 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_19 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_177 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_20 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_178 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_21 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_179 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_22 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_180 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_23 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_181 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_24 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_182 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_25 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_183 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_26 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_184 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_27 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_185 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_0 Pin=Y Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_186 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_1 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_187 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_2 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_188 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_3 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_189 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_4 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_190 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_5 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_191 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_6 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_192 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_7 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_193 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_8 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_194 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_9 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_195 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_10 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_196 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_11 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_197 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_12 Pin=S Type=1BIT PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_200 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_0_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_201 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_0_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_202 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_0_RNO_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_205 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_1_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_206 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_1_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_207 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_1_RNO_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_210 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_2_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_211 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_2_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_214 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_3_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_215 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_3_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_216 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_3_RNO_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_219 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_4_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_220 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_4_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_223 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_5_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_224 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_5_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_227 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_6_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_228 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_axb_6_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_231 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_7_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_232 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_7_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_235 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_8_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_236 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_8_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_239 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_9_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_240 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_9_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_243 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_10_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_244 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_10_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_247 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_11_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_248 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_11_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_251 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_12_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_252 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_12_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_255 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_13_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_256 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_13_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_259 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_14_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_260 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_14_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_263 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_15_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_264 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_15_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_267 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_16_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_268 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_16_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_271 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_17_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_272 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_17_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_275 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_18_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_276 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_18_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_279 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_19_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_280 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_19_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_283 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_20_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_284 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_20_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_287 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_21_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_288 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_21_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_291 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_22_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_292 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_22_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_295 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_23_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_296 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_23_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_299 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_24_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_300 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_24_RNO_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_303 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_axb_25_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_306 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/m0_2_03_0_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_307 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIJ1LO1[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_308 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_26_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_311 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIETLO1[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_312 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_27_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_315 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI9PMO1[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_316 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_28_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_319 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI4LNO1[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_320 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_29_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_323 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIVGOO1[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_324 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIVL9S[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_327 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIS5O71[33] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_332 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNICS021[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_402 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI37AA1[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_403 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIMRRD1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_404 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI7BAA1[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_405 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI7HGO1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_406 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI5HIO1[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_407 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIFTKO1[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_408 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIRQLM[25] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_409 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIPMJM[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_410 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIVULM[27] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_411 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNITSLM[26] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_412 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIVSJM[18] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_413 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIHGLM[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_414 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNILKLM[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_415 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIQQMM[29] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_416 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNINONM[32] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_417 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNINMLM[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_418 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIPOLM[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_419 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIOMKM[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_420 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNITQJM[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_421 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIJILM[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_422 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIJKNM[30] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_423 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI11MM[28] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_424 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNINKJM[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_425 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIROJM[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_426 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNILMNM[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_427 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNILIJM[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_428 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIHEJM[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_429 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIJGJM[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_430 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIFCJM[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_431 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIRLGF[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_432 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNITNGF[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_433 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI622J[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_434 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIPJGF[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_435 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIJDGF[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_436 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIHBGF[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_437 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_0_RNO_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_438 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNILFGF[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_439 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNINHGF[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_440 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_1_RNO_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_441 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI3DGO1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_442 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIV8GO1[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_443 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIR4GO1[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_444 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIN0GO1[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_445 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNICKUK1[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_446 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI18DH1[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_447 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIBFAA1[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_448 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/un3_s_out_scale_cry_2_RNO_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_449 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIBPKO1[24] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_450 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI7LKO1[23] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_451 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI3HKO1[22] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_452 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIVCKO1[21] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_453 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIR8KO1[20] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_454 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNI0DJO1[19] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_455 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIALHO1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_456 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIFPGO1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/MSC_net_457 Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_16/s_filter_incr_RNIBLGO1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[27] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[23] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[26] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[22] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[25] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[21] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[24] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[20] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[23] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[19] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[22] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[18] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[21] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[17] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[20] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[16] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[19] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[15] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[18] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[14] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[17] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[13] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC.op_mult.un3_product_o[16] Inst=BLDC_HALL_Axis_0/MSC_i_15/MSC_i_17/MAS_PROC_op_mult_un3_product_o_mulonly_0[23_0]/U0/INST_MACC_IP Pin=P[12] Type=MATH PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_2[31] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_2_iv[31] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_valpha_o_m[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_0_RNO[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_valpha_o_m[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_10_RNO_1[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_vbeta_o_m[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_RNO_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_vbeta_o_m[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_10_RNO_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_0_5[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_0_5[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_1_0[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_1_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/ADC_SCALING_0_ia_adc_o_m_0[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_1_0_RNO[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/ADC_SCALING_0_ia_adc_o_m_0[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_1[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/ADC_SCALING_0_ia_adc_o_m_0[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0_RNO_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_ibeta_o_m[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_0_RNO_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_0[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_0[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_2[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_0[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_0[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_0[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_0[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14_RNO_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_9_RNO_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14_RNO_0[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14_RNO_0[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch2_o_m[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14_RNO_0[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_0[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_0[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_0[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO_0[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/HALL_INTERFACE_1_angle_out_raw_o_m_0[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0_RNO[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch1_o_m[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_9_0_RNO[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_0[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14_RNO[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_10_RNO_2[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14_RNO[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14_RNO[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_interface_0_result_ch0_o_m[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_14_RNO[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/ADC_SCALING_0_ib_adc_o_m[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_0_5_RNO[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_ialpha_o_m[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_5_RNO_2[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_id_o_m[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_5_RNO_1[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_id_o_m[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_13_RNO[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/FOC_TRANSFORMS_0_iq_o_m[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1_5_RNO_0[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/SPEED_ID_IQ_PI_0_speed_pi_output_o_m[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o266_0_RNIOT9L Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/SPEED_ID_IQ_PI_0_iq_pi_output_o_m[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_10_RNO[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/HALL_INTERFACE_1_angle_out_raw_o_m[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_14_RNO[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_13[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_8[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_7[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_6[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_5[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_4[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_3[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_2[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[12] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[12] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[11] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[11] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[10] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[10] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[9] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[9] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[8] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[8] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[7] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[7] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[6] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[6] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[5] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_iv_1[5] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_13[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_13[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_13[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_13[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_13[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_13[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_8[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_8[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_8[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_8[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_8[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_8[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_8[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_8[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_6[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_5[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_4[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_3[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_2[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[16] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[16] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[15] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[15] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[14] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[14] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[13] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[13] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[2] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[2] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[1] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[1] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[0] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_1[0] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_9_0[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_9_0[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_9[4] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_9[4] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_0_7[17] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_7[17] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_10[3] Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o_1_0_iv_10[3] Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_theta_factor_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_rate_cnt_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_slew_cnt_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o_0_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o_0_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_filter_factor_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_filter_factor_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch1_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_speed_factor_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/stop_motor_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/stop_motor_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/start_motor_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/start_motor_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_sensor_polarity_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_sensor_polarity_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/direction_config_o_1_sqmuxa_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/direction_config_o_1_sqmuxa Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o276 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o276 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_filter_factor_o_1_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_filter_factor_o_1_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o_1_sqmuxa_1_0_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o_1_sqmuxa_1_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_3 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o258_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o_1_sqmuxa_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o_1_sqmuxa_RNO Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_4 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o257_5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_iq_ref_in_o_1_sqmuxa_8 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o257_5_RNI31DT Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o269_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o269_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o274_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o274_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o257_1_1_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o257_1_1_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o276_2_0_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o276_2_0_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o275_1_0_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o275_1_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_5 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o_1_sqmuxa_6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/stop_motor_o_1_sqmuxa_5 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o_1_sqmuxa_6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o_0_sqmuxa_3 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o_1_sqmuxa_3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_5 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o258_5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/start_motor_o_1_sqmuxa_3 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o258_3 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_4_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o_1_sqmuxa_3 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o_1_sqmuxa_4 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o_1_sqmuxa_6 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o270_5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o_0_sqmuxa_6 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o274_5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o271_6 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o265_6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_5_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_5 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_6 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o_1_sqmuxa_6 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o_1_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/rate_limit_ref_in_o_1_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_0_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o_1_sqmuxa_0_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o_1_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o_1_sqmuxa_0_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_control_reg_val_o_1_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_sensor_polarity_o_1_sqmuxa_0_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/hall_sensor_polarity_o_1_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/direction_config_o_1_sqmuxa_0_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/direction_config_o_1_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o_1_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o_1_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o_1_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o_1_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o258_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o258_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o277_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o277_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o276_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o276_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o264_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o264_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o264_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o264_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o268_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o268_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o268_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o268_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o270_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o270_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o263_2 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o263_2 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o263_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o263_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o267_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o267_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o261_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o261_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o259_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o259_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o266_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o266_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o273_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o273_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o260_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o260_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o262_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o262_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o272_2_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o272_2_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o271_2_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o271_2_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o275_1_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o275_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o267_1_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o259_1_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_9_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_9_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o_1_sqmuxa_9 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/stop_motor_o_1_sqmuxa_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_cl_omega_o_1_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o262_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o260_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o271_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o271_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o271_3_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o270_3_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o266_1_0 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o258_1_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_delay_time_val_o_1_sqmuxa_8 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o264_2_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o_1_sqmuxa_8_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o_1_sqmuxa_8 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o_1_sqmuxa_9_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o_1_sqmuxa_8_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_oc_thresh_o_1_sqmuxa_8 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o_1_sqmuxa_9_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_dead_time_val_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o_1_sqmuxa_9_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/seq_cntl_config_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/start_motor_o_1_sqmuxa_8_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/start_motor_o_1_sqmuxa_8 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_gain_val_o_1_sqmuxa_9 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_scale_val_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o_0_sqmuxa_9 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/direction_config_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_8_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_8 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o_1_sqmuxa_8_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/pwm_period_val_o_1_sqmuxa_8 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_9_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o_1_sqmuxa_9_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/auto_restart_no_o_1_sqmuxa_9 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o_0_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_kp_o_0_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o_1_sqmuxa_1_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_kp_o_1_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o_1_sqmuxa_0_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/speed_pi_ki_o_1_sqmuxa_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o270 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o270 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o269 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o269 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o261 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o261 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o260 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o260 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o259 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o259 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o258 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o258 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o266 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o266 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o264 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o264 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o263 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o263 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_1 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch0_o_1_sqmuxa_1 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o267 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o267 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o268 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o268 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o273 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o273 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o274 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o274 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o271 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o271 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/prdata_o275 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/READ_DECODE_PROC_prdata_o275 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/stop_motor_o_1_sqmuxa_7 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch2_o_1_sqmuxa_7 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_7_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/idq_pi_ki_o_1_sqmuxa_7 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/olmng_dv_o_1_sqmuxa_7 Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/fault_clr_o_1_sqmuxa_7 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o_1_sqmuxa_1_0_Z Inst=BLDC_HALL_Axis_0/apb3_hall_if_0/adc_channel_ch3_o_1_sqmuxa_1_0 Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=ff_to_start_net Inst=flash_freeze_inst/INST_FLASH_FREEZE_IP Pin=FF_TO_START Type=G4C PkgPin= Port=
ProbePoint: Net=MC_System_0_FIC_0_LOCK Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=CFG0_GND_INST_NET Inst=CFG0_GND_INST Pin=Y Type=COMB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB0_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB0 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB0_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB0 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB1_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB1 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB1_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB1 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB2_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB2 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB2_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB2 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB3_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB3 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB3_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB3 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB4_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB4 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB4_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB4 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB5_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB5 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB5_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB5 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB6_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB6 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB6_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB6 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB7_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB7 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB8_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB8 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB9_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB9 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB10_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB10 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB10_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB10 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB11_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB11 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB11_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB11 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB12_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB12 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB12_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB12 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB13_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB13 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB13_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB13 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB14_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB14 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB14_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB14 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB15_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB15 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB15_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB15 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB16_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB16 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB16_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB16 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB17_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB17 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB17_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB17 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB18_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB18 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB18_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB18 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB19_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB19 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB19_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB19 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB20_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB20 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB20_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB20 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB21_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB21 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB21_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB21 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB22_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB22 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB23_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_RGB1_RGB23 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_YR Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB0_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB0 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB1_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB1 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB1_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB1 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB2_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB2 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB2_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB2 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB3_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB3 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB3_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB3 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB4_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB4 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB4_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB4 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB5_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB5 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB5_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB5 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB6_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB6 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB6_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB6 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB7_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB7 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB7_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB7 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB8_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB8 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB9_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB9 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB10_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB10 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB11_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB11 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB11_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB11 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB12_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB12 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB12_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB12 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB13_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB13 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB13_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB13 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB14_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB14 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB14_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB14 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB15_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB15 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB15_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB15 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB16_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB16 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB16_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB16 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB17_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB17 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB17_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB17 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB18_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB18 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB18_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB18 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB19_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB19 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB19_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB19 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB20_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB20 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB20_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB20 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB21_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB21 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB21_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB21 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB22_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB22 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB22_rgbl_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB22 Pin=YL Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB23_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB23 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB24_rgbr_net_1 Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_RGB1_RGB24 Pin=YR Type=RGB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0_YNn_GSouth Inst=MC_System_0/MC_System_sb_0/CCC_0/CCC_INST_RNI2QPF/U0 Pin=YSn Type=GB PkgPin= Port=
ProbePoint: Net=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0_YNn_GSouth Inst=MC_System_0/MC_System_sb_0/CCC_0/GL0_INST/U0 Pin=YSn Type=GB PkgPin= Port=
PkgPin: Id=1 Name=D5 Port= Status=2
PkgPin: Id=2 Name=C4 Port= Status=2
PkgPin: Id=3 Name=B3 Port= Status=2
PkgPin: Id=4 Name=C3 Port= Status=2
PkgPin: Id=5 Name=G6 Port= Status=2
PkgPin: Id=6 Name=G5 Port= Status=2
PkgPin: Id=7 Name=F6 Port=A0_PWM_UL_O Status=2
PkgPin: Id=8 Name=F5 Port= Status=2
PkgPin: Id=9 Name=D4 Port= Status=2
PkgPin: Id=10 Name=D3 Port= Status=2
PkgPin: Id=11 Name=A2 Port= Status=2
PkgPin: Id=12 Name=B2 Port= Status=2
PkgPin: Id=13 Name=E5 Port= Status=2
PkgPin: Id=14 Name=E4 Port=A0_PWM_UH_O Status=2
PkgPin: Id=15 Name=B1 Port= Status=2
PkgPin: Id=16 Name=C1 Port= Status=2
PkgPin: Id=17 Name=D2 Port= Status=2
PkgPin: Id=18 Name=D1 Port= Status=2
PkgPin: Id=19 Name=E2 Port= Status=2
PkgPin: Id=20 Name=E1 Port= Status=2
PkgPin: Id=21 Name=F4 Port= Status=2
PkgPin: Id=22 Name=F3 Port= Status=2
PkgPin: Id=23 Name=G7 Port=A0_PWM_WH_O Status=2
PkgPin: Id=24 Name=H7 Port=A0_PWM_VH_O Status=2
PkgPin: Id=25 Name=J6 Port=A0_PWM_WL_O Status=2
PkgPin: Id=27 Name=H5 Port= Status=2
PkgPin: Id=28 Name=H4 Port= Status=2
PkgPin: Id=29 Name=G1 Port= Status=2
PkgPin: Id=30 Name=H1 Port= Status=2
PkgPin: Id=31 Name=J4 Port= Status=2
PkgPin: Id=32 Name=J3 Port= Status=2
PkgPin: Id=33 Name=J2 Port= Status=2
PkgPin: Id=34 Name=J1 Port= Status=2
PkgPin: Id=35 Name=K7 Port=A0_PWM_VL_O Status=2
PkgPin: Id=36 Name=K6 Port= Status=2
PkgPin: Id=37 Name=K5 Port= Status=2
PkgPin: Id=38 Name=K4 Port= Status=2
PkgPin: Id=39 Name=L8 Port= Status=2
PkgPin: Id=40 Name=K8 Port= Status=2
PkgPin: Id=41 Name=L7 Port= Status=2
PkgPin: Id=42 Name=M7 Port= Status=2
PkgPin: Id=43 Name=K2 Port= Status=2
PkgPin: Id=44 Name=K1 Port= Status=2
PkgPin: Id=45 Name=L3 Port= Status=2
PkgPin: Id=46 Name=L2 Port= Status=2
PkgPin: Id=47 Name=L5 Port= Status=2
PkgPin: Id=48 Name=L4 Port= Status=2
PkgPin: Id=49 Name=M6 Port= Status=2
PkgPin: Id=50 Name=M5 Port= Status=2
PkgPin: Id=51 Name=N6 Port= Status=2
PkgPin: Id=52 Name=N5 Port= Status=2
PkgPin: Id=53 Name=M2 Port= Status=2
PkgPin: Id=54 Name=M3 Port= Status=2
PkgPin: Id=55 Name=N4 Port= Status=2
PkgPin: Id=56 Name=N3 Port= Status=2
PkgPin: Id=57 Name=M1 Port= Status=2
PkgPin: Id=58 Name=N1 Port= Status=2
PkgPin: Id=59 Name=P3 Port= Status=2
PkgPin: Id=60 Name=P4 Port= Status=2
PkgPin: Id=61 Name=P2 Port= Status=2
PkgPin: Id=62 Name=P1 Port= Status=2
PkgPin: Id=63 Name=M8 Port= Status=2
PkgPin: Id=64 Name=N8 Port= Status=2
PkgPin: Id=65 Name=P7 Port= Status=2
PkgPin: Id=66 Name=P6 Port= Status=2
PkgPin: Id=67 Name=R1 Port= Status=2
PkgPin: Id=68 Name=R2 Port= Status=2
PkgPin: Id=69 Name=R4 Port= Status=2
PkgPin: Id=70 Name=R3 Port= Status=2
PkgPin: Id=71 Name=T3 Port= Status=2
PkgPin: Id=72 Name=T4 Port= Status=2
PkgPin: Id=73 Name=T1 Port= Status=2
PkgPin: Id=74 Name=U1 Port= Status=2
PkgPin: Id=76 Name=U4 Port= Status=2
PkgPin: Id=77 Name=U3 Port= Status=2
PkgPin: Id=98 Name=W9 Port= Status=2
PkgPin: Id=99 Name=Y9 Port= Status=2
PkgPin: Id=102 Name=V11 Port= Status=2
PkgPin: Id=103 Name=W11 Port= Status=2
PkgPin: Id=104 Name=AB13 Port= Status=2
PkgPin: Id=105 Name=AB14 Port= Status=2
PkgPin: Id=106 Name=AA13 Port= Status=2
PkgPin: Id=107 Name=Y13 Port= Status=2
PkgPin: Id=108 Name=U13 Port= Status=2
PkgPin: Id=109 Name=T13 Port= Status=2
PkgPin: Id=110 Name=V13 Port= Status=2
PkgPin: Id=111 Name=V14 Port= Status=2
PkgPin: Id=112 Name=Y14 Port= Status=2
PkgPin: Id=113 Name=W14 Port= Status=2
PkgPin: Id=114 Name=AB15 Port= Status=2
PkgPin: Id=115 Name=AA15 Port= Status=2
PkgPin: Id=116 Name=Y15 Port= Status=2
PkgPin: Id=117 Name=W15 Port= Status=2
PkgPin: Id=118 Name=U14 Port= Status=2
PkgPin: Id=119 Name=U15 Port= Status=2
PkgPin: Id=120 Name=AB17 Port= Status=2
PkgPin: Id=121 Name=AA18 Port= Status=2
PkgPin: Id=122 Name=AA16 Port= Status=2
PkgPin: Id=123 Name=AA17 Port= Status=2
PkgPin: Id=124 Name=W16 Port= Status=2
PkgPin: Id=125 Name=V16 Port= Status=2
PkgPin: Id=126 Name=Y17 Port= Status=2
PkgPin: Id=127 Name=W17 Port= Status=2
PkgPin: Id=128 Name=Y18 Port= Status=2
PkgPin: Id=129 Name=Y19 Port= Status=2
PkgPin: Id=130 Name=AB18 Port=A0_RUNNING_LED Status=2
PkgPin: Id=131 Name=AB19 Port= Status=2
PkgPin: Id=144 Name=U19 Port= Status=2
PkgPin: Id=148 Name=T18 Port=USB_ULPI_STP Status=2
PkgPin: Id=157 Name=P18 Port= Status=2
PkgPin: Id=158 Name=R16 Port= Status=2
PkgPin: Id=159 Name=P16 Port= Status=2
PkgPin: Id=160 Name=N16 Port= Status=2
PkgPin: Id=161 Name=N17 Port= Status=2
PkgPin: Id=168 Name=P22 Port= Status=2
PkgPin: Id=169 Name=R22 Port= Status=2
PkgPin: Id=170 Name=N19 Port= Status=2
PkgPin: Id=171 Name=N20 Port= Status=2
PkgPin: Id=172 Name=N21 Port= Status=2
PkgPin: Id=173 Name=N22 Port= Status=2
PkgPin: Id=174 Name=M21 Port= Status=2
PkgPin: Id=175 Name=M22 Port= Status=2
PkgPin: Id=176 Name=L21 Port= Status=2
PkgPin: Id=177 Name=L20 Port= Status=2
PkgPin: Id=178 Name=L19 Port=GPIO_0_M2F Status=2
PkgPin: Id=179 Name=L18 Port= Status=2
PkgPin: Id=181 Name=K20 Port=A0_ADC_SDO_O Status=2
PkgPin: Id=184 Name=K17 Port= Status=2
PkgPin: Id=185 Name=K16 Port= Status=2
PkgPin: Id=186 Name=K18 Port= Status=2
PkgPin: Id=187 Name=J18 Port= Status=2
PkgPin: Id=188 Name=H20 Port= Status=2
PkgPin: Id=189 Name=H19 Port= Status=2
PkgPin: Id=190 Name=G19 Port= Status=2
PkgPin: Id=191 Name=G18 Port= Status=2
PkgPin: Id=192 Name=F21 Port=A0_ADC_SCK_O Status=2
PkgPin: Id=193 Name=F20 Port=A0_ADC_CS_O Status=2
PkgPin: Id=194 Name=F19 Port= Status=2
PkgPin: Id=195 Name=F18 Port= Status=2
PkgPin: Id=196 Name=E22 Port= Status=2
PkgPin: Id=197 Name=E21 Port= Status=2
PkgPin: Id=199 Name=D21 Port= Status=2
PkgPin: Id=200 Name=C22 Port= Status=2
PkgPin: Id=201 Name=B22 Port= Status=2
PkgPin: Id=202 Name=G17 Port= Status=2
PkgPin: Id=203 Name=G16 Port= Status=2
PkgPin: Id=210 Name=E18 Port= Status=2
PkgPin: Id=211 Name=D18 Port= Status=2
PkgPin: Id=212 Name=D20 Port= Status=2
PkgPin: Id=213 Name=E19 Port= Status=2
PkgPin: Id=214 Name=B21 Port= Status=2
PkgPin: Id=215 Name=A21 Port= Status=2
PkgPin: Id=216 Name=F17 Port= Status=2
PkgPin: Id=217 Name=E17 Port= Status=2
PkgPin: Id=218 Name=C19 Port= Status=2
PkgPin: Id=219 Name=C20 Port= Status=2
PkgPin: Id=220 Name=A20 Port= Status=2
PkgPin: Id=221 Name=B19 Port= Status=2
PkgPin: Id=222 Name=C18 Port= Status=2
PkgPin: Id=223 Name=C17 Port= Status=2
PkgPin: Id=224 Name=E16 Port= Status=2
PkgPin: Id=225 Name=D16 Port= Status=2
PkgPin: Id=226 Name=B17 Port= Status=2
PkgPin: Id=227 Name=C16 Port= Status=2
PkgPin: Id=228 Name=A19 Port= Status=2
PkgPin: Id=229 Name=A18 Port= Status=2
PkgPin: Id=230 Name=A17 Port= Status=2
PkgPin: Id=231 Name=A16 Port= Status=2
PkgPin: Id=232 Name=F15 Port= Status=2
PkgPin: Id=233 Name=E15 Port= Status=2
PkgPin: Id=234 Name=C15 Port= Status=2
PkgPin: Id=235 Name=B15 Port= Status=2
PkgPin: Id=236 Name=G14 Port= Status=2
PkgPin: Id=237 Name=F14 Port= Status=2
PkgPin: Id=238 Name=E13 Port= Status=2
PkgPin: Id=239 Name=D14 Port= Status=2
PkgPin: Id=240 Name=A15 Port= Status=2
PkgPin: Id=241 Name=A14 Port= Status=2
PkgPin: Id=242 Name=G13 Port= Status=2
PkgPin: Id=243 Name=G12 Port= Status=2
PkgPin: Id=244 Name=C13 Port= Status=2
PkgPin: Id=245 Name=B13 Port= Status=2
PkgPin: Id=246 Name=D13 Port= Status=2
PkgPin: Id=247 Name=D12 Port= Status=2
PkgPin: Id=248 Name=A13 Port= Status=2
PkgPin: Id=249 Name=A12 Port= Status=2
PkgPin: Id=250 Name=F12 Port= Status=2
PkgPin: Id=251 Name=E12 Port= Status=2
PkgPin: Id=252 Name=D11 Port= Status=2
PkgPin: Id=253 Name=D10 Port= Status=2
PkgPin: Id=254 Name=A11 Port= Status=2
PkgPin: Id=255 Name=A10 Port= Status=2
PkgPin: Id=256 Name=C11 Port= Status=2
PkgPin: Id=257 Name=B11 Port= Status=2
PkgPin: Id=258 Name=E10 Port= Status=2
PkgPin: Id=259 Name=F10 Port= Status=2
PkgPin: Id=260 Name=A9 Port= Status=2
PkgPin: Id=261 Name=B9 Port= Status=2
PkgPin: Id=262 Name=C9 Port= Status=2
PkgPin: Id=263 Name=D9 Port= Status=2
PkgPin: Id=264 Name=A8 Port= Status=2
PkgPin: Id=265 Name=A7 Port= Status=2
PkgPin: Id=266 Name=D8 Port= Status=2
PkgPin: Id=267 Name=E8 Port= Status=2
PkgPin: Id=268 Name=B7 Port= Status=2
PkgPin: Id=269 Name=C7 Port= Status=2
PkgPin: Id=271 Name=A6 Port= Status=2
PkgPin: Id=272 Name=B6 Port= Status=2
PkgPin: Id=273 Name=F8 Port= Status=2
PkgPin: Id=274 Name=E7 Port= Status=2
PkgPin: Id=275 Name=D6 Port= Status=2
PkgPin: Id=276 Name=C5 Port= Status=2
PkgPin: Id=277 Name=A5 Port= Status=2
PkgPin: Id=278 Name=B5 Port= Status=2
PkgPin: Id=279 Name=A3 Port= Status=2
PkgPin: Id=280 Name=A4 Port= Status=2
