# Microsemi Physical design constraints file

# Version: v11.8 SP2 11.8.2.4

# Design Name:  

# Input Netlist Format: EDIF 

# Family: SmartFusion2 , Die: M2S010 , Package: 484 FBGA , Speed grade: -1 

# Date generated: Wed Nov 29 15:56:54 2017 


#
# IO banks setting
#

set_iobank Bank1 -vcci 2.50 -fixed no
set_iobank Bank2 -vcci 2.50 -fixed no
set_iobank Bank4 -vcci 2.50 -fixed no
set_iobank Bank7 -vcci 2.50 -fixed no

#
# Local clock constraints
#


#
# Region constraints
#


#
# I/O constraints
#

set_io A0_ADC_CS_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname F20 -fixed yes
set_io A0_ADC_SCK_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname F21 -fixed yes
set_io A0_ADC_SDI_I -DIRECTION INPUT -pinname K21 -fixed yes
set_io A0_ADC_SDO_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname K20 -fixed yes
set_io A0_PWM_UH_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname E4 -fixed yes
set_io A0_PWM_UL_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname F6 -fixed yes
set_io A0_PWM_VH_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname H7 -fixed yes
set_io A0_PWM_VL_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname K7 -fixed yes
set_io A0_PWM_WH_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname G7 -fixed yes
set_io A0_PWM_WL_O -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname J6 -fixed yes
set_io A0_RUNNING_LED -DIRECTION OUTPUT -pinname AB18 -fixed yes
set_io GPIO_0_M2F -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname L19 -fixed yes
set_io GPIO_41 -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname K17 -fixed yes
set_io GPIO_43 -DIRECTION OUTPUT -OUT_DRIVE 12 -pinname F18 -fixed yes
set_io PPS -DIRECTION INPUT -RES_PULL Up -pinname AA16 -fixed yes
set_io TD -DIRECTION INPUT -RES_PULL Up -pinname AA17 -fixed yes
set_io USB_ULPI_DATA\[0\] -DIRECTION INOUT -pinname V22 -fixed yes
set_io USB_ULPI_DATA\[1\] -DIRECTION INOUT -pinname V21 -fixed yes
set_io USB_ULPI_DATA\[2\] -DIRECTION INOUT -pinname U22 -fixed yes
set_io USB_ULPI_DATA\[3\] -DIRECTION INOUT -pinname U21 -fixed yes
set_io USB_ULPI_DATA\[4\] -DIRECTION INOUT -pinname T20 -fixed yes
set_io USB_ULPI_DATA\[5\] -DIRECTION INOUT -pinname T21 -fixed yes
set_io USB_ULPI_DATA\[6\] -DIRECTION INOUT -pinname P17 -fixed yes
set_io USB_ULPI_DATA\[7\] -DIRECTION INOUT -pinname V19 -fixed yes
set_io USB_ULPI_DIR -DIRECTION INPUT -pinname R18 -fixed yes
set_io USB_ULPI_NXT -DIRECTION INPUT -pinname T19 -fixed yes
set_io USB_ULPI_STP -DIRECTION OUTPUT -pinname T18 -fixed yes
set_io USB_ULPI_XCLK -DIRECTION INPUT -pinname R17 -fixed yes

#
# Core cell constraints
#

