# Microsemi I/O Physical Design Constraints file
# Auto Generated User I/O Constraints file

# Version: v11.3 11.3.0.112
# Family: SmartFusion2 , Die: M2S010 , Package: 484 FBGA
# Date generated: Thu Oct 16 13:50:49 2014 


# 
# User Locked I/O Bank Settings
# 


# 
# Unlocked I/O Bank Settings
# The I/O Bank Settings can be locked by directly editing this file
# or by making changes in the I/O Attribute Editor
# 


# 
# User Locked I/O settings
# 

set_io A0_ADC_CS_O     \
    -pinname F20       \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_ADC_SCK_O    \
    -pinname F21       \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_ADC_SDI_I   \
    -pinname K21      \
    -fixed yes        \
    -DIRECTION INPUT


set_io A0_ADC_SDO_O    \
    -pinname K20       \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_PWM_UH_O     \
    -pinname E4        \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_PWM_UL_O     \
    -pinname F6        \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_PWM_VH_O     \
    -pinname H7        \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_PWM_VL_O     \
    -pinname K7        \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_PWM_WH_O     \
    -pinname G7        \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_PWM_WL_O     \
    -pinname J6        \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io A0_RUNNING_LED  \
    -pinname AB18      \
    -fixed yes         \
    -DIRECTION OUTPUT


set_io GPIO_0_M2F      \
    -pinname L19       \
    -fixed yes         \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io GPIO_41        \
    -pinname K17      \
    -fixed yes        \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io GPIO_43       \
    -pinname F18      \
    -fixed yes        \
    -OUT_DRIVE 12      \
    -DIRECTION OUTPUT


set_io PPS            \
    -pinname AA16     \
    -fixed yes        \
    -RES_PULL Up      \
    -DIRECTION INPUT

set_io TD             \
    -pinname AA17     \
    -fixed yes        \
    -RES_PULL Up      \
    -DIRECTION INPUT



# 
# Dedicated Peripheral I/O Settings
# 


# 
# Unlocked I/O settings
# The I/Os in this section are unplaced or placed but are not locked
# the other listed attributes have been applied
# 

