# Generated by Microsemi Libero SoC
# I/O physical design constraints file created from top ports of root module

# Version: v11.5 SP2 11.5.2.6
# Family: SmartFusion2 Die: M2S010 Package: 484 FBGA
# Date generated: Thu Jun 04 16:05:13 2015

# 
# I/O constraints
# 

set_io {GPIO_0_M2F}        \
	-direction Output

set_io {A0_PWM_UL_O}       \
	-direction Output

set_io {A0_PWM_UH_O}       \
	-direction Output

set_io {A0_PWM_WH_O}       \
	-direction Output

set_io {A0_PWM_WL_O}       \
	-direction Output

set_io {A0_ADC_SCK_O}      \
	-direction Output

set_io {A0_PWM_VL_O}       \
	-direction Output

set_io {A0_PWM_VH_O}       \
	-direction Output

set_io {A0_ADC_SDI_I}      \
	-direction Input

set_io {A0_ADC_CS_O}       \
	-direction Output

set_io {A0_ADC_SDO_O}      \
	-direction Output

set_io {A0_RUNNING_LED}    \
	-direction Output

set_io {USB_ULPI_DIR}      \
	-direction Input

set_io {USB_ULPI_NXT}      \
	-direction Input

set_io {USB_ULPI_STP}      \
	-direction Output

set_io {USB_ULPI_XCLK}     \
	-direction Input

set_io {DEVRST_N}          \
	-direction Input

set_io {A0_FAULT_CLR_I}    \
	-direction Input

set_io {USB_ULPI_DATA(7)} \
	-direction Inout

set_io {USB_ULPI_DATA(6)} \
	-direction Inout

set_io {USB_ULPI_DATA(5)} \
	-direction Inout

set_io {USB_ULPI_DATA(4)} \
	-direction Inout

set_io {USB_ULPI_DATA(3)} \
	-direction Inout

set_io {USB_ULPI_DATA(2)} \
	-direction Inout

set_io {USB_ULPI_DATA(1)} \
	-direction Inout

set_io {USB_ULPI_DATA(0)} \
	-direction Inout

set_io {A1_ADC_SCK_O}      \
	-direction Output

set_io {A1_PWM_VL_O}       \
	-direction Output

set_io {A1_PWM_VH_O}       \
	-direction Output

set_io {A1_ADC_CS_O}       \
	-direction Output

set_io {A1_PWM_WH_O}       \
	-direction Output

set_io {A1_PWM_UL_O}       \
	-direction Output

set_io {A1_ADC_SDO_O}      \
	-direction Output

set_io {A1_PWM_WL_O}       \
	-direction Output

set_io {A1_PWM_UH_O}       \
	-direction Output

set_io {A1_ADC_SDI_I}      \
	-direction Input

set_io {A1_RUNNING_LED}    \
	-direction Output
