@P:  Worst Slack : -0.647
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Estimated Frequency : 93.9 MHz
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Requested Frequency : 100.0 MHz
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Estimated Period : 10.647
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Requested Period : 10.000
@P:  MC_System_sb_CCC_0_FCCC|GL0_net_inferred_clock - Slack : -0.647
@P:  MC_System_sb_CCC_0_FCCC|GL1_net_inferred_clock - Estimated Frequency : 139.4 MHz
@P:  MC_System_sb_CCC_0_FCCC|GL1_net_inferred_clock - Requested Frequency : 100.0 MHz
@P:  MC_System_sb_CCC_0_FCCC|GL1_net_inferred_clock - Estimated Period : 7.174
@P:  MC_System_sb_CCC_0_FCCC|GL1_net_inferred_clock - Requested Period : 10.000
@P:  MC_System_sb_CCC_0_FCCC|GL1_net_inferred_clock - Slack : 2.826
@P:  System - Estimated Frequency : 1029.4 MHz
@P:  System - Requested Frequency : 100.0 MHz
@P:  System - Estimated Period : 0.971
@P:  System - Requested Period : 10.000
@P:  System - Slack : 9.029
@P: MC_System_top Part : m2s010fbga484-1
@P: MC_System_top Register bits  : 4578 
@P: MC_System_top DSP Blocks  : 12
@P: MC_System_top I/O primitives : 35
@P:  CPU Time : 0h:00m:29s
