

##### START OF TIMING REPORT #####[
# Timing Report written on Mon Apr 23 18:34:15 2012
#


Top view:               Voltage_Monitor
Operating conditions:   smartfusion.COMWC-2
Requested Frequency:    100.0 MHz
Wire load mode:         top
Wire load model:        smartfusion
Paths requested:        5
Constraint File(s):    
@N: MT320 |This timing report estimates place and route data. Please look at the place and route timing report for final timing.

@N: MT322 |Clock constraints cover only FF-to-FF paths associated with the clock.



Performance Summary 
*******************


Worst slack in design: NA




Clock Relationships
*******************

Clocks            |    rise  to  rise   |    fall  to  fall   |    rise  to  fall   |    fall  to  rise 
--------------------------------------------------------------------------------------------------------
Starting  Ending  |  constraint  slack  |  constraint  slack  |  constraint  slack  |  constraint  slack
--------------------------------------------------------------------------------------------------------
========================================================================================================
 Note: 'No paths' indicates there are no paths in the design for that pair of clock edges.
       'Diff grp' indicates that paths exist but the starting clock and ending clock are in different clock groups.



Interface Information 
*********************

No IO constraint found


##### END OF TIMING REPORT #####]

