Selecting top level module Voltage_Monitor
@N: CG364 :"F:\Microsemi\Libero_v9.1\Synopsys\synplify_E201009A-1\lib\proasic\smartfusion.v":2609:7:2609:13|Synthesizing module INBUF_A

@N: CG364 :"F:\Microsemi\Libero_v9.1\Synopsys\synplify_E201009A-1\lib\proasic\smartfusion.v":1133:7:1133:9|Synthesizing module GND

@N: CG364 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":37:7:37:16|Synthesizing module OUTBUF_MSS

@N: CG364 :"F:\Microsemi\Libero_v9.1\Synopsys\synplify_E201009A-1\lib\proasic\smartfusion.v":1814:7:1814:9|Synthesizing module VCC

@N: CG364 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\mss_tshell.v":1:7:1:13|Synthesizing module MSS_APB

@N: CG364 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":23:7:23:15|Synthesizing module INBUF_MSS

@N: CG364 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\Actel\SmartFusionMSS\MSS\2.5.106\mss_comps.v":151:7:151:13|Synthesizing module MSS_CCC

@N: CG364 :"F:\Microsemi\Libero_v9.1\Synopsys\synplify_E201009A-1\lib\proasic\smartfusion.v":2566:7:2566:11|Synthesizing module RCOSC

@N: CG364 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":5:7:5:47|Synthesizing module Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC

@N: CG364 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\Voltage_Monitor_MSS.v":5:7:5:25|Synthesizing module Voltage_Monitor_MSS

@N: CG364 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor\Voltage_Monitor.v":5:7:5:21|Synthesizing module Voltage_Monitor

@W: CL168 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor\Voltage_Monitor.v":34:8:34:10|Pruning instance GND - not in use ...

@W: CL168 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor\Voltage_Monitor.v":33:8:33:10|Pruning instance VCC - not in use ...

@W: CL157 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":62:7:62:18|*Output RCOSC_CLKOUT has undriven bits - a simulation mismatch is possible 
@W: CL157 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":63:7:63:20|*Output MAINXIN_CLKOUT has undriven bits - a simulation mismatch is possible 
@W: CL157 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":64:7:64:18|*Output LPXIN_CLKOUT has undriven bits - a simulation mismatch is possible 
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":36:7:36:10|Input CLKA is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":37:7:37:14|Input CLKA_PAD is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":38:7:38:15|Input CLKA_PADP is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":39:7:39:15|Input CLKA_PADN is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":40:7:40:10|Input CLKB is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":41:7:41:14|Input CLKB_PAD is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":42:7:42:15|Input CLKB_PADP is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":43:7:43:15|Input CLKB_PADN is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":44:7:44:10|Input CLKC is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":45:7:45:14|Input CLKC_PAD is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":46:7:46:15|Input CLKC_PADP is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":47:7:47:15|Input CLKC_PADN is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":48:7:48:13|Input MAINXIN is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":49:7:49:11|Input LPXIN is unused
@W: CL159 :"C:\SF_LiberoIAR_POTlevel_tutorial_DF\EVAL_KIT\POT_LED_Libero_IAR\Voltage_Monitor\component\work\Voltage_Monitor_MSS\MSS_CCC_0\Voltage_Monitor_MSS_tmp_MSS_CCC_0_MSS_CCC.v":50:7:50:13|Input MAC_CLK is unused
