;-----------------------------------------------------------------------------------
;	Definition of Peripheral I/O registers,
;	Interrupt/Exception vectors
;	for microcontroller Fusion2.
;	
;	This definition file can be used by the C-SPY debugger,
;	all flavours (simulator, emulator and ROM-monitor).
;
; IAP:						v1.0.116
; Timer:					v1.0.108
; Analog Conversion Engine: v1.0.108	
; System Registers: 		v1.0.122
; 
; SVN $Revision: 623 $
; SVN $Date: 2009-01-28 22:04:42 +0000 (Wed, 28 Jan 2009) $
;------------------------------------------------------------------------------------

;
; Start of SFR definition.
;
[Sfr]

;
;		UART_0
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "RBR"                   , "Memory", 0x40000000,        1, base=16

sfr = "THR"                   , "Memory", 0x40000000,        1, base=16

sfr = "DLR"                   , "Memory", 0x40000000,        1, base=16

sfr = "DMR"                   , "Memory", 0x40000004,        1, base=16

sfr = "IER"                   , "Memory", 0x40000004,        1, base=16
sfr = "IER.ERBFI"             , "Memory", 0x40000004,        1, base=16,    bitRange=0-0
sfr = "IER.ETBEI"             , "Memory", 0x40000004,        1, base=16,    bitRange=1-1
sfr = "IER.ELSI"              , "Memory", 0x40000004,        1, base=16,    bitRange=2-2
sfr = "IER.EDSSI"             , "Memory", 0x40000004,        1, base=16,    bitRange=3-3

sfr = "IIR"                   , "Memory", 0x40000008,        1, base=16
sfr = "IIR.IIR"               , "Memory", 0x40000008,        1, base=16,    bitRange=0-3
sfr = "IIR.Mode"              , "Memory", 0x40000008,        1, base=16,    bitRange=6-7

sfr = "FCR"                   , "Memory", 0x40000008,        1, base=16
sfr = "FCR.Bit0"              , "Memory", 0x40000008,        1, base=16,    bitRange=0-0
sfr = "FCR.Bit1"              , "Memory", 0x40000008,        1, base=16,    bitRange=1-1
sfr = "FCR.Bit2"              , "Memory", 0x40000008,        1, base=16,    bitRange=2-2
sfr = "FCR.Bit3"              , "Memory", 0x40000008,        1, base=16,    bitRange=3-3
sfr = "FCR.Bit6"              , "Memory", 0x40000008,        1, base=16,    bitRange=6-7

sfr = "LCR"                   , "Memory", 0x4000000C,        1, base=16
sfr = "LCR.WLS"               , "Memory", 0x4000000C,        1, base=16,    bitRange=0-1
sfr = "LCR.STB"               , "Memory", 0x4000000C,        1, base=16,    bitRange=2-2
sfr = "LCR.PEN"               , "Memory", 0x4000000C,        1, base=16,    bitRange=3-3
sfr = "LCR.EPS"               , "Memory", 0x4000000C,        1, base=16,    bitRange=4-4
sfr = "LCR.SP"                , "Memory", 0x4000000C,        1, base=16,    bitRange=5-5
sfr = "LCR.SB"                , "Memory", 0x4000000C,        1, base=16,    bitRange=6-6
sfr = "LCR.DLAB"              , "Memory", 0x4000000C,        1, base=16,    bitRange=7-7

sfr = "MCR"                   , "Memory", 0x40000010,        1, base=16
sfr = "MCR.DTR"               , "Memory", 0x40000010,        1, base=16,    bitRange=0-0
sfr = "MCR.RTS"               , "Memory", 0x40000010,        1, base=16,    bitRange=1-1
sfr = "MCR.Out1"              , "Memory", 0x40000010,        1, base=16,    bitRange=2-2
sfr = "MCR.Out2"              , "Memory", 0x40000010,        1, base=16,    bitRange=3-3
sfr = "MCR.Loop"              , "Memory", 0x40000010,        1, base=16,    bitRange=4-4

sfr = "LSR"                   , "Memory", 0x40000014,        1, base=16
sfr = "LSR.DR"                , "Memory", 0x40000014,        1, base=16,    bitRange=0-0
sfr = "LSR.OE"                , "Memory", 0x40000014,        1, base=16,    bitRange=1-1
sfr = "LSR.PE"                , "Memory", 0x40000014,        1, base=16,    bitRange=2-2
sfr = "LSR.FE"                , "Memory", 0x40000014,        1, base=16,    bitRange=3-3
sfr = "LSR.BI"                , "Memory", 0x40000014,        1, base=16,    bitRange=4-4
sfr = "LSR.THRE"              , "Memory", 0x40000014,        1, base=16,    bitRange=5-5
sfr = "LSR.TEMT"              , "Memory", 0x40000014,        1, base=16,    bitRange=6-6
sfr = "LSR.FIER"              , "Memory", 0x40000014,        1, base=16,    bitRange=7-7

sfr = "MSR"                   , "Memory", 0x40000018,        1, base=16
sfr = "MSR.DCTS"              , "Memory", 0x40000018,        1, base=16,    bitRange=0-0
sfr = "MSR.DDSR"              , "Memory", 0x40000018,        1, base=16,    bitRange=1-1
sfr = "MSR.TERI"              , "Memory", 0x40000018,        1, base=16,    bitRange=2-2
sfr = "MSR.DDCD"              , "Memory", 0x40000018,        1, base=16,    bitRange=3-3
sfr = "MSR.CTS"               , "Memory", 0x40000018,        1, base=16,    bitRange=4-4
sfr = "MSR.DSR"               , "Memory", 0x40000018,        1, base=16,    bitRange=5-5
sfr = "MSR.RI"                , "Memory", 0x40000018,        1, base=16,    bitRange=6-6
sfr = "MSR.DCD"               , "Memory", 0x40000018,        1, base=16,    bitRange=7-7

sfr = "SR"                    , "Memory", 0x4000001C,        1, base=16

;
;		SPI_0
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "SPI0_CONTROL"                        , "Memory", 0x40001000,        4, base=16
sfr = "SPI0_CONTROL.CTL_SPH"                , "Memory", 0x40001000,        4, base=16,    bitRange=25-25
sfr = "SPI0_CONTROL.CTL_SPO"                , "Memory", 0x40001000,        4, base=16,    bitRange=24-24
sfr = "SPI0_CONTROL.CTL_TXRXDFCOUNT"        , "Memory", 0x40001000,        4, base=16,    bitRange=8-23
sfr = "SPI0_CONTROL.INT_TXUR"               , "Memory", 0x40001000,        4, base=16,    bitRange=7-7
sfr = "SPI0_CONTROL.INT_RXOVF"              , "Memory", 0x40001000,        4, base=16,    bitRange=6-6
sfr = "SPI0_CONTROL.INT_TX"                 , "Memory", 0x40001000,        4, base=16,    bitRange=5-5
sfr = "SPI0_CONTROL.INT_RX"                 , "Memory", 0x40001000,        4, base=16,    bitRange=4-4
sfr = "SPI0_CONTROL.MODE"                   , "Memory", 0x40001000,        4, base=16,    bitRange=2-3
sfr = "SPI0_CONTROL.MASTER"                 , "Memory", 0x40001000,        4, base=16,    bitRange=1-1
sfr = "SPI0_CONTROL.ENABLE"                 , "Memory", 0x40001000,        4, base=16,    bitRange=0-0

sfr = "SPI0_TXRXDF_SIZE"                    , "Memory", 0x40001004,        4, base=16
sfr = "SPI0_TXRXDF_SIZE.TXRXDF_SIZE"        , "Memory", 0x40001004,        4, base=16,    bitRange=0-5

sfr = "SPI0_STATUS"                         , "Memory", 0x40001008,        4, base=16
sfr = "SPI0_STATUS.TX_FIFO_EMPTY_NEXT"   , "Memory", 0x40001008,        4, base=16,    bitRange=11-11
sfr = "SPI0_STATUS.TX_FIFO_EMPTY"        , "Memory", 0x40001008,        4, base=16,    bitRange=10-10
sfr = "SPI0_STATUS.TX_FIFO_FULL_NEXT"    , "Memory", 0x40001008,        4, base=16,    bitRange=9-9
sfr = "SPI0_STATUS.TX_FIFO_FULL"         , "Memory", 0x40001008,        4, base=16,    bitRange=8-8
sfr = "SPI0_STATUS.RX_FIFO_EMPTY_NEXT"   , "Memory", 0x40001008,        4, base=16,    bitRange=7-7
sfr = "SPI0_STATUS.RX_FIFO_EMPTY"        , "Memory", 0x40001008,        4, base=16,    bitRange=6-6
sfr = "SPI0_STATUS.RX_FIFO_FULL_NEXT"    , "Memory", 0x40001008,        4, base=16,    bitRange=5-5
sfr = "SPI0_STATUS.RX_FIFO_FULL"         , "Memory", 0x40001008,        4, base=16,    bitRange=4-4
sfr = "SPI0_STATUS.TX_CH_UV"                , "Memory", 0x40001008,        4, base=16,    bitRange=3-3
sfr = "SPI0_STATUS.RX_CH_OV"                , "Memory", 0x40001008,        4, base=16,    bitRange=2-2
sfr = "SPI0_STATUS.RX_RDY"                  , "Memory", 0x40001008,        4, base=16,    bitRange=1-1
sfr = "SPI0_STATUS.TX_DONE"                 , "Memory", 0x40001008,        4, base=16,    bitRange=0-0

sfr = "SPI0_INT_CLR"                        , "Memory", 0x4000100c,        4, base=16
sfr = "SPI0_INT_CLR.TX_CH_UV"               , "Memory", 0x4000100c,        4, base=16,    bitRange=3-3
sfr = "SPI0_INT_CLR.RX_CH_OV"               , "Memory", 0x4000100c,        4, base=16,    bitRange=2-2
sfr = "SPI0_INT_CLR.RX_RDY"                 , "Memory", 0x4000100c,        4, base=16,    bitRange=1-1
sfr = "SPI0_INT_CLR.TX_DONE"                , "Memory", 0x4000100c,        4, base=16,    bitRange=0-0

sfr = "SPI0_RX_DATA"                        , "Memory", 0x40001010,        4, base=16
sfr = "SPI0_RX_DATA.RX_DATA"                , "Memory", 0x40001010,        4, base=16,    bitRange=0-31

sfr = "SPI0_TX_DATA"                        , "Memory", 0x40001014,        4, base=16
sfr = "SPI0_TX_DATA.TX_DATA"                , "Memory", 0x40001014,        4, base=16,    bitRange=0-31

sfr = "SPI0_CLK_GEN"                        , "Memory", 0x40001018,        4, base=16
sfr = "SPI0_CLK_GEN.CLK_GEN"                , "Memory", 0x40001018,        4, base=16,    bitRange=0-3

sfr = "SPI0_SLAVE_SELECT"                   , "Memory", 0x4000101c,        4, base=16
sfr = "SPI0_SLAVE_SELECT.SLAVE_SELECT"      , "Memory", 0x4000101c,        4, base=16,    bitRange=0-7

sfr = "SPI0_MIS"                            , "Memory", 0x40001020,        4, base=16
sfr = "SPI0_MIS.TX_CH_UV"                   , "Memory", 0x40001020,        4, base=16,    bitRange=3-3
sfr = "SPI0_MIS.RX_CH_OV"                   , "Memory", 0x40001020,        4, base=16,    bitRange=2-2
sfr = "SPI0_MIS.RX_RDY"                     , "Memory", 0x40001020,        4, base=16,    bitRange=1-1
sfr = "SPI0_MIS.TX_DONE"                    , "Memory", 0x40001020,        4, base=16,    bitRange=0-0

sfr = "SPI0_RIS"                            , "Memory", 0x40001024,        4, base=16
sfr = "SPI0_RIS.TX_CH_UV"                   , "Memory", 0x40001024,        4, base=16,    bitRange=3-3
sfr = "SPI0_RIS.RX_CH_OV"                   , "Memory", 0x40001024,        4, base=16,    bitRange=2-2
sfr = "SPI0_RIS.RX_RDY"                     , "Memory", 0x40001024,        4, base=16,    bitRange=1-1
sfr = "SPI0_RIS.TX_DONE"                    , "Memory", 0x40001024,        4, base=16,    bitRange=0-0

;
;		I2C_0
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "CTRL"                  , "Memory", 0x40002000,        1, base=16
sfr = "CTRL.CR2"              , "Memory", 0x40002000,        1, base=16,    bitRange=7-7
sfr = "CTRL.ENS1"             , "Memory", 0x40002000,        1, base=16,    bitRange=6-6
sfr = "CTRL.STA"              , "Memory", 0x40002000,        1, base=16,    bitRange=5-5
sfr = "CTRL.STO"              , "Memory", 0x40002000,        1, base=16,    bitRange=4-4
sfr = "CTRL.SI"               , "Memory", 0x40002000,        1, base=16,    bitRange=3-3
sfr = "CTRL.AA"               , "Memory", 0x40002000,        1, base=16,    bitRange=2-2
sfr = "CTRL.CR1"              , "Memory", 0x40002000,        1, base=16,    bitRange=1-1
sfr = "CTRL.CR0"              , "Memory", 0x40002000,        1, base=16,    bitRange=0-0

sfr = "STAT"                  , "Memory", 0x40002004,        1, base=16
sfr = "STAT.STAT"             , "Memory", 0x40002004,        1, base=16,    bitRange=0-7

sfr = "DATA"                  , "Memory", 0x40002008,        1, base=16
sfr = "DATA.DATA"             , "Memory", 0x40002008,        1, base=16,    bitRange=0-7

sfr = "ADDR"                  , "Memory", 0x4000200C,        1, base=16
sfr = "ADDR.ADR"              , "Memory", 0x4000200C,        1, base=16,    bitRange=1-7
sfr = "ADDR.GC"               , "Memory", 0x4000200C,        1, base=16,    bitRange=0-0

sfr = "SMBUS"                 , "Memory", 0x40002010,        1, base=16
sfr = "SMBUS.smbus_reset"     , "Memory", 0x40002010,        1, base=16,    bitRange=7-7
sfr = "SMBUS.smbsus_no_control"   , "Memory", 0x40002010,        1, base=16,    bitRange=6-6
sfr = "SMBUS.smbsus_ni_status"   , "Memory", 0x40002010,        1, base=16,    bitRange=5-5
sfr = "SMBUS.smbalert_no_control"   , "Memory", 0x40002010,        1, base=16,    bitRange=4-4
sfr = "SMBUS.smbalert_ni_status"   , "Memory", 0x40002010,        1, base=16,    bitRange=3-3
sfr = "SMBUS.smbus_enable"   , "Memory", 0x40002010,        1, base=16,    bitRange=2-2
sfr = "SMBUS.smbsus_interrupt_enable"   , "Memory", 0x40002010,        1, base=16,    bitRange=1-1
sfr = "SMBUS.smbalert_interrupt_enable"   , "Memory", 0x40002010,        1, base=16,    bitRange=0-0

sfr = "FREQ"                  , "Memory", 0x40002014,        1, base=16
sfr = "FREQ.FREQ"             , "Memory", 0x40002014,        1, base=16,    bitRange=0-7

sfr = "GLITCHREG"             , "Memory", 0x40002018,        1, base=16
sfr = "GLITCHREG.GLITCHREG"   , "Memory", 0x40002018,        1, base=16,    bitRange=0-7

;
;		Ethernet MAC
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "CSR0"   , "Memory", 0x40003000,        4, base=16
sfr = "CSR0.SPEED"   , "Memory", 0x40003000,        4, base=16,    bitRange=21-21
sfr = "CSR0.DBO"   , "Memory", 0x40003000,        4, base=16,    bitRange=20-20
sfr = "CSR0.TAP"   , "Memory", 0x40003000,        4, base=16,    bitRange=17-19
sfr = "CSR0.PBL"   , "Memory", 0x40003000,        4, base=16,    bitRange=8-13
sfr = "CSR0.BLE"   , "Memory", 0x40003000,        4, base=16,    bitRange=7-7
sfr = "CSR0.DSL"   , "Memory", 0x40003000,        4, base=16,    bitRange=2-6
sfr = "CSR0.BAR"   , "Memory", 0x40003000,        4, base=16,    bitRange=1-1
sfr = "CSR0.SWR"   , "Memory", 0x40003000,        4, base=16,    bitRange=0-0

sfr = "CSR1"   , "Memory", 0x40003008,        4, base=16
sfr = "CSR1.TPD3"   , "Memory", 0x40003008,        4, base=16,    bitRange=24-31
sfr = "CSR1.TPD2"   , "Memory", 0x40003008,        4, base=16,    bitRange=16-23
sfr = "CSR1.TPD1"   , "Memory", 0x40003008,        4, base=16,    bitRange=8-15
sfr = "CSR1.TPD0"   , "Memory", 0x40003008,        4, base=16,    bitRange=0-7

sfr = "CSR2"   , "Memory", 0x40003010,        4, base=16
sfr = "CSR2.RPD3"   , "Memory", 0x40003010,        4, base=16,    bitRange=24-31
sfr = "CSR2.RPD2"   , "Memory", 0x40003010,        4, base=16,    bitRange=16-23
sfr = "CSR2.RPD1"   , "Memory", 0x40003010,        4, base=16,    bitRange=8-15
sfr = "CSR2.RPD0"   , "Memory", 0x40003010,        4, base=16,    bitRange=0-7

sfr = "CSR3"   , "Memory", 0x40003018,        4, base=16
sfr = "CSR3.RLA3"   , "Memory", 0x40003018,        4, base=16,    bitRange=24-31
sfr = "CSR3.RLA2"   , "Memory", 0x40003018,        4, base=16,    bitRange=16-23
sfr = "CSR3.RLA1"   , "Memory", 0x40003018,        4, base=16,    bitRange=8-15
sfr = "CSR3.RLA0"   , "Memory", 0x40003018,        4, base=16,    bitRange=0-7

sfr = "CSR4"   , "Memory", 0x40003020,        4, base=16
sfr = "CSR4.TLA3"   , "Memory", 0x40003020,        4, base=16,    bitRange=24-31
sfr = "CSR4.TLA2"   , "Memory", 0x40003020,        4, base=16,    bitRange=16-23
sfr = "CSR4.TLA1"   , "Memory", 0x40003020,        4, base=16,    bitRange=8-15
sfr = "CSR4.TLA0"   , "Memory", 0x40003020,        4, base=16,    bitRange=0-7

sfr = "CSR5"   , "Memory", 0x40003028,        4, base=16
sfr = "CSR5.TS"   , "Memory", 0x40003028,        4, base=16,    bitRange=20-22
sfr = "CSR5.RS"   , "Memory", 0x40003028,        4, base=16,    bitRange=17-18
sfr = "CSR5.NIS"   , "Memory", 0x40003028,        4, base=16,    bitRange=16-16
sfr = "CSR5.AIS"   , "Memory", 0x40003028,        4, base=16,    bitRange=15-15
sfr = "CSR5.ERI"   , "Memory", 0x40003028,        4, base=16,    bitRange=14-14
sfr = "CSR5.GTE"   , "Memory", 0x40003028,        4, base=16,    bitRange=11-11
sfr = "CSR5.ETI"   , "Memory", 0x40003028,        4, base=16,    bitRange=10-10
sfr = "CSR5.RPS"   , "Memory", 0x40003028,        4, base=16,    bitRange=8-8
sfr = "CSR5.RU"   , "Memory", 0x40003028,        4, base=16,    bitRange=7-7
sfr = "CSR5.RI"   , "Memory", 0x40003028,        4, base=16,    bitRange=6-6
sfr = "CSR5.UNF"   , "Memory", 0x40003028,        4, base=16,    bitRange=5-5
sfr = "CSR5.TU"   , "Memory", 0x40003028,        4, base=16,    bitRange=2-2
sfr = "CSR5.TPS"   , "Memory", 0x40003028,        4, base=16,    bitRange=1-1
sfr = "CSR5.TI"   , "Memory", 0x40003028,        4, base=16,    bitRange=0-0

sfr = "CSR6"   , "Memory", 0x40003030,        4, base=16
sfr = "CSR6.RA"   , "Memory", 0x40003030,        4, base=16,    bitRange=30-30
sfr = "CSR6.TTM"   , "Memory", 0x40003030,        4, base=16,    bitRange=22-22
sfr = "CSR6.SF"   , "Memory", 0x40003030,        4, base=16,    bitRange=21-21
sfr = "CSR6.TR"   , "Memory", 0x40003030,        4, base=16,    bitRange=14-15
sfr = "CSR6.ST"   , "Memory", 0x40003030,        4, base=16,    bitRange=13-13
sfr = "CSR6.FD"   , "Memory", 0x40003030,        4, base=16,    bitRange=9-9
sfr = "CSR6.PM"   , "Memory", 0x40003030,        4, base=16,    bitRange=7-7
sfr = "CSR6.PR"   , "Memory", 0x40003030,        4, base=16,    bitRange=6-6
sfr = "CSR6.IF"   , "Memory", 0x40003030,        4, base=16,    bitRange=4-4
sfr = "CSR6.PB"   , "Memory", 0x40003030,        4, base=16,    bitRange=3-3
sfr = "CSR6.HO"   , "Memory", 0x40003030,        4, base=16,    bitRange=2-2
sfr = "CSR6.SR"   , "Memory", 0x40003030,        4, base=16,    bitRange=1-1
sfr = "CSR6.HP"   , "Memory", 0x40003030,        4, base=16,    bitRange=0-0

sfr = "CSR7"   , "Memory", 0x40003038,        4, base=16
sfr = "CSR7.NIE"   , "Memory", 0x40003038,        4, base=16,    bitRange=16-16
sfr = "CSR7.AIE"   , "Memory", 0x40003038,        4, base=16,    bitRange=15-15
sfr = "CSR7.ERE"   , "Memory", 0x40003038,        4, base=16,    bitRange=14-14
sfr = "CSR7.GTE"   , "Memory", 0x40003038,        4, base=16,    bitRange=11-11
sfr = "CSR7.ETE"   , "Memory", 0x40003038,        4, base=16,    bitRange=10-10
sfr = "CSR7.RSE"   , "Memory", 0x40003038,        4, base=16,    bitRange=8-8
sfr = "CSR7.RUE"   , "Memory", 0x40003038,        4, base=16,    bitRange=7-7
sfr = "CSR7.RIE"   , "Memory", 0x40003038,        4, base=16,    bitRange=6-6
sfr = "CSR7.UNE"   , "Memory", 0x40003038,        4, base=16,    bitRange=5-5
sfr = "CSR7.TUE"   , "Memory", 0x40003038,        4, base=16,    bitRange=2-2
sfr = "CSR7.TSE"   , "Memory", 0x40003038,        4, base=16,    bitRange=1-1
sfr = "CSR7.TIE"   , "Memory", 0x40003038,        4, base=16,    bitRange=0-0

sfr = "CSR8"   , "Memory", 0x40003040,        4, base=16
sfr = "CSR8.OCO"   , "Memory", 0x40003040,        4, base=16,    bitRange=28-28
sfr = "CSR8.FOC"   , "Memory", 0x40003040,        4, base=16,    bitRange=17-27
sfr = "CSR8.MFO"   , "Memory", 0x40003040,        4, base=16,    bitRange=16-16
sfr = "CSR8.MFC"   , "Memory", 0x40003040,        4, base=16,    bitRange=0-15

sfr = "CSR9"   , "Memory", 0x40003048,        4, base=16
sfr = "CSR9.MDI"   , "Memory", 0x40003048,        4, base=16,    bitRange=19-19
sfr = "CSR9.MII"   , "Memory", 0x40003048,        4, base=16,    bitRange=18-18
sfr = "CSR9.MDO"   , "Memory", 0x40003048,        4, base=16,    bitRange=17-17
sfr = "CSR9.MDC"   , "Memory", 0x40003048,        4, base=16,    bitRange=16-16
sfr = "CSR9.SDO"   , "Memory", 0x40003048,        4, base=16,    bitRange=3-3
sfr = "CSR9.SDI"   , "Memory", 0x40003048,        4, base=16,    bitRange=2-2
sfr = "CSR9.SCLK"   , "Memory", 0x40003048,        4, base=16,    bitRange=1-1
sfr = "CSR9.SCS"   , "Memory", 0x40003048,        4, base=16,    bitRange=0-0

sfr = "CSR11"   , "Memory", 0x40003058,        4, base=16
sfr = "CSR11.CS"   , "Memory", 0x40003058,        4, base=16,    bitRange=31-31
sfr = "CSR11.TT"   , "Memory", 0x40003058,        4, base=16,    bitRange=27-30
sfr = "CSR11.NTP"   , "Memory", 0x40003058,        4, base=16,    bitRange=24-26
sfr = "CSR11.RT"   , "Memory", 0x40003058,        4, base=16,    bitRange=20-23
sfr = "CSR11.NRP"   , "Memory", 0x40003058,        4, base=16,    bitRange=17-19
sfr = "CSR11.CON"   , "Memory", 0x40003058,        4, base=16,    bitRange=16-16
sfr = "CSR11.TIM"   , "Memory", 0x40003058,        4, base=16,    bitRange=0-15


;
;		Peripheral DMA
;
;     Name                                Zone      Address     Bytesize  Displaybase Bitrange
;     ----                                ----      -------     --------  ----------- --------

sfr = "RATIO_HIGH_LOW"                  , "Memory", 0x40004000,        4, base=16

sfr = "BUFFER_STATUS"                   , "Memory", 0x40004004,        4, base=16
sfr = "BUFFER_STATUS.ch0BufAComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=0-0
sfr = "BUFFER_STATUS.ch0BufBComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=1-1
sfr = "BUFFER_STATUS.ch1BufAComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=2-2
sfr = "BUFFER_STATUS.ch1BufBComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=3-3
sfr = "BUFFER_STATUS.ch2BufAComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=4-4
sfr = "BUFFER_STATUS.ch2BufBComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=5-5
sfr = "BUFFER_STATUS.ch3BufAComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=6-6
sfr = "BUFFER_STATUS.ch3BufBComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=7-7
sfr = "BUFFER_STATUS.ch4BufAComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=8-8
sfr = "BUFFER_STATUS.ch4BufBComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=9-9
sfr = "BUFFER_STATUS.ch5BufAComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=10-10
sfr = "BUFFER_STATUS.ch5BufBComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=11-11
sfr = "BUFFER_STATUS.ch6BufAComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=12-12
sfr = "BUFFER_STATUS.ch6BufBComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=13-13
sfr = "BUFFER_STATUS.ch7BufAComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=14-14
sfr = "BUFFER_STATUS.ch7BufBComplete"   , "Memory", 0x40004004,        4, base=16,    bitRange=15-15

sfr = "CHAN_0_CTRL"                     , "Memory", 0x40004020,        4, base=16
sfr = "CHAN_0_CTRL.PeriphDMA"           , "Memory", 0x40004020,        4, base=16,    bitRange=0-0
sfr = "CHAN_0_CTRL.Direction"           , "Memory", 0x40004020,        4, base=16,    bitRange=1-1
sfr = "CHAN_0_CTRL.TransferSize"        , "Memory", 0x40004020,        4, base=16,    bitRange=2-3
sfr = "CHAN_0_CTRL.Pause"               , "Memory", 0x40004020,        4, base=16,    bitRange=4-4
sfr = "CHAN_0_CTRL.Reset"               , "Memory", 0x40004020,        4, base=16,    bitRange=5-5
sfr = "CHAN_0_CTRL.InterruptEnable"     , "Memory", 0x40004020,        4, base=16,    bitRange=6-6
sfr = "CHAN_0_CTRL.ClearDmaPortDoneA"   , "Memory", 0x40004020,        4, base=16,    bitRange=7-7
sfr = "CHAN_0_CTRL.ClearDmaPortDoneB"   , "Memory", 0x40004020,        4, base=16,    bitRange=8-8
sfr = "CHAN_0_CTRL.PortHighPriority"    , "Memory", 0x40004020,        4, base=16,    bitRange=9-9
sfr = "CHAN_0_CTRL.SrcAddrInc"          , "Memory", 0x40004020,        4, base=16,    bitRange=10-11
sfr = "CHAN_0_CTRL.DestAddrInc"         , "Memory", 0x40004020,        4, base=16,    bitRange=12-13
sfr = "CHAN_0_CTRL.PostedWriteAdjust"   , "Memory", 0x40004020,        4, base=16,    bitRange=14-21
sfr = "CHAN_0_CTRL.PeriphSelect"        , "Memory", 0x40004020,        4, base=16,    bitRange=23-26

sfr = "CHAN_0_STATUS"                   , "Memory", 0x40004024,        4, base=16
sfr = "CHAN_0_STATUS.CompleteA"         , "Memory", 0x40004024,        4, base=16,    bitRange=0-0
sfr = "CHAN_0_STATUS.CompleteB"         , "Memory", 0x40004024,        4, base=16,    bitRange=1-1
sfr = "CHAN_0_STATUS.BuffBSelect"       , "Memory", 0x40004024,        4, base=16,    bitRange=2-2

sfr = "CHAN_0_BUFF_A_SRC"               , "Memory", 0x40004028,        4, base=16
sfr = "CHAN_0_BUFF_A_DST"               , "Memory", 0x4000402C,        4, base=16
sfr = "CHAN_0_BUFF_A_COUNT"             , "Memory", 0x40004030,        2, base=16
sfr = "CHAN_0_BUFF_B_SRC"               , "Memory", 0x40004034,        4, base=16
sfr = "CHAN_0_BUFF_B_DST"               , "Memory", 0x40004038,        4, base=16
sfr = "CHAN_0_BUFF_B_COUNT"             , "Memory", 0x4000403C,        2, base=16

sfr = "CHAN_1_CTRL"                     , "Memory", 0x40004040,        4, base=16
sfr = "CHAN_1_CTRL.PeriphDMA"           , "Memory", 0x40004040,        4, base=16,    bitRange=0-0
sfr = "CHAN_1_CTRL.Direction"           , "Memory", 0x40004040,        4, base=16,    bitRange=1-1
sfr = "CHAN_1_CTRL.TransferSize"        , "Memory", 0x40004040,        4, base=16,    bitRange=2-3
sfr = "CHAN_1_CTRL.Pause"               , "Memory", 0x40004040,        4, base=16,    bitRange=4-4
sfr = "CHAN_1_CTRL.Reset"               , "Memory", 0x40004040,        4, base=16,    bitRange=5-5
sfr = "CHAN_1_CTRL.InterruptEnable"     , "Memory", 0x40004040,        4, base=16,    bitRange=6-6
sfr = "CHAN_1_CTRL.ClearDmaPortDoneA"   , "Memory", 0x40004040,        4, base=16,    bitRange=7-7
sfr = "CHAN_1_CTRL.ClearDmaPortDoneB"   , "Memory", 0x40004040,        4, base=16,    bitRange=8-8
sfr = "CHAN_1_CTRL.PortHighPriority"    , "Memory", 0x40004040,        4, base=16,    bitRange=9-9
sfr = "CHAN_1_CTRL.SrcAddrInc"          , "Memory", 0x40004040,        4, base=16,    bitRange=10-11
sfr = "CHAN_1_CTRL.DestAddrInc"         , "Memory", 0x40004040,        4, base=16,    bitRange=12-13
sfr = "CHAN_1_CTRL.PostedWriteAdjust"   , "Memory", 0x40004040,        4, base=16,    bitRange=14-21
sfr = "CHAN_1_CTRL.PeriphSelect"        , "Memory", 0x40004040,        4, base=16,    bitRange=23-26

sfr = "CHAN_1_STATUS"                   , "Memory", 0x40004044,        4, base=16
sfr = "CHAN_1_STATUS.CompleteA"         , "Memory", 0x40004044,        4, base=16,    bitRange=0-0
sfr = "CHAN_1_STATUS.CompleteB"         , "Memory", 0x40004044,        4, base=16,    bitRange=1-1
sfr = "CHAN_1_STATUS.BuffBSelect"       , "Memory", 0x40004044,        4, base=16,    bitRange=2-2

sfr = "CHAN_1_BUFF_A_SRC"               , "Memory", 0x40004048,        4, base=16
sfr = "CHAN_1_BUFF_A_DST"               , "Memory", 0x4000404C,        4, base=16
sfr = "CHAN_1_BUFF_A_COUNT"             , "Memory", 0x40004050,        2, base=16
sfr = "CHAN_1_BUFF_B_SRC"               , "Memory", 0x40004054,        4, base=16
sfr = "CHAN_1_BUFF_B_DST"               , "Memory", 0x40004058,        4, base=16
sfr = "CHAN_1_BUFF_B_COUNT"             , "Memory", 0x4000405C,        2, base=16

;-------------------
sfr = "CHAN_2_CTRL"                     , "Memory", 0x40004060,        4, base=16
sfr = "CHAN_2_CTRL.PeriphDMA"           , "Memory", 0x40004060,        4, base=16,    bitRange=0-0
sfr = "CHAN_2_CTRL.Direction"           , "Memory", 0x40004060,        4, base=16,    bitRange=1-1
sfr = "CHAN_2_CTRL.TransferSize"        , "Memory", 0x40004060,        4, base=16,    bitRange=2-3
sfr = "CHAN_2_CTRL.Pause"               , "Memory", 0x40004060,        4, base=16,    bitRange=4-4
sfr = "CHAN_2_CTRL.Reset"               , "Memory", 0x40004060,        4, base=16,    bitRange=5-5
sfr = "CHAN_2_CTRL.InterruptEnable"     , "Memory", 0x40004060,        4, base=16,    bitRange=6-6
sfr = "CHAN_2_CTRL.ClearDmaPortDoneA"   , "Memory", 0x40004060,        4, base=16,    bitRange=7-7
sfr = "CHAN_2_CTRL.ClearDmaPortDoneB"   , "Memory", 0x40004060,        4, base=16,    bitRange=8-8
sfr = "CHAN_2_CTRL.PortHighPriority"    , "Memory", 0x40004060,        4, base=16,    bitRange=9-9
sfr = "CHAN_2_CTRL.SrcAddrInc"          , "Memory", 0x40004060,        4, base=16,    bitRange=10-11
sfr = "CHAN_2_CTRL.DestAddrInc"         , "Memory", 0x40004060,        4, base=16,    bitRange=12-13
sfr = "CHAN_2_CTRL.PostedWriteAdjust"   , "Memory", 0x40004060,        4, base=16,    bitRange=14-21
sfr = "CHAN_2_CTRL.PeriphSelect"        , "Memory", 0x40004060,        4, base=16,    bitRange=23-26

sfr = "CHAN_2_STATUS"                   , "Memory", 0x40004064,        4, base=16
sfr = "CHAN_2_STATUS.CompleteA"         , "Memory", 0x40004064,        4, base=16,    bitRange=0-0
sfr = "CHAN_2_STATUS.CompleteB"         , "Memory", 0x40004064,        4, base=16,    bitRange=1-1
sfr = "CHAN_2_STATUS.BuffBSelect"       , "Memory", 0x40004064,        4, base=16,    bitRange=2-2

sfr = "CHAN_2_BUFF_A_SRC"               , "Memory", 0x40004068,        4, base=16
sfr = "CHAN_2_BUFF_A_DST"               , "Memory", 0x4000406C,        4, base=16
sfr = "CHAN_2_BUFF_A_COUNT"             , "Memory", 0x40004070,        2, base=16
sfr = "CHAN_2_BUFF_B_SRC"               , "Memory", 0x40004074,        4, base=16
sfr = "CHAN_2_BUFF_B_DST"               , "Memory", 0x40004078,        4, base=16
sfr = "CHAN_2_BUFF_B_COUNT"             , "Memory", 0x4000407C,        2, base=16

;-------------------
sfr = "CHAN_3_CTRL"                     , "Memory", 0x40004080,        4, base=16
sfr = "CHAN_3_CTRL.PeriphDMA"           , "Memory", 0x40004080,        4, base=16,    bitRange=0-0
sfr = "CHAN_3_CTRL.Direction"           , "Memory", 0x40004080,        4, base=16,    bitRange=1-1
sfr = "CHAN_3_CTRL.TransferSize"        , "Memory", 0x40004080,        4, base=16,    bitRange=2-3
sfr = "CHAN_3_CTRL.Pause"               , "Memory", 0x40004080,        4, base=16,    bitRange=4-4
sfr = "CHAN_3_CTRL.Reset"               , "Memory", 0x40004080,        4, base=16,    bitRange=5-5
sfr = "CHAN_3_CTRL.InterruptEnable"     , "Memory", 0x40004080,        4, base=16,    bitRange=6-6
sfr = "CHAN_3_CTRL.ClearDmaPortDoneA"   , "Memory", 0x40004080,        4, base=16,    bitRange=7-7
sfr = "CHAN_3_CTRL.ClearDmaPortDoneB"   , "Memory", 0x40004080,        4, base=16,    bitRange=8-8
sfr = "CHAN_3_CTRL.PortHighPriority"    , "Memory", 0x40004080,        4, base=16,    bitRange=9-9
sfr = "CHAN_3_CTRL.SrcAddrInc"          , "Memory", 0x40004080,        4, base=16,    bitRange=10-11
sfr = "CHAN_3_CTRL.DestAddrInc"         , "Memory", 0x40004080,        4, base=16,    bitRange=12-13
sfr = "CHAN_3_CTRL.PostedWriteAdjust"   , "Memory", 0x40004080,        4, base=16,    bitRange=14-21
sfr = "CHAN_3_CTRL.PeriphSelect"        , "Memory", 0x40004080,        4, base=16,    bitRange=23-26

sfr = "CHAN_3_STATUS"                   , "Memory", 0x40004084,        4, base=16
sfr = "CHAN_3_STATUS.CompleteA"         , "Memory", 0x40004084,        4, base=16,    bitRange=0-0
sfr = "CHAN_3_STATUS.CompleteB"         , "Memory", 0x40004084,        4, base=16,    bitRange=1-1
sfr = "CHAN_3_STATUS.BuffBSelect"       , "Memory", 0x40004084,        4, base=16,    bitRange=2-2

sfr = "CHAN_3_BUFF_A_SRC"               , "Memory", 0x40004088,        4, base=16
sfr = "CHAN_3_BUFF_A_DST"               , "Memory", 0x4000408C,        4, base=16
sfr = "CHAN_3_BUFF_A_COUNT"             , "Memory", 0x40004090,        2, base=16
sfr = "CHAN_3_BUFF_B_SRC"               , "Memory", 0x40004094,        4, base=16
sfr = "CHAN_3_BUFF_B_DST"               , "Memory", 0x40004098,        4, base=16
sfr = "CHAN_3_BUFF_B_COUNT"             , "Memory", 0x4000409C,        2, base=16

;-------------------
sfr = "CHAN_4_CTRL"                     , "Memory", 0x400040A0,        4, base=16
sfr = "CHAN_4_CTRL.PeriphDMA"           , "Memory", 0x400040A0,        4, base=16,    bitRange=0-0
sfr = "CHAN_4_CTRL.Direction"           , "Memory", 0x400040A0,        4, base=16,    bitRange=1-1
sfr = "CHAN_4_CTRL.TransferSize"        , "Memory", 0x400040A0,        4, base=16,    bitRange=2-3
sfr = "CHAN_4_CTRL.Pause"               , "Memory", 0x400040A0,        4, base=16,    bitRange=4-4
sfr = "CHAN_4_CTRL.Reset"               , "Memory", 0x400040A0,        4, base=16,    bitRange=5-5
sfr = "CHAN_4_CTRL.InterruptEnable"     , "Memory", 0x400040A0,        4, base=16,    bitRange=6-6
sfr = "CHAN_4_CTRL.ClearDmaPortDoneA"   , "Memory", 0x400040A0,        4, base=16,    bitRange=7-7
sfr = "CHAN_4_CTRL.ClearDmaPortDoneB"   , "Memory", 0x400040A0,        4, base=16,    bitRange=8-8
sfr = "CHAN_4_CTRL.PortHighPriority"    , "Memory", 0x400040A0,        4, base=16,    bitRange=9-9
sfr = "CHAN_4_CTRL.SrcAddrInc"          , "Memory", 0x400040A0,        4, base=16,    bitRange=10-11
sfr = "CHAN_4_CTRL.DestAddrInc"         , "Memory", 0x400040A0,        4, base=16,    bitRange=12-13
sfr = "CHAN_4_CTRL.PostedWriteAdjust"   , "Memory", 0x400040A0,        4, base=16,    bitRange=14-21
sfr = "CHAN_4_CTRL.PeriphSelect"        , "Memory", 0x400040A0,        4, base=16,    bitRange=23-26

sfr = "CHAN_4_STATUS"                   , "Memory", 0x400040A4,        4, base=16
sfr = "CHAN_4_STATUS.CompleteA"         , "Memory", 0x400040A4,        4, base=16,    bitRange=0-0
sfr = "CHAN_4_STATUS.CompleteB"         , "Memory", 0x400040A4,        4, base=16,    bitRange=1-1
sfr = "CHAN_4_STATUS.BuffBSelect"       , "Memory", 0x400040A4,        4, base=16,    bitRange=2-2

sfr = "CHAN_4_BUFF_A_SRC"               , "Memory", 0x400040A8,        4, base=16
sfr = "CHAN_4_BUFF_A_DST"               , "Memory", 0x400040AC,        4, base=16
sfr = "CHAN_4_BUFF_A_COUNT"             , "Memory", 0x400040B0,        2, base=16
sfr = "CHAN_4_BUFF_B_SRC"               , "Memory", 0x400040B4,        4, base=16
sfr = "CHAN_4_BUFF_B_DST"               , "Memory", 0x400040B8,        4, base=16
sfr = "CHAN_4_BUFF_B_COUNT"             , "Memory", 0x400040BC,        2, base=16

;-------------------
sfr = "CHAN_5_CTRL"                     , "Memory", 0x400040C0,        4, base=16
sfr = "CHAN_5_CTRL.PeriphDMA"           , "Memory", 0x400040C0,        4, base=16,    bitRange=0-0
sfr = "CHAN_5_CTRL.Direction"           , "Memory", 0x400040C0,        4, base=16,    bitRange=1-1
sfr = "CHAN_5_CTRL.TransferSize"        , "Memory", 0x400040C0,        4, base=16,    bitRange=2-3
sfr = "CHAN_5_CTRL.Pause"               , "Memory", 0x400040C0,        4, base=16,    bitRange=4-4
sfr = "CHAN_5_CTRL.Reset"               , "Memory", 0x400040C0,        4, base=16,    bitRange=5-5
sfr = "CHAN_5_CTRL.InterruptEnable"     , "Memory", 0x400040C0,        4, base=16,    bitRange=6-6
sfr = "CHAN_5_CTRL.ClearDmaPortDoneA"   , "Memory", 0x400040C0,        4, base=16,    bitRange=7-7
sfr = "CHAN_5_CTRL.ClearDmaPortDoneB"   , "Memory", 0x400040C0,        4, base=16,    bitRange=8-8
sfr = "CHAN_5_CTRL.PortHighPriority"    , "Memory", 0x400040C0,        4, base=16,    bitRange=9-9
sfr = "CHAN_5_CTRL.SrcAddrInc"          , "Memory", 0x400040C0,        4, base=16,    bitRange=10-11
sfr = "CHAN_5_CTRL.DestAddrInc"         , "Memory", 0x400040C0,        4, base=16,    bitRange=12-13
sfr = "CHAN_5_CTRL.PostedWriteAdjust"   , "Memory", 0x400040C0,        4, base=16,    bitRange=14-21
sfr = "CHAN_5_CTRL.PeriphSelect"        , "Memory", 0x400040C0,        4, base=16,    bitRange=23-26

sfr = "CHAN_5_STATUS"                   , "Memory", 0x400040C4,        4, base=16
sfr = "CHAN_5_STATUS.CompleteA"         , "Memory", 0x400040C4,        4, base=16,    bitRange=0-0
sfr = "CHAN_5_STATUS.CompleteB"         , "Memory", 0x400040C4,        4, base=16,    bitRange=1-1
sfr = "CHAN_5_STATUS.BuffBSelect"       , "Memory", 0x400040C4,        4, base=16,    bitRange=2-2

sfr = "CHAN_5_BUFF_A_SRC"               , "Memory", 0x400040C8,        4, base=16
sfr = "CHAN_5_BUFF_A_DST"               , "Memory", 0x400040CC,        4, base=16
sfr = "CHAN_5_BUFF_A_COUNT"             , "Memory", 0x400040D0,        2, base=16
sfr = "CHAN_5_BUFF_B_SRC"               , "Memory", 0x400040D4,        4, base=16
sfr = "CHAN_5_BUFF_B_DST"               , "Memory", 0x400040D8,        4, base=16
sfr = "CHAN_5_BUFF_B_COUNT"             , "Memory", 0x400040DC,        2, base=16

;-------------------
sfr = "CHAN_6_CTRL"                     , "Memory", 0x400040E0,        4, base=16
sfr = "CHAN_6_CTRL.PeriphDMA"           , "Memory", 0x400040E0,        4, base=16,    bitRange=0-0
sfr = "CHAN_6_CTRL.Direction"           , "Memory", 0x400040E0,        4, base=16,    bitRange=1-1
sfr = "CHAN_6_CTRL.TransferSize"        , "Memory", 0x400040E0,        4, base=16,    bitRange=2-3
sfr = "CHAN_6_CTRL.Pause"               , "Memory", 0x400040E0,        4, base=16,    bitRange=4-4
sfr = "CHAN_6_CTRL.Reset"               , "Memory", 0x400040E0,        4, base=16,    bitRange=5-5
sfr = "CHAN_6_CTRL.InterruptEnable"     , "Memory", 0x400040E0,        4, base=16,    bitRange=6-6
sfr = "CHAN_6_CTRL.ClearDmaPortDoneA"   , "Memory", 0x400040E0,        4, base=16,    bitRange=7-7
sfr = "CHAN_6_CTRL.ClearDmaPortDoneB"   , "Memory", 0x400040E0,        4, base=16,    bitRange=8-8
sfr = "CHAN_6_CTRL.PortHighPriority"    , "Memory", 0x400040E0,        4, base=16,    bitRange=9-9
sfr = "CHAN_6_CTRL.SrcAddrInc"          , "Memory", 0x400040E0,        4, base=16,    bitRange=10-11
sfr = "CHAN_6_CTRL.DestAddrInc"         , "Memory", 0x400040E0,        4, base=16,    bitRange=12-13
sfr = "CHAN_6_CTRL.PostedWriteAdjust"   , "Memory", 0x400040E0,        4, base=16,    bitRange=14-21
sfr = "CHAN_6_CTRL.PeriphSelect"        , "Memory", 0x400040E0,        4, base=16,    bitRange=23-26

sfr = "CHAN_6_STATUS"                   , "Memory", 0x400040E4,        4, base=16
sfr = "CHAN_6_STATUS.CompleteA"         , "Memory", 0x400040E4,        4, base=16,    bitRange=0-0
sfr = "CHAN_6_STATUS.CompleteB"         , "Memory", 0x400040E4,        4, base=16,    bitRange=1-1
sfr = "CHAN_6_STATUS.BuffBSelect"       , "Memory", 0x400040E4,        4, base=16,    bitRange=2-2

sfr = "CHAN_6_BUFF_A_SRC"               , "Memory", 0x400040E8,        4, base=16
sfr = "CHAN_6_BUFF_A_DST"               , "Memory", 0x400040EC,        4, base=16
sfr = "CHAN_6_BUFF_A_COUNT"             , "Memory", 0x400040F0,        2, base=16
sfr = "CHAN_6_BUFF_B_SRC"               , "Memory", 0x400040F4,        4, base=16
sfr = "CHAN_6_BUFF_B_DST"               , "Memory", 0x400040F8,        4, base=16
sfr = "CHAN_6_BUFF_B_COUNT"             , "Memory", 0x400040FC,        2, base=16

;-------------------
sfr = "CHAN_7_CTRL"                     , "Memory", 0x40004100,        4, base=16
sfr = "CHAN_7_CTRL.PeriphDMA"           , "Memory", 0x40004100,        4, base=16,    bitRange=0-0
sfr = "CHAN_7_CTRL.Direction"           , "Memory", 0x40004100,        4, base=16,    bitRange=1-1
sfr = "CHAN_7_CTRL.TransferSize"        , "Memory", 0x40004100,        4, base=16,    bitRange=2-3
sfr = "CHAN_7_CTRL.Pause"               , "Memory", 0x40004100,        4, base=16,    bitRange=4-4
sfr = "CHAN_7_CTRL.Reset"               , "Memory", 0x40004100,        4, base=16,    bitRange=5-5
sfr = "CHAN_7_CTRL.InterruptEnable"     , "Memory", 0x40004100,        4, base=16,    bitRange=6-6
sfr = "CHAN_7_CTRL.ClearDmaPortDoneA"   , "Memory", 0x40004100,        4, base=16,    bitRange=7-7
sfr = "CHAN_7_CTRL.ClearDmaPortDoneB"   , "Memory", 0x40004100,        4, base=16,    bitRange=8-8
sfr = "CHAN_7_CTRL.PortHighPriority"    , "Memory", 0x40004100,        4, base=16,    bitRange=9-9
sfr = "CHAN_7_CTRL.SrcAddrInc"          , "Memory", 0x40004100,        4, base=16,    bitRange=10-11
sfr = "CHAN_7_CTRL.DestAddrInc"         , "Memory", 0x40004100,        4, base=16,    bitRange=12-13
sfr = "CHAN_7_CTRL.PostedWriteAdjust"   , "Memory", 0x40004100,        4, base=16,    bitRange=14-21
sfr = "CHAN_7_CTRL.PeriphSelect"        , "Memory", 0x40004100,        4, base=16,    bitRange=23-26

sfr = "CHAN_7_STATUS"                   , "Memory", 0x40004104,        4, base=16
sfr = "CHAN_7_STATUS.CompleteA"         , "Memory", 0x40004104,        4, base=16,    bitRange=0-0
sfr = "CHAN_7_STATUS.CompleteB"         , "Memory", 0x40004104,        4, base=16,    bitRange=1-1
sfr = "CHAN_7_STATUS.BuffBSelect"       , "Memory", 0x40004104,        4, base=16,    bitRange=2-2

sfr = "CHAN_7_BUFF_A_SRC"               , "Memory", 0x40004108,        4, base=16
sfr = "CHAN_7_BUFF_A_DST"               , "Memory", 0x4000410C,        4, base=16
sfr = "CHAN_7_BUFF_A_COUNT"             , "Memory", 0x40004110,        2, base=16
sfr = "CHAN_7_BUFF_B_SRC"               , "Memory", 0x40004114,        4, base=16
sfr = "CHAN_7_BUFF_B_DST"               , "Memory", 0x40004118,        4, base=16
sfr = "CHAN_7_BUFF_B_COUNT"             , "Memory", 0x4000411C,        2, base=16

;-------------------

;
;		Timer
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "TIM1_BGLOADVAL"   , "Memory", 0x40005008,        4, base=16

sfr = "TIM1_CTRL"   , "Memory", 0x4000500c,        4, base=16
sfr = "TIM1_CTRL.ENABLE"   , "Memory", 0x4000500c,        4, base=16,    bitRange=0-0
sfr = "TIM1_CTRL.MODE"   , "Memory", 0x4000500c,        4, base=16,    bitRange=1-1
sfr = "TIM1_CTRL.INTEN"   , "Memory", 0x4000500c,        4, base=16,    bitRange=2-2

sfr = "TIM1_LOADVAL"   , "Memory", 0x40005004,        4, base=16

sfr = "TIM1_MIS"   , "Memory", 0x40005014,        4, base=16

sfr = "TIM1_RIS"   , "Memory", 0x40005010,        4, base=16

sfr = "TIM1_VALUE"   , "Memory", 0x40005000,        4, base=16

sfr = "TIM2_BGLOADVAL"   , "Memory", 0x40005020,        4, base=16

sfr = "TIM2_CTRL"   , "Memory", 0x40005024,        4, base=16
sfr = "TIM2_CTRL.ENABLE"   , "Memory", 0x40005024,        4, base=16,    bitRange=0-0
sfr = "TIM2_CTRL.MODE"   , "Memory", 0x40005024,        4, base=16,    bitRange=1-1
sfr = "TIM2_CTRL.INTEN"   , "Memory", 0x40005024,        4, base=16,    bitRange=2-2

sfr = "TIM2_LOADVAL"   , "Memory", 0x4000501C,        4, base=16

sfr = "TIM2_MIS"   , "Memory", 0x4000502C,        4, base=16

sfr = "TIM2_RIS"   , "Memory", 0x40005028,        4, base=16

sfr = "TIM2_VALUE"   , "Memory", 0x40005018,        4, base=16

sfr = "TIM64BGLOADVALUEL"   , "Memory", 0x40005044,        4, base=16

sfr = "TIM64BGLOADVALUEU"   , "Memory", 0x40005040,        4, base=16

sfr = "TIM64LOADVALUEL"   , "Memory", 0x4000503C,        4, base=16

sfr = "TIM64LOADVALUEU"   , "Memory", 0x40005038,        4, base=16

sfr = "TIM64VALUEL"   , "Memory", 0x40005034,        4, base=16

sfr = "TIM64VALUEU"   , "Memory", 0x40005030,        4, base=16

sfr = "TIM64_CTRL"   , "Memory", 0x40005048,        4, base=16
sfr = "TIM64_CTRL.ENABLE"   , "Memory", 0x40005048,        4, base=16,    bitRange=0-0
sfr = "TIM64_CTRL.MODE"   , "Memory", 0x40005048,        4, base=16,    bitRange=1-1
sfr = "TIM64_CTRL.INTEN"   , "Memory", 0x40005048,        4, base=16,    bitRange=2-2

sfr = "TIM64_MIS"   , "Memory", 0x40005050,        4, base=16

sfr = "TIM64_MODE"   , "Memory", 0x40005054,        4, base=16

sfr = "TIM64_RIS"   , "Memory", 0x4000504c,        4, base=16



;
;		Watchdog
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "WATCHDOG"              , "Memory", 0x40006000,        4, base=16

;
;		H2F Interrupt Ctrl
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "H2F"                   , "Memory", 0x40007000,        4, base=16

;
;		UART_1
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "RBR1"                   , "Memory", 0x40010000,        1, base=16

sfr = "THR1"                   , "Memory", 0x40010000,        1, base=16

sfr = "DLR1"                   , "Memory", 0x40010000,        1, base=16

sfr = "DMR1"                   , "Memory", 0x40010004,        1, base=16

sfr = "IER1"                   , "Memory", 0x40010004,        1, base=16
sfr = "IER1.ERBFI"             , "Memory", 0x40010004,        1, base=16,    bitRange=0-0
sfr = "IER1.ETBEI"             , "Memory", 0x40010004,        1, base=16,    bitRange=1-1
sfr = "IER1.ELSI"              , "Memory", 0x40010004,        1, base=16,    bitRange=2-2
sfr = "IER1.EDSSI"             , "Memory", 0x40010004,        1, base=16,    bitRange=3-3

sfr = "IIR1"                   , "Memory", 0x40010008,        1, base=16
sfr = "IIR1.IIR"               , "Memory", 0x40010008,        1, base=16,    bitRange=0-3
sfr = "IIR1.Mode"              , "Memory", 0x40010008,        1, base=16,    bitRange=6-7

sfr = "FCR1"                   , "Memory", 0x40010008,        1, base=16
sfr = "FCR1.Bit0"              , "Memory", 0x40010008,        1, base=16,    bitRange=0-0
sfr = "FCR1.Bit1"              , "Memory", 0x40010008,        1, base=16,    bitRange=1-1
sfr = "FCR1.Bit2"              , "Memory", 0x40010008,        1, base=16,    bitRange=2-2
sfr = "FCR1.Bit3"              , "Memory", 0x40010008,        1, base=16,    bitRange=3-3
sfr = "FCR1.Bit6"              , "Memory", 0x40010008,        1, base=16,    bitRange=6-7

sfr = "LCR1"                   , "Memory", 0x4001000C,        1, base=16
sfr = "LCR1.WLS"               , "Memory", 0x4001000C,        1, base=16,    bitRange=0-1
sfr = "LCR1.STB"               , "Memory", 0x4001000C,        1, base=16,    bitRange=2-2
sfr = "LCR1.PEN"               , "Memory", 0x4001000C,        1, base=16,    bitRange=3-3
sfr = "LCR1.EPS"               , "Memory", 0x4001000C,        1, base=16,    bitRange=4-4
sfr = "LCR1.SP"                , "Memory", 0x4001000C,        1, base=16,    bitRange=5-5
sfr = "LCR1.SB"                , "Memory", 0x4001000C,        1, base=16,    bitRange=6-6
sfr = "LCR1.DLAB"              , "Memory", 0x4001000C,        1, base=16,    bitRange=7-7

sfr = "MCR1"                   , "Memory", 0x40010010,        1, base=16
sfr = "MCR1.DTR"               , "Memory", 0x40010010,        1, base=16,    bitRange=0-0
sfr = "MCR1.RTS"               , "Memory", 0x40010010,        1, base=16,    bitRange=1-1
sfr = "MCR1.Out1"              , "Memory", 0x40010010,        1, base=16,    bitRange=2-2
sfr = "MCR1.Out2"              , "Memory", 0x40010010,        1, base=16,    bitRange=3-3
sfr = "MCR1.Loop"              , "Memory", 0x40010010,        1, base=16,    bitRange=4-4

sfr = "LSR1"                   , "Memory", 0x40010014,        1, base=16
sfr = "LSR1.DR"                , "Memory", 0x40010014,        1, base=16,    bitRange=0-0
sfr = "LSR1.OE"                , "Memory", 0x40010014,        1, base=16,    bitRange=1-1
sfr = "LSR1.PE"                , "Memory", 0x40010014,        1, base=16,    bitRange=2-2
sfr = "LSR1.FE"                , "Memory", 0x40010014,        1, base=16,    bitRange=3-3
sfr = "LSR1.BI"                , "Memory", 0x40010014,        1, base=16,    bitRange=4-4
sfr = "LSR1.THRE"              , "Memory", 0x40010014,        1, base=16,    bitRange=5-5
sfr = "LSR1.TEMT"              , "Memory", 0x40010014,        1, base=16,    bitRange=6-6
sfr = "LSR1.FIER"              , "Memory", 0x40010014,        1, base=16,    bitRange=7-7

sfr = "MSR1"                   , "Memory", 0x40010018,        1, base=16
sfr = "MSR1.DCTS"              , "Memory", 0x40010018,        1, base=16,    bitRange=0-0
sfr = "MSR1.DDSR"              , "Memory", 0x40010018,        1, base=16,    bitRange=1-1
sfr = "MSR1.TERI"              , "Memory", 0x40010018,        1, base=16,    bitRange=2-2
sfr = "MSR1.DDCD"              , "Memory", 0x40010018,        1, base=16,    bitRange=3-3
sfr = "MSR1.CTS"               , "Memory", 0x40010018,        1, base=16,    bitRange=4-4
sfr = "MSR1.DSR"               , "Memory", 0x40010018,        1, base=16,    bitRange=5-5
sfr = "MSR1.RI"                , "Memory", 0x40010018,        1, base=16,    bitRange=6-6
sfr = "MSR1.DCD"               , "Memory", 0x40010018,        1, base=16,    bitRange=7-7

sfr = "SR1"                    , "Memory", 0x4001001C,        1, base=16

;
;		SPI_1
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "SPI1_CONTROL"                        , "Memory", 0x40011000,        4, base=16
sfr = "SPI1_CONTROL.CTL_SPH"   	            , "Memory", 0x40011000,        4, base=16,    bitRange=25-25
sfr = "SPI1_CONTROL.CTL_SPO"   	            , "Memory", 0x40011000,        4, base=16,    bitRange=24-24
sfr = "SPI1_CONTROL.CTL_TXRXDFCOUNT"        , "Memory", 0x40011000,        4, base=16,    bitRange=8-23
sfr = "SPI1_CONTROL.INT_TXUR"               , "Memory", 0x40011000,        4, base=16,    bitRange=7-7
sfr = "SPI1_CONTROL.INT_RXOVF"              , "Memory", 0x40011000,        4, base=16,    bitRange=6-6
sfr = "SPI1_CONTROL.INT_TX"                 , "Memory", 0x40011000,        4, base=16,    bitRange=5-5
sfr = "SPI1_CONTROL.INT_RX"                 , "Memory", 0x40011000,        4, base=16,    bitRange=4-4
sfr = "SPI1_CONTROL.MODE"                   , "Memory", 0x40011000,        4, base=16,    bitRange=2-3
sfr = "SPI1_CONTROL.MASTER"                 , "Memory", 0x40011000,        4, base=16,    bitRange=1-1
sfr = "SPI1_CONTROL.ENABLE"                 , "Memory", 0x40011000,        4, base=16,    bitRange=0-0

sfr = "SPI1_TXRXDF_SIZE"                    , "Memory", 0x40011004,        4, base=16
sfr = "SPI1_TXRXDF_SIZE.TXRXDF_SIZE"        , "Memory", 0x40011004,        4, base=16,    bitRange=0-5

sfr = "SPI1_STATUS"                         , "Memory", 0x40011008,        4, base=16
sfr = "SPI1_STATUS.TX_FIFO_EMPTY_NEXT"   , "Memory", 0x40011008,        4, base=16,    bitRange=11-11
sfr = "SPI1_STATUS.TX_FIFO_EMPTY"        , "Memory", 0x40011008,        4, base=16,    bitRange=10-10
sfr = "SPI1_STATUS.TX_FIFO_FULL_NEXT"    , "Memory", 0x40011008,        4, base=16,    bitRange=9-9
sfr = "SPI1_STATUS.TX_FIFO_FULL"         , "Memory", 0x40011008,        4, base=16,    bitRange=8-8
sfr = "SPI1_STATUS.RX_FIFO_EMPTY_NEXT"   , "Memory", 0x40011008,        4, base=16,    bitRange=7-7
sfr = "SPI1_STATUS.RX_FIFO_EMPTY"        , "Memory", 0x40011008,        4, base=16,    bitRange=6-6
sfr = "SPI1_STATUS.RX_FIFO_FULL_NEXT"    , "Memory", 0x40011008,        4, base=16,    bitRange=5-5
sfr = "SPI1_STATUS.RX_FIFO_FULL"         , "Memory", 0x40011008,        4, base=16,    bitRange=4-4
sfr = "SPI1_STATUS.TX_CH_UV"                , "Memory", 0x40011008,        4, base=16,    bitRange=3-3
sfr = "SPI1_STATUS.RX_CH_OV"                , "Memory", 0x40011008,        4, base=16,    bitRange=2-2
sfr = "SPI1_STATUS.RX_RDY"                  , "Memory", 0x40011008,        4, base=16,    bitRange=1-1
sfr = "SPI1_STATUS.TX_DONE"                 , "Memory", 0x40011008,        4, base=16,    bitRange=0-0

sfr = "SPI1_INT_CLR"                        , "Memory", 0x4001100c,        4, base=16
sfr = "SPI1_INT_CLR.TX_CH_UV"               , "Memory", 0x4001100c,        4, base=16,    bitRange=3-3
sfr = "SPI1_INT_CLR.RX_CH_OV"               , "Memory", 0x4001100c,        4, base=16,    bitRange=2-2
sfr = "SPI1_INT_CLR.RX_RDY"                 , "Memory", 0x4001100c,        4, base=16,    bitRange=1-1
sfr = "SPI1_INT_CLR.TX_DONE"                , "Memory", 0x4001100c,        4, base=16,    bitRange=0-0

sfr = "SPI1_RX_DATA"                        , "Memory", 0x40011010,        4, base=16
sfr = "SPI1_RX_DATA.RX_DATA"                , "Memory", 0x40011010,        4, base=16,    bitRange=0-31

sfr = "SPI1_TX_DATA"                        , "Memory", 0x40011014,        4, base=16
sfr = "SPI1_TX_DATA.TX_DATA"                , "Memory", 0x40011014,        4, base=16,    bitRange=0-31

sfr = "SPI1_CLK_GEN"                        , "Memory", 0x40011018,        4, base=16
sfr = "SPI1_CLK_GEN.CLK_GEN"                , "Memory", 0x40011018,        4, base=16,    bitRange=0-3

sfr = "SPI1_SLAVE_SELECT"                   , "Memory", 0x4001101c,        4, base=16
sfr = "SPI1_SLAVE_SELECT.SLAVE_SELECT"      , "Memory", 0x4001101c,        4, base=16,    bitRange=0-7

sfr = "SPI1_MIS"                            , "Memory", 0x40011020,        4, base=16
sfr = "SPI1_MIS.TX_CH_UV"                   , "Memory", 0x40011020,        4, base=16,    bitRange=3-3
sfr = "SPI1_MIS.RX_CH_OV"                   , "Memory", 0x40011020,        4, base=16,    bitRange=2-2
sfr = "SPI1_MIS.RX_RDY"                     , "Memory", 0x40011020,        4, base=16,    bitRange=1-1
sfr = "SPI1_MIS.TX_DONE"                    , "Memory", 0x40011020,        4, base=16,    bitRange=0-0

sfr = "SPI1_RIS"                            , "Memory", 0x40011024,        4, base=16
sfr = "SPI1_RIS.TX_CH_UV"                   , "Memory", 0x40011024,        4, base=16,    bitRange=3-3
sfr = "SPI1_RIS.RX_CH_OV"                   , "Memory", 0x40011024,        4, base=16,    bitRange=2-2
sfr = "SPI1_RIS.RX_RDY"                     , "Memory", 0x40011024,        4, base=16,    bitRange=1-1
sfr = "SPI1_RIS.TX_DONE"                    , "Memory", 0x40011024,        4, base=16,    bitRange=0-0


;
;		I2C_1
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "CTRL1"                  , "Memory", 0x40012000,        1, base=16
sfr = "CTRL1.CR2"              , "Memory", 0x40012000,        1, base=16,    bitRange=7-7
sfr = "CTRL1.ENS1"             , "Memory", 0x40012000,        1, base=16,    bitRange=6-6
sfr = "CTRL1.STA"              , "Memory", 0x40012000,        1, base=16,    bitRange=5-5
sfr = "CTRL1.STO"              , "Memory", 0x40012000,        1, base=16,    bitRange=4-4
sfr = "CTRL1.SI"               , "Memory", 0x40012000,        1, base=16,    bitRange=3-3
sfr = "CTRL1.AA"               , "Memory", 0x40012000,        1, base=16,    bitRange=2-2
sfr = "CTRL1.CR1"              , "Memory", 0x40012000,        1, base=16,    bitRange=1-1
sfr = "CTRL1.CR0"              , "Memory", 0x40012000,        1, base=16,    bitRange=0-0

sfr = "STAT1"                  , "Memory", 0x40012004,        1, base=16
sfr = "STAT1.STAT"             , "Memory", 0x40012004,        1, base=16,    bitRange=0-7

sfr = "DATA1"                  , "Memory", 0x40012008,        1, base=16
sfr = "DATA1.DATA"             , "Memory", 0x40012008,        1, base=16,    bitRange=0-7

sfr = "ADDR1"                  , "Memory", 0x4001200C,        1, base=16
sfr = "ADDR1.ADR"              , "Memory", 0x4001200C,        1, base=16,    bitRange=1-7
sfr = "ADDR1.GC"               , "Memory", 0x4001200C,        1, base=16,    bitRange=0-0

sfr = "SMBUS1"                 , "Memory", 0x40012010,        1, base=16
sfr = "SMBUS1.smbus_reset"     , "Memory", 0x40012010,        1, base=16,    bitRange=7-7
sfr = "SMBUS1.smbsus_no_control"   , "Memory", 0x40012010,        1, base=16,    bitRange=6-6
sfr = "SMBUS1.smbsus_ni_status"   , "Memory", 0x40012010,        1, base=16,    bitRange=5-5
sfr = "SMBUS1.smbalert_no_control"   , "Memory", 0x40012010,        1, base=16,    bitRange=4-4
sfr = "SMBUS1.smbalert_ni_status"   , "Memory", 0x40012010,        1, base=16,    bitRange=3-3
sfr = "SMBUS1.smbus_enable"   , "Memory", 0x40012010,        1, base=16,    bitRange=2-2
sfr = "SMBUS1.smbsus_interrupt_enable"   , "Memory", 0x40012010,        1, base=16,    bitRange=1-1
sfr = "SMBUS1.smbalert_interrupt_enable"   , "Memory", 0x40012010,        1, base=16,    bitRange=0-0

sfr = "FREQ1"                  , "Memory", 0x40012014,        1, base=16
sfr = "FREQ1.FREQ"             , "Memory", 0x40012014,        1, base=16,    bitRange=0-7

sfr = "GLITCHREG1"             , "Memory", 0x40012018,        1, base=16
sfr = "GLITCHREG1.GLITCHREG"   , "Memory", 0x40012018,        1, base=16,    bitRange=0-7


;
;		GPIO
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "CONFIG_01"             , "Memory", 0x40013000,        4, base=16
sfr = "CONFIG_01.IT"          , "Memory", 0x40013000,        4, base=16,    bitRange=5-7
sfr = "CONFIG_01.IE"          , "Memory", 0x40013000,        4, base=16,    bitRange=3-3
sfr = "CONFIG_01.OBE"         , "Memory", 0x40013000,        4, base=16,    bitRange=2-2
sfr = "CONFIG_01.IRE"         , "Memory", 0x40013000,        4, base=16,    bitRange=1-1
sfr = "CONFIG_01.ORE"         , "Memory", 0x40013000,        4, base=16,    bitRange=0-0

sfr = "CONFIG_02"             , "Memory", 0x40013004,        4, base=16
sfr = "CONFIG_02.IT"          , "Memory", 0x40013004,        4, base=16,    bitRange=5-7
sfr = "CONFIG_02.IE"          , "Memory", 0x40013004,        4, base=16,    bitRange=3-3
sfr = "CONFIG_02.OBE"         , "Memory", 0x40013004,        4, base=16,    bitRange=2-2
sfr = "CONFIG_02.IRE"         , "Memory", 0x40013004,        4, base=16,    bitRange=1-1
sfr = "CONFIG_02.ORE"         , "Memory", 0x40013004,        4, base=16,    bitRange=0-0

sfr = "CONFIG_03"             , "Memory", 0x40013008,        4, base=16
sfr = "CONFIG_03.IT"          , "Memory", 0x40013008,        4, base=16,    bitRange=5-7
sfr = "CONFIG_03.IE"          , "Memory", 0x40013008,        4, base=16,    bitRange=3-3
sfr = "CONFIG_03.OBE"         , "Memory", 0x40013008,        4, base=16,    bitRange=2-2
sfr = "CONFIG_03.IRE"         , "Memory", 0x40013008,        4, base=16,    bitRange=1-1
sfr = "CONFIG_03.ORE"         , "Memory", 0x40013008,        4, base=16,    bitRange=0-0

sfr = "CONFIG_04"             , "Memory", 0x4001300c,        4, base=16
sfr = "CONFIG_04.IT"          , "Memory", 0x4001300c,        4, base=16,    bitRange=5-7
sfr = "CONFIG_04.IE"          , "Memory", 0x4001300c,        4, base=16,    bitRange=3-3
sfr = "CONFIG_04.OBE"         , "Memory", 0x4001300c,        4, base=16,    bitRange=2-2
sfr = "CONFIG_04.IRE"         , "Memory", 0x4001300c,        4, base=16,    bitRange=1-1
sfr = "CONFIG_04.ORE"         , "Memory", 0x4001300c,        4, base=16,    bitRange=0-0

sfr = "CONFIG_05"             , "Memory", 0x40013010,        4, base=16
sfr = "CONFIG_05.IT"          , "Memory", 0x40013010,        4, base=16,    bitRange=5-7
sfr = "CONFIG_05.IE"          , "Memory", 0x40013010,        4, base=16,    bitRange=3-3
sfr = "CONFIG_05.OBE"         , "Memory", 0x40013010,        4, base=16,    bitRange=2-2
sfr = "CONFIG_05.IRE"         , "Memory", 0x40013010,        4, base=16,    bitRange=1-1
sfr = "CONFIG_05.ORE"         , "Memory", 0x40013010,        4, base=16,    bitRange=0-0

sfr = "CONFIG_06"             , "Memory", 0x40013014,        4, base=16
sfr = "CONFIG_06.IT"          , "Memory", 0x40013014,        4, base=16,    bitRange=5-7
sfr = "CONFIG_06.IE"          , "Memory", 0x40013014,        4, base=16,    bitRange=3-3
sfr = "CONFIG_06.OBE"         , "Memory", 0x40013014,        4, base=16,    bitRange=2-2
sfr = "CONFIG_06.IRE"         , "Memory", 0x40013014,        4, base=16,    bitRange=1-1
sfr = "CONFIG_06.ORE"         , "Memory", 0x40013014,        4, base=16,    bitRange=0-0

sfr = "CONFIG_07"             , "Memory", 0x40013018,        4, base=16
sfr = "CONFIG_07.IT"          , "Memory", 0x40013018,        4, base=16,    bitRange=5-7
sfr = "CONFIG_07.IE"          , "Memory", 0x40013018,        4, base=16,    bitRange=3-3
sfr = "CONFIG_07.OBE"         , "Memory", 0x40013018,        4, base=16,    bitRange=2-2
sfr = "CONFIG_07.IRE"         , "Memory", 0x40013018,        4, base=16,    bitRange=1-1
sfr = "CONFIG_07.ORE"         , "Memory", 0x40013018,        4, base=16,    bitRange=0-0

sfr = "CONFIG_08"             , "Memory", 0x4001301c,        4, base=16
sfr = "CONFIG_08.IT"          , "Memory", 0x4001301c,        4, base=16,    bitRange=5-7
sfr = "CONFIG_08.IE"          , "Memory", 0x4001301c,        4, base=16,    bitRange=3-3
sfr = "CONFIG_08.OBE"         , "Memory", 0x4001301c,        4, base=16,    bitRange=2-2
sfr = "CONFIG_08.IRE"         , "Memory", 0x4001301c,        4, base=16,    bitRange=1-1
sfr = "CONFIG_08.ORE"         , "Memory", 0x4001301c,        4, base=16,    bitRange=0-0

sfr = "CONFIG_09"             , "Memory", 0x40013020,        4, base=16
sfr = "CONFIG_09.IT"          , "Memory", 0x40013020,        4, base=16,    bitRange=5-7
sfr = "CONFIG_09.IE"          , "Memory", 0x40013020,        4, base=16,    bitRange=3-3
sfr = "CONFIG_09.OBE"         , "Memory", 0x40013020,        4, base=16,    bitRange=2-2
sfr = "CONFIG_09.IRE"         , "Memory", 0x40013020,        4, base=16,    bitRange=1-1
sfr = "CONFIG_09.ORE"         , "Memory", 0x40013020,        4, base=16,    bitRange=0-0

sfr = "CONFIG_10"             , "Memory", 0x40013024,        4, base=16
sfr = "CONFIG_10.IT"          , "Memory", 0x40013024,        4, base=16,    bitRange=5-7
sfr = "CONFIG_10.IE"          , "Memory", 0x40013024,        4, base=16,    bitRange=3-3
sfr = "CONFIG_10.OBE"         , "Memory", 0x40013024,        4, base=16,    bitRange=2-2
sfr = "CONFIG_10.IRE"         , "Memory", 0x40013024,        4, base=16,    bitRange=1-1
sfr = "CONFIG_10.ORE"         , "Memory", 0x40013024,        4, base=16,    bitRange=0-0

sfr = "CONFIG_11"             , "Memory", 0x40013028,        4, base=16
sfr = "CONFIG_11.IT"          , "Memory", 0x40013028,        4, base=16,    bitRange=5-7
sfr = "CONFIG_11.IE"          , "Memory", 0x40013028,        4, base=16,    bitRange=3-3
sfr = "CONFIG_11.OBE"         , "Memory", 0x40013028,        4, base=16,    bitRange=2-2
sfr = "CONFIG_11.IRE"         , "Memory", 0x40013028,        4, base=16,    bitRange=1-1
sfr = "CONFIG_11.ORE"         , "Memory", 0x40013028,        4, base=16,    bitRange=0-0

sfr = "CONFIG_12"             , "Memory", 0x4001302C,        4, base=16
sfr = "CONFIG_12.IT"          , "Memory", 0x4001302C,        4, base=16,    bitRange=5-7
sfr = "CONFIG_12.IE"          , "Memory", 0x4001302C,        4, base=16,    bitRange=3-3
sfr = "CONFIG_12.OBE"         , "Memory", 0x4001302C,        4, base=16,    bitRange=2-2
sfr = "CONFIG_12.IRE"         , "Memory", 0x4001302C,        4, base=16,    bitRange=1-1
sfr = "CONFIG_12.ORE"         , "Memory", 0x4001302C,        4, base=16,    bitRange=0-0

sfr = "CONFIG_13"             , "Memory", 0x40013030,        4, base=16
sfr = "CONFIG_13.IT"          , "Memory", 0x40013030,        4, base=16,    bitRange=5-7
sfr = "CONFIG_13.IE"          , "Memory", 0x40013030,        4, base=16,    bitRange=3-3
sfr = "CONFIG_13.OBE"         , "Memory", 0x40013030,        4, base=16,    bitRange=2-2
sfr = "CONFIG_13.IRE"         , "Memory", 0x40013030,        4, base=16,    bitRange=1-1
sfr = "CONFIG_13.ORE"         , "Memory", 0x40013030,        4, base=16,    bitRange=0-0

sfr = "CONFIG_14"             , "Memory", 0x40013034,        4, base=16
sfr = "CONFIG_14.IT"          , "Memory", 0x40013034,        4, base=16,    bitRange=5-7
sfr = "CONFIG_14.IE"          , "Memory", 0x40013034,        4, base=16,    bitRange=3-3
sfr = "CONFIG_14.OBE"         , "Memory", 0x40013034,        4, base=16,    bitRange=2-2
sfr = "CONFIG_14.IRE"         , "Memory", 0x40013034,        4, base=16,    bitRange=1-1
sfr = "CONFIG_14.ORE"         , "Memory", 0x40013034,        4, base=16,    bitRange=0-0

sfr = "CONFIG_15"             , "Memory", 0x40013038,        4, base=16
sfr = "CONFIG_15.IT"          , "Memory", 0x40013038,        4, base=16,    bitRange=5-7
sfr = "CONFIG_15.IE"          , "Memory", 0x40013038,        4, base=16,    bitRange=3-3
sfr = "CONFIG_15.OBE"         , "Memory", 0x40013038,        4, base=16,    bitRange=2-2
sfr = "CONFIG_15.IRE"         , "Memory", 0x40013038,        4, base=16,    bitRange=1-1
sfr = "CONFIG_15.ORE"         , "Memory", 0x40013038,        4, base=16,    bitRange=0-0

sfr = "CONFIG_16"             , "Memory", 0x4001303C,        4, base=16
sfr = "CONFIG_16.IT"          , "Memory", 0x4001303C,        4, base=16,    bitRange=5-7
sfr = "CONFIG_16.IE"          , "Memory", 0x4001303C,        4, base=16,    bitRange=3-3
sfr = "CONFIG_16.OBE"         , "Memory", 0x4001303C,        4, base=16,    bitRange=2-2
sfr = "CONFIG_16.IRE"         , "Memory", 0x4001303C,        4, base=16,    bitRange=1-1
sfr = "CONFIG_16.ORE"         , "Memory", 0x4001303C,        4, base=16,    bitRange=0-0

sfr = "CONFIG_17"             , "Memory", 0x40013040,        4, base=16
sfr = "CONFIG_17.IT"          , "Memory", 0x40013040,        4, base=16,    bitRange=5-7
sfr = "CONFIG_17.IE"          , "Memory", 0x40013040,        4, base=16,    bitRange=3-3
sfr = "CONFIG_17.OBE"         , "Memory", 0x40013040,        4, base=16,    bitRange=2-2
sfr = "CONFIG_17.IRE"         , "Memory", 0x40013040,        4, base=16,    bitRange=1-1
sfr = "CONFIG_17.ORE"         , "Memory", 0x40013040,        4, base=16,    bitRange=0-0

sfr = "CONFIG_18"             , "Memory", 0x40013044,        4, base=16
sfr = "CONFIG_18.IT"          , "Memory", 0x40013044,        4, base=16,    bitRange=5-7
sfr = "CONFIG_18.IE"          , "Memory", 0x40013044,        4, base=16,    bitRange=3-3
sfr = "CONFIG_18.OBE"         , "Memory", 0x40013044,        4, base=16,    bitRange=2-2
sfr = "CONFIG_18.IRE"         , "Memory", 0x40013044,        4, base=16,    bitRange=1-1
sfr = "CONFIG_18.ORE"         , "Memory", 0x40013044,        4, base=16,    bitRange=0-0

sfr = "CONFIG_19"             , "Memory", 0x40013048,        4, base=16
sfr = "CONFIG_19.IT"          , "Memory", 0x40013048,        4, base=16,    bitRange=5-7
sfr = "CONFIG_19.IE"          , "Memory", 0x40013048,        4, base=16,    bitRange=3-3
sfr = "CONFIG_19.OBE"         , "Memory", 0x40013048,        4, base=16,    bitRange=2-2
sfr = "CONFIG_19.IRE"         , "Memory", 0x40013048,        4, base=16,    bitRange=1-1
sfr = "CONFIG_19.ORE"         , "Memory", 0x40013048,        4, base=16,    bitRange=0-0

sfr = "CONFIG_20"             , "Memory", 0x4001304C,        4, base=16
sfr = "CONFIG_20.IT"          , "Memory", 0x4001304C,        4, base=16,    bitRange=5-7
sfr = "CONFIG_20.IE"          , "Memory", 0x4001304C,        4, base=16,    bitRange=3-3
sfr = "CONFIG_20.OBE"         , "Memory", 0x4001304C,        4, base=16,    bitRange=2-2
sfr = "CONFIG_20.IRE"         , "Memory", 0x4001304C,        4, base=16,    bitRange=1-1
sfr = "CONFIG_20.ORE"         , "Memory", 0x4001304C,        4, base=16,    bitRange=0-0

sfr = "CONFIG_21"             , "Memory", 0x40013050,        4, base=16
sfr = "CONFIG_21.IT"          , "Memory", 0x40013050,        4, base=16,    bitRange=5-7
sfr = "CONFIG_21.IE"          , "Memory", 0x40013050,        4, base=16,    bitRange=3-3
sfr = "CONFIG_21.OBE"         , "Memory", 0x40013050,        4, base=16,    bitRange=2-2
sfr = "CONFIG_21.IRE"         , "Memory", 0x40013050,        4, base=16,    bitRange=1-1
sfr = "CONFIG_21.ORE"         , "Memory", 0x40013050,        4, base=16,    bitRange=0-0

sfr = "CONFIG_22"             , "Memory", 0x40013054,        4, base=16
sfr = "CONFIG_22.IT"          , "Memory", 0x40013054,        4, base=16,    bitRange=5-7
sfr = "CONFIG_22.IE"          , "Memory", 0x40013054,        4, base=16,    bitRange=3-3
sfr = "CONFIG_22.OBE"         , "Memory", 0x40013054,        4, base=16,    bitRange=2-2
sfr = "CONFIG_22.IRE"         , "Memory", 0x40013054,        4, base=16,    bitRange=1-1
sfr = "CONFIG_22.ORE"         , "Memory", 0x40013054,        4, base=16,    bitRange=0-0

sfr = "CONFIG_23"             , "Memory", 0x40013058,        4, base=16
sfr = "CONFIG_23.IT"          , "Memory", 0x40013058,        4, base=16,    bitRange=5-7
sfr = "CONFIG_23.IE"          , "Memory", 0x40013058,        4, base=16,    bitRange=3-3
sfr = "CONFIG_23.OBE"         , "Memory", 0x40013058,        4, base=16,    bitRange=2-2
sfr = "CONFIG_23.IRE"         , "Memory", 0x40013058,        4, base=16,    bitRange=1-1
sfr = "CONFIG_23.ORE"         , "Memory", 0x40013058,        4, base=16,    bitRange=0-0

sfr = "CONFIG_24"             , "Memory", 0x4001305C,        4, base=16
sfr = "CONFIG_24.IT"          , "Memory", 0x4001305C,        4, base=16,    bitRange=5-7
sfr = "CONFIG_24.IE"          , "Memory", 0x4001305C,        4, base=16,    bitRange=3-3
sfr = "CONFIG_24.OBE"         , "Memory", 0x4001305C,        4, base=16,    bitRange=2-2
sfr = "CONFIG_24.IRE"         , "Memory", 0x4001305C,        4, base=16,    bitRange=1-1
sfr = "CONFIG_24.ORE"         , "Memory", 0x4001305C,        4, base=16,    bitRange=0-0

sfr = "CONFIG_25"             , "Memory", 0x40013060,        4, base=16
sfr = "CONFIG_25.IT"          , "Memory", 0x40013060,        4, base=16,    bitRange=5-7
sfr = "CONFIG_25.IE"          , "Memory", 0x40013060,        4, base=16,    bitRange=3-3
sfr = "CONFIG_25.OBE"         , "Memory", 0x40013060,        4, base=16,    bitRange=2-2
sfr = "CONFIG_25.IRE"         , "Memory", 0x40013060,        4, base=16,    bitRange=1-1
sfr = "CONFIG_25.ORE"         , "Memory", 0x40013060,        4, base=16,    bitRange=0-0

sfr = "CONFIG_26"             , "Memory", 0x40013064,        4, base=16
sfr = "CONFIG_26.IT"          , "Memory", 0x40013064,        4, base=16,    bitRange=5-7
sfr = "CONFIG_26.IE"          , "Memory", 0x40013064,        4, base=16,    bitRange=3-3
sfr = "CONFIG_26.OBE"         , "Memory", 0x40013064,        4, base=16,    bitRange=2-2
sfr = "CONFIG_26.IRE"         , "Memory", 0x40013064,        4, base=16,    bitRange=1-1
sfr = "CONFIG_26.ORE"         , "Memory", 0x40013064,        4, base=16,    bitRange=0-0

sfr = "CONFIG_27"             , "Memory", 0x40013068,        4, base=16
sfr = "CONFIG_27.IT"          , "Memory", 0x40013068,        4, base=16,    bitRange=5-7
sfr = "CONFIG_27.IE"          , "Memory", 0x40013068,        4, base=16,    bitRange=3-3
sfr = "CONFIG_27.OBE"         , "Memory", 0x40013068,        4, base=16,    bitRange=2-2
sfr = "CONFIG_27.IRE"         , "Memory", 0x40013068,        4, base=16,    bitRange=1-1
sfr = "CONFIG_27.ORE"         , "Memory", 0x40013068,        4, base=16,    bitRange=0-0

sfr = "CONFIG_28"             , "Memory", 0x4001306C,        4, base=16
sfr = "CONFIG_28.IT"          , "Memory", 0x4001306C,        4, base=16,    bitRange=5-7
sfr = "CONFIG_28.IE"          , "Memory", 0x4001306C,        4, base=16,    bitRange=3-3
sfr = "CONFIG_28.OBE"         , "Memory", 0x4001306C,        4, base=16,    bitRange=2-2
sfr = "CONFIG_28.IRE"         , "Memory", 0x4001306C,        4, base=16,    bitRange=1-1
sfr = "CONFIG_28.ORE"         , "Memory", 0x4001306C,        4, base=16,    bitRange=0-0

sfr = "CONFIG_29"             , "Memory", 0x40013070,        4, base=16
sfr = "CONFIG_29.IT"          , "Memory", 0x40013070,        4, base=16,    bitRange=5-7
sfr = "CONFIG_29.IE"          , "Memory", 0x40013070,        4, base=16,    bitRange=3-3
sfr = "CONFIG_29.OBE"         , "Memory", 0x40013070,        4, base=16,    bitRange=2-2
sfr = "CONFIG_29.IRE"         , "Memory", 0x40013070,        4, base=16,    bitRange=1-1
sfr = "CONFIG_29.ORE"         , "Memory", 0x40013070,        4, base=16,    bitRange=0-0

sfr = "CONFIG_30"             , "Memory", 0x40013074,        4, base=16
sfr = "CONFIG_30.IT"          , "Memory", 0x40013074,        4, base=16,    bitRange=5-7
sfr = "CONFIG_30.IE"          , "Memory", 0x40013074,        4, base=16,    bitRange=3-3
sfr = "CONFIG_30.OBE"         , "Memory", 0x40013074,        4, base=16,    bitRange=2-2
sfr = "CONFIG_30.IRE"         , "Memory", 0x40013074,        4, base=16,    bitRange=1-1
sfr = "CONFIG_30.ORE"         , "Memory", 0x40013074,        4, base=16,    bitRange=0-0

sfr = "CONFIG_31"             , "Memory", 0x40013078,        4, base=16
sfr = "CONFIG_31.IT"          , "Memory", 0x40013078,        4, base=16,    bitRange=5-7
sfr = "CONFIG_31.IE"          , "Memory", 0x40013078,        4, base=16,    bitRange=3-3
sfr = "CONFIG_31.OBE"         , "Memory", 0x40013078,        4, base=16,    bitRange=2-2
sfr = "CONFIG_31.IRE"         , "Memory", 0x40013078,        4, base=16,    bitRange=1-1
sfr = "CONFIG_31.ORE"         , "Memory", 0x40013078,        4, base=16,    bitRange=0-0

sfr = "CONFIG_32"             , "Memory", 0x4001307C,        4, base=16
sfr = "CONFIG_32.IT"          , "Memory", 0x4001307C,        4, base=16,    bitRange=5-7
sfr = "CONFIG_32.IE"          , "Memory", 0x4001307C,        4, base=16,    bitRange=3-3
sfr = "CONFIG_32.OBE"         , "Memory", 0x4001307C,        4, base=16,    bitRange=2-2
sfr = "CONFIG_32.IRE"         , "Memory", 0x4001307C,        4, base=16,    bitRange=1-1
sfr = "CONFIG_32.ORE"         , "Memory", 0x4001307C,        4, base=16,    bitRange=0-0

sfr = "INTR"                  , "Memory", 0x40013080,        4, base=16
sfr = "INTR.IT32"             , "Memory", 0x40013080,        4, base=16,    bitRange=0-31

sfr = "GPIN"                  , "Memory", 0x40013084,        4, base=16
sfr = "GPIN.GPIN32"           , "Memory", 0x40013084,        4, base=16,    bitRange=0-31

sfr = "GPOUT"                 , "Memory", 0x40013088,        4, base=16
sfr = "GPOUT.GPOUT32"         , "Memory", 0x40013088,        4, base=16,    bitRange=0-31

;
;		RTC
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "RTC"                 , "Memory", 0x40013000,        4, base=16

;
;		FROM
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "FROM"                 , "Memory", 0x40013000,        4, base=16

;
;		IAP Controller
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "IAP_DR"   , "Memory", 0x40016018,        4, base=16

sfr = "IAP_DR2"   , "Memory", 0x40016004,        4, base=16

sfr = "IAP_DR26"   , "Memory", 0x40016010,        4, base=16

sfr = "IAP_DR3"   , "Memory", 0x40016008,        4, base=16

sfr = "IAP_DR32"   , "Memory", 0x40016014,        4, base=16

sfr = "IAP_DR5"   , "Memory", 0x4001600C,        4, base=16

sfr = "IAP_DR_LENGTH"   , "Memory", 0x4001601C,        4, base=16

sfr = "IAP_IR"   , "Memory", 0x40016000,        4, base=16

sfr = "IAP_STATUS"   , "Memory", 0x40016028,        4, base=16
sfr = "IAP_STATUS.M3_IAP_INTR"   , "Memory", 0x40016028,        4, base=16,    bitRange=0-0
sfr = "IAP_STATUS.PRG_IAP_BUSY"   , "Memory", 0x40016028,        4, base=16,    bitRange=1-1
sfr = "IAP_STATUS.IDLE"   , "Memory", 0x40016028,        4, base=16,    bitRange=1-1
sfr = "IAP_STATUS.PRG_IAP_READY"   , "Memory", 0x40016028,        4, base=16,    bitRange=3-3

sfr = "IAP_TAP_CONTROL"   , "Memory", 0x40016024,        4, base=16
sfr = "IAP_TAP_CONTROL.TMS"   , "Memory", 0x40016024,        4, base=16,    bitRange=0-0
sfr = "IAP_TAP_CONTROL.TDI"   , "Memory", 0x40016024,        4, base=16,    bitRange=1-1
sfr = "IAP_TAP_CONTROL.TCK"   , "Memory", 0x40016024,        4, base=16,    bitRange=2-2
sfr = "IAP_TAP_CONTROL.TRSTB"   , "Memory", 0x40016024,        4, base=16,    bitRange=3-3
sfr = "IAP_TAP_CONTROL.TDO"   , "Memory", 0x40016024,        4, base=16,    bitRange=4-4
sfr = "IAP_TAP_CONTROL.IAP_ENABLE"   , "Memory", 0x40016024,        4, base=16,    bitRange=5-5
sfr = "IAP_TAP_CONTROL.CURRSTATE"   , "Memory", 0x40016024,        4, base=16,    bitRange=6-9
sfr = "IAP_TAP_CONTROL.PRG_IAP_M3DONE"   , "Memory", 0x40016024,        4, base=16,    bitRange=10-10
sfr = "IAP_TAP_CONTROL.PRG_IAP_M3ACK"   , "Memory", 0x40016024,        4, base=16,    bitRange=11-11

sfr = "IAP_TAP_NEW_STATE"   , "Memory", 0x40016020,        4, base=16
sfr = "IAP_TAP_NEW_STATE.STATE"   , "Memory", 0x40016020,        4, base=16,    bitRange=0-3
sfr = "IAP_TAP_NEW_STATE.DELAYCOUNT"   , "Memory", 0x40016020,        4, base=16,    bitRange=4-10
sfr = "IAP_TAP_NEW_STATE.BUSYINTEN"   , "Memory", 0x40016020,        4, base=16,    bitRange=11-11


;
;		Analog Conversion Engine
;
;     Name                      			Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      			----      -------     --------  ----------- --------

sfr = "NOP"   							, "Memory", 0x40020000,        4, base=16
sfr = "NOP.NOP"   						, "Memory", 0x40020000,        4, base=16,    bitRange=0-7

sfr = "SSE_TS_CTRL"   					, "Memory", 0x40020004,        4, base=16
sfr = "SSE_TS_CTRL.SSE_SRAM_ENABLE" 	, "Memory", 0x40020004,        4, base=16,    bitRange=1-1
sfr = "SSE_TS_CTRL.TS_ENABLE"   		, "Memory", 0x40020004,        4, base=16,    bitRange=0-0

sfr = "ADC_SYNC_CONV"   				, "Memory", 0x40020008,        4, base=16
sfr = "ADC_SYNC_CONV.CONVWAIT2"   		, "Memory", 0x40020008,        4, base=16,    bitRange=6-6
sfr = "ADC_SYNC_CONV.CONVWAIT1"   		, "Memory", 0x40020008,        4, base=16,    bitRange=5-5
sfr = "ADC_SYNC_CONV.CONVWAIT0"   		, "Memory", 0x40020008,        4, base=16,    bitRange=4-4
sfr = "ADC_SYNC_CONV.ADCSTART2"   		, "Memory", 0x40020008,        4, base=16,    bitRange=2-2
sfr = "ADC_SYNC_CONV.ADCSTART1"   		, "Memory", 0x40020008,        4, base=16,    bitRange=1-1
sfr = "ADC_SYNC_CONV.ADCSTART0"   		, "Memory", 0x40020008,        4, base=16,    bitRange=0-0

sfr = "ANA_COMM_CTRL"   				, "Memory", 0x4002000C,        4, base=16
sfr = "ANA_COMM_CTRL.ACB_RESETN"   		, "Memory", 0x4002000C,        4, base=16,    bitRange=4-4
sfr = "ANA_COMM_CTRL.ABPOWERON"   		, "Memory", 0x4002000C,        4, base=16,    bitRange=3-3
sfr = "ANA_COMM_CTRL.PWRDWN"   			, "Memory", 0x4002000C,        4, base=16,    bitRange=2-2
sfr = "ANA_COMM_CTRL.ADCRESET"   		, "Memory", 0x4002000C,        4, base=16,    bitRange=1-1
sfr = "ANA_COMM_CTRL.VREFSEL"   		, "Memory", 0x4002000C,        4, base=16,    bitRange=0-0

sfr = "DAC_SYNC_CTRL"   				, "Memory", 0x40020010,        4, base=16
sfr = "DAC_SYNC_CTRL.DAC2_SYNC_EN"  	, "Memory", 0x40020010,        4, base=16,    bitRange=6-6
sfr = "DAC_SYNC_CTRL.DAC1_SYNC_EN"  	, "Memory", 0x40020010,        4, base=16,    bitRange=5-5
sfr = "DAC_SYNC_CTRL.DAC0_SYNC_EN"  	, "Memory", 0x40020010,        4, base=16,    bitRange=4-4
sfr = "DAC_SYNC_CTRL.DAC2_SYNC_UPDATE"  , "Memory", 0x40020010,        4, base=16,    bitRange=2-2
sfr = "DAC_SYNC_CTRL.DAC1_SYNC_UPDATE"  , "Memory", 0x40020010,        4, base=16,    bitRange=1-1
sfr = "DAC_SYNC_CTRL.DAC0_SYNC_UPDATE"  , "Memory", 0x40020010,        4, base=16,    bitRange=0-0

sfr = "PDMA_REQUEST"   					, "Memory", 0x40020014,        4, base=16
sfr = "PDMA_REQUEST.NUM_WORDS"   		, "Memory", 0x40020014,        4, base=16,    bitRange=0-7

sfr = "PC0_LO"   						, "Memory", 0x40020040,        4, base=16
sfr = "PC0_LO.PC"   					, "Memory", 0x40020040,        4, base=16,    bitRange=0-7

sfr = "PC0_HI"   						, "Memory", 0x40020044,        4, base=16
sfr = "PC0_HI.PC"   					, "Memory", 0x40020044,        4, base=16,    bitRange=0-7

sfr = "PC0_CTRL"   						, "Memory", 0x40020048,        4, base=16
sfr = "PC0_CTRL.PC0_EN"   				, "Memory", 0x40020048,        4, base=16,    bitRange=0-0

sfr = "PC0_DLY"   						, "Memory", 0x4002004C,        4, base=16
sfr = "PC0_DLY.DLY"   					, "Memory", 0x4002004C,        4, base=16,    bitRange=0-7

sfr = "ADC0_CONV_CTRL"   				, "Memory", 0x40020050,        4, base=16
sfr = "ADC0_CONV_CTRL.ADCSTART"   		, "Memory", 0x40020050,        4, base=16,    bitRange=7-7
sfr = "ADC0_CONV_CTRL.CONVWAIT"   		, "Memory", 0x40020050,        4, base=16,    bitRange=6-6
sfr = "ADC0_CONV_CTRL.AMUXSEL"   		, "Memory", 0x40020050,        4, base=16,    bitRange=0-4

sfr = "ADC0_STC"   						, "Memory", 0x40020054,        4, base=16
sfr = "ADC0_STC.STC"   					, "Memory", 0x40020054,        4, base=16,    bitRange=0-7

sfr = "ADC0_TVC"   						, "Memory", 0x40020058,        4, base=16
sfr = "ADC0_TVC.TVC"   					, "Memory", 0x40020058,        4, base=16,    bitRange=0-7

sfr = "ADC0_MISC_CTRL"   				, "Memory", 0x4002005C,        4, base=16
sfr = "ADC0_MISC_CTRL.PWRDWN"   		, "Memory", 0x4002005C,        4, base=16,    bitRange=5-5
sfr = "ADC0_MISC_CTRL.ADCRESET"   		, "Memory", 0x4002005C,        4, base=16,    bitRange=4-4
sfr = "ADC0_MISC_CTRL.MODE"   			, "Memory", 0x4002005C,        4, base=16,    bitRange=0-3

sfr = "DAC0_CTRL"   					, "Memory", 0x40020060,        4, base=16
sfr = "DAC0_CTRL.REG_SEL"   			, "Memory", 0x40020060,        4, base=16,    bitRange=6-6
sfr = "DAC0_CTRL.EN"   					, "Memory", 0x40020060,        4, base=16,    bitRange=5-5
sfr = "DAC0_CTRL.SW_OBD"   				, "Memory", 0x40020060,        4, base=16,    bitRange=4-4
sfr = "DAC0_CTRL.DACRES"   				, "Memory", 0x40020060,        4, base=16,    bitRange=2-3
sfr = "DAC0_CTRL.DACSEL"   				, "Memory", 0x40020060,        4, base=16,    bitRange=0-1

sfr = "DAC0_BYTE0"   					, "Memory", 0x40020064,        4, base=16
sfr = "DAC0_BYTE0.BYTE"   				, "Memory", 0x40020064,        4, base=16,    bitRange=0-7

sfr = "DAC0_BYTE1"   					, "Memory", 0x40020068,        4, base=16
sfr = "DAC0_BYTE1.BYTE"   				, "Memory", 0x40020068,        4, base=16,    bitRange=0-7

sfr = "DAC0_BYTE2"   					, "Memory", 0x4002006C,        4, base=16
sfr = "DAC0_BYTE2.BYTE"   				, "Memory", 0x4002006C,        4, base=16,    bitRange=0-7

sfr = "LC0"   							, "Memory", 0x40020070,        4, base=16
sfr = "LC0.LPCNT"   					, "Memory", 0x40020070,        4, base=16,    bitRange=0-7

sfr = "LC0_JMP_LO"   					, "Memory", 0x40020074,        4, base=16
sfr = "LC0_JMP_LO.ADDR"   				, "Memory", 0x40020074,        4, base=16,    bitRange=0-7

sfr = "LC0_JMP_HI"   					, "Memory", 0x40020078,        4, base=16
sfr = "LC0_JMP_HI.ADDR"   				, "Memory", 0x40020078,        4, base=16,    bitRange=0-7

sfr = "PC0_FLAGS"   					, "Memory", 0x4002007C,        4, base=16
sfr = "PC0_FLAGS.GP3"   				, "Memory", 0x4002007C,        4, base=16,    bitRange=3-3
sfr = "PC0_FLAGS.GP2"   				, "Memory", 0x4002007C,        4, base=16,    bitRange=2-2
sfr = "PC0_FLAGS.GP1"   				, "Memory", 0x4002007C,        4, base=16,    bitRange=1-1
sfr = "PC0_FLAGS.GP0"   				, "Memory", 0x4002007C,        4, base=16,    bitRange=0-0

sfr = "PC1_LO"   						, "Memory", 0x40020080,        4, base=16
sfr = "PC1_LO.PC"   					, "Memory", 0x40020080,        4, base=16,    bitRange=0-7

sfr = "PC1_HI"   						, "Memory", 0x40020084,        4, base=16
sfr = "PC1_HI.PC"   					, "Memory", 0x40020084,        4, base=16,    bitRange=0-7

sfr = "PC1_CTRL"   						, "Memory", 0x40020088,        4, base=16
sfr = "PC1_CTRL.PC1_EN"   				, "Memory", 0x40020088,        4, base=16,    bitRange=0-0

sfr = "PC1_DLY"   						, "Memory", 0x4002008C,        4, base=16
sfr = "PC1_DLY.DLY"   					, "Memory", 0x4002008C,        4, base=16,    bitRange=0-7

sfr = "ADC1_CONV_CTRL"   				, "Memory", 0x40020090,        4, base=16
sfr = "ADC1_CONV_CTRL.ADCSTART"   		, "Memory", 0x40020090,        4, base=16,    bitRange=7-7
sfr = "ADC1_CONV_CTRL.CONVWAIT"   		, "Memory", 0x40020090,        4, base=16,    bitRange=6-6
sfr = "ADC1_CONV_CTRL.AMUXSEL"   		, "Memory", 0x40020090,        4, base=16,    bitRange=0-4

sfr = "ADC1_STC"   						, "Memory", 0x40020094,        4, base=16
sfr = "ADC1_STC.STC"   					, "Memory", 0x40020094,        4, base=16,    bitRange=0-7

sfr = "ADC1_TVC"   						, "Memory", 0x40020098,        4, base=16
sfr = "ADC1_TVC.TVC"   					, "Memory", 0x40020098,        4, base=16,    bitRange=0-7

sfr = "ADC1_MISC_CTRL"   				, "Memory", 0x4002009C,        4, base=16
sfr = "ADC1_MISC_CTRL.PWRDWN"   		, "Memory", 0x4002009C,        4, base=16,    bitRange=5-5
sfr = "ADC1_MISC_CTRL.ADCRESET"   		, "Memory", 0x4002009C,        4, base=16,    bitRange=4-4
sfr = "ADC1_MISC_CTRL.MODE"   			, "Memory", 0x4002009C,        4, base=16,    bitRange=0-3

sfr = "DAC1_CTRL"   					, "Memory", 0x400200A0,        4, base=16
sfr = "DAC1_CTRL.EN"   					, "Memory", 0x400200A0,        4, base=16,    bitRange=5-5
sfr = "DAC1_CTRL.SW_OBD"   				, "Memory", 0x400200A0,        4, base=16,    bitRange=4-4
sfr = "DAC1_CTRL.DACRES"   				, "Memory", 0x400200A0,        4, base=16,    bitRange=2-3
sfr = "DAC1_CTRL.DACSEL"   				, "Memory", 0x400200A0,        4, base=16,    bitRange=0-1

sfr = "DAC1_BYTE0"   					, "Memory", 0x400200A4,        4, base=16
sfr = "DAC1_BYTE0.BYTE"   				, "Memory", 0x400200A4,        4, base=16,    bitRange=0-7

sfr = "DAC1_BYTE1"   					, "Memory", 0x400200A8,        4, base=16
sfr = "DAC1_BYTE1.BYTE"   				, "Memory", 0x400200A8,        4, base=16,    bitRange=0-7

sfr = "DAC1_BYTE2"   					, "Memory", 0x400200AC,        4, base=16
sfr = "DAC1_BYTE2.BYTE"   				, "Memory", 0x400200AC,        4, base=16,    bitRange=0-7

sfr = "LC1"   							, "Memory", 0x400200B0,        4, base=16
sfr = "LC1.LPCNT"   					, "Memory", 0x400200B0,        4, base=16,    bitRange=0-7

sfr = "LC1_JMP_LO"   					, "Memory", 0x400200B4,        4, base=16
sfr = "LC1_JMP_LO.ADDR"   				, "Memory", 0x400200B4,        4, base=16,    bitRange=0-7

sfr = "LC1_JMP_HI"   					, "Memory", 0x400200B8,        4, base=16
sfr = "LC1_JMP_HI.ADDR"   				, "Memory", 0x400200B8,        4, base=16,    bitRange=0-7

sfr = "PC1_FLAGS"   					, "Memory", 0x400200BC,        4, base=16
sfr = "PC1_FLAGS.GP3"   				, "Memory", 0x400200BC,        4, base=16,    bitRange=3-3
sfr = "PC1_FLAGS.GP2"   				, "Memory", 0x400200BC,        4, base=16,    bitRange=2-2
sfr = "PC1_FLAGS.GP1"   				, "Memory", 0x400200BC,        4, base=16,    bitRange=1-1
sfr = "PC1_FLAGS.GP0"   				, "Memory", 0x400200BC,        4, base=16,    bitRange=0-0

sfr = "PC2_LO"   						, "Memory", 0x400200C0,        4, base=16
sfr = "PC2_LO.PC"   					, "Memory", 0x400200C0,        4, base=16,    bitRange=0-7

sfr = "PC2_HI"   						, "Memory", 0x400200C4,        4, base=16
sfr = "PC2_HI.PC"   					, "Memory", 0x400200C4,        4, base=16,    bitRange=0-7

sfr = "PC2_CTRL"   						, "Memory", 0x400200C8,        4, base=16
sfr = "PC2_CTRL.PC2_EN"   				, "Memory", 0x400200C8,        4, base=16,    bitRange=0-0

sfr = "PC2_DLY"   						, "Memory", 0x400200CC,        4, base=16
sfr = "PC2_DLY.DLY"   					, "Memory", 0x400200CC,        4, base=16,    bitRange=0-7

sfr = "ADC2_CONV_CTRL"   				, "Memory", 0x400200D0,        4, base=16
sfr = "ADC2_CONV_CTRL.ADCSTART"   		, "Memory", 0x400200D0,        4, base=16,    bitRange=7-7
sfr = "ADC2_CONV_CTRL.CONVWAIT"   		, "Memory", 0x400200D0,        4, base=16,    bitRange=6-6
sfr = "ADC2_CONV_CTRL.AMUXSEL"   		, "Memory", 0x400200D0,        4, base=16,    bitRange=0-4

sfr = "ADC2_STC"   						, "Memory", 0x400200D4,        4, base=16
sfr = "ADC2_STC.STC"   					, "Memory", 0x400200D4,        4, base=16,    bitRange=0-7

sfr = "ADC2_TVC"   						, "Memory", 0x400200D8,        4, base=16
sfr = "ADC2_TVC.TVC"   					, "Memory", 0x400200D8,        4, base=16,    bitRange=0-7

sfr = "ADC2_MISC_CTRL"   				, "Memory", 0x400200DC,        4, base=16
sfr = "ADC2_MISC_CTRL.PWRDWN"   		, "Memory", 0x400200DC,        4, base=16,    bitRange=5-5
sfr = "ADC2_MISC_CTRL.ADCRESET"   		, "Memory", 0x400200DC,        4, base=16,    bitRange=4-4
sfr = "ADC2_MISC_CTRL.MODE"   			, "Memory", 0x400200DC,        4, base=16,    bitRange=0-3

sfr = "DAC2_CTRL"   					, "Memory", 0x400200E0,        4, base=16
sfr = "DAC2_CTRL.EN"   					, "Memory", 0x400200E0,        4, base=16,    bitRange=5-5
sfr = "DAC2_CTRL.SW_OBD"   				, "Memory", 0x400200E0,        4, base=16,    bitRange=4-4
sfr = "DAC2_CTRL.DACRES"   				, "Memory", 0x400200E0,        4, base=16,    bitRange=2-3
sfr = "DAC2_CTRL.DACSEL"   				, "Memory", 0x400200E0,        4, base=16,    bitRange=0-1

sfr = "DAC2_BYTE0"   					, "Memory", 0x400200E4,        4, base=16
sfr = "DAC2_BYTE0.BYTE"   				, "Memory", 0x400200E4,        4, base=16,    bitRange=0-7

sfr = "DAC2_BYTE1"   					, "Memory", 0x400200E8,        4, base=16
sfr = "DAC2_BYTE1.BYTE"   				, "Memory", 0x400200E8,        4, base=16,    bitRange=0-7

sfr = "DAC2_BYTE2"   					, "Memory", 0x400200EC,        4, base=16
sfr = "DAC2_BYTE2.BYTE"  				, "Memory", 0x400200EC,        4, base=16,    bitRange=0-7

sfr = "LC2"   							, "Memory", 0x400200F0,        4, base=16
sfr = "LC2.LPCNT"   					, "Memory", 0x400200F0,        4, base=16,    bitRange=0-7

sfr = "LC2_JMP_LO"   					, "Memory", 0x400200F4,        4, base=16
sfr = "LC2_JMP_LO.ADDR"   				, "Memory", 0x400200F4,        4, base=16,    bitRange=0-7

sfr = "LC2_JMP_HI"   					, "Memory", 0x400200F8,        4, base=16
sfr = "LC2_JMP_HI.ADDR"   				, "Memory", 0x400200F8,        4, base=16,    bitRange=0-7

sfr = "PC2_FLAGS"   					, "Memory", 0x400200FC,        4, base=16
sfr = "PC2_FLAGS.GP3"   				, "Memory", 0x400200FC,        4, base=16,    bitRange=3-3
sfr = "PC2_FLAGS.GP2"   				, "Memory", 0x400200FC,        4, base=16,    bitRange=2-2
sfr = "PC2_FLAGS.GP1"   				, "Memory", 0x400200FC,        4, base=16,    bitRange=1-1
sfr = "PC2_FLAGS.GP0"   				, "Memory", 0x400200FC,        4, base=16,    bitRange=0-0
sfr = "PC2_FLAGS.ADDR"   				, "Memory", 0x400200FC,        4, base=16,    bitRange=0-7
sfr = "PC2_FLAGS.ADDR"   				, "Memory", 0x400200FC,        4, base=16,    bitRange=0-7

sfr = "SSE_RAM_LO_IDATA"   				, "Memory", 0x40020108,        4, base=16
sfr = "SSE_RAM_LO_IDATA.DATA"   		, "Memory", 0x40020108,        4, base=16,    bitRange=0-7

sfr = "SSE_RAM_HI_IDATA"   				, "Memory", 0x4002010C,        4, base=16
sfr = "SSE_RAM_HI_IDATA.DATA"   		, "Memory", 0x4002010C,        4, base=16,    bitRange=0-7

sfr = "ACB_DATA_FIRST"   				, "Memory", 0x40020200,        4, base=16
sfr = "ACB_DATA_FIRST.DATA"   			, "Memory", 0x40020200,        4, base=16,    bitRange=0-7

sfr = "ACB_DATA_LAST"   				, "Memory", 0x400203FC,        4, base=16
sfr = "ACB_DATA_LAST.DATA"   			, "Memory", 0x400203FC,        4, base=16,    bitRange=0-7

sfr = "SSE_PC0"   						, "Memory", 0x40020410,        4, base=16
sfr = "SSE_PC0.PC"   					, "Memory", 0x40020410,        4, base=16,    bitRange=0-8

sfr = "SSE_PC1"   						, "Memory", 0x40020414,        4, base=16
sfr = "SSE_PC1.PC"   					, "Memory", 0x40020414,        4, base=16,    bitRange=0-8

sfr = "SSE_PC2"   						, "Memory", 0x40020418,        4, base=16
sfr = "SSE_PC2.PC"   					, "Memory", 0x40020418,        4, base=16,    bitRange=0-8

sfr = "SSE_DAC0_BYTES01"   				, "Memory", 0x40020500,        4, base=16
sfr = "SSE_DAC0_BYTES01.DAC0_16BITS"   	, "Memory", 0x40020500,        4, base=16,    bitRange=0-15

sfr = "SSE_DAC1_BYTES01"   				, "Memory", 0x40020504,        4, base=16
sfr = "SSE_DAC1_BYTES01.DAC1_16BITS"   	, "Memory", 0x40020504,        4, base=16,    bitRange=0-15

sfr = "SSE_DAC2_BYTES01"   				, "Memory", 0x40020508,        4, base=16
sfr = "SSE_DAC2_BYTES01.DAC2_16BITS"   	, "Memory", 0x40020508,        4, base=16,    bitRange=0-15

sfr = "SSE_ADC0_RESULTS"   				, "Memory", 0x40020600,        4, base=16
sfr = "SSE_ADC0_RESULTS.ADC0_Results"   , "Memory", 0x40020600,        4, base=16,    bitRange=0-15

sfr = "SSE_ADC1_RESULTS"   				, "Memory", 0x40020604,        4, base=16
sfr = "SSE_ADC1_RESULTS.ADC1_Results"   , "Memory", 0x40020604,        4, base=16,    bitRange=0-15

sfr = "SSE_ADC2_RESULTS"   				, "Memory", 0x40020608,        4, base=16
sfr = "SSE_ADC2_RESULTS.ADC2_Results"   , "Memory", 0x40020608,        4, base=16,    bitRange=0-15

sfr = "SSE_PDMA_DATAIN"   				, "Memory", 0x40020700,        4, base=16
sfr = "SSE_PDMA_DATAIN.ADDRESS"   		, "Memory", 0x40020700,        4, base=16,    bitRange=16-27
sfr = "SSE_PDMA_DATAIN.DATA"   			, "Memory", 0x40020700,        4, base=16,    bitRange=0-15

sfr = "SSE_RAM_DATA_FIRST"   			, "Memory", 0x40020800,        4, base=16
sfr = "SSE_RAM_DATA_FIRST.DATA"   		, "Memory", 0x40020800,        4, base=16,    bitRange=0-15

sfr = "SSE_RAM_DATA_LAST"   			, "Memory", 0x40020FFC,        4, base=16
sfr = "SSE_RAM_DATA_LAST.DATA"   		, "Memory", 0x40020FFC,        4, base=16,    bitRange=0-15

sfr = "ADC0_STATUS"   					, "Memory", 0x40021000,        4, base=16
sfr = "ADC0_STATUS.CALIBRATE"   		, "Memory", 0x40021000,        4, base=16,    bitRange=15-15
sfr = "ADC0_STATUS.SAMPLE"   			, "Memory", 0x40021000,        4, base=16,    bitRange=14-14
sfr = "ADC0_STATUS.BUSY"   				, "Memory", 0x40021000,        4, base=16,    bitRange=13-13
sfr = "ADC0_STATUS.DATAVALID"   		, "Memory", 0x40021000,        4, base=16,    bitRange=12-12
sfr = "ADC0_STATUS.RESULT"   			, "Memory", 0x40021000,        4, base=16,    bitRange=0-11

sfr = "ADC1_STATUS"   					, "Memory", 0x40021004,        4, base=16
sfr = "ADC1_STATUS.CALIBRATE"   		, "Memory", 0x40021004,        4, base=16,    bitRange=15-15
sfr = "ADC1_STATUS.SAMPLE"   			, "Memory", 0x40021004,        4, base=16,    bitRange=14-14
sfr = "ADC1_STATUS.BUSY"   				, "Memory", 0x40021004,        4, base=16,    bitRange=13-13
sfr = "ADC1_STATUS.DATAVALID"   		, "Memory", 0x40021004,        4, base=16,    bitRange=12-12
sfr = "ADC1_STATUS.RESULT"   			, "Memory", 0x40021004,        4, base=16,    bitRange=0-11

sfr = "ADC2_STATUS"   					, "Memory", 0x40021008,        4, base=16
sfr = "ADC2_STATUS.CALIBRATE"   		, "Memory", 0x40021008,        4, base=16,    bitRange=15-15
sfr = "ADC2_STATUS.SAMPLE"   			, "Memory", 0x40021008,        4, base=16,    bitRange=14-14
sfr = "ADC2_STATUS.BUSY"   				, "Memory", 0x40021008,        4, base=16,    bitRange=13-13
sfr = "ADC2_STATUS.DATAVALID"   		, "Memory", 0x40021008,        4, base=16,    bitRange=12-12
sfr = "ADC2_STATUS.RESULT"   			, "Memory", 0x40021008,        4, base=16,    bitRange=0-11

sfr = "COMPARATOR_STATUS"   			, "Memory", 0x4002100C,        4, base=16
sfr = "COMPARATOR_STATUS.COMPARATOR"   	, "Memory", 0x4002100C,        4, base=16,    bitRange=0-11

sfr = "SSE_IRQ_EN"   					, "Memory", 0x40021200,        4, base=16
sfr = "SSE_IRQ_EN.IRQ_EN"   			, "Memory", 0x40021200,        4, base=16,    bitRange=0-20

sfr = "SSE_IRQ"   						, "Memory", 0x40021204,        4, base=16
sfr = "SSE_IRQ.ADC2_CAL_RISE"   		, "Memory", 0x40021204,        4, base=16,    bitRange=20-20
sfr = "SSE_IRQ.ADC1_CAL_RISE"   		, "Memory", 0x40021204,        4, base=16,    bitRange=19-19
sfr = "SSE_IRQ.ADC0_CAL_RISE"   		, "Memory", 0x40021204,        4, base=16,    bitRange=18-18
sfr = "SSE_IRQ.ADC2_CAL_FALL"   		, "Memory", 0x40021204,        4, base=16,    bitRange=17-17
sfr = "SSE_IRQ.ADC1_CAL_FALL"   		, "Memory", 0x40021204,        4, base=16,    bitRange=16-16
sfr = "SSE_IRQ.ADC0_CAL_FALL"   		, "Memory", 0x40021204,        4, base=16,    bitRange=15-15
sfr = "SSE_IRQ.ADC2_DV_RISE"   			, "Memory", 0x40021204,        4, base=16,    bitRange=14-14
sfr = "SSE_IRQ.ADC1_DV_RISE"   			, "Memory", 0x40021204,        4, base=16,    bitRange=13-13
sfr = "SSE_IRQ.ADC0_DV_RISE"   			, "Memory", 0x40021204,        4, base=16,    bitRange=12-12
sfr = "SSE_IRQ.PC2_FLAGS"   			, "Memory", 0x40021204,        4, base=16,    bitRange=8-11
sfr = "SSE_IRQ.PC1_FLAGS"   			, "Memory", 0x40021204,        4, base=16,    bitRange=4-7
sfr = "SSE_IRQ.PC0_FLAGS"   			, "Memory", 0x40021204,        4, base=16,    bitRange=0-3

sfr = "SSE_IRQ_CLR"   					, "Memory", 0x40021208,        4, base=16
sfr = "SSE_IRQ_CLR.IRQ_CLR"   			, "Memory", 0x40021208,        4, base=16,    bitRange=0-20

sfr = "COMP_IRQ_EN"   					, "Memory", 0x4002120C,        4, base=16
sfr = "COMP_IRQ_EN.IRQ_EN"   			, "Memory", 0x4002120C,        4, base=16,    bitRange=0-23

sfr = "COMP_IRQ"   						, "Memory", 0x40021210,        4, base=16
sfr = "COMP_IRQ.COMP_RISE"   			, "Memory", 0x40021210,        4, base=16,    bitRange=12-23
sfr = "COMP_IRQ.COMP_FALL"   			, "Memory", 0x40021210,        4, base=16,    bitRange=0-11

sfr = "COMP_IRQ_CLR"   					, "Memory", 0x40021214,        4, base=16
sfr = "COMP_IRQ_CLR.IRQ_CLR"   			, "Memory", 0x40021214,        4, base=16,    bitRange=0-23

sfr = "PPE_FIFO_IRQ_EN"   				, "Memory", 0x40021218,        4, base=16
sfr = "PPE_FIFO_IRQ_EN.IRQ_EN"   		, "Memory", 0x40021218,        4, base=16,    bitRange=0-8

sfr = "PPE_FIFO_IRQ"   					, "Memory", 0x4002121C,        4, base=16
sfr = "PPE_FIFO_IRQ.EMPTY2_FALL"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=8-8
sfr = "PPE_FIFO_IRQ.AFULL2_RISE"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=7-7
sfr = "PPE_FIFO_IRQ.FULL2_RISE"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=6-6
sfr = "PPE_FIFO_IRQ.EMPTY1_FALL"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=5-5
sfr = "PPE_FIFO_IRQ.AFULL1_RISE"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=4-4
sfr = "PPE_FIFO_IRQ.FULL1_RISE"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=3-3
sfr = "PPE_FIFO_IRQ.EMPTY0_FALL"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=2-2
sfr = "PPE_FIFO_IRQ.AFULL0_RISE"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=1-1
sfr = "PPE_FIFO_IRQ.FULL0_RISE"   		, "Memory", 0x4002121C,        4, base=16,    bitRange=0-0

sfr = "PPE_FIFO_IRQ_CLR"   				, "Memory", 0x40021220,        4, base=16
sfr = "PPE_FIFO_IRQ_CLR.IRQ_CLR"   		, "Memory", 0x40021220,        4, base=16,    bitRange=0-8

sfr = "PPE_FLAGS0_IRQ_EN"   			, "Memory", 0x40021224,        4, base=16
sfr = "PPE_FLAGS0_IRQ_EN.IRQ_EN"   		, "Memory", 0x40021224,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS0_IRQ"   				, "Memory", 0x40021228,        4, base=16
sfr = "PPE_FLAGS0_IRQ.FLAGS0_RISE"   	, "Memory", 0x40021228,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS0_IRQ_CLR"   			, "Memory", 0x4002122C,        4, base=16
sfr = "PPE_FLAGS0_IRQ_CLR.IRQ_CLR"   	, "Memory", 0x4002122C,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS1_IRQ_EN"   			, "Memory", 0x40021230,        4, base=16
sfr = "PPE_FLAGS1_IRQ_EN.IRQ_EN"   		, "Memory", 0x40021230,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS1_IRQ"   				, "Memory", 0x40021234,        4, base=16
sfr = "PPE_FLAGS1_IRQ.FLAGS1_RISE"   	, "Memory", 0x40021234,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS1_IRQ_CLR"   			, "Memory", 0x40021238,        4, base=16
sfr = "PPE_FLAGS1_IRQ_CLR.IRQ_CLR"   	, "Memory", 0x40021238,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS2_IRQ_EN"   			, "Memory", 0x4002123C,        4, base=16
sfr = "PPE_FLAGS2_IRQ_EN.IRQ_EN"   		, "Memory", 0x4002123C,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS2_IRQ"   				, "Memory", 0x40021240,        4, base=16
sfr = "PPE_FLAGS2_IRQ.FLAGS2_RISE"   	, "Memory", 0x40021240,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS2_IRQ_CLR"   			, "Memory", 0x40021244,        4, base=16
sfr = "PPE_FLAGS2_IRQ_CLR.IRQ_CLR"   	, "Memory", 0x40021244,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS3_IRQ_EN"   			, "Memory", 0x40021248,        4, base=16
sfr = "PPE_FLAGS3_IRQ_EN.IRQ_EN"   		, "Memory", 0x40021248,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS3_IRQ"   				, "Memory", 0x4002124C,        4, base=16
sfr = "PPE_FLAGS3_IRQ.FLAGS3_RISE"   	, "Memory", 0x4002124C,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS3_IRQ_CLR"   			, "Memory", 0x40021250,        4, base=16
sfr = "PPE_FLAGS3_IRQ_CLR.IRQ_CLR"   	, "Memory", 0x40021250,        4, base=16,    bitRange=0-31

sfr = "PPE_SFFLAGS_IRQ_EN"   			, "Memory", 0x40021254,        4, base=16
sfr = "PPE_SFFLAGS_IRQ_EN.IRQ_EN"   	, "Memory", 0x40021254,        4, base=16,    bitRange=0-31

sfr = "PPE_SFFLAGS_IRQ"   				, "Memory", 0x40021258,        4, base=16
sfr = "PPE_SFFLAGS_IRQ.SFFLAGS_RISE"   	, "Memory", 0x40021258,        4, base=16,    bitRange=0-31

sfr = "PPE_SFFLAGS_IRQ_CLR"   			, "Memory", 0x4002125C,        4, base=16
sfr = "PPE_SFFLAGS_IRQ_CLR.IRQ_CLR"   	, "Memory", 0x4002125C,        4, base=16,    bitRange=0-31

sfr = "FPGA_FLAGS_SEL"   				, "Memory", 0x40021260,        4, base=16
sfr = "FPGA_FLAGS_SEL.PPE_BUSY_SEL"   	, "Memory", 0x40021260,        4, base=16,    bitRange=9-9
sfr = "FPGA_FLAGS_SEL.FIFO_FULL2_SEL"   , "Memory", 0x40021260,        4, base=16,    bitRange=8-8
sfr = "FPGA_FLAGS_SEL.FIFO_FULL1_SEL"   , "Memory", 0x40021260,        4, base=16,    bitRange=7-7
sfr = "FPGA_FLAGS_SEL.FIFO_FULL0_SEL"   , "Memory", 0x40021260,        4, base=16,    bitRange=6-6
sfr = "FPGA_FLAGS_SEL.FIFO_AFULL2_SEL"  , "Memory", 0x40021260,        4, base=16,    bitRange=5-5
sfr = "FPGA_FLAGS_SEL.FIFO_AFULL1_SEL"  , "Memory", 0x40021260,        4, base=16,    bitRange=4-4
sfr = "FPGA_FLAGS_SEL.FIFO_AFULL0_SEL"  , "Memory", 0x40021260,        4, base=16,    bitRange=3-3
sfr = "FPGA_FLAGS_SEL.FIFO_EMPTY2_SEL"  , "Memory", 0x40021260,        4, base=16,    bitRange=2-2
sfr = "FPGA_FLAGS_SEL.FIFO_EMPTY1_SEL"  , "Memory", 0x40021260,        4, base=16,    bitRange=1-1
sfr = "FPGA_FLAGS_SEL.FIFO_EMPTY0_SEL"  , "Memory", 0x40021260,        4, base=16,    bitRange=0-0

sfr = "PPE_PDMA_CTRL"   				, "Memory", 0x40021300,        4, base=16
sfr = "PPE_PDMA_CTRL.DATAOUT_CLR"   	, "Memory", 0x40021300,        4, base=16,    bitRange=2-2
sfr = "PPE_PDMA_CTRL.TAG"   			, "Memory", 0x40021300,        4, base=16,    bitRange=0-1

sfr = "PDMA_STATUS"   					, "Memory", 0x40021304,        4, base=16
sfr = "PDMA_STATUS.DATAOUT_FULL"   		, "Memory", 0x40021304,        4, base=16,    bitRange=2-2
sfr = "PDMA_STATUS.ACE_INREADY"   		, "Memory", 0x40021304,        4, base=16,    bitRange=1-1
sfr = "PDMA_STATUS.ACE_OUTREADY"   		, "Memory", 0x40021304,        4, base=16,    bitRange=0-0

sfr = "PPE_PDMA_DATAOUT"   				, "Memory", 0x40021308,        4, base=16
sfr = "PPE_PDMA_DATAOUT.DATA"   		, "Memory", 0x40021308,        4, base=16,    bitRange=0-31

sfr = "PPE_NOP"   						, "Memory", 0x40021400,        4, base=16
sfr = "PPE_NOP.NOP"   					, "Memory", 0x40021400,        4, base=16,    bitRange=0-31

sfr = "PPE_CTRL"   						, "Memory", 0x40021404,        4, base=16
sfr = "PPE_CTRL.RRDIS2"   				, "Memory", 0x40021404,        4, base=16,    bitRange=16-16
sfr = "PPE_CTRL.RRDIS1"   				, "Memory", 0x40021404,        4, base=16,    bitRange=15-15
sfr = "PPE_CTRL.RRDIS0"   				, "Memory", 0x40021404,        4, base=16,    bitRange=14-14
sfr = "PPE_CTRL.CURRCHAN"   			, "Memory", 0x40021404,        4, base=16,    bitRange=8-13
sfr = "PPE_CTRL.Ci"   					, "Memory", 0x40021404,        4, base=16,    bitRange=7-7
sfr = "PPE_CTRL.C2d"   					, "Memory", 0x40021404,        4, base=16,    bitRange=5-5
sfr = "PPE_CTRL.s2B"   					, "Memory", 0x40021404,        4, base=16,    bitRange=4-4
sfr = "PPE_CTRL.C2a"   					, "Memory", 0x40021404,        4, base=16,    bitRange=3-3
sfr = "PPE_CTRL.NegA"   				, "Memory", 0x40021404,        4, base=16,    bitRange=2-2
sfr = "PPE_CTRL.PPE_IDLE"   			, "Memory", 0x40021404,        4, base=16,    bitRange=1-1
sfr = "PPE_CTRL.PPE_EN"   				, "Memory", 0x40021404,        4, base=16,    bitRange=0-0

sfr = "PPE_PC_ETC"   					, "Memory", 0x40021408,        4, base=16
sfr = "PPE_PC_ETC.A_HI_SET"   			, "Memory", 0x40021408,        4, base=16,    bitRange=23-23
sfr = "PPE_PC_ETC.A_LO_SET"   			, "Memory", 0x40021408,        4, base=16,    bitRange=22-22
sfr = "PPE_PC_ETC.B_HI_SET"   			, "Memory", 0x40021408,        4, base=16,    bitRange=21-21
sfr = "PPE_PC_ETC.B_LO_SET"   			, "Memory", 0x40021408,        4, base=16,    bitRange=20-20
sfr = "PPE_PC_ETC.C_HI_SET"   			, "Memory", 0x40021408,        4, base=16,    bitRange=19-19
sfr = "PPE_PC_ETC.C_LO_SET"   			, "Memory", 0x40021408,        4, base=16,    bitRange=18-18
sfr = "PPE_PC_ETC.A_HI_CLR"   			, "Memory", 0x40021408,        4, base=16,    bitRange=17-17
sfr = "PPE_PC_ETC.A_LO_CLR"   			, "Memory", 0x40021408,        4, base=16,    bitRange=16-16
sfr = "PPE_PC_ETC.B_HI_CLR"   			, "Memory", 0x40021408,        4, base=16,    bitRange=15-15
sfr = "PPE_PC_ETC.B_LO_CLR"   			, "Memory", 0x40021408,        4, base=16,    bitRange=14-14
sfr = "PPE_PC_ETC.C_HI_CLR"   			, "Memory", 0x40021408,        4, base=16,    bitRange=13-13
sfr = "PPE_PC_ETC.C_LO_CLR"   			, "Memory", 0x40021408,        4, base=16,    bitRange=12-12
sfr = "PPE_PC_ETC.PC_OP"   				, "Memory", 0x40021408,        4, base=16,    bitRange=10-11
sfr = "PPE_PC_ETC.PC"   				, "Memory", 0x40021408,        4, base=16,    bitRange=0-9

sfr = "PPE_SF"   						, "Memory", 0x4002140C,        4, base=16
sfr = "PPE_SF.SF_DIR"   				, "Memory", 0x4002140C,        4, base=16,    bitRange=19-19
sfr = "PPE_SF.SF_STATE"   				, "Memory", 0x4002140C,        4, base=16,    bitRange=18-18
sfr = "PPE_SF.SF_MATCH_0_1"   			, "Memory", 0x4002140C,        4, base=16,    bitRange=12-17
sfr = "PPE_SF.SF_MATCH_1_0"   			, "Memory", 0x4002140C,        4, base=16,    bitRange=6-11
sfr = "PPE_SF.SF_CNT"   				, "Memory", 0x4002140C,        4, base=16,    bitRange=0-5

sfr = "PPE_SCRATCH"   					, "Memory", 0x40021410,        4, base=16
sfr = "PPE_SCRATCH.DATA"   				, "Memory", 0x40021410,        4, base=16,    bitRange=0-31

sfr = "ALU_CTRL"   						, "Memory", 0x40021418,        4, base=16
sfr = "ALU_CTRL.NSAT_EN"   				, "Memory", 0x40021418,        4, base=16,    bitRange=1-1
sfr = "ALU_CTRL.PSAT_EN"   				, "Memory", 0x40021418,        4, base=16,    bitRange=0-0

sfr = "ALU_STATUS"   					, "Memory", 0x4002141C,        4, base=16
sfr = "ALU_STATUS.Co"   				, "Memory", 0x4002141C,        4, base=16,    bitRange=2-2
sfr = "ALU_STATUS.NSAT"   				, "Memory", 0x4002141C,        4, base=16,    bitRange=1-1
sfr = "ALU_STATUS.PSAT"   				, "Memory", 0x4002141C,        4, base=16,    bitRange=0-0

sfr = "ALU_A"   						, "Memory", 0x40021420,        4, base=16
sfr = "ALU_A.DATA"   					, "Memory", 0x40021420,        4, base=16,    bitRange=0-31

sfr = "ALU_B"   						, "Memory", 0x40021428,        4, base=16
sfr = "ALU_B.DATA"   					, "Memory", 0x40021428,        4, base=16,    bitRange=0-31

sfr = "ALU_C"   						, "Memory", 0x40021430,        4, base=16
sfr = "ALU_C.DATA"   					, "Memory", 0x40021430,        4, base=16,    bitRange=0-31

sfr = "ALU_D"   						, "Memory", 0x40021438,        4, base=16
sfr = "ALU_D.DATA"   					, "Memory", 0x40021438,        4, base=16,    bitRange=0-15

sfr = "ALU_E"   						, "Memory", 0x40021440,        4, base=16
sfr = "ALU_E.DATA"  					, "Memory", 0x40021440,        4, base=16,    bitRange=0-15

sfr = "PPE_FPTR"   						, "Memory", 0x40021448,        4, base=16
sfr = "PPE_FPTR.FD"   					, "Memory", 0x40021448,        4, base=16,    bitRange=10-10
sfr = "PPE_FPTR.TP"   					, "Memory", 0x40021448,        4, base=16,    bitRange=9-9
sfr = "PPE_FPTR.TC"   					, "Memory", 0x40021448,        4, base=16,    bitRange=8-8
sfr = "PPE_FPTR.FBANK"   				, "Memory", 0x40021448,        4, base=16,    bitRange=5-7
sfr = "PPE_FPTR.FPTR"   				, "Memory", 0x40021448,        4, base=16,    bitRange=0-4

sfr = "PPE_FLAGS0"   					, "Memory", 0x40021450,        4, base=16
sfr = "PPE_FLAGS0.FLAGS"   				, "Memory", 0x40021450,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS1"   					, "Memory", 0x40021454,        4, base=16
sfr = "PPE_FLAGS1.FLAGS"   				, "Memory", 0x40021454,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS2"   					, "Memory", 0x40021458,        4, base=16
sfr = "PPE_FLAGS2.FLAGS"   				, "Memory", 0x40021458,        4, base=16,    bitRange=0-31

sfr = "PPE_FLAGS3"   					, "Memory", 0x4002145C,        4, base=16
sfr = "PPE_FLAGS3.FLAGS"   				, "Memory", 0x4002145C,        4, base=16,    bitRange=0-31

sfr = "PPE_SFFLAGS"   					, "Memory", 0x40021460,        4, base=16
sfr = "PPE_SFFLAGS.FLAGS"   			, "Memory", 0x40021460,        4, base=16,    bitRange=0-31

sfr = "ADC0_FIFO_CTRL"   				, "Memory", 0x40021490,        4, base=16
sfr = "ADC0_FIFO_CTRL.CLR"   			, "Memory", 0x40021490,        4, base=16,    bitRange=2-2
sfr = "ADC0_FIFO_CTRL.AFULL_WT_EN"   	, "Memory", 0x40021490,        4, base=16,    bitRange=1-1
sfr = "ADC0_FIFO_CTRL.FULL_WT_EN"   	, "Memory", 0x40021490,        4, base=16,    bitRange=0-0

sfr = "ADC0_FIFO_STATUS"   				, "Memory", 0x40021494,        4, base=16
sfr = "ADC0_FIFO_STATUS.FULL"   		, "Memory", 0x40021494,        4, base=16,    bitRange=6-6
sfr = "ADC0_FIFO_STATUS.AFULL"   		, "Memory", 0x40021494,        4, base=16,    bitRange=5-5
sfr = "ADC0_FIFO_STATUS.EMPTY"   		, "Memory", 0x40021494,        4, base=16,    bitRange=4-4
sfr = "ADC0_FIFO_STATUS.RDPTR"   		, "Memory", 0x40021494,        4, base=16,    bitRange=2-3
sfr = "ADC0_FIFO_STATUS.WRPTR"   		, "Memory", 0x40021494,        4, base=16,    bitRange=0-1

sfr = "ADC0_FIFO_DATA"   				, "Memory", 0x40021498,        4, base=16
sfr = "ADC0_FIFO_DATA.CHAN"   			, "Memory", 0x40021498,        4, base=16,    bitRange=12-15
sfr = "ADC0_FIFO_DATA.RESULT"   		, "Memory", 0x40021498,        4, base=16,    bitRange=0-11

sfr = "ADC1_FIFO_CTRL"   				, "Memory", 0x4002149C,        4, base=16
sfr = "ADC1_FIFO_CTRL.CLR"   			, "Memory", 0x4002149C,        4, base=16,    bitRange=2-2
sfr = "ADC1_FIFO_CTRL.AFULL_WT_EN"   	, "Memory", 0x4002149C,        4, base=16,    bitRange=1-1
sfr = "ADC1_FIFO_CTRL.FULL_WT_EN"   	, "Memory", 0x4002149C,        4, base=16,    bitRange=0-0

sfr = "ADC1_FIFO_STATUS"   				, "Memory", 0x400214A0,        4, base=16
sfr = "ADC1_FIFO_STATUS.FULL"   		, "Memory", 0x400214A0,        4, base=16,    bitRange=6-6
sfr = "ADC1_FIFO_STATUS.AFULL"   		, "Memory", 0x400214A0,        4, base=16,    bitRange=5-5
sfr = "ADC1_FIFO_STATUS.EMPTY"   		, "Memory", 0x400214A0,        4, base=16,    bitRange=4-4
sfr = "ADC1_FIFO_STATUS.RDPTR"   		, "Memory", 0x400214A0,        4, base=16,    bitRange=2-3
sfr = "ADC1_FIFO_STATUS.WRPTR"   		, "Memory", 0x400214A0,        4, base=16,    bitRange=0-1

sfr = "ADC1_FIFO_DATA"   				, "Memory", 0x400214A4,        4, base=16
sfr = "ADC1_FIFO_DATA.CHAN"   			, "Memory", 0x400214A4,        4, base=16,    bitRange=12-15
sfr = "ADC1_FIFO_DATA.RESULT"   		, "Memory", 0x400214A4,        4, base=16,    bitRange=0-11

sfr = "ADC2_FIFO_CTRL"   				, "Memory", 0x400214A8,        4, base=16
sfr = "ADC2_FIFO_CTRL.CLR"   			, "Memory", 0x400214A8,        4, base=16,    bitRange=2-2
sfr = "ADC2_FIFO_CTRL.AFULL_WT_EN"   	, "Memory", 0x400214A8,        4, base=16,    bitRange=1-1
sfr = "ADC2_FIFO_CTRL.FULL_WT_EN"   	, "Memory", 0x400214A8,        4, base=16,    bitRange=0-0

sfr = "ADC2_FIFO_STATUS"   				, "Memory", 0x400214AC,        4, base=16
sfr = "ADC2_FIFO_STATUS.FULL"   		, "Memory", 0x400214AC,        4, base=16,    bitRange=6-6
sfr = "ADC2_FIFO_STATUS.AFULL"   		, "Memory", 0x400214AC,        4, base=16,    bitRange=5-5
sfr = "ADC2_FIFO_STATUS.EMPTY"   		, "Memory", 0x400214AC,        4, base=16,    bitRange=4-4
sfr = "ADC2_FIFO_STATUS.RDPTR"   		, "Memory", 0x400214AC,        4, base=16,    bitRange=2-3
sfr = "ADC2_FIFO_STATUS.WRPTR"   		, "Memory", 0x400214AC,        4, base=16,    bitRange=0-1

sfr = "ADC2_FIFO_DATA"   				, "Memory", 0x400214B0,        4, base=16
sfr = "ADC2_FIFO_DATA.CHAN"   			, "Memory", 0x400214B0,        4, base=16,    bitRange=12-15
sfr = "ADC2_FIFO_DATA.RESULT"   		, "Memory", 0x400214B0,        4, base=16,    bitRange=0-11
	
sfr = "ADC0_FIFO_DATA_PEEK"   			, "Memory", 0x40021500,        4, base=16
sfr = "ADC0_FIFO_DATA_PEEK.CHAN"   		, "Memory", 0x40021500,        4, base=16,    bitRange=12-15
sfr = "ADC0_FIFO_DATA_PEEK.RESULT"   	, "Memory", 0x40021500,        4, base=16,    bitRange=0-11

sfr = "ADC0_FIFO_DATA0"   				, "Memory", 0x40021504,        4, base=16
sfr = "ADC0_FIFO_DATA0.CHAN"   			, "Memory", 0x40021504,        4, base=16,    bitRange=12-15
sfr = "ADC0_FIFO_DATA0.RESULT"   		, "Memory", 0x40021504,        4, base=16,    bitRange=0-11

sfr = "ADC0_FIFO_DATA1"   				, "Memory", 0x40021508,        4, base=16
sfr = "ADC0_FIFO_DATA1.CHAN"   			, "Memory", 0x40021508,        4, base=16,    bitRange=12-15
sfr = "ADC0_FIFO_DATA1.RESULT"   		, "Memory", 0x40021508,        4, base=16,    bitRange=0-11

sfr = "ADC0_FIFO_DATA2"   				, "Memory", 0x4002150C,        4, base=16
sfr = "ADC0_FIFO_DATA2.CHAN"   			, "Memory", 0x4002150C,        4, base=16,    bitRange=12-15
sfr = "ADC0_FIFO_DATA2.RESULT"   		, "Memory", 0x4002150C,        4, base=16,    bitRange=0-11

sfr = "ADC0_FIFO_DATA3"   				, "Memory", 0x40021510,        4, base=16
sfr = "ADC0_FIFO_DATA3.CHAN"   			, "Memory", 0x40021510,        4, base=16,    bitRange=12-15
sfr = "ADC0_FIFO_DATA3.RESULT"   		, "Memory", 0x40021510,        4, base=16,    bitRange=0-11

sfr = "ADC1_FIFO_DATA_PEEK"   			, "Memory", 0x40021514,        4, base=16
sfr = "ADC1_FIFO_DATA_PEEK.CHAN"   		, "Memory", 0x40021514,        4, base=16,    bitRange=12-15
sfr = "ADC1_FIFO_DATA_PEEK.RESULT"   	, "Memory", 0x40021514,        4, base=16,    bitRange=0-11

sfr = "ADC1_FIFO_DATA0"   				, "Memory", 0x40021518,        4, base=16
sfr = "ADC1_FIFO_DATA0.CHAN"   			, "Memory", 0x40021518,        4, base=16,    bitRange=12-15
sfr = "ADC1_FIFO_DATA0.RESULT"   		, "Memory", 0x40021518,        4, base=16,    bitRange=0-11

sfr = "ADC1_FIFO_DATA1"   				, "Memory", 0x4002151C,        4, base=16
sfr = "ADC1_FIFO_DATA1.CHAN"   			, "Memory", 0x4002151C,        4, base=16,    bitRange=12-15
sfr = "ADC1_FIFO_DATA1.RESULT"   		, "Memory", 0x4002151C,        4, base=16,    bitRange=0-11

sfr = "ADC1_FIFO_DATA2"   				, "Memory", 0x40021520,        4, base=16
sfr = "ADC1_FIFO_DATA2.CHAN"   			, "Memory", 0x40021520,        4, base=16,    bitRange=12-15
sfr = "ADC1_FIFO_DATA2.RESULT"   		, "Memory", 0x40021520,        4, base=16,    bitRange=0-11

sfr = "ADC1_FIFO_DATA3"   				, "Memory", 0x40021524,        4, base=16
sfr = "ADC1_FIFO_DATA3.CHAN"   			, "Memory", 0x40021524,        4, base=16,    bitRange=12-15
sfr = "ADC1_FIFO_DATA3.RESULT"   		, "Memory", 0x40021524,        4, base=16,    bitRange=0-11

sfr = "ADC2_FIFO_DATA_PEEK"   			, "Memory", 0x40021528,        4, base=16
sfr = "ADC2_FIFO_DATA_PEEK.CHAN"   		, "Memory", 0x40021528,        4, base=16,    bitRange=12-15
sfr = "ADC2_FIFO_DATA_PEEK.RESULT"   	, "Memory", 0x40021528,        4, base=16,    bitRange=0-11

sfr = "ADC2_FIFO_DATA0"   				, "Memory", 0x4002152C,        4, base=16
sfr = "ADC2_FIFO_DATA0.CHAN"   			, "Memory", 0x4002152C,        4, base=16,    bitRange=12-15
sfr = "ADC2_FIFO_DATA0.RESULT"   		, "Memory", 0x4002152C,        4, base=16,    bitRange=0-11

sfr = "ADC2_FIFO_DATA1"   				, "Memory", 0x40021530,        4, base=16
sfr = "ADC2_FIFO_DATA1.CHAN"   			, "Memory", 0x40021530,        4, base=16,    bitRange=12-15
sfr = "ADC2_FIFO_DATA1.RESULT"   		, "Memory", 0x40021530,        4, base=16,    bitRange=0-11

sfr = "ADC2_FIFO_DATA2"   				, "Memory", 0x40021534,        4, base=16
sfr = "ADC2_FIFO_DATA2.CHAN"   			, "Memory", 0x40021534,        4, base=16,    bitRange=12-15
sfr = "ADC2_FIFO_DATA2.RESULT" 	  		, "Memory", 0x40021534,        4, base=16,    bitRange=0-11

sfr = "ADC2_FIFO_DATA3"   				, "Memory", 0x40021538,        4, base=16
sfr = "ADC2_FIFO_DATA3.CHAN"   			, "Memory", 0x40021538,        4, base=16,    bitRange=12-15
sfr = "ADC2_FIFO_DATA3.RESULT"   		, "Memory", 0x40021538,        4, base=16,    bitRange=0-11

sfr = "PPE_RAM_DATA_FIRST"   			, "Memory", 0x40021800,        4, base=16
sfr = "PPE_RAM_DATA_FIRST.DATA"   		, "Memory", 0x40021800,        4, base=16,    bitRange=0-31

sfr = "PPE_RAM_DATA_LAST"   			, "Memory", 0x40021FFC,        4, base=16
sfr = "PPE_RAM_DATA_LAST.DATA"   		, "Memory", 0x40021FFC,        4, base=16,    bitRange=0-31


;
;		System Registers
;
;     Name                      				    Zone      Address    Bytesize Displaybase Bitrange
;     ----                      				    ----      -------    -------- ----------- --------
sfr = "ESRAM_CONFIG"                            , "Memory", 0xE0042000,        4, base=16
sfr = "ESRAM_CONFIG.COM_ESRAMFWREMAP"           , "Memory", 0xE0042000,        4, base=16,    bitRange=0-0
sfr = "ESRAM_CONFIG.F2_TESTREMAPENABLE_SYNC"    , "Memory", 0xE0042000,        4, base=16,    bitRange=1-1
sfr = "ESRAM_CONFIG.F2_TESTESRAM1REMAP_SYNC"    , "Memory", 0xE0042000,        4, base=16,    bitRange=2-2
sfr = "ESRAM_CONFIG.F2_ESRAMSIZE"               , "Memory", 0xE0042000,        4, base=16,    bitRange=3-4

sfr = "ENVM_CONFIG"                             , "Memory", 0xE0042004,        4, base=16
sfr = "ENVM_CONFIG.COM_ENVMREMAPSIZE"           , "Memory", 0xE0042004,        4, base=16,    bitRange=0-4
sfr = "ENVM_CONFIG.F2_ENVMPOWEREDDOWN"          , "Memory", 0xE0042004,        4, base=16,    bitRange=5-5
sfr = "ENVM_CONFIG.ENVM_PIPE_BYPASS"            , "Memory", 0xE0042004,        4, base=16,    bitRange=6-6
sfr = "ENVM_CONFIG.ENVM_SIX_CYCLE"              , "Memory", 0xE0042004,        4, base=16,    bitRange=7-7

sfr = "ENVM_REMAP_BASE"                         , "Memory", 0xE0042008,        4, base=16
sfr = "ENVM_REMAP_BASE.COM_ENVMREMAPBASE"       , "Memory", 0xE0042008,        4, base=16,    bitRange=0-19

sfr = "ENVM_FAB_REMAP"                          , "Memory", 0xE004200C,        4, base=16
sfr = "ENVM_FAB_REMAP.COM_ENVMFABREMAPBASE"     , "Memory", 0xE004200C,        4, base=16,    bitRange=0-19

sfr = "FAB_PROT_SIZE"                           , "Memory", 0xE0042010,        4, base=16
sfr = "FAB_PROT_SIZE.COM_PROTREGIONSIZE"        , "Memory", 0xE0042010,        4, base=16,    bitRange=0-4

sfr = "FAB_PROT_BASE"                           , "Memory", 0xE0042014,        4, base=16
sfr = "FAB_PROT_BASE.COM_PROTREGIONBASE"        , "Memory", 0xE0042014,        4, base=16,    bitRange=0-31

sfr = "MATRIX_CONFIG"                           , "Memory", 0xE0042018,	       4, base=16
sfr = "MATRIX_CONFIG.COM_MASTERENABLE"          , "Memory", 0xE0042018,        4, base=16,    bitRange=0-2
sfr = "MATRIX_CONFIG.COM_WEIGHTEDMODE"          , "Memory", 0xE0042018,        4, base=16,    bitRange=3-3

sfr = "DSS_STATUS"                              , "Memory", 0xE004201C,        4, base=16
sfr = "DSS_STATUS.RTCMATCHEVENT"                , "Memory", 0xE004201C,        4, base=16,    bitRange=0-0
sfr = "DSS_STATUS.WDOGTIMEOUTEVENT"             , "Memory", 0xE004201C,        4, base=16,    bitRange=1-1
sfr = "DSS_STATUS.BROWNOUT1_5VINT"              , "Memory", 0xE004201C,        4, base=16,    bitRange=2-2
sfr = "DSS_STATUS.BROWNOUT3_3VINT"              , "Memory", 0xE004201C,        4, base=16,    bitRange=3-3
sfr = "DSS_STATUS.COM_ERRORSTATUS"              , "Memory", 0xE004201C,        4, base=16,    bitRange=4-8
sfr = "DSS_STATUS.PLLLOCKINT"                   , "Memory", 0xE004201C,        4, base=16,    bitRange=9-9
sfr = "DSS_STATUS.PLLLOCKLOSTINT"               , "Memory", 0xE004201C,        4, base=16,    bitRange=10-10

sfr = "CLR_DSS_STATUS"                          , "Memory", 0xE0042020,        4, base=16
sfr = "CLR_DSS_STATUS.CLRRTCMATCHEVENT"         , "Memory", 0xE0042020,        4, base=16,    bitRange=0-0
sfr = "CLR_DSS_STATUS.CLRWDOGTIMEOUTEVENT"      , "Memory", 0xE0042020,        4, base=16,    bitRange=1-1
sfr = "CLR_DSS_STATUS.CLRBROWNOUT1_5VINT"       , "Memory", 0xE0042020,        4, base=16,    bitRange=2-2
sfr = "CLR_DSS_STATUS.CLRBROWNOUT3_3VINT"       , "Memory", 0xE0042020,        4, base=16,    bitRange=3-3
sfr = "CLR_DSS_STATUS.COM_CLEARSTATUS"          , "Memory", 0xE0042020,        4, base=16,    bitRange=4-8
sfr = "CLR_DSS_STATUS.CLRPLLLOCKINT"            , "Memory", 0xE0042020,        4, base=16,    bitRange=9-9
sfr = "CLR_DSS_STATUS.CLRPLLLOCKLOSTINT"        , "Memory", 0xE0042020,        4, base=16,    bitRange=10-10

sfr = "FROM_CONFIG"                             , "Memory", 0xE0042024,        4, base=16
sfr = "FROM_CONFIG.SYS_TOPT"                    , "Memory", 0xE0042024,        4, base=16,    bitRange=0-3

sfr = "IAP_CONFIG"                              , "Memory", 0xE0042028,        4, base=16
sfr = "IAP_CONFIG.SYS_FCFG"                     , "Memory", 0xE0042028,        4, base=16,    bitRange=0-2

sfr = "SOFT_INTERRUPT"                          , "Memory", 0xE004202C,        4, base=16
sfr = "SOFT_INTERRUPT.SOFTINTERRUPT"            , "Memory", 0xE004202C,        4, base=16,    bitRange=0-0

sfr = "SOFT_RESET"                              , "Memory", 0xE0042030,        4, base=16
sfr = "SOFT_RESET.ENVM_SOFTRESET"               , "Memory", 0xE0042030,        4, base=16,    bitRange=0-0
sfr = "SOFT_RESET.ESRAM0_SOFTRESET"             , "Memory", 0xE0042030,        4, base=16,    bitRange=1-1
sfr = "SOFT_RESET.ESRAM1_SOFTRESET"             , "Memory", 0xE0042030,        4, base=16,    bitRange=2-2
sfr = "SOFT_RESET.EMC_SOFTRESET"                , "Memory", 0xE0042030,        4, base=16,    bitRange=3-3
sfr = "SOFT_RESET.MAC_SOFTRESET"                , "Memory", 0xE0042030,        4, base=16,    bitRange=4-4
sfr = "SOFT_RESET.PDMA_SOFTRESET"               , "Memory", 0xE0042030,        4, base=16,    bitRange=5-5
sfr = "SOFT_RESET.TIMER_SOFTRESET"              , "Memory", 0xE0042030,        4, base=16,    bitRange=6-6
sfr = "SOFT_RESET.UART0_SOFTRESET"              , "Memory", 0xE0042030,        4, base=16,    bitRange=7-7
sfr = "SOFT_RESET.UART1_SOFTRESET"              , "Memory", 0xE0042030,        4, base=16,    bitRange=8-8
sfr = "SOFT_RESET.SPI0_SOFTRESET"               , "Memory", 0xE0042030,        4, base=16,    bitRange=9-9
sfr = "SOFT_RESET.SPI1_SOFTRESET"               , "Memory", 0xE0042030,        4, base=16,    bitRange=10-10
sfr = "SOFT_RESET.I2C0_SOFTRESET"               , "Memory", 0xE0042030,        4, base=16,    bitRange=11-11
sfr = "SOFT_RESET.I2C1_SOFTRESET"               , "Memory", 0xE0042030,        4, base=16,    bitRange=12-12
sfr = "SOFT_RESET.ACE_SOFTRESET"                , "Memory", 0xE0042030,        4, base=16,    bitRange=13-13
sfr = "SOFT_RESET.GPIO_SOFTRESET"               , "Memory", 0xE0042030,        4, base=16,    bitRange=14-14
sfr = "SOFT_RESET.IAP_SOFTRESET"                , "Memory", 0xE0042030,        4, base=16,    bitRange=15-15
sfr = "SOFT_RESET.EXT_SOFTRESET"                , "Memory", 0xE0042030,        4, base=16,    bitRange=16-16
sfr = "SOFT_RESET.FPGA_SOFTRESET"               , "Memory", 0xE0042030,        4, base=16,    bitRange=17-17
sfr = "SOFT_RESET.USERRESETACTIVE"              , "Memory", 0xE0042030,        4, base=16,    bitRange=18-18
sfr = "SOFT_RESET.PADRESETENABLE"               , "Memory", 0xE0042030,        4, base=16,    bitRange=19-19

sfr = "DEVICE_STATUS"                           , "Memory", 0xE0042034,        4, base=16
sfr = "DEVICE_STATUS.BROWNOUT1_5V"              , "Memory", 0xE0042034,        4, base=16,    bitRange=0-0
sfr = "DEVICE_STATUS.BROWNOUT3_3V"              , "Memory", 0xE0042034,        4, base=16,    bitRange=1-1
sfr = "DEVICE_STATUS.VCCIBGOOD_SYNC"            , "Memory", 0xE0042034,        4, base=16,    bitRange=2-2
sfr = "DEVICE_STATUS.F2_PC_ACCESS_SYNC"         , "Memory", 0xE0042034,        4, base=16,    bitRange=3-4
sfr = "DEVICE_STATUS.FPGAPROGRAMMING_SYNC"      , "Memory", 0xE0042034,        4, base=16,    bitRange=5-5
sfr = "DEVICE_STATUS.FPGAGOOD_SYNC"             , "Memory", 0xE0042034,        4, base=16,    bitRange=6-6

sfr = "SYSTICK_CONFIG"                          , "Memory", 0xE0042038,        4, base=16
sfr = "SYSTICK_CONFIG.STCALIB"                  , "Memory", 0xE0042038,        4, base=16,    bitRange=0-25
sfr = "SYSTICK_CONFIG.Reserved"                 , "Memory", 0xE0042038,        4, base=16,    bitRange=26-27
sfr = "SYSTICK_CONFIG.STCLK_DIVISOR"            , "Memory", 0xE0042038,        4, base=16,    bitRange=28-29

sfr = "EM_MUX_CONFIG"                           , "Memory", 0xE004203C,        4, base=16
sfr = "EM_MUX_CONFIG.EM_SEL"                    , "Memory", 0xE004203C,        4, base=16,    bitRange=0-0

sfr = "EM_CONFIG_0"                             , "Memory", 0xE0042040,        4, base=16
sfr = "EM_CONFIG_0.EM_MEMTYPE0"                 , "Memory", 0xE0042040,        4, base=16,    bitRange=0-1
sfr = "EM_CONFIG_0.EM_PORTSIZE0"                , "Memory", 0xE0042040,        4, base=16,    bitRange=2-2
sfr = "EM_CONFIG_0.EM_RDLATFIRST0"              , "Memory", 0xE0042040,        4, base=16,    bitRange=3-6
sfr = "EM_CONFIG_0.EM_RDLATREST0"               , "Memory", 0xE0042040,        4, base=16,    bitRange=7-10
sfr = "EM_CONFIG_0.EM_WRITELAT0"                , "Memory", 0xE0042040,        4, base=16,    bitRange=11-14
sfr = "EM_CONFIG_0.EM_IDD0"                     , "Memory", 0xE0042040,        4, base=16,    bitRange=15-16
sfr = "EM_CONFIG_0.EM_PIPERDN0"                 , "Memory", 0xE0042040,        4, base=16,    bitRange=17-17
sfr = "EM_CONFIG_0.EM_PIPEWRN0"                 , "Memory", 0xE0042040,        4, base=16,    bitRange=18-18
sfr = "EM_CONFIG_0.EM_RWPOL0"                   , "Memory", 0xE0042040,        4, base=16,    bitRange=19-19
sfr = "EM_CONFIG_0.EM_WENBEN0"                  , "Memory", 0xE0042040,        4, base=16,    bitRange=20-20
sfr = "EM_CONFIG_0.EM_CSFE0"                    , "Memory", 0xE0042040,        4, base=16,    bitRange=21-21

sfr = "EM_CONFIG_1"                             , "Memory", 0xE0042044,        4, base=16
sfr = "EM_CONFIG_1.EM_MEMTYPE1"                 , "Memory", 0xE0042044,        4, base=16,    bitRange=0-1
sfr = "EM_CONFIG_1.EM_PORTSIZE1"                , "Memory", 0xE0042044,        4, base=16,    bitRange=2-2
sfr = "EM_CONFIG_1.EM_RDLATFIRST1"              , "Memory", 0xE0042044,        4, base=16,    bitRange=3-6
sfr = "EM_CONFIG_1.EM_RDLATREST1"               , "Memory", 0xE0042044,        4, base=16,    bitRange=7-10
sfr = "EM_CONFIG_1.EM_WRITELAT1"                , "Memory", 0xE0042044,        4, base=16,    bitRange=11-14
sfr = "EM_CONFIG_1.EM_IDD1"                     , "Memory", 0xE0042044,        4, base=16,    bitRange=15-16
sfr = "EM_CONFIG_1.EM_PIPERDN1"                 , "Memory", 0xE0042044,        4, base=16,    bitRange=17-17
sfr = "EM_CONFIG_1.EM_PIPEWRN1"                 , "Memory", 0xE0042044,        4, base=16,    bitRange=18-18
sfr = "EM_CONFIG_1.EM_RWPOL1"                   , "Memory", 0xE0042044,        4, base=16,    bitRange=19-19
sfr = "EM_CONFIG_1.EM_WENBEN1"                  , "Memory", 0xE0042044,        4, base=16,    bitRange=20-20
sfr = "EM_CONFIG_1.EM_CSFE1"                    , "Memory", 0xE0042044,        4, base=16,    bitRange=21-21

sfr = "CLK_CTRL"                                , "Memory", 0xE0042048,        4, base=16
sfr = "CLK_CTRL.Reserved"                       , "Memory", 0xE0042048,        4, base=16,    bitRange=0-0
sfr = "CLK_CTRL.RMIICLKSEL"                     , "Memory", 0xE0042048,        4, base=16,    bitRange=1-1
sfr = "CLK_CTRL.PCLK0DIVISOR"                   , "Memory", 0xE0042048,        4, base=16,    bitRange=2-3
sfr = "CLK_CTRL.PCLK1DIVISOR"                   , "Memory", 0xE0042048,        4, base=16,    bitRange=4-5
sfr = "CLK_CTRL.ACLKDIVISOR"                    , "Memory", 0xE0042048,        4, base=16,    bitRange=6-7
sfr = "CLK_CTRL.RTCIF_ACMDIVISOR"               , "Memory", 0xE0042048,        4, base=16,    bitRange=8-11
sfr = "CLK_CTRL.GLBDIVISOR"                     , "Memory", 0xE0042048,        4, base=16,    bitRange=2-13

sfr = "CCC_DIV_CONFIG"                          , "Memory", 0xE004204C,        4, base=16
sfr = "CCC_DIV_CONFIG.OADIV"                    , "Memory", 0xE004204C,        4, base=16,    bitRange=0-4
sfr = "CCC_DIV_CONFIG.OADIVHALF"                , "Memory", 0xE004204C,        4, base=16,    bitRange=5-5
sfr = "CCC_DIV_CONFIG.OADIVRST"                 , "Memory", 0xE004204C,        4, base=16,    bitRange=6-6
sfr = "CCC_DIV_CONFIG.OBDIV"                    , "Memory", 0xE004204C,        4, base=16,    bitRange=8-12
sfr = "CCC_DIV_CONFIG.OBDIVHALF"                , "Memory", 0xE004204C,        4, base=16,    bitRange=13-13
sfr = "CCC_DIV_CONFIG.OBDIVRST"                 , "Memory", 0xE004204C,        4, base=16,    bitRange=14-14
sfr = "CCC_DIV_CONFIG.OCDIV"                    , "Memory", 0xE004204C,        4, base=16,    bitRange=16-20
sfr = "CCC_DIV_CONFIG.OCDIVHALF"                , "Memory", 0xE004204C,        4, base=16,    bitRange=21-21
sfr = "CCC_DIV_CONFIG.OCDIVRST"                 , "Memory", 0xE004204C,        4, base=16,    bitRange=22-22

sfr = "CCC_MUX_CONFIG"                          , "Memory", 0xE0042050,        4, base=16
sfr = "CCC_MUX_CONFIG.STATASEL"                 , "Memory", 0xE0042050,        4, base=16,    bitRange=0-0
sfr = "CCC_MUX_CONFIG.RXASEL"                   , "Memory", 0xE0042050,        4, base=16,    bitRange=1-1
sfr = "CCC_MUX_CONFIG.DYNASEL"                  , "Memory", 0xE0042050,        4, base=16,    bitRange=2-2
sfr = "CCC_MUX_CONFIG.OAMUX"                    , "Memory", 0xE0042050,        4, base=16,    bitRange=3-5
sfr = "CCC_MUX_CONFIG.BYPASS_PLL1"              , "Memory", 0xE0042050,        4, base=16,    bitRange=6-6
sfr = "CCC_MUX_CONFIG.STATBSEL"                 , "Memory", 0xE0042050,        4, base=16,    bitRange=8-8
sfr = "CCC_MUX_CONFIG.RXBSEL"                   , "Memory", 0xE0042050,        4, base=16,    bitRange=9-9
sfr = "CCC_MUX_CONFIG.DYNBSEL"                  , "Memory", 0xE0042050,        4, base=16,    bitRange=10-10
sfr = "CCC_MUX_CONFIG.OBMUX"                    , "Memory", 0xE0042050,        4, base=16,    bitRange=11-13
sfr = "CCC_MUX_CONFIG.BYPASS_PLL2"              , "Memory", 0xE0042050,        4, base=16,    bitRange=14-14
sfr = "CCC_MUX_CONFIG.STATCSEL"                 , "Memory", 0xE0042050,        4, base=16,    bitRange=16-16
sfr = "CCC_MUX_CONFIG.RXCSEL"                   , "Memory", 0xE0042050,        4, base=16,    bitRange=17-17
sfr = "CCC_MUX_CONFIG.DYNCSEL"                  , "Memory", 0xE0042050,        4, base=16,    bitRange=18-18
sfr = "CCC_MUX_CONFIG.OCMUX"                    , "Memory", 0xE0042050,        4, base=16,    bitRange=19-21
sfr = "CCC_MUX_CONFIG.BYPASSP_PLL3"             , "Memory", 0xE0042050,        4, base=16,    bitRange=22-22
sfr = "CCC_MUX_CONFIG.GLMUXSEL"                 , "Memory", 0xE0042050,        4, base=16,    bitRange=24-25
sfr = "CCC_MUX_CONFIG.GLMUXCFG"                 , "Memory", 0xE0042050,        4, base=16,    bitRange=26-27

sfr = "CCC_PLL_CONFIG"                          , "Memory", 0xE0042054,        4, base=16
sfr = "CCC_PLL_CONFIG.FINDIV"                   , "Memory", 0xE0042054,        4, base=16,    bitRange=0-6
sfr = "CCC_PLL_CONFIG.FBDIV"                    , "Memory", 0xE0042054,        4, base=16,    bitRange=7-13
sfr = "CCC_PLL_CONFIG.FBSEL"                    , "Memory", 0xE0042054,        4, base=16,    bitRange=14-15
sfr = "CCC_PLL_CONFIG.FBDLY"                    , "Memory", 0xE0042054,        4, base=16,    bitRange=16-20
sfr = "CCC_PLL_CONFIG.XDLYSEL"                  , "Memory", 0xE0042054,        4, base=16,    bitRange=21-21
sfr = "CCC_PLL_CONFIG.VCOSEL"                   , "Memory", 0xE0042054,        4, base=16,    bitRange=22-24
sfr = "CCC_PLL_CONFIG.POWERDOWN"                , "Memory", 0xE0042054,        4, base=16,    bitRange=31-31

sfr = "CCC_DLY_CONFIG"                          , "Memory", 0xE0042058,        4, base=16
sfr = "CCC_DLY_CONFIG.DLYHCA"                   , "Memory", 0xE0042058,        4, base=16,    bitRange=0-4
sfr = "CCC_DLY_CONFIG.DLYHCB"                   , "Memory", 0xE0042058,        4, base=16,    bitRange=5-9
sfr = "CCC_DLY_CONFIG.DLYHCC"                   , "Memory", 0xE0042058,        4, base=16,    bitRange=10-14
sfr = "CCC_DLY_CONFIG.DLYA0"                    , "Memory", 0xE0042058,        4, base=16,    bitRange=15-19
sfr = "CCC_DLY_CONFIG.DLYA1"                    , "Memory", 0xE0042058,        4, base=16,    bitRange=20-24

sfr = "CCC_STATUS"                              , "Memory", 0xE004205C,        4, base=16
sfr = "CCC_STATUS.PLLLOCK"                      , "Memory", 0xE004205C,        4, base=16,    bitRange=0-0

sfr = "OSC_CTRL"                                , "Memory", 0xE0042060,        4, base=16
sfr = "OSC_CTRL.OSC32KHZDISABLE"                , "Memory", 0xE0042060,        4, base=16,    bitRange=0-0
sfr = "OSC_CTRL.OSCMAINDISABLE"                 , "Memory", 0xE0042060,        4, base=16,    bitRange=1-1

sfr = "VTG_CTRL"                                , "Memory", 0xE0042064,        4, base=16
sfr = "VTG_CTRL.RTCIF_FWVRON"                   , "Memory", 0xE0042064,        4, base=16,    bitRange=0-0
sfr = "VTG_CTRL.RTCIF_VRONENABLE"               , "Memory", 0xE0042064,        4, base=16,    bitRange=1-1
sfr = "VTG_CTRL.RTCIF_CLRPUBINT"                , "Memory", 0xE0042064,        4, base=16,    bitRange=2-2
sfr = "VTG_CTRL.VBATSELECT"                     , "Memory", 0xE0042064,        4, base=16,    bitRange=3-3
sfr = "VTG_CTRL.BGPSMENABLE"                    , "Memory", 0xE0042064,        4, base=16,    bitRange=4-4

sfr = "SPARE"                                   , "Memory", 0xE0042068,        4, base=16
sfr = "SPARE.DSS_SPARE_OUT"                     , "Memory", 0xE0042068,        4, base=16,    bitRange=0-15
sfr = "SPARE.DSS_SPARE_IN"                      , "Memory", 0xE0042068,        4, base=16,    bitRange=16-31

sfr = "FAB_IF"                                  , "Memory", 0xE004206C,        4, base=16
sfr = "FAB_IF.FAB_AHB_BYPASS"                   , "Memory", 0xE004206C,        4, base=16,    bitRange=0-0
sfr = "FAB_IF.F2_AHBCAPABLE"                    , "Memory", 0xE004206C,        4, base=16,    bitRange=1-1
sfr = "FAB_IF.FAB_AHBIF"                        , "Memory", 0xE004206C,        4, base=16,    bitRange=2-2
sfr = "FAB_IF.FAB_APB32"                        , "Memory", 0xE004206C,        4, base=16,    bitRange=3-3
sfr = "FAB_IF.F2_LARGE_CT_XS"                   , "Memory", 0xE004206C,        4, base=16,    bitRange=4-4
sfr = "FAB_IF.FABCALIBSTART"                    , "Memory", 0xE004206C,        4, base=16,    bitRange=5-5
sfr = "FAB_IF.FABCALIBFAIL"                     , "Memory", 0xE004206C,        4, base=16,    bitRange=6-6

sfr = "APB_EXTN"                                , "Memory", 0xE0042070,        4, base=16
sfr = "APB_EXTN.APB16_XHOLD"                    , "Memory", 0xE0042070,        4, base=16,    bitRange=0-15

sfr = "LOOPBACK_CTRL"                           , "Memory", 0xE0042074,        4, base=16
sfr = "LOOPBACK_CTRL.DSS_UARTLOOPBACK"          , "Memory", 0xE0042074,        4, base=16,    bitRange=0-0
sfr = "LOOPBACK_CTRL.DSS_SPILOOPBACK"           , "Memory", 0xE0042074,        4, base=16,    bitRange=1-1
sfr = "LOOPBACK_CTRL.DSS_I2CLOOPBACK"           , "Memory", 0xE0042074,        4, base=16,    bitRange=2-2
sfr = "LOOPBACK_CTRL.DSS_GPIOLOOPBACK"          , "Memory", 0xE0042074,        4, base=16,    bitRange=3-3
sfr = "LOOPBACK_CTRL.DSS_EMACLOOPBACK"          , "Memory", 0xE0042074,        4, base=16,    bitRange=4-4

sfr = "IO_BANK_CONFIG"                          , "Memory", 0xE0042078,        4, base=16
sfr = "IO_BANK_CONFIG.BTEAST"                   , "Memory", 0xE0042078,        4, base=16,    bitRange=0-1
sfr = "IO_BANK_CONFIG.BTWEST"                   , "Memory", 0xE0042078,        4, base=16,    bitRange=2-3

sfr = "GPIN_SRC_SEL"                            , "Memory", 0xE004207C,        4, base=16
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE0"            , "Memory", 0xE004207C,        4, base=16,    bitRange=0-0
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE1"            , "Memory", 0xE004207C,        4, base=16,    bitRange=1-1
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE2"            , "Memory", 0xE004207C,        4, base=16,    bitRange=2-2
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE3"            , "Memory", 0xE004207C,        4, base=16,    bitRange=3-3
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE4"            , "Memory", 0xE004207C,        4, base=16,    bitRange=4-4
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE5"            , "Memory", 0xE004207C,        4, base=16,    bitRange=5-5
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE6"            , "Memory", 0xE004207C,        4, base=16,    bitRange=6-6
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE7"            , "Memory", 0xE004207C,        4, base=16,    bitRange=7-7
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE8"            , "Memory", 0xE004207C,        4, base=16,    bitRange=8-8
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE9"            , "Memory", 0xE004207C,        4, base=16,    bitRange=9-9
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE10"           , "Memory", 0xE004207C,        4, base=16,    bitRange=10-10
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE11"           , "Memory", 0xE004207C,        4, base=16,    bitRange=11-11
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE12"           , "Memory", 0xE004207C,        4, base=16,    bitRange=12-12
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE13"           , "Memory", 0xE004207C,        4, base=16,    bitRange=13-13
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE14"           , "Memory", 0xE004207C,        4, base=16,    bitRange=14-14
sfr = "GPIN_SRC_SEL.DSS_GPINSOURCE15"           , "Memory", 0xE004207C,        4, base=16,    bitRange=15-15

sfr = "TEST_STATUS"                             , "Memory", 0xE0042080,        4, base=16
sfr = "TEST_STATUS.F2_FACTORY_TEST_MODE"        , "Memory", 0xE0042080,        4, base=16,    bitRange=0-0
sfr = "TEST_STATUS.RED_REP_NOGO"                , "Memory", 0xE0042080,        4, base=16,    bitRange=1-1
sfr = "TEST_STATUS.Reserved"                    , "Memory", 0xE0042080,        4, base=16,    bitRange=2-3
sfr = "TEST_STATUS.RED_REP_LOC00VALID"          , "Memory", 0xE0042080,        4, base=16,    bitRange=4-4
sfr = "TEST_STATUS.RED_REP_LOC01VALID"          , "Memory", 0xE0042080,        4, base=16,    bitRange=5-5
sfr = "TEST_STATUS.RED_REP_LOC02VALID"          , "Memory", 0xE0042080,        4, base=16,    bitRange=6-6
sfr = "TEST_STATUS.RED_REP_LOC03VALID"          , "Memory", 0xE0042080,        4, base=16,    bitRange=7-7
sfr = "TEST_STATUS.RED_REP_LOC10VALID"          , "Memory", 0xE0042080,        4, base=16,    bitRange=8-8
sfr = "TEST_STATUS.RED_REP_LOC11VALID"          , "Memory", 0xE0042080,        4, base=16,    bitRange=9-9
sfr = "TEST_STATUS.RED_REP_LOC12VALID"          , "Memory", 0xE0042080,        4, base=16,    bitRange=10-10
sfr = "TEST_STATUS.RED_REP_LOC13VALID"          , "Memory", 0xE0042080,        4, base=16,    bitRange=11-11
sfr = "TEST_STATUS.MAX_REACHED"                 , "Memory", 0xE0042080,        4, base=16,    bitRange=12-12

sfr = "RED_REP_ADDR0"                           , "Memory", 0xE0042084,        4, base=16
sfr = "RED_REP_ADDR0.RED_REP_ADDR0"             , "Memory", 0xE0042084,        4, base=16,    bitRange=0-12

sfr = "RED_REP_LOW_LOCS0"                       , "Memory", 0xE0042088,        4, base=16
sfr = "RED_REP_LOW_LOCS0.RED_REP_LOC00"         , "Memory", 0xE0042088,        4, base=16,    bitRange=0-12
sfr = "RED_REP_LOW_LOCS0.RED_REP_LOC01"         , "Memory", 0xE0042088,        4, base=16,    bitRange=16-28

sfr = "RED_REP_HIGH_LOCS0"                       , "Memory", 0xE004208C,        4, base=16
sfr = "RED_REP_HIGH_LOCS0.RED_REP_LOC02"         , "Memory", 0xE004208C,        4, base=16,    bitRange=0-12
sfr = "RED_REP_HIGH_LOCS0.RED_REP_LOC03"         , "Memory", 0xE004208C,        4, base=16,    bitRange=16-28

sfr = "RED_REP_ADDR1"                           , "Memory", 0xE0042090,        4, base=16
sfr = "RED_REP_ADDR1.RED_REP_ADDR1"             , "Memory", 0xE0042090,        4, base=16,    bitRange=0-12

sfr = "RED_REP_LOW_LOCS1"                       , "Memory", 0xE0042094,        4, base=16
sfr = "RED_REP_LOW_LOCS1.RED_REP_LOC10"         , "Memory", 0xE0042094,        4, base=16,    bitRange=0-12
sfr = "RED_REP_LOW_LOCS1.RED_REP_LOC11"         , "Memory", 0xE0042094,        4, base=16,    bitRange=16-28

sfr = "RED_REP_HIGH_LOCS1"                       , "Memory", 0xE0042098,        4, base=16
sfr = "RED_REP_HIGH_LOCS1.RED_REP_LOC12"         , "Memory", 0xE0042098,        4, base=16,    bitRange=0-12
sfr = "RED_REP_HIGH_LOCS1.RED_REP_LOC13"         , "Memory", 0xE0042098,        4, base=16,    bitRange=16-28

sfr = "FPGA_CTRL"                               , "Memory", 0xE004209C,        4, base=16
sfr = "FPGA_CTRL.USTDBY_D"                      , "Memory", 0xE004209C,        4, base=16,    bitRange=0-0
sfr = "FPGA_CTRL.IO_CNTL"                       , "Memory", 0xE004209C,        4, base=16,    bitRange=1-1
sfr = "FPGA_CTRL.FPGA_ENABLE"                   , "Memory", 0xE004209C,        4, base=16,    bitRange=2-2

sfr = "IOMUXCELL_0_CONFIG"   , "Memory", 0xE0042100,        4, base=16
sfr = "IOMUXCELL_0_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042100,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_0_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042100,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_0_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042100,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_0_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042100,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_0_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042100,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_0_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042100,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_0_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042100,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_0_CONFIG.DSS_PU"   , "Memory", 0xE0042100,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_0_CONFIG.DSS_PD"   , "Memory", 0xE0042100,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_0_CONFIG.DSS_ST"   , "Memory", 0xE0042100,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_1_CONFIG"   , "Memory", 0xE0042104,        4, base=16
sfr = "IOMUXCELL_1_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042104,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_1_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042104,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_1_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042104,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_1_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042104,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_1_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042104,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_1_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042104,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_1_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042104,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_1_CONFIG.DSS_PU"   , "Memory", 0xE0042104,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_1_CONFIG.DSS_PD"   , "Memory", 0xE0042104,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_1_CONFIG.DSS_ST"   , "Memory", 0xE0042104,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_2_CONFIG"   , "Memory", 0xE0042108,        4, base=16
sfr = "IOMUXCELL_2_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042108,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_2_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042108,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_2_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042108,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_2_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042108,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_2_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042108,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_2_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042108,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_2_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042108,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_2_CONFIG.DSS_PU"   , "Memory", 0xE0042108,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_2_CONFIG.DSS_PD"   , "Memory", 0xE0042108,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_2_CONFIG.DSS_ST"   , "Memory", 0xE0042108,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_3_CONFIG"   , "Memory", 0xE004210C,        4, base=16
sfr = "IOMUXCELL_3_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004210C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_3_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004210C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_3_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004210C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_3_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004210C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_3_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004210C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_3_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004210C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_3_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004210C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_3_CONFIG.DSS_PU"   , "Memory", 0xE004210C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_3_CONFIG.DSS_PD"   , "Memory", 0xE004210C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_3_CONFIG.DSS_ST"   , "Memory", 0xE004210C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_4_CONFIG"   , "Memory", 0xE0042110,        4, base=16
sfr = "IOMUXCELL_4_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042110,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_4_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042110,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_4_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042110,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_4_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042110,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_4_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042110,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_4_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042110,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_4_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042110,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_4_CONFIG.DSS_PU"   , "Memory", 0xE0042110,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_4_CONFIG.DSS_PD"   , "Memory", 0xE0042110,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_4_CONFIG.DSS_ST"   , "Memory", 0xE0042110,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_5_CONFIG"   , "Memory", 0xE0042114,        4, base=16
sfr = "IOMUXCELL_5_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042114,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_5_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042114,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_5_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042114,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_5_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042114,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_5_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042114,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_5_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042114,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_5_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042114,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_5_CONFIG.DSS_PU"   , "Memory", 0xE0042114,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_5_CONFIG.DSS_PD"   , "Memory", 0xE0042114,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_5_CONFIG.DSS_ST"   , "Memory", 0xE0042114,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_6_CONFIG"   , "Memory", 0xE0042118,        4, base=16
sfr = "IOMUXCELL_6_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042118,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_6_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042118,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_6_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042118,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_6_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042118,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_6_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042118,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_6_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042118,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_6_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042118,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_6_CONFIG.DSS_PU"   , "Memory", 0xE0042118,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_6_CONFIG.DSS_PD"   , "Memory", 0xE0042118,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_6_CONFIG.DSS_ST"   , "Memory", 0xE0042118,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_7_CONFIG"   , "Memory", 0xE004211C,        4, base=16
sfr = "IOMUXCELL_7_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004211C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_7_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004211C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_7_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004211C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_7_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004211C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_7_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004211C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_7_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004211C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_7_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004211C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_7_CONFIG.DSS_PU"   , "Memory", 0xE004211C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_7_CONFIG.DSS_PD"   , "Memory", 0xE004211C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_7_CONFIG.DSS_ST"   , "Memory", 0xE004211C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_8_CONFIG"   , "Memory", 0xE0042120,        4, base=16
sfr = "IOMUXCELL_8_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042120,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_8_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042120,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_8_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042120,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_8_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042120,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_8_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042120,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_8_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042120,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_8_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042120,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_8_CONFIG.DSS_PU"   , "Memory", 0xE0042120,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_8_CONFIG.DSS_PD"   , "Memory", 0xE0042120,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_8_CONFIG.DSS_ST"   , "Memory", 0xE0042120,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_9_CONFIG"   , "Memory", 0xE0042124,        4, base=16
sfr = "IOMUXCELL_9_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042124,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_9_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042124,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_9_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042124,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_9_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042124,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_9_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042124,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_9_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042124,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_9_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042124,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_9_CONFIG.DSS_PU"   , "Memory", 0xE0042124,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_9_CONFIG.DSS_PD"   , "Memory", 0xE0042124,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_9_CONFIG.DSS_ST"   , "Memory", 0xE0042124,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_10_CONFIG"   , "Memory", 0xE0042128,        4, base=16
sfr = "IOMUXCELL_10_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042128,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_10_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042128,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_10_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042128,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_10_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042128,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_10_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042128,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_10_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042128,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_10_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042128,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_10_CONFIG.DSS_PU"   , "Memory", 0xE0042128,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_10_CONFIG.DSS_PD"   , "Memory", 0xE0042128,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_10_CONFIG.DSS_ST"   , "Memory", 0xE0042128,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_11_CONFIG"   , "Memory", 0xE004212C,        4, base=16
sfr = "IOMUXCELL_11_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004212C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_11_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004212C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_11_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004212C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_11_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004212C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_11_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004212C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_11_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004212C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_11_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004212C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_11_CONFIG.DSS_PU"   , "Memory", 0xE004212C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_11_CONFIG.DSS_PD"   , "Memory", 0xE004212C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_11_CONFIG.DSS_ST"   , "Memory", 0xE004212C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_12_CONFIG"   , "Memory", 0xE0042130,        4, base=16
sfr = "IOMUXCELL_12_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042130,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_12_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042130,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_12_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042130,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_12_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042130,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_12_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042130,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_12_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042130,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_12_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042130,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_12_CONFIG.DSS_PU"   , "Memory", 0xE0042130,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_12_CONFIG.DSS_PD"   , "Memory", 0xE0042130,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_12_CONFIG.DSS_ST"   , "Memory", 0xE0042130,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_13_CONFIG"   , "Memory", 0xE0042134,        4, base=16
sfr = "IOMUXCELL_13_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042134,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_13_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042134,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_13_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042134,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_13_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042134,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_13_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042134,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_13_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042134,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_13_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042134,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_13_CONFIG.DSS_PU"   , "Memory", 0xE0042134,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_13_CONFIG.DSS_PD"   , "Memory", 0xE0042134,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_13_CONFIG.DSS_ST"   , "Memory", 0xE0042134,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_14_CONFIG"   , "Memory", 0xE0042138,        4, base=16
sfr = "IOMUXCELL_14_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042138,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_14_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042138,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_14_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042138,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_14_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042138,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_14_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042138,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_14_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042138,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_14_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042138,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_14_CONFIG.DSS_PU"   , "Memory", 0xE0042138,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_14_CONFIG.DSS_PD"   , "Memory", 0xE0042138,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_14_CONFIG.DSS_ST"   , "Memory", 0xE0042138,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_15_CONFIG"   , "Memory", 0xE004213C,        4, base=16
sfr = "IOMUXCELL_15_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004213C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_15_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004213C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_15_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004213C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_15_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004213C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_15_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004213C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_15_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004213C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_15_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004213C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_15_CONFIG.DSS_PU"   , "Memory", 0xE004213C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_15_CONFIG.DSS_PD"   , "Memory", 0xE004213C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_15_CONFIG.DSS_ST"   , "Memory", 0xE004213C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_16_CONFIG"   , "Memory", 0xE0042140,        4, base=16
sfr = "IOMUXCELL_16_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042140,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_16_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042140,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_16_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042140,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_16_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042140,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_16_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042140,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_16_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042140,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_16_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042140,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_16_CONFIG.DSS_PU"   , "Memory", 0xE0042140,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_16_CONFIG.DSS_PD"   , "Memory", 0xE0042140,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_16_CONFIG.DSS_ST"   , "Memory", 0xE0042140,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_17_CONFIG"   , "Memory", 0xE0042144,        4, base=16
sfr = "IOMUXCELL_17_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042144,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_17_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042144,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_17_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042144,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_17_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042144,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_17_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042144,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_17_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042144,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_17_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042144,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_17_CONFIG.DSS_PU"   , "Memory", 0xE0042144,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_17_CONFIG.DSS_PD"   , "Memory", 0xE0042144,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_17_CONFIG.DSS_ST"   , "Memory", 0xE0042144,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_18_CONFIG"   , "Memory", 0xE0042148,        4, base=16
sfr = "IOMUXCELL_18_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042148,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_18_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042148,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_18_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042148,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_18_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042148,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_18_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042148,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_18_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042148,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_18_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042148,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_18_CONFIG.DSS_PU"   , "Memory", 0xE0042148,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_18_CONFIG.DSS_PD"   , "Memory", 0xE0042148,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_18_CONFIG.DSS_ST"   , "Memory", 0xE0042148,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_19_CONFIG"   , "Memory", 0xE004214C,        4, base=16
sfr = "IOMUXCELL_19_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004214C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_19_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004214C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_19_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004214C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_19_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004214C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_19_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004214C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_19_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004214C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_19_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004214C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_19_CONFIG.DSS_PU"   , "Memory", 0xE004214C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_19_CONFIG.DSS_PD"   , "Memory", 0xE004214C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_19_CONFIG.DSS_ST"   , "Memory", 0xE004214C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_20_CONFIG"   , "Memory", 0xE0042150,        4, base=16
sfr = "IOMUXCELL_20_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042150,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_20_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042150,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_20_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042150,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_20_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042150,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_20_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042150,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_20_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042150,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_20_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042150,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_20_CONFIG.DSS_PU"   , "Memory", 0xE0042150,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_20_CONFIG.DSS_PD"   , "Memory", 0xE0042150,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_20_CONFIG.DSS_ST"   , "Memory", 0xE0042150,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_21_CONFIG"   , "Memory", 0xE0042154,        4, base=16
sfr = "IOMUXCELL_21_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042154,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_21_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042154,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_21_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042154,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_21_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042154,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_21_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042154,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_21_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042154,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_21_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042154,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_21_CONFIG.DSS_PU"   , "Memory", 0xE0042154,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_21_CONFIG.DSS_PD"   , "Memory", 0xE0042154,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_21_CONFIG.DSS_ST"   , "Memory", 0xE0042154,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_22_CONFIG"   , "Memory", 0xE0042158,        4, base=16
sfr = "IOMUXCELL_22_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042158,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_22_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042158,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_22_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042158,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_22_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042158,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_22_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042158,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_22_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042158,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_22_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042158,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_22_CONFIG.DSS_PU"   , "Memory", 0xE0042158,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_22_CONFIG.DSS_PD"   , "Memory", 0xE0042158,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_22_CONFIG.DSS_ST"   , "Memory", 0xE0042158,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_23_CONFIG"   , "Memory", 0xE004215C,        4, base=16
sfr = "IOMUXCELL_23_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004215C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_23_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004215C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_23_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004215C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_23_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004215C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_23_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004215C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_23_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004215C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_23_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004215C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_23_CONFIG.DSS_PU"   , "Memory", 0xE004215C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_23_CONFIG.DSS_PD"   , "Memory", 0xE004215C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_23_CONFIG.DSS_ST"   , "Memory", 0xE004215C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_24_CONFIG"   , "Memory", 0xE0042160,        4, base=16
sfr = "IOMUXCELL_24_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042160,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_24_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042160,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_24_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042160,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_24_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042160,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_24_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042160,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_24_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042160,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_24_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042160,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_24_CONFIG.DSS_PU"   , "Memory", 0xE0042160,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_24_CONFIG.DSS_PD"   , "Memory", 0xE0042160,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_24_CONFIG.DSS_ST"   , "Memory", 0xE0042160,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_25_CONFIG"   , "Memory", 0xE0042164,        4, base=16
sfr = "IOMUXCELL_25_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042164,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_25_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042164,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_25_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042164,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_25_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042164,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_25_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042164,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_25_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042164,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_25_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042164,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_25_CONFIG.DSS_PU"   , "Memory", 0xE0042164,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_25_CONFIG.DSS_PD"   , "Memory", 0xE0042164,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_25_CONFIG.DSS_ST"   , "Memory", 0xE0042164,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_26_CONFIG"   , "Memory", 0xE0042168,        4, base=16
sfr = "IOMUXCELL_26_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042168,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_26_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042168,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_26_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042168,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_26_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042168,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_26_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042168,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_26_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042168,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_26_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042168,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_26_CONFIG.DSS_PU"   , "Memory", 0xE0042168,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_26_CONFIG.DSS_PD"   , "Memory", 0xE0042168,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_26_CONFIG.DSS_ST"   , "Memory", 0xE0042168,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_27_CONFIG"   , "Memory", 0xE004216C,        4, base=16
sfr = "IOMUXCELL_27_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004216C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_27_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004216C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_27_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004216C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_27_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004216C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_27_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004216C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_27_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004216C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_27_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004216C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_27_CONFIG.DSS_PU"   , "Memory", 0xE004216C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_27_CONFIG.DSS_PD"   , "Memory", 0xE004216C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_27_CONFIG.DSS_ST"   , "Memory", 0xE004216C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_28_CONFIG"   , "Memory", 0xE0042170,        4, base=16
sfr = "IOMUXCELL_28_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042170,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_28_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042170,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_28_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042170,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_28_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042170,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_28_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042170,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_28_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042170,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_28_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042170,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_28_CONFIG.DSS_PU"   , "Memory", 0xE0042170,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_28_CONFIG.DSS_PD"   , "Memory", 0xE0042170,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_28_CONFIG.DSS_ST"   , "Memory", 0xE0042170,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_29_CONFIG"   , "Memory", 0xE0042174,        4, base=16
sfr = "IOMUXCELL_29_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042174,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_29_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042174,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_29_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042174,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_29_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042174,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_29_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042174,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_29_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042174,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_29_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042174,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_29_CONFIG.DSS_PU"   , "Memory", 0xE0042174,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_29_CONFIG.DSS_PD"   , "Memory", 0xE0042174,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_29_CONFIG.DSS_ST"   , "Memory", 0xE0042174,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_30_CONFIG"   , "Memory", 0xE0042178,        4, base=16
sfr = "IOMUXCELL_30_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042178,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_30_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042178,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_30_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042178,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_30_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042178,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_30_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042178,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_30_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042178,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_30_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042178,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_30_CONFIG.DSS_PU"   , "Memory", 0xE0042178,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_30_CONFIG.DSS_PD"   , "Memory", 0xE0042178,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_30_CONFIG.DSS_ST"   , "Memory", 0xE0042178,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_31_CONFIG"   , "Memory", 0xE004217C,        4, base=16
sfr = "IOMUXCELL_31_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004217C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_31_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004217C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_31_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004217C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_31_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004217C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_31_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004217C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_31_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004217C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_31_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004217C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_31_CONFIG.DSS_PU"   , "Memory", 0xE004217C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_31_CONFIG.DSS_PD"   , "Memory", 0xE004217C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_31_CONFIG.DSS_ST"   , "Memory", 0xE004217C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_32_CONFIG"   , "Memory", 0xE0042180,        4, base=16
sfr = "IOMUXCELL_32_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042180,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_32_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042180,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_32_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042180,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_32_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042180,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_32_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042180,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_32_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042180,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_32_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042180,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_32_CONFIG.DSS_PU"   , "Memory", 0xE0042180,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_32_CONFIG.DSS_PD"   , "Memory", 0xE0042180,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_32_CONFIG.DSS_ST"   , "Memory", 0xE0042180,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_33_CONFIG"   , "Memory", 0xE0042184,        4, base=16
sfr = "IOMUXCELL_33_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042184,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_33_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042184,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_33_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042184,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_33_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042184,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_33_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042184,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_33_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042184,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_33_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042184,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_33_CONFIG.DSS_PU"   , "Memory", 0xE0042184,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_33_CONFIG.DSS_PD"   , "Memory", 0xE0042184,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_33_CONFIG.DSS_ST"   , "Memory", 0xE0042184,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_34_CONFIG"   , "Memory", 0xE0042188,        4, base=16
sfr = "IOMUXCELL_34_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042188,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_34_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042188,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_34_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042188,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_34_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042188,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_34_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042188,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_34_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042188,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_34_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042188,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_34_CONFIG.DSS_PU"   , "Memory", 0xE0042188,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_34_CONFIG.DSS_PD"   , "Memory", 0xE0042188,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_34_CONFIG.DSS_ST"   , "Memory", 0xE0042188,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_35_CONFIG"   , "Memory", 0xE004218C,        4, base=16
sfr = "IOMUXCELL_35_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004218C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_35_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004218C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_35_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004218C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_35_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004218C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_35_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004218C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_35_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004218C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_35_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004218C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_35_CONFIG.DSS_PU"   , "Memory", 0xE004218C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_35_CONFIG.DSS_PD"   , "Memory", 0xE004218C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_35_CONFIG.DSS_ST"   , "Memory", 0xE004218C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_36_CONFIG"   , "Memory", 0xE0042190,        4, base=16
sfr = "IOMUXCELL_36_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042190,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_36_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042190,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_36_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042190,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_36_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042190,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_36_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042190,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_36_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042190,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_36_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042190,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_36_CONFIG.DSS_PU"   , "Memory", 0xE0042190,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_36_CONFIG.DSS_PD"   , "Memory", 0xE0042190,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_36_CONFIG.DSS_ST"   , "Memory", 0xE0042190,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_37_CONFIG"   , "Memory", 0xE0042194,        4, base=16
sfr = "IOMUXCELL_37_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042194,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_37_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042194,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_37_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042194,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_37_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042194,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_37_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042194,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_37_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042194,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_37_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042194,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_37_CONFIG.DSS_PU"   , "Memory", 0xE0042194,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_37_CONFIG.DSS_PD"   , "Memory", 0xE0042194,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_37_CONFIG.DSS_ST"   , "Memory", 0xE0042194,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_38_CONFIG"   , "Memory", 0xE0042198,        4, base=16
sfr = "IOMUXCELL_38_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042198,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_38_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042198,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_38_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042198,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_38_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042198,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_38_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042198,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_38_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042198,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_38_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042198,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_38_CONFIG.DSS_PU"   , "Memory", 0xE0042198,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_38_CONFIG.DSS_PD"   , "Memory", 0xE0042198,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_38_CONFIG.DSS_ST"   , "Memory", 0xE0042198,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_39_CONFIG"   , "Memory", 0xE004219C,        4, base=16
sfr = "IOMUXCELL_39_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004219C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_39_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004219C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_39_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004219C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_39_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004219C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_39_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004219C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_39_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004219C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_39_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004219C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_39_CONFIG.DSS_PU"   , "Memory", 0xE004219C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_39_CONFIG.DSS_PD"   , "Memory", 0xE004219C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_39_CONFIG.DSS_ST"   , "Memory", 0xE004219C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_40_CONFIG"   , "Memory", 0xE00421A0,        4, base=16
sfr = "IOMUXCELL_40_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_40_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_40_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_40_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_40_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_40_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_40_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_40_CONFIG.DSS_PU"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_40_CONFIG.DSS_PD"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_40_CONFIG.DSS_ST"   , "Memory", 0xE00421A0,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_41_CONFIG"   , "Memory", 0xE00421A4,        4, base=16
sfr = "IOMUXCELL_41_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_41_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_41_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_41_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_41_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_41_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_41_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_41_CONFIG.DSS_PU"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_41_CONFIG.DSS_PD"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_41_CONFIG.DSS_ST"   , "Memory", 0xE00421A4,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_42_CONFIG"   , "Memory", 0xE00421A8,        4, base=16
sfr = "IOMUXCELL_42_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_42_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_42_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_42_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_42_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_42_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_42_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_42_CONFIG.DSS_PU"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_42_CONFIG.DSS_PD"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_42_CONFIG.DSS_ST"   , "Memory", 0xE00421A8,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_43_CONFIG"   , "Memory", 0xE00421AC,        4, base=16
sfr = "IOMUXCELL_43_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_43_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_43_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_43_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_43_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_43_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_43_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_43_CONFIG.DSS_PU"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_43_CONFIG.DSS_PD"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_43_CONFIG.DSS_ST"   , "Memory", 0xE00421AC,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_44_CONFIG"   , "Memory", 0xE00421B0,        4, base=16
sfr = "IOMUXCELL_44_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_44_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_44_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_44_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_44_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_44_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_44_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_44_CONFIG.DSS_PU"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_44_CONFIG.DSS_PD"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_44_CONFIG.DSS_ST"   , "Memory", 0xE00421B0,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_45_CONFIG"   , "Memory", 0xE00421B4,        4, base=16
sfr = "IOMUXCELL_45_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_45_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_45_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_45_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_45_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_45_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_45_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_45_CONFIG.DSS_PU"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_45_CONFIG.DSS_PD"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_45_CONFIG.DSS_ST"   , "Memory", 0xE00421B4,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_46_CONFIG"   , "Memory", 0xE00421B8,        4, base=16
sfr = "IOMUXCELL_46_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_46_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_46_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_46_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_46_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_46_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_46_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_46_CONFIG.DSS_PU"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_46_CONFIG.DSS_PD"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_46_CONFIG.DSS_ST"   , "Memory", 0xE00421B8,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_47_CONFIG"   , "Memory", 0xE00421BC,        4, base=16
sfr = "IOMUXCELL_47_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_47_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_47_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_47_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_47_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_47_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_47_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_47_CONFIG.DSS_PU"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_47_CONFIG.DSS_PD"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_47_CONFIG.DSS_ST"   , "Memory", 0xE00421BC,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_48_CONFIG"   , "Memory", 0xE00421C0,        4, base=16
sfr = "IOMUXCELL_48_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_48_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_48_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_48_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_48_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_48_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_48_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_48_CONFIG.DSS_PU"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_48_CONFIG.DSS_PD"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_48_CONFIG.DSS_ST"   , "Memory", 0xE00421C0,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_49_CONFIG"   , "Memory", 0xE00421C4,        4, base=16
sfr = "IOMUXCELL_49_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_49_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_49_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_49_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_49_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_49_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_49_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_49_CONFIG.DSS_PU"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_49_CONFIG.DSS_PD"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_49_CONFIG.DSS_ST"   , "Memory", 0xE00421C4,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_50_CONFIG"   , "Memory", 0xE00421C8,        4, base=16
sfr = "IOMUXCELL_50_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_50_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_50_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_50_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_50_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_50_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_50_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_50_CONFIG.DSS_PU"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_50_CONFIG.DSS_PD"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_50_CONFIG.DSS_ST"   , "Memory", 0xE00421C8,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_51_CONFIG"   , "Memory", 0xE00421CC,        4, base=16
sfr = "IOMUXCELL_51_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_51_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_51_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_51_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_51_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_51_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_51_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_51_CONFIG.DSS_PU"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_51_CONFIG.DSS_PD"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_51_CONFIG.DSS_ST"   , "Memory", 0xE00421CC,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_52_CONFIG"   , "Memory", 0xE00421D0,        4, base=16
sfr = "IOMUXCELL_52_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_52_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_52_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_52_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_52_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_52_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_52_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_52_CONFIG.DSS_PU"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_52_CONFIG.DSS_PD"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_52_CONFIG.DSS_ST"   , "Memory", 0xE00421D0,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_53_CONFIG"   , "Memory", 0xE00421D4,        4, base=16
sfr = "IOMUXCELL_53_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_53_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_53_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_53_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_53_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_53_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_53_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_53_CONFIG.DSS_PU"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_53_CONFIG.DSS_PD"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_53_CONFIG.DSS_ST"   , "Memory", 0xE00421D4,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_54_CONFIG"   , "Memory", 0xE00421D8,        4, base=16
sfr = "IOMUXCELL_54_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_54_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_54_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_54_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_54_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_54_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_54_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_54_CONFIG.DSS_PU"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_54_CONFIG.DSS_PD"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_54_CONFIG.DSS_ST"   , "Memory", 0xE00421D8,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_55_CONFIG"   , "Memory", 0xE00421DC,        4, base=16
sfr = "IOMUXCELL_55_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_55_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_55_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_55_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_55_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_55_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_55_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_55_CONFIG.DSS_PU"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_55_CONFIG.DSS_PD"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_55_CONFIG.DSS_ST"   , "Memory", 0xE00421DC,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_56_CONFIG"   , "Memory", 0xE00421E0,        4, base=16
sfr = "IOMUXCELL_56_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_56_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_56_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_56_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_56_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_56_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_56_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_56_CONFIG.DSS_PU"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_56_CONFIG.DSS_PD"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_56_CONFIG.DSS_ST"   , "Memory", 0xE00421E0,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_57_CONFIG"   , "Memory", 0xE00421E4,        4, base=16
sfr = "IOMUXCELL_57_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_57_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_57_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_57_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_57_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_57_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_57_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_57_CONFIG.DSS_PU"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_57_CONFIG.DSS_PD"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_57_CONFIG.DSS_ST"   , "Memory", 0xE00421E4,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_58_CONFIG"   , "Memory", 0xE00421E8,        4, base=16
sfr = "IOMUXCELL_58_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_58_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_58_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_58_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_58_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_58_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_58_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_58_CONFIG.DSS_PU"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_58_CONFIG.DSS_PD"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_58_CONFIG.DSS_ST"   , "Memory", 0xE00421E8,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_59_CONFIG"   , "Memory", 0xE00421EC,        4, base=16
sfr = "IOMUXCELL_59_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_59_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_59_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_59_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_59_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_59_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_59_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_59_CONFIG.DSS_PU"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_59_CONFIG.DSS_PD"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_59_CONFIG.DSS_ST"   , "Memory", 0xE00421EC,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_60_CONFIG"   , "Memory", 0xE00421F0,        4, base=16
sfr = "IOMUXCELL_60_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_60_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_60_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_60_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_60_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_60_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_60_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_60_CONFIG.DSS_PU"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_60_CONFIG.DSS_PD"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_60_CONFIG.DSS_ST"   , "Memory", 0xE00421F0,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_61_CONFIG"   , "Memory", 0xE00421F4,        4, base=16
sfr = "IOMUXCELL_61_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_61_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_61_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_61_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_61_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_61_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_61_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_61_CONFIG.DSS_PU"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_61_CONFIG.DSS_PD"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_61_CONFIG.DSS_ST"   , "Memory", 0xE00421F4,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_62_CONFIG"   , "Memory", 0xE00421F8,        4, base=16
sfr = "IOMUXCELL_62_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_62_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_62_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_62_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_62_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_62_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_62_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_62_CONFIG.DSS_PU"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_62_CONFIG.DSS_PD"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_62_CONFIG.DSS_ST"   , "Memory", 0xE00421F8,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_63_CONFIG"   , "Memory", 0xE00421FC,        4, base=16
sfr = "IOMUXCELL_63_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_63_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_63_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_63_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_63_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_63_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_63_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_63_CONFIG.DSS_PU"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_63_CONFIG.DSS_PD"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_63_CONFIG.DSS_ST"   , "Memory", 0xE00421FC,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_64_CONFIG"   , "Memory", 0xE0042200,        4, base=16
sfr = "IOMUXCELL_64_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042200,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_64_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042200,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_64_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042200,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_64_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042200,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_64_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042200,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_64_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042200,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_64_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042200,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_64_CONFIG.DSS_PU"   , "Memory", 0xE0042200,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_64_CONFIG.DSS_PD"   , "Memory", 0xE0042200,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_64_CONFIG.DSS_ST"   , "Memory", 0xE0042200,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_65_CONFIG"   , "Memory", 0xE0042204,        4, base=16
sfr = "IOMUXCELL_65_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042204,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_65_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042204,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_65_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042204,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_65_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042204,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_65_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042204,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_65_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042204,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_65_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042204,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_65_CONFIG.DSS_PU"   , "Memory", 0xE0042204,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_65_CONFIG.DSS_PD"   , "Memory", 0xE0042204,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_65_CONFIG.DSS_ST"   , "Memory", 0xE0042204,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_66_CONFIG"   , "Memory", 0xE0042208,        4, base=16
sfr = "IOMUXCELL_66_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042208,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_66_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042208,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_66_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042208,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_66_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042208,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_66_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042208,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_66_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042208,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_66_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042208,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_66_CONFIG.DSS_PU"   , "Memory", 0xE0042208,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_66_CONFIG.DSS_PD"   , "Memory", 0xE0042208,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_66_CONFIG.DSS_ST"   , "Memory", 0xE0042208,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_67_CONFIG"   , "Memory", 0xE004220C,        4, base=16
sfr = "IOMUXCELL_67_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004220C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_67_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004220C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_67_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004220C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_67_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004220C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_67_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004220C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_67_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004220C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_67_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004220C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_67_CONFIG.DSS_PU"   , "Memory", 0xE004220C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_67_CONFIG.DSS_PD"   , "Memory", 0xE004220C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_67_CONFIG.DSS_ST"   , "Memory", 0xE004220C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_68_CONFIG"   , "Memory", 0xE0042210,        4, base=16
sfr = "IOMUXCELL_68_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042210,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_68_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042210,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_68_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042210,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_68_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042210,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_68_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042210,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_68_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042210,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_68_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042210,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_68_CONFIG.DSS_PU"   , "Memory", 0xE0042210,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_68_CONFIG.DSS_PD"   , "Memory", 0xE0042210,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_68_CONFIG.DSS_ST"   , "Memory", 0xE0042210,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_69_CONFIG"   , "Memory", 0xE0042214,        4, base=16
sfr = "IOMUXCELL_69_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042214,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_69_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042214,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_69_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042214,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_69_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042214,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_69_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042214,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_69_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042214,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_69_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042214,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_69_CONFIG.DSS_PU"   , "Memory", 0xE0042214,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_69_CONFIG.DSS_PD"   , "Memory", 0xE0042214,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_69_CONFIG.DSS_ST"   , "Memory", 0xE0042214,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_70_CONFIG"   , "Memory", 0xE0042218,        4, base=16
sfr = "IOMUXCELL_70_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042218,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_70_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042218,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_70_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042218,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_70_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042218,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_70_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042218,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_70_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042218,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_70_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042218,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_70_CONFIG.DSS_PU"   , "Memory", 0xE0042218,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_70_CONFIG.DSS_PD"   , "Memory", 0xE0042218,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_70_CONFIG.DSS_ST"   , "Memory", 0xE0042218,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_71_CONFIG"   , "Memory", 0xE004221C,        4, base=16
sfr = "IOMUXCELL_71_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004221C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_71_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004221C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_71_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004221C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_71_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004221C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_71_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004221C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_71_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004221C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_71_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004221C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_71_CONFIG.DSS_PU"   , "Memory", 0xE004221C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_71_CONFIG.DSS_PD"   , "Memory", 0xE004221C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_71_CONFIG.DSS_ST"   , "Memory", 0xE004221C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_72_CONFIG"   , "Memory", 0xE0042220,        4, base=16
sfr = "IOMUXCELL_72_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042220,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_72_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042220,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_72_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042220,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_72_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042220,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_72_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042220,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_72_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042220,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_72_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042220,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_72_CONFIG.DSS_PU"   , "Memory", 0xE0042220,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_72_CONFIG.DSS_PD"   , "Memory", 0xE0042220,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_72_CONFIG.DSS_ST"   , "Memory", 0xE0042220,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_73_CONFIG"   , "Memory", 0xE0042224,        4, base=16
sfr = "IOMUXCELL_73_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042224,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_73_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042224,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_73_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042224,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_73_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042224,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_73_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042224,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_73_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042224,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_73_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042224,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_73_CONFIG.DSS_PU"   , "Memory", 0xE0042224,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_73_CONFIG.DSS_PD"   , "Memory", 0xE0042224,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_73_CONFIG.DSS_ST"   , "Memory", 0xE0042224,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_74_CONFIG"   , "Memory", 0xE0042228,        4, base=16
sfr = "IOMUXCELL_74_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042228,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_74_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042228,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_74_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042228,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_74_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042228,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_74_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042228,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_74_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042228,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_74_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042228,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_74_CONFIG.DSS_PU"   , "Memory", 0xE0042228,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_74_CONFIG.DSS_PD"   , "Memory", 0xE0042228,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_74_CONFIG.DSS_ST"   , "Memory", 0xE0042228,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_75_CONFIG"   , "Memory", 0xE004222C,        4, base=16
sfr = "IOMUXCELL_75_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004222C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_75_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004222C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_75_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004222C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_75_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004222C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_75_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004222C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_75_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004222C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_75_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004222C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_75_CONFIG.DSS_PU"   , "Memory", 0xE004222C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_75_CONFIG.DSS_PD"   , "Memory", 0xE004222C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_75_CONFIG.DSS_ST"   , "Memory", 0xE004222C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_76_CONFIG"   , "Memory", 0xE0042230,        4, base=16
sfr = "IOMUXCELL_76_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042230,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_76_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042230,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_76_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042230,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_76_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042230,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_76_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042230,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_76_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042230,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_76_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042230,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_76_CONFIG.DSS_PU"   , "Memory", 0xE0042230,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_76_CONFIG.DSS_PD"   , "Memory", 0xE0042230,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_76_CONFIG.DSS_ST"   , "Memory", 0xE0042230,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_77_CONFIG"   , "Memory", 0xE0042234,        4, base=16
sfr = "IOMUXCELL_77_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042234,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_77_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042234,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_77_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042234,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_77_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042234,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_77_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042234,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_77_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042234,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_77_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042234,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_77_CONFIG.DSS_PU"   , "Memory", 0xE0042234,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_77_CONFIG.DSS_PD"   , "Memory", 0xE0042234,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_77_CONFIG.DSS_ST"   , "Memory", 0xE0042234,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_78_CONFIG"   , "Memory", 0xE0042238,        4, base=16
sfr = "IOMUXCELL_78_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042238,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_78_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042238,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_78_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042238,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_78_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042238,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_78_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042238,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_78_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042238,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_78_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042238,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_78_CONFIG.DSS_PU"   , "Memory", 0xE0042238,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_78_CONFIG.DSS_PD"   , "Memory", 0xE0042238,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_78_CONFIG.DSS_ST"   , "Memory", 0xE0042238,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_79_CONFIG"   , "Memory", 0xE004223C,        4, base=16
sfr = "IOMUXCELL_79_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE004223C,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_79_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE004223C,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_79_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE004223C,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_79_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE004223C,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_79_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE004223C,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_79_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE004223C,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_79_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE004223C,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_79_CONFIG.DSS_PU"   , "Memory", 0xE004223C,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_79_CONFIG.DSS_PD"   , "Memory", 0xE004223C,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_79_CONFIG.DSS_ST"   , "Memory", 0xE004223C,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_80_CONFIG"   , "Memory", 0xE0042240,        4, base=16
sfr = "IOMUXCELL_80_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042240,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_80_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042240,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_80_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042240,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_80_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042240,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_80_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042240,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_80_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042240,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_80_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042240,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_80_CONFIG.DSS_PU"   , "Memory", 0xE0042240,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_80_CONFIG.DSS_PD"   , "Memory", 0xE0042240,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_80_CONFIG.DSS_ST"   , "Memory", 0xE0042240,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_81_CONFIG"   , "Memory", 0xE0042244,        4, base=16
sfr = "IOMUXCELL_81_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042244,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_81_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042244,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_81_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042244,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_81_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042244,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_81_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042244,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_81_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042244,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_81_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042244,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_81_CONFIG.DSS_PU"   , "Memory", 0xE0042244,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_81_CONFIG.DSS_PD"   , "Memory", 0xE0042244,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_81_CONFIG.DSS_ST"   , "Memory", 0xE0042244,        4, base=16,    bitRange=9-9

sfr = "IOMUXCELL_82_CONFIG"   , "Memory", 0xE0042248,        4, base=16
sfr = "IOMUXCELL_82_CONFIG.DSS_IOMUXSEL0"   , "Memory", 0xE0042248,        4, base=16,    bitRange=0-0
sfr = "IOMUXCELL_82_CONFIG.DSS_IOMUXSEL1UPPER"   , "Memory", 0xE0042248,        4, base=16,    bitRange=1-1
sfr = "IOMUXCELL_82_CONFIG.DSS_IOMUXSEL1LOWER"   , "Memory", 0xE0042248,        4, base=16,    bitRange=2-2
sfr = "IOMUXCELL_82_CONFIG.DSS_IOMUXSEL2UPPER"   , "Memory", 0xE0042248,        4, base=16,    bitRange=3-3
sfr = "IOMUXCELL_82_CONFIG.DSS_IOMUXSEL2LOWER"   , "Memory", 0xE0042248,        4, base=16,    bitRange=4-4
sfr = "IOMUXCELL_82_CONFIG.DSS_IOMUXSEL3"   , "Memory", 0xE0042248,        4, base=16,    bitRange=5-5
sfr = "IOMUXCELL_82_CONFIG.DSS_IOMUXSEL4"   , "Memory", 0xE0042248,        4, base=16,    bitRange=6-6
sfr = "IOMUXCELL_82_CONFIG.DSS_PU"   , "Memory", 0xE0042248,        4, base=16,    bitRange=7-7
sfr = "IOMUXCELL_82_CONFIG.DSS_PD"   , "Memory", 0xE0042248,        4, base=16,    bitRange=8-8
sfr = "IOMUXCELL_82_CONFIG.DSS_ST"   , "Memory", 0xE0042248,        4, base=16,    bitRange=9-9


;
;		NVIC
;
;     Name                      Zone      Address     Bytesize  Displaybase Bitrange
;     ----                      ----      -------     --------  ----------- --------

sfr = "NVIC"                  , "Memory", 0xE000E004,        4, base=16
sfr = "NVIC.INTLINESNUM"      , "Memory", 0xE000E004,        4, base=16,    bitRange=0-4

sfr = "SYSTICKCSR"            , "Memory", 0xE000E010,        4, base=16
sfr = "SYSTICKCSR.ENABLE"     , "Memory", 0xE000E010,        4, base=16,    bitRange=0-0
sfr = "SYSTICKCSR.TICKINT"    , "Memory", 0xE000E010,        4, base=16,    bitRange=1-1
sfr = "SYSTICKCSR.CLKSOURCE"  , "Memory", 0xE000E010,        4, base=16,    bitRange=2-2
sfr = "SYSTICKCSR.COUNTFLAG"  , "Memory", 0xE000E010,        4, base=16,    bitRange=16-16

sfr = "SYSTICKRVR"            , "Memory", 0xE000E014,        4, base=16
sfr = "SYSTICKRVR.RELOAD"     , "Memory", 0xE000E014,        4, base=16,    bitRange=0-23

sfr = "SYSTICKCVR"            , "Memory", 0xE000E018,        4, base=16
sfr = "SYSTICKCVR.CURRENT"    , "Memory", 0xE000E018,        4, base=16,    bitRange=0-23

sfr = "SYSTICKCALVR"          , "Memory", 0xE000E01C,        4, base=16
sfr = "SYSTICKCALVR.TENMS"    , "Memory", 0xE000E01C,        4, base=16,    bitRange=0-23
sfr = "SYSTICKCALVR.SKEW"     , "Memory", 0xE000E01C,        4, base=16,    bitRange=30-30
sfr = "SYSTICKCALVR.NOREF"    , "Memory", 0xE000E01C,        4, base=16,    bitRange=31-31

sfr = "SETENA0"               , "Memory", 0xE000E100,        4, base=16
sfr = "SETENA0.SETENA0"       , "Memory", 0xE000E100,        4, base=16,    bitRange=0-0
sfr = "SETENA0.SETENA1"       , "Memory", 0xE000E100,        4, base=16,    bitRange=1-1
sfr = "SETENA0.SETENA2"       , "Memory", 0xE000E100,        4, base=16,    bitRange=2-2
sfr = "SETENA0.SETENA3"       , "Memory", 0xE000E100,        4, base=16,    bitRange=3-3
sfr = "SETENA0.SETENA4"       , "Memory", 0xE000E100,        4, base=16,    bitRange=4-4
sfr = "SETENA0.SETENA5"       , "Memory", 0xE000E100,        4, base=16,    bitRange=5-5
sfr = "SETENA0.SETENA6"       , "Memory", 0xE000E100,        4, base=16,    bitRange=6-6
sfr = "SETENA0.SETENA7"       , "Memory", 0xE000E100,        4, base=16,    bitRange=7-7
sfr = "SETENA0.SETENA8"       , "Memory", 0xE000E100,        4, base=16,    bitRange=8-8
sfr = "SETENA0.SETENA9"       , "Memory", 0xE000E100,        4, base=16,    bitRange=9-9
sfr = "SETENA0.SETENA10"      , "Memory", 0xE000E100,        4, base=16,    bitRange=10-10
sfr = "SETENA0.SETENA11"      , "Memory", 0xE000E100,        4, base=16,    bitRange=11-11
sfr = "SETENA0.SETENA12"      , "Memory", 0xE000E100,        4, base=16,    bitRange=12-12
sfr = "SETENA0.SETENA13"      , "Memory", 0xE000E100,        4, base=16,    bitRange=13-13
sfr = "SETENA0.SETENA14"      , "Memory", 0xE000E100,        4, base=16,    bitRange=14-14
sfr = "SETENA0.SETENA15"      , "Memory", 0xE000E100,        4, base=16,    bitRange=15-15
sfr = "SETENA0.SETENA16"      , "Memory", 0xE000E100,        4, base=16,    bitRange=16-16
sfr = "SETENA0.SETENA17"      , "Memory", 0xE000E100,        4, base=16,    bitRange=17-17
sfr = "SETENA0.SETENA18"      , "Memory", 0xE000E100,        4, base=16,    bitRange=18-18
sfr = "SETENA0.SETENA19"      , "Memory", 0xE000E100,        4, base=16,    bitRange=19-19
sfr = "SETENA0.SETENA20"      , "Memory", 0xE000E100,        4, base=16,    bitRange=20-20
sfr = "SETENA0.SETENA21"      , "Memory", 0xE000E100,        4, base=16,    bitRange=21-21
sfr = "SETENA0.SETENA22"      , "Memory", 0xE000E100,        4, base=16,    bitRange=22-22
sfr = "SETENA0.SETENA23"      , "Memory", 0xE000E100,        4, base=16,    bitRange=23-23
sfr = "SETENA0.SETENA24"      , "Memory", 0xE000E100,        4, base=16,    bitRange=24-24
sfr = "SETENA0.SETENA25"      , "Memory", 0xE000E100,        4, base=16,    bitRange=25-25
sfr = "SETENA0.SETENA26"      , "Memory", 0xE000E100,        4, base=16,    bitRange=26-26
sfr = "SETENA0.SETENA27"      , "Memory", 0xE000E100,        4, base=16,    bitRange=27-27
sfr = "SETENA0.SETENA28"      , "Memory", 0xE000E100,        4, base=16,    bitRange=28-28
sfr = "SETENA0.SETENA29"      , "Memory", 0xE000E100,        4, base=16,    bitRange=29-29
sfr = "SETENA0.SETENA30"      , "Memory", 0xE000E100,        4, base=16,    bitRange=30-30
sfr = "SETENA0.SETENA31"      , "Memory", 0xE000E100,        4, base=16,    bitRange=31-31

sfr = "SETENA1"               , "Memory", 0xE000E104,        4, base=16
sfr = "SETENA1.SETENA32"      , "Memory", 0xE000E104,        4, base=16,    bitRange=0-0
sfr = "SETENA1.SETENA33"      , "Memory", 0xE000E104,        4, base=16,    bitRange=1-1
sfr = "SETENA1.SETENA34"      , "Memory", 0xE000E104,        4, base=16,    bitRange=2-2
sfr = "SETENA1.SETENA35"      , "Memory", 0xE000E104,        4, base=16,    bitRange=3-3
sfr = "SETENA1.SETENA36"      , "Memory", 0xE000E104,        4, base=16,    bitRange=4-4
sfr = "SETENA1.SETENA37"      , "Memory", 0xE000E104,        4, base=16,    bitRange=5-5
sfr = "SETENA1.SETENA38"      , "Memory", 0xE000E104,        4, base=16,    bitRange=6-6
sfr = "SETENA1.SETENA39"      , "Memory", 0xE000E104,        4, base=16,    bitRange=7-7
sfr = "SETENA1.SETENA40"      , "Memory", 0xE000E104,        4, base=16,    bitRange=8-8
sfr = "SETENA1.SETENA41"      , "Memory", 0xE000E104,        4, base=16,    bitRange=9-9
sfr = "SETENA1.SETENA42"      , "Memory", 0xE000E104,        4, base=16,    bitRange=10-10
sfr = "SETENA1.SETENA43"      , "Memory", 0xE000E104,        4, base=16,    bitRange=11-11
sfr = "SETENA1.SETENA44"      , "Memory", 0xE000E104,        4, base=16,    bitRange=12-12
sfr = "SETENA1.SETENA45"      , "Memory", 0xE000E104,        4, base=16,    bitRange=13-13
sfr = "SETENA1.SETENA46"      , "Memory", 0xE000E104,        4, base=16,    bitRange=14-14
sfr = "SETENA1.SETENA47"      , "Memory", 0xE000E104,        4, base=16,    bitRange=15-15
sfr = "SETENA1.SETENA48"      , "Memory", 0xE000E104,        4, base=16,    bitRange=16-16
sfr = "SETENA1.SETENA49"      , "Memory", 0xE000E104,        4, base=16,    bitRange=17-17
sfr = "SETENA1.SETENA50"      , "Memory", 0xE000E104,        4, base=16,    bitRange=18-18
sfr = "SETENA1.SETENA51"      , "Memory", 0xE000E104,        4, base=16,    bitRange=19-19
sfr = "SETENA1.SETENA52"      , "Memory", 0xE000E104,        4, base=16,    bitRange=20-20
sfr = "SETENA1.SETENA53"      , "Memory", 0xE000E104,        4, base=16,    bitRange=21-21
sfr = "SETENA1.SETENA54"      , "Memory", 0xE000E104,        4, base=16,    bitRange=22-22
sfr = "SETENA1.SETENA55"      , "Memory", 0xE000E104,        4, base=16,    bitRange=23-23
sfr = "SETENA1.SETENA56"      , "Memory", 0xE000E104,        4, base=16,    bitRange=24-24
sfr = "SETENA1.SETENA57"      , "Memory", 0xE000E104,        4, base=16,    bitRange=25-25
sfr = "SETENA1.SETENA58"      , "Memory", 0xE000E104,        4, base=16,    bitRange=26-26
sfr = "SETENA1.SETENA59"      , "Memory", 0xE000E104,        4, base=16,    bitRange=27-27
sfr = "SETENA1.SETENA60"      , "Memory", 0xE000E104,        4, base=16,    bitRange=28-28
sfr = "SETENA1.SETENA61"      , "Memory", 0xE000E104,        4, base=16,    bitRange=29-29
sfr = "SETENA1.SETENA62"      , "Memory", 0xE000E104,        4, base=16,    bitRange=30-30
sfr = "SETENA1.SETENA63"      , "Memory", 0xE000E104,        4, base=16,    bitRange=31-31

sfr = "CLRENA0"               , "Memory", 0xE000E180,        4, base=16
sfr = "CLRENA0.CLRENA0"       , "Memory", 0xE000E180,        4, base=16,    bitRange=0-0
sfr = "CLRENA0.CLRENA1"       , "Memory", 0xE000E180,        4, base=16,    bitRange=1-1
sfr = "CLRENA0.CLRENA2"       , "Memory", 0xE000E180,        4, base=16,    bitRange=2-2
sfr = "CLRENA0.CLRENA3"       , "Memory", 0xE000E180,        4, base=16,    bitRange=3-3
sfr = "CLRENA0.CLRENA4"       , "Memory", 0xE000E180,        4, base=16,    bitRange=4-4
sfr = "CLRENA0.CLRENA5"       , "Memory", 0xE000E180,        4, base=16,    bitRange=5-5
sfr = "CLRENA0.CLRENA6"       , "Memory", 0xE000E180,        4, base=16,    bitRange=6-6
sfr = "CLRENA0.CLRENA7"       , "Memory", 0xE000E180,        4, base=16,    bitRange=7-7
sfr = "CLRENA0.CLRENA8"       , "Memory", 0xE000E180,        4, base=16,    bitRange=8-8
sfr = "CLRENA0.CLRENA9"       , "Memory", 0xE000E180,        4, base=16,    bitRange=9-9
sfr = "CLRENA0.CLRENA10"      , "Memory", 0xE000E180,        4, base=16,    bitRange=10-10
sfr = "CLRENA0.CLRENA11"      , "Memory", 0xE000E180,        4, base=16,    bitRange=11-11
sfr = "CLRENA0.CLRENA12"      , "Memory", 0xE000E180,        4, base=16,    bitRange=12-12
sfr = "CLRENA0.CLRENA13"      , "Memory", 0xE000E180,        4, base=16,    bitRange=13-13
sfr = "CLRENA0.CLRENA14"      , "Memory", 0xE000E180,        4, base=16,    bitRange=14-14
sfr = "CLRENA0.CLRENA15"      , "Memory", 0xE000E180,        4, base=16,    bitRange=15-15
sfr = "CLRENA0.CLRENA16"      , "Memory", 0xE000E180,        4, base=16,    bitRange=16-16
sfr = "CLRENA0.CLRENA17"      , "Memory", 0xE000E180,        4, base=16,    bitRange=17-17
sfr = "CLRENA0.CLRENA18"      , "Memory", 0xE000E180,        4, base=16,    bitRange=18-18
sfr = "CLRENA0.CLRENA19"      , "Memory", 0xE000E180,        4, base=16,    bitRange=19-19
sfr = "CLRENA0.CLRENA20"      , "Memory", 0xE000E180,        4, base=16,    bitRange=20-20
sfr = "CLRENA0.CLRENA21"      , "Memory", 0xE000E180,        4, base=16,    bitRange=21-21
sfr = "CLRENA0.CLRENA22"      , "Memory", 0xE000E180,        4, base=16,    bitRange=22-22
sfr = "CLRENA0.CLRENA23"      , "Memory", 0xE000E180,        4, base=16,    bitRange=23-23
sfr = "CLRENA0.CLRENA24"      , "Memory", 0xE000E180,        4, base=16,    bitRange=24-24
sfr = "CLRENA0.CLRENA25"      , "Memory", 0xE000E180,        4, base=16,    bitRange=25-25
sfr = "CLRENA0.CLRENA26"      , "Memory", 0xE000E180,        4, base=16,    bitRange=26-26
sfr = "CLRENA0.CLRENA27"      , "Memory", 0xE000E180,        4, base=16,    bitRange=27-27
sfr = "CLRENA0.CLRENA28"      , "Memory", 0xE000E180,        4, base=16,    bitRange=28-28
sfr = "CLRENA0.CLRENA29"      , "Memory", 0xE000E180,        4, base=16,    bitRange=29-29
sfr = "CLRENA0.CLRENA30"      , "Memory", 0xE000E180,        4, base=16,    bitRange=30-30
sfr = "CLRENA0.CLRENA31"      , "Memory", 0xE000E180,        4, base=16,    bitRange=31-31

sfr = "CLRENA1"               , "Memory", 0xE000E184,        4, base=16
sfr = "CLRENA1.CLRENA32"      , "Memory", 0xE000E184,        4, base=16,    bitRange=0-0
sfr = "CLRENA1.CLRENA33"      , "Memory", 0xE000E184,        4, base=16,    bitRange=1-1
sfr = "CLRENA1.CLRENA34"      , "Memory", 0xE000E184,        4, base=16,    bitRange=2-2
sfr = "CLRENA1.CLRENA35"      , "Memory", 0xE000E184,        4, base=16,    bitRange=3-3
sfr = "CLRENA1.CLRENA36"      , "Memory", 0xE000E184,        4, base=16,    bitRange=4-4
sfr = "CLRENA1.CLRENA37"      , "Memory", 0xE000E184,        4, base=16,    bitRange=5-5
sfr = "CLRENA1.CLRENA38"      , "Memory", 0xE000E184,        4, base=16,    bitRange=6-6
sfr = "CLRENA1.CLRENA39"      , "Memory", 0xE000E184,        4, base=16,    bitRange=7-7
sfr = "CLRENA1.CLRENA40"      , "Memory", 0xE000E184,        4, base=16,    bitRange=8-8
sfr = "CLRENA1.CLRENA41"      , "Memory", 0xE000E184,        4, base=16,    bitRange=9-9
sfr = "CLRENA1.CLRENA42"      , "Memory", 0xE000E184,        4, base=16,    bitRange=10-10
sfr = "CLRENA1.CLRENA43"      , "Memory", 0xE000E184,        4, base=16,    bitRange=11-11
sfr = "CLRENA1.CLRENA44"      , "Memory", 0xE000E184,        4, base=16,    bitRange=12-12
sfr = "CLRENA1.CLRENA45"      , "Memory", 0xE000E184,        4, base=16,    bitRange=13-13
sfr = "CLRENA1.CLRENA46"      , "Memory", 0xE000E184,        4, base=16,    bitRange=14-14
sfr = "CLRENA1.CLRENA47"      , "Memory", 0xE000E184,        4, base=16,    bitRange=15-15
sfr = "CLRENA1.CLRENA48"      , "Memory", 0xE000E184,        4, base=16,    bitRange=16-16
sfr = "CLRENA1.CLRENA49"      , "Memory", 0xE000E184,        4, base=16,    bitRange=17-17
sfr = "CLRENA1.CLRENA50"      , "Memory", 0xE000E184,        4, base=16,    bitRange=18-18
sfr = "CLRENA1.CLRENA51"      , "Memory", 0xE000E184,        4, base=16,    bitRange=19-19
sfr = "CLRENA1.CLRENA52"      , "Memory", 0xE000E184,        4, base=16,    bitRange=20-20
sfr = "CLRENA1.CLRENA53"      , "Memory", 0xE000E184,        4, base=16,    bitRange=21-21
sfr = "CLRENA1.CLRENA54"      , "Memory", 0xE000E184,        4, base=16,    bitRange=22-22
sfr = "CLRENA1.CLRENA55"      , "Memory", 0xE000E184,        4, base=16,    bitRange=23-23
sfr = "CLRENA1.CLRENA56"      , "Memory", 0xE000E184,        4, base=16,    bitRange=24-24
sfr = "CLRENA1.CLRENA57"      , "Memory", 0xE000E184,        4, base=16,    bitRange=25-25
sfr = "CLRENA1.CLRENA58"      , "Memory", 0xE000E184,        4, base=16,    bitRange=26-26
sfr = "CLRENA1.CLRENA59"      , "Memory", 0xE000E184,        4, base=16,    bitRange=27-27
sfr = "CLRENA1.CLRENA60"      , "Memory", 0xE000E184,        4, base=16,    bitRange=28-28
sfr = "CLRENA1.CLRENA61"      , "Memory", 0xE000E184,        4, base=16,    bitRange=29-29
sfr = "CLRENA1.CLRENA62"      , "Memory", 0xE000E184,        4, base=16,    bitRange=30-30
sfr = "CLRENA1.CLRENA63"      , "Memory", 0xE000E184,        4, base=16,    bitRange=31-31

sfr = "SETPEND0"              , "Memory", 0xE000E200,        4, base=16
sfr = "SETPEND0.SETPEND0"     , "Memory", 0xE000E200,        4, base=16,    bitRange=0-0
sfr = "SETPEND0.SETPEND1"     , "Memory", 0xE000E200,        4, base=16,    bitRange=1-1
sfr = "SETPEND0.SETPEND2"     , "Memory", 0xE000E200,        4, base=16,    bitRange=2-2
sfr = "SETPEND0.SETPEND3"     , "Memory", 0xE000E200,        4, base=16,    bitRange=3-3
sfr = "SETPEND0.SETPEND4"     , "Memory", 0xE000E200,        4, base=16,    bitRange=4-4
sfr = "SETPEND0.SETPEND5"     , "Memory", 0xE000E200,        4, base=16,    bitRange=5-5
sfr = "SETPEND0.SETPEND6"     , "Memory", 0xE000E200,        4, base=16,    bitRange=6-6
sfr = "SETPEND0.SETPEND7"     , "Memory", 0xE000E200,        4, base=16,    bitRange=7-7
sfr = "SETPEND0.SETPEND8"     , "Memory", 0xE000E200,        4, base=16,    bitRange=8-8
sfr = "SETPEND0.SETPEND9"     , "Memory", 0xE000E200,        4, base=16,    bitRange=9-9
sfr = "SETPEND0.SETPEND10"    , "Memory", 0xE000E200,        4, base=16,    bitRange=10-10
sfr = "SETPEND0.SETPEND11"    , "Memory", 0xE000E200,        4, base=16,    bitRange=11-11
sfr = "SETPEND0.SETPEND12"    , "Memory", 0xE000E200,        4, base=16,    bitRange=12-12
sfr = "SETPEND0.SETPEND13"    , "Memory", 0xE000E200,        4, base=16,    bitRange=13-13
sfr = "SETPEND0.SETPEND14"    , "Memory", 0xE000E200,        4, base=16,    bitRange=14-14
sfr = "SETPEND0.SETPEND15"    , "Memory", 0xE000E200,        4, base=16,    bitRange=15-15
sfr = "SETPEND0.SETPEND16"    , "Memory", 0xE000E200,        4, base=16,    bitRange=16-16
sfr = "SETPEND0.SETPEND17"    , "Memory", 0xE000E200,        4, base=16,    bitRange=17-17
sfr = "SETPEND0.SETPEND18"    , "Memory", 0xE000E200,        4, base=16,    bitRange=18-18
sfr = "SETPEND0.SETPEND19"    , "Memory", 0xE000E200,        4, base=16,    bitRange=19-19
sfr = "SETPEND0.SETPEND20"    , "Memory", 0xE000E200,        4, base=16,    bitRange=20-20
sfr = "SETPEND0.SETPEND21"    , "Memory", 0xE000E200,        4, base=16,    bitRange=21-21
sfr = "SETPEND0.SETPEND22"    , "Memory", 0xE000E200,        4, base=16,    bitRange=22-22
sfr = "SETPEND0.SETPEND23"    , "Memory", 0xE000E200,        4, base=16,    bitRange=23-23
sfr = "SETPEND0.SETPEND24"    , "Memory", 0xE000E200,        4, base=16,    bitRange=24-24
sfr = "SETPEND0.SETPEND25"    , "Memory", 0xE000E200,        4, base=16,    bitRange=25-25
sfr = "SETPEND0.SETPEND26"    , "Memory", 0xE000E200,        4, base=16,    bitRange=26-26
sfr = "SETPEND0.SETPEND27"    , "Memory", 0xE000E200,        4, base=16,    bitRange=27-27
sfr = "SETPEND0.SETPEND28"    , "Memory", 0xE000E200,        4, base=16,    bitRange=28-28
sfr = "SETPEND0.SETPEND29"    , "Memory", 0xE000E200,        4, base=16,    bitRange=29-29
sfr = "SETPEND0.SETPEND30"    , "Memory", 0xE000E200,        4, base=16,    bitRange=30-30
sfr = "SETPEND0.SETPEND31"    , "Memory", 0xE000E200,        4, base=16,    bitRange=31-31

sfr = "SETPEND1"              , "Memory", 0xE000E204,        4, base=16
sfr = "SETPEND1.SETPEND32"    , "Memory", 0xE000E204,        4, base=16,    bitRange=0-0
sfr = "SETPEND1.SETPEND33"    , "Memory", 0xE000E204,        4, base=16,    bitRange=1-1
sfr = "SETPEND1.SETPEND34"    , "Memory", 0xE000E204,        4, base=16,    bitRange=2-2
sfr = "SETPEND1.SETPEND35"    , "Memory", 0xE000E204,        4, base=16,    bitRange=3-3
sfr = "SETPEND1.SETPEND36"    , "Memory", 0xE000E204,        4, base=16,    bitRange=4-4
sfr = "SETPEND1.SETPEND37"    , "Memory", 0xE000E204,        4, base=16,    bitRange=5-5
sfr = "SETPEND1.SETPEND38"    , "Memory", 0xE000E204,        4, base=16,    bitRange=6-6
sfr = "SETPEND1.SETPEND39"    , "Memory", 0xE000E204,        4, base=16,    bitRange=7-7
sfr = "SETPEND1.SETPEND40"    , "Memory", 0xE000E204,        4, base=16,    bitRange=8-8
sfr = "SETPEND1.SETPEND41"    , "Memory", 0xE000E204,        4, base=16,    bitRange=9-9
sfr = "SETPEND1.SETPEND42"    , "Memory", 0xE000E204,        4, base=16,    bitRange=10-10
sfr = "SETPEND1.SETPEND43"    , "Memory", 0xE000E204,        4, base=16,    bitRange=11-11
sfr = "SETPEND1.SETPEND44"    , "Memory", 0xE000E204,        4, base=16,    bitRange=12-12
sfr = "SETPEND1.SETPEND45"    , "Memory", 0xE000E204,        4, base=16,    bitRange=13-13
sfr = "SETPEND1.SETPEND46"    , "Memory", 0xE000E204,        4, base=16,    bitRange=14-14
sfr = "SETPEND1.SETPEND47"    , "Memory", 0xE000E204,        4, base=16,    bitRange=15-15
sfr = "SETPEND1.SETPEND48"    , "Memory", 0xE000E204,        4, base=16,    bitRange=16-16
sfr = "SETPEND1.SETPEND49"    , "Memory", 0xE000E204,        4, base=16,    bitRange=17-17
sfr = "SETPEND1.SETPEND50"    , "Memory", 0xE000E204,        4, base=16,    bitRange=18-18
sfr = "SETPEND1.SETPEND51"    , "Memory", 0xE000E204,        4, base=16,    bitRange=19-19
sfr = "SETPEND1.SETPEND52"    , "Memory", 0xE000E204,        4, base=16,    bitRange=20-20
sfr = "SETPEND1.SETPEND53"    , "Memory", 0xE000E204,        4, base=16,    bitRange=21-21
sfr = "SETPEND1.SETPEND54"    , "Memory", 0xE000E204,        4, base=16,    bitRange=22-22
sfr = "SETPEND1.SETPEND55"    , "Memory", 0xE000E204,        4, base=16,    bitRange=23-23
sfr = "SETPEND1.SETPEND56"    , "Memory", 0xE000E204,        4, base=16,    bitRange=24-24
sfr = "SETPEND1.SETPEND57"    , "Memory", 0xE000E204,        4, base=16,    bitRange=25-25
sfr = "SETPEND1.SETPEND58"    , "Memory", 0xE000E204,        4, base=16,    bitRange=26-26
sfr = "SETPEND1.SETPEND59"    , "Memory", 0xE000E204,        4, base=16,    bitRange=27-27
sfr = "SETPEND1.SETPEND60"    , "Memory", 0xE000E204,        4, base=16,    bitRange=28-28
sfr = "SETPEND1.SETPEND61"    , "Memory", 0xE000E204,        4, base=16,    bitRange=29-29
sfr = "SETPEND1.SETPEND62"    , "Memory", 0xE000E204,        4, base=16,    bitRange=30-30
sfr = "SETPEND1.SETPEND63"    , "Memory", 0xE000E204,        4, base=16,    bitRange=31-31

sfr = "CLRPEND0"              , "Memory", 0xE000E280,        4, base=16
sfr = "CLRPEND0.CLRPEND0"     , "Memory", 0xE000E280,        4, base=16,    bitRange=0-0
sfr = "CLRPEND0.CLRPEND1"     , "Memory", 0xE000E280,        4, base=16,    bitRange=1-1
sfr = "CLRPEND0.CLRPEND2"     , "Memory", 0xE000E280,        4, base=16,    bitRange=2-2
sfr = "CLRPEND0.CLRPEND3"     , "Memory", 0xE000E280,        4, base=16,    bitRange=3-3
sfr = "CLRPEND0.CLRPEND4"     , "Memory", 0xE000E280,        4, base=16,    bitRange=4-4
sfr = "CLRPEND0.CLRPEND5"     , "Memory", 0xE000E280,        4, base=16,    bitRange=5-5
sfr = "CLRPEND0.CLRPEND6"     , "Memory", 0xE000E280,        4, base=16,    bitRange=6-6
sfr = "CLRPEND0.CLRPEND7"     , "Memory", 0xE000E280,        4, base=16,    bitRange=7-7
sfr = "CLRPEND0.CLRPEND8"     , "Memory", 0xE000E280,        4, base=16,    bitRange=8-8
sfr = "CLRPEND0.CLRPEND9"     , "Memory", 0xE000E280,        4, base=16,    bitRange=9-9
sfr = "CLRPEND0.CLRPEND10"    , "Memory", 0xE000E280,        4, base=16,    bitRange=10-10
sfr = "CLRPEND0.CLRPEND11"    , "Memory", 0xE000E280,        4, base=16,    bitRange=11-11
sfr = "CLRPEND0.CLRPEND12"    , "Memory", 0xE000E280,        4, base=16,    bitRange=12-12
sfr = "CLRPEND0.CLRPEND13"    , "Memory", 0xE000E280,        4, base=16,    bitRange=13-13
sfr = "CLRPEND0.CLRPEND14"    , "Memory", 0xE000E280,        4, base=16,    bitRange=14-14
sfr = "CLRPEND0.CLRPEND15"    , "Memory", 0xE000E280,        4, base=16,    bitRange=15-15
sfr = "CLRPEND0.CLRPEND16"    , "Memory", 0xE000E280,        4, base=16,    bitRange=16-16
sfr = "CLRPEND0.CLRPEND17"    , "Memory", 0xE000E280,        4, base=16,    bitRange=17-17
sfr = "CLRPEND0.CLRPEND18"    , "Memory", 0xE000E280,        4, base=16,    bitRange=18-18
sfr = "CLRPEND0.CLRPEND19"    , "Memory", 0xE000E280,        4, base=16,    bitRange=19-19
sfr = "CLRPEND0.CLRPEND20"    , "Memory", 0xE000E280,        4, base=16,    bitRange=20-20
sfr = "CLRPEND0.CLRPEND21"    , "Memory", 0xE000E280,        4, base=16,    bitRange=21-21
sfr = "CLRPEND0.CLRPEND22"    , "Memory", 0xE000E280,        4, base=16,    bitRange=22-22
sfr = "CLRPEND0.CLRPEND23"    , "Memory", 0xE000E280,        4, base=16,    bitRange=23-23
sfr = "CLRPEND0.CLRPEND24"    , "Memory", 0xE000E280,        4, base=16,    bitRange=24-24
sfr = "CLRPEND0.CLRPEND25"    , "Memory", 0xE000E280,        4, base=16,    bitRange=25-25
sfr = "CLRPEND0.CLRPEND26"    , "Memory", 0xE000E280,        4, base=16,    bitRange=26-26
sfr = "CLRPEND0.CLRPEND27"    , "Memory", 0xE000E280,        4, base=16,    bitRange=27-27
sfr = "CLRPEND0.CLRPEND28"    , "Memory", 0xE000E280,        4, base=16,    bitRange=28-28
sfr = "CLRPEND0.CLRPEND29"    , "Memory", 0xE000E280,        4, base=16,    bitRange=29-29
sfr = "CLRPEND0.CLRPEND30"    , "Memory", 0xE000E280,        4, base=16,    bitRange=30-30
sfr = "CLRPEND0.CLRPEND31"    , "Memory", 0xE000E280,        4, base=16,    bitRange=31-31

sfr = "CLRPEND1"              , "Memory", 0xE000E284,        4, base=16
sfr = "CLRPEND1.CLRPEND32"    , "Memory", 0xE000E284,        4, base=16,    bitRange=0-0
sfr = "CLRPEND1.CLRPEND33"    , "Memory", 0xE000E284,        4, base=16,    bitRange=1-1
sfr = "CLRPEND1.CLRPEND34"    , "Memory", 0xE000E284,        4, base=16,    bitRange=2-2
sfr = "CLRPEND1.CLRPEND35"    , "Memory", 0xE000E284,        4, base=16,    bitRange=3-3
sfr = "CLRPEND1.CLRPEND36"    , "Memory", 0xE000E284,        4, base=16,    bitRange=4-4
sfr = "CLRPEND1.CLRPEND37"    , "Memory", 0xE000E284,        4, base=16,    bitRange=5-5
sfr = "CLRPEND1.CLRPEND38"    , "Memory", 0xE000E284,        4, base=16,    bitRange=6-6
sfr = "CLRPEND1.CLRPEND39"    , "Memory", 0xE000E284,        4, base=16,    bitRange=7-7
sfr = "CLRPEND1.CLRPEND40"    , "Memory", 0xE000E284,        4, base=16,    bitRange=8-8
sfr = "CLRPEND1.CLRPEND41"    , "Memory", 0xE000E284,        4, base=16,    bitRange=9-9
sfr = "CLRPEND1.CLRPEND42"    , "Memory", 0xE000E284,        4, base=16,    bitRange=10-10
sfr = "CLRPEND1.CLRPEND43"    , "Memory", 0xE000E284,        4, base=16,    bitRange=11-11
sfr = "CLRPEND1.CLRPEND44"    , "Memory", 0xE000E284,        4, base=16,    bitRange=12-12
sfr = "CLRPEND1.CLRPEND45"    , "Memory", 0xE000E284,        4, base=16,    bitRange=13-13
sfr = "CLRPEND1.CLRPEND46"    , "Memory", 0xE000E284,        4, base=16,    bitRange=14-14
sfr = "CLRPEND1.CLRPEND47"    , "Memory", 0xE000E284,        4, base=16,    bitRange=15-15
sfr = "CLRPEND1.CLRPEND48"    , "Memory", 0xE000E284,        4, base=16,    bitRange=16-16
sfr = "CLRPEND1.CLRPEND49"    , "Memory", 0xE000E284,        4, base=16,    bitRange=17-17
sfr = "CLRPEND1.CLRPEND50"    , "Memory", 0xE000E284,        4, base=16,    bitRange=18-18
sfr = "CLRPEND1.CLRPEND51"    , "Memory", 0xE000E284,        4, base=16,    bitRange=19-19
sfr = "CLRPEND1.CLRPEND52"    , "Memory", 0xE000E284,        4, base=16,    bitRange=20-20
sfr = "CLRPEND1.CLRPEND53"    , "Memory", 0xE000E284,        4, base=16,    bitRange=21-21
sfr = "CLRPEND1.CLRPEND54"    , "Memory", 0xE000E284,        4, base=16,    bitRange=22-22
sfr = "CLRPEND1.CLRPEND55"    , "Memory", 0xE000E284,        4, base=16,    bitRange=23-23
sfr = "CLRPEND1.CLRPEND56"    , "Memory", 0xE000E284,        4, base=16,    bitRange=24-24
sfr = "CLRPEND1.CLRPEND57"    , "Memory", 0xE000E284,        4, base=16,    bitRange=25-25
sfr = "CLRPEND1.CLRPEND58"    , "Memory", 0xE000E284,        4, base=16,    bitRange=26-26
sfr = "CLRPEND1.CLRPEND59"    , "Memory", 0xE000E284,        4, base=16,    bitRange=27-27
sfr = "CLRPEND1.CLRPEND60"    , "Memory", 0xE000E284,        4, base=16,    bitRange=28-28
sfr = "CLRPEND1.CLRPEND61"    , "Memory", 0xE000E284,        4, base=16,    bitRange=29-29
sfr = "CLRPEND1.CLRPEND62"    , "Memory", 0xE000E284,        4, base=16,    bitRange=30-30
sfr = "CLRPEND1.CLRPEND63"    , "Memory", 0xE000E284,        4, base=16,    bitRange=31-31

sfr = "ACTIVE0"               , "Memory", 0xE000E300,        4, base=16
sfr = "ACTIVE0.ACTIVE0"       , "Memory", 0xE000E300,        4, base=16,    bitRange=0-0
sfr = "ACTIVE0.ACTIVE1"       , "Memory", 0xE000E300,        4, base=16,    bitRange=1-1
sfr = "ACTIVE0.ACTIVE2"       , "Memory", 0xE000E300,        4, base=16,    bitRange=2-2
sfr = "ACTIVE0.ACTIVE3"       , "Memory", 0xE000E300,        4, base=16,    bitRange=3-3
sfr = "ACTIVE0.ACTIVE4"       , "Memory", 0xE000E300,        4, base=16,    bitRange=4-4
sfr = "ACTIVE0.ACTIVE5"       , "Memory", 0xE000E300,        4, base=16,    bitRange=5-5
sfr = "ACTIVE0.ACTIVE6"       , "Memory", 0xE000E300,        4, base=16,    bitRange=6-6
sfr = "ACTIVE0.ACTIVE7"       , "Memory", 0xE000E300,        4, base=16,    bitRange=7-7
sfr = "ACTIVE0.ACTIVE8"       , "Memory", 0xE000E300,        4, base=16,    bitRange=8-8
sfr = "ACTIVE0.ACTIVE9"       , "Memory", 0xE000E300,        4, base=16,    bitRange=9-9
sfr = "ACTIVE0.ACTIVE10"      , "Memory", 0xE000E300,        4, base=16,    bitRange=10-10
sfr = "ACTIVE0.ACTIVE11"      , "Memory", 0xE000E300,        4, base=16,    bitRange=11-11
sfr = "ACTIVE0.ACTIVE12"      , "Memory", 0xE000E300,        4, base=16,    bitRange=12-12
sfr = "ACTIVE0.ACTIVE13"      , "Memory", 0xE000E300,        4, base=16,    bitRange=13-13
sfr = "ACTIVE0.ACTIVE14"      , "Memory", 0xE000E300,        4, base=16,    bitRange=14-14
sfr = "ACTIVE0.ACTIVE15"      , "Memory", 0xE000E300,        4, base=16,    bitRange=15-15
sfr = "ACTIVE0.ACTIVE16"      , "Memory", 0xE000E300,        4, base=16,    bitRange=16-16
sfr = "ACTIVE0.ACTIVE17"      , "Memory", 0xE000E300,        4, base=16,    bitRange=17-17
sfr = "ACTIVE0.ACTIVE18"      , "Memory", 0xE000E300,        4, base=16,    bitRange=18-18
sfr = "ACTIVE0.ACTIVE19"      , "Memory", 0xE000E300,        4, base=16,    bitRange=19-19
sfr = "ACTIVE0.ACTIVE20"      , "Memory", 0xE000E300,        4, base=16,    bitRange=20-20
sfr = "ACTIVE0.ACTIVE21"      , "Memory", 0xE000E300,        4, base=16,    bitRange=21-21
sfr = "ACTIVE0.ACTIVE22"      , "Memory", 0xE000E300,        4, base=16,    bitRange=22-22
sfr = "ACTIVE0.ACTIVE23"      , "Memory", 0xE000E300,        4, base=16,    bitRange=23-23
sfr = "ACTIVE0.ACTIVE24"      , "Memory", 0xE000E300,        4, base=16,    bitRange=24-24
sfr = "ACTIVE0.ACTIVE25"      , "Memory", 0xE000E300,        4, base=16,    bitRange=25-25
sfr = "ACTIVE0.ACTIVE26"      , "Memory", 0xE000E300,        4, base=16,    bitRange=26-26
sfr = "ACTIVE0.ACTIVE27"      , "Memory", 0xE000E300,        4, base=16,    bitRange=27-27
sfr = "ACTIVE0.ACTIVE28"      , "Memory", 0xE000E300,        4, base=16,    bitRange=28-28
sfr = "ACTIVE0.ACTIVE29"      , "Memory", 0xE000E300,        4, base=16,    bitRange=29-29
sfr = "ACTIVE0.ACTIVE30"      , "Memory", 0xE000E300,        4, base=16,    bitRange=30-30
sfr = "ACTIVE0.ACTIVE31"      , "Memory", 0xE000E300,        4, base=16,    bitRange=31-31

sfr = "ACTIVE1"               , "Memory", 0xE000E304,        4, base=16
sfr = "ACTIVE1.ACTIVE32"      , "Memory", 0xE000E304,        4, base=16,    bitRange=0-0
sfr = "ACTIVE1.ACTIVE33"      , "Memory", 0xE000E304,        4, base=16,    bitRange=1-1
sfr = "ACTIVE1.ACTIVE34"      , "Memory", 0xE000E304,        4, base=16,    bitRange=2-2
sfr = "ACTIVE1.ACTIVE35"      , "Memory", 0xE000E304,        4, base=16,    bitRange=3-3
sfr = "ACTIVE1.ACTIVE36"      , "Memory", 0xE000E304,        4, base=16,    bitRange=4-4
sfr = "ACTIVE1.ACTIVE37"      , "Memory", 0xE000E304,        4, base=16,    bitRange=5-5
sfr = "ACTIVE1.ACTIVE38"      , "Memory", 0xE000E304,        4, base=16,    bitRange=6-6
sfr = "ACTIVE1.ACTIVE39"      , "Memory", 0xE000E304,        4, base=16,    bitRange=7-7
sfr = "ACTIVE1.ACTIVE40"      , "Memory", 0xE000E304,        4, base=16,    bitRange=8-8
sfr = "ACTIVE1.ACTIVE41"      , "Memory", 0xE000E304,        4, base=16,    bitRange=9-9
sfr = "ACTIVE1.ACTIVE42"      , "Memory", 0xE000E304,        4, base=16,    bitRange=10-10
sfr = "ACTIVE1.ACTIVE43"      , "Memory", 0xE000E304,        4, base=16,    bitRange=11-11
sfr = "ACTIVE1.ACTIVE44"      , "Memory", 0xE000E304,        4, base=16,    bitRange=12-12
sfr = "ACTIVE1.ACTIVE45"      , "Memory", 0xE000E304,        4, base=16,    bitRange=13-13
sfr = "ACTIVE1.ACTIVE46"      , "Memory", 0xE000E304,        4, base=16,    bitRange=14-14
sfr = "ACTIVE1.ACTIVE47"      , "Memory", 0xE000E304,        4, base=16,    bitRange=15-15
sfr = "ACTIVE1.ACTIVE48"      , "Memory", 0xE000E304,        4, base=16,    bitRange=16-16
sfr = "ACTIVE1.ACTIVE49"      , "Memory", 0xE000E304,        4, base=16,    bitRange=17-17
sfr = "ACTIVE1.ACTIVE50"      , "Memory", 0xE000E304,        4, base=16,    bitRange=18-18
sfr = "ACTIVE1.ACTIVE51"      , "Memory", 0xE000E304,        4, base=16,    bitRange=19-19
sfr = "ACTIVE1.ACTIVE52"      , "Memory", 0xE000E304,        4, base=16,    bitRange=20-20
sfr = "ACTIVE1.ACTIVE53"      , "Memory", 0xE000E304,        4, base=16,    bitRange=21-21
sfr = "ACTIVE1.ACTIVE54"      , "Memory", 0xE000E304,        4, base=16,    bitRange=22-22
sfr = "ACTIVE1.ACTIVE55"      , "Memory", 0xE000E304,        4, base=16,    bitRange=23-23
sfr = "ACTIVE1.ACTIVE56"      , "Memory", 0xE000E304,        4, base=16,    bitRange=24-24
sfr = "ACTIVE1.ACTIVE57"      , "Memory", 0xE000E304,        4, base=16,    bitRange=25-25
sfr = "ACTIVE1.ACTIVE58"      , "Memory", 0xE000E304,        4, base=16,    bitRange=26-26
sfr = "ACTIVE1.ACTIVE59"      , "Memory", 0xE000E304,        4, base=16,    bitRange=27-27
sfr = "ACTIVE1.ACTIVE60"      , "Memory", 0xE000E304,        4, base=16,    bitRange=28-28
sfr = "ACTIVE1.ACTIVE61"      , "Memory", 0xE000E304,        4, base=16,    bitRange=29-29
sfr = "ACTIVE1.ACTIVE62"      , "Memory", 0xE000E304,        4, base=16,    bitRange=30-30
sfr = "ACTIVE1.ACTIVE63"      , "Memory", 0xE000E304,        4, base=16,    bitRange=31-31

;;
;; Group info for SFR Window.
;;
[SfrGroupInfo]

group = "UART_0","RBR","THR","DLR","DMR","IER","IIR","LCR","MCR","LSR","MSR","SR"
group = "SPI_0","SPI0_CONTROL","SPI0_TXRXDF_SIZE","SPI0_STATUS", "SPI0_INT_CLR","SPI0_RX_DATA","SPI0_TX_DATA","SPI0_CLK_GEN","SPI0_SLAVE_SELECT","SPI0_MIS","SPI0_RIS"
group = "I2C_0","CTRL","STAT","DATA","ADDR","SMBUS","FREQ","GLITCHREG"
group = "Ethernet MAC","CSR0","CSR1","CSR2","CSR3","CSR4","CSR5","CSR6","CSR7","CSR8","CSR9","CSR11"
;group = "Peripheral DMA","PDMA"
group = "Peripheral DMA","RATIO_HIGH_LOW","BUFFER_STATUS","CHAN_0_CTRL","CHAN_0_STATUS","CHAN_0_BUFF_A_SRC","CHAN_0_BUFF_A_DST","CHAN_0_BUFF_A_COUNT","CHAN_0_BUFF_B_SRC","CHAN_0_BUFF_B_DST","CHAN_0_BUFF_B_COUNT","CHAN_1_CTRL","CHAN_1_STATUS","CHAN_1_BUFF_A_SRC","CHAN_1_BUFF_A_DST","CHAN_1_BUFF_A_COUNT","CHAN_1_BUFF_B_SRC","CHAN_1_BUFF_B_DST","CHAN_1_BUFF_B_COUNT","CHAN_2_CTRL","CHAN_2_STATUS","CHAN_2_BUFF_A_SRC","CHAN_2_BUFF_A_DST","CHAN_2_BUFF_A_COUNT","CHAN_2_BUFF_B_SRC","CHAN_2_BUFF_B_DST","CHAN_2_BUFF_B_COUNT","CHAN_3_CTRL","CHAN_3_STATUS","CHAN_3_BUFF_A_SRC","CHAN_3_BUFF_A_DST","CHAN_3_BUFF_A_COUNT","CHAN_3_BUFF_B_SRC","CHAN_3_BUFF_B_DST","CHAN_3_BUFF_B_COUNT","CHAN_4_CTRL","CHAN_4_STATUS","CHAN_4_BUFF_A_SRC","CHAN_4_BUFF_A_DST","CHAN_4_BUFF_A_COUNT","CHAN_4_BUFF_B_SRC","CHAN_4_BUFF_B_DST","CHAN_4_BUFF_B_COUNT","CHAN_5_CTRL","CHAN_5_STATUS","CHAN_5_BUFF_A_SRC","CHAN_5_BUFF_A_DST","CHAN_5_BUFF_A_COUNT","CHAN_5_BUFF_B_SRC","CHAN_5_BUFF_B_DST","CHAN_5_BUFF_B_COUNT","CHAN_6_CTRL","CHAN_6_STATUS","CHAN_6_BUFF_A_SRC","CHAN_6_BUFF_A_DST","CHAN_6_BUFF_A_COUNT","CHAN_6_BUFF_B_SRC","CHAN_6_BUFF_B_DST","CHAN_6_BUFF_B_COUNT","CHAN_7_CTRL","CHAN_7_STATUS","CHAN_7_BUFF_A_SRC","CHAN_7_BUFF_A_DST","CHAN_7_BUFF_A_COUNT","CHAN_7_BUFF_B_SRC","CHAN_7_BUFF_B_DST","CHAN_7_BUFF_B_COUNT"
group = "Timer","TIM1_BGLOADVAL","TIM1_CTRL","TIM1_LOADVAL","TIM1_MIS","TIM1_RIS","TIM1_VALUE","TIM2_BGLOADVAL","TIM2_CTRL","TIM2_LOADVAL","TIM2_MIS","TIM2_RIS","TIM2_VALUE","TIM64BGLOADVALUEL","TIM64BGLOADVALUEU","TIM64LOADVALUEL","TIM64LOADVALUEU","TIM64VALUEL","TIM64VALUEU","TIM64_CTRL","TIM64_MIS","TIM64_MODE","TIM64_RIS"
group = "Watchdog","WATCHDOG"
group = "H2F Interrupt Controller","H2F"
group = "UART_1","RBR1","THR1","DLR1","DMR1","IER1","IIR1","LCR1","MCR1","LSR1","MSR1","SR1"
group = "SPI_1","SPI1_CONTROL","SPI1_TXRXDF_SIZE","SPI1_STATUS", "SPI1_INT_CLR","SPI1_RX_DATA","SPI1_TX_DATA","SPI1_CLK_GEN","SPI1_SLAVE_SELECT","SPI1_MIS","SPI1_RIS"
group = "I2C_1","CTRL1","STAT1","DATA1","ADDR1","SMBUS1","FREQ1","GLITCHREG1"
group = "GPIO","CONFIG_01","CONFIG_02","CONFIG_03","CONFIG_04","CONFIG_05","CONFIG_06","CONFIG_07","CONFIG_08","CONFIG_09","CONFIG_10","CONFIG_11","CONFIG_12","CONFIG_13","CONFIG_14","CONFIG_15","CONFIG_16","CONFIG_17","CONFIG_18","CONFIG_19","CONFIG_20","CONFIG_21","CONFIG_22","CONFIG_23","CONFIG_24","CONFIG_25","CONFIG_26","CONFIG_27","CONFIG_28","CONFIG_29","CONFIG_30","CONFIG_31","CONFIG_32","INTR","GPIN","GPOUT"
group = "RTC","RTC"
group = "FROM","FROM"
group = "IAP Controller","IAP_DR","IAP_DR2","IAP_DR26","IAP_DR3","IAP_DR32","IAP_DR5","IAP_DR_LENGTH","IAP_IR","IAP_STATUS","IAP_TAP_CONTROL","IAP_TAP_NEW_STATE"
group = "Analog Conversion Engine","NOP","SSE_TS_CTRL","ADC_SYNC_CONV","ANA_COMM_CTRL","DAC_SYNC_CTRL","PDMA_REQUEST","PC0_LO","PC0_HI","PC0_CTRL","PC0_DLY","PC0_DLY","ADC0_STC","ADC0_TVC","ADC0_MISC_CTRL","DAC0_CTRL","DAC0_BYTE0","DAC0_BYTE1","DAC0_BYTE2","LC0","LC0_JMP_LO","LC0_JMP_HI","PC0_FLAGS","PC1_LO","PC1_HI","PC1_CTRL","PC1_DLY","ADC1_CONV_CTRL","ADC1_STC","ADC1_TVC","ADC1_MISC_CTRL","DAC1_CTRL","DAC1_BYTE0","DAC1_BYTE1","DAC1_BYTE2","LC1","LC1_JMP_LO","LC1_JMP_HI","PC1_FLAGS","PC2_LO","PC2_HI","PC2_CTRL","PC2_DLY","ADC2_CONV_CTRL","ADC2_STC","ADC2_TVC","ADC2_MISC_CTRL","DAC2_CTRL","DAC2_BYTE0","DAC2_BYTE1","DAC2_BYTE2","LC2","LC2_JMP_LO","LC2_JMP_HI","PC2_FLAGS","SSE_RAM_LO_IDATA","SSE_RAM_HI_IDATA","ACB_DATA_FIRST","ACB_DATA_LAST","SSE_PC0","SSE_PC1","SSE_PC2","SSE_DAC0_BYTES01","SSE_DAC1_BYTES01","SSE_DAC2_BYTES01","SSE_ADC0_RESULTS","SSE_ADC1_RESULTS","SSE_ADC2_RESULTS","SSE_PDMA_DATAIN","SSE_RAM_DATA_FIRST","SSE_RAM_DATA_LAST","ADC0_STATUS","ADC1_STATUS","ADC2_STATUS","COMPARATOR_STATUS","SSE_IRQ_EN","SSE_IRQ","SSE_IRQ_CLR","COMP_IRQ_EN","COMP_IRQ","COMP_IRQ_CLR","PPE_FIFO_IRQ_EN","PPE_FIFO_IRQ","PPE_FIFO_IRQ_CLR","PPE_FLAGS0_IRQ_EN","PPE_FLAGS0_IRQ","PPE_FLAGS0_IRQ_CLR","PPE_FLAGS1_IRQ_EN","PPE_FLAGS1_IRQ","PPE_FLAGS1_IRQ_CLR","PPE_FLAGS2_IRQ_EN","PPE_FLAGS2_IRQ","PPE_FLAGS2_IRQ_CLR","PPE_FLAGS3_IRQ_EN","PPE_FLAGS3_IRQ","PPE_FLAGS3_IRQ_CLR","PPE_SFFLAGS_IRQ_EN","PPE_SFFLAGS_IRQ","PPE_SFFLAGS_IRQ_CLR","FPGA_FLAGS_SEL","PPE_PDMA_CTRL","PDMA_STATUS","PPE_PDMA_DATAOUT","PPE_NOP","PPE_CTRL","PPE_PC_ETC","PPE_SF","PPE_SCRATCH","ALU_CTRL","ALU_STATUS","ALU_A","ALU_B","ALU_C","ALU_D","ALU_E","PPE_FPTR","PPE_FLAGS0","PPE_FLAGS1","PPE_FLAGS2","PPE_FLAGS3","PPE_SFFLAGS","ADC0_FIFO_CTRL","ADC0_FIFO_STATUS","ADC0_FIFO_DATA","ADC1_FIFO_CTRL","ADC1_FIFO_STATUS","ADC1_FIFO_DATA","ADC2_FIFO_CTRL","ADC2_FIFO_STATUS","ADC2_FIFO_DATA","ADC0_FIFO_DATA_PEEK","ADC0_FIFO_DATA0","ADC0_FIFO_DATA1","ADC0_FIFO_DATA2","ADC0_FIFO_DATA3","ADC1_FIFO_DATA_PEEK","ADC1_FIFO_DATA0","ADC1_FIFO_DATA1","ADC1_FIFO_DATA2","ADC1_FIFO_DATA3","ADC2_FIFO_DATA_PEEK","ADC2_FIFO_DATA0","ADC2_FIFO_DATA1","ADC2_FIFO_DATA2","ADC2_FIFO_DATA3","PPE_RAM_DATA_FIRST","PPE_RAM_DATA_LAST"
group = "System Register","ESRAM_CONFIG","ENVM_CONFIG","ENVM_REMAP_BASE","ENVM_FAB_REMAP","FAB_PROT_SIZE","FAB_PROT_BASE","MATRIX_CONFIG","DSS_STATUS","CLR_DSS_STATUS","FROM_CONFIG","IAP_CONFIG","SOFT_INTERRUPT","SOFT_RESET","DEVICE_STATUS","SYSTICK_CONFIG","EM_MUX_CONFIG","EM_CONFIG_0","EM_CONFIG_1","CLK_CTRL","CCC_DIV_CONFIG","CCC_MUX_CONFIG","CCC_PLL_CONFIG","CCC_DLY_CONFIG","CCC_STATUS","OSC_CTRL","VTG_CTRL","SPARE","FAB_IF","APB_EXTN","IO_BANK_CONFIG","GPIN_SRC_SEL","LOOPBACK_CTRL","TEST_STATUS","RED_REP_ADDR0""RED_REP_LOW_LOCS0","RED_REP_HIGH_LOCS0","RED_REP_ADDR1","RED_REP_LOW_LOCS1","RED_REP_HIGH_LOCS1","FPGA_CTRL","IOMUXCELL_0_CONFIG","IOMUXCELL_1_CONFIG","IOMUXCELL_2_CONFIG","IOMUXCELL_3_CONFIG","IOMUXCELL_4_CONFIG","IOMUXCELL_5_CONFIG","IOMUXCELL_6_CONFIG","IOMUXCELL_7_CONFIG","IOMUXCELL_8_CONFIG","IOMUXCELL_9_CONFIG","IOMUXCELL_10_CONFIG","IOMUXCELL_11_CONFIG","IOMUXCELL_12_CONFIG","IOMUXCELL_13_CONFIG","IOMUXCELL_14_CONFIG","IOMUXCELL_15_CONFIG","IOMUXCELL_16_CONFIG","IOMUXCELL_17_CONFIG","IOMUXCELL_18_CONFIG","IOMUXCELL_19_CONFIG","IOMUXCELL_20_CONFIG","IOMUXCELL_21_CONFIG","IOMUXCELL_22_CONFIG","IOMUXCELL_23_CONFIG","IOMUXCELL_24_CONFIG","IOMUXCELL_25_CONFIG","IOMUXCELL_26_CONFIG","IOMUXCELL_27_CONFIG","IOMUXCELL_28_CONFIG","IOMUXCELL_29_CONFIG","IOMUXCELL_30_CONFIG","IOMUXCELL_31_CONFIG","IOMUXCELL_32_CONFIG","IOMUXCELL_33_CONFIG","IOMUXCELL_34_CONFIG","IOMUXCELL_35_CONFIG","IOMUXCELL_36_CONFIG","IOMUXCELL_37_CONFIG","IOMUXCELL_38_CONFIG","IOMUXCELL_39_CONFIG","IOMUXCELL_40_CONFIG","IOMUXCELL_41_CONFIG","IOMUXCELL_42_CONFIG","IOMUXCELL_43_CONFIG","IOMUXCELL_44_CONFIG","IOMUXCELL_45_CONFIG","IOMUXCELL_46_CONFIG","IOMUXCELL_47_CONFIG","IOMUXCELL_48_CONFIG","IOMUXCELL_49_CONFIG","IOMUXCELL_50_CONFIG","IOMUXCELL_51_CONFIG","IOMUXCELL_52_CONFIG","IOMUXCELL_53_CONFIG","IOMUXCELL_54_CONFIG","IOMUXCELL_55_CONFIG","IOMUXCELL_56_CONFIG","IOMUXCELL_57_CONFIG","IOMUXCELL_58_CONFIG","IOMUXCELL_59_CONFIG","IOMUXCELL_60_CONFIG","IOMUXCELL_61_CONFIG","IOMUXCELL_62_CONFIG","IOMUXCELL_63_CONFIG","IOMUXCELL_64_CONFIG","IOMUXCELL_65_CONFIG","IOMUXCELL_66_CONFIG","IOMUXCELL_67_CONFIG","IOMUXCELL_68_CONFIG","IOMUXCELL_69_CONFIG","IOMUXCELL_70_CONFIG","IOMUXCELL_71_CONFIG","IOMUXCELL_72_CONFIG","IOMUXCELL_73_CONFIG","IOMUXCELL_74_CONFIG","IOMUXCELL_75_CONFIG","IOMUXCELL_76_CONFIG","IOMUXCELL_77_CONFIG","IOMUXCELL_78_CONFIG","IOMUXCELL_79_CONFIG","IOMUXCELL_80_CONFIG","IOMUXCELL_81_CONFIG","IOMUXCELL_82_CONFIG"
group = "NVIC","NVIC","SYSTICKCSR","SYSTICKRVR","SYSTICKCVR","SYSTICKCALVR","SETENA0","SETENA1","CLRENA0","CLRENA1","SETPEND0","SETPEND1","CLRPEND0","CLRPEND1","ACTIVE0","ACTIVE1"
