# Actel Physical design constraints file
# Generated file

# Version: 10.1 SP1 10.1.1.6
# Family: SmartFusion , Die: A2F500M3G , Package: 484 FBGA
# Date generated: Tue Nov 20 11:06:42 2012 


# 
# IO banks setting
# 


# 
# User Groups
# 

define_group -name UART_0

define_group -name UART_0_PADs


# 
# I/O constraints
# 

set_io MSS_RESET_N        \
    -pinname R1           \
    -fixed yes            \
    -iostd LVTTL          \
    -RES_PULL None        \
    -SCHMITT_TRIGGER Off  \
    -DIRECTION Input


# User Group UART_0_PADs

set_io UART_0_RXD            \
    -pinname U18             \
    -fixed yes               \
    -iostd LVTTL             \
    -RES_PULL None           \
    -SCHMITT_TRIGGER Off     \
    -GROUP_NAME UART_0_PADs  \
    -DIRECTION Input


set_io UART_0_TXD            \
    -pinname Y22             \
    -fixed yes               \
    -iostd LVTTL             \
    -OUT_LOAD 35             \
    -RES_PULL None           \
    -SKEW Off                \
    -SLEW High               \
    -GROUP_NAME UART_0_PADs  \
    -DIRECTION Output



#
# Non IO constraints
#


#
# Old IO constraints, commented out for reference
#

# set_io MSS_RESET_N -pinname R1 -fixed yes -iostd LVTTL -RES_PULL None -SCHMITT_TRIGGER Off -DIRECTION Input 
# set_io UART_0_RXD -pinname U18 -fixed yes -iostd LVTTL -RES_PULL None -SCHMITT_TRIGGER Off -GROUP_NAME UART_0_PADs -DIRECTION Input 
# set_io UART_0_TXD -pinname Y22 -fixed yes -iostd LVTTL -OUT_LOAD 35 -RES_PULL None -SKEW Off -SLEW High -GROUP_NAME UART_0_PADs -DIRECTION Output 
