<?xml version="1.0" encoding="UTF-8" standalone="no" ?><Component xmlns="http://actel.com/sweng/afi"><name>DESIGN_FIRMWARE</name><vendor/><library/><version/><fileSets/><hwModel><views/></hwModel><category>AppFirmwareDesign</category><function>AppFirmwareDesign</function><variation/><vendor/><version/><vendorExtension><type>AppFirmwareDesign</type></vendorExtension><vendorExtension><state value="SAVED"/></vendorExtension><vendorExtensions><dependentModules><module id_library="Firmware" id_name="HAL" id_vendor="Actel" id_version="2.2.102" module_class="FirmWareModule" name="HAL" state="GOOD" type="3"/><module id_library="Firmware" id_name="MSS_GPIO_Driver" id_vendor="Actel" id_version="2.0.105" module_class="FirmWareModule" name="MSS_GPIO_Driver" state="GOOD" type="3"/><module id_library="Firmware" id_name="MSS_IAP_Driver" id_vendor="Actel" id_version="2.2.101" module_class="FirmWareModule" name="MSS_IAP_Driver" state="GOOD" type="3"/><module id_library="Firmware" id_name="MSS_NVM_Driver" id_vendor="Actel" id_version="2.2.102" module_class="FirmWareModule" name="MSS_NVM_Driver" state="GOOD" type="3"/><module id_library="Firmware" id_name="MSS_PDMA_Driver" id_vendor="Actel" id_version="2.0.102" module_class="FirmWareModule" name="MSS_PDMA_Driver" state="GOOD" type="3"/><module id_library="Firmware" id_name="MSS_RTC_Driver" id_vendor="Actel" id_version="2.0.100" module_class="FirmWareModule" name="MSS_RTC_Driver" state="GOOD" type="3"/><module id_library="Firmware" id_name="MSS_Timer_Driver" id_vendor="Actel" id_version="2.1.101" module_class="FirmWareModule" name="MSS_Timer_Driver" state="GOOD" type="3"/><module id_library="Firmware" id_name="MSS_UART_Driver" id_vendor="Actel" id_version="2.3.101" module_class="FirmWareModule" name="MSS_UART_Driver" state="GOOD" type="3"/><module id_library="Firmware" id_name="SmartFusion_CMSIS_PAL" id_vendor="Actel" id_version="2.3.103" module_class="FirmWareModule" name="SmartFusion_CMSIS_PAL" state="GOOD" type="3"/></dependentModules></vendorExtensions></Component>