# Actel Physical design constraints file
# Generated file

# Version: 10.1 SP1 10.1.1.6
# Family: SmartFusion , Die: A2F500M3G , Package: 484 FBGA
# Date generated: Mon Nov 19 14:09:37 2012 


# 
# IO banks setting
# 


# 
# I/O constraints
# 

set_io MSS_RESET_N    \
    -pinname R1       \
    -fixed yes        \
    -DIRECTION Input


set_io UART_0_RXD     \
    -pinname U18      \
    -fixed yes        \
    -DIRECTION Input


set_io UART_0_TXD      \
    -pinname Y22       \
    -fixed yes         \
    -DIRECTION Output



#
# Non IO constraints
#


#
# Old IO constraints, commented out for reference
#

# set_io MSS_RESET_N -pinname R1 -fixed yes -DIRECTION Input 
# set_io UART_0_RXD -pinname U18 -fixed yes -DIRECTION Input 
# set_io UART_0_TXD -pinname Y22 -fixed yes -DIRECTION Output 
# set_io MSS_RESET_N -pinname R1 -fixed yes -DIRECTION Input 
# set_io UART_0_RXD -pinname U18 -fixed yes -DIRECTION Input 
# set_io UART_0_TXD -pinname Y22 -fixed yes -DIRECTION Output 
