Timing Report Min Delay Analysis

SmartTime Version v10.1 SP1
Actel Corporation - Actel Designer Software Release v10.1 SP1 (Version 10.1.1.6)
Copyright (c) 1989-2012
Date: Mon Nov 19 13:29:56 2012


Design: SF_UART
Family: SmartFusion
Die: A2F200M3F
Package: 484 FBGA
Temperature: COM
Voltage: COM
Speed Grade: -1
Design State: Post-Layout
Data source: Silicon verified
Min Operating Condition: BEST
Max Operating Condition: WORST
Using Enhanced Min Delay Analysis
Scenario for Timing Analysis: Primary


-----------------------------------------------------
SUMMARY

Clock Domain:               mss_aclk
Period (ns):                N/A
Frequency (MHz):            N/A
Required Period (ns):       12.500
Required Frequency (MHz):   80.000
External Setup (ns):        N/A
External Hold (ns):         N/A
Min Clock-To-Out (ns):      N/A
Max Clock-To-Out (ns):      N/A

Clock Domain:               mss_fabric_interface_clock
Period (ns):                N/A
Frequency (MHz):            N/A
Required Period (ns):       12.500
Required Frequency (MHz):   80.000
External Setup (ns):        N/A
External Hold (ns):         N/A
Min Clock-To-Out (ns):      N/A
Max Clock-To-Out (ns):      N/A

Clock Domain:               mss_pclk1
Period (ns):                N/A
Frequency (MHz):            N/A
Required Period (ns):       12.500
Required Frequency (MHz):   80.000
External Setup (ns):        N/A
External Hold (ns):         N/A
Min Clock-To-Out (ns):      N/A
Max Clock-To-Out (ns):      N/A

Clock Domain:               mss_ccc_gla0
Period (ns):                10.000
Frequency (MHz):            100.000
Required Period (ns):       12.500
Required Frequency (MHz):   80.000
External Setup (ns):        -5.119
External Hold (ns):         4.172
Min Clock-To-Out (ns):      N/A
Max Clock-To-Out (ns):      N/A

Clock Domain:               SF_UART_MSS_0/MSS_CCC_0/I_RCOSC:CLKOUT
Period (ns):                N/A
Frequency (MHz):            N/A
Required Period (ns):       10.000
Required Frequency (MHz):   100.000
External Setup (ns):        N/A
External Hold (ns):         N/A
Min Clock-To-Out (ns):      N/A
Max Clock-To-Out (ns):      N/A

                            Input to Output
Min Delay (ns):             N/A
Max Delay (ns):             N/A

END SUMMARY
-----------------------------------------------------

Clock Domain mss_aclk

SET Register to Register

No Path

END SET Register to Register

----------------------------------------------------

SET External Hold

No Path

END SET External Hold

----------------------------------------------------

SET Clock to Output

No Path

END SET Clock to Output

----------------------------------------------------

SET Register to Asynchronous

No Path

END SET Register to Asynchronous

----------------------------------------------------

SET External Removal

No Path

END SET External Removal

----------------------------------------------------

SET Asynchronous to Register

No Path

END SET Asynchronous to Register

----------------------------------------------------

Clock Domain mss_fabric_interface_clock

SET Register to Register

No Path

END SET Register to Register

----------------------------------------------------

SET External Hold

No Path

END SET External Hold

----------------------------------------------------

SET Clock to Output

No Path

END SET Clock to Output

----------------------------------------------------

SET Register to Asynchronous

No Path

END SET Register to Asynchronous

----------------------------------------------------

SET External Removal

No Path

END SET External Removal

----------------------------------------------------

SET Asynchronous to Register

No Path

END SET Asynchronous to Register

----------------------------------------------------

Clock Domain mss_pclk1

SET Register to Register

No Path

END SET Register to Register

----------------------------------------------------

SET External Hold

No Path

END SET External Hold

----------------------------------------------------

SET Clock to Output

No Path

END SET Clock to Output

----------------------------------------------------

SET Register to Asynchronous

No Path

END SET Register to Asynchronous

----------------------------------------------------

SET External Removal

No Path

END SET External Removal

----------------------------------------------------

SET Asynchronous to Register

No Path

END SET Asynchronous to Register

----------------------------------------------------

Clock Domain mss_ccc_gla0

Info: The maximum frequency of this clock domain is limited by the period of pin SF_UART_MSS_0/MSS_ADLIB_INST/U_CORE:FCLK

SET Register to Register

No Path

END SET Register to Register

----------------------------------------------------

SET External Hold

Path 1
  From:                        MSS_RESET_N
  To:                          SF_UART_MSS_0/MSS_ADLIB_INST/U_CORE:MSSRESETn
  Delay (ns):                  0.276
  Slack (ns):
  Arrival (ns):                0.276
  Required (ns):
  Hold (ns):                   1.354
  External Hold (ns):          4.172


Expanded Path 1
  From: MSS_RESET_N
  To: SF_UART_MSS_0/MSS_ADLIB_INST/U_CORE:MSSRESETn
  data arrival time                              0.276
  data required time                         -   N/C
  slack                                          N/C
  ________________________________________________________
  Data arrival time calculation
  0.000                        MSS_RESET_N (f)
               +     0.000          net: MSS_RESET_N
  0.000                        SF_UART_MSS_0/MSS_RESET_0_MSS_RESET_N:PAD (f)
               +     0.276          cell: ADLIB:IOPAD_IN
  0.276                        SF_UART_MSS_0/MSS_RESET_0_MSS_RESET_N:Y (f)
               +     0.000          net: SF_UART_MSS_0/MSS_RESET_0_MSS_RESET_N_Y
  0.276                        SF_UART_MSS_0/MSS_ADLIB_INST/U_CORE:MSSRESETn (f)
                                    
  0.276                        data arrival time
  ________________________________________________________
  Data required time calculation
  N/C                          mss_ccc_gla0
               +     0.000          Clock source
  N/C                          SF_UART_MSS_0/MSS_CCC_0/I_MSSCCC/U_MSSCCC:GLAMSS (r)
               +     2.724          Clock generation
  N/C
               +     0.370          net: SF_UART_MSS_0/MSS_ADLIB_INST_FCLK
  N/C                          SF_UART_MSS_0/MSS_ADLIB_INST/U_CORE:FCLK (r)
               +     1.354          Library hold time: ADLIB:MSS_APB_IP
  N/C                          SF_UART_MSS_0/MSS_ADLIB_INST/U_CORE:MSSRESETn


END SET External Hold

----------------------------------------------------

SET Clock to Output

No Path

END SET Clock to Output

----------------------------------------------------

SET Register to Asynchronous

No Path

END SET Register to Asynchronous

----------------------------------------------------

SET External Removal

No Path

END SET External Removal

----------------------------------------------------

SET Asynchronous to Register

No Path

END SET Asynchronous to Register

----------------------------------------------------

Clock Domain SF_UART_MSS_0/MSS_CCC_0/I_RCOSC:CLKOUT

SET Register to Register

No Path

END SET Register to Register

----------------------------------------------------

SET External Hold

No Path

END SET External Hold

----------------------------------------------------

SET Clock to Output

No Path

END SET Clock to Output

----------------------------------------------------

SET Register to Asynchronous

No Path

END SET Register to Asynchronous

----------------------------------------------------

SET External Removal

No Path

END SET External Removal

----------------------------------------------------

SET Asynchronous to Register

No Path

END SET Asynchronous to Register

----------------------------------------------------

Path set Pin to Pin

SET Input to Output

No Path

END SET Input to Output

----------------------------------------------------

Path set User Sets

