@W: MO111 :"c:\sf_uart_sw_flow_df\dev_kit\sc_standalone_pf\printf_uart\uart\component\work\uart_mss\mss_ccc_0\uart_mss_tmp_mss_ccc_0_mss_ccc.v":64:7:64:18|Tristate driver LPXIN_CLKOUT on net LPXIN_CLKOUT has its enable tied to GND (module UART_MSS_tmp_MSS_CCC_0_MSS_CCC) 
@W: MO111 :"c:\sf_uart_sw_flow_df\dev_kit\sc_standalone_pf\printf_uart\uart\component\work\uart_mss\mss_ccc_0\uart_mss_tmp_mss_ccc_0_mss_ccc.v":63:7:63:20|Tristate driver MAINXIN_CLKOUT on net MAINXIN_CLKOUT has its enable tied to GND (module UART_MSS_tmp_MSS_CCC_0_MSS_CCC) 
@W: MO111 :"c:\sf_uart_sw_flow_df\dev_kit\sc_standalone_pf\printf_uart\uart\component\work\uart_mss\mss_ccc_0\uart_mss_tmp_mss_ccc_0_mss_ccc.v":62:7:62:18|Tristate driver RCOSC_CLKOUT on net RCOSC_CLKOUT has its enable tied to GND (module UART_MSS_tmp_MSS_CCC_0_MSS_CCC) 
