<Actel_Data_File>
    <format name="NVM File" version="01.00.00"/>
    <header>
        <die>
            A2F500M3G
        </die>
        <family>
            SmartFusion
        </family>
        <module>
            envm
        </module>
        <package>
            484 FBGA
        </package>
        <version>
            10.1.1.6
        </version>
    </header>
    <nvm>
        <region name="ACTEL_SYSTEM_BOOT" address="0x101100" retrieveAddressFromFile="false" size="5632" format="HEX" type="Data Storage" wordSize="32" numberWords="1408" memFile="" memType="" memFileTimeStamp="" clientType="private" program="true">
            [encoded data, 11220 characters]
            00000000000000000000000000000000000000000000
            <crc>
                0a8d
            </crc>
        </region>
        <region name="ACTEL_AB_MSS_CONFIG" address="0x103e00" retrieveAddressFromFile="false" size="208" format="HEX" type="Data Storage" wordSize="32" numberWords="52" memFile="" memType="" memFileTimeStamp="" clientType="private" program="true">
            000000000000000000000000000000000000000000000000221f1f000a45
            45007e7f010000000a0000082001aa40f903010000d2000000000000001e
            1a0707000500100005001000000000002bacb0c20a1828b0c20a2bacb0c2
            0a2bacb0c20a2bacb0c20a2bacb0c20a2bacb0c20a2bacb0c20a2bacb0c2
            0a2bacb0c20a2bacb0c20a2bacb0c20a2bacb0c20a2bacb0c20a2bacb0c2
            0a2bacb0c20a2bacb0c20a2bacb0c20a2bacb0c20a2bacb0c20a2bacb002
            0000000078ff080090d0030080ff070080ff0700000000000000091b
            <crc>
                90af
            </crc>
        </region>
    </nvm>
</Actel_Data_File>
