***** Place and Route Configurations *****
Timing-driven       : ON
Power-driven        : OFF
High-effort         : ON
Repair Min-delay    : ON
Incremental         : OFF

TDPR Scenario       : Primary
Running 'g4layout.exe' in 64-bit mode


Running the I/O Bank and Globals Assigner.

Info:  I/O Bank and Globals Assigner identified 51 fixed I/O macros, 0 unfixed I/O macros



I/O Bank and Globals Assigner completed successfully.

Total time spent in I/O Bank and Globals Assigner: 0 seconds

Running 'g4placer.exe' in 64-bit mode


Placer V4.0 - 11.6.0 


Design: MDDR_TA_top                     Started: Tue Sep 29 15:04:33 2015





Initializing High-Effort Timing-Driven Placement ...


Placing design...


End of placement.


Pre-Placement Runtime        : 3 seconds


Placement Runtime            : 27 seconds





Placer completed successfully.





Design: MDDR_TA_top                     


Finished: Tue Sep 29 15:05:22 2015


Total CPU Time:     00:00:48            Total Elapsed Time: 00:00:49


Total Memory Usage: 330.4 Mbytes


                        o - o - o - o - o - o





Running 'g4layout.exe' in 64-bit mode
Running 'g4router.exe' in 64-bit mode


Timing-driven Router 


Design: D:\Libero_11.6_migration\Libero_designs\m2gl_ac424_new_without_workaround\Libero_Project\MDDR_TA\designer\MDDR_TA_top\MDDR_TA_topStarted: Tue Sep 29 15:05:24 2015








Timing-driven Router completed successfully.





Design: D:\Libero_11.6_migration\Libero_designs\m2gl_ac424_new_without_workaround\Libero_Project\MDDR_TA\designer\MDDR_TA_top\MDDR_TA_top


Finished: Tue Sep 29 15:05:50 2015


Total CPU Time:     00:00:24            Total Elapsed Time: 00:00:26


Total Memory Usage: 622.3 Mbytes


                        o - o - o - o - o - o





Info: Iteration 1:

  Number of violating paths: 1

  Worst minimum delay slack: -0.117 ns

Running 'g4router.exe' in 64-bit mode


Router 


Design: D:\Libero_11.6_migration\Libero_designs\m2gl_ac424_new_without_workaround\Libero_Project\MDDR_TA\designer\MDDR_TA_top\MDDR_TA_topStarted: Tue Sep 29 15:06:01 2015





Loading routing information for ECO mode...


After loading previous routing information: Shorts = 0. Open nets = 2.





Router completed successfully.





Design: D:\Libero_11.6_migration\Libero_designs\m2gl_ac424_new_without_workaround\Libero_Project\MDDR_TA\designer\MDDR_TA_top\MDDR_TA_top


Finished: Tue Sep 29 15:06:06 2015


Total CPU Time:     00:00:04            Total Elapsed Time: 00:00:05


Total Memory Usage: 504.5 Mbytes


                        o - o - o - o - o - o





Info: Iteration 2:

  Number of violating paths: 1

  Worst minimum delay slack: -0.072 ns

Running 'g4router.exe' in 64-bit mode


Router 


Design: D:\Libero_11.6_migration\Libero_designs\m2gl_ac424_new_without_workaround\Libero_Project\MDDR_TA\designer\MDDR_TA_top\MDDR_TA_topStarted: Tue Sep 29 15:06:18 2015





Loading routing information for ECO mode...


After loading previous routing information: Shorts = 0. Open nets = 2.





Router completed successfully.





Design: D:\Libero_11.6_migration\Libero_designs\m2gl_ac424_new_without_workaround\Libero_Project\MDDR_TA\designer\MDDR_TA_top\MDDR_TA_top


Finished: Tue Sep 29 15:06:23 2015


Total CPU Time:     00:00:05            Total Elapsed Time: 00:00:05


Total Memory Usage: 504.4 Mbytes


                        o - o - o - o - o - o





Resource Usage

+---------------+------+-------+------------+

| Type          | Used | Total | Percentage |

+---------------+------+-------+------------+

| 4LUT          | 1634 | 12084 | 13.52      |

| DFF           | 1071 | 12084 | 8.86       |

| I/O Register  | 0    | 693   | 0.00       |

| Logic Element | 1736 | 12084 | 14.37      |

+---------------+------+-------+------------+



The 'probe' command succeeded.

The Execute Script command succeeded.

Running 'g4layout.exe' in 64-bit mode
