set_component MDDR_TA_CCC_0_FCCC
create_clock -period 20 [ get_pins {CCC_INST/RCOSC_25_50MHZ} ]
create_generated_clock -multiply_by 83 -divide_by 200 -source [ get_pins {CCC_INST/RCOSC_25_50MHZ} ] [ get_pins {CCC_INST/GL0} ]
create_generated_clock -multiply_by 83 -divide_by 50 -source [ get_pins {CCC_INST/RCOSC_25_50MHZ} ] [ get_pins {CCC_INST/GL2} ]
