Resource Usage Report for MDDR_TA_top 

Mapping to part: m2gl010tfbga484-1
Cell usage:
CCC             1 use
CLKINT          9 uses
MSS_010         1 use
RCOSC_25_50MHZ  1 use
RCOSC_25_50MHZ_FAB  1 use
SYSRESET        1 use
CFG1           25 uses
CFG2           252 uses
CFG3           264 uses
CFG4           680 uses

Carry primitives used for arithmetic functions:
ARI1           299 uses


Sequential Cells: 
SLE            963 uses

DSP Blocks:    0

I/O ports: 53
I/O primitives: 51
BIBUF          20 uses
INBUF          2 uses
OUTBUF         28 uses
OUTBUF_DIFF    1 use


Global Clock Buffers: 9


Total LUTs:    1520

Extra resources required for RAM and MACC interface logic during P&R:

RAM64x18 Interface Logic : SLEs = 0; LUTs = 0;
RAM1K18  Interface Logic : SLEs = 108; LUTs = 108;
MACC     Interface Logic : SLEs = 0; LUTs = 0;

Total number of SLEs after P&R:  963 + 0 + 108 + 0 = 1071;
Total number of LUTs after P&R:  1520 + 0 + 108 + 0 = 1628;

