# Power Report for design top with the following settings:

Vendor: | Microsemi Corporation
Program: | Microsemi Libero Software, Release v12.6 (Version 12.900.20.24)
| Copyright (C) 1989-
Date: | Fri Mar 19 13:50:05 2021
Version: | 3.0

Design: | top
Family: | IGLOO2
Die: | M2GL010TS
Package: | 484 FBGA
Temperature Range: | COM
Voltage Range: | COM
Operating Conditions: | Typical
Operating Mode: | Active
Process: | Typical
Data Source: | Production

## Power Summary

| Power (mW) | Percentage
--- | --- | ---
Total Power | 94.491 | 100.0%
Static Power | 10.330 | 10.9%
Dynamic Power | 84.161 | 89.1%

## Breakdown by Rail

| Power (mW) | Voltage (V) | Current (mA)
--- | --- | --- | ---
Rail VDD | 64.447 | 1.200 | 53.706
Rail CCC_NE1_PLL_VDDA | 9.000 | 3.300 | 2.727
Rail VDDI 2.5 | 2.919 | 2.500 | 1.168
Rail MDDR_PLL_VDDA | 5.000 | 3.300 | 1.515
Rail VPP | 13.125 | 2.500 | 5.250

## Breakdown by Clock

| Power (mW) | Percentage
--- | --- | ---
my_hpms_top_0/my_hpms_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (clocks) | 48.402 | 89.6%
my_hpms_top_0/my_hpms_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (register outputs) | 1.256 | 2.3%
my_hpms_top_0/my_hpms_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (primary inputs) | 0.000 | 0.0%
my_hpms_top_0/my_hpms_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (combinational outputs) | 4.336 | 8.0%
my_hpms_top_0/my_hpms_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 (set/reset nets) | 0.000 | 0.0%
my_hpms_top_0/my_hpms_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (clocks) | 0.000 | 0.0%
my_hpms_top_0/my_hpms_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (register outputs) | 0.001 | 0.0%
my_hpms_top_0/my_hpms_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (primary inputs) | 0.000 | 0.0%
my_hpms_top_0/my_hpms_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (combinational outputs) | 0.000 | 0.0%
my_hpms_top_0/my_hpms_0/FABOSC_0/I_RCOSC_25_50MHZ/U0:CLKOUT (set/reset nets) | 0.000 | 0.0%
Input to Output | 0.000 | 0.0%

## Breakdown by Type

| Power (mW) | Percentage
--- | --- | ---
Type Net | 2.883 | 3.1%
Type Gate | 12.210 | 12.9%
Type I/O | 1.482 | 1.6%
Type Memory | 1.564 | 1.7%
Type Core Static | 8.262 | 8.7%
Type Banks Static | 1.443 | 1.5%
Type VPP Static | 0.625 | 0.7%
Type Built-in Blocks | 66.023 | 69.9%