# Global Net Report

Microsemi Corporation - Microsemi Libero Software Release v12.6 (Version 12.900.20.24)

Date: Thu Mar 25 18:23:01 2021

## Global Nets Information

| From | GB Location | Net Name | Fanout
--- | --- | --- | --- | ---
1 | GB[3] | (221, 54) | my_hpms_top_0/my_hpms_0/CCC_0/GL0_INST/U0_YNn | 954
2 | GB[1] | (219, 54) | my_hpms_top_0/my_hpms_0/CORERESETP_0/MSS_HPMS_READY_int_rep_RNID6U1/U0_YNn | 571
3 | GB[2] | (220, 54) | UART_top_0/COREABC_0/genblk2.RSTSYNC2_RNIRG27/U0_YNn | 261

## I/O to GB Connections

(none)

## Fabric to GB Connections

| From | From Location | To | Net Name | Net Type | Fanout
--- | --- | --- | --- | --- | --- | ---
1 | my_hpms_top_0/my_hpms_0/CORERESETP_0/MSS_HPMS_READY_int_rep:Q | (380, 70) | GB[1] | my_hpms_top_0/my_hpms_0/CORERESETP_0/MSS_HPMS_READY_int_rep_Z | ROUTED | 1
2 | UART_top_0/COREABC_0/genblk2.RSTSYNC2:Q | (254, 70) | GB[2] | UART_top_0/COREABC_0/genblk2.RSTSYNC2_Z | ROUTED | 3

## CCC to GB Connections

| From | From Location | Pin Swapped for Back Annotation Only | To | Net Name | Net Type | Fanout
--- | --- | --- | --- | --- | --- | --- | ---
1 | my_hpms_top_0/my_hpms_0/CCC_0/CCC_INST/INST_CCC_IP:GL0 | CCC-NE1 (390, 92) | GL0 => GL3 | GB[3] | my_hpms_top_0/my_hpms_0/CCC_0/GL0_net | HARDWIRED | 1

## CCC Input Connections

| From | From Location | To (Pin Swapped for Back Annotation Only) | CCC Location | Net Name | Net Type | Fanout
--- | --- | --- | --- | --- | --- | --- | ---
1 | my_hpms_top_0/my_hpms_0/FABOSC_0/I_RCOSC_25_50MHZ:CLKOUT | (396, 92) | my_hpms_top_0/my_hpms_0/CCC_0/CCC_INST/INST_CCC_IP:RCOSC_25_50MHZ | CCC-NE1 (390, 92) | my_hpms_top_0/my_hpms_0/FABOSC_0_RCOSC_25_50MHZ_CCC_OUT_RCOSC_25_50MHZ_CCC | HARDWIRED | 1

## Local Nets to RGB Connections

(none)

## Global Nets to RGB Connections

| From | From Location | Net Name | Fanout |  | RGB Location | Local Fanout
--- | --- | --- | --- | --- | --- | --- | ---
1 | GB[3] | (221, 54) | my_hpms_top_0/my_hpms_0/CCC_0/GL0_INST/U0_YNn | 954 | 1 | (218, 57) | 69
|  |  |  |  | 2 | (218, 60) | 60
|  |  |  |  | 3 | (218, 63) | 56
|  |  |  |  | 4 | (218, 66) | 44
|  |  |  |  | 5 | (218, 69) | 79
|  |  |  |  | 6 | (218, 72) | 32
|  |  |  |  | 7 | (218, 75) | 21
|  |  |  |  | 8 | (218, 102) | 1
2 | GB[1] | (219, 54) | my_hpms_top_0/my_hpms_0/CORERESETP_0/MSS_HPMS_READY_int_rep_RNID6U1/U0_YNn | 571 | 1 | (220, 57) | 25
|  |  |  |  | 2 | (220, 60) | 8
3 | GB[2] | (220, 54) | UART_top_0/COREABC_0/genblk2.RSTSYNC2_RNIRG27/U0_YNn | 261 | 1 | (219, 57) | 23
|  |  |  |  | 2 | (219, 60) | 43
|  |  |  |  | 3 | (219, 63) | 39
|  |  |  |  | 4 | (219, 66) | 40
|  |  |  |  | 5 | (219, 69) | 33
|  |  |  |  | 6 | (219, 72) | 32
|  |  |  |  | 7 | (219, 75) | 21