"eNVM_DataClient_0/CCC_0/CCC_INST/INST_CCC_IP:GL0",10,"eNVM_DataClient_0/CCC_0/CCC_INST/INST_CCC_IP:GL0","eNVM_DataClient_0/CCC_0/CCC_INST/INST_CCC_IP:GL0"
"eNVM_DataClient_0/FABOSC_0/I_RCOSC_25_50MHZ:CLKOUT",20,"eNVM_DataClient_0/FABOSC_0/I_RCOSC_25_50MHZ:CLKOUT","eNVM_DataClient_0/FABOSC_0/I_RCOSC_25_50MHZ:CLKOUT"
