<Actel_Data_File>
    <format name="NVM File" version="01.00.00"/>
    <header>
        <die>
            M2S010T
        </die>
        <family>
            SmartFusion2
        </family>
        <module>
            
        </module>
        <package>
            484 FBGA
        </package>
        <version>
            11.8.1.12
        </version>
    </header>
    <nvm>
        <region name="envm_client" address="0x000000" retrieveAddressFromFile="false" size="5744" format="HEX" type="Data Storage" wordSize="8" numberWords="5744" memFile="D:/test/m2s_dg0441_starter_liberov11p8_sp1_df/SF2_Starter_Adaptive_FIR_filter_Demo_DF/DesignFiles/Adaptive_FIR_filter_Demo/SoftConsole4.0/Adaptive_FIR_MSS_CM3/Release/Adaptive_FIR_MSS_CM3.hex" memType="INTELHEX" memFileTimeStamp="1505139714" clientType="public" program="true">
            [encoded data, 11460 characters]
            f50500e1f50500e1f50500e1f505
            <crc>
                f480
            </crc>
        </region>
    </nvm>
</Actel_Data_File>
