@W: BN231 |Constraints on tristate nets currently not supported
@W: BN132 :"d:\libero_11_7_publish\tu0547_iar_ncf\component\actel\directcore\coreresetp\7.0.104\rtl\vlog\core\coreresetp.v":1089:4:1089:9|Removing sequential instance SPI_Flash_sb_0.CORERESETP_0.MDDR_DDR_AXI_S_CORE_RESET_N_int,  because it is equivalent to instance SPI_Flash_sb_0.CORERESETP_0.FDDR_CORE_RESET_N_int
