# Global Net Report

Microsemi Corporation - Microsemi Libero Software Release v12.6 (Version 12.900.20.24)

Date: Thu Jan 7 09:28:42 2021

## Global Nets Information

| From | GB Location | Net Name | Fanout
--- | --- | --- | --- | ---
1 | PF_CLK_DIV_C0_0/PF_CLK_DIV_C0_0/I_CD_RNIF7Q3/U0 | (1165, 162) | PF_CLK_DIV_C0_0/PF_CLK_DIV_C0_0/I_CD_RNIF7Q3/U0_Y | 128
2 | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0 | (1152, 162) | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0_Y | 103
3 | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_INT/U0 | (1173, 162) | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_INT/U0_Y | 2
4 | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0_GB0 | (1164, 163) | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0_gbs_1 | 1

## I/O to GB Connections

(none)

## Fabric to GB Connections

| From | From Location | To | Net Name | Net Type | Fanout
--- | --- | --- | --- | --- | --- | ---
1 | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_INT/U0_RGB1_RGB0:Y | (1749, 179) | PF_CLK_DIV_C0_0/PF_CLK_DIV_C0_0/I_CD_RNIF7Q3/U0 | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_INT/U0_RGB1_RGB0_rgb_net_1 | ROUTED | 1
2 | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160:CLK | (512, 2) | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_INT/U0 | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_CLK_c | HARDWIRED | 1

## CCC to GB Connections

| From | From Location | To | Net Name | Net Type | Fanout
--- | --- | --- | --- | --- | --- | ---
1 | PF_CCC_50_0/PF_CCC_50_0/pll_inst_0:OUT0 | (2460, 377) | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0 | PF_CCC_50_0/PF_CCC_50_0/pll_inst_0_clkint_0 | HARDWIRED | 1
2 | PF_CCC_50_0/PF_CCC_50_0/pll_inst_0:OUT0 | (2460, 377) | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0_GB0 | PF_CCC_50_0/PF_CCC_50_0/pll_inst_0_clkint_0 | HARDWIRED | 1

## CCC Input Connections

| From | From Location | To | CCC Location | Net Name | Net Type | Fanout
--- | --- | --- | --- | --- | --- | --- | ---
1 | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160:CLK | (512, 2) | PF_CCC_50_0/PF_CCC_50_0/pll_inst_0:REF_CLK_0 | (2460, 377) | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_CLK_c | ROUTED | 1

## Local Nets to RGB Connections

| From | From Location | Net Name | Net Type | Fanout | RGB Location | Local Fanout
--- | --- | --- | --- | --- | --- | --- | ---
1 | PF_XCVR_0_0/I_XCVR/LANE0:TX_CLK_R | (2460, 317) | PF_XCVR_0_0/I_XCVR/LANE0_tx_rclkint_input_net | HARDWIRED | 177 | (1747, 313) | 177
2 | PF_XCVR_0_0/I_XCVR/LANE0:RX_CLK_R | (2460, 317) | PF_XCVR_0_0/I_XCVR/LANE0_rx_rclkint_input_net | HARDWIRED | 117 | (1750, 178) | 2
|  |  |  |  |  | (1750, 232) | 1
|  |  |  |  |  | (1750, 286) | 14
|  |  |  |  |  | (1750, 313) | 100

## Global Nets to RGB Connections

| From | From Location | Net Name | Fanout |  | RGB Location | Local Fanout
--- | --- | --- | --- | --- | --- | --- | ---
1 | PF_CLK_DIV_C0_0/PF_CLK_DIV_C0_0/I_CD_RNIF7Q3/U0 | (1165, 162) | PF_CLK_DIV_C0_0/PF_CLK_DIV_C0_0/I_CD_RNIF7Q3/U0_Y | 128 |  | (1749, 312) | 128
2 | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0 | (1152, 162) | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0_Y | 103 | 1 | (576, 12) | 99
|  |  |  |  | 2 | (576, 39) | 2
|  |  |  |  | 3 | (582, 12) | 2
3 | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_INT/U0 | (1173, 162) | PF_OSC_160_0/PF_OSC_160_0/I_OSC_160_INT/U0_Y | 2 | 1 | (1749, 179) | 1
|  |  |  |  | 2 | (1749, 368) | 1
4 | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0_GB0 | (1164, 163) | PF_CCC_50_0/PF_CCC_50_0/clkint_0/U0_gbs_1 | 1 |  | (1747, 312) | 1

## Clock Signals Summary

The number of clock signals through H-Chip Global resources | 3
The number of clock signals through Row Global resources | 10
The number of clock signals through Sector Global resources | 16
The number of clock signals through Cluster Global resources | 81