# Microsemi I/O Physical Design Constraints file

# User I/O Constraints file 

# Version: v12.6 12.900.20.24

# Family: PolarFire , Die: MPF300T , Package: FCG1152

# Date generated: Tue Aug 10 12:36:22 2021 


# 
# User Locked I/O Bank Settings
# 


# 
# Unlocked I/O Bank Settings
# The I/O Bank Settings can be locked by directly editing this file
# or by making changes in the I/O Attribute Editor
# 


# 
# User Locked I/O settings
# 

set_io -port_name RX  \
    -pin_name H18     \
    -fixed true       \
    -DIRECTION INPUT


set_io -port_name TX   \
    -pin_name G17      \
    -fixed true        \
    -DIRECTION OUTPUT



# 
# Dedicated Peripheral I/O Settings
# 


# 
# Unlocked I/O settings
# The I/Os in this section are unplaced or placed but are not locked
# the other listed attributes have been applied
# 


#
#Ports using Dedicated Pins

#
set_io -port_name REF_CLK_PAD_N  \
    -pin_name AF30               \
    -DIRECTION INPUT


set_io -port_name REF_CLK_PAD_P  \
    -pin_name AF29               \
    -DIRECTION INPUT
	

set_io -port_name LANE0_RXD_N  \
    -pin_name AD30             \
    -DIRECTION INPUT


set_io -port_name LANE0_RXD_P  \
    -pin_name AD29             \
    -DIRECTION INPUT


set_io -port_name LANE0_TXD_N  \
    -pin_name AE32             \
    -DIRECTION OUTPUT


set_io -port_name LANE0_TXD_P  \
    -pin_name AE31             \
    -DIRECTION OUTPUT

#
#set_io -port_name atck  \
    #-pin_name J10       \
    #-DIRECTION INPUT
#
#
#set_io -port_name atdi  \
    #-pin_name K11       \
    #-DIRECTION INPUT
#
#
#set_io -port_name atdo  \
    #-pin_name K9        \
    #-DIRECTION OUTPUT
#
#
#set_io -port_name atms  \
    #-pin_name J9        \
    #-DIRECTION INPUT
#
#
#set_io -port_name atrstb  \
    #-pin_name N14         \
    #-DIRECTION INPUT


