# Configuration Report for PolarFireSoC MSS Configurator (Pre-production)

## Design Information

Design Parameter Name | Design Parameter Value
--- | ---
Family | PolarFireSoC
Die | MPFS250T_ES
Package | FCG1152
Version | 2021.2
Date | Thu Feb 24 14:54:12 2022

## FPGA Fabric

FPGA Fabric Programming | Required
--- | ---

## MSS to/from Fabric Interface Controllers

Interface Controller Name | Enabled
--- | ---
FIC_0 AXI4 Initiator Interface | true
FIC_0 AXI4 Target Interface | false
FIC_1 AXI4 Initiator Interface | true
FIC_1 AXI4 Target Interface | false
FIC_2 AXI4 Target Interface | false
FIC_3 APB Initiator Interface | false

## Peripherals

Peripheral Name | Enabled
--- | ---
eMMC | MSSIO_B4
USB | MSSIO_B2
SD/SDIO | UNUSED
Gigabit Ethernet MAC_0 | SGMII_IO_B5
Gigabit Ethernet MAC_1 | UNUSED
QSPI | UNUSED
SPI_0 | UNUSED
SPI_1 | UNUSED
MMUART_0 | FABRIC
MMUART_1 | FABRIC
MMUART_2 | UNUSED
MMUART_3 | UNUSED
MMUART_4 | UNUSED
I2C_0 | FABRIC
I2C_1 | UNUSED
CAN_0 | UNUSED
CAN_1 | UNUSED
GPIO_0_0 | UNUSED
GPIO_0_1 | UNUSED
GPIO_0_2 | UNUSED
GPIO_0_3 | UNUSED
GPIO_0_4 | UNUSED
GPIO_0_5 | UNUSED
GPIO_0_6 | UNUSED
GPIO_0_7 | UNUSED
GPIO_0_8 | UNUSED
GPIO_0_9 | UNUSED
GPIO_0_10 | UNUSED
GPIO_0_11 | UNUSED
GPIO_0_12 | UNUSED
GPIO_0_13 | UNUSED
GPIO_1_0 | UNUSED
GPIO_1_1 | UNUSED
GPIO_1_2 | UNUSED
GPIO_1_3 | UNUSED
GPIO_1_4 | UNUSED
GPIO_1_5 | UNUSED
GPIO_1_6 | UNUSED
GPIO_1_7 | UNUSED
GPIO_1_8 | UNUSED
GPIO_1_9 | UNUSED
GPIO_1_10 | UNUSED
GPIO_1_11 | UNUSED
GPIO_1_12 | MSSIO_B2
GPIO_1_13 | UNUSED
GPIO_1_14 | UNUSED
GPIO_1_15 | UNUSED
GPIO_1_16 | MSSIO_B2
GPIO_1_17 | UNUSED
GPIO_1_18 | UNUSED
GPIO_1_19 | UNUSED
GPIO_1_20 | MSSIO_B2
GPIO_1_21 | UNUSED
GPIO_1_22 | UNUSED
GPIO_1_23 | MSSIO_B2
GPIO_2_0 | UNUSED
GPIO_2_1 | UNUSED
GPIO_2_2 | FABRIC
GPIO_2_3 | FABRIC
GPIO_2_4 | FABRIC
GPIO_2_5 | UNUSED
GPIO_2_6 | UNUSED
GPIO_2_7 | UNUSED
GPIO_2_8 | FABRIC
GPIO_2_9 | FABRIC
GPIO_2_10 | UNUSED
GPIO_2_11 | UNUSED
GPIO_2_12 | UNUSED
GPIO_2_13 | UNUSED
GPIO_2_14 | UNUSED
GPIO_2_15 | UNUSED
GPIO_2_16 | UNUSED
GPIO_2_17 | UNUSED
GPIO_2_18 | FABRIC
GPIO_2_19 | FABRIC
GPIO_2_20 | UNUSED
GPIO_2_21 | UNUSED
GPIO_2_22 | UNUSED
GPIO_2_23 | UNUSED
GPIO_2_24 | UNUSED
GPIO_2_25 | UNUSED
GPIO_2_26 | UNUSED
GPIO_2_27 | UNUSED
GPIO_2_28 | UNUSED
GPIO_2_29 | UNUSED
GPIO_2_30 | UNUSED
GPIO_2_31 | UNUSED

## DDR Memory

DDR | Protocol
--- | ---
Memory Type | LPDDR4

## List of Ports

Port Name | Direction
--- | ---
FIC_0_ACLK | INPUT
FIC_0_AXI4_M_AWREADY | INPUT
FIC_0_AXI4_M_WREADY | INPUT
FIC_0_AXI4_M_BID[7:0] | INPUT
FIC_0_AXI4_M_BRESP[1:0] | INPUT
FIC_0_AXI4_M_BVALID | INPUT
FIC_0_AXI4_M_ARREADY | INPUT
FIC_0_AXI4_M_RID[7:0] | INPUT
FIC_0_AXI4_M_RDATA[63:0] | INPUT
FIC_0_AXI4_M_RRESP[1:0] | INPUT
FIC_0_AXI4_M_RLAST | INPUT
FIC_0_AXI4_M_RVALID | INPUT
FIC_1_ACLK | INPUT
FIC_1_AXI4_M_AWREADY | INPUT
FIC_1_AXI4_M_WREADY | INPUT
FIC_1_AXI4_M_BID[7:0] | INPUT
FIC_1_AXI4_M_BRESP[1:0] | INPUT
FIC_1_AXI4_M_BVALID | INPUT
FIC_1_AXI4_M_ARREADY | INPUT
FIC_1_AXI4_M_RID[7:0] | INPUT
FIC_1_AXI4_M_RDATA[63:0] | INPUT
FIC_1_AXI4_M_RRESP[1:0] | INPUT
FIC_1_AXI4_M_RLAST | INPUT
FIC_1_AXI4_M_RVALID | INPUT
MMUART_0_RXD_F2M | INPUT
MMUART_1_RXD_F2M | INPUT
I2C_0_SCL_F2M | INPUT
I2C_0_SDA_F2M | INPUT
I2C_0_BCLK_F2M | INPUT
MSS_RESET_N_F2M | INPUT
FIC_0_DLL_LOCK_M2F | OUTPUT
FIC_1_DLL_LOCK_M2F | OUTPUT
FIC_0_AXI4_M_AWID[7:0] | OUTPUT
FIC_0_AXI4_M_AWADDR[37:0] | OUTPUT
FIC_0_AXI4_M_AWLEN[7:0] | OUTPUT
FIC_0_AXI4_M_AWSIZE[2:0] | OUTPUT
FIC_0_AXI4_M_AWBURST[1:0] | OUTPUT
FIC_0_AXI4_M_AWLOCK | OUTPUT
FIC_0_AXI4_M_AWQOS[3:0] | OUTPUT
FIC_0_AXI4_M_AWCACHE[3:0] | OUTPUT
FIC_0_AXI4_M_AWPROT[2:0] | OUTPUT
FIC_0_AXI4_M_AWVALID | OUTPUT
FIC_0_AXI4_M_WDATA[63:0] | OUTPUT
FIC_0_AXI4_M_WSTRB[7:0] | OUTPUT
FIC_0_AXI4_M_WLAST | OUTPUT
FIC_0_AXI4_M_WVALID | OUTPUT
FIC_0_AXI4_M_BREADY | OUTPUT
FIC_0_AXI4_M_ARID[7:0] | OUTPUT
FIC_0_AXI4_M_ARADDR[37:0] | OUTPUT
FIC_0_AXI4_M_ARLEN[7:0] | OUTPUT
FIC_0_AXI4_M_ARSIZE[2:0] | OUTPUT
FIC_0_AXI4_M_ARBURST[1:0] | OUTPUT
FIC_0_AXI4_M_ARLOCK | OUTPUT
FIC_0_AXI4_M_ARQOS[3:0] | OUTPUT
FIC_0_AXI4_M_ARCACHE[3:0] | OUTPUT
FIC_0_AXI4_M_ARPROT[2:0] | OUTPUT
FIC_0_AXI4_M_ARVALID | OUTPUT
FIC_0_AXI4_M_RREADY | OUTPUT
FIC_1_AXI4_M_AWID[7:0] | OUTPUT
FIC_1_AXI4_M_AWADDR[37:0] | OUTPUT
FIC_1_AXI4_M_AWLEN[7:0] | OUTPUT
FIC_1_AXI4_M_AWSIZE[2:0] | OUTPUT
FIC_1_AXI4_M_AWBURST[1:0] | OUTPUT
FIC_1_AXI4_M_AWLOCK | OUTPUT
FIC_1_AXI4_M_AWQOS[3:0] | OUTPUT
FIC_1_AXI4_M_AWCACHE[3:0] | OUTPUT
FIC_1_AXI4_M_AWPROT[2:0] | OUTPUT
FIC_1_AXI4_M_AWVALID | OUTPUT
FIC_1_AXI4_M_WDATA[63:0] | OUTPUT
FIC_1_AXI4_M_WSTRB[7:0] | OUTPUT
FIC_1_AXI4_M_WLAST | OUTPUT
FIC_1_AXI4_M_WVALID | OUTPUT
FIC_1_AXI4_M_BREADY | OUTPUT
FIC_1_AXI4_M_ARID[7:0] | OUTPUT
FIC_1_AXI4_M_ARADDR[37:0] | OUTPUT
FIC_1_AXI4_M_ARLEN[7:0] | OUTPUT
FIC_1_AXI4_M_ARSIZE[2:0] | OUTPUT
FIC_1_AXI4_M_ARBURST[1:0] | OUTPUT
FIC_1_AXI4_M_ARLOCK | OUTPUT
FIC_1_AXI4_M_ARQOS[3:0] | OUTPUT
FIC_1_AXI4_M_ARCACHE[3:0] | OUTPUT
FIC_1_AXI4_M_ARPROT[2:0] | OUTPUT
FIC_1_AXI4_M_ARVALID | OUTPUT
FIC_1_AXI4_M_RREADY | OUTPUT
MMUART_0_TXD_M2F | OUTPUT
MMUART_0_TXD_OE_M2F | OUTPUT
MMUART_1_TXD_M2F | OUTPUT
MMUART_1_TXD_OE_M2F | OUTPUT
I2C_0_SCL_OE_M2F | OUTPUT
I2C_0_SDA_OE_M2F | OUTPUT
GPIO_2_M2F_19 | OUTPUT
GPIO_2_M2F_18 | OUTPUT
GPIO_2_M2F_9 | OUTPUT
GPIO_2_M2F_8 | OUTPUT
GPIO_2_M2F_4 | OUTPUT
GPIO_2_M2F_3 | OUTPUT
GPIO_2_M2F_2 | OUTPUT
PLL_CPU_LOCK_M2F | OUTPUT
PLL_DDR_LOCK_M2F | OUTPUT
PLL_SGMII_LOCK_M2F | OUTPUT
MSS_RESET_N_M2F | OUTPUT
MAC_0_MDIO | INOUT
MAC_0_MDC | OUTPUT
GPIO_1_12_OUT | OUTPUT
GPIO_1_16_OUT | OUTPUT
GPIO_1_20_OUT | OUTPUT
GPIO_1_23_OUT | OUTPUT
USB_CLK | INPUT
USB_DIR | INPUT
USB_NXT | INPUT
USB_STP | OUTPUT
USB_DATA0 | INOUT
USB_DATA1 | INOUT
USB_DATA2 | INOUT
USB_DATA3 | INOUT
USB_DATA4 | INOUT
USB_DATA5 | INOUT
USB_DATA6 | INOUT
USB_DATA7 | INOUT
EMMC_CLK | OUTPUT
EMMC_CMD | INOUT
EMMC_DATA0 | INOUT
EMMC_DATA1 | INOUT
EMMC_DATA2 | INOUT
EMMC_DATA3 | INOUT
EMMC_DATA4 | INOUT
EMMC_DATA5 | INOUT
EMMC_DATA6 | INOUT
EMMC_DATA7 | INOUT
EMMC_STRB | INPUT
EMMC_RSTN | OUTPUT
SGMII_RX0_P | INPUT
SGMII_RX0_N | INPUT
SGMII_TX0_P | OUTPUT
SGMII_TX0_N | OUTPUT
REFCLK | INPUT
REFCLK_N | INPUT
DQ[31:0] | INOUT
DQS[3:0] | INOUT
DQS_N[3:0] | INOUT
DM[3:0] | OUTPUT
RESET_N | OUTPUT
ODT | OUTPUT
CKE | OUTPUT
CS | OUTPUT
CK | OUTPUT
CK_N | OUTPUT
CA[5:0] | OUTPUT

## I/O REFCLK Port settings

Port Name | Package Pin Name | Direction | I/O Standard | Schmitt Trigger | On Die Termination | Thevenin Termination | Pull Up
--- | --- | --- | --- | --- | --- | --- | ---
REFCLK_N | W3 | INPUT | LVDS25 | OFF | 100 | OFF | OFF
REFCLK | V3 | INPUT | LVDS25 | OFF | 100 | OFF | OFF

## MSSIO Port Settings

Port Name | MSS I/O Number | Package Pin Name | Direction | Resistor Pull | Persist | Clamp Diode | Lock Down | Schmitt Trigger | Low Power Mode Input Receiver | Output Drive (mA) | Low Power Mode Output Buffer
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
EMMC_CLK | MSSIO0 | AA8 | OUTPUT | UP | OFF | OFF | OFF | -- | -- | 8 | OFF
EMMC_CMD | MSSIO1 | AA9 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
EMMC_DATA0 | MSSIO2 | AA7 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
EMMC_DATA1 | MSSIO3 | Y6 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
EMMC_DATA2 | MSSIO4 | AA10 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
EMMC_DATA3 | MSSIO5 | AA13 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
EMMC_STRB | MSSIO6 | Y10 | INPUT | UP | OFF | OFF | OFF | OFF | OFF | -- | --
EMMC_RSTN | MSSIO7 | Y7 | OUTPUT | UP | OFF | OFF | OFF | -- | -- | 8 | OFF
EMMC_DATA4 | MSSIO8 | Y14 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
EMMC_DATA5 | MSSIO9 | Y13 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
EMMC_DATA6 | MSSIO10 | Y8 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
EMMC_DATA7 | MSSIO11 | Y11 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
USB_CLK | MSSIO14 | W6 | INPUT | UP | OFF | OFF | OFF | OFF | OFF | -- | --
USB_DIR | MSSIO15 | V6 | INPUT | UP | OFF | OFF | OFF | OFF | OFF | -- | --
USB_NXT | MSSIO16 | W8 | INPUT | UP | OFF | OFF | OFF | OFF | OFF | -- | --
USB_STP | MSSIO17 | V8 | OUTPUT | UP | OFF | OFF | OFF | -- | -- | 8 | OFF
USB_DATA0 | MSSIO18 | V4 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
USB_DATA1 | MSSIO19 | U5 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
USB_DATA2 | MSSIO20 | W9 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
USB_DATA3 | MSSIO21 | U7 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
USB_DATA4 | MSSIO22 | U6 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
USB_DATA5 | MSSIO23 | V7 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
USB_DATA6 | MSSIO24 | V9 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
USB_DATA7 | MSSIO25 | U9 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
GPIO_1_12_OUT | MSSIO26 | V14 | OUTPUT | UP | OFF | OFF | OFF | -- | -- | 8 | OFF
GPIO_1_16_OUT | MSSIO30 | W14 | OUTPUT | UP | OFF | OFF | OFF | -- | -- | 8 | OFF
GPIO_1_20_OUT | MSSIO34 | V11 | OUTPUT | UP | OFF | OFF | OFF | -- | -- | 8 | OFF
MAC_0_MDC | MSSIO35 | U10 | OUTPUT | UP | OFF | OFF | OFF | -- | -- | 8 | OFF
MAC_0_MDIO | MSSIO36 | U14 | INOUT | UP | OFF | OFF | OFF | OFF | OFF | 8 | OFF
GPIO_1_23_OUT | MSSIO37 | V12 | OUTPUT | UP | OFF | OFF | OFF | -- | -- | 8 | OFF

## DDRIO Port Settings

Port Name | Package Pin Name | Direction | On Die Termination | Output Drive (mA)
--- | --- | --- | --- | ---
DQ[0] | AF8 | INOUT | 40 | 40
DQ[1] | AF7 | INOUT | 40 | 40
DQ[2] | AE8 | INOUT | 40 | 40
DQ[3] | AE7 | INOUT | 40 | 40
DQ[4] | AH7 | INOUT | 40 | 40
DQ[5] | AH8 | INOUT | 40 | 40
DQ[6] | AF5 | INOUT | 40 | 40
DQ[7] | AF4 | INOUT | 40 | 40
DQ[8] | AF3 | INOUT | 40 | 40
DQ[9] | AF2 | INOUT | 40 | 40
DQ[10] | AE2 | INOUT | 40 | 40
DQ[11] | AE1 | INOUT | 40 | 40
DQ[12] | AG1 | INOUT | 40 | 40
DQ[13] | AH1 | INOUT | 40 | 40
DQ[14] | AH3 | INOUT | 40 | 40
DQ[15] | AJ3 | INOUT | 40 | 40
DQ[16] | AJ6 | INOUT | 40 | 40
DQ[17] | AG5 | INOUT | 40 | 40
DQ[18] | AH6 | INOUT | 40 | 40
DQ[19] | AH4 | INOUT | 40 | 40
DQ[20] | AG6 | INOUT | 40 | 40
DQ[21] | AG4 | INOUT | 40 | 40
DQ[22] | AK5 | INOUT | 40 | 40
DQ[23] | AL5 | INOUT | 40 | 40
DQ[24] | AK3 | INOUT | 40 | 40
DQ[25] | AL3 | INOUT | 40 | 40
DQ[26] | AK2 | INOUT | 40 | 40
DQ[27] | AK1 | INOUT | 40 | 40
DQ[28] | AL2 | INOUT | 40 | 40
DQ[29] | AM1 | INOUT | 40 | 40
DQ[30] | AM2 | INOUT | 40 | 40
DQ[31] | AN2 | INOUT | 40 | 40
DQS[0] | AE6 | INOUT | 40 | 40
DQS[1] | AG2 | INOUT | 40 | 40
DQS[2] | AJ4 | INOUT | 40 | 40
DQS[3] | AL4 | INOUT | 40 | 40
DQS_N[0] | AE5 | INOUT | 40 | 40
DQS_N[1] | AH2 | INOUT | 40 | 40
DQS_N[2] | AJ5 | INOUT | 40 | 40
DQS_N[3] | AM4 | INOUT | 40 | 40
DM[0] | AG7 | OUTPUT | -- | 40
DM[1] | AJ1 | OUTPUT | -- | 40
DM[2] | AK6 | OUTPUT | -- | 40
DM[3] | AN1 | OUTPUT | -- | 40
RESET_N | AB12 | OUTPUT | -- | 34
ODT | AB11 | OUTPUT | -- | 34
CKE | AC11 | OUTPUT | -- | 34
CS | AC14 | OUTPUT | -- | 34
CK | AC1 | OUTPUT | -- | 34
CK_N | AC2 | OUTPUT | -- | 34
CA[0] | AB1 | OUTPUT | -- | 34
CA[1] | AB2 | OUTPUT | -- | 34
CA[2] | AE3 | OUTPUT | -- | 34
CA[3] | AD1 | OUTPUT | -- | 34
CA[4] | AA2 | OUTPUT | -- | 34
CA[5] | AA3 | OUTPUT | -- | 34

## SGMII I/O Port settings

Port Name | Package Pin Name | Direction | I/O Standard | Resistor Pull | VCM Input Range | On Die Termination (Ohm) | Output Drive (mA) | Source Termination (Ohm)
--- | --- | --- | --- | --- | --- | --- | --- | ---
SGMII_RX0_P | W1 | INPUT | LVDS33 | NONE | MID | 100 | -- | --
SGMII_RX0_N | Y1 | INPUT | LVDS33 | NONE | MID | 100 | -- | --
SGMII_TX0_P | Y5 | OUTPUT | LVDS33 | NONE | -- | -- | 6 | 100
SGMII_TX0_N | AA5 | OUTPUT | LVDS33 | NONE | -- | -- | 6 | 100