# 7.2. Error code list

# | Blink Pattern | ID | Description | Comments
--- | --- | --- | --- | ---
Traps
1 | 2 | ERR_OSC_FAIL | oscillator failure |
2 | 3 | ERR_ADDRESS_ERROR | address error (e.g. alignment) |
3 | 4 | ERR_HARD_TRAP | hard trap |
4 | 1 2 | ERR_STACK_ERROR | stack pointer error |
5 | 2 2 | ERR_MATH | arithmetic error |
6 | 3 2 | ERR_RESERVED_TRAP5 | code for trap 5 unused |
7 | 4 2 | ERR_SOFT_TRAP | hard trap |
8 | 1 3 | ERR_RESERVED_TRAP7 | reserved trap #7 |
255 | 4 4 4 4 | ERR_UNEXPECTED_TRAP | unexpected trap from MCC trap handler |
Application errors
16 | 1 1 2 | ERR_STALL_RETRY_EXCEEDED | number of stall retries exceeded |
17 | 2 1 2 | ERR_INVALID_STARTUP_FSM_STATE | invalid startup FSM state |
18 | 3 1 2 | ERR_HW_OVERCURRENT | hardware overcurrent |
19 | 4 1 2 | ERR_DCLINK_OVERVOLTAGE | DC link overvoltage |
20 | 1 2 2 | ERR_DCLINK_UNDERVOLTAGE | DC link undervoltage |
32 | 1 1 3 | MCAF_ERR_RCON_TRAPR | trap conflict |
33 | 2 1 3 | MCAF_ERR_RCON_IOPUWR | IOPUWR illegal opcode / uninitialized W |
34 | 3 1 3 | MCAF_ERR_RCON_CM | configuration mismatch |
35 | 4 1 3 | MCAF_ERR_RCON_WDTO_ISR | watchdog timeout, ISR |
36 | 1 2 3 | ERR_RCON_WDTO_MAINLOOP | watchdog timeout, main loop |
37 | 2 2 3 | ERR_BOARD_CONFIG_FAIL | board configuration failed |
38 | 3 2 3 | ERR_BOARD_FAULT | board fault detected |
Unexpected interrupt errors
256 | 1 1 1 1 2 | ERR_UNEXPECTED_INTERRUPT_BASE |  | This covers a range of codes; if you encounter blink patterns in a similar range, please contact Microchip support, as this indicates an unexpected error that may be caused by a software bug.