
1. Corrected the silkscreen position for R65 and R72

From  to 

1. Added the board number information on the bottom layer as it is one of the requirements for the RTM and changed the revision number.

