<map id="main" name="main">
<area shape="rect" id="node2" href="$qdec__signal__generator_8c.html#a6adf375eb93247662f05483aedaab755" title="Initializes TCE0 to create Qadrature signal. " alt="" coords="108,5,256,32"/>
<area shape="rect" id="node3" href="$qdec__driver_8c.html#a81a14baaa57e91e95ba68f1203d744aa" title="This function set up the needed configuration for a Timer/Counter to handle the frequency/speed measu..." alt="" coords="104,56,260,83"/>
<area shape="rect" id="node4" href="$qdec__driver_8c.html#a2864f45f96dff4a8ce1b34fbd7599c2a" title="Wrapperfunction to set up all parameters for the quadrature decoder. " alt="" coords="115,107,249,133"/>
<area shape="rect" id="node5" href="$qdec__driver_8c.html#a63f330178c4e54f642a84a249ea72785" title="This function configure the event system for quadrature decoding. " alt="" coords="309,56,461,83"/>
<area shape="rect" id="node6" href="$qdec__driver_8c.html#a332418d6f5dcf52455d2454fba2f42b9" title="This function set up the needed configuration for the port used for the quadrature decoding..." alt="" coords="319,107,450,133"/>
<area shape="rect" id="node7" href="$qdec__driver_8c.html#a200eb47dd9a0a33d4881c6b739d61ed3" title="This function set up the needed configuration for the Timer/Counter to handle the quadrature decoding..." alt="" coords="308,157,461,184"/>
</map>
