| BLDC control on ATAVRMC303 with ATxMega128A1

Modules | Macros
DAC Defines Configuration Values
ADC Defines Configuration Values

Defines allowing to init the DAC with the wanted configuration. More...

Collaboration diagram for DAC Defines Configuration Values:

## Modules
| COMPARATORs Defines Configuration Values
| Defines allowing to init the COMPARATORs with the wanted configuration.

## Macros
#define | DAC_INPUT_RIGHT_ADJUST 0
| 0: Result left adjusted 1: Result right adjusted More...
#define | DAC_INTERNAL_VREF 1
#define | DAC_OUTPUT_DRIVER 1
#define | USE_DAC

## Detailed Description

Defines allowing to init the DAC with the wanted configuration.

## Macro Definition Documentation

## ◆ DAC_INPUT_RIGHT_ADJUST

#define DAC_INPUT_RIGHT_ADJUST 0

0: Result left adjusted 1: Result right adjusted

Definition at line 103 of file config.h.

## ◆ DAC_INTERNAL_VREF

#define DAC_INTERNAL_VREF 1

Definition at line 104 of file config.h.

## ◆ DAC_OUTPUT_DRIVER

#define DAC_OUTPUT_DRIVER 1

Definition at line 105 of file config.h.

## ◆ USE_DAC

#define USE_DAC

Definition at line 101 of file config.h.