digraph "ADC_Offset_Get"
{
  edge [fontname="Helvetica",fontsize="10",labelfontname="Helvetica",labelfontsize="10"];
  node [fontname="Helvetica",fontsize="10",shape=record];
  rankdir="LR";
  Node2 [label="ADC_Offset_Get",height=0.2,width=0.4,color="black", fillcolor="grey75", style="filled", fontcolor="black"];
  Node2 -> Node3 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node3 [label="ADC_ResultCh_GetLowByte",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8c.html#a234b91011bafc8394b5443c65be01573",tooltip="This function clears the interrupt flag and returns the low byte of the coversion result..."];
  Node2 -> Node4 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node4 [label="ADC_Wait_32MHz",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8c.html#a0e13135d7b45df0c9c615ed40765c786",tooltip="This function waits until the adc common mode is settled. "];
  Node2 -> Node5 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node5 [label="SP_ReadCalibrationByte",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8h.html#abcc2ef603c461cd65a0fd08b2d97d78c"];
}
