| BLDC control on ATAVRMC303 with ATxMega128A1

Modules | Macros
ADC Defines Configuration Values

Defines allowing to init the ADC with the wanted configuration. More...

Collaboration diagram for ADC Defines Configuration Values:

## Modules
| DAC Defines Configuration Values
| Defines allowing to init the DAC with the wanted configuration.

## Macros
#define | ADC_HIGH_SPEED_MODE 1
#define | ADC_INTERNAL_VREF 1
| 0: External Vref 1: Internal Vref 2: Vref is connected to Vcc More...
#define | ADC_IT 1
| 0: No ADC End of Conv IT 1: ADC End of conversion generates an IT More...
#define | ADC_PRESCALER 4
| 2, 4, 8, 16, 32, 64, 128 : The input ADC frequency is the system clock frequency divided by the const value More...
#define | ADC_RIGHT_ADJUST_RESULT 0
| 0: Result left adjusted 1: Result right adjusted More...
#define | USE_ADC

## Detailed Description

Defines allowing to init the ADC with the wanted configuration.

## Macro Definition Documentation

## ◆ ADC_HIGH_SPEED_MODE

#define ADC_HIGH_SPEED_MODE 1

Definition at line 93 of file config.h.

## ◆ ADC_INTERNAL_VREF

#define ADC_INTERNAL_VREF 1

0: External Vref 1: Internal Vref 2: Vref is connected to Vcc

Definition at line 94 of file config.h.

## ◆ ADC_IT

#define ADC_IT 1

0: No ADC End of Conv IT 1: ADC End of conversion generates an IT

Definition at line 95 of file config.h.

## ◆ ADC_PRESCALER

#define ADC_PRESCALER 4

2, 4, 8, 16, 32, 64, 128 : The input ADC frequency is the system clock frequency divided by the const value

Definition at line 96 of file config.h.

## ◆ ADC_RIGHT_ADJUST_RESULT

#define ADC_RIGHT_ADJUST_RESULT 0

0: Result left adjusted 1: Result right adjusted

Definition at line 92 of file config.h.

## ◆ USE_ADC

#define USE_ADC

Definition at line 90 of file config.h.