digraph "mc_init_HW"
{
  edge [fontname="Helvetica",fontsize="10",labelfontname="Helvetica",labelfontsize="10"];
  node [fontname="Helvetica",fontsize="10",shape=record];
  rankdir="LR";
  Node28 [label="mc_init_HW",height=0.2,width=0.4,color="black", fillcolor="grey75", style="filled", fontcolor="black"];
  Node28 -> Node29 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node29 [label="ADC_Init",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$mc__drv_8c.html#a3fdaf3b8949082abe85a7e7083087eb7"];
  Node29 -> Node30 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node30 [label="ADC_CalibrationValues_Set",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8c.html#a0db8be0c56deef76de33ae9dd5296b01",tooltip="This function get the calibration data from the production calibration. "];
  Node30 -> Node31 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node31 [label="SP_ReadCalibrationByte",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8h.html#abcc2ef603c461cd65a0fd08b2d97d78c"];
  Node29 -> Node32 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node32 [label="ADC_Offset_Get",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8c.html#a18a7d5f720fc404a58e3ffa7909953ef",tooltip="This function get the offset of the ADC. "];
  Node32 -> Node33 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node33 [label="ADC_ResultCh_GetLowByte",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8c.html#a234b91011bafc8394b5443c65be01573",tooltip="This function clears the interrupt flag and returns the low byte of the coversion result..."];
  Node32 -> Node34 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node34 [label="ADC_Wait_32MHz",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8c.html#a0e13135d7b45df0c9c615ed40765c786",tooltip="This function waits until the adc common mode is settled. "];
  Node32 -> Node31 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node29 -> Node35 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node35 [label="ADC_Wait_8MHz",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$adc__driver_8c.html#a98a478448d5c15720de6d517589e974e",tooltip="This function waits until the adc common mode is settled. "];
  Node28 -> Node36 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node36 [label="mc_init_timer0",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$mc__drv_8c.html#a017c4abbfd10869b10a5511562c46ecf",tooltip="Timer 0 Configuration The timer 0 is used to generate an IT when an overflow occurs. "];
  Node28 -> Node37 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node37 [label="mc_init_timer1",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$mc__drv_8c.html#ac6fa4b2d2da40ce7e590165c1583757a",tooltip="timer 1 Configuration Use to generate a 250us activation for sampling speed regulation ..."];
  Node28 -> Node38 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node38 [label="PWM_Init",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$mc__drv_8c.html#abc3c5f6664425b4006f003f05835d214",tooltip="Initialization of PWM generator PSC0. "];
  Node38 -> Node39 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node39 [label="ConfigDTI",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$mc__drv_8c.html#abf1a67edfe2a7111963d78d791c76515"];
  Node39 -> Node40 [color="midnightblue",fontsize="10",style="solid",fontname="Helvetica"];
  Node40 [label="AWEX_EnableDeadTimeInsertion",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$awex__driver_8c.html#aa12e5f06b573669304fef464f66f0952",tooltip="Enable Dead Time Insertion. "];
}
