| BLDC control on ATAVRMC303 with ATxMega128A1

Macros
COMPARATORs Defines Configuration Values
ADC Defines Configuration Values » DAC Defines Configuration Values

Defines allowing to init the COMPARATORs with the wanted configuration. More...

Collaboration diagram for COMPARATORs Defines Configuration Values:

## Macros
#define | COMPARATOR0_IT 1
| 0: Disable Comparator Interrupt 1: Enable Comparator Interrupt More...
#define | COMPARATOR0_IT_EVENT 0
| Comparator Interrupt on outut => 0: toggle 2: falling edge 3: rising edge. More...
#define | COMPARATOR0_NEGATIVE_INPUT 4
| Comparator negative input selection => 0: vref/6.40 1: vref/3.20 2: vref/2.13 3: vref/1.60 4: ACMPM 5: DAC result. More...
#define | COMPARATOR1_IT 1
| 0: Disable Comparator Interrupt 1: Enable Comparator Interrupt More...
#define | COMPARATOR1_IT_EVENT 0
| Comparator Interrupt on outut => 0: toggle 2: falling edge 3: rising edge. More...
#define | COMPARATOR1_NEGATIVE_INPUT 4
| Comparator negative input selection => 0: vref/6.40 1: vref/3.20 2: vref/2.13 3: vref/1.60 4: ACMPM 5: DAC result. More...
#define | COMPARATOR2_IT 1
| 0: Disable Comparator Interrupt 1: Enable Comparator Interrupt More...
#define | COMPARATOR2_IT_EVENT 0
| Comparator Interrupt on outut => 0: toggle 2: falling edge 3: rising edge. More...
#define | COMPARATOR2_NEGATIVE_INPUT 4
| Comparator negative input selection => 0: vref/6.40 1: vref/3.20 2: vref/2.13 3: vref/1.60 4: ACMPM 5: DAC result. More...
#define | USE_COMP0
#define | USE_COMP1
#define | USE_COMP2

## Detailed Description

Defines allowing to init the COMPARATORs with the wanted configuration.

## Macro Definition Documentation

## ◆ COMPARATOR0_IT

#define COMPARATOR0_IT 1

0: Disable Comparator Interrupt 1: Enable Comparator Interrupt

Definition at line 112 of file config.h.

## ◆ COMPARATOR0_IT_EVENT

#define COMPARATOR0_IT_EVENT 0

Comparator Interrupt on outut => 0: toggle 2: falling edge 3: rising edge.

Definition at line 113 of file config.h.

## ◆ COMPARATOR0_NEGATIVE_INPUT

#define COMPARATOR0_NEGATIVE_INPUT 4

Comparator negative input selection => 0: vref/6.40 1: vref/3.20 2: vref/2.13 3: vref/1.60 4: ACMPM 5: DAC result.

Definition at line 114 of file config.h.

## ◆ COMPARATOR1_IT

#define COMPARATOR1_IT 1

0: Disable Comparator Interrupt 1: Enable Comparator Interrupt

Definition at line 117 of file config.h.

## ◆ COMPARATOR1_IT_EVENT

#define COMPARATOR1_IT_EVENT 0

Comparator Interrupt on outut => 0: toggle 2: falling edge 3: rising edge.

Definition at line 118 of file config.h.

## ◆ COMPARATOR1_NEGATIVE_INPUT

#define COMPARATOR1_NEGATIVE_INPUT 4

Comparator negative input selection => 0: vref/6.40 1: vref/3.20 2: vref/2.13 3: vref/1.60 4: ACMPM 5: DAC result.

Definition at line 119 of file config.h.

## ◆ COMPARATOR2_IT

#define COMPARATOR2_IT 1

0: Disable Comparator Interrupt 1: Enable Comparator Interrupt

Definition at line 122 of file config.h.

## ◆ COMPARATOR2_IT_EVENT

#define COMPARATOR2_IT_EVENT 0

Comparator Interrupt on outut => 0: toggle 2: falling edge 3: rising edge.

Definition at line 123 of file config.h.

## ◆ COMPARATOR2_NEGATIVE_INPUT

#define COMPARATOR2_NEGATIVE_INPUT 4

Comparator negative input selection => 0: vref/6.40 1: vref/3.20 2: vref/2.13 3: vref/1.60 4: ACMPM 5: DAC result.

Definition at line 124 of file config.h.

## ◆ USE_COMP0

#define USE_COMP0

Definition at line 111 of file config.h.

## ◆ USE_COMP1

#define USE_COMP1

Definition at line 116 of file config.h.

## ◆ USE_COMP2

#define USE_COMP2

Definition at line 121 of file config.h.