| BLDC control on ATAVRMC303 with ATxMega128A1

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - u -

- uart_putchar : config.h
- UpdateScreen() : DB101_IF.c , DB101_IF.h
- USART_Baudrate_Set : usart_driver.h
- USART_Buffer_t : usart_driver.h
- USART_data_t : usart_driver.h
- USART_DataRegEmpty() : usart_driver.h , usart_driver.c
- USART_DreInterruptLevel_Set : usart_driver.h
- USART_Format_Set : usart_driver.h
- USART_GetChar : usart_driver.h
- USART_InterruptDriver_DreInterruptLevel_Set() : usart_driver.c , usart_driver.h
- USART_InterruptDriver_Initialize() : usart_driver.c , usart_driver.h
- USART_IsRXComplete : usart_driver.h
- USART_IsTXDataRegisterEmpty : usart_driver.h
- USART_NineBits_GetChar() : usart_driver.c , usart_driver.h
- USART_NineBits_PutChar() : usart_driver.c , usart_driver.h
- USART_PutChar : usart_driver.h
- USART_RX_BUFFER_MASK : usart_driver.h
- USART_RX_BUFFER_SIZE : usart_driver.h
- USART_Rx_Disable : usart_driver.h
- USART_Rx_Enable : usart_driver.h
- USART_RXBuffer_GetByte() : usart_driver.c , usart_driver.h
- USART_RXBufferData_Available() : usart_driver.c , usart_driver.h
- USART_RXComplete() : usart_driver.h , usart_driver.c
- USART_RxdInterruptLevel_Set : usart_driver.h
- USART_SetMode : usart_driver.h
- USART_TX_BUFFER_MASK : usart_driver.h
- USART_TX_BUFFER_SIZE : usart_driver.h
- USART_Tx_Disable : usart_driver.h
- USART_Tx_Enable : usart_driver.h
- USART_TXBuffer_FreeSpace() : usart_driver.c , usart_driver.h
- USART_TXBuffer_PutByte() : usart_driver.h , usart_driver.c
- USART_TxdInterruptLevel_Set : usart_driver.h
- USE_ADC : config.h
- USE_COMP0 : config.h
- USE_COMP1 : config.h
- USE_COMP2 : config.h
- USE_DAC : config.h
- ushell_active : ushell_task.c , ushell_task.h
- ushell_task() : ushell_task.h , ushell_task.c
- ushell_task_init() : ushell_task.c , ushell_task.h