| BLDC control on ATAVRMC303 with ATxMega128A1

Macros
ADC High Speed Mode Configuration
ADC Module » ADC Macros

Set the high spped mode in case ADC frequency is higher than 200KHz. More...

Collaboration diagram for ADC High Speed Mode Configuration:

## Macros
#define | Disable_adc_high_speed_mode() (ADCSRB &= ~(1<<ADHSM))
#define | Enable_adc_high_speed_mode() (ADCSRB |= (1<<ADHSM))

## Detailed Description

Set the high spped mode in case ADC frequency is higher than 200KHz.

## Macro Definition Documentation

## ◆ Disable_adc_high_speed_mode

#define Disable_adc_high_speed_mode | ( |  | ) | (ADCSRB &= ~(1<<ADHSM))

Definition at line 49 of file adc_drv.h.

## ◆ Enable_adc_high_speed_mode

#define Enable_adc_high_speed_mode | ( |  | ) | (ADCSRB |= (1<<ADHSM))

Definition at line 48 of file adc_drv.h.