| BLDC control on ATAVRMC303 with ATxMega128A1

Macros
ADC Start Idle Conversion
ADC Module » ADC Macros » ADC Start Conversion

Start the Analog to Digital Conversion in noise reduction mode. More...

Collaboration diagram for ADC Start Idle Conversion:

## Macros
#define | Clear_sleep_mode() (SMCR &= ~(1<<SM0)|(1<<SE) )
#define | Start_conv_idle() (SMCR |= (1<<SM0)|(1<<SE) )
#define | Start_conv_idle_channel(channel) (Select_adc_channel(channel), Start_conv_idle() )

## Detailed Description

Start the Analog to Digital Conversion in noise reduction mode.

## Macro Definition Documentation

## ◆ Clear_sleep_mode

#define Clear_sleep_mode | ( |  | ) | (SMCR &= ~(1<<SM0)|(1<<SE) )

Definition at line 107 of file adc_drv.h.

## ◆ Start_conv_idle

#define Start_conv_idle | ( |  | ) | (SMCR |= (1<<SM0)|(1<<SE) )

Definition at line 105 of file adc_drv.h.

## ◆ Start_conv_idle_channel

#define Start_conv_idle_channel | ( |  | channel | ) | (Select_adc_channel(channel), Start_conv_idle() )

Definition at line 106 of file adc_drv.h.