<map id="G" name="G">
<area shape="rect" id="node3" href="$a00112.html#gacf7a0ccc90d9cc3f25f8ba740f970b37" title="This function update the OSCCAL value following the temperature and the voltage." alt="" coords="112,32,243,61"/>
<area shape="rect" id="node11" href="$a00110.html#gab15cf82f0329bc4d7262c03559eaaa8e" title="&lt; this define is set on config.h file" alt="" coords="144,85,211,115"/>
<area shape="rect" id="node13" href="$a00045.html#a9fa00b0be5d3c4781048861e2506eb63" title="Init &amp; run the scheduler." alt="" coords="139,139,216,168"/>
<area shape="rect" id="node21" href="$a00050.html#ac19c11a3fb5c7d94bf81d4b43acaccd9" title="This function calls the on&#45;chip bootloader." alt="" coords="104,192,251,221"/>
<area shape="rect" id="node23" href="$a00124.html#gacda568275630927dc6caa7e40fab2647" title="This functions stops the hardware watchdog timer." alt="" coords="124,245,231,275"/>
<area shape="rect" id="node5" href="$a00112.html#ga3d0c2ecab107719fbb85efd9267e9583" title="This function get the calibration values." alt="" coords="317,5,424,35"/>
<area shape="rect" id="node9" href="$a00112.html#gabf3eda5f92d2edecd1b8a472bd83432d" title="Read and return internal temperature sensor ADC channel." alt="" coords="299,59,443,88"/>
<area shape="rect" id="node7" href="$a00033.html#ac0ea9526f3d413fe250b958f8701648f" title="This macro function allows to read device IDs of the product." alt="" coords="511,5,615,35"/>
<area shape="rect" id="node15" href="$a00045.html#ab258cc2856e5f6bb125907cc23358fbd" title="_____ M A C R O S ________________________________________________________ _____ D E F I N I T I O N ..." alt="" coords="320,112,421,141"/>
<area shape="rect" id="node17" href="$a00045.html#aac47313d2feeea0627a5469b1a311547" title="Task execution scheduler." alt="" coords="312,165,429,195"/>
<area shape="rect" id="node19" href="$a00045.html#a3f25f16571b50207c563196ce3d1385c" title="Do nothing Avoid uncalled segment warning if the empty function is not used." alt="" coords="492,165,633,195"/>
</map>
